{"text_format":"1","workbook":"xlsx","n_sheets":37,"sheets":["Translation-EN","Translation-FR","Cover_Couverture","License","Introduction","Introduction-FR","USER INPUT SHEET","Conctete Selections","Footings & Slabs","Foundation Walls","Structural Elements","Ext. Walls","Ext. Wall Systems","Party Walls","Cladding","Windows","Int. Walls","Floors","Ceilings","Roof","Garage","User-Defined","REVIEW","RESULTS","SCENARIOS","Scenarios-DB","Glossary","Glossaire","Energy GHG","Element Properties","Master sheet","Composite Master Sheet","Data","Windows Methodology","Dropdown Lists","Setting","Formulas & Formats"],"not_rendered":{"charts":4,"images":33,"macros":1,"external_links":1,"defined_names":186,"comments":9,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Translation-EN","index":0,"n_rows":2531,"n_cols":9,"rows_kept":2531,"cut":false,"hidden":true,"merged":[[1076,4,1076,11],[1013,4,1013,5],[1019,4,1020,4],[1021,4,1022,4],[1023,4,1024,4],[1025,4,1026,4],[1048,4,1048,7],[1012,4,1012,11],[751,4,751,16],[756,4,757,4],[758,4,759,4],[760,4,761,4],[762,4,763,4],[827,4,827,16],[832,4,833,4],[834,4,835,4],[836,4,837,4],[838,4,839,4],[1011,4,1011,7],[740,4,741,4],[633,4,634,4],[635,4,636,4],[668,4,668,16],[673,4,674,4],[675,4,676,4],[677,4,678,4],[679,4,680,4],[729,4,729,16],[734,4,735,4],[736,4,737,4],[738,4,739,4],[631,4,632,4],[573,4,574,4],[575,4,576,4],[577,4,578,4],[579,4,580,4],[605,4,605,16],[610,4,611,4],[612,4,613,4],[614,4,615,4],[616,4,617,4],[624,4,624,16],[629,4,630,4],[568,4,568,16],[431,4,432,4],[433,4,434,4],[435,4,436,4],[437,4,438,4],[451,4,457,5],[467,4,467,16],[472,4,473,4],[474,4,475,4],[476,4,477,4],[478,4,479,4],[556,4,561,5],[426,4,426,16],[284,4,290,5],[325,4,325,16],[330,4,331,4],[332,4,333,4],[334,4,335,4],[336,4,337,4],[349,4,349,16],[354,4,355,4],[356,4,357,4],[358,4,359,4],[360,4,361,4],[246,4,247,4],[149,4,149,6],[160,4,160,15],[163,4,163,16],[168,4,169,4],[170,4,171,4],[172,4,173,4],[174,4,175,4],[235,4,235,16],[240,4,241,4],[242,4,243,4],[244,4,245,4],[143,4,143,9],[27,4,28,11],[29,4,29,6],[33,4,35,11],[40,4,43,11],[57,4,58,4],[59,4,60,4],[66,4,66,11],[67,4,67,6],[117,4,117,17],[119,4,119,14],[134,4,134,9],[15,4,15,5],[0,4,0,5],[0,6,0,7],[4,4,8,12],[13,4,13,5],[14,4,14,5]]}
[null,null,null,null,"English",null,"French"]
["Type","Sheet","Address","Additional Info","Value","Comment/Title","Value","Comment/Title"]
["Range","USER INPUT SHEET","Q1",null,"UNIT CONVERSIONS"]
["Range","USER INPUT SHEET","A2",null,"November 2023"]
["Range","USER INPUT SHEET","B2",true,"Material Carbon Emissions Estimator (MCE2)"]
["-"]
["-"]
["-"]
["-"]
["Range","USER INPUT SHEET","K2",null,"Project Carbon Content "]
["Range","USER INPUT SHEET","Q3",null,"Volume"]
["Range","USER INPUT SHEET","W3",null,"Area"]
["Range","USER INPUT SHEET","AB3",null,"Length"]
["Range","USER INPUT SHEET","R5",true,"ft3 à"]
["Range","USER INPUT SHEET","X5",true,"ft2à"]
["Range","USER INPUT SHEET","AC5",true,"ft à"]
["Range","USER INPUT SHEET","A7",null," Step"]
["Range","USER INPUT SHEET","B7",true,"      Import project data from HOT2000 (If no HOT2000 file, skip to Step 2)"]
["Range","USER INPUT SHEET","M7",null,"Energy Consumption"]
["Range","USER INPUT SHEET","O7",null,"Energy Generation"]
["Range","USER INPUT SHEET","R7",null,"Notes on Energy Consumption"]
["Shape","USER INPUT SHEET","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Press Here to import HOT2000 Data"]
["Shape","USER INPUT SHEET","Rounded Rectangle 16||Rectangle: Rounded Corners 16",null,"Clear All (User Input and all Assembly Tabs)"]
["Shape","USER INPUT SHEET","Rounded Rectangle 15||Rectangle: Rounded Corners 15",null,"Clear This Sheet Only (User Input)"]
["Range","USER INPUT SHEET","M8",null,"Elec. kWh/yr"]
["Range","USER INPUT SHEET","N8",true,"N. Gas m3/yr"]
["Range","USER INPUT SHEET","O8",null,"Elec. kWh/yr",null,null,"2023_July_new"]
["Range","USER INPUT SHEET","R8",true,"Electricity generated on-site has already been subtracted from the total energy consumption in cell M9."]
["-"]
["Range","USER INPUT SHEET","P10",true,"Note: kg/m2 comes from total kg divided by habitable floor area"]
["Range","USER INPUT SHEET","M11",null,"Propane L/yr"]
["Range","USER INPUT SHEET","N11",null,"Oil L/yr"]
["Range","USER INPUT SHEET","O11",null,"Wood kg/yr"]
["Range","USER INPUT SHEET","R11",true,"Energy consumption reflects values from HOT2000, users should manually update values if using a different modeling software. "]
["-"]
["-"]
["Range","USER INPUT SHEET","M13",null,"To override energy GHG intensities, use the Energy GHG tab."]
["Range","USER INPUT SHEET","A14",null,{"$f":"$E$17","v":" Step"}]
["Range","USER INPUT SHEET","B14",true,"      Confirm or enter project information"]
["Range","USER INPUT SHEET","M14",null,"Operational Emissions"]
["Range","USER INPUT SHEET","R14",null,"When considering different scenarios, users should ensure that thermal resistances of assemblies are consistent, as these will determine the energy consumption of the home. Where these change, users should also revise the energy model and update the energy consumption values. "]
["-"]
["-"]
["-"]
["Range","USER INPUT SHEET","B15",null,"Address:"]
["Range","USER INPUT SHEET","E15",null,"Province:"]
["Range","USER INPUT SHEET","M15",true,"tonnes CO2e / yr"]
["Range","USER INPUT SHEET","N15",true,"t CO2e / 30 yrs"]
["Range","USER INPUT SHEET","B16",null,"City:"]
["Range","USER INPUT SHEET","E16",null,"Postal code:"]
["Range","USER INPUT SHEET","B17",null,"Building Type:"]
["Range","USER INPUT SHEET","E17",null,"Evaluation date:"]
["Range","USER INPUT SHEET","B18",null,"Storeys:"]
["Range","USER INPUT SHEET","E18",null,"File ID:"]
["Range","USER INPUT SHEET","M18",null,"Material Emissions"]
["Range","USER INPUT SHEET","B19",null,"Year Built:"]
["Range","USER INPUT SHEET","E19",null,"File name:"]
["Range","USER INPUT SHEET","M19",true,"tonnes CO2e"]
["-"]
["Range","USER INPUT SHEET","N19",true,"kg CO2e / m2"]
["-"]
["Range","USER INPUT SHEET","B20",true,"Heated Floor Area (above grade, m2):"]
["Range","USER INPUT SHEET","B21",true,"Heated Floor Area (below grade, m2):"]
["Range","USER INPUT SHEET","B22",null,"Heating Degree Days:"]
["Range","USER INPUT SHEET","A24",null,{"$f":"$E$17","v":" Step"}]
["Range","USER INPUT SHEET","B24",true,"      Confirm or enter project dimensions"]
["Range","USER INPUT SHEET","E24",true,"HOT2000 values are imported to the BLUE cells below. \nIf no HOT2000 file imported, then enter values into the BLUE cells. "]
["Range","USER INPUT SHEET","M24",true,"For all YELLOW cells below, manually enter all relevant values. Exclude any garage quantities."]
["Range","USER INPUT SHEET","P24",null,"YOUR DATA"]
["Range","USER INPUT SHEET","B25",null,"  COMPONENT"]
["Range","USER INPUT SHEET","C25",null,"AREA/\nVOLUME"]
["Range","USER INPUT SHEET","E25",null,"UNIT"]
["Range","USER INPUT SHEET","F25",null,"   APPLICATION OF INPUT VALUE"]
["Range","USER INPUT SHEET","M25",null,"   DESCRIPTION OF REQUIRED UNITS"]
["Range","USER INPUT SHEET","B27",null,"FOOTINGS, PADS & PIERS"]
["Range","USER INPUT SHEET","B29",null,"FOUNDATION WALL AREA"]
["Range","USER INPUT SHEET","B30",null,"FOUNDATION SLAB/FLOOR AREA"]
["Range","USER INPUT SHEET","B31",null,"EXTERIOR WALL AREA"]
["Range","USER INPUT SHEET","B32",null,"WINDOW AREA"]
["Range","USER INPUT SHEET","B33",null,"INTERIOR WALL AREA"]
["Range","USER INPUT SHEET","B34",null,"FRAMED FLOOR AREA"]
["Range","USER INPUT SHEET","B35",null,"CEILING AREA"]
["Range","USER INPUT SHEET","B36",null,"ROOFING AREA"]
["Range","USER INPUT SHEET","B37",null,"ROOF INSULATION AREA"]
["Range","USER INPUT SHEET","B38",null,"HEAVY TIMBER ELEMENTS"]
["Range","USER INPUT SHEET","B39",null,"PARTY WALL AREA"]
["Range","USER INPUT SHEET","F27",null,"Footing Length"]
["Range","USER INPUT SHEET","H27",null,"Footing Depth"]
["Range","USER INPUT SHEET","J27",null,"Footing Width"]
["Range","USER INPUT SHEET","F29",null,"Foundation wall, exterior continuous insulation, interior framing, interior insulation, interior wall finish"]
["Range","USER INPUT SHEET","F30",null,"Slab, aggregate base, sub-slab insulation, basement flooring"]
["Range","USER INPUT SHEET","F31",null,"Framing, insulation, sheathing, exterior cladding, interior cladding of exterior walls only"]
["Range","USER INPUT SHEET","F32",null,"Windows"]
["Range","USER INPUT SHEET","F33",null,"Framing, insulation and interior cladding of interior walls "]
["Range","USER INPUT SHEET","F34",null,"Floor framing, subfloor, floor insulation, flooring"]
["Range","USER INPUT SHEET","F35",null,"Ceiling cladding/coverings"]
["Range","USER INPUT SHEET","F36",null,"Roof framing,  decking, roofing, and insulation parallel to roof deck"]
["Range","USER INPUT SHEET","F37",null,"Roof insulation parallel to ceiling"]
["Range","USER INPUT SHEET","F38",null,"Heavy timber framing members (e.g. posts and beams)"]
["Range","USER INPUT SHEET","F39",null,"Party wall framing, insulation, sheathing, interior cladding."]
["Range","USER INPUT SHEET","M27",null,"Total cubic metres of all footings, piers and posts"]
["Range","USER INPUT SHEET","M29",null,"Total wall area (exclude windows and doors)"]
["Range","USER INPUT SHEET","M30",null,"Square metres"]
["Range","USER INPUT SHEET","M31",null,"Total exterior wall area (include gable ends; exclude window & door openings). Exclude all garage wall, garage partition wall and party wall areas"]
["Range","USER INPUT SHEET","M32",null,"Square metres (include full area of glazing units)"]
["Range","USER INPUT SHEET","M33",null,"Square metres (one side only) of all interior walls. Quantity will be doubled for cladding materials"]
["Range","USER INPUT SHEET","M34",null,"Square metres (includes all levels, excludes basement slab, stairs and other openings)"]
["Range","USER INPUT SHEET","M35",null,"Square metres (all levels; include basement ceiling if applicable)"]
["Range","USER INPUT SHEET","M36",null,"Square metres (Include sloped and flat roofs; exclude overhangs and gable ends)"]
["Range","USER INPUT SHEET","M37",null,"Square metres of insulation in the roof cavity. Typically this is equal to the attic floor or top floor ceiling area. "]
["Range","USER INPUT SHEET","M38",null,"Cubic metres of total wood volume in posts & beams. (Heavy steel members input in Structural Elements tab)"]
["Range","USER INPUT SHEET","M39",null,"Square meters of wall area that partitions one dwelling from another. Used for row housing units, apartment units, etc."]
["Range","USER INPUT SHEET","Q36",null,"HEAVY TIMBER BEAM VOLUME CALCULATOR"]
["Range","USER INPUT SHEET","Q37",null,"Beam Length (M)"]
["Range","USER INPUT SHEET","S37",null,"Beam Depth (mm)"]
["Range","USER INPUT SHEET","U37",null,"Beam Width (mm)"]
["Range","USER INPUT SHEET","W37",null,"Beam Volume (m3)"]
["Range","USER INPUT SHEET","B41",true,"If this building includes a GARAGE, click the PLUS symbol on the left to expand the Garage section. "]
["Range","USER INPUT SHEET","B42",null,"GARAGE"]
["Range","USER INPUT SHEET","B43",true,"Enter garage measurements in the YELLOW cells below. "]
["Range","USER INPUT SHEET","B44",null,{"$f":"$E$70","v":"  COMPONENT"}]
["Range","USER INPUT SHEET","C44",null,"QUANTITY"]
["Range","USER INPUT SHEET","E44",null,{"$f":"$E$72","v":"UNIT"}]
["Range","USER INPUT SHEET","F44",null,{"$f":"$E$73","v":"   APPLICATION OF INPUT VALUE"}]
["Range","USER INPUT SHEET","M44",null,{"$f":"$E$74","v":"   DESCRIPTION OF REQUIRED UNITS"}]
["Range","USER INPUT SHEET","B46",null,"ATTACHED GARAGE WALL AREA"]
["Range","USER INPUT SHEET","B47",null,"GARAGE FOOTINGS & PADS"]
["Range","USER INPUT SHEET","B49",null,"GARAGE FOUNDATION WALL AREA"]
["Range","USER INPUT SHEET","B50",null,"GARAGE SLAB/FLOOR AREA"]
["Range","USER INPUT SHEET","B51",null,"GARAGE EXTERIOR WALL AREA"]
["Range","USER INPUT SHEET","B52",null,"GARAGE WINDOW AREA"]
["Range","USER INPUT SHEET","B53",null,"GARAGE FINISHED CEILING AREA"]
["Range","USER INPUT SHEET","B54",null,"GARAGE ROOFING AREA"]
["Range","USER INPUT SHEET","B55",null,"GARAGE HEAVY TIMBERS"]
["Range","USER INPUT SHEET","F46",true,"Exterior wall framing, interior wall cladding, partition wall insulation (hover cursor for details)"]
["Range","USER INPUT SHEET","F47",null,{"$f":"$E$87","v":"Footing Length"}]
["Range","USER INPUT SHEET","H47",null,{"$f":"$E$88","v":"Footing Depth"}]
["Range","USER INPUT SHEET","J47",null,{"$f":"$E$89","v":"Footing Width"}]
["Range","USER INPUT SHEET","F49",null,"Garage foundation wall, interior framing, interior wall finish"]
["Range","USER INPUT SHEET","F50",null,"Slab, aggregate base"]
["Range","USER INPUT SHEET","F51",null,"Framing, sheathing, exterior cladding, interior cladding"]
["Range","USER INPUT SHEET","F52",null,{"$f":"$E$93","v":"Windows"}]
["Range","USER INPUT SHEET","F53",null,{"$f":"$E$96","v":"Ceiling cladding/coverings"}]
["Range","USER INPUT SHEET","F54",true,"Roof framing, decking, roofing. HOT2000 users: see Note (hover cursor)"]
["Range","USER INPUT SHEET","F55",null,{"$f":"$E$99","v":"Heavy timber framing members (e.g. posts and beams)"}]
["Range","USER INPUT SHEET","M46",null,"Area of wall that attaches the garage to the building (excludes openings and exterior garage walls).\nIf the garage is detached, leave this cell blank. "]
["Range","USER INPUT SHEET","M47",null,"Cubic metres. Only include volume additional to main building footings, pads and piers"]
["Range","USER INPUT SHEET","M49",null,"Square metres (exclude windows and doors). Only include foundation area additional to main building foundation"]
["Range","USER INPUT SHEET","M50",null,{"$f":"$E$103","v":"Square metres"}]
["Range","USER INPUT SHEET","M51",true,"Exterior garage wall area (include gable area, exclude window & door openings) Exclude attached wall area"]
["Range","USER INPUT SHEET","M52",null,"Square metres (full area of glazing units)"]
["Range","USER INPUT SHEET","M53",null,"Square metres (all levels)"]
["Range","USER INPUT SHEET","M54",null,"Square metres (Includes sloped and flat roofs; excludes overhangs) "]
["Range","USER INPUT SHEET","M55",null,{"$f":"$E$111","v":"Cubic metres of total wood volume in posts & beams. (Heavy steel members input in Structural Elements tab)"}]
["Range","USER INPUT SHEET","A58",null,{"$f":"$E$17","v":" Step"}]
["Range","USER INPUT SHEET","B58",true,"      Define all building assemblies in the following building section tabs."]
["Range","USER INPUT SHEET","A61",null,{"$f":"$E$17","v":" Step"}]
["Range","USER INPUT SHEET","B61",true,"      Review the selected materials in the REVIEW tab. "]
["Range","USER INPUT SHEET","A64",null,{"$f":"$E$17","v":" Step"}]
["Range","USER INPUT SHEET","B64",true,"      View the carbon emissions report in the RESULTS tabs."]
["Range","USER INPUT SHEET","B67",true,"Helpful Notes:\n- See the Glossary tab for descriptions of unfamiliar terms or acronyms.\n- Use the User-Defined tab for any materials you wish to add but that could not be included in the section tabs.\n- To jump to a tab, right-click the arrows in the lower left corner and select the tab.\n- All framing spacing is 24 inches on centre by default, even when Framing Spacing value is blank"]
["Range","Footings & Slabs","A1",null,"SECTION 1 ➜ COMPONENT MATERIALS FOR "]
["Range","Footings & Slabs","D1",null,"FOUNDATION - FOOTINGS & SLABS"]
["Range","Footings & Slabs","A2",true,"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["Range","Footings & Slabs","A3",null,"CATEGORY"]
["Range","Footings & Slabs","C3",null,"MATERIAL"]
["Range","Footings & Slabs","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Footings & Slabs","H3",null," SELECT"]
["Range","Footings & Slabs","I3",true,"NET kgCO2e EMISSIONS"]
["-"]
["Range","Footings & Slabs","J3",true,"SELECTED MATERIAL kgCO2e CONTENT"]
["-"]
["Range","Footings & Slabs","K3",true,"kgCO2e EMISSIONS"]
["-"]
["Range","Footings & Slabs","L3",true,"kgCO2 STORAGE"]
["-"]
["Range","Footings & Slabs","M3",true,"kgCO2e SUBTOTAL FOR FOUNDATION FOOTINGS & SLAB"]
["Range","Footings & Slabs","A5",null,"CRUSHED STONE BASE"]
["Range","Footings & Slabs","D5",null,"THICKNESS:"]
["Range","Footings & Slabs","B6",null,"AGGREGATE"]
["Range","Footings & Slabs","A7",null,"If you do not know the specific carbon footprint of your aggregate, chose the \"AVERAGE\" value"]
["Range","Footings & Slabs","A12",null,"FOOTINGS, PIERS & PADS"]
["Range","Footings & Slabs","B13",null,"CONCRETE – 25 MPa or less"]
["Range","Footings & Slabs","A14",null,"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."]
["Range","Footings & Slabs","B21",null,"CONCRETE – 26-30 MPa"]
["Range","Footings & Slabs","A22",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Footings & Slabs","B29",null,"CONCRETE – 31-35 MPa"]
["Range","Footings & Slabs","A30",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Footings & Slabs","A37",null,"REBAR"]
["Range","Footings & Slabs","D37",null,"CUSTOM LENGTH"]
["Range","Footings & Slabs","B38",null,"CONCRETE REINFORCING BAR"]
["Range","Footings & Slabs","A39",null,"Specify an overall rebar length."]
["Range","Footings & Slabs","A47",null,"STEEL REINFORCING MESH"]
["Range","Footings & Slabs","D47",null,"CUSTOM AREA:"]
["Range","Footings & Slabs","B48",null,"WELDED WIRE MESH"]
["Range","Footings & Slabs","A50",null,"HELICAL PIERS"]
["Range","Footings & Slabs","D50",null,"TOTAL LENGTH OF ALL PIERS:"]
["Range","Footings & Slabs","B51",null,{"$f":"$E$196","v":"HELICAL PIERS"}]
["Range","Footings & Slabs","A52",null,"Specify the total length of all piers. Use % to adjust for different sized piers"]
["Range","Footings & Slabs","A53",null,"CONCRETE SLAB FLOOR(S)"]
["Range","Footings & Slabs","D53",null,{"$f":"$E$179","v":"THICKNESS:"}]
["Range","Footings & Slabs","B54",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Footings & Slabs","A55",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Footings & Slabs","B62",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Footings & Slabs","A63",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Footings & Slabs","B70",null,{"$f":"$E$187","v":"CONCRETE – 31-35 MPa"}]
["Range","Footings & Slabs","A71",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Footings & Slabs","A78",null,"OTHER SLAB FLOOR(S)"]
["Range","Footings & Slabs","B79",null,"EARTHEN FLOOR"]
["Range","Footings & Slabs","A81",null,"SUB-SLAB INSULATION"]
["Range","Footings & Slabs","B82",null,"EPS FOAM BOARD"]
["Range","Footings & Slabs","C83",null,"EPS foam board - AVERAGE"]
["Range","Footings & Slabs","B86",null,"XPS FOAM BOARD"]
["Range","Footings & Slabs","C87",null,"XPS foam board - AVERAGE",null,null,null,"New Aug"]
["Range","Footings & Slabs","B92",null,"MINERAL WOOL BOARD"]
["Range","Footings & Slabs","B94",null,"FOAMGLASS AGGREGATE"]
["Range","Footings & Slabs","C95",null,"Foam glass aggregate - AVERAGE"]
["Range","Footings & Slabs","B99",null,"FOAMGLASS BOARD"]
["Range","Footings & Slabs","C100",null,"Foam glass board - AVERAGE"]
["Range","Footings & Slabs","B103",null,"CORK BOARD"]
["Range","Footings & Slabs","A105",null,"BASEMENT FLOORING"]
["Range","Footings & Slabs","B106",null,"HARDWOOD FLOORING"]
["Range","Footings & Slabs","C107",null,"Hardwood flooring - AVERAGE"]
["Range","Footings & Slabs","B111",null,"LINOLEUM FLOORING"]
["Range","Footings & Slabs","C113",null,"Linoleum flooring - AVERAGE 2.5 mm"]
["Range","Footings & Slabs","B118",null,"TILE FLOORING"]
["Range","Footings & Slabs","C119",null,"Tile flooring - AVERAGE"]
["Range","Footings & Slabs","B125",null,"VINYL FLOORING"]
["Range","Footings & Slabs","C126",null,"Vinyl flooring - AVERAGE"]
["Range","Footings & Slabs","B133",null,"LAMINATE FLOORING"]
["Range","Footings & Slabs","B135",null,"CORK FLOORING"]
["Range","Footings & Slabs","B138",null,"CARPET"]
["Range","Footings & Slabs","B142",null,"FLOORING - VARIOUS"]
["Range","Foundation Walls","A1",null,"SECTION 2 ➜ COMPONENT MATERIALS FOR "]
["Range","Foundation Walls","D1",null,"FOUNDATION - WALLS"]
["Range","Foundation Walls","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Foundation Walls","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Foundation Walls","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Foundation Walls","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Foundation Walls","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Foundation Walls","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Foundation Walls","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Foundation Walls","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Foundation Walls","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Foundation Walls","M3",true,"kgCO2e SUBTOTAL FOR FOUNDATION WALLS"]
["Range","Foundation Walls","A5",null,"CONCRETE WALLS"]
["Range","Foundation Walls","D5",null,{"$f":"$E$179","v":"THICKNESS:"}]
["Range","Foundation Walls","B6",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Foundation Walls","A7",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Foundation Walls","B14",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Foundation Walls","A15",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Foundation Walls","B22",null,{"$f":"$E$187","v":"CONCRETE – 31-35 MPa"}]
["Range","Foundation Walls","A23",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Foundation Walls","A30",null,"MASONRY UNIT WALLS"]
["Range","Foundation Walls","B31",null,"CONCRETE MASONRY UNITS"]
["Range","Foundation Walls","A32",null,"If concrete grout and/or fill are being used for the CMU wall, be sure to add the volume of concrete separately."]
["Range","Foundation Walls","C32",null,"CMU Walls 8\" Hollow, No Grout - AVERAGE"]
["Range","Foundation Walls","A39",null,"TREATED WOOD FOUNDATION"]
["Range","Foundation Walls","A41",null,"CONTINUOUS INSULATION (Exterior and/or Interior)"]
["Range","Foundation Walls","B42",null,"EPS FOAM"]
["Range","Foundation Walls","C43",null,{"$f":"$E$212","v":"EPS foam board - AVERAGE"}]
["Range","Foundation Walls","B46",null,"XPS FOAM"]
["Range","Foundation Walls","C47",null,{"$f":"$E$214","v":"XPS foam board - AVERAGE"},null,null,null,"New Aug"]
["Range","Foundation Walls","B52",null,{"$f":"$E$215","v":"MINERAL WOOL BOARD"}]
["Range","Foundation Walls","C53",null,"Mineral wool board - light density – AVERAGE"]
["Range","Foundation Walls","B57",null,"WOOD FIBER BOARD"]
["Range","Foundation Walls","C58",null,"Wood fiber board - AVERAGE"]
["Range","Foundation Walls","B64",null,{"$f":"$E$220","v":"CORK BOARD"}]
["Range","Foundation Walls","B66",null,"SPRAY FOAM - CLOSED CELL"]
["Range","Foundation Walls","A70",null,"INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
["Range","Foundation Walls","A71",null,"Step 1: Select ICF size"]
["Range","Foundation Walls","B72",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Foundation Walls","A73",null,"Step 2: Select concrete fill option."]
["Range","Foundation Walls","B80",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Foundation Walls","A81",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Foundation Walls","B88",null,{"$f":"$E$187","v":"CONCRETE – 31-35 MPa"}]
["Range","Foundation Walls","A89",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Foundation Walls","A96",null,"INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
["Range","Foundation Walls","A97",null,{"$f":"$E$275","v":"Step 1: Select ICF size"}]
["Range","Foundation Walls","B101",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Foundation Walls","A102",true,"Step 2: Select concrete fill option for the ICF wall system. The quantity of concrete fill adapts to the form size selected."]
["-"]
["-"]
["-"]
["-"]
["-"]
["-"]
["Range","Foundation Walls","B109",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Foundation Walls","A110",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Foundation Walls","B117",null,{"$f":"$E$187","v":"CONCRETE – 31-35 MPa"}]
["Range","Foundation Walls","A118",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Foundation Walls","A125",null,"INTERIOR FRAMING - WOOD"]
["Range","Foundation Walls","D125",null,"FRAMING SPACING:"]
["Range","Foundation Walls","B126",null,"WOOD FRAME CONSTRUCTION"]
["Range","Foundation Walls","B130",null,"Double 2x4"]
["Range","Foundation Walls","A131",null,"INTERIOR FRAMING - STEEL"]
["Range","Foundation Walls","D131",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Foundation Walls","B132",null,"STEEL FRAMING, 2x4"]
["Range","Foundation Walls","A133",null,"Use % to adjust if heavier gauge steel studs will be used. Framing factor based on 10' wall."]
["Range","Foundation Walls","C133",null,"Steel Framing - AVERAGE"]
["Range","Foundation Walls","A138",null,"CAVITY INSULATION"]
["Range","Foundation Walls","B139",null,{"$f":"$E$273","v":"SPRAY FOAM - CLOSED CELL"}]
["Range","Foundation Walls","B143",null,"FIBERGLASS BATT"]
["Range","Foundation Walls","C144",null,"Fiberglass batt - Foundation Wall Insulation - AVERAGE"]
["Range","Foundation Walls","B148",null,"CELLULOSE INSULATION"]
["Range","Foundation Walls","C149",null,"Cellulose - Foundation Wall Insulation - AVERAGE"]
["Range","Foundation Walls","B153",null,"MINERAL WOOL BATT"]
["Range","Foundation Walls","C154",null,"Mineral wool batt - Foundation Wall Insulation - AVERAGE"]
["Range","Foundation Walls","B162",null,"WOOD FIBER BATT"]
["Range","Foundation Walls","C163",null,"Wood fiber batt - Foundation Wall Insulation - AVERAGE"]
["Range","Foundation Walls","B167",null,"OTHER NATURAL FIBER INSULATIONS"]
["Range","Foundation Walls","B171",null,"HEMPCRETE INSULATION"]
["Range","Foundation Walls","C172",null,"Hempcrete - Foundation Wall Insulation - AVERAGE"]
["Range","Foundation Walls","B176",null,"HIGH R-VALUE INSULATION"]
["Range","Foundation Walls","A179",null,"INTERIOR WALL CLADDING"]
["Range","Foundation Walls","B180",null,"DRYWALL 1/2\""]
["Range","Foundation Walls","C181",null,"Drywall 1/2\" - AVERAGE"]
["Range","Foundation Walls","B187",null,"DRYWALL 5/8\""]
["Range","Foundation Walls","B191",null,"OTHER CLADDING MATERIALS"]
["Range","Structural Elements","A1",null,"SECTION 3 ➜ COMPONENT MATERIALS FOR "]
["Range","Structural Elements","D1",null,"STRUCTURAL ELEMENTS"]
["Range","Structural Elements","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Structural Elements","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Structural Elements","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Structural Elements","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Structural Elements","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Structural Elements","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Structural Elements","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Structural Elements","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Structural Elements","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Structural Elements","M3",true,"kgCO2e SUBTOTAL FOR HEAVY STRUCTURE ELEMENTS"]
["Range","Structural Elements","A5",null,"HEAVY TIMBER FRAMING"]
["Range","Structural Elements","B6",null,"MASS TIMBER"]
["Range","Structural Elements","A7",null,"Use % function if multiple types of mass timber will be used."]
["Range","Structural Elements","C7",null,"Heavy Timber Framing - AVERAGE"]
["Range","Structural Elements","A14",null,"HEAVY STEEL COMPONENTS"]
["Range","Structural Elements","B15",null,"STEEL POSTS & BEAMS"]
["Range","Structural Elements","A16",null,"Select beam section from drop-down menu and input linear metres for each component type, as values do not come from User Input Sheet."]
["Range","Structural Elements","C16",null,"Steel Beam W Section – AVERAGE"]
["Range","Ext. Walls","A1",null,"SECTION 4 ➜ COMPONENT MATERIALS FOR "]
["Range","Ext. Walls","D1",null,"EXTERIOR WALLS"]
["Range","Ext. Walls","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Ext. Walls","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Ext. Walls","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Ext. Walls","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Ext. Walls","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Ext. Walls","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Ext. Walls","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Ext. Walls","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Ext. Walls","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Ext. Walls","M3",true,"kgCO2e SUBTOTAL FOR EXTERIOR WALLS"]
["Range","Ext. Walls","A5",null,"WOOD FRAME WALLS"]
["Range","Ext. Walls","D5",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Ext. Walls","F5",null,"in. o/c"]
["Range","Ext. Walls","B6",null,{"$f":"$E$298","v":"WOOD FRAME CONSTRUCTION"}]
["Range","Ext. Walls","B10",null,{"$f":"$E$299","v":"Double 2x4"}]
["Range","Ext. Walls","A11",null,"STEEL FRAME WALLS"]
["Range","Ext. Walls","D11",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Ext. Walls","F11",null,{"$f":"$E$366","v":"in. o/c"}]
["Range","Ext. Walls","B12",null,"STEEL FRAMING, 2x6"]
["Range","Ext. Walls","A13",null,"Use % function to adjust for other gauges of steel studs based on steel mass per unit length ratio."]
["Range","Ext. Walls","C13",null,"Steel Framing - Load bearing - AVERAGE"]
["Range","Ext. Walls","A19",null,"WOOD I-BEAM (TJI) FRAMING"]
["Range","Ext. Walls","D19",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Ext. Walls","F19",null,{"$f":"$E$366","v":"in. o/c"}]
["Range","Ext. Walls","A20",null,"Does not include any other framing members. To include these, use Wood Frame Construction section above to enter % of wall that is lumber."]
["Range","Ext. Walls","A22",null,"CROSS LAMINATED TIMBER WALLS - 3-1/2\" (90mm)"]
["Range","Ext. Walls","B23",null,"CROSS LAMINATED TIMBER"]
["Range","Ext. Walls","C24",null,"Cross Laminated Timber - AVERAGE"]
["Range","Ext. Walls","A25",null,"Use % function to adjust for other thicknesses of CLT panel."]
["Range","Ext. Walls","A28",null,"CONCRETE MASONRY UNIT WALLS"]
["Range","Ext. Walls","B29",null,"CMU 8\" – HOLLOW, NO GROUT"]
["Range","Ext. Walls","C30",null,"CMU 8\" – hollow, no grout - AVERAGE"]
["Range","Ext. Walls","A31",null,"Use % function to adjust for other thicknesses of CMU. If filled, enter fill volume in CONCRETE FILL for CMU WALLS below"]
["Range","Ext. Walls","A37",null,"CONCRETE FILL for CMU WALLS"]
["Range","Ext. Walls","D37",null,"CONCRETE VOLUME"]
["Range","Ext. Walls","B38",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Ext. Walls","A39",null,"Calculate the total concrete fill volume required for the CMU Wall area entered above."]
["Range","Ext. Walls","B46",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Ext. Walls","A47",null,{"$f":"$E$390","v":"Calculate the total concrete fill volume required for the CMU Wall area entered above."}]
["Range","Ext. Walls","A54",null,"STRUCTURAL SHEATHING"]
["Range","Ext. Walls","B55",null,"ORIENTED STRAND BOARD"]
["Range","Ext. Walls","B60",null,"PLYWOOD"]
["Range","Ext. Walls","B64",null,"GYPSUM STRUCTURAL SHEATHING"]
["Range","Ext. Walls","B68",null,"CEMENT BOARD"]
["Range","Ext. Walls","A71",null,{"$f":"$E$305","v":"CAVITY INSULATION"}]
["Range","Ext. Walls","B72",null,{"$f":"$E$307","v":"FIBERGLASS BATT"}]
["Range","Ext. Walls","C73",null,"Fiberglass batt - AVERAGE"]
["Range","Ext. Walls","B77",null,"FIBERGLASS BLOWN-IN"]
["Range","Ext. Walls","C78",null,"Fiberglass loose fill - AVERAGE"]
["Range","Ext. Walls","B83",null,{"$f":"$E$311","v":"MINERAL WOOL BATT"}]
["Range","Ext. Walls","B91",null,{"$f":"$E$309","v":"CELLULOSE INSULATION"}]
["Range","Ext. Walls","C92",null,"Cellulose - AVERAGE"]
["Range","Ext. Walls","B96",null,{"$f":"$E$313","v":"WOOD FIBER BATT"}]
["Range","Ext. Walls","C97",null,"Wood fiber batt - AVERAGE"]
["Range","Ext. Walls","B102",null,"OTHER NATURAL FIBER INSULATION"]
["Range","Ext. Walls","B108",null,"SPRAY FOAM, CLOSED CELL"]
["Range","Ext. Walls","B112",null,"SPRAY FOAM, OPEN CELL"]
["Range","Ext. Walls","B115",null,"HEMPCRETE"]
["Range","Ext. Walls","C116",null,"Hempcrete - AVERAGE"]
["Range","Ext. Walls","A120",null,"CONTINUOUS INSULATION (EXT. or INT.)"]
["Range","Ext. Walls","B121",null,{"$f":"$E$211","v":"EPS FOAM BOARD"}]
["Range","Ext. Walls","C122",null,{"$f":"$E$212","v":"EPS foam board - AVERAGE"}]
["Range","Ext. Walls","B125",null,{"$f":"$E$270","v":"WOOD FIBER BOARD"}]
["Range","Ext. Walls","C126",null,{"$f":"$E$271","v":"Wood fiber board - AVERAGE"}]
["Range","Ext. Walls","B132",null,{"$f":"$E$213","v":"XPS FOAM BOARD"}]
["Range","Ext. Walls","C133",null,{"$f":"$E$214","v":"XPS foam board - AVERAGE"}]
["Range","Ext. Walls","B138",null,"POLYISOCYANURATE FOAM BOARD"]
["Range","Ext. Walls","C139",null,"Polyisocyanurate - AVERAGE"]
["Range","Ext. Walls","B144",null,{"$f":"$E$215","v":"MINERAL WOOL BOARD"}]
["Range","Ext. Walls","C145",null,"Mineral wool board - AVERAGE"]
["Range","Ext. Walls","A149",null,"HIGH R-VALUE INSULATIONS"]
["Range","Ext. Wall Systems","A1",null,"SECTION 5 ➜ COMPONENT MATERIALS FOR "]
["Range","Ext. Wall Systems","D1",null,"EXTERIOR WALL SYSTEMS"]
["Range","Ext. Wall Systems","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Ext. Wall Systems","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Ext. Wall Systems","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Ext. Wall Systems","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Ext. Wall Systems","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Ext. Wall Systems","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Ext. Wall Systems","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Ext. Wall Systems","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Ext. Wall Systems","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Ext. Wall Systems","M3",true,"kgCO2e SUBTOTAL FOR EXTERIOR WALL SYSTEMS"]
["Range","Ext. Wall Systems","A5",null,{"$f":"$E$274","v":"INSULATED CONCRETE FORMS (ICF) - EPS FOAM"}]
["Range","Ext. Wall Systems","A6",null,{"$f":"$E$275","v":"Step 1: Select ICF size"}]
["Range","Ext. Wall Systems","B7",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Ext. Wall Systems","A8",null,{"$f":"$E$277","v":"Step 2: Select concrete fill option."}]
["Range","Ext. Wall Systems","B15",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Ext. Wall Systems","A16",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Ext. Wall Systems","B23",null,{"$f":"$E$187","v":"CONCRETE – 31-35 MPa"}]
["Range","Ext. Wall Systems","A24",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Ext. Wall Systems","A31",null,{"$f":"$E$282","v":"INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"}]
["Range","Ext. Wall Systems","A32",null,"Step 1: Select ICF size and insulation"]
["Range","Ext. Wall Systems","B36",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Ext. Wall Systems","A37",true,"Step 2: Select concrete fill option for the ICF wall system. The quantity of concrete adapts to the ICF selected."]
["-"]
["-"]
["-"]
["-"]
["-"]
["-"]
["Range","Ext. Wall Systems","B44",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Ext. Wall Systems","A45",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Ext. Wall Systems","B52",null,{"$f":"$E$187","v":"CONCRETE – 31-35 MPa"}]
["Range","Ext. Wall Systems","A53",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Ext. Wall Systems","A60",null,"PREFABRICATED PANELS"]
["Range","Ext. Wall Systems","B61",null,"WOOD FRAME & STRAW PANELS"]
["Range","Ext. Wall Systems","B64",null,"SIP PANELS - OSB & EPS FOAM"]
["Range","Party Walls","A1",null,"SECTION 6 ➜ COMPONENT MATERIALS FOR "]
["Range","Party Walls","D1",null,"PARTY WALLS"]
["Range","Party Walls","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Party Walls","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Party Walls","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Party Walls","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Party Walls","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Party Walls","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Party Walls","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Party Walls","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Party Walls","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Party Walls","M3",true,"kgCO2e SUBTOTAL FOR PARTY WALLS"]
["Range","Party Walls","A5",true,"Note: only include half the thickness of total party wall materials using either the percentage or R-value fields. (The other half belongs to the adjacent building.) "]
["Range","Party Walls","A6",null,"PARTY WALL FRAMING"]
["Range","Party Walls","A7",null,{"$f":"$E$364","v":"WOOD FRAME WALLS"}]
["Range","Party Walls","D7",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Party Walls","B8",null,{"$f":"$E$298","v":"WOOD FRAME CONSTRUCTION"}]
["Range","Party Walls","B12",null,{"$f":"$E$299","v":"Double 2x4"}]
["Range","Party Walls","A13",null,{"$f":"$E$369","v":"STEEL FRAME WALLS"}]
["Range","Party Walls","D13",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Party Walls","B14",null,{"$f":"$E$302","v":"STEEL FRAMING, 2x4"}]
["Range","Party Walls","C15",null,"Steel Framing - Interior Walls - AVERAGE"]
["Range","Party Walls","A16",null,"Use % function to adjust for different gauges of steel studs."]
["Range","Party Walls","B21",null,{"$f":"$E$372","v":"STEEL FRAMING, 2x6"}]
["Range","Party Walls","A22",null,"Use % function to adjust for other gauges of steel studs."]
["Range","Party Walls","C22",null,{"$f":"$E$374","v":"Steel Framing - Load bearing - AVERAGE"}]
["Range","Party Walls","A28",null,"CONCRETE MASONRY UNIT PARTY WALLS"]
["Range","Party Walls","A29",null,"CMU PARTY WALLS"]
["Range","Party Walls","B30",null,"CMU 8\" - HOLLOW, NO GROUT"]
["Range","Party Walls","C31",null,"Concrete Masonry Units -  AVERAGE"]
["Range","Party Walls","A32",null,"Use % function to adjust for other thicknesses of CMU."]
["Range","Party Walls","A38",null,"CMU WALL CONCRETE FILL"]
["Range","Party Walls","D38",null,"CONCRETE FILL VOLUME"]
["Range","Party Walls","B39",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Party Walls","A40",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Party Walls","B47",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Party Walls","A48",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Party Walls","A55",null,"PARTY WALL INSULATION"]
["Range","Party Walls","A56",null,{"$f":"$E$305","v":"CAVITY INSULATION"}]
["Range","Party Walls","B57",null,{"$f":"$E$307","v":"FIBERGLASS BATT"}]
["Range","Party Walls","C58",null,{"$f":"$E$400","v":"Fiberglass batt - AVERAGE"}]
["Range","Party Walls","B62",null,{"$f":"$E$401","v":"FIBERGLASS BLOWN-IN"}]
["Range","Party Walls","C63",null,{"$f":"$E$402","v":"Fiberglass loose fill - AVERAGE"}]
["Range","Party Walls","B68",null,{"$f":"$E$311","v":"MINERAL WOOL BATT"}]
["Range","Party Walls","B76",null,{"$f":"$E$309","v":"CELLULOSE INSULATION"}]
["Range","Party Walls","C77",null,{"$f":"$E$405","v":"Cellulose - AVERAGE"}]
["Range","Party Walls","B81",null,{"$f":"$E$313","v":"WOOD FIBER BATT"}]
["Range","Party Walls","C82",null,{"$f":"$E$407","v":"Wood fiber batt - AVERAGE"}]
["Range","Party Walls","B87",null,{"$f":"$E$408","v":"OTHER NATURAL FIBER INSULATION"}]
["Range","Party Walls","B93",null,{"$f":"$E$409","v":"SPRAY FOAM, CLOSED CELL"}]
["Range","Party Walls","B97",null,{"$f":"$E$410","v":"SPRAY FOAM, OPEN CELL"}]
["Range","Party Walls","B100",null,{"$f":"$E$411","v":"HEMPCRETE"}]
["Range","Party Walls","C101",null,{"$f":"$E$412","v":"Hempcrete - AVERAGE"}]
["Range","Party Walls","A105",null,"RIGID INSULATION"]
["Range","Party Walls","B106",null,{"$f":"$E$211","v":"EPS FOAM BOARD"}]
["Range","Party Walls","C107",null,{"$f":"$E$212","v":"EPS foam board - AVERAGE"}]
["Range","Party Walls","B110",null,{"$f":"$E$270","v":"WOOD FIBER BOARD"}]
["Range","Party Walls","C111",null,{"$f":"$E$271","v":"Wood fiber board - AVERAGE"}]
["Range","Party Walls","B117",null,{"$f":"$E$213","v":"XPS FOAM BOARD"}]
["Range","Party Walls","C118",null,{"$f":"$E$214","v":"XPS foam board - AVERAGE"}]
["Range","Party Walls","B123",null,{"$f":"$E$420","v":"POLYISOCYANURATE FOAM BOARD"}]
["Range","Party Walls","C124",null,{"$f":"$E$421","v":"Polyisocyanurate - AVERAGE"}]
["Range","Party Walls","B129",null,{"$f":"$E$215","v":"MINERAL WOOL BOARD"}]
["Range","Party Walls","C130",null,{"$f":"$E$423","v":"Mineral wool board - AVERAGE"}]
["Range","Party Walls","A134",null,"PARTY WALL SHEETING"]
["Range","Party Walls","A135",null,"INTERIOR CLADDING for PARTY WALLS"]
["Range","Party Walls","B136",null,{"$f":"$E$320","v":"DRYWALL 1/2\""}]
["Range","Party Walls","C137",null,"Drywall 1/2\" Typical - Interior Cladding for Exterior Walls - AVERAGE"]
["Range","Party Walls","B143",null,{"$f":"$E$322","v":"DRYWALL 5/8\""}]
["Range","Party Walls","B147",null,{"$f":"$E$323","v":"OTHER CLADDING MATERIALS"}]
["Range","Party Walls","A158",null,{"$f":"$E$393","v":"STRUCTURAL SHEATHING"}]
["Range","Party Walls","B159",null,{"$f":"$E$394","v":"ORIENTED STRAND BOARD"}]
["Range","Party Walls","B164",null,{"$f":"$E$395","v":"PLYWOOD"}]
["Range","Party Walls","B168",null,{"$f":"$E$396","v":"GYPSUM STRUCTURAL SHEATHING"}]
["Range","Party Walls","B172",null,{"$f":"$E$397","v":"CEMENT BOARD"}]
["Range","Party Walls","A175",null,"PARTY WALL ICFs"]
["Range","Party Walls","A176",null,{"$f":"$E$274","v":"INSULATED CONCRETE FORMS (ICF) - EPS FOAM"}]
["Range","Party Walls","A177",null,{"$f":"$E$275","v":"Step 1: Select ICF size"}]
["Range","Party Walls","B178",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Party Walls","A179",null,{"$f":"$E$277","v":"Step 2: Select concrete fill option."}]
["Range","Party Walls","B186",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Party Walls","A187",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Party Walls","B194",null,{"$f":"$E$187","v":"CONCRETE – 31-35 MPa"}]
["Range","Party Walls","A195",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Party Walls","A202",null,{"$f":"$E$282","v":"INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"}]
["Range","Party Walls","A203",null,{"$f":"$E$450","v":"Step 1: Select ICF size and insulation"}]
["Range","Party Walls","B207",null,{"$f":"$E$451","v":"CONCRETE – 25 MPa or less"}]
["Range","Party Walls","A208",true,{"$f":"$E$452","v":"Step 2: Select concrete fill option for the ICF wall system. The quantity of concrete adapts to the ICF selected."}]
["-"]
["-"]
["-"]
["-"]
["-"]
["Range","Party Walls","B215",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Party Walls","A216",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Party Walls","B223",null,{"$f":"$E$187","v":"CONCRETE – 31-35 MPa"}]
["Range","Party Walls","A224",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Cladding","A1",null,"SECTION 7 ➜ COMPONENT MATERIALS FOR "]
["Range","Cladding","D1",null,"EXTERIOR WALLS - CLADDING"]
["Range","Cladding","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Cladding","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Cladding","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Cladding","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Cladding","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Cladding","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Cladding","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Cladding","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Cladding","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Cladding","M3",true,"kgCO2e SUBTOTAL FOR EXTERIOR WALLS CLADDING"]
["Range","Cladding","A5",null,"EXTERIOR CLADDING"]
["Range","Cladding","B6",null,"BRICK"]
["Range","Cladding","B14",null,"WOOD CLADDING"]
["Range","Cladding","B17",null,"FIBER CEMENT"]
["Range","Cladding","C18",null,"Fiber Cement siding - AVERAGE"]
["Range","Cladding","B27",null,"VINYL SIDING"]
["Range","Cladding","B29",null,"POLYPROPYLENE SIDING"]
["Range","Cladding","C30",null,"Polypropylene siding - AVERAGE"]
["Range","Cladding","B33",null,"STEEL PANEL SIDING"]
["Range","Cladding","C34",null,"Steel Panel Siding - AVERAGE"]
["Range","Cladding","B41",null,"ALUMINUM PANEL SIDING"]
["Range","Cladding","C42",null,"Aluminum Panel Siding - AVERAGE"]
["Range","Cladding","B45",null,"PLASTER FINISHES"]
["Range","Cladding","B50",null,"ENGINEERED WOOD SIDING",null,null,null,"New Aug"]
["Range","Cladding","A54",null,"STRAPPING for RAIN SCREEN"]
["Range","Cladding","D54",null,"STRAPPING SPACING:"]
["Range","Cladding","A57",null,"INTERIOR CLADDING for EXTERIOR WALLS"]
["Range","Cladding","B58",null,{"$f":"$E$320","v":"DRYWALL 1/2\""}]
["Range","Cladding","C59",null,{"$f":"$E$537","v":"Drywall 1/2\" Typical - Interior Cladding for Exterior Walls - AVERAGE"}]
["Range","Cladding","B65",null,{"$f":"$E$322","v":"DRYWALL 5/8\""}]
["Range","Cladding","B69",null,{"$f":"$E$323","v":"OTHER CLADDING MATERIALS"}]
["Range","Windows","A1",null,"SECTION 8 ➜ COMPONENT MATERIALS FOR "]
["Range","Windows","D1",null,"WINDOWS"]
["Range","Windows","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Windows","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Windows","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Windows","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Windows","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Windows","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Windows","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Windows","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Windows","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Windows","M3",true,"kgCO2e SUBTOTAL FOR WINDOWS"]
["Range","Windows","A5",null,"DOUBLE PANE WINDOWS"]
["Range","Windows","A12",null,"TRIPLE PANE WINDOWS"]
["Range","Windows","A19",null,"WINDOWS - SPECIFIC MANUFACTURERS"]
["Range","Int. Walls","A1",null,"SECTION 9 ➜ COMPONENT MATERIALS FOR "]
["Range","Int. Walls","D1",null,"INTERIOR WALLS"]
["Range","Int. Walls","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Int. Walls","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Int. Walls","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Int. Walls","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Int. Walls","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Int. Walls","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Int. Walls","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Int. Walls","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Int. Walls","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Int. Walls","M3",true,"kgCO2e SUBTOTAL FOR INTERIOR WALLS"]
["Range","Int. Walls","A5",null,{"$f":"$E$298","v":"WOOD FRAME CONSTRUCTION"}]
["Range","Int. Walls","D5",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Int. Walls","B6",null,{"$f":"$E$298","v":"WOOD FRAME CONSTRUCTION"}]
["Range","Int. Walls","A10",null,"STEEL FRAME CONSTRUCTION"]
["Range","Int. Walls","D10",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Int. Walls","B11",null,{"$f":"$E$302","v":"STEEL FRAMING, 2x4"}]
["Range","Int. Walls","C12",null,{"$f":"$E$491","v":"Steel Framing - Interior Walls - AVERAGE"}]
["Range","Int. Walls","A13",null,{"$f":"$E$492","v":"Use % function to adjust for different gauges of steel studs."}]
["Range","Int. Walls","A18",null,{"$f":"$E$319","v":"INTERIOR WALL CLADDING"}]
["Range","Int. Walls","B19",null,{"$f":"$E$320","v":"DRYWALL 1/2\""}]
["Range","Int. Walls","C20",null,"Drywall 1/2\" Typical - Interior Walls - AVERAGE"]
["Range","Int. Walls","B26",null,{"$f":"$E$322","v":"DRYWALL 5/8\""}]
["Range","Int. Walls","B30",null,{"$f":"$E$323","v":"OTHER CLADDING MATERIALS"}]
["Range","Int. Walls","A41",null,{"$f":"$E$305","v":"CAVITY INSULATION"}]
["Range","Int. Walls","B42",null,{"$f":"$E$307","v":"FIBERGLASS BATT"}]
["Range","Int. Walls","C43",null,{"$f":"$E$400","v":"Fiberglass batt - AVERAGE"}]
["Range","Int. Walls","B47",null,{"$f":"$E$401","v":"FIBERGLASS BLOWN-IN"}]
["Range","Int. Walls","C48",null,{"$f":"$E$402","v":"Fiberglass loose fill - AVERAGE"}]
["Range","Int. Walls","B53",null,{"$f":"$E$311","v":"MINERAL WOOL BATT"}]
["Range","Int. Walls","B61",null,{"$f":"$E$309","v":"CELLULOSE INSULATION"}]
["Range","Int. Walls","C62",null,{"$f":"$E$405","v":"Cellulose - AVERAGE"}]
["Range","Int. Walls","B66",null,{"$f":"$E$313","v":"WOOD FIBER BATT"}]
["Range","Int. Walls","C67",null,{"$f":"$E$407","v":"Wood fiber batt - AVERAGE"}]
["Range","Int. Walls","B72",null,{"$f":"$E$408","v":"OTHER NATURAL FIBER INSULATION"}]
["Range","Int. Walls","B78",null,{"$f":"$E$409","v":"SPRAY FOAM, CLOSED CELL"}]
["Range","Int. Walls","B82",null,{"$f":"$E$410","v":"SPRAY FOAM, OPEN CELL"}]
["Range","Int. Walls","B85",null,{"$f":"$E$411","v":"HEMPCRETE"}]
["Range","Int. Walls","C86",null,{"$f":"$E$412","v":"Hempcrete - AVERAGE"}]
["Range","Floors","A1",null,"SECTION 10 ➜ COMPONENT MATERIALS FOR "]
["Range","Floors","D1",null,"FLOORS"]
["Range","Floors","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Floors","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Floors","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Floors","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Floors","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Floors","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Floors","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Floors","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Floors","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Floors","M3",true,"kgCO2e SUBTOTAL FOR FLOORS"]
["Range","Floors","A5",null,"WOOD FLOOR FRAMING"]
["Range","Floors","D5",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Floors","B6",null,"WOOD LUMBER FRAMING"]
["Range","Floors","B10",null,"WOOD I-JOIST FRAMING"]
["Range","Floors","B11",null,"9-1/2\""]
["Range","Floors","B14",null,"WOOD TRUSS FRAMING"]
["Range","Floors","A16",null,"STEEL FLOOR FRAMING"]
["Range","Floors","D16",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Floors","B17",null,"OPEN WEB STEEL JOIST"]
["Range","Floors","A19",null,"SUBFLOORING"]
["Range","Floors","A26",null,"CROSS-LAMINATED TIMBER"]
["Range","Floors","B27",null,"CLT FLOOR SYSTEM"]
["Range","Floors","C28",null,"CLT Floor System – 3-1/2\" (90 mm) AVERAGE"]
["Range","Floors","A32",null,"CLAY-BASED FLOOR SYSTEM"]
["Range","Floors","B33",null,{"$f":"$E$209","v":"EARTHEN FLOOR"}]
["Range","Floors","A35",null,"FINISHED FLOORING"]
["Range","Floors","B36",null,"HARDWOOD 3/4\""]
["Range","Floors","C37",null,{"$f":"$E$223","v":"Hardwood flooring - AVERAGE"}]
["Range","Floors","B41",null,{"$f":"$E$224","v":"LINOLEUM FLOORING"}]
["Range","Floors","C42",null,"Linoleum flooring - AVERAGE"]
["Range","Floors","B48",null,{"$f":"$E$226","v":"TILE FLOORING"}]
["Range","Floors","C49",null,"Ceramic tile flooring - AVERAGE"]
["Range","Floors","B55",null,{"$f":"$E$228","v":"VINYL FLOORING"}]
["Range","Floors","C56",null,{"$f":"$E$229","v":"Vinyl flooring - AVERAGE"}]
["Range","Floors","B63",null,{"$f":"$E$230","v":"LAMINATE FLOORING"}]
["Range","Floors","B65",null,{"$f":"$E$231","v":"CORK FLOORING"}]
["Range","Floors","B68",null,{"$f":"$E$232","v":"CARPET"}]
["Range","Floors","B72",null,"OTHER FLOORING OPTIONS"]
["Range","Floors","A76",null,"FLOOR CAVITY INSULATION"]
["Range","Floors","B77",null,{"$f":"$E$307","v":"FIBERGLASS BATT"}]
["Range","Floors","C78",null,"Fiberglass batt - Floor Insulation - AVERAGE"]
["Range","Floors","B82",null,"FIBERGLASS LOOSE FILL"]
["Range","Floors","C83",null,"Fiberglass loose fill - Floor Insulation - AVERAGE"]
["Range","Floors","B88",null,{"$f":"$E$311","v":"MINERAL WOOL BATT"}]
["Range","Floors","C89",null,"Mineral wool batt - Floor Insulation - AVERAGE"]
["Range","Floors","B97",null,"MINERAL WOOL LOOSE FILL"]
["Range","Floors","B99",null,{"$f":"$E$409","v":"SPRAY FOAM, CLOSED CELL"}]
["Range","Floors","B103",null,{"$f":"$E$410","v":"SPRAY FOAM, OPEN CELL"}]
["Range","Floors","B106",null,{"$f":"$E$309","v":"CELLULOSE INSULATION"}]
["Range","Floors","C107",null,"Cellulose - Floor Insulation - AVERAGE"]
["Range","Floors","B112",null,{"$f":"$E$313","v":"WOOD FIBER BATT"}]
["Range","Floors","C113",null,"Wood fiber batt - Floor Insulation - AVERAGE"]
["Range","Floors","B117",null,{"$f":"$E$408","v":"OTHER NATURAL FIBER INSULATION"}]
["Range","Floors","B124",null,"HEMPCRETE LOOSE FILL"]
["Range","Floors","C125",null,"Hempcrete - Floor Insulation - AVERAGE"]
["Range","Ceilings","A1",null,"SECTION 11 ➜ COMPONENT MATERIALS FOR "]
["Range","Ceilings","D1",null,"CEILINGS"]
["Range","Ceilings","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Ceilings","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Ceilings","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Ceilings","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Ceilings","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Ceilings","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Ceilings","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Ceilings","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Ceilings","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Ceilings","M3",true,"kgCO2e SUBTOTAL FOR CEILINGS"]
["Range","Ceilings","A5",null,"CEILING FINISHES"]
["Range","Ceilings","B6",null,{"$f":"$E$320","v":"DRYWALL 1/2\""}]
["Range","Ceilings","C7",null,"Drywall 1/2\" - Ceilings - AVERAGE"]
["Range","Ceilings","B13",null,{"$f":"$E$322","v":"DRYWALL 5/8\""}]
["Range","Ceilings","C14",null,"Drywall 5/8\" - Ceilings - AVERAGE"]
["Range","Ceilings","B18",null,"OTHER CEILING FINISHES"]
["Range","Roof","A1",null,"SECTION 12 ➜ COMPONENT MATERIALS FOR "]
["Range","Roof","D1",null,"ROOF"]
["Range","Roof","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Roof","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Roof","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Roof","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Roof","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Roof","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Roof","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Roof","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Roof","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Roof","M3",true,"kgCO2e SUBTOTAL FOR ROOF"]
["Range","Roof","A5",null,"WOOD FRAME ROOF"]
["Range","Roof","D5",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Roof","B6",null,"WOOD FRAMING"]
["Range","Roof","B12",null,{"$f":"$E$688","v":"WOOD TRUSS FRAMING"}]
["Range","Roof","A13",null,"Use percent function to adjust wood volume relative to described roof design"]
["Range","Roof","B14",null,{"$f":"$E$686","v":"WOOD I-JOIST FRAMING"}]
["Range","Roof","A19",null,"ROOF DECKING"]
["Range","Roof","B20",null,"WOOD SHEET PRODUCTS - 5/8\""]
["Range","Roof","B23",null,"GYPSUM PANELS 1/2\""]
["Range","Roof","A27",null,"ROOFING MEMBRANE"]
["Range","Roof","B28",null,{"$f":"$E$775","v":"ROOFING MEMBRANE"}]
["Range","Roof","A33",null,"ROOF STRAPPING"]
["Range","Roof","D33",null,{"$f":"$E$598","v":"STRAPPING SPACING:"}]
["Range","Roof","B34",null,"WOOD STRAPPING"]
["Range","Roof","A38",null,"ROOFING"]
["Range","Roof","B39",null,"ASPHALT SHINGLES"]
["Range","Roof","C40",null,"Asphalt Shingles - Roofing - AVERAGE"]
["Range","Roof","B47",null,"STEEL PANELS"]
["Range","Roof","C48",null,"Steel Panels - Roofing - AVERAGE"]
["Range","Roof","B54",null,"ALUMINUM PANELS"]
["Range","Roof","C55",null,"Aluminum l Panels - Roofing - AVERAGE"]
["Range","Roof","B58",null,"FIBER CEMENT ROOFING"]
["Range","Roof","C59",null,"Fiber Cement roofing - AVERAGE"]
["Range","Roof","B63",null,"OTHER ROOFING OPTIONS"]
["Range","Roof","A65",null,"ROOF CAVITY INSULATION"]
["Range","Roof","F65",null,"INSULATION PARALLEL TO:"]
["Range","Roof","I65",null,"Ceiling surface"]
["Range","Roof","B66",null,{"$f":"$E$307","v":"FIBERGLASS BATT"}]
["Range","Roof","C67",null,"Fiberglass batt - Roof Insulation - AVERAGE"]
["Range","Roof","B71",null,{"$f":"$E$714","v":"FIBERGLASS LOOSE FILL"}]
["Range","Roof","C72",null,"Fiberglass loose fill - Roof Insulation - AVERAGE"]
["Range","Roof","B77",null,{"$f":"$E$311","v":"MINERAL WOOL BATT"}]
["Range","Roof","C78",null,"Mineral wool batt - Roof Insulation - AVERAGE"]
["Range","Roof","B86",null,{"$f":"$E$718","v":"MINERAL WOOL LOOSE FILL"}]
["Range","Roof","B88",null,{"$f":"$E$409","v":"SPRAY FOAM, CLOSED CELL"}]
["Range","Roof","B92",null,{"$f":"$E$410","v":"SPRAY FOAM, OPEN CELL"}]
["Range","Roof","B95",null,{"$f":"$E$309","v":"CELLULOSE INSULATION"}]
["Range","Roof","C96",null,"Cellulose - Roof Insulation - AVERAGE"]
["Range","Roof","B101",null,{"$f":"$E$313","v":"WOOD FIBER BATT"}]
["Range","Roof","C102",null,"Wood fiber batt - Roof Insulation - AVERAGE"]
["Range","Roof","B106",null,{"$f":"$E$408","v":"OTHER NATURAL FIBER INSULATION"}]
["Range","Roof","B113",null,{"$f":"$E$726","v":"HEMPCRETE LOOSE FILL"}]
["Range","Roof","C114",null,"Hempcrete - Roof Insulation - AVERAGE"]
["Range","Roof","B117",null,{"$f":"$E$318","v":"HIGH R-VALUE INSULATION"}]
["Range","Roof","A120",null,"RIGID ROOF INSULATION"]
["Range","Roof","F120",null,{"$f":"$E$791","v":"INSULATION PARALLEL TO:"}]
["Range","Roof","I120",null,"Roof surface"]
["Range","Roof","B121",null,{"$f":"$E$211","v":"EPS FOAM BOARD"}]
["Range","Roof","C122",null,{"$f":"$E$212","v":"EPS foam board - AVERAGE"}]
["Range","Roof","B125",null,{"$f":"$E$270","v":"WOOD FIBER BOARD"}]
["Range","Roof","C126",null,{"$f":"$E$271","v":"Wood fiber board - AVERAGE"}]
["Range","Roof","B132",null,{"$f":"$E$213","v":"XPS FOAM BOARD"}]
["Range","Roof","C133",null,{"$f":"$E$214","v":"XPS foam board - AVERAGE"}]
["Range","Roof","B138",null,{"$f":"$E$420","v":"POLYISOCYANURATE FOAM BOARD"}]
["Range","Roof","C139",null,{"$f":"$E$421","v":"Polyisocyanurate - AVERAGE"}]
["Range","Roof","B144",null,{"$f":"$E$215","v":"MINERAL WOOL BOARD"}]
["Range","Roof","C145",null,{"$f":"$E$423","v":"Mineral wool board - AVERAGE"}]
["Range","Roof","A149",null,"INSULATED ROOFING PANELS"]
["Range","Roof","B150",null,"SIP PANEL - EPS FOAM CORE with OSB"]
["Range","Roof","C151",null,"SIP panel - Roof - AVERAGE"]
["Range","Garage","A1",null,"SECTION 13 ➜ COMPONENT MATERIALS FOR "]
["Range","Garage","D1",null,{"$f":"$E$119","v":"GARAGE"}]
["Range","Garage","A2",true,{"$f":"$E$164","v":"INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."}]
["Range","Garage","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","Garage","C3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Garage","D3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","Garage","H3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","Garage","I3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","Garage","J3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","Garage","K3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","Garage","L3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","Garage","M3",true,"kgCO2e SUBTOTAL FOR GARAGE"]
["Range","Garage","A5",null,"GARAGE FOOTINGS & SLABS"]
["Range","Garage","A6",null,{"$f":"$E$178","v":"CRUSHED STONE BASE"}]
["Range","Garage","D6",null,{"$f":"$E$179","v":"THICKNESS:"}]
["Range","Garage","B7",null,{"$f":"$E$180","v":"AGGREGATE"}]
["Range","Garage","A8",null,{"$f":"$E$181","v":"If you do not know the specific carbon footprint of your aggregate, chose the \"AVERAGE\" value"}]
["Range","Garage","A13",null,"CONCRETE SLAB FLOOR"]
["Range","Garage","D13",null,{"$f":"$E$179","v":"THICKNESS:"}]
["Range","Garage","B14",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Garage","A15",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Garage","B22",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Garage","A23",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Garage","A30",null,"SLAB REINFORCING MESH"]
["Range","Garage","D30",null,{"$f":"$E$194","v":"CUSTOM AREA:"}]
["Range","Garage","B31",null,"WELDED WIRE MESH (WWM)"]
["Range","Garage","A33",null,{"$f":"$E$182","v":"FOOTINGS, PIERS & PADS"}]
["Range","Garage","B34",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Garage","A35",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Garage","B42",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Garage","A43",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Garage","A50",null,{"$f":"$E$189","v":"REBAR"}]
["Range","Garage","D50",null,"CUSTOM LENGTH:"]
["Range","Garage","B51",null,{"$f":"$E$191","v":"CONCRETE REINFORCING BAR"}]
["Range","Garage","A52",null,{"$f":"$E$192","v":"Specify an overall rebar length."}]
["Range","Garage","A60",null,{"$f":"$E$196","v":"HELICAL PIERS"}]
["Range","Garage","D60",null,{"$f":"$E$197","v":"TOTAL LENGTH OF ALL PIERS:"}]
["Range","Garage","B61",null,{"$f":"$E$196","v":"HELICAL PIERS"}]
["Range","Garage","A62",null,{"$f":"$E$199","v":"Specify the total length of all piers. Use % to adjust for different sized piers"}]
["Range","Garage","A63",null,"GARAGE FOUNDATION WALLS"]
["Range","Garage","A64",null,"CONCRETE FOUNDATION WALLS"]
["Range","Garage","D64",null,{"$f":"$E$179","v":"THICKNESS:"}]
["Range","Garage","B65",null,{"$f":"$E$183","v":"CONCRETE – 25 MPa or less"}]
["Range","Garage","A66",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Garage","B73",null,{"$f":"$E$185","v":"CONCRETE – 26-30 MPa"}]
["Range","Garage","A74",null,{"$f":"$E$184","v":"Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier."}]
["Range","Garage","A81",null,"CMU FOUNDATION WALLS"]
["Range","Garage","B82",null,{"$f":"$E$259","v":"CONCRETE MASONRY UNITS"}]
["Range","Garage","A83",null,"If concrete grout is being used in the CMU wall use the concrete wall area to specify the quantity of concrete fill being used in the CMUs."]
["Range","Garage","C83",null,"CMU Walls 8\" Hollow, no grout - AVERAGE"]
["Range","Garage","A90",null,"GARAGE HEAVY STRUCTURAL ELEMENTS"]
["Range","Garage","A91",null,"MASS TIMBER FRAMING"]
["Range","Garage","B92",null,{"$f":"$E$341","v":"MASS TIMBER"}]
["Range","Garage","A93",null,{"$f":"$E$342","v":"Use % function if multiple types of mass timber will be used."}]
["Range","Garage","C93",null,{"$f":"$E$343","v":"Heavy Timber Framing - AVERAGE"}]
["Range","Garage","A100",null,{"$f":"$E$344","v":"HEAVY STEEL COMPONENTS"}]
["Range","Garage","B101",null,{"$f":"$E$345","v":"STEEL POSTS & BEAMS"}]
["Range","Garage","A102",null,"Choose steel beam section from drop-down menu and input linear metres for each component type, as values do not come from User Input Sheet."]
["Range","Garage","C102",null,{"$f":"$E$347","v":"Steel Beam W Section – AVERAGE"}]
["Range","Garage","A105",null,"GARAGE EXTERIOR WALLS"]
["Range","Garage","A106",null,{"$f":"$E$298","v":"WOOD FRAME CONSTRUCTION"}]
["Range","Garage","D106",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Garage","B107",null,{"$f":"$E$298","v":"WOOD FRAME CONSTRUCTION"}]
["Range","Garage","B111",null,{"$f":"$E$299","v":"Double 2x4"}]
["Range","Garage","A112",null,{"$f":"$E$642","v":"STEEL FRAME CONSTRUCTION"}]
["Range","Garage","D112",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Garage","B113",null,{"$f":"$E$372","v":"STEEL FRAMING, 2x6"}]
["Range","Garage","A114",null,{"$f":"$E$494","v":"Use % function to adjust for other gauges of steel studs."}]
["Range","Garage","C114",null,{"$f":"$E$374","v":"Steel Framing - Load bearing - AVERAGE"}]
["Range","Garage","B120",null,{"$f":"$E$302","v":"STEEL FRAMING, 2x4"}]
["Range","Garage","C121",null,{"$f":"$E$491","v":"Steel Framing - Interior Walls - AVERAGE"}]
["Range","Garage","A122",null,{"$f":"$E$492","v":"Use % function to adjust for different gauges of steel studs."}]
["Range","Garage","A127",null,{"$f":"$E$393","v":"STRUCTURAL SHEATHING"}]
["Range","Garage","B128",null,{"$f":"$E$394","v":"ORIENTED STRAND BOARD"}]
["Range","Garage","B133",null,{"$f":"$E$395","v":"PLYWOOD"}]
["Range","Garage","B137",null,{"$f":"$E$396","v":"GYPSUM STRUCTURAL SHEATHING"}]
["Range","Garage","A141",null,"CMU EXTERIOR WALLS"]
["Range","Garage","B142",null,"CMU 8\""]
["Range","Garage","C143",null,"Concrete Masonry Units - AVERAGE"]
["Range","Garage","A144",null,{"$f":"$E$500","v":"Use % function to adjust for other thicknesses of CMU."}]
["Range","Garage","A150",null,"EXTERIOR GARAGE WALL CAVITY INSULATION"]
["Range","Garage","G150",null,"(Excludes attachment wall area, specified separately in section below)"]
["Range","Garage","B151",null,{"$f":"$E$307","v":"FIBERGLASS BATT"}]
["Range","Garage","C152",null,{"$f":"$E$400","v":"Fiberglass batt - AVERAGE"}]
["Range","Garage","B156",null,{"$f":"$E$401","v":"FIBERGLASS BLOWN-IN"}]
["Range","Garage","C157",null,{"$f":"$E$402","v":"Fiberglass loose fill - AVERAGE"}]
["Range","Garage","B162",null,{"$f":"$E$311","v":"MINERAL WOOL BATT"}]
["Range","Garage","B170",null,{"$f":"$E$309","v":"CELLULOSE INSULATION"}]
["Range","Garage","C171",null,{"$f":"$E$405","v":"Cellulose - AVERAGE"}]
["Range","Garage","B175",null,{"$f":"$E$313","v":"WOOD FIBER BATT"}]
["Range","Garage","C176",null,{"$f":"$E$407","v":"Wood fiber batt - AVERAGE"}]
["Range","Garage","B181",null,{"$f":"$E$408","v":"OTHER NATURAL FIBER INSULATION"}]
["Range","Garage","B187",null,{"$f":"$E$409","v":"SPRAY FOAM, CLOSED CELL"}]
["Range","Garage","B191",null,{"$f":"$E$410","v":"SPRAY FOAM, OPEN CELL"}]
["Range","Garage","B194",null,{"$f":"$E$411","v":"HEMPCRETE"}]
["Range","Garage","C195",null,{"$f":"$E$412","v":"Hempcrete - AVERAGE"}]
["Range","Garage","A199",null,"EXTERIOR GARAGE WALL RIGID INSULATION"]
["Range","Garage","G199",null,"(Excludes attachment wall area)"]
["Range","Garage","B200",null,{"$f":"$E$211","v":"EPS FOAM BOARD"}]
["Range","Garage","C201",null,{"$f":"$E$212","v":"EPS foam board - AVERAGE"}]
["Range","Garage","B204",null,{"$f":"$E$270","v":"WOOD FIBER BOARD"}]
["Range","Garage","C205",null,{"$f":"$E$271","v":"Wood fiber board - AVERAGE"}]
["Range","Garage","B211",null,{"$f":"$E$213","v":"XPS FOAM BOARD"}]
["Range","Garage","C212",null,{"$f":"$E$214","v":"XPS foam board - AVERAGE"}]
["Range","Garage","B217",null,{"$f":"$E$420","v":"POLYISOCYANURATE FOAM BOARD"}]
["Range","Garage","C218",null,{"$f":"$E$421","v":"Polyisocyanurate - AVERAGE"}]
["Range","Garage","B223",null,{"$f":"$E$215","v":"MINERAL WOOL BOARD"}]
["Range","Garage","C224",null,{"$f":"$E$423","v":"Mineral wool board - AVERAGE"}]
["Range","Garage","A228",null,"GARAGE ATTACHMENT WALL INSULATION"]
["Range","Garage","A229",null,"GARAGE ATTACHMENT WALL CAVITY INSULATION"]
["Range","Garage","B230",null,{"$f":"$E$307","v":"FIBERGLASS BATT"}]
["Range","Garage","C231",null,{"$f":"$E$400","v":"Fiberglass batt - AVERAGE"}]
["Range","Garage","B235",null,{"$f":"$E$401","v":"FIBERGLASS BLOWN-IN"}]
["Range","Garage","C236",null,{"$f":"$E$402","v":"Fiberglass loose fill - AVERAGE"}]
["Range","Garage","B241",null,{"$f":"$E$311","v":"MINERAL WOOL BATT"}]
["Range","Garage","B249",null,{"$f":"$E$309","v":"CELLULOSE INSULATION"}]
["Range","Garage","C250",null,{"$f":"$E$405","v":"Cellulose - AVERAGE"}]
["Range","Garage","B254",null,{"$f":"$E$313","v":"WOOD FIBER BATT"}]
["Range","Garage","C255",null,{"$f":"$E$407","v":"Wood fiber batt - AVERAGE"}]
["Range","Garage","B260",null,{"$f":"$E$408","v":"OTHER NATURAL FIBER INSULATION"}]
["Range","Garage","B266",null,{"$f":"$E$409","v":"SPRAY FOAM, CLOSED CELL"}]
["Range","Garage","B270",null,{"$f":"$E$410","v":"SPRAY FOAM, OPEN CELL"}]
["Range","Garage","B273",null,{"$f":"$E$411","v":"HEMPCRETE"}]
["Range","Garage","C274",null,{"$f":"$E$412","v":"Hempcrete - AVERAGE"}]
["Range","Garage","A278",null,"GARAGE CLADDING"]
["Range","Garage","A279",null,{"$f":"$E$583","v":"EXTERIOR CLADDING"}]
["Range","Garage","B280",null,{"$f":"$E$584","v":"BRICK"}]
["Range","Garage","B288",null,{"$f":"$E$585","v":"WOOD CLADDING"}]
["Range","Garage","B291",null,{"$f":"$E$586","v":"FIBER CEMENT"}]
["Range","Garage","C292",null,{"$f":"$E$587","v":"Fiber Cement siding - AVERAGE"}]
["Range","Garage","B301",null,{"$f":"$E$588","v":"VINYL SIDING"}]
["Range","Garage","B303",null,{"$f":"$E$589","v":"POLYPROPYLENE SIDING"}]
["Range","Garage","C304",null,{"$f":"$E$590","v":"Polypropylene siding - AVERAGE"}]
["Range","Garage","B307",null,{"$f":"$E$591","v":"STEEL PANEL SIDING"}]
["Range","Garage","C308",null,{"$f":"$E$592","v":"Steel Panel Siding - AVERAGE"}]
["Range","Garage","B315",null,{"$f":"$E$593","v":"ALUMINUM PANEL SIDING"}]
["Range","Garage","C316",null,{"$f":"$E$594","v":"Aluminum Panel Siding - AVERAGE"}]
["Range","Garage","B319",null,{"$f":"$E$595","v":"PLASTER FINISHES"}]
["Range","Garage","B324",null,{"$f":"$E$596","v":"ENGINEERED WOOD SIDING"}]
["Range","Garage","A328",null,{"$f":"$E$597","v":"STRAPPING for RAIN SCREEN"}]
["Range","Garage","D328",null,{"$f":"$E$598","v":"STRAPPING SPACING:"}]
["Range","Garage","A331",null,"INTERIOR CLADDING of GARAGE WALLS"]
["Range","Garage","B332",null,{"$f":"$E$320","v":"DRYWALL 1/2\""}]
["Range","Garage","C333",null,{"$f":"$E$537","v":"Drywall 1/2\" Typical - Interior Cladding for Exterior Walls - AVERAGE"}]
["Range","Garage","B339",null,{"$f":"$E$322","v":"DRYWALL 5/8\""}]
["Range","Garage","B343",null,{"$f":"$E$323","v":"OTHER CLADDING MATERIALS"}]
["Range","Garage","A354",null,"GARAGE WINDOWS"]
["Range","Garage","A355",null,{"$f":"$E$620","v":"DOUBLE PANE WINDOWS"}]
["Range","Garage","A362",null,{"$f":"$E$622","v":"WINDOWS - SPECIFIC MANUFACTURERS"}]
["Range","Garage","A366",null,"GARAGE CEILING"]
["Range","Garage","A367",null,"GARAGE CEILING CLADDING"]
["Range","Garage","B368",null,{"$f":"$E$320","v":"DRYWALL 1/2\""}]
["Range","Garage","C369",null,{"$f":"$E$746","v":"Drywall 1/2\" - Ceilings - AVERAGE"}]
["Range","Garage","B375",null,{"$f":"$E$322","v":"DRYWALL 5/8\""}]
["Range","Garage","C376",null,{"$f":"$E$748","v":"Drywall 5/8\" - Ceilings - AVERAGE"}]
["Range","Garage","B380",null,{"$f":"$E$749","v":"OTHER CEILING FINISHES"}]
["Range","Garage","A387",null,"GARAGE ROOF"]
["Range","Garage","A388",null,{"$f":"$E$298","v":"WOOD FRAME CONSTRUCTION"}]
["Range","Garage","D388",null,{"$f":"$E$297","v":"FRAMING SPACING:"}]
["Range","Garage","B389",null,{"$f":"$E$768","v":"WOOD FRAMING"}]
["Range","Garage","B395",null,{"$f":"$E$688","v":"WOOD TRUSS FRAMING"}]
["Range","Garage","B397",null,{"$f":"$E$686","v":"WOOD I-JOIST FRAMING"}]
["Range","Garage","A402",null,{"$f":"$E$772","v":"ROOF DECKING"}]
["Range","Garage","B403",null,{"$f":"$E$773","v":"WOOD SHEET PRODUCTS - 5/8\""}]
["Range","Garage","B406",null,{"$f":"$E$774","v":"GYPSUM PANELS 1/2\""}]
["Range","Garage","A410",null,{"$f":"$E$775","v":"ROOFING MEMBRANE"}]
["Range","Garage","B411",null,{"$f":"$E$775","v":"ROOFING MEMBRANE"}]
["Range","Garage","A416",null,{"$f":"$E$777","v":"ROOF STRAPPING"}]
["Range","Garage","D416",null,{"$f":"$E$598","v":"STRAPPING SPACING:"}]
["Range","Garage","B417",null,{"$f":"$E$779","v":"WOOD STRAPPING"}]
["Range","Garage","A421",null,{"$f":"$E$780","v":"ROOFING"}]
["Range","Garage","B422",null,{"$f":"$E$781","v":"ASPHALT SHINGLES"}]
["Range","Garage","C423",null,{"$f":"$E$782","v":"Asphalt Shingles - Roofing - AVERAGE"}]
["Range","Garage","B430",null,{"$f":"$E$783","v":"STEEL PANELS"}]
["Range","Garage","C431",null,{"$f":"$E$784","v":"Steel Panels - Roofing - AVERAGE"}]
["Range","Garage","B437",null,{"$f":"$E$785","v":"ALUMINUM PANELS"}]
["Range","Garage","C438",null,{"$f":"$E$786","v":"Aluminum l Panels - Roofing - AVERAGE"}]
["Range","Garage","B441",null,{"$f":"$E$787","v":"FIBER CEMENT ROOFING"}]
["Range","Garage","C442",null,{"$f":"$E$788","v":"Fiber Cement roofing - AVERAGE"}]
["Range","Garage","B446",null,{"$f":"$E$789","v":"OTHER ROOFING OPTIONS"}]
["Range","User-Defined","A1",null,"SECTION 14 ➜ COMPONENT MATERIALS FOR "]
["Range","User-Defined","E1",null,"USER-DEFINED MATERIALS"]
["Range","User-Defined","B2",true,"INSTRUCTIONS FOR USING AN EXISTING DATABASE MATERIAL:         << double-click >>\n- Select material from LIGHT YELLOW DROPDOWN CELL (column C) matching the units of measurement for the material (volume, area, length, or R-value & area)\n- Enter all required inputs into DARK YELLOW cells for that row, including '1' in select column.\n- If adding insulation, enter its total R-VALUE (I-P units) in column B & surface area in column D.  \n\n"]
["Range","User-Defined","F2",true,"INSTRUCTIONS FOR ADDING A MATERIAL NOT IN THE DATABASE: \n(user must know all required information)\nIn a row with CUSTOM as the category, ENTER CUSTOM DATA into all DARK YELLOW fields (CATEGORY, MATERIAL, QUANITY, UNIT, %, kgCO2e EMISSIONS, kgCO2e STORAGE). \n- Only use A1-A3 values from EPDs.\n- Changing the category name does not move the entry to another building section total."]
["Range","User-Defined","N2",true,"Caution: Any user-defined options that have not been validated and approved will reduce the reliability of results. "]
["Range","User-Defined","A3",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","User-Defined","D3",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","User-Defined","E3",null,{"$f":"$E$122","v":"QUANTITY"}]
["Range","User-Defined","F3",null,{"$f":"$E$72","v":"UNIT"}]
["Range","User-Defined","I3",null,{"$f":"$E$168","v":" SELECT"}]
["Range","User-Defined","J3",true,{"$f":"$E$169","v":"NET kgCO2e EMISSIONS"}]
["-"]
["Range","User-Defined","K3",true,{"$f":"$E$171","v":"SELECTED MATERIAL kgCO2e CONTENT"}]
["-"]
["Range","User-Defined","L3",true,{"$f":"$E$173","v":"kgCO2e EMISSIONS"}]
["-"]
["Range","User-Defined","M3",true,{"$f":"$E$175","v":"kgCO2 STORAGE"}]
["-"]
["Range","User-Defined","N3",true,"kgCO2e SUBTOTAL FOR USER-DEFINED MATERIALS"]
["Range","User-Defined","A5",null,"EXISTING DATABASE MATERIALS"]
["Range","User-Defined","C6",null,"MATERIALS BY VOLUME"]
["Range","User-Defined","B7",null,"VOLUME"]
["Range","User-Defined","B8",null,{"$f":"$E$1031","v":"VOLUME"}]
["Range","User-Defined","B9",null,{"$f":"$E$1031","v":"VOLUME"}]
["Range","User-Defined","C10",null,"MATERIALS BY AREA"]
["Range","User-Defined","B11",null,"AREA"]
["Range","User-Defined","B12",null,{"$f":"$E$1035","v":"AREA"}]
["Range","User-Defined","B13",null,{"$f":"$E$1035","v":"AREA"}]
["Range","User-Defined","C14",null,"MATERIALS BY LENGTH"]
["Range","User-Defined","B15",null,"LENGTH"]
["Range","User-Defined","B16",null,{"$f":"$E$1039","v":"LENGTH"}]
["Range","User-Defined","B17",null,{"$f":"$E$1039","v":"LENGTH"}]
["Range","User-Defined","C18",null,"MATERIALS BY AREA & R-VALUE"]
["Range","User-Defined","A22",null,"CUSTOM USER-DEFINED MATERIALS"]
["-","_User-Defined","B23","Ignore this row","Cladding"]
["-","_User-Defined","B24","Ignore this row","User-Defined"]
["-","_User-Defined","B25","Ignore this row",{"$f":"$E$1045","v":"User-Defined"}]
["-","_User-Defined","B26","Ignore this row",{"$f":"$E$1045","v":"User-Defined"}]
["-","_User-Defined","B27","Ignore this row",{"$f":"$E$1045","v":"User-Defined"}]
["Range","User-Defined","B28",true,"Note: User-Defined materials will be listed separately in summary reports."]
["Range","REVIEW","A1",null,"SECTION 12 ➜ REVIEW"]
["Range","REVIEW","C1",null,"SELECTED MATERIALS"]
["Range","REVIEW","A2",null,"SECTION"]
["Range","REVIEW","B2",null,{"$f":"$E$165","v":"CATEGORY"}]
["Range","REVIEW","C2",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","REVIEW","D2",true,"NET CARBON FOOTPRINT \n[kg CO2e]"]
["Range","REVIEW","E2",true,"CARBON EMISSIONS \n[kg CO2e]"]
["Range","REVIEW","F2",true,"CARBON STORAGE\n[kg CO2e]"]
["Range","RESULTS","A2",null,"Material Carbon Emissions Estimator (MCE2)"]
["Range","RESULTS","H2",null,"Project Carbon Emissions Estimates"]
["Range","RESULTS","B3",null,"PROJECT SUMMARY"]
["Range","RESULTS","E5",null,"Project:"]
["Range","RESULTS","E6",null,"Evaluator:"]
["Range","RESULTS","E7",null,"Location:"]
["Range","RESULTS","E8",null,"Home description:"]
["Range","RESULTS","E9",null,"Building Size:"]
["Shape","RESULTS","Rectangle 3",null,"Project Photo or Image Here\n(Insert -> Pictures) "]
["Range","RESULTS","E11",null,{"$f":"$E$55","v":"Material Emissions"}]
["Range","RESULTS","H11",null,{"$f":"$E$40","v":"Operational Emissions"}]
["Range","RESULTS","E12",true,"tonnes CO2e"]
["Range","RESULTS","F12",true,"kg CO2e / m2"]
["Range","RESULTS","H12",true,"tonnes CO2e / yr"]
["Range","RESULTS","I12",true,"t CO2e / 30 yrs"]
["Range","RESULTS","B16",null,"Project Notes"]
["Range","RESULTS","B17",null,"Home is aiming to achieve XYZ level of performance… "]
["Range","RESULTS","B18",null,"PROJECT EMISSIONS TIMELINE"]
["Range","RESULTS","B28",null,"Chart information"]
["Range","RESULTS","B29",true,"Note: In grids with low carbon intensities, MCE2 users should consider energy efficiency measures to reduce overall loads on local and regional grids. \nThe Cumulative Carbon Emissions chart offers a simplified view of the climate impact of materials manufacturing and building operations for the initial 30 years. This chart should be used as a directional guidepost for where to focus carbon reduction efforts, rather than as a predictive model for future emissions. There are several unknowns which may cause deviations from this model, some of which are described below. \n\nNotes on simplifying assumptions\n- Only the cradle-to-gate new construction material carbon emissions are modeled. Realistically, there would be some fluctuations in material carbon due to renovations, maintenance, material decomposition, etc. \n- The operational carbon emissions, the grey line, is shown to increase at the same annual rate. This too, in reality, will vary from year to year and especially as the building ages. \n- GHG emissions associated with fuels and electricity generation (by province or territory) are unchanging values. These values should be reasonably expected to change over time."]
["Range","RESULTS","B34",null,"Project Carbon Emissions Results"]
["Range","RESULTS","B35",null,"EMISSIONS BY ELEMENT OF THE HOME"]
["Range","RESULTS","B53",null,"TOP 10 MOST IMPACTFUL MATERIALS"]
["Range","RESULTS","B55",null,"Rank"]
["Range","RESULTS","C55",true,"kg CO2e"]
["Range","RESULTS","D55",null,"Section"]
["Range","RESULTS","F55",null,"Material"]
["Range","RESULTS","B66",null,"RECOMMENDATIONS"]
["Range","RESULTS","B68",null,"User or embodied carbon advisor to provide recommendations here…"]
["Shape","RESULTS","Rounded Rectangle 1",null,"Save This Scenario"]
["Shape","RESULTS","Group 4,Rectangle 35","Shape inside another","  Material Carbon Intensity, kg CO2/m2"]
["Chart","RESULTS","Chart 9","Title","Cumulative Carbon Emissions"]
["Chart","RESULTS","Chart 9","Y-Axis Label","Global Warming Potential, tonnes CO2e"]
["Chart","RESULTS","Chart 9","X-Axis Label","Years"]
["Chart","RESULTS","Chart 42","Y-Axis Label","Marterial Carbon Emissions, kg CO2e"]
["Shape","SCENARIOS","btn_reset_1",null,"Reset Calculator"]
["Shape","SCENARIOS","btn_delete_1",null,"Delete Scenario"]
["Shape","SCENARIOS","btn_reset_all",null,"Recalculate All Scenarios"]
["Range","SCENARIOS","C2",null,"Project Carbon Emissions Scenarios"]
["Range","SCENARIOS","C3",null,"How to use this TAB:"]
["Range","SCENARIOS","D3",null,"1. Users can save scenarios to this page in order to compare results generated in the calculator.  "]
["Range","SCENARIOS","D4",null,"2. All data associated with the saved scenarios can be re-populated across the spreadsheet.  "]
["Range","SCENARIOS","D5",null,"3. To populate a scenario in the estimator, users can select the scenario by clicking on the green button labeled \"Reset Calculator\" on the left. "]
["Range","SCENARIOS","D6",null,"4. Users can establish custom scenarios and apply these to different homes by loading a new geometry in the USER INPUT SHEET and clicking on the blue button on the left labeled \"Recalculate all Scenarios\".  "]
["Range","SCENARIOS","D7",null,"5 . This will calculate new values associated with the updated geometry for each saved scenario below. "]
["Range","SCENARIOS","B10",null,"Notes"]
["Range","SCENARIOS","B11",true,"MCE Total (tonnes CO2e)"]
["Range","SCENARIOS","B12",true,"Embodied Carbon per m2 (kg CO2e / m2)"]
["Range","SCENARIOS","B13",true,"Footings & Slabs (kg CO2e)"]
["Range","SCENARIOS","B14",true,"Foundation Walls (kg CO2e)"]
["Range","SCENARIOS","B15",true,"Structural Elements (kg CO2e)"]
["Range","SCENARIOS","B16",true,"Ext. Walls (kg CO2e / m2)"]
["Range","SCENARIOS","B17",true,"Ext. Wall Systems (kg CO2e)"]
["Range","SCENARIOS","B18",true,"Party Walls (kg CO2e)"]
["Range","SCENARIOS","B19",true,"Cladding (kg CO2e)"]
["Range","SCENARIOS","B20",true,"Windows (kg CO2e)"]
["Range","SCENARIOS","B21",true,"Int. Walls (kg CO2e)"]
["Range","SCENARIOS","B22",true,"Floors (kg CO2e)"]
["Range","SCENARIOS","B23",true,"Ceilings (kg CO2e)"]
["Range","SCENARIOS","B24",true,"Roof (kg CO2e)"]
["Range","SCENARIOS","B25",true,"Garage (kg CO2e)"]
["Range","SCENARIOS","B26",true,"User-Defined (kg CO2e)"]
["Range","Dropdown Lists","A1",null,"Thickness"]
["Range","Dropdown Lists","B1",null,"Spacing"]
["Range","Dropdown Lists","C1",null,"Steel Joist Spacing"]
["Range","Dropdown Lists","D1",null,"Roof insulation parallel to…"]
["Range","Dropdown Lists","E1",null,"User-defined options: VOLUME – m3"]
["Range","Dropdown Lists","F1",null,"User-defined options: SURFACE AREA – m2"]
["Range","Dropdown Lists","G1",null,"User-defined options: Length - m"]
["Range","Dropdown Lists","H1",null,"User-defined options: R-Value & Area - m2-RSI"]
["Range","Dropdown Lists","J1",null,"Y/N?"]
["Range","Dropdown Lists","D2",null,{"$f":"$E$812","v":"Roof surface"}]
["Range","Dropdown Lists","J2",null,"Yes"]
["Range","Dropdown Lists","D3",null,{"$f":"$E$792","v":"Ceiling surface"}]
["Range","Dropdown Lists","J3",null,"No"]
["Range","Data","A1",null,{"$f":"$E$1052","v":"SECTION"}]
["Range","Data","B1",null,{"$f":"$E$70","v":"  COMPONENT"}]
["Range","Data","C1",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Data","H1",null,"Items selected"]
["Range","Data","I1",null,"RANK"]
["Range","Data","J1",null,"NET CARBON"]
["Range","Data","K1",null,"TAB"]
["Range","Data","L1",null,{"$f":"$E$1052","v":"SECTION"}]
["Range","Data","M1",null,{"$f":"$E$166","v":"MATERIAL"}]
["Range","Data","O1",null,"Year"]
["Range","Data","P1",null,"Materials"]
["Range","Data","Q1",null,"Operations"]
["Range","Data","R1",null,"Total"]
["Range","Data","T3",null,"Emissions"]
["Range","Data","U3",null,"Emissions Bar"]
["Range","Data","V3",null,"Scaled iIndicator"]
["Range","Data","W3",null,"Lower Bound"]
["Range","Data","X3",null,"Upper Bound"]
["Range","Data","K15",null,{"$f":"$E$1083","v":"Section"}]
["Range","Data","L15",true,"Embodied Carbon \n[kg CO2e]"]
["-","_Data","K16","Ignore this cell of the Data sheet","Footings & Slabs"]
["-","_Data","K17","Ignore this cell of the Data sheet","Foundation Walls"]
["-","_Data","K18","Ignore this cell of the Data sheet","Structural Elements"]
["-","_Data","K19","Ignore this cell of the Data sheet","Exterior Walls"]
["-","_Data","K20","Ignore this cell of the Data sheet","Exterior Wall Systems"]
["-","_Data","K21","Ignore this cell of the Data sheet","Party Walls"]
["-","_Data","K22","Ignore this cell of the Data sheet",{"$f":"$E$1044","v":"Cladding"}]
["-","_Data","K23","Ignore this cell of the Data sheet",{"$f":"$E$93","v":"Windows"}]
["-","_Data","K24","Ignore this cell of the Data sheet","Interior Walls"]
["-","_Data","K25","Ignore this cell of the Data sheet","Floors"]
["-","_Data","K26","Ignore this cell of the Data sheet","Ceilings"]
["-","_Data","K27","Ignore this cell of the Data sheet","Roof"]
["-","_Data","K28","Ignore this cell of the Data sheet","Garage"]
["-","_Data","K29","Ignore this cell of the Data sheet",{"$f":"$E$1045","v":"User-Defined"}]
["Range","Data","K30",null,"TOTAL"]
["Range","Composite Master Sheet","A1",null,"Composite Product"]
["Range","Composite Master Sheet","B1",null,"Composite Emissions co2"]
["Range","Composite Master Sheet","C1",null,"Composite Storage CO2/m2"]
["Range","Composite Master Sheet","D1",null,"Unit"]
["Range","Composite Master Sheet","E1",null,"Material1"]
["Range","Composite Master Sheet","F1",null,"Incoming Unit"]
["Range","Composite Master Sheet","G1",null,"M1 Emission"]
["Range","Composite Master Sheet","H1",null,"M1 Storage"]
["Range","Composite Master Sheet","I1",null,"Material2"]
["Range","Composite Master Sheet","J1",null,{"$f":"$E$1173","v":"Incoming Unit"}]
["Range","Composite Master Sheet","K1",null,"M2 Emission"]
["Range","Composite Master Sheet","L1",null,"M2 Storage"]
["Range","Composite Master Sheet","M1",null,"Material3"]
["Range","Composite Master Sheet","N1",null,{"$f":"$E$1173","v":"Incoming Unit"}]
["Range","Composite Master Sheet","O1",null,"M3 Emission"]
["Range","Composite Master Sheet","P1",null,"M3 Storage"]
["Range","Composite Master Sheet","Q1",null,"Material4"]
["Range","Composite Master Sheet","R1",null,{"$f":"$E$1173","v":"Incoming Unit"}]
["Range","Composite Master Sheet","S1",null,"M4 Emission"]
["Range","Composite Master Sheet","T1",null,"M4 Storage"]
["Range","Composite Master Sheet","U1",null,"Material5"]
["Range","Composite Master Sheet","V1",null,{"$f":"$E$1173","v":"Incoming Unit"}]
["Range","Composite Master Sheet","W1",null,"M5 Emission"]
["Range","Composite Master Sheet","X1",null,"M5 Storage"]
["Range","Composite Master Sheet","Y1",null,{"$f":"$E$1103","v":"Notes"}]
["Range","Composite Master Sheet","Z1",null,"Product ID of Material1"]
["Range","Composite Master Sheet","AA1",null,"Product ID of Material2"]
["Range","Composite Master Sheet","AB1",null,"Product ID of Material3"]
["Range","Composite Master Sheet","AC1",null,"Product ID of Material4"]
["Range","Composite Master Sheet","AD1",null,"Product ID of Material5"]
["Range","Composite Master Sheet","A2",null,"EPS FOAM ICF R-23, 2 Sheets of 2.75\" @ R4/in., 15M rebar (6\" CONCRETE CORE must be added separately)"]
["Range","Composite Master Sheet","A3",null,"SIP PANEL - R23 6.5\" - EPS 5.5\" @ R4/in. core, 2 sheets 1/2\" OSB"]
["Range","Composite Master Sheet","A4",null,"SIP PANEL - R30 8.25\" - EPS 7.25\" @ R4/in. core, 2 sheets 1/2\" OSB"]
["Range","Composite Master Sheet","A5",null,"SIP PANEL - R38 10.5\" - EPS 9.5\" @ R4/in. core, 2 sheets 1/2\" OSB"]
["Range","Composite Master Sheet","A6",null,"SIP PANEL - R48 12-7/8\" - EPS 11.875\" @ R4/in. core, 2 sheets 1/2\" OSB"]
["Range","Composite Master Sheet","A7",null,"WOOD CHIP CEMENT ICF 12\" R-22 with MINERAL WOOL INSERTS, (3 in. @ R4.2/in.), 15M REBAR"]
["Range","Composite Master Sheet","A8",null,"WOOD CHIP CEMENT ICF 14\" R-28 with MINERAL WOOL INSERTS (5 in. @ R4.2/in.), 15M REBAR"]
["Range","Composite Master Sheet","A9",null,"WOOD CHIP CEMENT ICF 12\" R-21 with CORK BOARD INSERTS (3 in. @ R4/in.), 15M REBAR"]
["Range","Composite Master Sheet","A10",null,"WOOD CHIP CEMENT ICF 14\" R-27 with CORK BOARD INSERTS (5 in. @ R4/in.), 15M REBAR"]
["Range","Composite Master Sheet","A11",null,"TREATED WOOD FOUNDATION - 2x8 framing @ 16\" OC, 3/4\" plywood sheathing"]
["Range","Composite Master Sheet","A12",null,"WOOD FRAME with STRAW BALE INFILL - 14\" R-46, Double 2x4 @ 30\" o/c"]
["Range","Master sheet","A1",null,"Product"]
["Range","Master sheet","B1",null,{"$f":"$E$1084","v":"Material"}]
["Range","Master sheet","C1",null,"Company (EPD Commissioner)"]
["Range","Master sheet","D1",null,"Brand"]
["Range","Master sheet","E1",null,"Spec's"]
["Range","Master sheet","F1",null,"CSI #"]
["Range","Master sheet","G1",null,"Category"]
["Range","Master sheet","H1",null,{"$f":"$E$1103","v":"Notes"}]
["Range","Master sheet","I1",null,"Country of Mfr"]
["Range","Master sheet","J1",null,"NRCan"]
["Range","Master sheet","K1",null,"Stated EPD kgCO2e / unit"]
["Range","Master sheet","L1",null,"EPD units kgCO2e per"]
["Range","Master sheet","M1",null,"Common Emissions kgCO2e/unit"]
["Range","Master sheet","N1",null,"Units: kgCO2e per"]
["Range","Master sheet","O1",null,"EPD #"]
["Range","Master sheet","P1",null,"Verifying agency"]
["Range","Master sheet","Q1",null,"Exp. Year"]
["Range","Master sheet","R1",null,"Density"]
["Range","Master sheet","S1",null,"Units"]
["Range","Master sheet","T1",null,"Addn'l factors"]
["Range","Master sheet","U1",null,{"$f":"$E$1227","v":"Units"}]
["Range","Master sheet","V1",null,"R-value/inch"]
["Range","Master sheet","W1",null,"Thermal Cond. (k) for RSI"]
["Range","Master sheet","X1",null,{"$f":"$E$1227","v":"Units"}]
["Range","Master sheet","Y1",null,"Biogenic carbon factor"]
["Range","Master sheet","Z1",null,"% Carbon content (kgC/kg)"]
["Range","Master sheet","AA1",null,"Biogenic Storage kgCO2/unit"]
["Range","Master sheet","AB1",null,{"$f":"$E$1222","v":"Units: kgCO2e per"}]
["Range","Master sheet","AC1",null,"WWF Storage Factor kgCO2/kgC"]
["Range","Master sheet","AD1",null,"Carbon content kgC/unit"]
["Range","Master sheet","AE1",null,{"$f":"$E$1227","v":"Units"}]
["Range","Master sheet","AF1",null,"Biogenic CO2 kg - full C value"]
["Range","Master sheet","AG1",null,"Height (m) "]
["Range","Master sheet","AH1",null,"Length (m) "]
["Range","Master sheet","AI1",null,"Width (m) "]
["Range","Master sheet","AJ1",null,"Unit Volume (m3)"]
["Range","Master sheet","AK1",null,"Units/m2"]
["Range","Master sheet","AL1",null,"Product ID"]
["Range","Master sheet","AP1",null,"EPD Note"]
["Range","Master sheet","B2",null,"ACQ wood treatment"]
["Range","Master sheet","B3",null,"Adobe block"]
["Range","Master sheet","D3",null,"8\" block wall"]
["Range","Master sheet","E3",null,"Avg of site made and factory made (Cyprus)"]
["Range","Master sheet","B4",null,"Aerogel blanket"]
["-","_Master sheet","C4","Ignore this cell of Master sheet. Company is not translatable","Aspen Aerogels"]
["Range","Master sheet","E4",null,"R9.6/inch, White/Grey blanket"]
["Range","Master sheet","B5",null,"Aggregate"]
["Range","Master sheet","E5",null,"Avg construction aggregate (gravel & sand)"]
["Range","Master sheet","B6",null,{"$f":"$E$1255","v":"Aggregate"}]
["-","_Master sheet","C6","Ignore this cell of Master sheet. Company is not translatable","Kangley Rock & Recycling"]
["Range","Master sheet","E6",null,{"$f":"$E$1256","v":"Avg construction aggregate (gravel & sand)"}]
["Range","Master sheet","B7",null,{"$f":"$E$1255","v":"Aggregate"}]
["-","_Master sheet","C7","Ignore this cell of Master sheet. Company is not translatable","Martin Marietta"]
["Range","Master sheet","E7",null,{"$f":"$E$1256","v":"Avg construction aggregate (gravel & sand)"}]
["Range","Master sheet","B8",null,{"$f":"$E$1255","v":"Aggregate"}]
["-","_Master sheet","C8","Ignore this cell of Master sheet. Company is not translatable","Polaris Mtls Corp."]
["Range","Master sheet","E8",null,{"$f":"$E$1256","v":"Avg construction aggregate (gravel & sand)"}]
["Range","Master sheet","B9",null,{"$f":"$E$1255","v":"Aggregate"}]
["-","_Master sheet","C9","Ignore this cell of Master sheet. Company is not translatable","Vulcan Mtls Co."]
["Range","Master sheet","E9",null,{"$f":"$E$1256","v":"Avg construction aggregate (gravel & sand)"}]
["Range","Master sheet","B10",null,"Air barrier"]
["-","_Master sheet","C10","Ignore this cell of Master sheet. Company is not translatable","Dupont"]
["Range","Master sheet","D10",null,"Tyvek Fluid Applied Weather Barrier System - All components"]
["Range","Master sheet","E10",null,"25 Perms "]
["Range","Master sheet","B11",null,{"$f":"$E$1269","v":"Air barrier"}]
["-","_Master sheet","C11","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1270","v":"Dupont"}]
["Range","Master sheet","D11",null,"Tyvek HomeWrap "]
["Range","Master sheet","E11",null,"54 Perms"]
["Range","Master sheet","B12",null,{"$f":"$E$1269","v":"Air barrier"}]
["-","_Master sheet","C12","Ignore this cell of Master sheet. Company is not translatable","GCP"]
["Range","Master sheet","D12",null,"Perm-a-Barrier VPL liquid applied permeable barrier"]
["Range","Master sheet","E12",null,"15 Perms, 40 mils thickness"]
["Range","Master sheet","B13",null,"Asphalt Shingles"]
["-","_Master sheet","C13","Ignore this cell of Master sheet. Company is not translatable","Includes: Atlas, BP, CertainTeed, GAF, IKO, Malarkey, Owens Corning, Pabco"]
["Range","Master sheet","B14",null,{"$f":"$E$1281","v":"Asphalt Shingles"}]
["-","_Master sheet","C14","Ignore this cell of Master sheet. Company is not translatable","GAF"]
["Range","Master sheet","D14",null,"Timberline"]
["Range","Master sheet","E14",null,{"$f":"$E$1285","v":"Timberline"}]
["Range","Master sheet","B15",null,{"$f":"$E$1281","v":"Asphalt Shingles"}]
["-","_Master sheet","C15","Ignore this cell of Master sheet. Company is not translatable","Owens Corning"]
["Range","Master sheet","D15",null,"Duration"]
["Range","Master sheet","B16",null,{"$f":"$E$1281","v":"Asphalt Shingles"}]
["-","_Master sheet","C16","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1288","v":"Owens Corning"}]
["Range","Master sheet","D16",null,"Oakridge"]
["Range","Master sheet","B17",null,{"$f":"$E$1281","v":"Asphalt Shingles"}]
["-","_Master sheet","C17","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1288","v":"Owens Corning"}]
["Range","Master sheet","D17",null,"Supreme"]
["Range","Master sheet","B18",null,"Bamboo plywood"]
["-","_Master sheet","C18","Ignore this cell of Master sheet. Company is not translatable","Smith & Fong"]
["Range","Master sheet","D18",null,"Plyboo"]
["Range","Master sheet","E18",null,"1/2\" (12.7 mm)"]
["Range","Master sheet","B19",null,"BioBased Tile"]
["-","_Master sheet","C19","Ignore this cell of Master sheet. Company is not translatable","Armstrong"]
["Range","Master sheet","D19",null,{"$f":"$E$1300","v":"BioBased Tile"}]
["Range","Master sheet","E19",null,"Non-PVC with BioStride polyester binder, Striations BBT and Migrations BBT"]
["Range","Master sheet","B20",null,"Brick, Calcium Silicate"]
["-","_Master sheet","C20","Ignore this cell of Master sheet. Company is not translatable","Arriscraft"]
["Range","Master sheet","D20",null,"Contemporary Brick"]
["Range","Master sheet","E20",null,"3-1/8\" x 3-1/2\" x any length, incl. mortar and ties"]
["Range","Master sheet","B21",null,"Brick, Cement"]
["-","_Master sheet","C21","Ignore this cell of Master sheet. Company is not translatable","MidWest"]
["Range","Master sheet","D21",null,"Architectural Face Brick"]
["Range","Master sheet","E21",null,"3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"]
["Range","Master sheet","B22",null,"Brick, Clay"]
["-","_Master sheet","C22","Ignore this cell of Master sheet. Company is not translatable","Interstate"]
["Range","Master sheet","D22",null,"Avg Face Brick"]
["Range","Master sheet","E22",null,{"$f":"$E$1311","v":"3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"}]
["Range","Master sheet","B23",null,{"$f":"$E$1312","v":"Brick, Clay"}]
["-","_Master sheet","C23","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1313","v":"Interstate"}]
["Range","Master sheet","D23",null,"Avg Thin Face Brick"]
["Range","Master sheet","E23",null,"3-9/16\" x 5/8\" x 11-5/8\" (90 x 16 mm x 295) incl. 3/8\" mortar"]
["Range","Master sheet","B24",null,"Brick, Clay, Generic Modular"]
["-","_Master sheet","C24","Ignore this cell of Master sheet. Company is not translatable","Brick Industry Association"]
["Range","Master sheet","D24",null,"US-Canada Industry Average"]
["Range","Master sheet","E24",null,"3-5/8\" x 2-3/4\" x 7-5/8\" incl. 3/8\" mortar"]
["Range","Master sheet","B25",null,{"$f":"$E$1312","v":"Brick, Clay"}]
["-","_Master sheet","C25","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1321","v":"Brick Industry Association"}]
["Range","Master sheet","D25",null,"US-Canada Industrywide Average"]
["Range","Master sheet","B26",null,"Carpet"]
["Range","Master sheet","E26",null,"Average from 150 samples in the EC3 database"]
["Range","Master sheet","B27",null,{"$f":"$E$1327","v":"Carpet"}]
["Range","Master sheet","D27",null,"Achievable from EC3"]
["Range","Master sheet","E27",null,"Achievable from 150 samples in the EC3 database"]
["Range","Master sheet","B28",null,{"$f":"$E$1327","v":"Carpet"}]
["Range","Master sheet","D28",null,"Conservative from EC3"]
["Range","Master sheet","E28",null,"Conservative from 150 samples in the EC3 database"]
["Range","Master sheet","B29",null,{"$f":"$E$1327","v":"Carpet"}]
["-","_Master sheet","C29","Ignore this cell of Master sheet. Company is not translatable","Interface"]
["Range","Master sheet","D29",null,"GLASBAC®RE, Nylon"]
["Range","Master sheet","E29",null,"Modular tile carpet (closed loop recycling)"]
["Range","Master sheet","B30",null,{"$f":"$E$1327","v":"Carpet"}]
["-","_Master sheet","C30","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1336","v":"Interface"}]
["Range","Master sheet","D30",null,"Cquest BioX"]
["Range","Master sheet","E30",null,"1.5 mm Modular tile carpet"]
["Range","Master sheet","B31",null,"Cedar Shingles/shakes"]
["Range","Master sheet","E31",null,"3/4\" coverage"]
["Range","Master sheet","B32",null,"Cedar Siding"]
["-","_Master sheet","C32","Ignore this cell of Master sheet. Company is not translatable","Western Red Cedar Lumber Assn"]
["Range","Master sheet","E32",null,"1 x 6 Boards"]
["Range","Master sheet","B33",null,"Cellulose - batt"]
["-","_Master sheet","C33","Ignore this cell of Master sheet. Company is not translatable","CMS"]
["Range","Master sheet","D33",null,"EcoCell"]
["Range","Master sheet","E33",null,"R 3.6/inch"]
["Range","Master sheet","B34",null,"Cellulose - dense pack"]
["Range","Master sheet","D34",null,"Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"]
["Range","Master sheet","E34",null,"R 3.7/inch"]
["Range","Master sheet","B35",null,"Cellulose - loose fill"]
["Range","Master sheet","D35",null,"Includes: AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"]
["Range","Master sheet","E35",null,{"$f":"$E$1354","v":"R 3.7/inch"}]
["Range","Master sheet","B36",null,"Cellulose - spray applied"]
["-","_Master sheet","C36","Ignore this cell of Master sheet. Company is not translatable","International Cellulose Corp."]
["Range","Master sheet","D36",null,"K-13, ThermoCon"]
["Range","Master sheet","E36",null,"R 3.75/inch"]
["Range","Master sheet","B37",null,"Cement board 1/2\""]
["-","_Master sheet","C37","Ignore this cell of Master sheet. Company is not translatable","USG"]
["Range","Master sheet","D37",null,"Durock (132)"]
["Range","Master sheet","E37",null,{"$f":"$E$1299","v":"1/2\" (12.7 mm)"}]
["Range","Master sheet","B38",null,{"$f":"$E$1362","v":"Cement board 1/2\""}]
["-","_Master sheet","C38","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1363","v":"USG"}]
["Range","Master sheet","D38",null,"Durock (133)"]
["Range","Master sheet","E38",null,{"$f":"$E$1299","v":"1/2\" (12.7 mm)"}]
["Range","Master sheet","B39",null,"Cement mortar, tile"]
["-","_Master sheet","C39","Ignore this cell of Master sheet. Company is not translatable","Tile Council of North America"]
["Range","Master sheet","E39",null,"Industry average. Includes dry-set, modified dry-set and improved modified dry-set cement mortar"]
["Range","Master sheet","B40",null,"Ceramic tile"]
["-","_Master sheet","C40","Ignore this cell of Master sheet. Company is not translatable","Crossville"]
["Range","Master sheet","D40",null,"Porcelain"]
["Range","Master sheet","E40",null,"Standard grade"]
["Range","Master sheet","B41",null,{"$f":"$E$1373","v":"Ceramic tile"}]
["-","_Master sheet","C41","Ignore this cell of Master sheet. Company is not translatable","StonePeak "]
["Range","Master sheet","D41",null,{"$f":"$E$1375","v":"Porcelain"}]
["Range","Master sheet","E41",null,"Porcelain, standard grade"]
["Range","Master sheet","B42",null,{"$f":"$E$1373","v":"Ceramic tile"}]
["-","_Master sheet","C42","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1371","v":"Tile Council of North America"}]
["Range","Master sheet","E42",null,"Industry average. Includes porcelain, pressed, mosaic and quarry tile"]
["Range","Master sheet","B43",null,"Clay plaster"]
["-","_Master sheet","C43","Ignore this cell of Master sheet. Company is not translatable","Site mixed"]
["Range","Master sheet","E43",null,"15 mm"]
["Range","Master sheet","B44",null,"Clay roof tiles"]
["-","_Master sheet","C44","Ignore this cell of Master sheet. Company is not translatable","HISPALYT"]
["Range","Master sheet","B45",null,"CMU - Light weight"]
["-","_Master sheet","C45","Ignore this cell of Master sheet. Company is not translatable","Angelus Block Co."]
["Range","Master sheet","D45",null,"8\" Light weight blocks"]
["Range","Master sheet","E45",null,"9 x 8 x 16 Precision"]
["Range","Master sheet","B46",null,{"$f":"$E$1389","v":"CMU - Light weight"}]
["-","_Master sheet","C46","Ignore this cell of Master sheet. Company is not translatable","Brampton Brick"]
["Range","Master sheet","D46",null,"8\" Carbon Cure Lightweight blocks"]
["Range","Master sheet","E46",null,"Carbon Cure 15 MPa"]
["Range","Master sheet","B47",null,{"$f":"$E$1389","v":"CMU - Light weight"}]
["-","_Master sheet","C47","Ignore this cell of Master sheet. Company is not translatable","Canadian Concrete Masonry Producers Assn"]
["Range","Master sheet","D47",null,{"$f":"$E$1391","v":"8\" Light weight blocks"}]
["Range","Master sheet","E47",null,"390 x 190 x 190 mm"]
["Range","Master sheet","B49",null,"CMU - Normal weight"]
["-","_Master sheet","C49","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1390","v":"Angelus Block Co."}]
["Range","Master sheet","D49",null,"8\" Normal weight blocks"]
["Range","Master sheet","E49",null,"8 x 8 x 16 Precision"]
["Range","Master sheet","B50",null,{"$f":"$E$1401","v":"CMU - Normal weight"}]
["-","_Master sheet","C50","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1398","v":"Canadian Concrete Masonry Producers Assn"}]
["Range","Master sheet","D50",null,{"$f":"$E$1403","v":"8\" Normal weight blocks"}]
["Range","Master sheet","E50",null,"390 x 190 x 190 mm"]
["Range","Master sheet","B52",null,{"$f":"$E$1401","v":"CMU - Normal weight"}]
["-","_Master sheet","C52","Ignore this cell of Master sheet. Company is not translatable","Permacon"]
["Range","Master sheet","D52",null,{"$f":"$E$1403","v":"8\" Normal weight blocks"}]
["Range","Master sheet","E52",null,"NW STD 20CM GLPW"]
["Range","Master sheet","B53",null,"CMU - Rammed earth"]
["-","_Master sheet","C53","Ignore this cell of Master sheet. Company is not translatable","Watershed Materials"]
["Range","Master sheet","D53",null,"Watershed Block"]
["Range","Master sheet","B54",null,{"$f":"$E$1413","v":"CMU - Rammed earth"}]
["-","_Master sheet","C54","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1414","v":"Watershed Materials"}]
["Range","Master sheet","D54",null,"Watershed ZeroBlock"]
["Range","Master sheet","B55",null,"Earthen Floor"]
["-","_Master sheet","C55","Ignore this cell of Master sheet. Company is not translatable","Site made"]
["Range","Master sheet","E55",null,"3\" cob, 1\" clay plaster"]
["Range","Master sheet","B56",null,"Cob wall"]
["-","_Master sheet","C56","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1385","v":"Site mixed"}]
["Range","Master sheet","E56",null,"18\" (457 mm) avg. thickness"]
["Range","Master sheet","B57",null,"Compressed earth block"]
["-","_Master sheet","C57","Ignore this cell of Master sheet. Company is not translatable","Factory made"]
["Range","Master sheet","D57",null,"Stabilized with 6.5% NHL"]
["Range","Master sheet","E57",null,"31.5 x 6 x 2.75 \" (300 x 150 x 70 mm)"]
["Range","Master sheet","B58",null,"Compressed straw board"]
["-","_Master sheet","C58","Ignore this cell of Master sheet. Company is not translatable","Stramit"]
["Range","Master sheet","D58",null,"60 mm board"]
["Range","Master sheet","E58",null,"R 3.9/inch"]
["Range","Master sheet","B59",null,"Concrete "]
["-","_Master sheet","C59","Ignore this cell of Master sheet. Company is not translatable","Butler Concrete"]
["Range","Master sheet","D59",null,"Avg of 19 different 25 Mpa mixes"]
["Range","Master sheet","B60",null,"Concrete - 0-25 MPa, Industry Average Benchmark"]
["-","_Master sheet","C60","Ignore this cell of Master sheet. Company is not translatable","CRMCA"]
["Range","Master sheet","D60",null,"Can. Avg."]
["Range","Master sheet","B61",null,"Concrete - 0-25 MPa, 0-14% FA/SL, GU"]
["-","_Master sheet","C61","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D61",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B62",null,"Concrete - 0-25 MPa, 15-29% Fly Ash, GU"]
["-","_Master sheet","C62","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D62",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B63",null,"Concrete - 0-25 MPa, 30-40% Fly Ash, GU"]
["-","_Master sheet","C63","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D63",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B64",null,"Concrete - 0-25 MPa, 25-34% Slag, GU"]
["-","_Master sheet","C64","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D64",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B65",null,"Concrete - 0-25 MPa, 35-50% Slag, GU"]
["-","_Master sheet","C65","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D65",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B66",null,"Concrete - 26-30 MPa, Canadian Benchmark Average"]
["-","_Master sheet","C66","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D66",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B67",null,"Concrete - 26-30 MPa, 0-14% FA/SL, GU"]
["-","_Master sheet","C67","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D67",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B68",null,"Concrete - 26-30 MPa, 15-29% Fly Ash, GU"]
["-","_Master sheet","C68","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D68",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B69",null,"Concrete - 26-30 MPa, 30-40% Fly Ash, GU"]
["-","_Master sheet","C69","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D69",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B70",null,"Concrete - 26-30 MPa, 25-34% Slag, GU"]
["-","_Master sheet","C70","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D70",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B71",null,"Concrete - 26-30 MPa, 35-50% Slag, GU"]
["-","_Master sheet","C71","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D71",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B72",null,"Concrete - 31-35 MPa, Canadian Benchmark Average"]
["-","_Master sheet","C72","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D72",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B73",null,"Concrete - 31-35 MPa, 0-14% FA/SL, GU"]
["-","_Master sheet","C73","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D73",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B74",null,"Concrete - 31-35 MPa, 15-29% Fly Ash, GU"]
["-","_Master sheet","C74","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D74",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B75",null,"Concrete - 31-35 MPa, 30-40% Fly Ash, GU"]
["-","_Master sheet","C75","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D75",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B76",null,"Concrete - 31-35 MPa, 25-34% Slag, GU"]
["-","_Master sheet","C76","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D76",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B77",null,"Concrete - 31-35 MPa, 35-50% Slag, GU"]
["-","_Master sheet","C77","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1437","v":"CRMCA"}]
["Range","Master sheet","D77",null,{"$f":"$E$1438","v":"Can. Avg."}]
["Range","Master sheet","B78",null,"Concrete - 20 MPa, Standard mix"]
["-","_Master sheet","C78","Ignore this cell of Master sheet. Company is not translatable","NRMCA"]
["Range","Master sheet","D78",null,"US Avg"]
["Range","Master sheet","B79",null,"Concrete - 20 MPa, 20-30% Fly Ash"]
["-","_Master sheet","C79","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1491","v":"NRMCA"}]
["Range","Master sheet","D79",null,{"$f":"$E$1492","v":"US Avg"}]
["Range","Master sheet","B80",null,"Concrete - 20 MPa, 30-40% FA/SL"]
["-","_Master sheet","C80","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1491","v":"NRMCA"}]
["Range","Master sheet","D80",null,{"$f":"$E$1492","v":"US Avg"}]
["Range","Master sheet","B81",null,"Concrete - 20 MPa, 40-50% FA/SL mix"]
["-","_Master sheet","C81","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1491","v":"NRMCA"}]
["Range","Master sheet","D81",null,{"$f":"$E$1492","v":"US Avg"}]
["Range","Master sheet","B82",null,"Concrete - 20 MPa, >50% SCM mix"]
["-","_Master sheet","C82","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1491","v":"NRMCA"}]
["Range","Master sheet","D82",null,{"$f":"$E$1492","v":"US Avg"}]
["Range","Master sheet","B83",null,"Cork board insulation"]
["-","_Master sheet","C83","Ignore this cell of Master sheet. Company is not translatable","Amorim "]
["Range","Master sheet","D83",null,"Isolamentos"]
["Range","Master sheet","E83",null,"R4/inch"]
["Range","Master sheet","B84",null,"Cork flooring"]
["-","_Master sheet","C84","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1506","v":"Amorim "}]
["Range","Master sheet","D84",null," Revestimentos S.A."]
["Range","Master sheet","E84",null,"Cork floating floor planks"]
["Range","Master sheet","B85",null,{"$f":"$E$1509","v":"Cork flooring"}]
["-","_Master sheet","C85","Ignore this cell of Master sheet. Company is not translatable","European Resilient Flooring Manufacturers' Institute"]
["Range","Master sheet","D85",null,"Includes: Altro, Amorim, Amtico, Artigo, Aspecta, BeauFlor, Dickson, Mflor, Forbo, Gerflor, IVC, Nora, Polyflor, Tarkett, Kahrs, Windmoller"]
["Range","Master sheet","E85",null,"Cork floor tiles"]
["Range","Master sheet","B86",null,"Cross Laminated Timber"]
["-","_Master sheet","C86","Ignore this cell of Master sheet. Company is not translatable","Nordic "]
["Range","Master sheet","D86",null,"X-Lam"]
["Range","Master sheet","E86",null,"3-1/2\" (90mm) thick"]
["Range","Master sheet","B87",null,{"$f":"$E$1517","v":"Cross Laminated Timber"}]
["-","_Master sheet","C87","Ignore this cell of Master sheet. Company is not translatable","Structurlam"]
["Range","Master sheet","D87",null,"CrossLam"]
["Range","Master sheet","E87",null,{"$f":"$E$1520","v":"3-1/2\" (90mm) thick"}]
["Range","Master sheet","B88",null,"Dowel Laminated Timber"]
["-","_Master sheet","C88","Ignore this cell of Master sheet. Company is not translatable","StructureCraft"]
["Range","Master sheet","D88",null,"DowelLam"]
["Range","Master sheet","E88",null,{"$f":"$E$1520","v":"3-1/2\" (90mm) thick"}]
["Range","Master sheet","B89",null,"Drywall 1/2\""]
["-","_Master sheet","C89","Ignore this cell of Master sheet. Company is not translatable","CertainTeed"]
["Range","Master sheet","D89",null,"AirRenew"]
["Range","Master sheet","E89",null,{"$f":"$E$1299","v":"1/2\" (12.7 mm)"}]
["Range","Master sheet","B90",null,{"$f":"$E$1529","v":"Drywall 1/2\""}]
["-","_Master sheet","C90","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1530","v":"CertainTeed"}]
["Range","Master sheet","D90",null,"Easi-Lite"]
["Range","Master sheet","E90",null,{"$f":"$E$1299","v":"1/2\" (12.7 mm)"}]
["Range","Master sheet","B91",null,{"$f":"$E$1529","v":"Drywall 1/2\""}]
["-","_Master sheet","C91","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1530","v":"CertainTeed"}]
["Range","Master sheet","D91",null,"M2Tech moisture resistant"]
["Range","Master sheet","E91",null,{"$f":"$E$1299","v":"1/2\" (12.7 mm)"}]
["Range","Master sheet","B92",null,{"$f":"$E$1529","v":"Drywall 1/2\""}]
["-","_Master sheet","C92","Ignore this cell of Master sheet. Company is not translatable","Pabco"]
["Range","Master sheet","D92",null,"QuietRock"]
["Range","Master sheet","E92",null,"QuietRock 1/2\""]
["Range","Master sheet","B93",null,"Drywall 5/8\""]
["Range","Master sheet","D93",null,"Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC"]
["Range","Master sheet","B94",null,{"$f":"$E$1545","v":"Drywall 5/8\""}]
["-","_Master sheet","C94","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1363","v":"USG"}]
["Range","Master sheet","D94",null,"EcoSmart Firecode "]
["Range","Master sheet","B95",null,"EPDM Roofing Membrane"]
["-","_Master sheet","C95","Ignore this cell of Master sheet. Company is not translatable","SPRI "]
["Range","Master sheet","B96",null,"EPS foam board"]
["-","_Master sheet","C96","Ignore this cell of Master sheet. Company is not translatable","EPS Industry Alliance"]
["Range","Master sheet","E96",null,"R 4.6/inch, Type IX, 25 psi (Type 3, 140 kPa)"]
["Range","Master sheet","B97",null,{"$f":"$E$1552","v":"EPS foam board"}]
["-","_Master sheet","C97","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1553","v":"EPS Industry Alliance"}]
["Range","Master sheet","E97",null,"R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"]
["Range","Master sheet","B98",null,"EPS foam board with graphite"]
["-","_Master sheet","C98","Ignore this cell of Master sheet. Company is not translatable","BASF "]
["Range","Master sheet","D98",null,"Neopor"]
["Range","Master sheet","E98",null,"R 4.7/inch, Type IX"]
["Range","Master sheet","B99",null,{"$f":"$E$1558","v":"EPS foam board with graphite"}]
["-","_Master sheet","C99","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1559","v":"BASF "}]
["Range","Master sheet","D99",null,{"$f":"$E$1560","v":"Neopor"}]
["Range","Master sheet","E99",null,"R 4.7/inch, Type II, 15 psi (Type 2, 110 kPa)"]
["Range","Master sheet","B100",null,"Fiber Cement roofing"]
["-","_Master sheet","C100","Ignore this cell of Master sheet. Company is not translatable","Cembrit"]
["Range","Master sheet","D100",null,"Corrugated sheets"]
["Range","Master sheet","E100",null,"6.5 mm"]
["Range","Master sheet","B101",null,{"$f":"$E$1566","v":"Fiber Cement roofing"}]
["-","_Master sheet","C101","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1567","v":"Cembrit"}]
["Range","Master sheet","D101",null,"Slates"]
["Range","Master sheet","E101",null,"4 mm"]
["Range","Master sheet","B102",null,{"$f":"$E$1566","v":"Fiber Cement roofing"}]
["-","_Master sheet","C102","Ignore this cell of Master sheet. Company is not translatable","Mahaphant "]
["Range","Master sheet","D102",null,"Fibre-Cement"]
["Range","Master sheet","E102",null,"5 mm"]
["Range","Master sheet","B103",null,"Fiber Cement siding"]
["-","_Master sheet","C103","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1567","v":"Cembrit"}]
["Range","Master sheet","D103",null,"Patina"]
["Range","Master sheet","B104",null,{"$f":"$E$1578","v":"Fiber Cement siding"}]
["-","_Master sheet","C104","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1567","v":"Cembrit"}]
["Range","Master sheet","D104",null,"Solid & Express"]
["Range","Master sheet","B105",null,"Fiberglass batt"]
["-","_Master sheet","C105","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1530","v":"CertainTeed"}]
["Range","Master sheet","D105",null,"Sustainable Insulation"]
["Range","Master sheet","E105",null,{"$f":"$E$1351","v":"R 3.6/inch"}]
["Range","Master sheet","B106",null,{"$f":"$E$1584","v":"Fiberglass batt"}]
["-","_Master sheet","C106","Ignore this cell of Master sheet. Company is not translatable","Knauf"]
["Range","Master sheet","D106",null,"EcoBatt"]
["Range","Master sheet","E106",null,{"$f":"$E$1351","v":"R 3.6/inch"}]
["Range","Master sheet","B107",null,{"$f":"$E$1584","v":"Fiberglass batt"}]
["-","_Master sheet","C107","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1288","v":"Owens Corning"}]
["Range","Master sheet","D107",null,"EcoTouch Pink batt and roll"]
["Range","Master sheet","E107",null,{"$f":"$E$1351","v":"R 3.6/inch"}]
["Range","Master sheet","B108",null,"Fiberglass loose fill"]
["-","_Master sheet","C108","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1530","v":"CertainTeed"}]
["Range","Master sheet","D108",null,"InsulSafe, Optima, TruComfort"]
["Range","Master sheet","E108",null,"R 2.6/inch"]
["Range","Master sheet","B109",null,{"$f":"$E$1596","v":"Fiberglass loose fill"}]
["-","_Master sheet","C109","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1589","v":"Knauf"}]
["Range","Master sheet","D109",null,"Jet Stream ULTRA"]
["Range","Master sheet","E109",null,"R 2.2/inch"]
["Range","Master sheet","B110",null,{"$f":"$E$1596","v":"Fiberglass loose fill"}]
["-","_Master sheet","C110","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1288","v":"Owens Corning"}]
["Range","Master sheet","D110",null,"AttiCat, ProCat, ProPink"]
["Range","Master sheet","E110",null,"R 2.8/inch"]
["Range","Master sheet","B111",null,"Foam glass aggregate"]
["-","_Master sheet","C111","Ignore this cell of Master sheet. Company is not translatable","Glasopor AS"]
["Range","Master sheet","E111",null,"R 1.7/inch, 10-60 mm"]
["Range","Master sheet","B112",null,{"$f":"$E$1608","v":"Foam glass aggregate"}]
["-","_Master sheet","C112","Ignore this cell of Master sheet. Company is not translatable","Hasopor"]
["Range","Master sheet","E112",null,{"$f":"$E$1610","v":"R 1.7/inch, 10-60 mm"}]
["Range","Master sheet","B113",null,{"$f":"$E$1608","v":"Foam glass aggregate"}]
["-","_Master sheet","C113","Ignore this cell of Master sheet. Company is not translatable","Misapor "]
["Range","Master sheet","D113",null,"Glavel"]
["Range","Master sheet","E113",null,{"$f":"$E$1610","v":"R 1.7/inch, 10-60 mm"}]
["Range","Master sheet","B114",null,"Foam glass board"]
["-","_Master sheet","C114","Ignore this cell of Master sheet. Company is not translatable","Pittsburgh Corning Europe"]
["Range","Master sheet","D114",null,"Foamglas T4"]
["Range","Master sheet","E114",null,"R3.7/inch"]
["Range","Master sheet","B115",null,{"$f":"$E$1618","v":"Foam glass board"}]
["-","_Master sheet","C115","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1619","v":"Pittsburgh Corning Europe"}]
["Range","Master sheet","D115",null,"Foamglas W+F, Foamglas T3"]
["Range","Master sheet","E115",null,{"$f":"$E$1508","v":"R4/inch"}]
["Range","Master sheet","B116",null,"Glued laminated timber"]
["-","_Master sheet","C116","Ignore this cell of Master sheet. Company is not translatable","American Wood Council & Canadian Wood Council"]
["Range","Master sheet","B117",null,{"$f":"$E$1626","v":"Glued laminated timber"}]
["-","_Master sheet","C117","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1522","v":"Structurlam"}]
["Range","Master sheet","D117",null,"Glulam Plus"]
["Range","Master sheet","E117",null,{"$f":"$E$1520","v":"3-1/2\" (90mm) thick"}]
["Range","Master sheet","B118",null,"Gypsum panels - glass mat"]
["Range","Master sheet","D118",null,{"$f":"$E$1546","v":"Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC"}]
["Range","Master sheet","B119",null,{"$f":"$E$1632","v":"Gypsum panels - glass mat"}]
["-","_Master sheet","C119","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1363","v":"USG"}]
["Range","Master sheet","D119",null,"Securock ExoAir 430"]
["Range","Master sheet","B120",null,"Hardwood flooring"]
["-","_Master sheet","C120","Ignore this cell of Master sheet. Company is not translatable","Action Floor Systems"]
["Range","Master sheet","E120",null,"25/32\" x 3-1/4\" FSC certified"]
["Range","Master sheet","B121",null,{"$f":"$E$1637","v":"Hardwood flooring"}]
["-","_Master sheet","C121","Ignore this cell of Master sheet. Company is not translatable","mafi"]
["Range","Master sheet","D121",null,"Natural Hardwood Planks"]
["Range","Master sheet","E121",null,"3/4\", 3 ply laminated solid, oil pre-finished"]
["Range","Master sheet","B122",null,{"$f":"$E$1637","v":"Hardwood flooring"}]
["-","_Master sheet","C122","Ignore this cell of Master sheet. Company is not translatable","Typical Eastern Canadian, solid, pre-finished"]
["Range","Master sheet","E122",null,"3-12\" x 3/4\" prefinished"]
["Range","Master sheet","B123",null,"Helical pier"]
["-","_Master sheet","C123","Ignore this cell of Master sheet. Company is not translatable","Generic"]
["Range","Master sheet","E123",null,"3\" Nominal Pipe, 3.5 x 3/16\" (89 x 5.5 mm), 10\" Helix, Sched 40 STD Galvanized steel"]
["Range","Master sheet","B124",null,"Hemp fiber batt"]
["-","_Master sheet","C124","Ignore this cell of Master sheet. Company is not translatable","NaturFibre"]
["Range","Master sheet","D124",null,"Hemp Wool"]
["Range","Master sheet","E124",null,{"$f":"$E$1354","v":"R 3.7/inch"}]
["Range","Master sheet","B125",null,"Hempcrete"]
["-","_Master sheet","C125","Ignore this cell of Master sheet. Company is not translatable","IsoHemp"]
["Range","Master sheet","D125",null,"Europe"]
["Range","Master sheet","E125",null,"R 2.1/inch"]
["Range","Master sheet","B126",null,{"$f":"$E$1654","v":"Hempcrete"}]
["-","_Master sheet","C126","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1385","v":"Site mixed"}]
["Range","Master sheet","D126",null,{"$f":"$E$1656","v":"Europe"}]
["Range","Master sheet","E126",null,"R 2.1/inch, Avg. of 9 mixes"]
["Range","Master sheet","B127",null,{"$f":"$E$1654","v":"Hempcrete"}]
["-","_Master sheet","C127","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1385","v":"Site mixed"}]
["Range","Master sheet","D127",null,"USA"]
["Range","Master sheet","E127",null,"R 2.1/inch, Avg. mix using NHL & PHL"]
["Range","Master sheet","B128",null,"Laminate flooring"]
["-","_Master sheet","C128","Ignore this cell of Master sheet. Company is not translatable","Novalis "]
["Range","Master sheet","D128",null,"LVT"]
["Range","Master sheet","B130",null,"Laminated strand lumber (LSL)",null,null,"2023_July_new"]
["-","_Master sheet","C130","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1627","v":"American Wood Council & Canadian Wood Council"}]
["Range","Master sheet","B131",null,"Laminated veneer lumber (LVL)",null,null,"2023_July_new"]
["-","_Master sheet","C131","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1627","v":"American Wood Council & Canadian Wood Council"}]
["Range","Master sheet","B132",null,{"$f":"$E$1671","v":"Laminated veneer lumber (LVL)"},null,null,"2023_July_new"]
["-","_Master sheet","C132","Ignore this cell of Master sheet. Company is not translatable","RedBuilt"]
["Range","Master sheet","D132",null,"RedLam"]
["Range","Master sheet","B133",null,"Lime Plaster"]
["-","_Master sheet","C133","Ignore this cell of Master sheet. Company is not translatable","Mapei"]
["Range","Master sheet","D133",null,"MapeWall Muratura"]
["Range","Master sheet","E133",null,"3/4\" Natural Hydraulic Lime (NHL)"]
["Range","Master sheet","B134",null,"Lime/Cork Plaster"]
["-","_Master sheet","C134","Ignore this cell of Master sheet. Company is not translatable","Diasen "]
["Range","Master sheet","D134",null,"Diathonite Evolution"]
["Range","Master sheet","E134",null,"Exterior plaster cladding, 3/4\""]
["Range","Master sheet","B135",null,"Linoleum flooring"]
["-","_Master sheet","C135","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1301","v":"Armstrong"}]
["Range","Master sheet","D135",null,"Sheet style "]
["Range","Master sheet","E135",null,"2.5 mm sheet style linoleum"]
["Range","Master sheet","B136",null,{"$f":"$E$1684","v":"Linoleum flooring"}]
["-","_Master sheet","C136","Ignore this cell of Master sheet. Company is not translatable","Forbo "]
["Range","Master sheet","D136",null,"Marmoleum"]
["Range","Master sheet","E136",null,{"$f":"$E$1687","v":"2.5 mm sheet style linoleum"}]
["Range","Master sheet","B137",null,{"$f":"$E$1684","v":"Linoleum flooring"}]
["-","_Master sheet","C137","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1689","v":"Forbo "}]
["Range","Master sheet","D137",null,"Marmoleum Striato"]
["Range","Master sheet","E137",null,{"$f":"$E$1687","v":"2.5 mm sheet style linoleum"}]
["Range","Master sheet","B138",null,{"$f":"$E$1684","v":"Linoleum flooring"}]
["-","_Master sheet","C138","Ignore this cell of Master sheet. Company is not translatable","Gerflor "]
["Range","Master sheet","D138",null,"DLW Linoleum Acousticplus",null,null,"2023_July_new"]
["Range","Master sheet","E138",null,"4.0 mm sheet style linoleum"]
["Range","Master sheet","B140",null,"Liquid linoleum flooring"]
["-","_Master sheet","C140","Ignore this cell of Master sheet. Company is not translatable","Duracryl Corques"]
["Range","Master sheet","D140",null,"Liquid Lino"]
["Range","Master sheet","E140",null,"2.0 mm liquid applied"]
["Range","Master sheet","B141",null,"Masonry cement"]
["-","_Master sheet","C141","Ignore this cell of Master sheet. Company is not translatable","Portland Cement Association"]
["Range","Master sheet","D141",null,"Includes Argos, Buzzi, CalPortland, Capitol Aggregates, Cemex, Essroc, LafargeHolcim, Monarch, St. Mary's, Titan"]
["Range","Master sheet","B142",null,"Masonry Mortar Mix"]
["-","_Master sheet","C142","Ignore this cell of Master sheet. Company is not translatable","1 part Masonry cement"]
["Range","Master sheet","D142",null,"3 parts avg sand"]
["Range","Master sheet","B143",null,"Metal Panels - Aluminum"]
["-","_Master sheet","C143","Ignore this cell of Master sheet. Company is not translatable","Metal Construction Assn. "]
["Range","Master sheet","D143",null,"Includes: ATAS, DMI, Englert, Fabral,McElroy, Pac-Clad"]
["Range","Master sheet","E143",null,"22 gauge"]
["Range","Master sheet","B144",null,{"$f":"$E$1710","v":"Metal Panels - Aluminum"}]
["-","_Master sheet","C144","Ignore this cell of Master sheet. Company is not translatable","Petersen Aluminum Corp"]
["Range","Master sheet","D144",null,"Pac-Clad"]
["Range","Master sheet","E144",null,"20EQ gauge"]
["Range","Master sheet","B145",null,"Metal Panels - Steel"]
["-","_Master sheet","C145","Ignore this cell of Master sheet. Company is not translatable","AEP Span"]
["Range","Master sheet","D145",null,"All products"]
["Range","Master sheet","E145",null,"24 gauge"]
["Range","Master sheet","B146",null,{"$f":"$E$1718","v":"Metal Panels - Steel"}]
["-","_Master sheet","C146","Ignore this cell of Master sheet. Company is not translatable","ArcelorMittal"]
["Range","Master sheet","D146",null,{"$f":"$E$1720","v":"All products"}]
["Range","Master sheet","E146",null,{"$f":"$E$1721","v":"24 gauge"}]
["Range","Master sheet","B147",null,{"$f":"$E$1718","v":"Metal Panels - Steel"}]
["-","_Master sheet","C147","Ignore this cell of Master sheet. Company is not translatable","Canadian Sheet Steel Building Institute"]
["Range","Master sheet","D147",null,"Includes: Agway, Bailey, Behlen, Canam,DASS, DCM, Duchesne, EB, Exsteel, Ideal Roofing, Imperial, LKME, Manugypse, Metal Up, Scotia, Steel Tile Co, Steelway, Trebor, Vicwest, Vulcraft, Westform, Westman"]
["Range","Master sheet","E147",null,{"$f":"$E$1721","v":"24 gauge"}]
["Range","Master sheet","B148",null,{"$f":"$E$1718","v":"Metal Panels - Steel"}]
["-","_Master sheet","C148","Ignore this cell of Master sheet. Company is not translatable","Metal Building Manufacturers Assn"]
["Range","Master sheet","D148",null,"See all members"]
["Range","Master sheet","E148",null,{"$f":"$E$1721","v":"24 gauge"}]
["Range","Master sheet","B149",null,{"$f":"$E$1718","v":"Metal Panels - Steel"}]
["-","_Master sheet","C149","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1711","v":"Metal Construction Assn. "}]
["Range","Master sheet","D149",null,{"$f":"$E$1712","v":"Includes: ATAS, DMI, Englert, Fabral,McElroy, Pac-Clad"}]
["Range","Master sheet","E149",null,{"$f":"$E$1721","v":"24 gauge"}]
["Range","Master sheet","B150",null,{"$f":"$E$1718","v":"Metal Panels - Steel"}]
["-","_Master sheet","C150","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1715","v":"Petersen Aluminum Corp"}]
["Range","Master sheet","D150",null,"PAC-CLAD"]
["Range","Master sheet","E150",null,{"$f":"$E$1721","v":"24 gauge"}]
["Range","Master sheet","B151",null,"MgO board 1/2\""]
["-","_Master sheet","C151","Ignore this cell of Master sheet. Company is not translatable","North American MgO"]
["Range","Master sheet","D151",null,"MagTech Ultra"]
["Range","Master sheet","B152",null,"Mineral wool batt"]
["-","_Master sheet","C152","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1288","v":"Owens Corning"}]
["Range","Master sheet","D152",null,"Thermafiber UltraBatt"]
["Range","Master sheet","E152",null,"R 4.3/inch"]
["Range","Master sheet","B153",null,{"$f":"$E$1745","v":"Mineral wool batt"}]
["-","_Master sheet","C153","Ignore this cell of Master sheet. Company is not translatable","Rockwool"]
["Range","Master sheet","D153",null,"Safe'n'Sound, ComfortBatt"]
["Range","Master sheet","E153",null,"R 3.8/inch"]
["Range","Master sheet","B154",null,"Mineral wool board - heavy density"]
["-","_Master sheet","C154","Ignore this cell of Master sheet. Company is not translatable","NAIMA "]
["Range","Master sheet","D154",null,"Includes: Rolan, Armstrong, Rockwool, Thermafiber, American Rock Wool, IIG, Delta, USG"]
["Range","Master sheet","E154",null,"R 4.2/inch"]
["Range","Master sheet","B155",null,"Mineral wool board "]
["-","_Master sheet","C155","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1750","v":"Rockwool"}]
["Range","Master sheet","D155",null,"Rockboard 60"]
["Range","Master sheet","E155",null,{"$f":"$E$1748","v":"R 4.3/inch"}]
["Range","Master sheet","B156",null,"Mineral wool board - light density"]
["-","_Master sheet","C156","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1754","v":"NAIMA "}]
["Range","Master sheet","D156",null,{"$f":"$E$1755","v":"Includes: Rolan, Armstrong, Rockwool, Thermafiber, American Rock Wool, IIG, Delta, USG"}]
["Range","Master sheet","E156",null,{"$f":"$E$1354","v":"R 3.7/inch"}]
["Range","Master sheet","B157",null,"Mineral wool loose fill"]
["-","_Master sheet","C157","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1754","v":"NAIMA "}]
["Range","Master sheet","D157",null,{"$f":"$E$1755","v":"Includes: Rolan, Armstrong, Rockwool, Thermafiber, American Rock Wool, IIG, Delta, USG"}]
["Range","Master sheet","E157",null,"R 3/inch"]
["Range","Master sheet","B158",null,"Mycelium board"]
["-","_Master sheet","C158","Ignore this cell of Master sheet. Company is not translatable","Ecovative "]
["Range","Master sheet","D158",null,"Mycofoam"]
["Range","Master sheet","E158",null,{"$f":"$E$1354","v":"R 3.7/inch"}]
["Range","Master sheet","B159",null,"OSB sheathing"]
["-","_Master sheet","C159","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1627","v":"American Wood Council & Canadian Wood Council"}]
["Range","Master sheet","B160",null,{"$f":"$E$1773","v":"OSB sheathing"}]
["-","_Master sheet","C160","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1627","v":"American Wood Council & Canadian Wood Council"}]
["Range","Master sheet","B161",null,{"$f":"$E$1773","v":"OSB sheathing"}]
["-","_Master sheet","C161","Ignore this cell of Master sheet. Company is not translatable","Huber "]
["Range","Master sheet","D161",null,"AdvanTech"]
["Range","Master sheet","E161",null,"1/2\" Sheathing"]
["Range","Master sheet","B163",null,{"$f":"$E$1773","v":"OSB sheathing"}]
["-","_Master sheet","C163","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1778","v":"Huber "}]
["Range","Master sheet","D163",null,"ZIP System"]
["Range","Master sheet","E163",null,"7/16\" Sheathing, protective barrier and tape"]
["Range","Master sheet","B165",null,"OSB subflooring"]
["-","_Master sheet","C165","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1778","v":"Huber "}]
["Range","Master sheet","D165",null,{"$f":"$E$1779","v":"AdvanTech"}]
["Range","Master sheet","E165",null,"19/32\" Subflooring"]
["Range","Master sheet","B167",null,"Plywood"]
["-","_Master sheet","C167","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1627","v":"American Wood Council & Canadian Wood Council"}]
["Range","Master sheet","B168",null,{"$f":"$E$1789","v":"Plywood"}]
["-","_Master sheet","C168","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1627","v":"American Wood Council & Canadian Wood Council"}]
["Range","Master sheet","B169",null,{"$f":"$E$1789","v":"Plywood"}]
["-","_Master sheet","C169","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1627","v":"American Wood Council & Canadian Wood Council"}]
["Range","Master sheet","B170",null,"Polyiso - roof boards"]
["-","_Master sheet","C170","Ignore this cell of Master sheet. Company is not translatable","Carlisle"]
["Range","Master sheet","D170",null,"GRF cellulosic facer",null,null,"2023_July_new"]
["Range","Master sheet","E170",null,"R 5.8/inch"]
["Range","Master sheet","B172",null,{"$f":"$E$1795","v":"Polyiso - roof boards"}]
["-","_Master sheet","C172","Ignore this cell of Master sheet. Company is not translatable","Hunter"]
["Range","Master sheet","D172",null,"Polysio Roof insulation boards",null,null,"2023_July_new"]
["Range","Master sheet","E172",null,{"$f":"$E$1798","v":"R 5.8/inch"}]
["Range","Master sheet","B174",null,{"$f":"$E$1795","v":"Polyiso - roof boards"}]
["-","_Master sheet","C174","Ignore this cell of Master sheet. Company is not translatable","PIMA"]
["Range","Master sheet","D174",null,"Includes: Atlas, Firestone, GAF, Johns Manville, Rmax"]
["Range","Master sheet","E174",null,{"$f":"$E$1798","v":"R 5.8/inch"}]
["Range","Master sheet","B175",null,{"$f":"$E$1795","v":"Polyiso - roof boards"}]
["-","_Master sheet","C175","Ignore this cell of Master sheet. Company is not translatable","Versico"]
["Range","Master sheet","D175",null,"VersiCore, SecurShield, DuraFaceR"]
["Range","Master sheet","E175",null,{"$f":"$E$1798","v":"R 5.8/inch"}]
["Range","Master sheet","B176",null,"Polyiso - wall boards"]
["-","_Master sheet","C176","Ignore this cell of Master sheet. Company is not translatable","Dow Chemical Company"]
["Range","Master sheet","D176",null,"Tuff-R, Super Tuff-R, Thermax"]
["Range","Master sheet","E176",null,"R 6.5/inch"]
["Range","Master sheet","B177",null,{"$f":"$E$1811","v":"Polyiso - wall boards"}]
["-","_Master sheet","C177","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1800","v":"Hunter"}]
["Range","Master sheet","D177",null,"Polysio Wall insulation boards",null,null,"2023_July_new"]
["Range","Master sheet","E177",null,{"$f":"$E$1814","v":"R 6.5/inch"}]
["Range","Master sheet","B179",null,{"$f":"$E$1811","v":"Polyiso - wall boards"}]
["-","_Master sheet","C179","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1804","v":"PIMA"}]
["Range","Master sheet","D179",null,{"$f":"$E$1805","v":"Includes: Atlas, Firestone, GAF, Johns Manville, Rmax"}]
["Range","Master sheet","E179",null,{"$f":"$E$1814","v":"R 6.5/inch"}]
["Range","Master sheet","B180",null,"Polypropylene siding"]
["-","_Master sheet","C180","Ignore this cell of Master sheet. Company is not translatable","Novik"]
["Range","Master sheet","D180",null,"NovikStone, NovikShake"]
["Range","Master sheet","E180",null,"Avg of 5 products"]
["Range","Master sheet","B181",null,{"$f":"$E$1823","v":"Polypropylene siding"}]
["-","_Master sheet","C181","Ignore this cell of Master sheet. Company is not translatable","Vinyl Siding Institute "]
["Range","Master sheet","E181",null,"0.085\" Single 7\" wood Shake appearance",null,null,"2023_July_new"]
["Range","Master sheet","B183",null,"Polypropylene ICF webbing"]
["Range","Master sheet","B184",null,"PVC Roofing Membrane"]
["-","_Master sheet","C184","Ignore this cell of Master sheet. Company is not translatable","CIFA"]
["Range","Master sheet","D184",null,"Includes: Canadian General-Tower, Duro-Last, FiberTite"]
["Range","Master sheet","E184",null,"48 mils"]
["Range","Master sheet","B185",null,"Rammed earth"]
["Range","Master sheet","D185",null,"Stabilized with 3% NHL"]
["Range","Master sheet","B186",null,{"$f":"$E$1835","v":"Rammed earth"}]
["Range","Master sheet","D186",null,"Stabilized with 5% cement"]
["Range","Master sheet","B187",null,{"$f":"$E$1835","v":"Rammed earth"}]
["Range","Master sheet","D187",null,"Stabilized with 8% cement"]
["Range","Master sheet","B188",null,"Rebar"]
["-","_Master sheet","C188","Ignore this cell of Master sheet. Company is not translatable","Concrete Reinforcing Steel Institute"]
["Range","Master sheet","E188",null,"10M"]
["Range","Master sheet","B189",null,{"$f":"$E$1841","v":"Rebar"}]
["-","_Master sheet","C189","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1842","v":"Concrete Reinforcing Steel Institute"}]
["Range","Master sheet","E189",null,"15M"]
["Range","Master sheet","B190",null,"Rubber flooring"]
["-","_Master sheet","C190","Ignore this cell of Master sheet. Company is not translatable","ECOsurfaces"]
["Range","Master sheet","D190",null,{"$f":"$E$1848","v":"ECOsurfaces"}]
["Range","Master sheet","B191",null,{"$f":"$E$1847","v":"Rubber flooring"}]
["-","_Master sheet","C191","Ignore this cell of Master sheet. Company is not translatable","Resilient Floor Covering Institute"]
["Range","Master sheet","D191",null,"Includes tiles and rolls from American Biltrite, Armstrong, Burke, FLEXCO, Johnsonite, Mannington, Roppe, Tarkett"]
["Range","Master sheet","B192",null,"SBS Modified Bitumen Roofing"]
["-","_Master sheet","C192","Ignore this cell of Master sheet. Company is not translatable","ARMA"]
["Range","Master sheet","D192",null,"Includes: CertainTeed, Firestone, GAF, Henry, IKO, Johns Mansville, Malarkey, Siplast, Soprema"]
["Range","Master sheet","B193",null,"SIP panel - EPS foam core"]
["Range","Master sheet","E193",null,"7/16\" OSB, Type II EPS"]
["Range","Master sheet","B194",null,"SIP panel - Straw core"]
["-","_Master sheet","C194","Ignore this cell of Master sheet. Company is not translatable","Agriboard"]
["Range","Master sheet","D194",null,"Agriboard 7-7/8\""]
["Range","Master sheet","E194",null,"R?/inch"]
["Range","Master sheet","B195",null,"Spray polyurethane foam - Closed Cell (HFC)"]
["-","_Master sheet","C195","Ignore this cell of Master sheet. Company is not translatable","SPFA"]
["Range","Master sheet","E195",null,"R 6.6/inch"]
["Range","Master sheet","B196",null,"Spray polyurethane foam - Closed Cell - HFO gas filled",null,null,"2023_July_new"]
["-","_Master sheet","C196","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1863","v":"SPFA"}]
["Range","Master sheet","E196",null,{"$f":"$E$1864","v":"R 6.6/inch"}]
["Range","Master sheet","B198",null,"Spray polyurethane foam - High Density (HFC)"]
["-","_Master sheet","C198","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1863","v":"SPFA"}]
["Range","Master sheet","E198",null,"R 6.3/inch"]
["Range","Master sheet","B199",null,"Spray polyurethane foam - High Density - HFO gas filled",null,null,"2023_July_new"]
["-","_Master sheet","C199","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1863","v":"SPFA"}]
["Range","Master sheet","E199",null,{"$f":"$E$1814","v":"R 6.5/inch"}]
["Range","Master sheet","B201",null,"Spray polyurethane foam - Open Cell (HFC)"]
["-","_Master sheet","C201","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1863","v":"SPFA"}]
["Range","Master sheet","E201",null,"R 4.1/inch"]
["Range","Master sheet","B202",null,"Spray polyurethane foam - Open Cell - HFO gas",null,null,"2023_July_new"]
["-","_Master sheet","C202","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1863","v":"SPFA"}]
["Range","Master sheet","E202",null,{"$f":"$E$1876","v":"R 4.1/inch"}]
["Range","Master sheet","B204",null,"Steel beam"]
["-","_Master sheet","C204","Ignore this cell of Master sheet. Company is not translatable","American Institute of Steel Construction"]
["Range","Master sheet","D204",null,"Hot-rolled strucutural steel"]
["Range","Master sheet","E204",null,"W150x22 (W6x15)"]
["Range","Master sheet","B205",null,{"$f":"$E$1880","v":"Steel beam"}]
["-","_Master sheet","C205","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1881","v":"American Institute of Steel Construction"}]
["Range","Master sheet","D205",null,{"$f":"$E$1882","v":"Hot-rolled strucutural steel"}]
["Range","Master sheet","E205",null,"W200x22 (W8x15)"]
["Range","Master sheet","B206",null,{"$f":"$E$1880","v":"Steel beam"}]
["-","_Master sheet","C206","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1881","v":"American Institute of Steel Construction"}]
["Range","Master sheet","D206",null,{"$f":"$E$1882","v":"Hot-rolled strucutural steel"}]
["Range","Master sheet","E206",null,"W200x27 (W8x18)"]
["Range","Master sheet","B207",null,{"$f":"$E$1880","v":"Steel beam"}]
["-","_Master sheet","C207","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1881","v":"American Institute of Steel Construction"}]
["Range","Master sheet","D207",null,{"$f":"$E$1882","v":"Hot-rolled strucutural steel"}]
["Range","Master sheet","E207",null,"W200x31 (W8x21)"]
["Range","Master sheet","B208",null,{"$f":"$E$1880","v":"Steel beam"}]
["-","_Master sheet","C208","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1881","v":"American Institute of Steel Construction"}]
["Range","Master sheet","D208",null,{"$f":"$E$1882","v":"Hot-rolled strucutural steel"}]
["Range","Master sheet","E208",null,"W250x25 (W10x17)"]
["Range","Master sheet","B209",null,{"$f":"$E$1880","v":"Steel beam"}]
["-","_Master sheet","C209","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1881","v":"American Institute of Steel Construction"}]
["Range","Master sheet","D209",null,{"$f":"$E$1882","v":"Hot-rolled strucutural steel"}]
["Range","Master sheet","E209",null,"W250x33 (W10x22)"]
["Range","Master sheet","B210",null,{"$f":"$E$1880","v":"Steel beam"}]
["-","_Master sheet","C210","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1881","v":"American Institute of Steel Construction"}]
["Range","Master sheet","D210",null,{"$f":"$E$1882","v":"Hot-rolled strucutural steel"}]
["Range","Master sheet","E210",null,"W250x39 (W10x26)"]
["Range","Master sheet","B211",null,{"$f":"$E$1880","v":"Steel beam"}]
["-","_Master sheet","C211","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1881","v":"American Institute of Steel Construction"}]
["Range","Master sheet","D211",null,{"$f":"$E$1882","v":"Hot-rolled strucutural steel"}]
["Range","Master sheet","E211",null,"W310x33 (W12x22)"]
["Range","Master sheet","B212",null,{"$f":"$E$1880","v":"Steel beam"}]
["-","_Master sheet","C212","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1881","v":"American Institute of Steel Construction"}]
["Range","Master sheet","D212",null,{"$f":"$E$1882","v":"Hot-rolled strucutural steel"}]
["Range","Master sheet","E212",null,"W310x39 (W12x26)"]
["Range","Master sheet","B213",null,"Steel joist, open web"]
["-","_Master sheet","C213","Ignore this cell of Master sheet. Company is not translatable","Steel Joist Institute"]
["Range","Master sheet","E213",null,"12\" 12K3 joist"]
["Range","Master sheet","B214",null,"Steel post"]
["-","_Master sheet","C214","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1648","v":"Generic"}]
["Range","Master sheet","E214",null,"3.5 x 0.216\" (89 x 5.5 mm), Sched 40 STD"]
["Range","Master sheet","B215",null,"Steel studs - Load bearing"]
["-","_Master sheet","C215","Ignore this cell of Master sheet. Company is not translatable","ClarkDietrich"]
["Range","Master sheet","E215",null,"600-S-137-54, 16 gauge"]
["Range","Master sheet","B217",null,{"$f":"$E$1922","v":"Steel studs - Load bearing"}]
["-","_Master sheet","C217","Ignore this cell of Master sheet. Company is not translatable","MarinoWARE"]
["Range","Master sheet","D217",null,"Structural stud and track"]
["Range","Master sheet","E217",null,"600-S-137-54, 16 gauge, \"2x6\"",null,null,"2023_July_new"]
["Range","Master sheet","B219",null,{"$f":"$E$1922","v":"Steel studs - Load bearing"}]
["-","_Master sheet","C219","Ignore this cell of Master sheet. Company is not translatable","MBA Building Supplies"]
["Range","Master sheet","E219",null,{"$f":"$E$1924","v":"600-S-137-54, 16 gauge"}]
["Range","Master sheet","B220",null,{"$f":"$E$1922","v":"Steel studs - Load bearing"}]
["-","_Master sheet","C220","Ignore this cell of Master sheet. Company is not translatable","Scafco"]
["Range","Master sheet","E220",null,{"$f":"$E$1924","v":"600-S-137-54, 16 gauge"}]
["Range","Master sheet","B221",null,{"$f":"$E$1922","v":"Steel studs - Load bearing"}]
["-","_Master sheet","C221","Ignore this cell of Master sheet. Company is not translatable","Steel Recycling Institute"]
["Range","Master sheet","E221",null,{"$f":"$E$1924","v":"600-S-137-54, 16 gauge"}]
["Range","Master sheet","B222",null,"Steel studs - Non-loadbearing"]
["-","_Master sheet","C222","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1923","v":"ClarkDietrich"}]
["Range","Master sheet","E222",null,"362-S-125-18, 20EQ gauge, \"2x4\"",null,null,"2023_July_new"]
["Range","Master sheet","B224",null,{"$f":"$E$1938","v":"Steel studs - Non-loadbearing"}]
["-","_Master sheet","C224","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1926","v":"MarinoWARE"}]
["Range","Master sheet","D224",null,"Viper Stud Viper 20"]
["Range","Master sheet","E224",null,{"$f":"$E$1940","v":"362-S-125-18, 20EQ gauge, \"2x4\""},null,null,"2023_July_new"]
["Range","Master sheet","B226",null,{"$f":"$E$1938","v":"Steel studs - Non-loadbearing"}]
["-","_Master sheet","C226","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1930","v":"MBA Building Supplies"}]
["Range","Master sheet","E226",null,"362-S-125-18, 20EQ gauge, ProSTUD, ProTRAK"]
["Range","Master sheet","B227",null,{"$f":"$E$1938","v":"Steel studs - Non-loadbearing"}]
["-","_Master sheet","C227","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1933","v":"Scafco"}]
["Range","Master sheet","E227",null,"362VS125-18, 20EQ gauge"]
["Range","Master sheet","B228",null,{"$f":"$E$1938","v":"Steel studs - Non-loadbearing"}]
["-","_Master sheet","C228","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1936","v":"Steel Recycling Institute"}]
["Range","Master sheet","E228",null,"362-S-125-18, 20EQ gauge"]
["Range","Master sheet","B229",null,"Straw Bale"]
["Range","Master sheet","D229",null,"Wheat & rye straw"]
["Range","Master sheet","E229",null,"R 3.3/inch"]
["Range","Master sheet","B230",null,"Straw Panels"]
["-","_Master sheet","C230","Ignore this cell of Master sheet. Company is not translatable","EcoCocon"]
["Range","Master sheet","E230",null,"R 2.9/inch"]
["Range","Master sheet","B231",null,"Acrylic Stucco Textured Finish"]
["-","_Master sheet","C231","Ignore this cell of Master sheet. Company is not translatable","Sto"]
["Range","Master sheet","D231",null,"Stolit 1.0, Stolit 1.5, Stolit Freeform"]
["Range","Master sheet","B232",null,"TPO Roofing Membrane"]
["-","_Master sheet","C232","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1796","v":"Carlisle"}]
["Range","Master sheet","E232",null,"60 mils"]
["Range","Master sheet","B233",null,"Vacuum Insulated Panel"]
["-","_Master sheet","C233","Ignore this cell of Master sheet. Company is not translatable","Porextherm "]
["Range","Master sheet","D233",null,"Vacupor"]
["Range","Master sheet","E233",null,"R 30/inch"]
["Range","Master sheet","B234",null,"Vinyl flooring"]
["-","_Master sheet","C234","Ignore this cell of Master sheet. Company is not translatable","Altro"]
["Range","Master sheet","D234",null,"Altro Lavencia Click"]
["Range","Master sheet","B235",null,{"$f":"$E$1970","v":"Vinyl flooring"}]
["-","_Master sheet","C235","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1971","v":"Altro"}]
["Range","Master sheet","D235",null,"Altro Lavencia Plus"]
["Range","Master sheet","B236",null,{"$f":"$E$1970","v":"Vinyl flooring"}]
["-","_Master sheet","C236","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1697","v":"Gerflor "}]
["Range","Master sheet","D236",null,"Creation 70 CLIC"]
["Range","Master sheet","B237",null,{"$f":"$E$1970","v":"Vinyl flooring"}]
["-","_Master sheet","C237","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1851","v":"Resilient Floor Covering Institute"}]
["Range","Master sheet","D237",null,"Includes tile products from Armstrong, Congoleum, Tarkett"]
["Range","Master sheet","B238",null,"Vinyl Siding"]
["-","_Master sheet","C238","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1828","v":"Vinyl Siding Institute "}]
["Range","Master sheet","D238",null,"Double 4.5\" products from: American Original, Associated Materials, CertainTeed, Novik, Ply Gem"]
["Range","Master sheet","E238",null,"0.040\" Double 4.5\""]
["Range","Master sheet","B240",null,"Waterproofing membrane adhesive"]
["-","_Master sheet","C240","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1278","v":"GCP"}]
["Range","Master sheet","D240",null,"Bituthene"]
["Range","Master sheet","B241",null,"Welded wire mesh"]
["-","_Master sheet","C241","Ignore this cell of Master sheet. Company is not translatable","Serfas"]
["Range","Master sheet","E241",null,"6\" x 6\" x 6/6g"]
["Range","Master sheet","B242",null,"Window - double pane"]
["Range","Master sheet","E242",null,"Fiberglass frame"]
["Range","Master sheet","B243",null,{"$f":"$E$1992","v":"Window - double pane"}]
["-","_Master sheet","C243","Ignore this cell of Master sheet. Company is not translatable","Andersen"]
["Range","Master sheet","D243",null,"Fibrex"]
["Range","Master sheet","E243",null,"PVC & Wood composite"]
["Range","Master sheet","B244",null,{"$f":"$E$1992","v":"Window - double pane"}]
["Range","Master sheet","E244",null,"Vinyl frame"]
["Range","Master sheet","B245",null,{"$f":"$E$1992","v":"Window - double pane"}]
["Range","Master sheet","E245",null,"Wood frame"]
["Range","Master sheet","B246",null,{"$f":"$E$1992","v":"Window - double pane"}]
["Range","Master sheet","E246",null,{"$f":"$E$2001","v":"Wood frame"}]
["Range","Master sheet","B247",null,{"$f":"$E$1992","v":"Window - double pane"}]
["Range","Master sheet","E247",null,"Wood frame, aluminum cladding"]
["Range","Master sheet","B248",null,{"$f":"$E$1992","v":"Window - double pane"}]
["Range","Master sheet","E248",null,{"$f":"$E$2005","v":"Wood frame, aluminum cladding"}]
["Range","Master sheet","B249",null,"Window - triple pane"]
["Range","Master sheet","E249",null,{"$f":"$E$1993","v":"Fiberglass frame"}]
["Range","Master sheet","B250",null,{"$f":"$E$2008","v":"Window - triple pane"}]
["Range","Master sheet","E250",null,{"$f":"$E$1999","v":"Vinyl frame"}]
["Range","Master sheet","B251",null,{"$f":"$E$2008","v":"Window - triple pane"}]
["Range","Master sheet","E251",null,{"$f":"$E$2001","v":"Wood frame"}]
["Range","Master sheet","B252",null,{"$f":"$E$2008","v":"Window - triple pane"}]
["Range","Master sheet","E252",null,{"$f":"$E$2001","v":"Wood frame"}]
["Range","Master sheet","B253",null,{"$f":"$E$2008","v":"Window - triple pane"}]
["Range","Master sheet","E253",null,{"$f":"$E$2005","v":"Wood frame, aluminum cladding"}]
["Range","Master sheet","B254",null,{"$f":"$E$2008","v":"Window - triple pane"}]
["Range","Master sheet","E254",null,{"$f":"$E$2005","v":"Wood frame, aluminum cladding"}]
["Range","Master sheet","B255",null,"Wood chip cement ICF"]
["-","_Master sheet","C255","Ignore this cell of Master sheet. Company is not translatable","Isospan"]
["Range","Master sheet","D255",null,"Okopur"]
["Range","Master sheet","E255",null,"NEEDS REVIEW"]
["Range","Master sheet","B256",null,{"$f":"$E$2020","v":"Wood chip cement ICF"}]
["-","_Master sheet","C256","Ignore this cell of Master sheet. Company is not translatable","Nexcem, Faswall"]
["Range","Master sheet","E256",null,"12\" R22 block"]
["Range","Master sheet","B257",null,{"$f":"$E$2020","v":"Wood chip cement ICF"}]
["-","_Master sheet","C257","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$2025","v":"Nexcem, Faswall"}]
["Range","Master sheet","E257",null,"14\" R28 block"]
["Range","Master sheet","B258",null,"Wood fiber - loose fill"]
["-","_Master sheet","C258","Ignore this cell of Master sheet. Company is not translatable","GUTEX"]
["Range","Master sheet","D258",null,"ThermoFiber"]
["Range","Master sheet","E258",null,{"$f":"$E$1351","v":"R 3.6/inch"}]
["Range","Master sheet","B260",null,"Wood fiber batt"]
["-","_Master sheet","C260","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$2031","v":"GUTEX"}]
["Range","Master sheet","D260",null,"ThermoFlex"]
["Range","Master sheet","E260",null,"R 4/inch "]
["Range","Master sheet","B261",null,{"$f":"$E$2034","v":"Wood fiber batt"}]
["-","_Master sheet","C261","Ignore this cell of Master sheet. Company is not translatable","Pavatex"]
["Range","Master sheet","D261",null,"Pavaflex"]
["Range","Master sheet","E261",null,{"$f":"$E$1752","v":"R 3.8/inch"}]
["Range","Master sheet","B262",null,{"$f":"$E$2034","v":"Wood fiber batt"}]
["-","_Master sheet","C262","Ignore this cell of Master sheet. Company is not translatable","Steico"]
["Range","Master sheet","D262",null,"SteicoFlex"]
["Range","Master sheet","E262",null,{"$f":"$E$1752","v":"R 3.8/inch"}]
["Range","Master sheet","B263",null,"Wood fiber board"]
["-","_Master sheet","C263","Ignore this cell of Master sheet. Company is not translatable","AWC/CWC"]
["Range","Master sheet","D263",null,"Includes: Georgia Pacific, Louisville, BPC, Temple-Inland, Blue Ridge, Int'l Bildrite"]
["Range","Master sheet","E263",null,"R 2.7/inch"]
["Range","Master sheet","B264",null,{"$f":"$E$2046","v":"Wood fiber board"}]
["-","_Master sheet","C264","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$2031","v":"GUTEX"}]
["Range","Master sheet","D264",null,"Multi-Therm"]
["Range","Master sheet","E264",null,"R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm"]
["Range","Master sheet","B266",null,{"$f":"$E$2046","v":"Wood fiber board"}]
["-","_Master sheet","C266","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$2039","v":"Pavatex"}]
["Range","Master sheet","D266",null,"Pavatherm"]
["Range","Master sheet","E266",null,"R 3.4/inch"]
["Range","Master sheet","B267",null,{"$f":"$E$2046","v":"Wood fiber board"}]
["-","_Master sheet","C267","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$2043","v":"Steico"}]
["Range","Master sheet","D267",null,"Special Dry"]
["Range","Master sheet","E267",null,"R 3.6/inch, 40, 120, 140, 160, 180, 200 mm"]
["Range","Master sheet","B268",null,"Wood framing - Softwood"]
["-","_Master sheet","C268","Ignore this cell of Master sheet. Company is not translatable","Roseburg"]
["Range","Master sheet","B269",null,"Wood framing & siding - Redwood"]
["-","_Master sheet","C269","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1627","v":"American Wood Council & Canadian Wood Council"}]
["Range","Master sheet","B270",null,"Wood framing & siding - SPF"]
["-","_Master sheet","C270","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1627","v":"American Wood Council & Canadian Wood Council"}]
["Range","Master sheet","B271",null,"Wood I joist"]
["-","_Master sheet","C271","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1627","v":"American Wood Council & Canadian Wood Council"}]
["Range","Master sheet","E271",null,"TJI 230/360"]
["Range","Master sheet","B272",null,{"$f":"$E$2068","v":"Wood I joist"}]
["-","_Master sheet","C272","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$2063","v":"Roseburg"}]
["Range","Master sheet","D272",null,"RFPI Joist"]
["Range","Master sheet","B273",null,"Wood floor truss - prefabricated"]
["-","_Master sheet","C273","Ignore this cell of Master sheet. Company is not translatable","Quebec Wood Export Bureau"]
["Range","Master sheet","D273",null,"Common (Warren, 45 deg) web pattern"]
["Range","Master sheet","E273",null,"Top chord bearing, variable depth"]
["Range","Master sheet","B274",null,"Wood roof truss - prefabricated"]
["-","_Master sheet","C274","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$2075","v":"Quebec Wood Export Bureau"}]
["Range","Master sheet","D274",null,"Common (Double Howe) Gabrel Roof"]
["Range","Master sheet","E274",null,"2x6 Chords, 2x4 Webs, 4:12 Pitch, 40 ft span, 20\" overhang"]
["Range","Master sheet","B275",null,"Wood wool boards"]
["-","_Master sheet","C275","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1301","v":"Armstrong"}]
["Range","Master sheet","D275",null,"Tectum"]
["Range","Master sheet","E275",null,"2\" (50.8 mm)"]
["Range","Master sheet","B276",null,"Wool batt"]
["-","_Master sheet","C276","Ignore this cell of Master sheet. Company is not translatable","Havelock Wool"]
["Range","Master sheet","E276",null,{"$f":"$E$1351","v":"R 3.6/inch"}]
["Range","Master sheet","B277",null,"Wool loose fill"]
["-","_Master sheet","C277","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$2087","v":"Havelock Wool"}]
["Range","Master sheet","E277",null,"R 4.4/inch"]
["Range","Master sheet","B278",null,"XPS foam board"]
["-","_Master sheet","C278","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1812","v":"Dow Chemical Company"}]
["Range","Master sheet","D278",null,"Styrofoam SM"]
["Range","Master sheet","E278",null,"R 5/inch"]
["Range","Master sheet","B279",null,{"$f":"$E$2092","v":"XPS foam board"}]
["-","_Master sheet","C279","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1288","v":"Owens Corning"}]
["Range","Master sheet","D279",null,"Foamular 250 "]
["Range","Master sheet","E279",null,{"$f":"$E$2095","v":"R 5/inch"}]
["Range","Master sheet","B280",null,{"$f":"$E$2092","v":"XPS foam board"}]
["-","_Master sheet","C280","Ignore this cell of Master sheet. Company is not translatable",{"$f":"$E$1288","v":"Owens Corning"}]
["Range","Master sheet","D280",null,"Foamular NGX 250 ",null,null,"2023_July_new"]
["Range","Master sheet","E280",null,{"$f":"$E$2095","v":"R 5/inch"}]
["Range","Master sheet","B281",null,"from Composite Master Sheet"]
["Range","Master sheet","B282",null,{"$f":"$E$2104","v":"from Composite Master Sheet"}]
["Range","Master sheet","B283",null,"from Composite Master Sheet"]
["Range","Master sheet","B284",null,"from Composite Master Sheet"]
["Range","Master sheet","B285",null,"from Composite Master Sheet"]
["Range","Master sheet","B286",null,"from Composite Master Sheet"]
["Range","Master sheet","B287",null,"from Composite Master Sheet"]
["Range","Master sheet","B288",null,"from Composite Master Sheet"]
["Range","Master sheet","B289",null,"from Composite Master Sheet"]
["Range","Master sheet","B290",null,"from Composite Master Sheet"]
["Range","Master sheet","B291",null,"from Composite Master Sheet"]
["Range","Master sheet","B292",null,"Concrete - 25 MPa, Quebec Baseline Average",null,null,"2023_July_new"]
["Range","Master sheet","D292",null,"Can. Quebec Avg.",null,null,"2023_July_new"]
["Range","Master sheet","B293",null,"Concrete - 25 MPa, 10% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D293",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B294",null,"Concrete - 25 MPa, 10% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D294",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B295",null,"Concrete - 25 MPa, 20% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D295",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B296",null,"Concrete - 25 MPa, 20% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D296",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B297",null,"Concrete - 25 MPa, 30% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D297",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B298",null,"Concrete - 25 MPa, 30% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D298",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B299",null,"Concrete - 30 MPa, Quebec Baseline Average",null,null,"2023_July_new"]
["Range","Master sheet","D299",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B300",null,"Concrete - 30 MPa, 10% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D300",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B301",null,"Concrete - 30 MPa, 10% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D301",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B302",null,"Concrete - 30 MPa, 20% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D302",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B303",null,"Concrete - 30 MPa, 20% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D303",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B304",null,"Concrete - 30 MPa, 30% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D304",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B305",null,"Concrete - 30 MPa, 30% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D305",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B306",null,"Concrete - 35 MPa, Quebec Baseline Average",null,null,"2023_July_new"]
["Range","Master sheet","D306",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B307",null,"Concrete - 35 MPa, 10% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D307",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B308",null,"Concrete - 35 MPa, 10% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D308",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B309",null,"Concrete - 35 MPa, 20% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D309",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B310",null,"Concrete - 35 MPa, 20% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D310",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B311",null,"Concrete - 35 MPa, 30% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D311",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B312",null,"Concrete - 35 MPa, 30% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D312",null,{"$f":"$E$2116","v":"Can. Quebec Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B313",null,"Concrete - 25 MPa, GU",null,null,"2023_July_new"]
["Range","Master sheet","D313",null,"Can. Ontario Avg.",null,null,"2023_July_new"]
["Range","Master sheet","B314",null,"Concrete - 25 MPa, 15% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D314",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B315",null,"Concrete - 25 MPa, 25% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D315",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B316",null,"Concrete - 25 MPa, 35% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D316",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B317",null,"Concrete - 25 MPa, 50% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D317",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B318",null,"Concrete - 30 MPa, GU",null,null,"2023_July_new"]
["Range","Master sheet","D318",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B319",null,"Concrete - 30 MPa, 15% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D319",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B320",null,"Concrete - 30 MPa, 25% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D320",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B321",null,"Concrete - 30 MPa, 35% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D321",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B322",null,"Concrete - 30 MPa, 50% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D322",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B323",null,"Concrete - 35 MPa, GU",null,null,"2023_July_new"]
["Range","Master sheet","D323",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B324",null,"Concrete - 35 MPa, 15% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D324",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B325",null,"Concrete - 35 MPa, 25% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D325",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B326",null,"Concrete - 35 MPa, 35% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D326",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B327",null,"Concrete - 35 MPa, 50% SL, GU",null,null,"2023_July_new"]
["Range","Master sheet","D327",null,{"$f":"$E$2158","v":"Can. Ontario Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B328",null,{"$f":"$E$2157","v":"Concrete - 25 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D328",null,"Can. Sask Avg.",null,null,"2023_July_new"]
["Range","Master sheet","B329",null,{"$f":"$E$2119","v":"Concrete - 25 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D329",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B330",null,{"$f":"$E$2123","v":"Concrete - 25 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D330",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B331",null,{"$f":"$E$2127","v":"Concrete - 25 MPa, 30% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D331",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B332",null,"Concrete - 25 MPa, 40% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D332",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B333",null,{"$f":"$E$2167","v":"Concrete - 30 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D333",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B334",null,{"$f":"$E$2133","v":"Concrete - 30 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D334",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B335",null,{"$f":"$E$2137","v":"Concrete - 30 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D335",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B336",null,{"$f":"$E$2141","v":"Concrete - 30 MPa, 30% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D336",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B337",null,"Concrete - 30 MPa, 40% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D337",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B338",null,{"$f":"$E$2177","v":"Concrete - 35 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D338",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B339",null,{"$f":"$E$2147","v":"Concrete - 35 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D339",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B340",null,{"$f":"$E$2151","v":"Concrete - 35 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D340",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B341",null,{"$f":"$E$2155","v":"Concrete - 35 MPa, 30% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D341",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B342",null,"Concrete - 35 MPa, 40% FA, GU",null,null,"2023_July_new"]
["Range","Master sheet","D342",null,{"$f":"$E$2188","v":"Can. Sask Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B343",null,{"$f":"$E$2157","v":"Concrete - 25 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D343",null,"Can. Manitoba Avg.",null,null,"2023_July_new"]
["Range","Master sheet","B344",null,{"$f":"$E$2119","v":"Concrete - 25 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D344",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B345",null,{"$f":"$E$2123","v":"Concrete - 25 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D345",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B346",null,{"$f":"$E$2127","v":"Concrete - 25 MPa, 30% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D346",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B347",null,{"$f":"$E$2195","v":"Concrete - 25 MPa, 40% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D347",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B348",null,{"$f":"$E$2167","v":"Concrete - 30 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D348",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B349",null,{"$f":"$E$2133","v":"Concrete - 30 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D349",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B350",null,{"$f":"$E$2137","v":"Concrete - 30 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D350",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B351",null,{"$f":"$E$2141","v":"Concrete - 30 MPa, 30% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D351",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B352",null,{"$f":"$E$2205","v":"Concrete - 30 MPa, 40% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D352",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B353",null,{"$f":"$E$2177","v":"Concrete - 35 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D353",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B354",null,{"$f":"$E$2147","v":"Concrete - 35 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D354",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B355",null,{"$f":"$E$2151","v":"Concrete - 35 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D355",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B356",null,{"$f":"$E$2155","v":"Concrete - 35 MPa, 30% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D356",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B357",null,{"$f":"$E$2215","v":"Concrete - 35 MPa, 40% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D357",null,{"$f":"$E$2218","v":"Can. Manitoba Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B358",null,{"$f":"$E$2157","v":"Concrete - 25 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D358",null,"Can. BC Avg.",null,null,"2023_July_new"]
["Range","Master sheet","B359",null,"Concrete - 25 MPa, 15% SCM, GU",null,null,"2023_July_new"]
["Range","Master sheet","D359",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B360",null,"Concrete - 25 MPa, 25% SCM, GU",null,null,"2023_July_new"]
["Range","Master sheet","D360",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B361",null,"Concrete - 25 MPa, 40% SCM, GU",null,null,"2023_July_new"]
["Range","Master sheet","D361",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B362",null,{"$f":"$E$2167","v":"Concrete - 30 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D362",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B363",null,"Concrete - 30 MPa, 15% SCM, GU",null,null,"2023_July_new"]
["Range","Master sheet","D363",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B364",null,"Concrete - 30 MPa, 25% SCM, GU",null,null,"2023_July_new"]
["Range","Master sheet","D364",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B365",null,"Concrete - 30 MPa, 40% SCM, GU",null,null,"2023_July_new"]
["Range","Master sheet","D365",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B366",null,{"$f":"$E$2177","v":"Concrete - 35 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D366",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B367",null,"Concrete - 35 MPa, 15% SCM, GU",null,null,"2023_July_new"]
["Range","Master sheet","D367",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B368",null,"Concrete - 35 MPa, 25% SCM, GU",null,null,"2023_July_new"]
["Range","Master sheet","D368",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B369",null,"Concrete - 35 MPa, 40% SCM, GU",null,null,"2023_July_new"]
["Range","Master sheet","D369",null,{"$f":"$E$2248","v":"Can. BC Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B370",null,{"$f":"$E$2157","v":"Concrete - 25 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D370",null,"Can. Atlantic Avg.",null,null,"2023_July_new"]
["Range","Master sheet","B371",null,{"$f":"$E$2119","v":"Concrete - 25 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D371",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B372",null,{"$f":"$E$2123","v":"Concrete - 25 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D372",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B373",null,{"$f":"$E$2127","v":"Concrete - 25 MPa, 30% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D373",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B374",null,{"$f":"$E$2195","v":"Concrete - 25 MPa, 40% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D374",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B375",null,{"$f":"$E$2167","v":"Concrete - 30 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D375",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B376",null,{"$f":"$E$2133","v":"Concrete - 30 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D376",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B377",null,{"$f":"$E$2137","v":"Concrete - 30 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D377",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B378",null,{"$f":"$E$2141","v":"Concrete - 30 MPa, 30% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D378",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B379",null,{"$f":"$E$2205","v":"Concrete - 30 MPa, 40% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D379",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B380",null,{"$f":"$E$2177","v":"Concrete - 35 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D380",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B381",null,{"$f":"$E$2147","v":"Concrete - 35 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D381",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B382",null,{"$f":"$E$2151","v":"Concrete - 35 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D382",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B383",null,{"$f":"$E$2155","v":"Concrete - 35 MPa, 30% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D383",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B384",null,{"$f":"$E$2215","v":"Concrete - 35 MPa, 40% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D384",null,{"$f":"$E$2272","v":"Can. Atlantic Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B385",null,{"$f":"$E$2157","v":"Concrete - 25 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D385",null,"Can. Alberta Avg.",null,null,"2023_July_new"]
["Range","Master sheet","B386",null,{"$f":"$E$2119","v":"Concrete - 25 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D386",null,{"$f":"$E$2302","v":"Can. Alberta Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B387",null,{"$f":"$E$2123","v":"Concrete - 25 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D387",null,{"$f":"$E$2302","v":"Can. Alberta Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B388",null,{"$f":"$E$2167","v":"Concrete - 30 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D388",null,{"$f":"$E$2302","v":"Can. Alberta Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B389",null,{"$f":"$E$2133","v":"Concrete - 30 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D389",null,{"$f":"$E$2302","v":"Can. Alberta Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B390",null,{"$f":"$E$2137","v":"Concrete - 30 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D390",null,{"$f":"$E$2302","v":"Can. Alberta Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B391",null,{"$f":"$E$2177","v":"Concrete - 35 MPa, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D391",null,{"$f":"$E$2302","v":"Can. Alberta Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B392",null,{"$f":"$E$2147","v":"Concrete - 35 MPa, 10% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D392",null,{"$f":"$E$2302","v":"Can. Alberta Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B393",null,{"$f":"$E$2151","v":"Concrete - 35 MPa, 20% FA, GU"},null,null,"2023_July_new"]
["Range","Master sheet","D393",null,{"$f":"$E$2302","v":"Can. Alberta Avg."},null,null,"2023_July_new"]
["Range","Master sheet","B394",null,{"$f":"$E$1970","v":"Vinyl flooring"},null,null,"2023_July_new"]
["Range","Master sheet","D394",null,"Luxury Vinyl Tile",null,null,"2023_July_new"]
["Range","Master sheet","B395",null,{"$f":"$E$1684","v":"Linoleum flooring"},null,null,"2023_July_new"]
["Range","Master sheet","D395",null,"DLW Linoleum Compact",null,null,"2023_July_new"]
["Range","Master sheet","E395",null,{"$f":"$E$1687","v":"2.5 mm sheet style linoleum"},null,null,"2023_July_new"]
["Range","Master sheet","B396",null,{"$f":"$E$1596","v":"Fiberglass loose fill"},null,null,"2023_July_new"]
["Range","Master sheet","D396",null,"Climate Pro, Attic Protector, JM Spider PLUS (Canada)",null,null,"2023_July_new"]
["Range","Master sheet","E396",null,"R 2.8/inch, Formaldehyde-free",null,null,"2023_July_new"]
["Range","Master sheet","B397",null,{"$f":"$E$1992","v":"Window - double pane"},null,null,"2023_July_new"]
["Range","Master sheet","D397",null,"E-series (Average Double-hung/Awning/Picture)",null,null,"2023_July_new"]
["Range","Master sheet","E397",null,{"$f":"$E$2005","v":"Wood frame, aluminum cladding"},null,null,"2023_July_new"]
["Range","Master sheet","B398",null,{"$f":"$E$1529","v":"Drywall 1/2\""},null,null,"2023_July_new"]
["Range","Master sheet","D398",null,"Gold Bond XP Gypsum Board ",null,null,"2023_July_new"]
["Range","Master sheet","B399",null,"Drywall 5/8\" Type X",null,null,"2023_July_new"]
["Range","Master sheet","D399",null,"Gold Bond XP Fire-Shield Gypsum Board ",null,null,"2023_July_new"]
["Range","Master sheet","E399",null,"5/8'' type X",null,null,"2023_July_new"]
["Range","Master sheet","B400",null,{"$f":"$E$1327","v":"Carpet"},null,null,"2023_July_new"]
["Range","Master sheet","D400",null,"Standard Back",null,null,"2023_July_new"]
["Range","Master sheet","E400",null,"all Broadloom styles",null,null,"2023_July_new"]
["Range","Master sheet","B401",null,{"$f":"$E$1970","v":"Vinyl flooring"},null,null,"2023_July_new"]
["Range","Master sheet","D401",null,{"$f":"$E$2320","v":"Luxury Vinyl Tile"},null,null,"2023_July_new"]
["Range","Master sheet","E401",null,"2.5 mm Tile and Plank",null,null,"2023_July_new"]
["Range","Master sheet","B402",null,{"$f":"$E$1281","v":"Asphalt Shingles"},null,null,"2023_July_new"]
["Range","Master sheet","D402",true,"Timberline Cool Series",null,null,"2023_July_new"]
["Range","Master sheet","B403",null,{"$f":"$E$1684","v":"Linoleum flooring"},null,null,"2023_July_new"]
["Range","Master sheet","D403",null,"Legato Flooring",null,null,"2023_July_new"]
["Range","Master sheet","E403",null,"liquid applied",null,null,"2023_July_new"]
["Range","Master sheet","B404",null,{"$f":"$E$1373","v":"Ceramic tile"},null,null,"2023_July_new"]
["Range","Master sheet","D404",null,"Ceramic - recycled content",null,null,"2023_July_new"]
["Range","Master sheet","E404",null,"Standard and Second grade",null,null,"2023_July_new"]
["Range","Master sheet","B405",null,{"$f":"$E$1373","v":"Ceramic tile"},null,null,"2023_July_new"]
["Range","Master sheet","D405",null,"Procelain - recycled content",null,null,"2023_July_new"]
["Range","Master sheet","E405",null,{"$f":"$E$2348","v":"Standard and Second grade"},null,null,"2023_July_new"]
["Range","Master sheet","B406",null,{"$f":"$E$1578","v":"Fiber Cement siding"},null,null,"2023_July_new"]
["Range","Master sheet","D406",null,"Pictura and Natura Pro",null,null,"2023_July_new"]
["Range","Master sheet","B407",null,{"$f":"$E$1578","v":"Fiber Cement siding"},null,null,"2023_July_new"]
["Range","Master sheet","D407",null,"Tectiva",null,null,"2023_July_new"]
["Range","Master sheet","B408",null,{"$f":"$E$1578","v":"Fiber Cement siding"},null,null,"2023_July_new"]
["Range","Master sheet","D408",null,"Natura, Textura and Materia",null,null,"2023_July_new"]
["Range","Master sheet","B409",null,{"$f":"$E$1957","v":"Straw Panels"},null,null,"2023_July_new"]
["Range","Master sheet","D409",null,"Standard and Brace Panels",null,null,"2023_July_new"]
["Range","Master sheet","E409",null,"40cm R16, panel only",null,null,"2023_July_new"]
["Range","Master sheet","B410",null,{"$f":"$E$1312","v":"Brick, Clay"},null,null,"2023_July_new"]
["Range","Master sheet","D410",null,"Slender - Thin Face Brick",null,null,"2023_July_new"]
["Range","Master sheet","E410",null,"2 1/4\" x 1/2\" x 7-1/2\" (57 x 12.7 mm x 190) incl. 3/8\" mortar",null,null,"2023_July_new"]
["Range","Master sheet","B411",null,{"$f":"$E$1312","v":"Brick, Clay"},null,null,"2023_July_new"]
["Range","Master sheet","D411",null,{"$f":"$E$1314","v":"Avg Face Brick"},null,null,"2023_July_new"]
["Range","Master sheet","E411",null,{"$f":"$E$1311","v":"3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"},null,null,"2023_July_new"]
["Range","Master sheet","B412",null,{"$f":"$E$1841","v":"Rebar"},null,null,"2023_July_new"]
["Range","Master sheet","D412",null,"Canadian sizes",null,null,"2023_July_new"]
["Range","Master sheet","B413",null,{"$f":"$E$1841","v":"Rebar"},null,null,"2023_July_new"]
["Range","Master sheet","D413",null,{"$f":"$E$2368","v":"Canadian sizes"},null,null,"2023_July_new"]
["Range","Master sheet","B414",null,{"$f":"$E$1841","v":"Rebar"},null,null,"2023_July_new"]
["Range","Master sheet","D414",null,{"$f":"$E$2368","v":"Canadian sizes"},null,null,"2023_July_new"]
["Range","Master sheet","B415",null,{"$f":"$E$1841","v":"Rebar"},null,null,"2023_July_new"]
["Range","Master sheet","D415",null,{"$f":"$E$2368","v":"Canadian sizes"},null,null,"2023_July_new"]
["Range","Master sheet","B416",null,{"$f":"$E$1841","v":"Rebar"},null,null,"2023_July_new"]
["Range","Master sheet","D416",null,{"$f":"$E$2368","v":"Canadian sizes"},null,null,"2023_July_new"]
["Range","Master sheet","B417",null,{"$f":"$E$1841","v":"Rebar"},null,null,"2023_July_new"]
["Range","Master sheet","D417",null,{"$f":"$E$2368","v":"Canadian sizes"},null,null,"2023_July_new"]
["Range","Master sheet","B418",null,{"$f":"$E$2046","v":"Wood fiber board"},null,null,"2023_July_new"]
["Range","Master sheet","D418",null,"Includes: MSL, Blue Ridge Fiberboard Inc.",null,null,"2023_July_new"]
["Range","Master sheet","B419",null,"(ARCHIVED 2023) XPS foam board",null,null,"2023_July_new"]
["Range","Master sheet","D419",null,"Styrofoam (Blue) (Legacy)",null,null,"2023_July_new"]
["Range","Master sheet","E419",null,"R 5.6/inch",null,null,"2023_July_new"]
["Range","Master sheet","B420",null,{"$f":"$E$2092","v":"XPS foam board"},null,null,"2023_July_new"]
["Range","Master sheet","D420",null,"Styrofoam (Grey, Reduced GWP)",null,null,"2023_July_new"]
["Range","Master sheet","E420",null,{"$f":"$E$2383","v":"R 5.6/inch"},null,null,"2023_July_new"]
["Range","Master sheet","B421",null,{"$f":"$E$2092","v":"XPS foam board"},null,null,"2023_July_new"]
["Range","Master sheet","D421",null,"Reduced GWP Grey Styrofoam™ (same as ST-100)",null,null,"2023_July_new"]
["Range","Master sheet","B422",null,{"$f":"$E$2092","v":"XPS foam board"},null,null,"2023_July_new"]
["Range","Master sheet","D422",null,"SOPRA-XPS",null,null,"2023_July_new"]
["Range","Master sheet","B423",null,{"$f":"$E$1745","v":"Mineral wool batt"},null,null,"2023_July_new"]
["Range","Master sheet","D423",null,"ComfortBatt R14",null,null,"2023_July_new"]
["Range","Master sheet","B424",null,{"$f":"$E$1745","v":"Mineral wool batt"},null,null,"2023_July_new"]
["Range","Master sheet","D424",null,"ComfortBatt R15",null,null,"2023_July_new"]
["Range","Master sheet","B425",null,{"$f":"$E$1745","v":"Mineral wool batt"},null,null,"2023_July_new"]
["Range","Master sheet","D425",null,"ComfortBatt R22",null,null,"2023_July_new"]
["Range","Master sheet","B426",null,{"$f":"$E$1745","v":"Mineral wool batt"},null,null,"2023_July_new"]
["Range","Master sheet","D426",null,"ComfortBatt R24",null,null,"2023_July_new"]
["Range","Master sheet","B427",null,{"$f":"$E$1745","v":"Mineral wool batt"},null,null,"2023_July_new"]
["Range","Master sheet","D427",null,"ComfortBatt R24 SS",null,null,"2023_July_new"]
["Range","Master sheet","E427",null,"R 4.0/inch, 6\" Steel Studs",null,null,"2023_July_new"]
["Range","Master sheet","B428",null,{"$f":"$E$1757","v":"Mineral wool board "},null,null,"2023_July_new"]
["Range","Master sheet","D428",null,"Comfortboard 80",null,null,"2023_July_new"]
["Range","Master sheet","B429",null,{"$f":"$E$1811","v":"Polyiso - wall boards"},null,null,"2023_July_new"]
["Range","Master sheet","D429",null,"Thermax",null,null,"2023_July_new"]
["Range","Master sheet","B430",null,"Laminated veneer lumber",null,null,"2023_July_new"]
["Range","Master sheet","D430",null,"RigidLam LVL",null,null,"2023_July_new"]
["Range","Master sheet","B431",null,"Spray polyurethane foam - Closed Cell (HFO)",null,null,"2023_July_new"]
["Range","Master sheet","D431",null,"Heatlok HFO & Heatlok Soya HFO",null,null,"2023_July_new"]
["Range","Master sheet","B432",null,{"$f":"$E$1811","v":"Polyiso - wall boards"},null,null,"2023_July_new"]
["Range","Master sheet","D432",null,"Includes: Atlas, Firestone, GAF, Johns Manville, Rmax, Carlisle, Iko, Soprema",null,null,"2023_July_new"]
["Range","Master sheet","B433",null,{"$f":"$E$1954","v":"Straw Bale"},null,null,"2023_July_new"]
["Range","Master sheet","D433",null,"Wheat & barley straw",null,null,"2023_July_new"]
["Range","Master sheet","B434",null,"Engineered Wood Siding & Trim",null,null,"2023_July_new"]
["Range","Master sheet","D434",null,"SmartSide",null,null,"2023_July_new"]
["Range","Master sheet","B435",null,{"$f":"$E$2414","v":"Engineered Wood Siding & Trim"},null,null,"2023_July_new"]
["Range","Master sheet","D435",null,{"$f":"$E$2415","v":"SmartSide"},null,null,"2023_July_new"]
["Range","Master sheet","B436",null,{"$f":"$E$2414","v":"Engineered Wood Siding & Trim"},null,null,"2023_July_new"]
["Range","Master sheet","D436",null,{"$f":"$E$2415","v":"SmartSide"},null,null,"2023_July_new"]
["Range","Master sheet","B437",null,{"$f":"$E$1992","v":"Window - double pane"},null,null,"2023_July_new"]
["Range","Master sheet","D437",null,"300 Series Tilt and Turn, 300 Series Fixed, 325 Series Awning/Casement, 325 Series Fixed, and 400 Series",null,null,"2023_July_new"]
["Range","Master sheet","E437",null,{"$f":"$E$1993","v":"Fiberglass frame"},null,null,"2023_July_new"]
["Range","Master sheet","B438",null,{"$f":"$E$1578","v":"Fiber Cement siding"},null,null,"2023_July_new"]
["Range","Master sheet","D438",true,"HardiePanel®",null,null,"2023_July_new"]
["Range","Master sheet","B439",null,{"$f":"$E$1632","v":"Gypsum panels - glass mat"},null,null,"2023_July_new"]
["Range","Master sheet","D439",null,"GlasRoc Sheathing gypsum board",null,null,"2023_July_new"]
["Range","Master sheet","B440",null,{"$f":"$E$1578","v":"Fiber Cement siding"},null,null,"2023_July_new"]
["Range","Master sheet","D440",null,"Hardie VL Plank",null,null,"2023_July_new"]
["Range","Master sheet","B441",null,{"$f":"$E$1578","v":"Fiber Cement siding"},null,null,"2023_July_new"]
["Range","Master sheet","D441",null,"HardiePlank",null,null,"2023_July_new"]
["Range","Energy GHG","C1",null,"Province"]
["Range","Energy GHG","D1",null,"GHG Factor Electricity"]
["Range","Energy GHG","E1",null,"GHG Factor Natural Gas"]
["Range","Energy GHG","F1",null,"GHG Factor Oil"]
["Range","Energy GHG","G1",null,"GHG Factor Propane"]
["Range","Energy GHG","H1",null,"GHG Factor Wood "]
["Range","Energy GHG","C2",null,"Newfoundland and Labrador"]
["Range","Energy GHG","C3",null,"Prince Edward Island"]
["Range","Energy GHG","C4",null,"Nova Scotia"]
["Range","Energy GHG","C5",null,"New Brunswick"]
["Range","Energy GHG","C6",null,"Quebec"]
["Range","Energy GHG","C7",null,"Ontario"]
["Range","Energy GHG","C8",null,"Manitoba"]
["Range","Energy GHG","C9",null,"Saskatchewan"]
["Range","Energy GHG","C10",null,"Alberta"]
["Range","Energy GHG","C11",null,"British Columbia"]
["Range","Energy GHG","C12",null,"Yukon"]
["Range","Energy GHG","C13",null,"Northwest Territories"]
["Range","Energy GHG","C14",null,"Nunavut"]
["Range","Energy GHG","C15",null,"Override Province"]
["Range","Energy GHG","C16",null,"Override Value"]
["Range","Energy GHG","C17",null,"Information Source"]
["Range","Energy GHG","C19",null,"GHG Calculations Results"]
["Range","Energy GHG","A20",null,"Fuel consumption from h2k file "]
["Range","Energy GHG","C20",null,{"$f":"$E$2431","v":"Province"}]
["Range","Energy GHG","D20",null,"Electricity"]
["Range","Energy GHG","E20",null,"Natural Gas"]
["Range","Energy GHG","F20",null,"Oil"]
["Range","Energy GHG","G20",null,"Propane"]
["Range","Energy GHG","H20",null,"Wood"]
["Range","Energy GHG","I20",null,{"$f":"$E$1145","v":"Total"}]
["Range","Energy GHG","A21",null,"Electricity_kWh"]
["Range","Energy GHG","C21",null,{"$f":"$E$2437","v":"Newfoundland and Labrador"}]
["Range","Energy GHG","A22",null,"Natural Gas_m3"]
["Range","Energy GHG","C22",null,{"$f":"$E$2438","v":"Prince Edward Island"}]
["Range","Energy GHG","A23",null,"Oil_Litres"]
["Range","Energy GHG","C23",null,{"$f":"$E$2439","v":"Nova Scotia"}]
["Range","Energy GHG","A24",null,"Propane_Litres"]
["Range","Energy GHG","C24",null,{"$f":"$E$2440","v":"New Brunswick"}]
["Range","Energy GHG","A25",null,"Wood_Kg"]
["Range","Energy GHG","C25",null,{"$f":"$E$2441","v":"Quebec"}]
["Range","Energy GHG","C26",null,{"$f":"$E$2442","v":"Ontario"}]
["Range","Energy GHG","C27",null,{"$f":"$E$2443","v":"Manitoba"}]
["Range","Energy GHG","C28",null,{"$f":"$E$2444","v":"Saskatchewan"}]
["Range","Energy GHG","C29",null,{"$f":"$E$2445","v":"Alberta"}]
["Range","Energy GHG","C30",null,{"$f":"$E$2446","v":"British Columbia"}]
["Range","Energy GHG","C31",null,{"$f":"$E$2447","v":"Yukon"}]
["Range","Energy GHG","A32",null,"Renewables_GJ"]
["Range","Energy GHG","C32",null,{"$f":"$E$2448","v":"Northwest Territories"}]
["Range","Energy GHG","C33",null,{"$f":"$E$2449","v":"Nunavut"}]
["Shape","Introduction","TextBox 8",true,"NRCan would like to acknowledge the foundational contribution of Chris Magwood and the team at Builders for Climate Action.  The Material Carbon Emissions Estimator (MCE2) was co-created by the team at Builders for Climate Action (https://www.buildersforclimateaction.org/) and NRCan.  It supports their mission to: \"offer future generations our best efforts to reign in the worst effects of climate change through smart, coordinated, and effective action to address emissions in the sector while making a world that is just and equitable.\" and NRCan's mandate of supporting industry in making informed decisions related to energy and carbon performance in the built environment.  "]
["MsgBox",null,"msgBVT",null,"Warning: the building is modeled with a special number of storeys (<~NoOfStoreys~>). Please input total ceiling area mannually."]
["MsgBox",null,"msgCTR",null,"Error: no results found. please run 'calculate' in HOT2000 and try again"]
["MsgBox",null,"msgVIU",null,"Error: Please select a .h2k file"]
["MsgBox",null,"msgXRT",null,"Scenario '<~new_SCN_Name~>' already exists. Please select a new name."]
["MsgBox",null,"msgCTI",null,"You already made '<~MAX_SCENARIOS~>' scenarios. The workbook does not support additional scenarios. You may want to delete a scenario and try again."]
["MsgBox",null,"msgMTD",null,"Scenario '<~scn_Name~>' does not exist. Please try again.","Scenario name"]
["MsgBox",null,"msgUOQ",null,"Scenario '<~scn_Name~>' could not be found. Please try again."]
["MsgBox",null,"msgVCU",null,"Are you sure to delete Scenario '<~scn_Name~>'?"," "]
["MsgBox",null,"msgUIM",null,"Address of orange cells are saved in the <~scnDBSh.Name~> sheet"]
["MsgBox",null,"msgFVT",null,"Please enter a name for your scenario","Scenario Name"]
["MsgBox",null,"msgEVU",null,"Select house file (h2k)"]
["MsgBox",null,"msgVRG",null,"All data on the “SCENARIOS” tab will be lost.  Do you want to proceed? ","Warning"]
["MsgBox",null,"msgCYT",null,"Changing the province changes both the GHG intensity factor of the electrical supply and the regionally available concrete mixes.  If you proceed, your current concrete selections for <~Province_Name~> will be saved for later use.  You will be required to make new concrete selections based on regionally available mixes for the province of choice."]
["MsgBox",null,"msgNTR",null,"Changing the province changes both the GHG intensity factor of the electrical supply and the regionally available concrete mixes.  Your previously selected concrete mixes for <~Province_Name~> will be loaded."]
["Forms",null,"frmSelectScenario",null,"Select Scenario"]
["Forms",null,"lblSelectScenToDelete","delete","Select a scenario to delete"]
["Forms",null,"lblSelectScenToDelete","restore","Select a scenario to restore"]
["Forms",null,"cmdCancel",null,"Cancel"]
["Forms",null,"cmdOk",null,"Select"]
["Forms",null,"lblWaitMessage",null,"One moment please…"]
["Validation.InputMessage","User-Defined","D19",null,"Select insulation from dropdown, enter R-value (left,imperial units) and surface area (right, square metres)"]
["Validation.InputMessage","User-Defined","D20",null,{"$f":"$E$2502","v":"Select insulation from dropdown, enter R-value (left,imperial units) and surface area (right, square metres)"}]
["Validation.InputMessage","User-Defined","D21",null,{"$f":"$E$2502","v":"Select insulation from dropdown, enter R-value (left,imperial units) and surface area (right, square metres)"}]
["Validation.InputMessage","Energy GHG","D15",null,"Select a province's GHG factor to override then enter the new GHG intensity value in the correstponding cell below.\n \n Note: only one province's fuel type can be overridden at a time."]
["Validation.InputMessage","Energy GHG","E15",null,{"$f":"$E$2505","v":"Select a province's GHG factor to override then enter the new GHG intensity value in the correstponding cell below.\n \n Note: only one province's fuel type can be overridden at a time."}]
["Validation.InputMessage","Energy GHG","F15",null,{"$f":"$E$2505","v":"Select a province's GHG factor to override then enter the new GHG intensity value in the correstponding cell below.\n \n Note: only one province's fuel type can be overridden at a time."}]
["Validation.InputMessage","Energy GHG","G15",null,{"$f":"$E$2505","v":"Select a province's GHG factor to override then enter the new GHG intensity value in the correstponding cell below.\n \n Note: only one province's fuel type can be overridden at a time."}]
["Validation.InputMessage","Energy GHG","H15",null,{"$f":"$E$2505","v":"Select a province's GHG factor to override then enter the new GHG intensity value in the correstponding cell below.\n \n Note: only one province's fuel type can be overridden at a time."}]
["Validation.InputMessage","Energy GHG","D17",null,"Enter source of information used for override value. Web link preferrable, if available."]
["Validation.InputMessage","Energy GHG","E17",null,{"$f":"$E$2510","v":"Enter source of information used for override value. Web link preferrable, if available."}]
["Validation.InputMessage","Energy GHG","F17",null,{"$f":"$E$2510","v":"Enter source of information used for override value. Web link preferrable, if available."}]
["Validation.InputMessage","Energy GHG","G17",null,{"$f":"$E$2510","v":"Enter source of information used for override value. Web link preferrable, if available."}]
["Validation.InputMessage","Energy GHG","H17",null,{"$f":"$E$2510","v":"Enter source of information used for override value. Web link preferrable, if available."}]
["Shape","Footings & Slabs","Rounded Rectangle 2||Rectangle: Rounded Corners 2",null,"Clear This Sheet Only"]
["Shape","Foundation Walls","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,{"$f":"$E$2515","v":"Clear This Sheet Only"}]
["Shape","Structural Elements","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,{"$f":"$E$2515","v":"Clear This Sheet Only"}]
["Shape","Ext. Walls","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
["Shape","Ext. Wall Systems","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
["Shape","Party Walls","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
["Shape","Cladding","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
["Shape","Windows","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
["Shape","Int. Walls","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
["Shape","Floors","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
["Shape","Ceilings","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
["Shape","Roof","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
["Shape","Garage","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
["Shape","User-Defined","Rounded Rectangle 1||Rectangle: Rounded Corners 1",null,"Clear This Sheet Only"]
[]
[null,null,null,null,null,null,null,"© His Majesty the king in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,null,null,null,null,null,null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Translation-FR","index":1,"n_rows":2531,"n_cols":9,"rows_kept":2531,"cut":false,"hidden":true,"merged":[[1076,4,1076,11],[1013,4,1013,5],[1019,4,1020,4],[1021,4,1022,4],[1023,4,1024,4],[1025,4,1026,4],[1048,4,1048,7],[1012,4,1012,11],[751,4,751,16],[756,4,757,4],[758,4,759,4],[760,4,761,4],[762,4,763,4],[827,4,827,16],[832,4,833,4],[834,4,835,4],[836,4,837,4],[838,4,839,4],[1011,4,1011,7],[740,4,741,4],[633,4,634,4],[635,4,636,4],[668,4,668,16],[673,4,674,4],[675,4,676,4],[677,4,678,4],[679,4,680,4],[729,4,729,16],[734,4,735,4],[736,4,737,4],[738,4,739,4],[631,4,632,4],[573,4,574,4],[575,4,576,4],[577,4,578,4],[579,4,580,4],[605,4,605,16],[610,4,611,4],[612,4,613,4],[614,4,615,4],[616,4,617,4],[624,4,624,16],[629,4,630,4],[568,4,568,16],[431,4,432,4],[433,4,434,4],[435,4,436,4],[437,4,438,4],[451,4,457,5],[467,4,467,16],[472,4,473,4],[474,4,475,4],[476,4,477,4],[478,4,479,4],[556,4,561,5],[426,4,426,16],[284,4,290,5],[325,4,325,16],[330,4,331,4],[332,4,333,4],[334,4,335,4],[336,4,337,4],[349,4,349,16],[354,4,355,4],[356,4,357,4],[358,4,359,4],[360,4,361,4],[246,4,247,4],[149,4,149,6],[160,4,160,15],[163,4,163,16],[168,4,169,4],[170,4,171,4],[172,4,173,4],[174,4,175,4],[235,4,235,16],[240,4,241,4],[242,4,243,4],[244,4,245,4],[143,4,143,9],[27,4,28,11],[29,4,29,6],[33,4,35,11],[40,4,43,11],[57,4,58,4],[59,4,60,4],[66,4,66,11],[67,4,67,6],[117,4,117,17],[119,4,119,14],[134,4,134,9],[15,4,15,5],[0,4,0,5],[0,6,0,7],[4,4,8,12],[13,4,13,5],[14,4,14,5]]}
[]
["Type","Sheet","Address","Additional Info","Valeur"]
[{"$f":"IF(LEN('Translation-EN'!A3)>0,'Translation-EN'!A3,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B3)>0,'Translation-EN'!B3,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C3)>0,'Translation-EN'!C3,\"\")","v":"Q1"},{"$f":"IF(LEN('Translation-EN'!D3)>0,'Translation-EN'!D3,\"\")","v":""},"CONVERSION D'UNITÉS DE MESURE"]
[{"$f":"IF(LEN('Translation-EN'!A4)>0,'Translation-EN'!A4,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B4)>0,'Translation-EN'!B4,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C4)>0,'Translation-EN'!C4,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D4)>0,'Translation-EN'!D4,\"\")","v":""},"Novembre 2023"]
[{"$f":"IF(LEN('Translation-EN'!A5)>0,'Translation-EN'!A5,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B5)>0,'Translation-EN'!B5,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C5)>0,'Translation-EN'!C5,\"\")","v":"B2"},{"$f":"IF(LEN('Translation-EN'!D5)>0,'Translation-EN'!D5,\"\")","v":true},"Estimateur d'émissions de carbone des matériaux (E2CM) "]
[{"$f":"IF(LEN('Translation-EN'!A6)>0,'Translation-EN'!A6,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B6)>0,'Translation-EN'!B6,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C6)>0,'Translation-EN'!C6,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D6)>0,'Translation-EN'!D6,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A7)>0,'Translation-EN'!A7,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B7)>0,'Translation-EN'!B7,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C7)>0,'Translation-EN'!C7,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D7)>0,'Translation-EN'!D7,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A8)>0,'Translation-EN'!A8,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B8)>0,'Translation-EN'!B8,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C8)>0,'Translation-EN'!C8,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D8)>0,'Translation-EN'!D8,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A9)>0,'Translation-EN'!A9,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B9)>0,'Translation-EN'!B9,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C9)>0,'Translation-EN'!C9,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D9)>0,'Translation-EN'!D9,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A10)>0,'Translation-EN'!A10,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B10)>0,'Translation-EN'!B10,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C10)>0,'Translation-EN'!C10,\"\")","v":"K2"},{"$f":"IF(LEN('Translation-EN'!D10)>0,'Translation-EN'!D10,\"\")","v":""},"Contenu de projet carbone"]
[{"$f":"IF(LEN('Translation-EN'!A11)>0,'Translation-EN'!A11,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B11)>0,'Translation-EN'!B11,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C11)>0,'Translation-EN'!C11,\"\")","v":"Q3"},{"$f":"IF(LEN('Translation-EN'!D11)>0,'Translation-EN'!D11,\"\")","v":""},"Volume"]
[{"$f":"IF(LEN('Translation-EN'!A12)>0,'Translation-EN'!A12,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B12)>0,'Translation-EN'!B12,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C12)>0,'Translation-EN'!C12,\"\")","v":"W3"},{"$f":"IF(LEN('Translation-EN'!D12)>0,'Translation-EN'!D12,\"\")","v":""},"Superficie"]
[{"$f":"IF(LEN('Translation-EN'!A13)>0,'Translation-EN'!A13,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B13)>0,'Translation-EN'!B13,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C13)>0,'Translation-EN'!C13,\"\")","v":"AB3"},{"$f":"IF(LEN('Translation-EN'!D13)>0,'Translation-EN'!D13,\"\")","v":""},"Longueur"]
[{"$f":"IF(LEN('Translation-EN'!A14)>0,'Translation-EN'!A14,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B14)>0,'Translation-EN'!B14,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C14)>0,'Translation-EN'!C14,\"\")","v":"R5"},{"$f":"IF(LEN('Translation-EN'!D14)>0,'Translation-EN'!D14,\"\")","v":true},"pi3 à"]
[{"$f":"IF(LEN('Translation-EN'!A15)>0,'Translation-EN'!A15,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B15)>0,'Translation-EN'!B15,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C15)>0,'Translation-EN'!C15,\"\")","v":"X5"},{"$f":"IF(LEN('Translation-EN'!D15)>0,'Translation-EN'!D15,\"\")","v":true},"pi2à"]
[{"$f":"IF(LEN('Translation-EN'!A16)>0,'Translation-EN'!A16,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B16)>0,'Translation-EN'!B16,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C16)>0,'Translation-EN'!C16,\"\")","v":"AC5"},{"$f":"IF(LEN('Translation-EN'!D16)>0,'Translation-EN'!D16,\"\")","v":true},"pi à"]
[{"$f":"IF(LEN('Translation-EN'!A17)>0,'Translation-EN'!A17,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B17)>0,'Translation-EN'!B17,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C17)>0,'Translation-EN'!C17,\"\")","v":"A7"},{"$f":"IF(LEN('Translation-EN'!D17)>0,'Translation-EN'!D17,\"\")","v":""}," Étape"]
[{"$f":"IF(LEN('Translation-EN'!A18)>0,'Translation-EN'!A18,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B18)>0,'Translation-EN'!B18,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C18)>0,'Translation-EN'!C18,\"\")","v":"B7"},{"$f":"IF(LEN('Translation-EN'!D18)>0,'Translation-EN'!D18,\"\")","v":true},"      Importer les données du projet à partir de HOT2000 (si ce n’est pas le fichier HOT2000, passez à l’étape 2)"]
[{"$f":"IF(LEN('Translation-EN'!A19)>0,'Translation-EN'!A19,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B19)>0,'Translation-EN'!B19,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C19)>0,'Translation-EN'!C19,\"\")","v":"M7"},{"$f":"IF(LEN('Translation-EN'!D19)>0,'Translation-EN'!D19,\"\")","v":""},"Consommation d’énergie"]
[{"$f":"IF(LEN('Translation-EN'!A20)>0,'Translation-EN'!A20,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B20)>0,'Translation-EN'!B20,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C20)>0,'Translation-EN'!C20,\"\")","v":"O7"},{"$f":"IF(LEN('Translation-EN'!D20)>0,'Translation-EN'!D20,\"\")","v":""},"Génération d'énergie"]
[{"$f":"IF(LEN('Translation-EN'!A21)>0,'Translation-EN'!A21,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B21)>0,'Translation-EN'!B21,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C21)>0,'Translation-EN'!C21,\"\")","v":"R7"},{"$f":"IF(LEN('Translation-EN'!D21)>0,'Translation-EN'!D21,\"\")","v":""},"Notes sur la consommation d'énergie"]
[{"$f":"IF(LEN('Translation-EN'!A22)>0,'Translation-EN'!A22,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B22)>0,'Translation-EN'!B22,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C22)>0,'Translation-EN'!C22,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D22)>0,'Translation-EN'!D22,\"\")","v":""},"Appuyez ici pour importer les données HOT2000"]
[{"$f":"IF(LEN('Translation-EN'!A23)>0,'Translation-EN'!A23,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B23)>0,'Translation-EN'!B23,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C23)>0,'Translation-EN'!C23,\"\")","v":"Rounded Rectangle 16||Rectangle: Rounded Corners 16"},{"$f":"IF(LEN('Translation-EN'!D23)>0,'Translation-EN'!D23,\"\")","v":""},"Effacer tout (entrée utilisateur et tous les fiches d'assemblage)"]
[{"$f":"IF(LEN('Translation-EN'!A24)>0,'Translation-EN'!A24,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B24)>0,'Translation-EN'!B24,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C24)>0,'Translation-EN'!C24,\"\")","v":"Rounded Rectangle 15||Rectangle: Rounded Corners 15"},{"$f":"IF(LEN('Translation-EN'!D24)>0,'Translation-EN'!D24,\"\")","v":""},"Effacer cette fiche seulement (entrée utilisateur)"]
[{"$f":"IF(LEN('Translation-EN'!A25)>0,'Translation-EN'!A25,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B25)>0,'Translation-EN'!B25,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C25)>0,'Translation-EN'!C25,\"\")","v":"M8"},{"$f":"IF(LEN('Translation-EN'!D25)>0,'Translation-EN'!D25,\"\")","v":""},"Élec. kWh/an"]
[{"$f":"IF(LEN('Translation-EN'!A26)>0,'Translation-EN'!A26,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B26)>0,'Translation-EN'!B26,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C26)>0,'Translation-EN'!C26,\"\")","v":"N8"},{"$f":"IF(LEN('Translation-EN'!D26)>0,'Translation-EN'!D26,\"\")","v":true},"Gaz nat. m3/an"]
[{"$f":"IF(LEN('Translation-EN'!A27)>0,'Translation-EN'!A27,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B27)>0,'Translation-EN'!B27,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C27)>0,'Translation-EN'!C27,\"\")","v":"O8"},{"$f":"IF(LEN('Translation-EN'!D27)>0,'Translation-EN'!D27,\"\")","v":""},"Elec. kWh/an"]
[{"$f":"IF(LEN('Translation-EN'!A28)>0,'Translation-EN'!A28,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B28)>0,'Translation-EN'!B28,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C28)>0,'Translation-EN'!C28,\"\")","v":"R8"},{"$f":"IF(LEN('Translation-EN'!D28)>0,'Translation-EN'!D28,\"\")","v":true},"L'électricité produite sur place a déjà été soustraite de la consommation totale d'énergie dans la cellule M9."]
[{"$f":"IF(LEN('Translation-EN'!A29)>0,'Translation-EN'!A29,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B29)>0,'Translation-EN'!B29,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C29)>0,'Translation-EN'!C29,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D29)>0,'Translation-EN'!D29,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A30)>0,'Translation-EN'!A30,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B30)>0,'Translation-EN'!B30,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C30)>0,'Translation-EN'!C30,\"\")","v":"P10"},{"$f":"IF(LEN('Translation-EN'!D30)>0,'Translation-EN'!D30,\"\")","v":true},"Remarque : le kg/m2 est calculé à partir du total de kg divisé par la surface habitable"]
[{"$f":"IF(LEN('Translation-EN'!A31)>0,'Translation-EN'!A31,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B31)>0,'Translation-EN'!B31,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C31)>0,'Translation-EN'!C31,\"\")","v":"M11"},{"$f":"IF(LEN('Translation-EN'!D31)>0,'Translation-EN'!D31,\"\")","v":""},"Propane, l/an"]
[{"$f":"IF(LEN('Translation-EN'!A32)>0,'Translation-EN'!A32,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B32)>0,'Translation-EN'!B32,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C32)>0,'Translation-EN'!C32,\"\")","v":"N11"},{"$f":"IF(LEN('Translation-EN'!D32)>0,'Translation-EN'!D32,\"\")","v":""},"Mazout, l/an"]
[{"$f":"IF(LEN('Translation-EN'!A33)>0,'Translation-EN'!A33,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B33)>0,'Translation-EN'!B33,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C33)>0,'Translation-EN'!C33,\"\")","v":"O11"},{"$f":"IF(LEN('Translation-EN'!D33)>0,'Translation-EN'!D33,\"\")","v":""},"Bois, kg/an"]
[{"$f":"IF(LEN('Translation-EN'!A34)>0,'Translation-EN'!A34,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B34)>0,'Translation-EN'!B34,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C34)>0,'Translation-EN'!C34,\"\")","v":"R11"},{"$f":"IF(LEN('Translation-EN'!D34)>0,'Translation-EN'!D34,\"\")","v":true},"La consommation d'énergie reflète les valeurs de HOT2000, les utilisateurs doivent mettre à jour manuellement les valeurs s'ils utilisent un autre logiciel de modélisation."]
[{"$f":"IF(LEN('Translation-EN'!A35)>0,'Translation-EN'!A35,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B35)>0,'Translation-EN'!B35,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C35)>0,'Translation-EN'!C35,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D35)>0,'Translation-EN'!D35,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A36)>0,'Translation-EN'!A36,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B36)>0,'Translation-EN'!B36,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C36)>0,'Translation-EN'!C36,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D36)>0,'Translation-EN'!D36,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A37)>0,'Translation-EN'!A37,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B37)>0,'Translation-EN'!B37,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C37)>0,'Translation-EN'!C37,\"\")","v":"M13"},{"$f":"IF(LEN('Translation-EN'!D37)>0,'Translation-EN'!D37,\"\")","v":""},"Pour remplacer l’intensité des émissions de GES, utilisez l’onglet émission de GES (énergie)."]
[{"$f":"IF(LEN('Translation-EN'!A38)>0,'Translation-EN'!A38,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B38)>0,'Translation-EN'!B38,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C38)>0,'Translation-EN'!C38,\"\")","v":"A14"},{"$f":"IF(LEN('Translation-EN'!D38)>0,'Translation-EN'!D38,\"\")","v":""},{"$f":"$E$17","v":" Étape"}]
[{"$f":"IF(LEN('Translation-EN'!A39)>0,'Translation-EN'!A39,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B39)>0,'Translation-EN'!B39,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C39)>0,'Translation-EN'!C39,\"\")","v":"B14"},{"$f":"IF(LEN('Translation-EN'!D39)>0,'Translation-EN'!D39,\"\")","v":true},"      Valider ou inscrire l’information sur le projet"]
[{"$f":"IF(LEN('Translation-EN'!A40)>0,'Translation-EN'!A40,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B40)>0,'Translation-EN'!B40,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C40)>0,'Translation-EN'!C40,\"\")","v":"M14"},{"$f":"IF(LEN('Translation-EN'!D40)>0,'Translation-EN'!D40,\"\")","v":""},"Émissions opérationnelles"]
[{"$f":"IF(LEN('Translation-EN'!A41)>0,'Translation-EN'!A41,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B41)>0,'Translation-EN'!B41,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C41)>0,'Translation-EN'!C41,\"\")","v":"R14"},{"$f":"IF(LEN('Translation-EN'!D41)>0,'Translation-EN'!D41,\"\")","v":""},"Lors de l'examen de différents scénarios, les utilisateurs doivent s'assurer que les résistances thermiques des assemblages sont constant, car elles détermineront la consommation énergétique de la maison. Lorsque ceux-ci changent, les utilisateurs doivent également réviser le modèle énergétique et mettre à jour les valeurs de consommation d'énergie."]
[{"$f":"IF(LEN('Translation-EN'!A42)>0,'Translation-EN'!A42,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B42)>0,'Translation-EN'!B42,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C42)>0,'Translation-EN'!C42,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D42)>0,'Translation-EN'!D42,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A43)>0,'Translation-EN'!A43,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B43)>0,'Translation-EN'!B43,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C43)>0,'Translation-EN'!C43,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D43)>0,'Translation-EN'!D43,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A44)>0,'Translation-EN'!A44,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B44)>0,'Translation-EN'!B44,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C44)>0,'Translation-EN'!C44,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D44)>0,'Translation-EN'!D44,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A45)>0,'Translation-EN'!A45,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B45)>0,'Translation-EN'!B45,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C45)>0,'Translation-EN'!C45,\"\")","v":"B15"},{"$f":"IF(LEN('Translation-EN'!D45)>0,'Translation-EN'!D45,\"\")","v":""},"Adresse :"]
[{"$f":"IF(LEN('Translation-EN'!A46)>0,'Translation-EN'!A46,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B46)>0,'Translation-EN'!B46,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C46)>0,'Translation-EN'!C46,\"\")","v":"E15"},{"$f":"IF(LEN('Translation-EN'!D46)>0,'Translation-EN'!D46,\"\")","v":""},"Province :"]
[{"$f":"IF(LEN('Translation-EN'!A47)>0,'Translation-EN'!A47,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B47)>0,'Translation-EN'!B47,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C47)>0,'Translation-EN'!C47,\"\")","v":"M15"},{"$f":"IF(LEN('Translation-EN'!D47)>0,'Translation-EN'!D47,\"\")","v":true},"tonnes CO2e/an"]
[{"$f":"IF(LEN('Translation-EN'!A48)>0,'Translation-EN'!A48,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B48)>0,'Translation-EN'!B48,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C48)>0,'Translation-EN'!C48,\"\")","v":"N15"},{"$f":"IF(LEN('Translation-EN'!D48)>0,'Translation-EN'!D48,\"\")","v":true},"t CO2e/30 ans"]
[{"$f":"IF(LEN('Translation-EN'!A49)>0,'Translation-EN'!A49,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B49)>0,'Translation-EN'!B49,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C49)>0,'Translation-EN'!C49,\"\")","v":"B16"},{"$f":"IF(LEN('Translation-EN'!D49)>0,'Translation-EN'!D49,\"\")","v":""},"Ville :"]
[{"$f":"IF(LEN('Translation-EN'!A50)>0,'Translation-EN'!A50,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B50)>0,'Translation-EN'!B50,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C50)>0,'Translation-EN'!C50,\"\")","v":"E16"},{"$f":"IF(LEN('Translation-EN'!D50)>0,'Translation-EN'!D50,\"\")","v":""},"Code postal :"]
[{"$f":"IF(LEN('Translation-EN'!A51)>0,'Translation-EN'!A51,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B51)>0,'Translation-EN'!B51,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C51)>0,'Translation-EN'!C51,\"\")","v":"B17"},{"$f":"IF(LEN('Translation-EN'!D51)>0,'Translation-EN'!D51,\"\")","v":""},"Type de bâtiment :"]
[{"$f":"IF(LEN('Translation-EN'!A52)>0,'Translation-EN'!A52,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B52)>0,'Translation-EN'!B52,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C52)>0,'Translation-EN'!C52,\"\")","v":"E17"},{"$f":"IF(LEN('Translation-EN'!D52)>0,'Translation-EN'!D52,\"\")","v":""},"Date d’évaluation :"]
[{"$f":"IF(LEN('Translation-EN'!A53)>0,'Translation-EN'!A53,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B53)>0,'Translation-EN'!B53,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C53)>0,'Translation-EN'!C53,\"\")","v":"B18"},{"$f":"IF(LEN('Translation-EN'!D53)>0,'Translation-EN'!D53,\"\")","v":""},"Étages :"]
[{"$f":"IF(LEN('Translation-EN'!A54)>0,'Translation-EN'!A54,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B54)>0,'Translation-EN'!B54,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C54)>0,'Translation-EN'!C54,\"\")","v":"E18"},{"$f":"IF(LEN('Translation-EN'!D54)>0,'Translation-EN'!D54,\"\")","v":""},"ID du fichier :"]
[{"$f":"IF(LEN('Translation-EN'!A55)>0,'Translation-EN'!A55,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B55)>0,'Translation-EN'!B55,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C55)>0,'Translation-EN'!C55,\"\")","v":"M18"},{"$f":"IF(LEN('Translation-EN'!D55)>0,'Translation-EN'!D55,\"\")","v":""},"Émissions provenant de matériaux"]
[{"$f":"IF(LEN('Translation-EN'!A56)>0,'Translation-EN'!A56,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B56)>0,'Translation-EN'!B56,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C56)>0,'Translation-EN'!C56,\"\")","v":"B19"},{"$f":"IF(LEN('Translation-EN'!D56)>0,'Translation-EN'!D56,\"\")","v":""},"Année de construction :"]
[{"$f":"IF(LEN('Translation-EN'!A57)>0,'Translation-EN'!A57,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B57)>0,'Translation-EN'!B57,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C57)>0,'Translation-EN'!C57,\"\")","v":"E19"},{"$f":"IF(LEN('Translation-EN'!D57)>0,'Translation-EN'!D57,\"\")","v":""},"ID du fichier :"]
[{"$f":"IF(LEN('Translation-EN'!A58)>0,'Translation-EN'!A58,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B58)>0,'Translation-EN'!B58,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C58)>0,'Translation-EN'!C58,\"\")","v":"M19"},{"$f":"IF(LEN('Translation-EN'!D58)>0,'Translation-EN'!D58,\"\")","v":true},"tonnes CO2e"]
[{"$f":"IF(LEN('Translation-EN'!A59)>0,'Translation-EN'!A59,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B59)>0,'Translation-EN'!B59,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C59)>0,'Translation-EN'!C59,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D59)>0,'Translation-EN'!D59,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A60)>0,'Translation-EN'!A60,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B60)>0,'Translation-EN'!B60,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C60)>0,'Translation-EN'!C60,\"\")","v":"N19"},{"$f":"IF(LEN('Translation-EN'!D60)>0,'Translation-EN'!D60,\"\")","v":true},"kg CO2e/m2"]
[{"$f":"IF(LEN('Translation-EN'!A61)>0,'Translation-EN'!A61,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B61)>0,'Translation-EN'!B61,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C61)>0,'Translation-EN'!C61,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D61)>0,'Translation-EN'!D61,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A62)>0,'Translation-EN'!A62,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B62)>0,'Translation-EN'!B62,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C62)>0,'Translation-EN'!C62,\"\")","v":"B20"},{"$f":"IF(LEN('Translation-EN'!D62)>0,'Translation-EN'!D62,\"\")","v":true},"Aire de plancher chauffée (au-dessus du niveau du sol, m2) :"]
[{"$f":"IF(LEN('Translation-EN'!A63)>0,'Translation-EN'!A63,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B63)>0,'Translation-EN'!B63,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C63)>0,'Translation-EN'!C63,\"\")","v":"B21"},{"$f":"IF(LEN('Translation-EN'!D63)>0,'Translation-EN'!D63,\"\")","v":true},"Aire de plancher chauffée (en dessous du niveau du sol, m2) :"]
[{"$f":"IF(LEN('Translation-EN'!A64)>0,'Translation-EN'!A64,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B64)>0,'Translation-EN'!B64,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C64)>0,'Translation-EN'!C64,\"\")","v":"B22"},{"$f":"IF(LEN('Translation-EN'!D64)>0,'Translation-EN'!D64,\"\")","v":""},"Nombre de degrés-jours de chauffage :"]
[{"$f":"IF(LEN('Translation-EN'!A65)>0,'Translation-EN'!A65,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B65)>0,'Translation-EN'!B65,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C65)>0,'Translation-EN'!C65,\"\")","v":"A24"},{"$f":"IF(LEN('Translation-EN'!D65)>0,'Translation-EN'!D65,\"\")","v":""},{"$f":"$E$17","v":" Étape"}]
[{"$f":"IF(LEN('Translation-EN'!A66)>0,'Translation-EN'!A66,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B66)>0,'Translation-EN'!B66,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C66)>0,'Translation-EN'!C66,\"\")","v":"B24"},{"$f":"IF(LEN('Translation-EN'!D66)>0,'Translation-EN'!D66,\"\")","v":true},"      Valider ou inscrire les dimensions du projet"]
[{"$f":"IF(LEN('Translation-EN'!A67)>0,'Translation-EN'!A67,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B67)>0,'Translation-EN'!B67,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C67)>0,'Translation-EN'!C67,\"\")","v":"E24"},{"$f":"IF(LEN('Translation-EN'!D67)>0,'Translation-EN'!D67,\"\")","v":true},"Les valeurs HOT2000 sont importées dans les cellules BLEUES ci-dessous.\nSi aucun fichier HOT2000 n'est importé, inscrire les valeurs dans les cellules BLEUES."]
[{"$f":"IF(LEN('Translation-EN'!A68)>0,'Translation-EN'!A68,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B68)>0,'Translation-EN'!B68,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C68)>0,'Translation-EN'!C68,\"\")","v":"M24"},{"$f":"IF(LEN('Translation-EN'!D68)>0,'Translation-EN'!D68,\"\")","v":true},"Concernant toutes les cellules JAUNES ci-dessous, inscrire manuellement toutes les valeurs pertinentes. Exclure les quantités relatives au garage."]
[{"$f":"IF(LEN('Translation-EN'!A69)>0,'Translation-EN'!A69,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B69)>0,'Translation-EN'!B69,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C69)>0,'Translation-EN'!C69,\"\")","v":"P24"},{"$f":"IF(LEN('Translation-EN'!D69)>0,'Translation-EN'!D69,\"\")","v":""},"VOS DONNÉES"]
[{"$f":"IF(LEN('Translation-EN'!A70)>0,'Translation-EN'!A70,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B70)>0,'Translation-EN'!B70,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C70)>0,'Translation-EN'!C70,\"\")","v":"B25"},{"$f":"IF(LEN('Translation-EN'!D70)>0,'Translation-EN'!D70,\"\")","v":""},"  COMPOSANT"]
[{"$f":"IF(LEN('Translation-EN'!A71)>0,'Translation-EN'!A71,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B71)>0,'Translation-EN'!B71,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C71)>0,'Translation-EN'!C71,\"\")","v":"C25"},{"$f":"IF(LEN('Translation-EN'!D71)>0,'Translation-EN'!D71,\"\")","v":""},"AIRE/VOLUME"]
[{"$f":"IF(LEN('Translation-EN'!A72)>0,'Translation-EN'!A72,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B72)>0,'Translation-EN'!B72,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C72)>0,'Translation-EN'!C72,\"\")","v":"E25"},{"$f":"IF(LEN('Translation-EN'!D72)>0,'Translation-EN'!D72,\"\")","v":""},"UNITÉ"]
[{"$f":"IF(LEN('Translation-EN'!A73)>0,'Translation-EN'!A73,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B73)>0,'Translation-EN'!B73,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C73)>0,'Translation-EN'!C73,\"\")","v":"F25"},{"$f":"IF(LEN('Translation-EN'!D73)>0,'Translation-EN'!D73,\"\")","v":""},"   APPLICATION DE LA VALEUR D’ENTRÉE"]
[{"$f":"IF(LEN('Translation-EN'!A74)>0,'Translation-EN'!A74,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B74)>0,'Translation-EN'!B74,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C74)>0,'Translation-EN'!C74,\"\")","v":"M25"},{"$f":"IF(LEN('Translation-EN'!D74)>0,'Translation-EN'!D74,\"\")","v":""},"   DESCRIPTION DES UNITÉS REQUISES"]
[{"$f":"IF(LEN('Translation-EN'!A75)>0,'Translation-EN'!A75,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B75)>0,'Translation-EN'!B75,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C75)>0,'Translation-EN'!C75,\"\")","v":"B27"},{"$f":"IF(LEN('Translation-EN'!D75)>0,'Translation-EN'!D75,\"\")","v":""},"SEMELLES, SOCLES ET PILIERS"]
[{"$f":"IF(LEN('Translation-EN'!A76)>0,'Translation-EN'!A76,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B76)>0,'Translation-EN'!B76,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C76)>0,'Translation-EN'!C76,\"\")","v":"B29"},{"$f":"IF(LEN('Translation-EN'!D76)>0,'Translation-EN'!D76,\"\")","v":""},"SURFACE DE MUR DE FONDATION"]
[{"$f":"IF(LEN('Translation-EN'!A77)>0,'Translation-EN'!A77,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B77)>0,'Translation-EN'!B77,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C77)>0,'Translation-EN'!C77,\"\")","v":"B30"},{"$f":"IF(LEN('Translation-EN'!D77)>0,'Translation-EN'!D77,\"\")","v":""},"SURFACE DE LA DALLE DE FONDATION/DU PLANCHER"]
[{"$f":"IF(LEN('Translation-EN'!A78)>0,'Translation-EN'!A78,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B78)>0,'Translation-EN'!B78,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C78)>0,'Translation-EN'!C78,\"\")","v":"B31"},{"$f":"IF(LEN('Translation-EN'!D78)>0,'Translation-EN'!D78,\"\")","v":""},"SURFACE DE MUR EXTÉRIEUR"]
[{"$f":"IF(LEN('Translation-EN'!A79)>0,'Translation-EN'!A79,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B79)>0,'Translation-EN'!B79,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C79)>0,'Translation-EN'!C79,\"\")","v":"B32"},{"$f":"IF(LEN('Translation-EN'!D79)>0,'Translation-EN'!D79,\"\")","v":""},"SURFACE DE FENÊTRES"]
[{"$f":"IF(LEN('Translation-EN'!A80)>0,'Translation-EN'!A80,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B80)>0,'Translation-EN'!B80,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C80)>0,'Translation-EN'!C80,\"\")","v":"B33"},{"$f":"IF(LEN('Translation-EN'!D80)>0,'Translation-EN'!D80,\"\")","v":""},"SURFACE DE MUR INTÉRIEUR"]
[{"$f":"IF(LEN('Translation-EN'!A81)>0,'Translation-EN'!A81,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B81)>0,'Translation-EN'!B81,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C81)>0,'Translation-EN'!C81,\"\")","v":"B34"},{"$f":"IF(LEN('Translation-EN'!D81)>0,'Translation-EN'!D81,\"\")","v":""},"AIRE DE PLANCHER ENCADRÉ"]
[{"$f":"IF(LEN('Translation-EN'!A82)>0,'Translation-EN'!A82,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B82)>0,'Translation-EN'!B82,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C82)>0,'Translation-EN'!C82,\"\")","v":"B35"},{"$f":"IF(LEN('Translation-EN'!D82)>0,'Translation-EN'!D82,\"\")","v":""},"SURFACE DE PLAFOND"]
[{"$f":"IF(LEN('Translation-EN'!A83)>0,'Translation-EN'!A83,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B83)>0,'Translation-EN'!B83,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C83)>0,'Translation-EN'!C83,\"\")","v":"B36"},{"$f":"IF(LEN('Translation-EN'!D83)>0,'Translation-EN'!D83,\"\")","v":""},"SURFACE DE TOIT"]
[{"$f":"IF(LEN('Translation-EN'!A84)>0,'Translation-EN'!A84,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B84)>0,'Translation-EN'!B84,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C84)>0,'Translation-EN'!C84,\"\")","v":"B37"},{"$f":"IF(LEN('Translation-EN'!D84)>0,'Translation-EN'!D84,\"\")","v":""},"SURFACE D’ISOLATION DU TOIT"]
[{"$f":"IF(LEN('Translation-EN'!A85)>0,'Translation-EN'!A85,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B85)>0,'Translation-EN'!B85,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C85)>0,'Translation-EN'!C85,\"\")","v":"B38"},{"$f":"IF(LEN('Translation-EN'!D85)>0,'Translation-EN'!D85,\"\")","v":""},"ÉLÉMENTS EN BOIS LOURD"]
[{"$f":"IF(LEN('Translation-EN'!A86)>0,'Translation-EN'!A86,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B86)>0,'Translation-EN'!B86,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C86)>0,'Translation-EN'!C86,\"\")","v":"B39"},{"$f":"IF(LEN('Translation-EN'!D86)>0,'Translation-EN'!D86,\"\")","v":""},"SURFACE DE MUR MITOYEN"]
[{"$f":"IF(LEN('Translation-EN'!A87)>0,'Translation-EN'!A87,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B87)>0,'Translation-EN'!B87,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C87)>0,'Translation-EN'!C87,\"\")","v":"F27"},{"$f":"IF(LEN('Translation-EN'!D87)>0,'Translation-EN'!D87,\"\")","v":""},"Longueur de la semelle"]
[{"$f":"IF(LEN('Translation-EN'!A88)>0,'Translation-EN'!A88,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B88)>0,'Translation-EN'!B88,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C88)>0,'Translation-EN'!C88,\"\")","v":"H27"},{"$f":"IF(LEN('Translation-EN'!D88)>0,'Translation-EN'!D88,\"\")","v":""},"Profondeur de la semelle"]
[{"$f":"IF(LEN('Translation-EN'!A89)>0,'Translation-EN'!A89,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B89)>0,'Translation-EN'!B89,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C89)>0,'Translation-EN'!C89,\"\")","v":"J27"},{"$f":"IF(LEN('Translation-EN'!D89)>0,'Translation-EN'!D89,\"\")","v":""},"Largeur de la semelle"]
[{"$f":"IF(LEN('Translation-EN'!A90)>0,'Translation-EN'!A90,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B90)>0,'Translation-EN'!B90,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C90)>0,'Translation-EN'!C90,\"\")","v":"F29"},{"$f":"IF(LEN('Translation-EN'!D90)>0,'Translation-EN'!D90,\"\")","v":""},"Mur de fondation, isolation extérieure continue, charpente intérieure, isolation intérieure, finition des murs intérieurs"]
[{"$f":"IF(LEN('Translation-EN'!A91)>0,'Translation-EN'!A91,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B91)>0,'Translation-EN'!B91,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C91)>0,'Translation-EN'!C91,\"\")","v":"F30"},{"$f":"IF(LEN('Translation-EN'!D91)>0,'Translation-EN'!D91,\"\")","v":""},"Dalle, base d’agrégats, isolation de la sous-dalle, plancher de sous-sol"]
[{"$f":"IF(LEN('Translation-EN'!A92)>0,'Translation-EN'!A92,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B92)>0,'Translation-EN'!B92,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C92)>0,'Translation-EN'!C92,\"\")","v":"F31"},{"$f":"IF(LEN('Translation-EN'!D92)>0,'Translation-EN'!D92,\"\")","v":""},"Charpente, isolation, revêtement, bardage extérieur, revêtement intérieur des murs extérieurs uniquement"]
[{"$f":"IF(LEN('Translation-EN'!A93)>0,'Translation-EN'!A93,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B93)>0,'Translation-EN'!B93,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C93)>0,'Translation-EN'!C93,\"\")","v":"F32"},{"$f":"IF(LEN('Translation-EN'!D93)>0,'Translation-EN'!D93,\"\")","v":""},"Fenêtres"]
[{"$f":"IF(LEN('Translation-EN'!A94)>0,'Translation-EN'!A94,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B94)>0,'Translation-EN'!B94,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C94)>0,'Translation-EN'!C94,\"\")","v":"F33"},{"$f":"IF(LEN('Translation-EN'!D94)>0,'Translation-EN'!D94,\"\")","v":""},"Encadrement, isolation et revêtement intérieur des murs intérieurs"]
[{"$f":"IF(LEN('Translation-EN'!A95)>0,'Translation-EN'!A95,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B95)>0,'Translation-EN'!B95,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C95)>0,'Translation-EN'!C95,\"\")","v":"F34"},{"$f":"IF(LEN('Translation-EN'!D95)>0,'Translation-EN'!D95,\"\")","v":""},"Encadrement du plancher, sous-plancher, isolation du plancher, revêtement de sol"]
[{"$f":"IF(LEN('Translation-EN'!A96)>0,'Translation-EN'!A96,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B96)>0,'Translation-EN'!B96,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C96)>0,'Translation-EN'!C96,\"\")","v":"F35"},{"$f":"IF(LEN('Translation-EN'!D96)>0,'Translation-EN'!D96,\"\")","v":""},"Revêtement de plafond"]
[{"$f":"IF(LEN('Translation-EN'!A97)>0,'Translation-EN'!A97,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B97)>0,'Translation-EN'!B97,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C97)>0,'Translation-EN'!C97,\"\")","v":"F36"},{"$f":"IF(LEN('Translation-EN'!D97)>0,'Translation-EN'!D97,\"\")","v":""},"Charpente du toit, platelage, toiture et isolation parallèle à la terrasse du toit"]
[{"$f":"IF(LEN('Translation-EN'!A98)>0,'Translation-EN'!A98,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B98)>0,'Translation-EN'!B98,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C98)>0,'Translation-EN'!C98,\"\")","v":"F37"},{"$f":"IF(LEN('Translation-EN'!D98)>0,'Translation-EN'!D98,\"\")","v":""},"Isolation de la toiture parallèle au plafond"]
[{"$f":"IF(LEN('Translation-EN'!A99)>0,'Translation-EN'!A99,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B99)>0,'Translation-EN'!B99,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C99)>0,'Translation-EN'!C99,\"\")","v":"F38"},{"$f":"IF(LEN('Translation-EN'!D99)>0,'Translation-EN'!D99,\"\")","v":""},"Éléments de charpente en bois lourd (poteaux, poutres, etc.)"]
[{"$f":"IF(LEN('Translation-EN'!A100)>0,'Translation-EN'!A100,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B100)>0,'Translation-EN'!B100,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C100)>0,'Translation-EN'!C100,\"\")","v":"F39"},{"$f":"IF(LEN('Translation-EN'!D100)>0,'Translation-EN'!D100,\"\")","v":""},"Encadrement des murs mitoyens, isolation, revêtement, revêtement intérieur"]
[{"$f":"IF(LEN('Translation-EN'!A101)>0,'Translation-EN'!A101,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B101)>0,'Translation-EN'!B101,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C101)>0,'Translation-EN'!C101,\"\")","v":"M27"},{"$f":"IF(LEN('Translation-EN'!D101)>0,'Translation-EN'!D101,\"\")","v":""},"Total des mètres cubes de toutes les semelles, piliers et poteaux"]
[{"$f":"IF(LEN('Translation-EN'!A102)>0,'Translation-EN'!A102,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B102)>0,'Translation-EN'!B102,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C102)>0,'Translation-EN'!C102,\"\")","v":"M29"},{"$f":"IF(LEN('Translation-EN'!D102)>0,'Translation-EN'!D102,\"\")","v":""},"Surface totale du mur (sans les fenêtres et les portes)"]
[{"$f":"IF(LEN('Translation-EN'!A103)>0,'Translation-EN'!A103,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B103)>0,'Translation-EN'!B103,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C103)>0,'Translation-EN'!C103,\"\")","v":"M30"},{"$f":"IF(LEN('Translation-EN'!D103)>0,'Translation-EN'!D103,\"\")","v":""},"Mètres carrés"]
[{"$f":"IF(LEN('Translation-EN'!A104)>0,'Translation-EN'!A104,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B104)>0,'Translation-EN'!B104,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C104)>0,'Translation-EN'!C104,\"\")","v":"M31"},{"$f":"IF(LEN('Translation-EN'!D104)>0,'Translation-EN'!D104,\"\")","v":""},"Superficie totale des murs extérieurs (y compris les extrémités des pignons ; exclure les ouvertures de fenêtres et de portes). Exclure tous les murs de garage, les cloisons de garage et les murs mitoyens."]
[{"$f":"IF(LEN('Translation-EN'!A105)>0,'Translation-EN'!A105,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B105)>0,'Translation-EN'!B105,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C105)>0,'Translation-EN'!C105,\"\")","v":"M32"},{"$f":"IF(LEN('Translation-EN'!D105)>0,'Translation-EN'!D105,\"\")","v":""},"Mètres carrés (y compris la surface totale des unités de vitrage)"]
[{"$f":"IF(LEN('Translation-EN'!A106)>0,'Translation-EN'!A106,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B106)>0,'Translation-EN'!B106,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C106)>0,'Translation-EN'!C106,\"\")","v":"M33"},{"$f":"IF(LEN('Translation-EN'!D106)>0,'Translation-EN'!D106,\"\")","v":""},"Mètres carrés (un seul côté) de tous les murs intérieurs. La quantité sera doublée pour les matériaux de revêtement."]
[{"$f":"IF(LEN('Translation-EN'!A107)>0,'Translation-EN'!A107,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B107)>0,'Translation-EN'!B107,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C107)>0,'Translation-EN'!C107,\"\")","v":"M34"},{"$f":"IF(LEN('Translation-EN'!D107)>0,'Translation-EN'!D107,\"\")","v":""},"Mètres carrés (comprend tous les niveaux, exclut la dalle du sous-sol, les escaliers et autres ouvertures)"]
[{"$f":"IF(LEN('Translation-EN'!A108)>0,'Translation-EN'!A108,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B108)>0,'Translation-EN'!B108,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C108)>0,'Translation-EN'!C108,\"\")","v":"M35"},{"$f":"IF(LEN('Translation-EN'!D108)>0,'Translation-EN'!D108,\"\")","v":""},"Mètres carrés (tous les niveaux ; inclure le plafond du sous-sol, le cas échéant)"]
[{"$f":"IF(LEN('Translation-EN'!A109)>0,'Translation-EN'!A109,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B109)>0,'Translation-EN'!B109,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C109)>0,'Translation-EN'!C109,\"\")","v":"M36"},{"$f":"IF(LEN('Translation-EN'!D109)>0,'Translation-EN'!D109,\"\")","v":""},"Mètres carrés (inclure les toits en pente et les toits plats ; exclure les surplombs et les pignons)"]
[{"$f":"IF(LEN('Translation-EN'!A110)>0,'Translation-EN'!A110,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B110)>0,'Translation-EN'!B110,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C110)>0,'Translation-EN'!C110,\"\")","v":"M37"},{"$f":"IF(LEN('Translation-EN'!D110)>0,'Translation-EN'!D110,\"\")","v":""},"Mètres carrés d’isolation dans la cavité du toit. En général, cette surface est égale à celle du plancher du grenier ou du plafond du dernier étage."]
[{"$f":"IF(LEN('Translation-EN'!A111)>0,'Translation-EN'!A111,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B111)>0,'Translation-EN'!B111,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C111)>0,'Translation-EN'!C111,\"\")","v":"M38"},{"$f":"IF(LEN('Translation-EN'!D111)>0,'Translation-EN'!D111,\"\")","v":""},"Mètres cubes du volume total de bois dans les poteaux et les poutres. (saisie des éléments en acier lourd dans l’onglet Éléments de structure)"]
[{"$f":"IF(LEN('Translation-EN'!A112)>0,'Translation-EN'!A112,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B112)>0,'Translation-EN'!B112,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C112)>0,'Translation-EN'!C112,\"\")","v":"M39"},{"$f":"IF(LEN('Translation-EN'!D112)>0,'Translation-EN'!D112,\"\")","v":""},"Mètres carrés de surface de mur qui séparent un logement d’un autre. Utilisé pour les logements en rangée, les appartements, etc."]
[{"$f":"IF(LEN('Translation-EN'!A113)>0,'Translation-EN'!A113,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B113)>0,'Translation-EN'!B113,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C113)>0,'Translation-EN'!C113,\"\")","v":"Q36"},{"$f":"IF(LEN('Translation-EN'!D113)>0,'Translation-EN'!D113,\"\")","v":""},"CALCULATRICE DE VOLUME POUR  ÉLÉMENTS EN BOIS LOURD"]
[{"$f":"IF(LEN('Translation-EN'!A114)>0,'Translation-EN'!A114,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B114)>0,'Translation-EN'!B114,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C114)>0,'Translation-EN'!C114,\"\")","v":"Q37"},{"$f":"IF(LEN('Translation-EN'!D114)>0,'Translation-EN'!D114,\"\")","v":""},"Longueur de la poutre (M)"]
[{"$f":"IF(LEN('Translation-EN'!A115)>0,'Translation-EN'!A115,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B115)>0,'Translation-EN'!B115,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C115)>0,'Translation-EN'!C115,\"\")","v":"S37"},{"$f":"IF(LEN('Translation-EN'!D115)>0,'Translation-EN'!D115,\"\")","v":""},"Profondeur de la poutre (mm)"]
[{"$f":"IF(LEN('Translation-EN'!A116)>0,'Translation-EN'!A116,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B116)>0,'Translation-EN'!B116,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C116)>0,'Translation-EN'!C116,\"\")","v":"U37"},{"$f":"IF(LEN('Translation-EN'!D116)>0,'Translation-EN'!D116,\"\")","v":""},"Largeur de la poutre (mm)"]
[{"$f":"IF(LEN('Translation-EN'!A117)>0,'Translation-EN'!A117,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B117)>0,'Translation-EN'!B117,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C117)>0,'Translation-EN'!C117,\"\")","v":"W37"},{"$f":"IF(LEN('Translation-EN'!D117)>0,'Translation-EN'!D117,\"\")","v":""},"Volume de la poutre (m3)"]
[{"$f":"IF(LEN('Translation-EN'!A118)>0,'Translation-EN'!A118,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B118)>0,'Translation-EN'!B118,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C118)>0,'Translation-EN'!C118,\"\")","v":"B41"},{"$f":"IF(LEN('Translation-EN'!D118)>0,'Translation-EN'!D118,\"\")","v":true},"Si ce bâtiment a un GARAGE, cliquez sur le symbole PLUS à gauche pour faire ressortir la section pour le garage."]
[{"$f":"IF(LEN('Translation-EN'!A119)>0,'Translation-EN'!A119,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B119)>0,'Translation-EN'!B119,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C119)>0,'Translation-EN'!C119,\"\")","v":"B42"},{"$f":"IF(LEN('Translation-EN'!D119)>0,'Translation-EN'!D119,\"\")","v":""},"GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A120)>0,'Translation-EN'!A120,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B120)>0,'Translation-EN'!B120,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C120)>0,'Translation-EN'!C120,\"\")","v":"B43"},{"$f":"IF(LEN('Translation-EN'!D120)>0,'Translation-EN'!D120,\"\")","v":true},"Inscrire les dimensions du garage dans les cellules  JAUNES ci-dessous. "]
[{"$f":"IF(LEN('Translation-EN'!A121)>0,'Translation-EN'!A121,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B121)>0,'Translation-EN'!B121,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C121)>0,'Translation-EN'!C121,\"\")","v":"B44"},{"$f":"IF(LEN('Translation-EN'!D121)>0,'Translation-EN'!D121,\"\")","v":""},{"$f":"$E$70","v":"  COMPOSANT"}]
[{"$f":"IF(LEN('Translation-EN'!A122)>0,'Translation-EN'!A122,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B122)>0,'Translation-EN'!B122,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C122)>0,'Translation-EN'!C122,\"\")","v":"C44"},{"$f":"IF(LEN('Translation-EN'!D122)>0,'Translation-EN'!D122,\"\")","v":""},"QUANTITÉ"]
[{"$f":"IF(LEN('Translation-EN'!A123)>0,'Translation-EN'!A123,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B123)>0,'Translation-EN'!B123,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C123)>0,'Translation-EN'!C123,\"\")","v":"E44"},{"$f":"IF(LEN('Translation-EN'!D123)>0,'Translation-EN'!D123,\"\")","v":""},{"$f":"$E$72","v":"UNITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A124)>0,'Translation-EN'!A124,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B124)>0,'Translation-EN'!B124,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C124)>0,'Translation-EN'!C124,\"\")","v":"F44"},{"$f":"IF(LEN('Translation-EN'!D124)>0,'Translation-EN'!D124,\"\")","v":""},{"$f":"$E$73","v":"   APPLICATION DE LA VALEUR D’ENTRÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A125)>0,'Translation-EN'!A125,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B125)>0,'Translation-EN'!B125,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C125)>0,'Translation-EN'!C125,\"\")","v":"M44"},{"$f":"IF(LEN('Translation-EN'!D125)>0,'Translation-EN'!D125,\"\")","v":""},{"$f":"$E$74","v":"   DESCRIPTION DES UNITÉS REQUISES"}]
[{"$f":"IF(LEN('Translation-EN'!A126)>0,'Translation-EN'!A126,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B126)>0,'Translation-EN'!B126,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C126)>0,'Translation-EN'!C126,\"\")","v":"B46"},{"$f":"IF(LEN('Translation-EN'!D126)>0,'Translation-EN'!D126,\"\")","v":""},"ZONE MURALE DU GARAGE ATTACHÉ"]
[{"$f":"IF(LEN('Translation-EN'!A127)>0,'Translation-EN'!A127,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B127)>0,'Translation-EN'!B127,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C127)>0,'Translation-EN'!C127,\"\")","v":"B47"},{"$f":"IF(LEN('Translation-EN'!D127)>0,'Translation-EN'!D127,\"\")","v":""},"SEMELLES ET SOCLES DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A128)>0,'Translation-EN'!A128,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B128)>0,'Translation-EN'!B128,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C128)>0,'Translation-EN'!C128,\"\")","v":"B49"},{"$f":"IF(LEN('Translation-EN'!D128)>0,'Translation-EN'!D128,\"\")","v":""},"SURFACE DE MUR DE FONDATION DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A129)>0,'Translation-EN'!A129,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B129)>0,'Translation-EN'!B129,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C129)>0,'Translation-EN'!C129,\"\")","v":"B50"},{"$f":"IF(LEN('Translation-EN'!D129)>0,'Translation-EN'!D129,\"\")","v":""},"SURFACE DE LA DALLE DE GARAGE/DU PLANCHER"]
[{"$f":"IF(LEN('Translation-EN'!A130)>0,'Translation-EN'!A130,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B130)>0,'Translation-EN'!B130,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C130)>0,'Translation-EN'!C130,\"\")","v":"B51"},{"$f":"IF(LEN('Translation-EN'!D130)>0,'Translation-EN'!D130,\"\")","v":""},"SURFACE DE MUR EXTÉRIEUR DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A131)>0,'Translation-EN'!A131,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B131)>0,'Translation-EN'!B131,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C131)>0,'Translation-EN'!C131,\"\")","v":"B52"},{"$f":"IF(LEN('Translation-EN'!D131)>0,'Translation-EN'!D131,\"\")","v":""},"SURFACE DE FENÊTRES DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A132)>0,'Translation-EN'!A132,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B132)>0,'Translation-EN'!B132,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C132)>0,'Translation-EN'!C132,\"\")","v":"B53"},{"$f":"IF(LEN('Translation-EN'!D132)>0,'Translation-EN'!D132,\"\")","v":""},"SURFACE DU PLAFOND FINI DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A133)>0,'Translation-EN'!A133,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B133)>0,'Translation-EN'!B133,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C133)>0,'Translation-EN'!C133,\"\")","v":"B54"},{"$f":"IF(LEN('Translation-EN'!D133)>0,'Translation-EN'!D133,\"\")","v":""},"SURFACE DE TOITURE DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A134)>0,'Translation-EN'!A134,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B134)>0,'Translation-EN'!B134,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C134)>0,'Translation-EN'!C134,\"\")","v":"B55"},{"$f":"IF(LEN('Translation-EN'!D134)>0,'Translation-EN'!D134,\"\")","v":""},"BOIS LOURDS DE GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A135)>0,'Translation-EN'!A135,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B135)>0,'Translation-EN'!B135,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C135)>0,'Translation-EN'!C135,\"\")","v":"F46"},{"$f":"IF(LEN('Translation-EN'!D135)>0,'Translation-EN'!D135,\"\")","v":true},"Encadrement des murs extérieurs, revêtement des murs intérieurs, isolation des cloisons (survoler le curseur pour plus de détails)"]
[{"$f":"IF(LEN('Translation-EN'!A136)>0,'Translation-EN'!A136,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B136)>0,'Translation-EN'!B136,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C136)>0,'Translation-EN'!C136,\"\")","v":"F47"},{"$f":"IF(LEN('Translation-EN'!D136)>0,'Translation-EN'!D136,\"\")","v":""},{"$f":"$E$87","v":"Longueur de la semelle"}]
[{"$f":"IF(LEN('Translation-EN'!A137)>0,'Translation-EN'!A137,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B137)>0,'Translation-EN'!B137,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C137)>0,'Translation-EN'!C137,\"\")","v":"H47"},{"$f":"IF(LEN('Translation-EN'!D137)>0,'Translation-EN'!D137,\"\")","v":""},{"$f":"$E$88","v":"Profondeur de la semelle"}]
[{"$f":"IF(LEN('Translation-EN'!A138)>0,'Translation-EN'!A138,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B138)>0,'Translation-EN'!B138,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C138)>0,'Translation-EN'!C138,\"\")","v":"J47"},{"$f":"IF(LEN('Translation-EN'!D138)>0,'Translation-EN'!D138,\"\")","v":""},{"$f":"$E$89","v":"Largeur de la semelle"}]
[{"$f":"IF(LEN('Translation-EN'!A139)>0,'Translation-EN'!A139,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B139)>0,'Translation-EN'!B139,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C139)>0,'Translation-EN'!C139,\"\")","v":"F49"},{"$f":"IF(LEN('Translation-EN'!D139)>0,'Translation-EN'!D139,\"\")","v":""},"Mur de fondation du garage, charpente intérieure, finition des murs intérieurs"]
[{"$f":"IF(LEN('Translation-EN'!A140)>0,'Translation-EN'!A140,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B140)>0,'Translation-EN'!B140,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C140)>0,'Translation-EN'!C140,\"\")","v":"F50"},{"$f":"IF(LEN('Translation-EN'!D140)>0,'Translation-EN'!D140,\"\")","v":""},"Dalle, base de granulats"]
[{"$f":"IF(LEN('Translation-EN'!A141)>0,'Translation-EN'!A141,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B141)>0,'Translation-EN'!B141,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C141)>0,'Translation-EN'!C141,\"\")","v":"F51"},{"$f":"IF(LEN('Translation-EN'!D141)>0,'Translation-EN'!D141,\"\")","v":""},"Charpente, revêtement, bardage extérieur, bardage intérieur"]
[{"$f":"IF(LEN('Translation-EN'!A142)>0,'Translation-EN'!A142,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B142)>0,'Translation-EN'!B142,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C142)>0,'Translation-EN'!C142,\"\")","v":"F52"},{"$f":"IF(LEN('Translation-EN'!D142)>0,'Translation-EN'!D142,\"\")","v":""},{"$f":"$E$93","v":"Fenêtres"}]
[{"$f":"IF(LEN('Translation-EN'!A143)>0,'Translation-EN'!A143,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B143)>0,'Translation-EN'!B143,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C143)>0,'Translation-EN'!C143,\"\")","v":"F53"},{"$f":"IF(LEN('Translation-EN'!D143)>0,'Translation-EN'!D143,\"\")","v":""},{"$f":"$E$96","v":"Revêtement de plafond"}]
[{"$f":"IF(LEN('Translation-EN'!A144)>0,'Translation-EN'!A144,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B144)>0,'Translation-EN'!B144,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C144)>0,'Translation-EN'!C144,\"\")","v":"F54"},{"$f":"IF(LEN('Translation-EN'!D144)>0,'Translation-EN'!D144,\"\")","v":true},"Charpente de toit, platelage, couverture. Utilisateurs de HOT2000 : voir la note (survoler le curseur pour plus de détails)"]
[{"$f":"IF(LEN('Translation-EN'!A145)>0,'Translation-EN'!A145,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B145)>0,'Translation-EN'!B145,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C145)>0,'Translation-EN'!C145,\"\")","v":"F55"},{"$f":"IF(LEN('Translation-EN'!D145)>0,'Translation-EN'!D145,\"\")","v":""},{"$f":"$E$99","v":"Éléments de charpente en bois lourd (poteaux, poutres, etc.)"}]
[{"$f":"IF(LEN('Translation-EN'!A146)>0,'Translation-EN'!A146,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B146)>0,'Translation-EN'!B146,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C146)>0,'Translation-EN'!C146,\"\")","v":"M46"},{"$f":"IF(LEN('Translation-EN'!D146)>0,'Translation-EN'!D146,\"\")","v":""},"Surface du mur qui relie le garage au bâtiment (excluant les ouvertures et les murs extérieurs du garage).\nSi le garage est détaché, laissez cette cellule vide. "]
[{"$f":"IF(LEN('Translation-EN'!A147)>0,'Translation-EN'!A147,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B147)>0,'Translation-EN'!B147,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C147)>0,'Translation-EN'!C147,\"\")","v":"M47"},{"$f":"IF(LEN('Translation-EN'!D147)>0,'Translation-EN'!D147,\"\")","v":""},"Mètres cubes. N’inclure que le volume supplémentaire aux semelles, socles et piliers du bâtiment principal."]
[{"$f":"IF(LEN('Translation-EN'!A148)>0,'Translation-EN'!A148,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B148)>0,'Translation-EN'!B148,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C148)>0,'Translation-EN'!C148,\"\")","v":"M49"},{"$f":"IF(LEN('Translation-EN'!D148)>0,'Translation-EN'!D148,\"\")","v":""},"Mètres carrés (sans les fenêtres et les portes). N’inclure que la zone de fondation supplémentaire à la fondation du bâtiment principal."]
[{"$f":"IF(LEN('Translation-EN'!A149)>0,'Translation-EN'!A149,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B149)>0,'Translation-EN'!B149,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C149)>0,'Translation-EN'!C149,\"\")","v":"M50"},{"$f":"IF(LEN('Translation-EN'!D149)>0,'Translation-EN'!D149,\"\")","v":""},{"$f":"$E$103","v":"Mètres carrés"}]
[{"$f":"IF(LEN('Translation-EN'!A150)>0,'Translation-EN'!A150,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B150)>0,'Translation-EN'!B150,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C150)>0,'Translation-EN'!C150,\"\")","v":"M51"},{"$f":"IF(LEN('Translation-EN'!D150)>0,'Translation-EN'!D150,\"\")","v":true},"Superficie du mur extérieur du garage (y compris la superficie du pignon, à l'exclusion des ouvertures de fenêtres et de portes)  SANS les ouvertures de fenêtres et de portes."]
[{"$f":"IF(LEN('Translation-EN'!A151)>0,'Translation-EN'!A151,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B151)>0,'Translation-EN'!B151,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C151)>0,'Translation-EN'!C151,\"\")","v":"M52"},{"$f":"IF(LEN('Translation-EN'!D151)>0,'Translation-EN'!D151,\"\")","v":""},"Mètres carrés (surface totale des unités de vitrage)"]
[{"$f":"IF(LEN('Translation-EN'!A152)>0,'Translation-EN'!A152,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B152)>0,'Translation-EN'!B152,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C152)>0,'Translation-EN'!C152,\"\")","v":"M53"},{"$f":"IF(LEN('Translation-EN'!D152)>0,'Translation-EN'!D152,\"\")","v":""},"Mètres carrés (tous les niveaux)"]
[{"$f":"IF(LEN('Translation-EN'!A153)>0,'Translation-EN'!A153,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B153)>0,'Translation-EN'!B153,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C153)>0,'Translation-EN'!C153,\"\")","v":"M54"},{"$f":"IF(LEN('Translation-EN'!D153)>0,'Translation-EN'!D153,\"\")","v":""},"Mètres carrés (y compris les toits en pente et les toits plats ; sans les surplombs)"]
[{"$f":"IF(LEN('Translation-EN'!A154)>0,'Translation-EN'!A154,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B154)>0,'Translation-EN'!B154,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C154)>0,'Translation-EN'!C154,\"\")","v":"M55"},{"$f":"IF(LEN('Translation-EN'!D154)>0,'Translation-EN'!D154,\"\")","v":""},{"$f":"$E$111","v":"Mètres cubes du volume total de bois dans les poteaux et les poutres. (saisie des éléments en acier lourd dans l’onglet Éléments de structure)"}]
[{"$f":"IF(LEN('Translation-EN'!A155)>0,'Translation-EN'!A155,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B155)>0,'Translation-EN'!B155,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C155)>0,'Translation-EN'!C155,\"\")","v":"A58"},{"$f":"IF(LEN('Translation-EN'!D155)>0,'Translation-EN'!D155,\"\")","v":""},{"$f":"$E$17","v":" Étape"}]
[{"$f":"IF(LEN('Translation-EN'!A156)>0,'Translation-EN'!A156,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B156)>0,'Translation-EN'!B156,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C156)>0,'Translation-EN'!C156,\"\")","v":"B58"},{"$f":"IF(LEN('Translation-EN'!D156)>0,'Translation-EN'!D156,\"\")","v":true},"      Définissez tous les assemblages de bâtiments dans les onglets de sections de bâtiments suivants."]
[{"$f":"IF(LEN('Translation-EN'!A157)>0,'Translation-EN'!A157,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B157)>0,'Translation-EN'!B157,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C157)>0,'Translation-EN'!C157,\"\")","v":"A61"},{"$f":"IF(LEN('Translation-EN'!D157)>0,'Translation-EN'!D157,\"\")","v":""},{"$f":"$E$17","v":" Étape"}]
[{"$f":"IF(LEN('Translation-EN'!A158)>0,'Translation-EN'!A158,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B158)>0,'Translation-EN'!B158,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C158)>0,'Translation-EN'!C158,\"\")","v":"B61"},{"$f":"IF(LEN('Translation-EN'!D158)>0,'Translation-EN'!D158,\"\")","v":true},"      Passez en revue les matériaux sélectionnés dans l’onglet RÉVISION."]
[{"$f":"IF(LEN('Translation-EN'!A159)>0,'Translation-EN'!A159,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B159)>0,'Translation-EN'!B159,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C159)>0,'Translation-EN'!C159,\"\")","v":"A64"},{"$f":"IF(LEN('Translation-EN'!D159)>0,'Translation-EN'!D159,\"\")","v":""},{"$f":"$E$17","v":" Étape"}]
[{"$f":"IF(LEN('Translation-EN'!A160)>0,'Translation-EN'!A160,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B160)>0,'Translation-EN'!B160,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C160)>0,'Translation-EN'!C160,\"\")","v":"B64"},{"$f":"IF(LEN('Translation-EN'!D160)>0,'Translation-EN'!D160,\"\")","v":true},"      Consultez le rapport sur les émissions de carbone dans les onglets RÉSULTATS."]
[{"$f":"IF(LEN('Translation-EN'!A161)>0,'Translation-EN'!A161,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B161)>0,'Translation-EN'!B161,\"\")","v":"USER INPUT SHEET"},{"$f":"IF(LEN('Translation-EN'!C161)>0,'Translation-EN'!C161,\"\")","v":"B67"},{"$f":"IF(LEN('Translation-EN'!D161)>0,'Translation-EN'!D161,\"\")","v":true},"Notes utiles :\n- L'onglet  Glossaire contient une description des termes et sigles peu connus.\n- Utilisez l'onglet Défini par l'utilisateur  pour tout matériel que vous souhaitez ajouter, mais qui n'a pas pu être inclus dans les onglets de section.\n- Pour passer à un onglet, cliquez à droite sur les flèches dans le coin inférieur gauche et sélectionnez l'onglet.\n- L'espacement des Charpentes est de  24 pouces au centre par défaut, même si la valeur  Espacement des Charpentes est vide."]
[{"$f":"IF(LEN('Translation-EN'!A162)>0,'Translation-EN'!A162,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B162)>0,'Translation-EN'!B162,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C162)>0,'Translation-EN'!C162,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D162)>0,'Translation-EN'!D162,\"\")","v":""},"SECTION 1 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A163)>0,'Translation-EN'!A163,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B163)>0,'Translation-EN'!B163,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C163)>0,'Translation-EN'!C163,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D163)>0,'Translation-EN'!D163,\"\")","v":""},"FONDATION – SEMELLES ET DALLES"]
[{"$f":"IF(LEN('Translation-EN'!A164)>0,'Translation-EN'!A164,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B164)>0,'Translation-EN'!B164,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C164)>0,'Translation-EN'!C164,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D164)>0,'Translation-EN'!D164,\"\")","v":true},"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."]
[{"$f":"IF(LEN('Translation-EN'!A165)>0,'Translation-EN'!A165,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B165)>0,'Translation-EN'!B165,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C165)>0,'Translation-EN'!C165,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D165)>0,'Translation-EN'!D165,\"\")","v":""},"CATÉGORIE"]
[{"$f":"IF(LEN('Translation-EN'!A166)>0,'Translation-EN'!A166,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B166)>0,'Translation-EN'!B166,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C166)>0,'Translation-EN'!C166,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D166)>0,'Translation-EN'!D166,\"\")","v":""},"MATÉRIAU"]
[{"$f":"IF(LEN('Translation-EN'!A167)>0,'Translation-EN'!A167,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B167)>0,'Translation-EN'!B167,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C167)>0,'Translation-EN'!C167,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D167)>0,'Translation-EN'!D167,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A168)>0,'Translation-EN'!A168,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B168)>0,'Translation-EN'!B168,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C168)>0,'Translation-EN'!C168,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D168)>0,'Translation-EN'!D168,\"\")","v":""}," SÉLECTIONNER"]
[{"$f":"IF(LEN('Translation-EN'!A169)>0,'Translation-EN'!A169,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B169)>0,'Translation-EN'!B169,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C169)>0,'Translation-EN'!C169,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D169)>0,'Translation-EN'!D169,\"\")","v":true},"ÉMISSIONS NETTES kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A170)>0,'Translation-EN'!A170,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B170)>0,'Translation-EN'!B170,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C170)>0,'Translation-EN'!C170,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D170)>0,'Translation-EN'!D170,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A171)>0,'Translation-EN'!A171,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B171)>0,'Translation-EN'!B171,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C171)>0,'Translation-EN'!C171,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D171)>0,'Translation-EN'!D171,\"\")","v":true},"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"]
[{"$f":"IF(LEN('Translation-EN'!A172)>0,'Translation-EN'!A172,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B172)>0,'Translation-EN'!B172,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C172)>0,'Translation-EN'!C172,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D172)>0,'Translation-EN'!D172,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A173)>0,'Translation-EN'!A173,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B173)>0,'Translation-EN'!B173,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C173)>0,'Translation-EN'!C173,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D173)>0,'Translation-EN'!D173,\"\")","v":true},"ÉMISSIONS EN kgCO2e "]
[{"$f":"IF(LEN('Translation-EN'!A174)>0,'Translation-EN'!A174,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B174)>0,'Translation-EN'!B174,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C174)>0,'Translation-EN'!C174,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D174)>0,'Translation-EN'!D174,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A175)>0,'Translation-EN'!A175,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B175)>0,'Translation-EN'!B175,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C175)>0,'Translation-EN'!C175,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D175)>0,'Translation-EN'!D175,\"\")","v":true},"STOCKAGE EN kgCO2"]
[{"$f":"IF(LEN('Translation-EN'!A176)>0,'Translation-EN'!A176,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B176)>0,'Translation-EN'!B176,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C176)>0,'Translation-EN'!C176,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D176)>0,'Translation-EN'!D176,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A177)>0,'Translation-EN'!A177,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B177)>0,'Translation-EN'!B177,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C177)>0,'Translation-EN'!C177,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D177)>0,'Translation-EN'!D177,\"\")","v":true},"TOTAL PARTIEL POUR LA SEMELLE DE FONDATION ET LES DALLES – kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A178)>0,'Translation-EN'!A178,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B178)>0,'Translation-EN'!B178,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C178)>0,'Translation-EN'!C178,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D178)>0,'Translation-EN'!D178,\"\")","v":""},"BASE DE PIERRE CONCASSÉE"]
[{"$f":"IF(LEN('Translation-EN'!A179)>0,'Translation-EN'!A179,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B179)>0,'Translation-EN'!B179,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C179)>0,'Translation-EN'!C179,\"\")","v":"D5"},{"$f":"IF(LEN('Translation-EN'!D179)>0,'Translation-EN'!D179,\"\")","v":""},"ÉPAISSEUR :"]
[{"$f":"IF(LEN('Translation-EN'!A180)>0,'Translation-EN'!A180,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B180)>0,'Translation-EN'!B180,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C180)>0,'Translation-EN'!C180,\"\")","v":"B6"},{"$f":"IF(LEN('Translation-EN'!D180)>0,'Translation-EN'!D180,\"\")","v":""},"AGGRÉGAT"]
[{"$f":"IF(LEN('Translation-EN'!A181)>0,'Translation-EN'!A181,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B181)>0,'Translation-EN'!B181,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C181)>0,'Translation-EN'!C181,\"\")","v":"A7"},{"$f":"IF(LEN('Translation-EN'!D181)>0,'Translation-EN'!D181,\"\")","v":""},"Si vous ne connaissez pas l’empreinte carbone spécifique de votre agrégat, choisissez la valeur « MOYENNE »."]
[{"$f":"IF(LEN('Translation-EN'!A182)>0,'Translation-EN'!A182,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B182)>0,'Translation-EN'!B182,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C182)>0,'Translation-EN'!C182,\"\")","v":"A12"},{"$f":"IF(LEN('Translation-EN'!D182)>0,'Translation-EN'!D182,\"\")","v":""},"SEMELLES, PILIERS ET SOCLES"]
[{"$f":"IF(LEN('Translation-EN'!A183)>0,'Translation-EN'!A183,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B183)>0,'Translation-EN'!B183,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C183)>0,'Translation-EN'!C183,\"\")","v":"B13"},{"$f":"IF(LEN('Translation-EN'!D183)>0,'Translation-EN'!D183,\"\")","v":""},"BÉTON –25 MPa ou moins"]
[{"$f":"IF(LEN('Translation-EN'!A184)>0,'Translation-EN'!A184,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B184)>0,'Translation-EN'!B184,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C184)>0,'Translation-EN'!C184,\"\")","v":"A14"},{"$f":"IF(LEN('Translation-EN'!D184)>0,'Translation-EN'!D184,\"\")","v":""},"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."]
[{"$f":"IF(LEN('Translation-EN'!A185)>0,'Translation-EN'!A185,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B185)>0,'Translation-EN'!B185,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C185)>0,'Translation-EN'!C185,\"\")","v":"B21"},{"$f":"IF(LEN('Translation-EN'!D185)>0,'Translation-EN'!D185,\"\")","v":""},"BÉTON –26-30 MPa"]
[{"$f":"IF(LEN('Translation-EN'!A186)>0,'Translation-EN'!A186,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B186)>0,'Translation-EN'!B186,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C186)>0,'Translation-EN'!C186,\"\")","v":"A22"},{"$f":"IF(LEN('Translation-EN'!D186)>0,'Translation-EN'!D186,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A187)>0,'Translation-EN'!A187,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B187)>0,'Translation-EN'!B187,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C187)>0,'Translation-EN'!C187,\"\")","v":"B29"},{"$f":"IF(LEN('Translation-EN'!D187)>0,'Translation-EN'!D187,\"\")","v":""},"BÉTON –31-35 MPa"]
[{"$f":"IF(LEN('Translation-EN'!A188)>0,'Translation-EN'!A188,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B188)>0,'Translation-EN'!B188,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C188)>0,'Translation-EN'!C188,\"\")","v":"A30"},{"$f":"IF(LEN('Translation-EN'!D188)>0,'Translation-EN'!D188,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A189)>0,'Translation-EN'!A189,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B189)>0,'Translation-EN'!B189,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C189)>0,'Translation-EN'!C189,\"\")","v":"A37"},{"$f":"IF(LEN('Translation-EN'!D189)>0,'Translation-EN'!D189,\"\")","v":""},"BARRE D’ARMATURE"]
[{"$f":"IF(LEN('Translation-EN'!A190)>0,'Translation-EN'!A190,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B190)>0,'Translation-EN'!B190,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C190)>0,'Translation-EN'!C190,\"\")","v":"D37"},{"$f":"IF(LEN('Translation-EN'!D190)>0,'Translation-EN'!D190,\"\")","v":""},"LONGUEUR ADAPTÉE"]
[{"$f":"IF(LEN('Translation-EN'!A191)>0,'Translation-EN'!A191,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B191)>0,'Translation-EN'!B191,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C191)>0,'Translation-EN'!C191,\"\")","v":"B38"},{"$f":"IF(LEN('Translation-EN'!D191)>0,'Translation-EN'!D191,\"\")","v":""},"BARRE D’ARMATURE DE BÉTON"]
[{"$f":"IF(LEN('Translation-EN'!A192)>0,'Translation-EN'!A192,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B192)>0,'Translation-EN'!B192,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C192)>0,'Translation-EN'!C192,\"\")","v":"A39"},{"$f":"IF(LEN('Translation-EN'!D192)>0,'Translation-EN'!D192,\"\")","v":""},"Indiquez une longueur totale de barres d’armature."]
[{"$f":"IF(LEN('Translation-EN'!A193)>0,'Translation-EN'!A193,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B193)>0,'Translation-EN'!B193,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C193)>0,'Translation-EN'!C193,\"\")","v":"A47"},{"$f":"IF(LEN('Translation-EN'!D193)>0,'Translation-EN'!D193,\"\")","v":""},"GRILLAGE D’ARMATURE EN ACIER"]
[{"$f":"IF(LEN('Translation-EN'!A194)>0,'Translation-EN'!A194,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B194)>0,'Translation-EN'!B194,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C194)>0,'Translation-EN'!C194,\"\")","v":"D47"},{"$f":"IF(LEN('Translation-EN'!D194)>0,'Translation-EN'!D194,\"\")","v":""},"SURFACE PERSONNALISÉE :"]
[{"$f":"IF(LEN('Translation-EN'!A195)>0,'Translation-EN'!A195,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B195)>0,'Translation-EN'!B195,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C195)>0,'Translation-EN'!C195,\"\")","v":"B48"},{"$f":"IF(LEN('Translation-EN'!D195)>0,'Translation-EN'!D195,\"\")","v":""},"GRILLAGE SOUDÉ"]
[{"$f":"IF(LEN('Translation-EN'!A196)>0,'Translation-EN'!A196,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B196)>0,'Translation-EN'!B196,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C196)>0,'Translation-EN'!C196,\"\")","v":"A50"},{"$f":"IF(LEN('Translation-EN'!D196)>0,'Translation-EN'!D196,\"\")","v":""},"PILIERS HÉLIQUES"]
[{"$f":"IF(LEN('Translation-EN'!A197)>0,'Translation-EN'!A197,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B197)>0,'Translation-EN'!B197,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C197)>0,'Translation-EN'!C197,\"\")","v":"D50"},{"$f":"IF(LEN('Translation-EN'!D197)>0,'Translation-EN'!D197,\"\")","v":""},"LA LONGUEUR TOTALE DE TOUS LES PILIERS :"]
[{"$f":"IF(LEN('Translation-EN'!A198)>0,'Translation-EN'!A198,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B198)>0,'Translation-EN'!B198,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C198)>0,'Translation-EN'!C198,\"\")","v":"B51"},{"$f":"IF(LEN('Translation-EN'!D198)>0,'Translation-EN'!D198,\"\")","v":""},{"$f":"$E$196","v":"PILIERS HÉLIQUES"}]
[{"$f":"IF(LEN('Translation-EN'!A199)>0,'Translation-EN'!A199,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B199)>0,'Translation-EN'!B199,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C199)>0,'Translation-EN'!C199,\"\")","v":"A52"},{"$f":"IF(LEN('Translation-EN'!D199)>0,'Translation-EN'!D199,\"\")","v":""},"Indiquez la longueur totale de tous les piliers. Utiliser le % pour ajuster les différentes tailles de piliers."]
[{"$f":"IF(LEN('Translation-EN'!A200)>0,'Translation-EN'!A200,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B200)>0,'Translation-EN'!B200,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C200)>0,'Translation-EN'!C200,\"\")","v":"A53"},{"$f":"IF(LEN('Translation-EN'!D200)>0,'Translation-EN'!D200,\"\")","v":""},"PLANCHERS EN DALLES DE BÉTON"]
[{"$f":"IF(LEN('Translation-EN'!A201)>0,'Translation-EN'!A201,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B201)>0,'Translation-EN'!B201,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C201)>0,'Translation-EN'!C201,\"\")","v":"D53"},{"$f":"IF(LEN('Translation-EN'!D201)>0,'Translation-EN'!D201,\"\")","v":""},{"$f":"$E$179","v":"ÉPAISSEUR :"}]
[{"$f":"IF(LEN('Translation-EN'!A202)>0,'Translation-EN'!A202,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B202)>0,'Translation-EN'!B202,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C202)>0,'Translation-EN'!C202,\"\")","v":"B54"},{"$f":"IF(LEN('Translation-EN'!D202)>0,'Translation-EN'!D202,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A203)>0,'Translation-EN'!A203,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B203)>0,'Translation-EN'!B203,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C203)>0,'Translation-EN'!C203,\"\")","v":"A55"},{"$f":"IF(LEN('Translation-EN'!D203)>0,'Translation-EN'!D203,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A204)>0,'Translation-EN'!A204,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B204)>0,'Translation-EN'!B204,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C204)>0,'Translation-EN'!C204,\"\")","v":"B62"},{"$f":"IF(LEN('Translation-EN'!D204)>0,'Translation-EN'!D204,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A205)>0,'Translation-EN'!A205,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B205)>0,'Translation-EN'!B205,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C205)>0,'Translation-EN'!C205,\"\")","v":"A63"},{"$f":"IF(LEN('Translation-EN'!D205)>0,'Translation-EN'!D205,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A206)>0,'Translation-EN'!A206,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B206)>0,'Translation-EN'!B206,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C206)>0,'Translation-EN'!C206,\"\")","v":"B70"},{"$f":"IF(LEN('Translation-EN'!D206)>0,'Translation-EN'!D206,\"\")","v":""},{"$f":"$E$187","v":"BÉTON –31-35 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A207)>0,'Translation-EN'!A207,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B207)>0,'Translation-EN'!B207,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C207)>0,'Translation-EN'!C207,\"\")","v":"A71"},{"$f":"IF(LEN('Translation-EN'!D207)>0,'Translation-EN'!D207,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A208)>0,'Translation-EN'!A208,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B208)>0,'Translation-EN'!B208,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C208)>0,'Translation-EN'!C208,\"\")","v":"A78"},{"$f":"IF(LEN('Translation-EN'!D208)>0,'Translation-EN'!D208,\"\")","v":""},"PLANCHERS EN DALLES (AUTRE MATÉRIAU)"]
[{"$f":"IF(LEN('Translation-EN'!A209)>0,'Translation-EN'!A209,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B209)>0,'Translation-EN'!B209,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C209)>0,'Translation-EN'!C209,\"\")","v":"B79"},{"$f":"IF(LEN('Translation-EN'!D209)>0,'Translation-EN'!D209,\"\")","v":""},"PLANCHER DE TERRE"]
[{"$f":"IF(LEN('Translation-EN'!A210)>0,'Translation-EN'!A210,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B210)>0,'Translation-EN'!B210,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C210)>0,'Translation-EN'!C210,\"\")","v":"A81"},{"$f":"IF(LEN('Translation-EN'!D210)>0,'Translation-EN'!D210,\"\")","v":""},"ISOLATION DE LA SOUS-DALLE"]
[{"$f":"IF(LEN('Translation-EN'!A211)>0,'Translation-EN'!A211,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B211)>0,'Translation-EN'!B211,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C211)>0,'Translation-EN'!C211,\"\")","v":"B82"},{"$f":"IF(LEN('Translation-EN'!D211)>0,'Translation-EN'!D211,\"\")","v":""},"PANNEAU DE MOUSSE EPS"]
[{"$f":"IF(LEN('Translation-EN'!A212)>0,'Translation-EN'!A212,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B212)>0,'Translation-EN'!B212,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C212)>0,'Translation-EN'!C212,\"\")","v":"C83"},{"$f":"IF(LEN('Translation-EN'!D212)>0,'Translation-EN'!D212,\"\")","v":""},"Panneau de mousse EPS – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A213)>0,'Translation-EN'!A213,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B213)>0,'Translation-EN'!B213,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C213)>0,'Translation-EN'!C213,\"\")","v":"B86"},{"$f":"IF(LEN('Translation-EN'!D213)>0,'Translation-EN'!D213,\"\")","v":""},"PANNEAU DE MOUSSE XPS"]
[{"$f":"IF(LEN('Translation-EN'!A214)>0,'Translation-EN'!A214,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B214)>0,'Translation-EN'!B214,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C214)>0,'Translation-EN'!C214,\"\")","v":"C87"},{"$f":"IF(LEN('Translation-EN'!D214)>0,'Translation-EN'!D214,\"\")","v":""},"Panneau de mousse XPS – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A215)>0,'Translation-EN'!A215,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B215)>0,'Translation-EN'!B215,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C215)>0,'Translation-EN'!C215,\"\")","v":"B92"},{"$f":"IF(LEN('Translation-EN'!D215)>0,'Translation-EN'!D215,\"\")","v":""},"PANNEAU DE LAINE MINÉRALE"]
[{"$f":"IF(LEN('Translation-EN'!A216)>0,'Translation-EN'!A216,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B216)>0,'Translation-EN'!B216,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C216)>0,'Translation-EN'!C216,\"\")","v":"B94"},{"$f":"IF(LEN('Translation-EN'!D216)>0,'Translation-EN'!D216,\"\")","v":""}," AGRÉGAT DE MOUSSE DE VERRE"]
[{"$f":"IF(LEN('Translation-EN'!A217)>0,'Translation-EN'!A217,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B217)>0,'Translation-EN'!B217,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C217)>0,'Translation-EN'!C217,\"\")","v":"C95"},{"$f":"IF(LEN('Translation-EN'!D217)>0,'Translation-EN'!D217,\"\")","v":""},"Agrégat de mousse de verre – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A218)>0,'Translation-EN'!A218,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B218)>0,'Translation-EN'!B218,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C218)>0,'Translation-EN'!C218,\"\")","v":"B99"},{"$f":"IF(LEN('Translation-EN'!D218)>0,'Translation-EN'!D218,\"\")","v":""},"PANNEAU EN MOUSSE DE VERRE"]
[{"$f":"IF(LEN('Translation-EN'!A219)>0,'Translation-EN'!A219,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B219)>0,'Translation-EN'!B219,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C219)>0,'Translation-EN'!C219,\"\")","v":"C100"},{"$f":"IF(LEN('Translation-EN'!D219)>0,'Translation-EN'!D219,\"\")","v":""},"Panneau en mousse de verre – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A220)>0,'Translation-EN'!A220,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B220)>0,'Translation-EN'!B220,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C220)>0,'Translation-EN'!C220,\"\")","v":"B103"},{"$f":"IF(LEN('Translation-EN'!D220)>0,'Translation-EN'!D220,\"\")","v":""},"PANNEAU EN LIÈGE"]
[{"$f":"IF(LEN('Translation-EN'!A221)>0,'Translation-EN'!A221,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B221)>0,'Translation-EN'!B221,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C221)>0,'Translation-EN'!C221,\"\")","v":"A105"},{"$f":"IF(LEN('Translation-EN'!D221)>0,'Translation-EN'!D221,\"\")","v":""},"REVÊTEMENT DE SOL DU SOUS-SOL"]
[{"$f":"IF(LEN('Translation-EN'!A222)>0,'Translation-EN'!A222,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B222)>0,'Translation-EN'!B222,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C222)>0,'Translation-EN'!C222,\"\")","v":"B106"},{"$f":"IF(LEN('Translation-EN'!D222)>0,'Translation-EN'!D222,\"\")","v":""},"PLANCHER EN BOIS DUR"]
[{"$f":"IF(LEN('Translation-EN'!A223)>0,'Translation-EN'!A223,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B223)>0,'Translation-EN'!B223,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C223)>0,'Translation-EN'!C223,\"\")","v":"C107"},{"$f":"IF(LEN('Translation-EN'!D223)>0,'Translation-EN'!D223,\"\")","v":""},"Plancher en bois dur – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A224)>0,'Translation-EN'!A224,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B224)>0,'Translation-EN'!B224,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C224)>0,'Translation-EN'!C224,\"\")","v":"B111"},{"$f":"IF(LEN('Translation-EN'!D224)>0,'Translation-EN'!D224,\"\")","v":""},"REVÊTEMENT DE SOL EN LINOLÉUM"]
[{"$f":"IF(LEN('Translation-EN'!A225)>0,'Translation-EN'!A225,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B225)>0,'Translation-EN'!B225,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C225)>0,'Translation-EN'!C225,\"\")","v":"C113"},{"$f":"IF(LEN('Translation-EN'!D225)>0,'Translation-EN'!D225,\"\")","v":""},"Revêtement de sol en linoléum – MOYENNE 2,5 mm"]
[{"$f":"IF(LEN('Translation-EN'!A226)>0,'Translation-EN'!A226,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B226)>0,'Translation-EN'!B226,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C226)>0,'Translation-EN'!C226,\"\")","v":"B118"},{"$f":"IF(LEN('Translation-EN'!D226)>0,'Translation-EN'!D226,\"\")","v":""},"REVÊTEMENT DE SOL EN CARRELAGE"]
[{"$f":"IF(LEN('Translation-EN'!A227)>0,'Translation-EN'!A227,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B227)>0,'Translation-EN'!B227,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C227)>0,'Translation-EN'!C227,\"\")","v":"C119"},{"$f":"IF(LEN('Translation-EN'!D227)>0,'Translation-EN'!D227,\"\")","v":""},"Plancher en carrelage – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A228)>0,'Translation-EN'!A228,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B228)>0,'Translation-EN'!B228,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C228)>0,'Translation-EN'!C228,\"\")","v":"B125"},{"$f":"IF(LEN('Translation-EN'!D228)>0,'Translation-EN'!D228,\"\")","v":""},"REVÊTEMENT DE SOL EN VINYLE"]
[{"$f":"IF(LEN('Translation-EN'!A229)>0,'Translation-EN'!A229,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B229)>0,'Translation-EN'!B229,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C229)>0,'Translation-EN'!C229,\"\")","v":"C126"},{"$f":"IF(LEN('Translation-EN'!D229)>0,'Translation-EN'!D229,\"\")","v":""},"Revêtement de sol en vinyle – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A230)>0,'Translation-EN'!A230,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B230)>0,'Translation-EN'!B230,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C230)>0,'Translation-EN'!C230,\"\")","v":"B133"},{"$f":"IF(LEN('Translation-EN'!D230)>0,'Translation-EN'!D230,\"\")","v":""},"PLANCHER LAMELLÉ"]
[{"$f":"IF(LEN('Translation-EN'!A231)>0,'Translation-EN'!A231,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B231)>0,'Translation-EN'!B231,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C231)>0,'Translation-EN'!C231,\"\")","v":"B135"},{"$f":"IF(LEN('Translation-EN'!D231)>0,'Translation-EN'!D231,\"\")","v":""},"PLANCHER DE LIÈGE"]
[{"$f":"IF(LEN('Translation-EN'!A232)>0,'Translation-EN'!A232,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B232)>0,'Translation-EN'!B232,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C232)>0,'Translation-EN'!C232,\"\")","v":"B138"},{"$f":"IF(LEN('Translation-EN'!D232)>0,'Translation-EN'!D232,\"\")","v":""},"TAPIS"]
[{"$f":"IF(LEN('Translation-EN'!A233)>0,'Translation-EN'!A233,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B233)>0,'Translation-EN'!B233,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C233)>0,'Translation-EN'!C233,\"\")","v":"B142"},{"$f":"IF(LEN('Translation-EN'!D233)>0,'Translation-EN'!D233,\"\")","v":""},"PLANCHER – DIVERS"]
[{"$f":"IF(LEN('Translation-EN'!A234)>0,'Translation-EN'!A234,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B234)>0,'Translation-EN'!B234,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C234)>0,'Translation-EN'!C234,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D234)>0,'Translation-EN'!D234,\"\")","v":""},"SECTION 2 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A235)>0,'Translation-EN'!A235,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B235)>0,'Translation-EN'!B235,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C235)>0,'Translation-EN'!C235,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D235)>0,'Translation-EN'!D235,\"\")","v":""},"FONDATION – MURS"]
[{"$f":"IF(LEN('Translation-EN'!A236)>0,'Translation-EN'!A236,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B236)>0,'Translation-EN'!B236,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C236)>0,'Translation-EN'!C236,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D236)>0,'Translation-EN'!D236,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A237)>0,'Translation-EN'!A237,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B237)>0,'Translation-EN'!B237,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C237)>0,'Translation-EN'!C237,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D237)>0,'Translation-EN'!D237,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A238)>0,'Translation-EN'!A238,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B238)>0,'Translation-EN'!B238,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C238)>0,'Translation-EN'!C238,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D238)>0,'Translation-EN'!D238,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A239)>0,'Translation-EN'!A239,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B239)>0,'Translation-EN'!B239,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C239)>0,'Translation-EN'!C239,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D239)>0,'Translation-EN'!D239,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A240)>0,'Translation-EN'!A240,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B240)>0,'Translation-EN'!B240,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C240)>0,'Translation-EN'!C240,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D240)>0,'Translation-EN'!D240,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A241)>0,'Translation-EN'!A241,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B241)>0,'Translation-EN'!B241,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C241)>0,'Translation-EN'!C241,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D241)>0,'Translation-EN'!D241,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A242)>0,'Translation-EN'!A242,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B242)>0,'Translation-EN'!B242,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C242)>0,'Translation-EN'!C242,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D242)>0,'Translation-EN'!D242,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A243)>0,'Translation-EN'!A243,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B243)>0,'Translation-EN'!B243,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C243)>0,'Translation-EN'!C243,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D243)>0,'Translation-EN'!D243,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A244)>0,'Translation-EN'!A244,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B244)>0,'Translation-EN'!B244,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C244)>0,'Translation-EN'!C244,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D244)>0,'Translation-EN'!D244,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A245)>0,'Translation-EN'!A245,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B245)>0,'Translation-EN'!B245,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C245)>0,'Translation-EN'!C245,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D245)>0,'Translation-EN'!D245,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A246)>0,'Translation-EN'!A246,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B246)>0,'Translation-EN'!B246,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C246)>0,'Translation-EN'!C246,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D246)>0,'Translation-EN'!D246,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A247)>0,'Translation-EN'!A247,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B247)>0,'Translation-EN'!B247,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C247)>0,'Translation-EN'!C247,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D247)>0,'Translation-EN'!D247,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A248)>0,'Translation-EN'!A248,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B248)>0,'Translation-EN'!B248,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C248)>0,'Translation-EN'!C248,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D248)>0,'Translation-EN'!D248,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A249)>0,'Translation-EN'!A249,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B249)>0,'Translation-EN'!B249,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C249)>0,'Translation-EN'!C249,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D249)>0,'Translation-EN'!D249,\"\")","v":true},"TOTAL PARTIEL POUR LES MURS DE FONDATION en kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A250)>0,'Translation-EN'!A250,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B250)>0,'Translation-EN'!B250,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C250)>0,'Translation-EN'!C250,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D250)>0,'Translation-EN'!D250,\"\")","v":""},"MURS EN BÉTON"]
[{"$f":"IF(LEN('Translation-EN'!A251)>0,'Translation-EN'!A251,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B251)>0,'Translation-EN'!B251,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C251)>0,'Translation-EN'!C251,\"\")","v":"D5"},{"$f":"IF(LEN('Translation-EN'!D251)>0,'Translation-EN'!D251,\"\")","v":""},{"$f":"$E$179","v":"ÉPAISSEUR :"}]
[{"$f":"IF(LEN('Translation-EN'!A252)>0,'Translation-EN'!A252,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B252)>0,'Translation-EN'!B252,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C252)>0,'Translation-EN'!C252,\"\")","v":"B6"},{"$f":"IF(LEN('Translation-EN'!D252)>0,'Translation-EN'!D252,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A253)>0,'Translation-EN'!A253,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B253)>0,'Translation-EN'!B253,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C253)>0,'Translation-EN'!C253,\"\")","v":"A7"},{"$f":"IF(LEN('Translation-EN'!D253)>0,'Translation-EN'!D253,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A254)>0,'Translation-EN'!A254,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B254)>0,'Translation-EN'!B254,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C254)>0,'Translation-EN'!C254,\"\")","v":"B14"},{"$f":"IF(LEN('Translation-EN'!D254)>0,'Translation-EN'!D254,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A255)>0,'Translation-EN'!A255,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B255)>0,'Translation-EN'!B255,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C255)>0,'Translation-EN'!C255,\"\")","v":"A15"},{"$f":"IF(LEN('Translation-EN'!D255)>0,'Translation-EN'!D255,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A256)>0,'Translation-EN'!A256,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B256)>0,'Translation-EN'!B256,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C256)>0,'Translation-EN'!C256,\"\")","v":"B22"},{"$f":"IF(LEN('Translation-EN'!D256)>0,'Translation-EN'!D256,\"\")","v":""},{"$f":"$E$187","v":"BÉTON –31-35 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A257)>0,'Translation-EN'!A257,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B257)>0,'Translation-EN'!B257,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C257)>0,'Translation-EN'!C257,\"\")","v":"A23"},{"$f":"IF(LEN('Translation-EN'!D257)>0,'Translation-EN'!D257,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A258)>0,'Translation-EN'!A258,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B258)>0,'Translation-EN'!B258,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C258)>0,'Translation-EN'!C258,\"\")","v":"A30"},{"$f":"IF(LEN('Translation-EN'!D258)>0,'Translation-EN'!D258,\"\")","v":""},"MURS EN ÉLÉMENTS DE MAÇONNERIE"]
[{"$f":"IF(LEN('Translation-EN'!A259)>0,'Translation-EN'!A259,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B259)>0,'Translation-EN'!B259,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C259)>0,'Translation-EN'!C259,\"\")","v":"B31"},{"$f":"IF(LEN('Translation-EN'!D259)>0,'Translation-EN'!D259,\"\")","v":""},"ÉLÉMENTS DE MAÇONNERIE EN BÉTON"]
[{"$f":"IF(LEN('Translation-EN'!A260)>0,'Translation-EN'!A260,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B260)>0,'Translation-EN'!B260,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C260)>0,'Translation-EN'!C260,\"\")","v":"A32"},{"$f":"IF(LEN('Translation-EN'!D260)>0,'Translation-EN'!D260,\"\")","v":""},"Si un coulis de béton ou un remplissage sont utilisés pour le mur en EMB, assurez-vous d’ajouter le volume de béton séparément."]
[{"$f":"IF(LEN('Translation-EN'!A261)>0,'Translation-EN'!A261,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B261)>0,'Translation-EN'!B261,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C261)>0,'Translation-EN'!C261,\"\")","v":"C32"},{"$f":"IF(LEN('Translation-EN'!D261)>0,'Translation-EN'!D261,\"\")","v":""},"Murs en EMB creux de 8 po, sans coulis – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A262)>0,'Translation-EN'!A262,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B262)>0,'Translation-EN'!B262,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C262)>0,'Translation-EN'!C262,\"\")","v":"A39"},{"$f":"IF(LEN('Translation-EN'!D262)>0,'Translation-EN'!D262,\"\")","v":""},"FONDATION EN BOIS TRAITÉ",null,null,null," "]
[{"$f":"IF(LEN('Translation-EN'!A263)>0,'Translation-EN'!A263,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B263)>0,'Translation-EN'!B263,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C263)>0,'Translation-EN'!C263,\"\")","v":"A41"},{"$f":"IF(LEN('Translation-EN'!D263)>0,'Translation-EN'!D263,\"\")","v":""},"ISOLATION CONTINUE (extérieure ou intérieure)"]
[{"$f":"IF(LEN('Translation-EN'!A264)>0,'Translation-EN'!A264,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B264)>0,'Translation-EN'!B264,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C264)>0,'Translation-EN'!C264,\"\")","v":"B42"},{"$f":"IF(LEN('Translation-EN'!D264)>0,'Translation-EN'!D264,\"\")","v":""},"MOUSSE EPS"]
[{"$f":"IF(LEN('Translation-EN'!A265)>0,'Translation-EN'!A265,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B265)>0,'Translation-EN'!B265,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C265)>0,'Translation-EN'!C265,\"\")","v":"C43"},{"$f":"IF(LEN('Translation-EN'!D265)>0,'Translation-EN'!D265,\"\")","v":""},{"$f":"$E$212","v":"Panneau de mousse EPS – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A266)>0,'Translation-EN'!A266,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B266)>0,'Translation-EN'!B266,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C266)>0,'Translation-EN'!C266,\"\")","v":"B46"},{"$f":"IF(LEN('Translation-EN'!D266)>0,'Translation-EN'!D266,\"\")","v":""},"MOUSSE XPS"]
[{"$f":"IF(LEN('Translation-EN'!A267)>0,'Translation-EN'!A267,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B267)>0,'Translation-EN'!B267,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C267)>0,'Translation-EN'!C267,\"\")","v":"C47"},{"$f":"IF(LEN('Translation-EN'!D267)>0,'Translation-EN'!D267,\"\")","v":""},{"$f":"$E$214","v":"Panneau de mousse XPS – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A268)>0,'Translation-EN'!A268,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B268)>0,'Translation-EN'!B268,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C268)>0,'Translation-EN'!C268,\"\")","v":"B52"},{"$f":"IF(LEN('Translation-EN'!D268)>0,'Translation-EN'!D268,\"\")","v":""},{"$f":"$E$215","v":"PANNEAU DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A269)>0,'Translation-EN'!A269,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B269)>0,'Translation-EN'!B269,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C269)>0,'Translation-EN'!C269,\"\")","v":"C53"},{"$f":"IF(LEN('Translation-EN'!D269)>0,'Translation-EN'!D269,\"\")","v":""},"Panneau de laine minérale – densité légère – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A270)>0,'Translation-EN'!A270,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B270)>0,'Translation-EN'!B270,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C270)>0,'Translation-EN'!C270,\"\")","v":"B57"},{"$f":"IF(LEN('Translation-EN'!D270)>0,'Translation-EN'!D270,\"\")","v":""},"PANNEAU DE FIBRES DE BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A271)>0,'Translation-EN'!A271,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B271)>0,'Translation-EN'!B271,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C271)>0,'Translation-EN'!C271,\"\")","v":"C58"},{"$f":"IF(LEN('Translation-EN'!D271)>0,'Translation-EN'!D271,\"\")","v":""},"Panneau de fibres de bois – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A272)>0,'Translation-EN'!A272,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B272)>0,'Translation-EN'!B272,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C272)>0,'Translation-EN'!C272,\"\")","v":"B64"},{"$f":"IF(LEN('Translation-EN'!D272)>0,'Translation-EN'!D272,\"\")","v":""},{"$f":"$E$220","v":"PANNEAU EN LIÈGE"}]
[{"$f":"IF(LEN('Translation-EN'!A273)>0,'Translation-EN'!A273,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B273)>0,'Translation-EN'!B273,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C273)>0,'Translation-EN'!C273,\"\")","v":"B66"},{"$f":"IF(LEN('Translation-EN'!D273)>0,'Translation-EN'!D273,\"\")","v":""},"MOUSSE À PULVÉRISER – CELLULE FERMÉE"]
[{"$f":"IF(LEN('Translation-EN'!A274)>0,'Translation-EN'!A274,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B274)>0,'Translation-EN'!B274,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C274)>0,'Translation-EN'!C274,\"\")","v":"A70"},{"$f":"IF(LEN('Translation-EN'!D274)>0,'Translation-EN'!D274,\"\")","v":""},"COFFRAGES ISOLÉS EN BÉTON (CIB) – MOUSSE EPS"]
[{"$f":"IF(LEN('Translation-EN'!A275)>0,'Translation-EN'!A275,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B275)>0,'Translation-EN'!B275,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C275)>0,'Translation-EN'!C275,\"\")","v":"A71"},{"$f":"IF(LEN('Translation-EN'!D275)>0,'Translation-EN'!D275,\"\")","v":""},"Étape 1 : Sélectionnez la taille du CIB"]
[{"$f":"IF(LEN('Translation-EN'!A276)>0,'Translation-EN'!A276,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B276)>0,'Translation-EN'!B276,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C276)>0,'Translation-EN'!C276,\"\")","v":"B72"},{"$f":"IF(LEN('Translation-EN'!D276)>0,'Translation-EN'!D276,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A277)>0,'Translation-EN'!A277,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B277)>0,'Translation-EN'!B277,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C277)>0,'Translation-EN'!C277,\"\")","v":"A73"},{"$f":"IF(LEN('Translation-EN'!D277)>0,'Translation-EN'!D277,\"\")","v":""},"Étape 2 : Sélectionnez l’option de remplissage en béton."]
[{"$f":"IF(LEN('Translation-EN'!A278)>0,'Translation-EN'!A278,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B278)>0,'Translation-EN'!B278,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C278)>0,'Translation-EN'!C278,\"\")","v":"B80"},{"$f":"IF(LEN('Translation-EN'!D278)>0,'Translation-EN'!D278,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A279)>0,'Translation-EN'!A279,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B279)>0,'Translation-EN'!B279,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C279)>0,'Translation-EN'!C279,\"\")","v":"A81"},{"$f":"IF(LEN('Translation-EN'!D279)>0,'Translation-EN'!D279,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A280)>0,'Translation-EN'!A280,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B280)>0,'Translation-EN'!B280,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C280)>0,'Translation-EN'!C280,\"\")","v":"B88"},{"$f":"IF(LEN('Translation-EN'!D280)>0,'Translation-EN'!D280,\"\")","v":""},{"$f":"$E$187","v":"BÉTON –31-35 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A281)>0,'Translation-EN'!A281,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B281)>0,'Translation-EN'!B281,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C281)>0,'Translation-EN'!C281,\"\")","v":"A89"},{"$f":"IF(LEN('Translation-EN'!D281)>0,'Translation-EN'!D281,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A282)>0,'Translation-EN'!A282,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B282)>0,'Translation-EN'!B282,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C282)>0,'Translation-EN'!C282,\"\")","v":"A96"},{"$f":"IF(LEN('Translation-EN'!D282)>0,'Translation-EN'!D282,\"\")","v":""},"COFFRAGES ISOLÉS EN BÉTON (CIB) – COPEAUX DE BOIS/CIMENT"]
[{"$f":"IF(LEN('Translation-EN'!A283)>0,'Translation-EN'!A283,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B283)>0,'Translation-EN'!B283,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C283)>0,'Translation-EN'!C283,\"\")","v":"A97"},{"$f":"IF(LEN('Translation-EN'!D283)>0,'Translation-EN'!D283,\"\")","v":""},{"$f":"$E$275","v":"Étape 1 : Sélectionnez la taille du CIB"}]
[{"$f":"IF(LEN('Translation-EN'!A284)>0,'Translation-EN'!A284,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B284)>0,'Translation-EN'!B284,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C284)>0,'Translation-EN'!C284,\"\")","v":"B101"},{"$f":"IF(LEN('Translation-EN'!D284)>0,'Translation-EN'!D284,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A285)>0,'Translation-EN'!A285,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B285)>0,'Translation-EN'!B285,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C285)>0,'Translation-EN'!C285,\"\")","v":"A102"},{"$f":"IF(LEN('Translation-EN'!D285)>0,'Translation-EN'!D285,\"\")","v":true},"Étape 2 : Sélectionnez l'option de remplissage en béton pour le système de mur en CIB. La quantité de béton de remplissage s'adapte à la taille du coffrage choisi."]
[{"$f":"IF(LEN('Translation-EN'!A286)>0,'Translation-EN'!A286,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B286)>0,'Translation-EN'!B286,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C286)>0,'Translation-EN'!C286,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D286)>0,'Translation-EN'!D286,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A287)>0,'Translation-EN'!A287,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B287)>0,'Translation-EN'!B287,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C287)>0,'Translation-EN'!C287,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D287)>0,'Translation-EN'!D287,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A288)>0,'Translation-EN'!A288,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B288)>0,'Translation-EN'!B288,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C288)>0,'Translation-EN'!C288,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D288)>0,'Translation-EN'!D288,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A289)>0,'Translation-EN'!A289,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B289)>0,'Translation-EN'!B289,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C289)>0,'Translation-EN'!C289,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D289)>0,'Translation-EN'!D289,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A290)>0,'Translation-EN'!A290,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B290)>0,'Translation-EN'!B290,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C290)>0,'Translation-EN'!C290,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D290)>0,'Translation-EN'!D290,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A291)>0,'Translation-EN'!A291,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B291)>0,'Translation-EN'!B291,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C291)>0,'Translation-EN'!C291,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D291)>0,'Translation-EN'!D291,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A292)>0,'Translation-EN'!A292,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B292)>0,'Translation-EN'!B292,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C292)>0,'Translation-EN'!C292,\"\")","v":"B109"},{"$f":"IF(LEN('Translation-EN'!D292)>0,'Translation-EN'!D292,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A293)>0,'Translation-EN'!A293,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B293)>0,'Translation-EN'!B293,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C293)>0,'Translation-EN'!C293,\"\")","v":"A110"},{"$f":"IF(LEN('Translation-EN'!D293)>0,'Translation-EN'!D293,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A294)>0,'Translation-EN'!A294,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B294)>0,'Translation-EN'!B294,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C294)>0,'Translation-EN'!C294,\"\")","v":"B117"},{"$f":"IF(LEN('Translation-EN'!D294)>0,'Translation-EN'!D294,\"\")","v":""},{"$f":"$E$187","v":"BÉTON –31-35 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A295)>0,'Translation-EN'!A295,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B295)>0,'Translation-EN'!B295,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C295)>0,'Translation-EN'!C295,\"\")","v":"A118"},{"$f":"IF(LEN('Translation-EN'!D295)>0,'Translation-EN'!D295,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A296)>0,'Translation-EN'!A296,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B296)>0,'Translation-EN'!B296,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C296)>0,'Translation-EN'!C296,\"\")","v":"A125"},{"$f":"IF(LEN('Translation-EN'!D296)>0,'Translation-EN'!D296,\"\")","v":""},"CHARPENTE INTÉRIEURE – BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A297)>0,'Translation-EN'!A297,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B297)>0,'Translation-EN'!B297,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C297)>0,'Translation-EN'!C297,\"\")","v":"D125"},{"$f":"IF(LEN('Translation-EN'!D297)>0,'Translation-EN'!D297,\"\")","v":""},"L’ESPACEMENT DES CHARPENTES :"]
[{"$f":"IF(LEN('Translation-EN'!A298)>0,'Translation-EN'!A298,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B298)>0,'Translation-EN'!B298,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C298)>0,'Translation-EN'!C298,\"\")","v":"B126"},{"$f":"IF(LEN('Translation-EN'!D298)>0,'Translation-EN'!D298,\"\")","v":""},"CONSTRUCTION EN BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A299)>0,'Translation-EN'!A299,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B299)>0,'Translation-EN'!B299,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C299)>0,'Translation-EN'!C299,\"\")","v":"B130"},{"$f":"IF(LEN('Translation-EN'!D299)>0,'Translation-EN'!D299,\"\")","v":""},"2x4 double"]
[{"$f":"IF(LEN('Translation-EN'!A300)>0,'Translation-EN'!A300,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B300)>0,'Translation-EN'!B300,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C300)>0,'Translation-EN'!C300,\"\")","v":"A131"},{"$f":"IF(LEN('Translation-EN'!D300)>0,'Translation-EN'!D300,\"\")","v":""},"CHARPENTE INTÉRIEURE – ACIER"]
[{"$f":"IF(LEN('Translation-EN'!A301)>0,'Translation-EN'!A301,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B301)>0,'Translation-EN'!B301,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C301)>0,'Translation-EN'!C301,\"\")","v":"D131"},{"$f":"IF(LEN('Translation-EN'!D301)>0,'Translation-EN'!D301,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A302)>0,'Translation-EN'!A302,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B302)>0,'Translation-EN'!B302,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C302)>0,'Translation-EN'!C302,\"\")","v":"B132"},{"$f":"IF(LEN('Translation-EN'!D302)>0,'Translation-EN'!D302,\"\")","v":""},"CHARPENTE D’ACIER, 2x4"]
[{"$f":"IF(LEN('Translation-EN'!A303)>0,'Translation-EN'!A303,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B303)>0,'Translation-EN'!B303,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C303)>0,'Translation-EN'!C303,\"\")","v":"A133"},{"$f":"IF(LEN('Translation-EN'!D303)>0,'Translation-EN'!D303,\"\")","v":""},"Utilisez le % pour ajuster si des montants en acier de plus gros calibre sont utilisés. Facteur d’encadrement basé sur un mur de 10 pi."]
[{"$f":"IF(LEN('Translation-EN'!A304)>0,'Translation-EN'!A304,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B304)>0,'Translation-EN'!B304,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C304)>0,'Translation-EN'!C304,\"\")","v":"C133"},{"$f":"IF(LEN('Translation-EN'!D304)>0,'Translation-EN'!D304,\"\")","v":""},"Charpente en acier – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A305)>0,'Translation-EN'!A305,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B305)>0,'Translation-EN'!B305,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C305)>0,'Translation-EN'!C305,\"\")","v":"A138"},{"$f":"IF(LEN('Translation-EN'!D305)>0,'Translation-EN'!D305,\"\")","v":""},"ISOLATION DE LA CAVITÉ"]
[{"$f":"IF(LEN('Translation-EN'!A306)>0,'Translation-EN'!A306,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B306)>0,'Translation-EN'!B306,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C306)>0,'Translation-EN'!C306,\"\")","v":"B139"},{"$f":"IF(LEN('Translation-EN'!D306)>0,'Translation-EN'!D306,\"\")","v":""},{"$f":"$E$273","v":"MOUSSE À PULVÉRISER – CELLULE FERMÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A307)>0,'Translation-EN'!A307,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B307)>0,'Translation-EN'!B307,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C307)>0,'Translation-EN'!C307,\"\")","v":"B143"},{"$f":"IF(LEN('Translation-EN'!D307)>0,'Translation-EN'!D307,\"\")","v":""},"NATTE DE FIBRE DE VERRE"]
[{"$f":"IF(LEN('Translation-EN'!A308)>0,'Translation-EN'!A308,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B308)>0,'Translation-EN'!B308,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C308)>0,'Translation-EN'!C308,\"\")","v":"C144"},{"$f":"IF(LEN('Translation-EN'!D308)>0,'Translation-EN'!D308,\"\")","v":""},"Natte de fibre de verre – Isolation des murs de fondation – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A309)>0,'Translation-EN'!A309,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B309)>0,'Translation-EN'!B309,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C309)>0,'Translation-EN'!C309,\"\")","v":"B148"},{"$f":"IF(LEN('Translation-EN'!D309)>0,'Translation-EN'!D309,\"\")","v":""},"ISOLATION EN CELLULOSE"]
[{"$f":"IF(LEN('Translation-EN'!A310)>0,'Translation-EN'!A310,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B310)>0,'Translation-EN'!B310,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C310)>0,'Translation-EN'!C310,\"\")","v":"C149"},{"$f":"IF(LEN('Translation-EN'!D310)>0,'Translation-EN'!D310,\"\")","v":""},"Cellulose – Isolation des murs de fondation – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A311)>0,'Translation-EN'!A311,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B311)>0,'Translation-EN'!B311,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C311)>0,'Translation-EN'!C311,\"\")","v":"B153"},{"$f":"IF(LEN('Translation-EN'!D311)>0,'Translation-EN'!D311,\"\")","v":""},"NATTE DE LAINE MINÉRALE"]
[{"$f":"IF(LEN('Translation-EN'!A312)>0,'Translation-EN'!A312,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B312)>0,'Translation-EN'!B312,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C312)>0,'Translation-EN'!C312,\"\")","v":"C154"},{"$f":"IF(LEN('Translation-EN'!D312)>0,'Translation-EN'!D312,\"\")","v":""},"Natte de laine minérale – Isolation des murs de fondation – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A313)>0,'Translation-EN'!A313,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B313)>0,'Translation-EN'!B313,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C313)>0,'Translation-EN'!C313,\"\")","v":"B162"},{"$f":"IF(LEN('Translation-EN'!D313)>0,'Translation-EN'!D313,\"\")","v":""},"NATTE DE FIBRES DE BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A314)>0,'Translation-EN'!A314,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B314)>0,'Translation-EN'!B314,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C314)>0,'Translation-EN'!C314,\"\")","v":"C163"},{"$f":"IF(LEN('Translation-EN'!D314)>0,'Translation-EN'!D314,\"\")","v":""},"Natte de fibres de bois – Isolation des murs de fondation – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A315)>0,'Translation-EN'!A315,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B315)>0,'Translation-EN'!B315,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C315)>0,'Translation-EN'!C315,\"\")","v":"B167"},{"$f":"IF(LEN('Translation-EN'!D315)>0,'Translation-EN'!D315,\"\")","v":""},"AUTRES ISOLANTS EN FIBRES NATURELLES"]
[{"$f":"IF(LEN('Translation-EN'!A316)>0,'Translation-EN'!A316,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B316)>0,'Translation-EN'!B316,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C316)>0,'Translation-EN'!C316,\"\")","v":"B171"},{"$f":"IF(LEN('Translation-EN'!D316)>0,'Translation-EN'!D316,\"\")","v":""},"ISOLATION EN BRIQUE DE CHANVRE"]
[{"$f":"IF(LEN('Translation-EN'!A317)>0,'Translation-EN'!A317,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B317)>0,'Translation-EN'!B317,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C317)>0,'Translation-EN'!C317,\"\")","v":"C172"},{"$f":"IF(LEN('Translation-EN'!D317)>0,'Translation-EN'!D317,\"\")","v":""},"Brique de chanvre – Isolation des murs de fondation – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A318)>0,'Translation-EN'!A318,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B318)>0,'Translation-EN'!B318,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C318)>0,'Translation-EN'!C318,\"\")","v":"B176"},{"$f":"IF(LEN('Translation-EN'!D318)>0,'Translation-EN'!D318,\"\")","v":""},"ISOLATION À VALEUR R ÉLEVÉE"]
[{"$f":"IF(LEN('Translation-EN'!A319)>0,'Translation-EN'!A319,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B319)>0,'Translation-EN'!B319,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C319)>0,'Translation-EN'!C319,\"\")","v":"A179"},{"$f":"IF(LEN('Translation-EN'!D319)>0,'Translation-EN'!D319,\"\")","v":""},"BARDAGE DES MURS INTÉRIEURS"]
[{"$f":"IF(LEN('Translation-EN'!A320)>0,'Translation-EN'!A320,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B320)>0,'Translation-EN'!B320,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C320)>0,'Translation-EN'!C320,\"\")","v":"B180"},{"$f":"IF(LEN('Translation-EN'!D320)>0,'Translation-EN'!D320,\"\")","v":""},"CLOISONS SÈCHES 1/2 po"]
[{"$f":"IF(LEN('Translation-EN'!A321)>0,'Translation-EN'!A321,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B321)>0,'Translation-EN'!B321,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C321)>0,'Translation-EN'!C321,\"\")","v":"C181"},{"$f":"IF(LEN('Translation-EN'!D321)>0,'Translation-EN'!D321,\"\")","v":""},"CLOISONS SÈCHES 1/2 po – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A322)>0,'Translation-EN'!A322,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B322)>0,'Translation-EN'!B322,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C322)>0,'Translation-EN'!C322,\"\")","v":"B187"},{"$f":"IF(LEN('Translation-EN'!D322)>0,'Translation-EN'!D322,\"\")","v":""},"CLOISONS SÈCHES 5/8 po"]
[{"$f":"IF(LEN('Translation-EN'!A323)>0,'Translation-EN'!A323,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B323)>0,'Translation-EN'!B323,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C323)>0,'Translation-EN'!C323,\"\")","v":"B191"},{"$f":"IF(LEN('Translation-EN'!D323)>0,'Translation-EN'!D323,\"\")","v":""},"AUTRES MATÉRIAUX DE BARDAGE"]
[{"$f":"IF(LEN('Translation-EN'!A324)>0,'Translation-EN'!A324,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B324)>0,'Translation-EN'!B324,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C324)>0,'Translation-EN'!C324,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D324)>0,'Translation-EN'!D324,\"\")","v":""},"SECTION 3 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A325)>0,'Translation-EN'!A325,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B325)>0,'Translation-EN'!B325,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C325)>0,'Translation-EN'!C325,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D325)>0,'Translation-EN'!D325,\"\")","v":""},"ÉLÉMENTS STRUCTURAUX"]
[{"$f":"IF(LEN('Translation-EN'!A326)>0,'Translation-EN'!A326,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B326)>0,'Translation-EN'!B326,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C326)>0,'Translation-EN'!C326,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D326)>0,'Translation-EN'!D326,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A327)>0,'Translation-EN'!A327,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B327)>0,'Translation-EN'!B327,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C327)>0,'Translation-EN'!C327,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D327)>0,'Translation-EN'!D327,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A328)>0,'Translation-EN'!A328,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B328)>0,'Translation-EN'!B328,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C328)>0,'Translation-EN'!C328,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D328)>0,'Translation-EN'!D328,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A329)>0,'Translation-EN'!A329,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B329)>0,'Translation-EN'!B329,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C329)>0,'Translation-EN'!C329,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D329)>0,'Translation-EN'!D329,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A330)>0,'Translation-EN'!A330,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B330)>0,'Translation-EN'!B330,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C330)>0,'Translation-EN'!C330,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D330)>0,'Translation-EN'!D330,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A331)>0,'Translation-EN'!A331,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B331)>0,'Translation-EN'!B331,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C331)>0,'Translation-EN'!C331,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D331)>0,'Translation-EN'!D331,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A332)>0,'Translation-EN'!A332,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B332)>0,'Translation-EN'!B332,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C332)>0,'Translation-EN'!C332,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D332)>0,'Translation-EN'!D332,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A333)>0,'Translation-EN'!A333,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B333)>0,'Translation-EN'!B333,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C333)>0,'Translation-EN'!C333,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D333)>0,'Translation-EN'!D333,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A334)>0,'Translation-EN'!A334,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B334)>0,'Translation-EN'!B334,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C334)>0,'Translation-EN'!C334,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D334)>0,'Translation-EN'!D334,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A335)>0,'Translation-EN'!A335,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B335)>0,'Translation-EN'!B335,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C335)>0,'Translation-EN'!C335,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D335)>0,'Translation-EN'!D335,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A336)>0,'Translation-EN'!A336,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B336)>0,'Translation-EN'!B336,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C336)>0,'Translation-EN'!C336,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D336)>0,'Translation-EN'!D336,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A337)>0,'Translation-EN'!A337,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B337)>0,'Translation-EN'!B337,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C337)>0,'Translation-EN'!C337,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D337)>0,'Translation-EN'!D337,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A338)>0,'Translation-EN'!A338,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B338)>0,'Translation-EN'!B338,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C338)>0,'Translation-EN'!C338,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D338)>0,'Translation-EN'!D338,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A339)>0,'Translation-EN'!A339,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B339)>0,'Translation-EN'!B339,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C339)>0,'Translation-EN'!C339,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D339)>0,'Translation-EN'!D339,\"\")","v":true},"TOTAL PARTIEL POUR LES ÉLÉMEMTS STRUCTURELS LOURDS kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A340)>0,'Translation-EN'!A340,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B340)>0,'Translation-EN'!B340,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C340)>0,'Translation-EN'!C340,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D340)>0,'Translation-EN'!D340,\"\")","v":""},"CHARPENTE EN BOIS LOURD"]
[{"$f":"IF(LEN('Translation-EN'!A341)>0,'Translation-EN'!A341,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B341)>0,'Translation-EN'!B341,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C341)>0,'Translation-EN'!C341,\"\")","v":"B6"},{"$f":"IF(LEN('Translation-EN'!D341)>0,'Translation-EN'!D341,\"\")","v":""},"BOIS MASSIF"]
[{"$f":"IF(LEN('Translation-EN'!A342)>0,'Translation-EN'!A342,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B342)>0,'Translation-EN'!B342,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C342)>0,'Translation-EN'!C342,\"\")","v":"A7"},{"$f":"IF(LEN('Translation-EN'!D342)>0,'Translation-EN'!D342,\"\")","v":""},"Utilisez la fonction % si plusieurs types de bois massifs sont utilisés."]
[{"$f":"IF(LEN('Translation-EN'!A343)>0,'Translation-EN'!A343,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B343)>0,'Translation-EN'!B343,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C343)>0,'Translation-EN'!C343,\"\")","v":"C7"},{"$f":"IF(LEN('Translation-EN'!D343)>0,'Translation-EN'!D343,\"\")","v":""},"Charpente lourde en bois – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A344)>0,'Translation-EN'!A344,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B344)>0,'Translation-EN'!B344,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C344)>0,'Translation-EN'!C344,\"\")","v":"A14"},{"$f":"IF(LEN('Translation-EN'!D344)>0,'Translation-EN'!D344,\"\")","v":""},"COMPOSANTS LOURDS EN ACIER"]
[{"$f":"IF(LEN('Translation-EN'!A345)>0,'Translation-EN'!A345,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B345)>0,'Translation-EN'!B345,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C345)>0,'Translation-EN'!C345,\"\")","v":"B15"},{"$f":"IF(LEN('Translation-EN'!D345)>0,'Translation-EN'!D345,\"\")","v":""},"POTEAUX ET POUTRES EN ACIER"]
[{"$f":"IF(LEN('Translation-EN'!A346)>0,'Translation-EN'!A346,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B346)>0,'Translation-EN'!B346,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C346)>0,'Translation-EN'!C346,\"\")","v":"A16"},{"$f":"IF(LEN('Translation-EN'!D346)>0,'Translation-EN'!D346,\"\")","v":""},"Sélectionnez la section de la poutre dans le menu déroulant et saisissez les mètres linéaires pour chaque type de composant, car les valeurs ne proviennent pas de la feuille de saisie de l’utilisateur."]
[{"$f":"IF(LEN('Translation-EN'!A347)>0,'Translation-EN'!A347,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B347)>0,'Translation-EN'!B347,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C347)>0,'Translation-EN'!C347,\"\")","v":"C16"},{"$f":"IF(LEN('Translation-EN'!D347)>0,'Translation-EN'!D347,\"\")","v":""},"Poutre en acier section W – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A348)>0,'Translation-EN'!A348,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B348)>0,'Translation-EN'!B348,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C348)>0,'Translation-EN'!C348,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D348)>0,'Translation-EN'!D348,\"\")","v":""},"SECTION 4 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A349)>0,'Translation-EN'!A349,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B349)>0,'Translation-EN'!B349,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C349)>0,'Translation-EN'!C349,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D349)>0,'Translation-EN'!D349,\"\")","v":""},"MURS EXTÉRIEURS"]
[{"$f":"IF(LEN('Translation-EN'!A350)>0,'Translation-EN'!A350,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B350)>0,'Translation-EN'!B350,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C350)>0,'Translation-EN'!C350,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D350)>0,'Translation-EN'!D350,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A351)>0,'Translation-EN'!A351,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B351)>0,'Translation-EN'!B351,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C351)>0,'Translation-EN'!C351,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D351)>0,'Translation-EN'!D351,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A352)>0,'Translation-EN'!A352,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B352)>0,'Translation-EN'!B352,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C352)>0,'Translation-EN'!C352,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D352)>0,'Translation-EN'!D352,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A353)>0,'Translation-EN'!A353,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B353)>0,'Translation-EN'!B353,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C353)>0,'Translation-EN'!C353,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D353)>0,'Translation-EN'!D353,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A354)>0,'Translation-EN'!A354,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B354)>0,'Translation-EN'!B354,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C354)>0,'Translation-EN'!C354,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D354)>0,'Translation-EN'!D354,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A355)>0,'Translation-EN'!A355,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B355)>0,'Translation-EN'!B355,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C355)>0,'Translation-EN'!C355,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D355)>0,'Translation-EN'!D355,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A356)>0,'Translation-EN'!A356,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B356)>0,'Translation-EN'!B356,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C356)>0,'Translation-EN'!C356,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D356)>0,'Translation-EN'!D356,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A357)>0,'Translation-EN'!A357,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B357)>0,'Translation-EN'!B357,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C357)>0,'Translation-EN'!C357,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D357)>0,'Translation-EN'!D357,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A358)>0,'Translation-EN'!A358,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B358)>0,'Translation-EN'!B358,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C358)>0,'Translation-EN'!C358,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D358)>0,'Translation-EN'!D358,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A359)>0,'Translation-EN'!A359,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B359)>0,'Translation-EN'!B359,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C359)>0,'Translation-EN'!C359,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D359)>0,'Translation-EN'!D359,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A360)>0,'Translation-EN'!A360,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B360)>0,'Translation-EN'!B360,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C360)>0,'Translation-EN'!C360,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D360)>0,'Translation-EN'!D360,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A361)>0,'Translation-EN'!A361,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B361)>0,'Translation-EN'!B361,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C361)>0,'Translation-EN'!C361,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D361)>0,'Translation-EN'!D361,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A362)>0,'Translation-EN'!A362,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B362)>0,'Translation-EN'!B362,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C362)>0,'Translation-EN'!C362,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D362)>0,'Translation-EN'!D362,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A363)>0,'Translation-EN'!A363,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B363)>0,'Translation-EN'!B363,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C363)>0,'Translation-EN'!C363,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D363)>0,'Translation-EN'!D363,\"\")","v":true},"TOTAL PARTIEL POUR LES MURS EXTÉRIEURS kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A364)>0,'Translation-EN'!A364,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B364)>0,'Translation-EN'!B364,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C364)>0,'Translation-EN'!C364,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D364)>0,'Translation-EN'!D364,\"\")","v":""},"MURS À CHARPENTE EN BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A365)>0,'Translation-EN'!A365,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B365)>0,'Translation-EN'!B365,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C365)>0,'Translation-EN'!C365,\"\")","v":"D5"},{"$f":"IF(LEN('Translation-EN'!D365)>0,'Translation-EN'!D365,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A366)>0,'Translation-EN'!A366,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B366)>0,'Translation-EN'!B366,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C366)>0,'Translation-EN'!C366,\"\")","v":"F5"},{"$f":"IF(LEN('Translation-EN'!D366)>0,'Translation-EN'!D366,\"\")","v":""},"po. o/ c"]
[{"$f":"IF(LEN('Translation-EN'!A367)>0,'Translation-EN'!A367,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B367)>0,'Translation-EN'!B367,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C367)>0,'Translation-EN'!C367,\"\")","v":"B6"},{"$f":"IF(LEN('Translation-EN'!D367)>0,'Translation-EN'!D367,\"\")","v":""},{"$f":"$E$298","v":"CONSTRUCTION EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A368)>0,'Translation-EN'!A368,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B368)>0,'Translation-EN'!B368,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C368)>0,'Translation-EN'!C368,\"\")","v":"B10"},{"$f":"IF(LEN('Translation-EN'!D368)>0,'Translation-EN'!D368,\"\")","v":""},{"$f":"$E$299","v":"2x4 double"}]
[{"$f":"IF(LEN('Translation-EN'!A369)>0,'Translation-EN'!A369,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B369)>0,'Translation-EN'!B369,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C369)>0,'Translation-EN'!C369,\"\")","v":"A11"},{"$f":"IF(LEN('Translation-EN'!D369)>0,'Translation-EN'!D369,\"\")","v":""},"MURS À CHARPENTE EN ACIER"]
[{"$f":"IF(LEN('Translation-EN'!A370)>0,'Translation-EN'!A370,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B370)>0,'Translation-EN'!B370,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C370)>0,'Translation-EN'!C370,\"\")","v":"D11"},{"$f":"IF(LEN('Translation-EN'!D370)>0,'Translation-EN'!D370,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A371)>0,'Translation-EN'!A371,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B371)>0,'Translation-EN'!B371,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C371)>0,'Translation-EN'!C371,\"\")","v":"F11"},{"$f":"IF(LEN('Translation-EN'!D371)>0,'Translation-EN'!D371,\"\")","v":""},{"$f":"$E$366","v":"po. o/ c"}]
[{"$f":"IF(LEN('Translation-EN'!A372)>0,'Translation-EN'!A372,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B372)>0,'Translation-EN'!B372,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C372)>0,'Translation-EN'!C372,\"\")","v":"B12"},{"$f":"IF(LEN('Translation-EN'!D372)>0,'Translation-EN'!D372,\"\")","v":""},"CHARPENTE D’ACIER, 2x6"]
[{"$f":"IF(LEN('Translation-EN'!A373)>0,'Translation-EN'!A373,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B373)>0,'Translation-EN'!B373,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C373)>0,'Translation-EN'!C373,\"\")","v":"A13"},{"$f":"IF(LEN('Translation-EN'!D373)>0,'Translation-EN'!D373,\"\")","v":""},"Utilisez la fonction % pour ajuster d’autres calibres de goujons en acier en fonction du rapport masse d’acier par unité de longueur."]
[{"$f":"IF(LEN('Translation-EN'!A374)>0,'Translation-EN'!A374,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B374)>0,'Translation-EN'!B374,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C374)>0,'Translation-EN'!C374,\"\")","v":"C13"},{"$f":"IF(LEN('Translation-EN'!D374)>0,'Translation-EN'!D374,\"\")","v":""},"Charpente en acier – porteur – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A375)>0,'Translation-EN'!A375,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B375)>0,'Translation-EN'!B375,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C375)>0,'Translation-EN'!C375,\"\")","v":"A19"},{"$f":"IF(LEN('Translation-EN'!D375)>0,'Translation-EN'!D375,\"\")","v":""},"CHARPENTE DE POUTRES EN I EN BOIS (TJI)"]
[{"$f":"IF(LEN('Translation-EN'!A376)>0,'Translation-EN'!A376,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B376)>0,'Translation-EN'!B376,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C376)>0,'Translation-EN'!C376,\"\")","v":"D19"},{"$f":"IF(LEN('Translation-EN'!D376)>0,'Translation-EN'!D376,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A377)>0,'Translation-EN'!A377,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B377)>0,'Translation-EN'!B377,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C377)>0,'Translation-EN'!C377,\"\")","v":"F19"},{"$f":"IF(LEN('Translation-EN'!D377)>0,'Translation-EN'!D377,\"\")","v":""},{"$f":"$E$366","v":"po. o/ c"}]
[{"$f":"IF(LEN('Translation-EN'!A378)>0,'Translation-EN'!A378,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B378)>0,'Translation-EN'!B378,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C378)>0,'Translation-EN'!C378,\"\")","v":"A20"},{"$f":"IF(LEN('Translation-EN'!D378)>0,'Translation-EN'!D378,\"\")","v":""},"Ne comprend pas les autres éléments de la charpente. Pour les inclure, utilisez la section Construction à charpente de bois ci-dessus pour entrer le pourcentage du mur qui est en bois."]
[{"$f":"IF(LEN('Translation-EN'!A379)>0,'Translation-EN'!A379,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B379)>0,'Translation-EN'!B379,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C379)>0,'Translation-EN'!C379,\"\")","v":"A22"},{"$f":"IF(LEN('Translation-EN'!D379)>0,'Translation-EN'!D379,\"\")","v":""},"MURS EN BOIS LAMINÉ CROISÉ –3-1/2 po (90 mm)"]
[{"$f":"IF(LEN('Translation-EN'!A380)>0,'Translation-EN'!A380,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B380)>0,'Translation-EN'!B380,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C380)>0,'Translation-EN'!C380,\"\")","v":"B23"},{"$f":"IF(LEN('Translation-EN'!D380)>0,'Translation-EN'!D380,\"\")","v":""},"BOIS LAMELLÉ-CROISÉ"]
[{"$f":"IF(LEN('Translation-EN'!A381)>0,'Translation-EN'!A381,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B381)>0,'Translation-EN'!B381,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C381)>0,'Translation-EN'!C381,\"\")","v":"C24"},{"$f":"IF(LEN('Translation-EN'!D381)>0,'Translation-EN'!D381,\"\")","v":""},"Bois lamellé-croisé – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A382)>0,'Translation-EN'!A382,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B382)>0,'Translation-EN'!B382,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C382)>0,'Translation-EN'!C382,\"\")","v":"A25"},{"$f":"IF(LEN('Translation-EN'!D382)>0,'Translation-EN'!D382,\"\")","v":""},"Utilisez la fonction % pour régler d’autres épaisseurs de panneaux de Bois lamellé-croisé (BLC)."]
[{"$f":"IF(LEN('Translation-EN'!A383)>0,'Translation-EN'!A383,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B383)>0,'Translation-EN'!B383,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C383)>0,'Translation-EN'!C383,\"\")","v":"A28"},{"$f":"IF(LEN('Translation-EN'!D383)>0,'Translation-EN'!D383,\"\")","v":""},"MURS EN ÉLÉMENTS DE MAÇONNERIE EN BÉTON"]
[{"$f":"IF(LEN('Translation-EN'!A384)>0,'Translation-EN'!A384,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B384)>0,'Translation-EN'!B384,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C384)>0,'Translation-EN'!C384,\"\")","v":"B29"},{"$f":"IF(LEN('Translation-EN'!D384)>0,'Translation-EN'!D384,\"\")","v":""},"EMB 8 po – CREUX, SANS COULIS"]
[{"$f":"IF(LEN('Translation-EN'!A385)>0,'Translation-EN'!A385,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B385)>0,'Translation-EN'!B385,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C385)>0,'Translation-EN'!C385,\"\")","v":"C30"},{"$f":"IF(LEN('Translation-EN'!D385)>0,'Translation-EN'!D385,\"\")","v":""},"EMB 8 po – creux, sans coulis – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A386)>0,'Translation-EN'!A386,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B386)>0,'Translation-EN'!B386,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C386)>0,'Translation-EN'!C386,\"\")","v":"A31"},{"$f":"IF(LEN('Translation-EN'!D386)>0,'Translation-EN'!D386,\"\")","v":""},"Utilisez la fonction % pour régler d’autres épaisseurs de EMB. Si c’est le cas, entrez le volume de remplissage dans la section REMPLISSAGE DU BÉTON pour les murs en EMB ci-dessous."]
[{"$f":"IF(LEN('Translation-EN'!A387)>0,'Translation-EN'!A387,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B387)>0,'Translation-EN'!B387,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C387)>0,'Translation-EN'!C387,\"\")","v":"A37"},{"$f":"IF(LEN('Translation-EN'!D387)>0,'Translation-EN'!D387,\"\")","v":""},"REMPLISSAGE EN BÉTON POUR LES MURS EN EMB"]
[{"$f":"IF(LEN('Translation-EN'!A388)>0,'Translation-EN'!A388,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B388)>0,'Translation-EN'!B388,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C388)>0,'Translation-EN'!C388,\"\")","v":"D37"},{"$f":"IF(LEN('Translation-EN'!D388)>0,'Translation-EN'!D388,\"\")","v":""},"VOLUME DE BÉTON"]
[{"$f":"IF(LEN('Translation-EN'!A389)>0,'Translation-EN'!A389,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B389)>0,'Translation-EN'!B389,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C389)>0,'Translation-EN'!C389,\"\")","v":"B38"},{"$f":"IF(LEN('Translation-EN'!D389)>0,'Translation-EN'!D389,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A390)>0,'Translation-EN'!A390,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B390)>0,'Translation-EN'!B390,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C390)>0,'Translation-EN'!C390,\"\")","v":"A39"},{"$f":"IF(LEN('Translation-EN'!D390)>0,'Translation-EN'!D390,\"\")","v":""},"Calculez le volume total de béton de remplissage nécessaire pour la surface du mur en EMB saisie ci-dessus."]
[{"$f":"IF(LEN('Translation-EN'!A391)>0,'Translation-EN'!A391,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B391)>0,'Translation-EN'!B391,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C391)>0,'Translation-EN'!C391,\"\")","v":"B46"},{"$f":"IF(LEN('Translation-EN'!D391)>0,'Translation-EN'!D391,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A392)>0,'Translation-EN'!A392,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B392)>0,'Translation-EN'!B392,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C392)>0,'Translation-EN'!C392,\"\")","v":"A47"},{"$f":"IF(LEN('Translation-EN'!D392)>0,'Translation-EN'!D392,\"\")","v":""},{"$f":"$E$390","v":"Calculez le volume total de béton de remplissage nécessaire pour la surface du mur en EMB saisie ci-dessus."}]
[{"$f":"IF(LEN('Translation-EN'!A393)>0,'Translation-EN'!A393,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B393)>0,'Translation-EN'!B393,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C393)>0,'Translation-EN'!C393,\"\")","v":"A54"},{"$f":"IF(LEN('Translation-EN'!D393)>0,'Translation-EN'!D393,\"\")","v":""},"PANNEAUX STRUCTURAUX"]
[{"$f":"IF(LEN('Translation-EN'!A394)>0,'Translation-EN'!A394,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B394)>0,'Translation-EN'!B394,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C394)>0,'Translation-EN'!C394,\"\")","v":"B55"},{"$f":"IF(LEN('Translation-EN'!D394)>0,'Translation-EN'!D394,\"\")","v":""},"PANNEAU À COPEAUX ORIENTÉS"]
[{"$f":"IF(LEN('Translation-EN'!A395)>0,'Translation-EN'!A395,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B395)>0,'Translation-EN'!B395,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C395)>0,'Translation-EN'!C395,\"\")","v":"B60"},{"$f":"IF(LEN('Translation-EN'!D395)>0,'Translation-EN'!D395,\"\")","v":""},"CONTREPLAQUÉ"]
[{"$f":"IF(LEN('Translation-EN'!A396)>0,'Translation-EN'!A396,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B396)>0,'Translation-EN'!B396,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C396)>0,'Translation-EN'!C396,\"\")","v":"B64"},{"$f":"IF(LEN('Translation-EN'!D396)>0,'Translation-EN'!D396,\"\")","v":""},"PANNEAUX STRUCTURAUX EN GYPSE"]
[{"$f":"IF(LEN('Translation-EN'!A397)>0,'Translation-EN'!A397,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B397)>0,'Translation-EN'!B397,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C397)>0,'Translation-EN'!C397,\"\")","v":"B68"},{"$f":"IF(LEN('Translation-EN'!D397)>0,'Translation-EN'!D397,\"\")","v":""},"PANNEAU DE CIMENT"]
[{"$f":"IF(LEN('Translation-EN'!A398)>0,'Translation-EN'!A398,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B398)>0,'Translation-EN'!B398,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C398)>0,'Translation-EN'!C398,\"\")","v":"A71"},{"$f":"IF(LEN('Translation-EN'!D398)>0,'Translation-EN'!D398,\"\")","v":""},{"$f":"$E$305","v":"ISOLATION DE LA CAVITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A399)>0,'Translation-EN'!A399,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B399)>0,'Translation-EN'!B399,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C399)>0,'Translation-EN'!C399,\"\")","v":"B72"},{"$f":"IF(LEN('Translation-EN'!D399)>0,'Translation-EN'!D399,\"\")","v":""},{"$f":"$E$307","v":"NATTE DE FIBRE DE VERRE"}]
[{"$f":"IF(LEN('Translation-EN'!A400)>0,'Translation-EN'!A400,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B400)>0,'Translation-EN'!B400,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C400)>0,'Translation-EN'!C400,\"\")","v":"C73"},{"$f":"IF(LEN('Translation-EN'!D400)>0,'Translation-EN'!D400,\"\")","v":""},"Natte en fibre de verre – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A401)>0,'Translation-EN'!A401,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B401)>0,'Translation-EN'!B401,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C401)>0,'Translation-EN'!C401,\"\")","v":"B77"},{"$f":"IF(LEN('Translation-EN'!D401)>0,'Translation-EN'!D401,\"\")","v":""},"FIBRE DE VERRE SOUFFLÉE"]
[{"$f":"IF(LEN('Translation-EN'!A402)>0,'Translation-EN'!A402,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B402)>0,'Translation-EN'!B402,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C402)>0,'Translation-EN'!C402,\"\")","v":"C78"},{"$f":"IF(LEN('Translation-EN'!D402)>0,'Translation-EN'!D402,\"\")","v":""},"Fibre de verre en vrac – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A403)>0,'Translation-EN'!A403,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B403)>0,'Translation-EN'!B403,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C403)>0,'Translation-EN'!C403,\"\")","v":"B83"},{"$f":"IF(LEN('Translation-EN'!D403)>0,'Translation-EN'!D403,\"\")","v":""},{"$f":"$E$311","v":"NATTE DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A404)>0,'Translation-EN'!A404,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B404)>0,'Translation-EN'!B404,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C404)>0,'Translation-EN'!C404,\"\")","v":"B91"},{"$f":"IF(LEN('Translation-EN'!D404)>0,'Translation-EN'!D404,\"\")","v":""},{"$f":"$E$309","v":"ISOLATION EN CELLULOSE"}]
[{"$f":"IF(LEN('Translation-EN'!A405)>0,'Translation-EN'!A405,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B405)>0,'Translation-EN'!B405,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C405)>0,'Translation-EN'!C405,\"\")","v":"C92"},{"$f":"IF(LEN('Translation-EN'!D405)>0,'Translation-EN'!D405,\"\")","v":""},"Cellulose – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A406)>0,'Translation-EN'!A406,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B406)>0,'Translation-EN'!B406,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C406)>0,'Translation-EN'!C406,\"\")","v":"B96"},{"$f":"IF(LEN('Translation-EN'!D406)>0,'Translation-EN'!D406,\"\")","v":""},{"$f":"$E$313","v":"NATTE DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A407)>0,'Translation-EN'!A407,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B407)>0,'Translation-EN'!B407,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C407)>0,'Translation-EN'!C407,\"\")","v":"C97"},{"$f":"IF(LEN('Translation-EN'!D407)>0,'Translation-EN'!D407,\"\")","v":""},"Natte de fibres de bois – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A408)>0,'Translation-EN'!A408,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B408)>0,'Translation-EN'!B408,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C408)>0,'Translation-EN'!C408,\"\")","v":"B102"},{"$f":"IF(LEN('Translation-EN'!D408)>0,'Translation-EN'!D408,\"\")","v":""},"AUTRES ISOLANTS EN FIBRES NATURELLES"]
[{"$f":"IF(LEN('Translation-EN'!A409)>0,'Translation-EN'!A409,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B409)>0,'Translation-EN'!B409,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C409)>0,'Translation-EN'!C409,\"\")","v":"B108"},{"$f":"IF(LEN('Translation-EN'!D409)>0,'Translation-EN'!D409,\"\")","v":""},"MOUSSE À PULVÉRISER – CELLULE FERMÉE"]
[{"$f":"IF(LEN('Translation-EN'!A410)>0,'Translation-EN'!A410,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B410)>0,'Translation-EN'!B410,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C410)>0,'Translation-EN'!C410,\"\")","v":"B112"},{"$f":"IF(LEN('Translation-EN'!D410)>0,'Translation-EN'!D410,\"\")","v":""},"MOUSSE À PULVÉRISER – CELLULE OUVERTE"]
[{"$f":"IF(LEN('Translation-EN'!A411)>0,'Translation-EN'!A411,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B411)>0,'Translation-EN'!B411,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C411)>0,'Translation-EN'!C411,\"\")","v":"B115"},{"$f":"IF(LEN('Translation-EN'!D411)>0,'Translation-EN'!D411,\"\")","v":""},"BRIQUES DE CHANVRE"]
[{"$f":"IF(LEN('Translation-EN'!A412)>0,'Translation-EN'!A412,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B412)>0,'Translation-EN'!B412,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C412)>0,'Translation-EN'!C412,\"\")","v":"C116"},{"$f":"IF(LEN('Translation-EN'!D412)>0,'Translation-EN'!D412,\"\")","v":""},"Briques de chanvre – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A413)>0,'Translation-EN'!A413,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B413)>0,'Translation-EN'!B413,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C413)>0,'Translation-EN'!C413,\"\")","v":"A120"},{"$f":"IF(LEN('Translation-EN'!D413)>0,'Translation-EN'!D413,\"\")","v":""},"ISOLATION CONTINUE (EXT. ou INT.)"]
[{"$f":"IF(LEN('Translation-EN'!A414)>0,'Translation-EN'!A414,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B414)>0,'Translation-EN'!B414,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C414)>0,'Translation-EN'!C414,\"\")","v":"B121"},{"$f":"IF(LEN('Translation-EN'!D414)>0,'Translation-EN'!D414,\"\")","v":""},{"$f":"$E$211","v":"PANNEAU DE MOUSSE EPS"}]
[{"$f":"IF(LEN('Translation-EN'!A415)>0,'Translation-EN'!A415,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B415)>0,'Translation-EN'!B415,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C415)>0,'Translation-EN'!C415,\"\")","v":"C122"},{"$f":"IF(LEN('Translation-EN'!D415)>0,'Translation-EN'!D415,\"\")","v":""},{"$f":"$E$212","v":"Panneau de mousse EPS – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A416)>0,'Translation-EN'!A416,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B416)>0,'Translation-EN'!B416,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C416)>0,'Translation-EN'!C416,\"\")","v":"B125"},{"$f":"IF(LEN('Translation-EN'!D416)>0,'Translation-EN'!D416,\"\")","v":""},{"$f":"$E$270","v":"PANNEAU DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A417)>0,'Translation-EN'!A417,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B417)>0,'Translation-EN'!B417,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C417)>0,'Translation-EN'!C417,\"\")","v":"C126"},{"$f":"IF(LEN('Translation-EN'!D417)>0,'Translation-EN'!D417,\"\")","v":""},{"$f":"$E$271","v":"Panneau de fibres de bois – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A418)>0,'Translation-EN'!A418,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B418)>0,'Translation-EN'!B418,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C418)>0,'Translation-EN'!C418,\"\")","v":"B132"},{"$f":"IF(LEN('Translation-EN'!D418)>0,'Translation-EN'!D418,\"\")","v":""},{"$f":"$E$213","v":"PANNEAU DE MOUSSE XPS"}]
[{"$f":"IF(LEN('Translation-EN'!A419)>0,'Translation-EN'!A419,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B419)>0,'Translation-EN'!B419,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C419)>0,'Translation-EN'!C419,\"\")","v":"C133"},{"$f":"IF(LEN('Translation-EN'!D419)>0,'Translation-EN'!D419,\"\")","v":""},{"$f":"$E$214","v":"Panneau de mousse XPS – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A420)>0,'Translation-EN'!A420,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B420)>0,'Translation-EN'!B420,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C420)>0,'Translation-EN'!C420,\"\")","v":"B138"},{"$f":"IF(LEN('Translation-EN'!D420)>0,'Translation-EN'!D420,\"\")","v":""},"PANNEAU DE MOUSSE POLYISOCYANURATE"]
[{"$f":"IF(LEN('Translation-EN'!A421)>0,'Translation-EN'!A421,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B421)>0,'Translation-EN'!B421,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C421)>0,'Translation-EN'!C421,\"\")","v":"C139"},{"$f":"IF(LEN('Translation-EN'!D421)>0,'Translation-EN'!D421,\"\")","v":""},"Polyisocyanurate – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A422)>0,'Translation-EN'!A422,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B422)>0,'Translation-EN'!B422,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C422)>0,'Translation-EN'!C422,\"\")","v":"B144"},{"$f":"IF(LEN('Translation-EN'!D422)>0,'Translation-EN'!D422,\"\")","v":""},{"$f":"$E$215","v":"PANNEAU DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A423)>0,'Translation-EN'!A423,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B423)>0,'Translation-EN'!B423,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C423)>0,'Translation-EN'!C423,\"\")","v":"C145"},{"$f":"IF(LEN('Translation-EN'!D423)>0,'Translation-EN'!D423,\"\")","v":""},"Panneau de laine minérale – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A424)>0,'Translation-EN'!A424,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B424)>0,'Translation-EN'!B424,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C424)>0,'Translation-EN'!C424,\"\")","v":"A149"},{"$f":"IF(LEN('Translation-EN'!D424)>0,'Translation-EN'!D424,\"\")","v":""},"ISOLATION À VALEUR R ÉLEVÉE"]
[{"$f":"IF(LEN('Translation-EN'!A425)>0,'Translation-EN'!A425,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B425)>0,'Translation-EN'!B425,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C425)>0,'Translation-EN'!C425,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D425)>0,'Translation-EN'!D425,\"\")","v":""},"SECTION 5 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A426)>0,'Translation-EN'!A426,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B426)>0,'Translation-EN'!B426,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C426)>0,'Translation-EN'!C426,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D426)>0,'Translation-EN'!D426,\"\")","v":""},"SYSTÈMES DE MUR EXTÉRIEUR"]
[{"$f":"IF(LEN('Translation-EN'!A427)>0,'Translation-EN'!A427,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B427)>0,'Translation-EN'!B427,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C427)>0,'Translation-EN'!C427,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D427)>0,'Translation-EN'!D427,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A428)>0,'Translation-EN'!A428,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B428)>0,'Translation-EN'!B428,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C428)>0,'Translation-EN'!C428,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D428)>0,'Translation-EN'!D428,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A429)>0,'Translation-EN'!A429,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B429)>0,'Translation-EN'!B429,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C429)>0,'Translation-EN'!C429,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D429)>0,'Translation-EN'!D429,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A430)>0,'Translation-EN'!A430,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B430)>0,'Translation-EN'!B430,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C430)>0,'Translation-EN'!C430,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D430)>0,'Translation-EN'!D430,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A431)>0,'Translation-EN'!A431,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B431)>0,'Translation-EN'!B431,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C431)>0,'Translation-EN'!C431,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D431)>0,'Translation-EN'!D431,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A432)>0,'Translation-EN'!A432,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B432)>0,'Translation-EN'!B432,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C432)>0,'Translation-EN'!C432,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D432)>0,'Translation-EN'!D432,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A433)>0,'Translation-EN'!A433,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B433)>0,'Translation-EN'!B433,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C433)>0,'Translation-EN'!C433,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D433)>0,'Translation-EN'!D433,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A434)>0,'Translation-EN'!A434,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B434)>0,'Translation-EN'!B434,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C434)>0,'Translation-EN'!C434,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D434)>0,'Translation-EN'!D434,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A435)>0,'Translation-EN'!A435,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B435)>0,'Translation-EN'!B435,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C435)>0,'Translation-EN'!C435,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D435)>0,'Translation-EN'!D435,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A436)>0,'Translation-EN'!A436,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B436)>0,'Translation-EN'!B436,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C436)>0,'Translation-EN'!C436,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D436)>0,'Translation-EN'!D436,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A437)>0,'Translation-EN'!A437,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B437)>0,'Translation-EN'!B437,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C437)>0,'Translation-EN'!C437,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D437)>0,'Translation-EN'!D437,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A438)>0,'Translation-EN'!A438,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B438)>0,'Translation-EN'!B438,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C438)>0,'Translation-EN'!C438,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D438)>0,'Translation-EN'!D438,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A439)>0,'Translation-EN'!A439,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B439)>0,'Translation-EN'!B439,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C439)>0,'Translation-EN'!C439,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D439)>0,'Translation-EN'!D439,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A440)>0,'Translation-EN'!A440,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B440)>0,'Translation-EN'!B440,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C440)>0,'Translation-EN'!C440,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D440)>0,'Translation-EN'!D440,\"\")","v":true},"TOTAL PARTIEL POUR LES SYSTÈMES DE MURS EXTÉRIEURS kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A441)>0,'Translation-EN'!A441,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B441)>0,'Translation-EN'!B441,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C441)>0,'Translation-EN'!C441,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D441)>0,'Translation-EN'!D441,\"\")","v":""},{"$f":"$E$274","v":"COFFRAGES ISOLÉS EN BÉTON (CIB) – MOUSSE EPS"}]
[{"$f":"IF(LEN('Translation-EN'!A442)>0,'Translation-EN'!A442,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B442)>0,'Translation-EN'!B442,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C442)>0,'Translation-EN'!C442,\"\")","v":"A6"},{"$f":"IF(LEN('Translation-EN'!D442)>0,'Translation-EN'!D442,\"\")","v":""},{"$f":"$E$275","v":"Étape 1 : Sélectionnez la taille du CIB"}]
[{"$f":"IF(LEN('Translation-EN'!A443)>0,'Translation-EN'!A443,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B443)>0,'Translation-EN'!B443,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C443)>0,'Translation-EN'!C443,\"\")","v":"B7"},{"$f":"IF(LEN('Translation-EN'!D443)>0,'Translation-EN'!D443,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A444)>0,'Translation-EN'!A444,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B444)>0,'Translation-EN'!B444,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C444)>0,'Translation-EN'!C444,\"\")","v":"A8"},{"$f":"IF(LEN('Translation-EN'!D444)>0,'Translation-EN'!D444,\"\")","v":""},{"$f":"$E$277","v":"Étape 2 : Sélectionnez l’option de remplissage en béton."}]
[{"$f":"IF(LEN('Translation-EN'!A445)>0,'Translation-EN'!A445,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B445)>0,'Translation-EN'!B445,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C445)>0,'Translation-EN'!C445,\"\")","v":"B15"},{"$f":"IF(LEN('Translation-EN'!D445)>0,'Translation-EN'!D445,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A446)>0,'Translation-EN'!A446,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B446)>0,'Translation-EN'!B446,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C446)>0,'Translation-EN'!C446,\"\")","v":"A16"},{"$f":"IF(LEN('Translation-EN'!D446)>0,'Translation-EN'!D446,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A447)>0,'Translation-EN'!A447,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B447)>0,'Translation-EN'!B447,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C447)>0,'Translation-EN'!C447,\"\")","v":"B23"},{"$f":"IF(LEN('Translation-EN'!D447)>0,'Translation-EN'!D447,\"\")","v":""},{"$f":"$E$187","v":"BÉTON –31-35 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A448)>0,'Translation-EN'!A448,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B448)>0,'Translation-EN'!B448,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C448)>0,'Translation-EN'!C448,\"\")","v":"A24"},{"$f":"IF(LEN('Translation-EN'!D448)>0,'Translation-EN'!D448,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A449)>0,'Translation-EN'!A449,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B449)>0,'Translation-EN'!B449,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C449)>0,'Translation-EN'!C449,\"\")","v":"A31"},{"$f":"IF(LEN('Translation-EN'!D449)>0,'Translation-EN'!D449,\"\")","v":""},{"$f":"$E$282","v":"COFFRAGES ISOLÉS EN BÉTON (CIB) – COPEAUX DE BOIS/CIMENT"}]
[{"$f":"IF(LEN('Translation-EN'!A450)>0,'Translation-EN'!A450,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B450)>0,'Translation-EN'!B450,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C450)>0,'Translation-EN'!C450,\"\")","v":"A32"},{"$f":"IF(LEN('Translation-EN'!D450)>0,'Translation-EN'!D450,\"\")","v":""},"Étape 1 : Choisir la taille et l’isolation des CIB"]
[{"$f":"IF(LEN('Translation-EN'!A451)>0,'Translation-EN'!A451,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B451)>0,'Translation-EN'!B451,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C451)>0,'Translation-EN'!C451,\"\")","v":"B36"},{"$f":"IF(LEN('Translation-EN'!D451)>0,'Translation-EN'!D451,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A452)>0,'Translation-EN'!A452,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B452)>0,'Translation-EN'!B452,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C452)>0,'Translation-EN'!C452,\"\")","v":"A37"},{"$f":"IF(LEN('Translation-EN'!D452)>0,'Translation-EN'!D452,\"\")","v":true},"Étape 2 : Sélectionnez l'option de remplissage en béton pour le système de mur en CIB. La quantité de béton s'adapte à la taille du CIB choisi."]
[{"$f":"IF(LEN('Translation-EN'!A453)>0,'Translation-EN'!A453,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B453)>0,'Translation-EN'!B453,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C453)>0,'Translation-EN'!C453,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D453)>0,'Translation-EN'!D453,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A454)>0,'Translation-EN'!A454,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B454)>0,'Translation-EN'!B454,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C454)>0,'Translation-EN'!C454,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D454)>0,'Translation-EN'!D454,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A455)>0,'Translation-EN'!A455,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B455)>0,'Translation-EN'!B455,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C455)>0,'Translation-EN'!C455,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D455)>0,'Translation-EN'!D455,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A456)>0,'Translation-EN'!A456,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B456)>0,'Translation-EN'!B456,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C456)>0,'Translation-EN'!C456,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D456)>0,'Translation-EN'!D456,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A457)>0,'Translation-EN'!A457,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B457)>0,'Translation-EN'!B457,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C457)>0,'Translation-EN'!C457,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D457)>0,'Translation-EN'!D457,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A458)>0,'Translation-EN'!A458,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B458)>0,'Translation-EN'!B458,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C458)>0,'Translation-EN'!C458,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D458)>0,'Translation-EN'!D458,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A459)>0,'Translation-EN'!A459,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B459)>0,'Translation-EN'!B459,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C459)>0,'Translation-EN'!C459,\"\")","v":"B44"},{"$f":"IF(LEN('Translation-EN'!D459)>0,'Translation-EN'!D459,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A460)>0,'Translation-EN'!A460,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B460)>0,'Translation-EN'!B460,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C460)>0,'Translation-EN'!C460,\"\")","v":"A45"},{"$f":"IF(LEN('Translation-EN'!D460)>0,'Translation-EN'!D460,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A461)>0,'Translation-EN'!A461,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B461)>0,'Translation-EN'!B461,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C461)>0,'Translation-EN'!C461,\"\")","v":"B52"},{"$f":"IF(LEN('Translation-EN'!D461)>0,'Translation-EN'!D461,\"\")","v":""},{"$f":"$E$187","v":"BÉTON –31-35 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A462)>0,'Translation-EN'!A462,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B462)>0,'Translation-EN'!B462,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C462)>0,'Translation-EN'!C462,\"\")","v":"A53"},{"$f":"IF(LEN('Translation-EN'!D462)>0,'Translation-EN'!D462,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A463)>0,'Translation-EN'!A463,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B463)>0,'Translation-EN'!B463,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C463)>0,'Translation-EN'!C463,\"\")","v":"A60"},{"$f":"IF(LEN('Translation-EN'!D463)>0,'Translation-EN'!D463,\"\")","v":""},"PANNEAUX PRÉFABRIQUÉS"]
[{"$f":"IF(LEN('Translation-EN'!A464)>0,'Translation-EN'!A464,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B464)>0,'Translation-EN'!B464,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C464)>0,'Translation-EN'!C464,\"\")","v":"B61"},{"$f":"IF(LEN('Translation-EN'!D464)>0,'Translation-EN'!D464,\"\")","v":""},"CHARPENTE BOIS ET PANNEAUX DE PAILLE"]
[{"$f":"IF(LEN('Translation-EN'!A465)>0,'Translation-EN'!A465,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B465)>0,'Translation-EN'!B465,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C465)>0,'Translation-EN'!C465,\"\")","v":"B64"},{"$f":"IF(LEN('Translation-EN'!D465)>0,'Translation-EN'!D465,\"\")","v":""},"PANNEAUX STRUCTURELS ISOLÉS – MOUSSE OSB ET EPS"]
[{"$f":"IF(LEN('Translation-EN'!A466)>0,'Translation-EN'!A466,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B466)>0,'Translation-EN'!B466,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C466)>0,'Translation-EN'!C466,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D466)>0,'Translation-EN'!D466,\"\")","v":""},"SECTION 6 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A467)>0,'Translation-EN'!A467,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B467)>0,'Translation-EN'!B467,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C467)>0,'Translation-EN'!C467,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D467)>0,'Translation-EN'!D467,\"\")","v":""},"MURS MITOYENS"]
[{"$f":"IF(LEN('Translation-EN'!A468)>0,'Translation-EN'!A468,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B468)>0,'Translation-EN'!B468,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C468)>0,'Translation-EN'!C468,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D468)>0,'Translation-EN'!D468,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A469)>0,'Translation-EN'!A469,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B469)>0,'Translation-EN'!B469,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C469)>0,'Translation-EN'!C469,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D469)>0,'Translation-EN'!D469,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A470)>0,'Translation-EN'!A470,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B470)>0,'Translation-EN'!B470,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C470)>0,'Translation-EN'!C470,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D470)>0,'Translation-EN'!D470,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A471)>0,'Translation-EN'!A471,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B471)>0,'Translation-EN'!B471,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C471)>0,'Translation-EN'!C471,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D471)>0,'Translation-EN'!D471,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A472)>0,'Translation-EN'!A472,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B472)>0,'Translation-EN'!B472,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C472)>0,'Translation-EN'!C472,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D472)>0,'Translation-EN'!D472,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A473)>0,'Translation-EN'!A473,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B473)>0,'Translation-EN'!B473,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C473)>0,'Translation-EN'!C473,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D473)>0,'Translation-EN'!D473,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A474)>0,'Translation-EN'!A474,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B474)>0,'Translation-EN'!B474,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C474)>0,'Translation-EN'!C474,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D474)>0,'Translation-EN'!D474,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A475)>0,'Translation-EN'!A475,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B475)>0,'Translation-EN'!B475,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C475)>0,'Translation-EN'!C475,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D475)>0,'Translation-EN'!D475,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A476)>0,'Translation-EN'!A476,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B476)>0,'Translation-EN'!B476,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C476)>0,'Translation-EN'!C476,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D476)>0,'Translation-EN'!D476,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A477)>0,'Translation-EN'!A477,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B477)>0,'Translation-EN'!B477,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C477)>0,'Translation-EN'!C477,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D477)>0,'Translation-EN'!D477,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A478)>0,'Translation-EN'!A478,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B478)>0,'Translation-EN'!B478,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C478)>0,'Translation-EN'!C478,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D478)>0,'Translation-EN'!D478,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A479)>0,'Translation-EN'!A479,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B479)>0,'Translation-EN'!B479,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C479)>0,'Translation-EN'!C479,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D479)>0,'Translation-EN'!D479,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A480)>0,'Translation-EN'!A480,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B480)>0,'Translation-EN'!B480,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C480)>0,'Translation-EN'!C480,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D480)>0,'Translation-EN'!D480,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A481)>0,'Translation-EN'!A481,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B481)>0,'Translation-EN'!B481,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C481)>0,'Translation-EN'!C481,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D481)>0,'Translation-EN'!D481,\"\")","v":true},"TOTAL PARTIEL POUR LES MURS MITOYENS kgCO2e "]
[{"$f":"IF(LEN('Translation-EN'!A482)>0,'Translation-EN'!A482,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B482)>0,'Translation-EN'!B482,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C482)>0,'Translation-EN'!C482,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D482)>0,'Translation-EN'!D482,\"\")","v":true},"Note : n’incluez que la moitié de l’épaisseur des matériaux du mur mitoyen total en utilisant les champs de pourcentage ou de valeur R.\n(L’autre moitié appartient au bâtiment adjacent)."]
[{"$f":"IF(LEN('Translation-EN'!A483)>0,'Translation-EN'!A483,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B483)>0,'Translation-EN'!B483,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C483)>0,'Translation-EN'!C483,\"\")","v":"A6"},{"$f":"IF(LEN('Translation-EN'!D483)>0,'Translation-EN'!D483,\"\")","v":""},"CHARPENTE DE MUR MITOYEN"]
[{"$f":"IF(LEN('Translation-EN'!A484)>0,'Translation-EN'!A484,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B484)>0,'Translation-EN'!B484,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C484)>0,'Translation-EN'!C484,\"\")","v":"A7"},{"$f":"IF(LEN('Translation-EN'!D484)>0,'Translation-EN'!D484,\"\")","v":""},{"$f":"$E$364","v":"MURS À CHARPENTE EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A485)>0,'Translation-EN'!A485,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B485)>0,'Translation-EN'!B485,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C485)>0,'Translation-EN'!C485,\"\")","v":"D7"},{"$f":"IF(LEN('Translation-EN'!D485)>0,'Translation-EN'!D485,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A486)>0,'Translation-EN'!A486,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B486)>0,'Translation-EN'!B486,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C486)>0,'Translation-EN'!C486,\"\")","v":"B8"},{"$f":"IF(LEN('Translation-EN'!D486)>0,'Translation-EN'!D486,\"\")","v":""},{"$f":"$E$298","v":"CONSTRUCTION EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A487)>0,'Translation-EN'!A487,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B487)>0,'Translation-EN'!B487,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C487)>0,'Translation-EN'!C487,\"\")","v":"B12"},{"$f":"IF(LEN('Translation-EN'!D487)>0,'Translation-EN'!D487,\"\")","v":""},{"$f":"$E$299","v":"2x4 double"}]
[{"$f":"IF(LEN('Translation-EN'!A488)>0,'Translation-EN'!A488,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B488)>0,'Translation-EN'!B488,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C488)>0,'Translation-EN'!C488,\"\")","v":"A13"},{"$f":"IF(LEN('Translation-EN'!D488)>0,'Translation-EN'!D488,\"\")","v":""},{"$f":"$E$369","v":"MURS À CHARPENTE EN ACIER"}]
[{"$f":"IF(LEN('Translation-EN'!A489)>0,'Translation-EN'!A489,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B489)>0,'Translation-EN'!B489,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C489)>0,'Translation-EN'!C489,\"\")","v":"D13"},{"$f":"IF(LEN('Translation-EN'!D489)>0,'Translation-EN'!D489,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A490)>0,'Translation-EN'!A490,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B490)>0,'Translation-EN'!B490,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C490)>0,'Translation-EN'!C490,\"\")","v":"B14"},{"$f":"IF(LEN('Translation-EN'!D490)>0,'Translation-EN'!D490,\"\")","v":""},{"$f":"$E$302","v":"CHARPENTE D’ACIER, 2x4"}]
[{"$f":"IF(LEN('Translation-EN'!A491)>0,'Translation-EN'!A491,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B491)>0,'Translation-EN'!B491,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C491)>0,'Translation-EN'!C491,\"\")","v":"C15"},{"$f":"IF(LEN('Translation-EN'!D491)>0,'Translation-EN'!D491,\"\")","v":""},"Charpente en acier – murs intérieurs – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A492)>0,'Translation-EN'!A492,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B492)>0,'Translation-EN'!B492,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C492)>0,'Translation-EN'!C492,\"\")","v":"A16"},{"$f":"IF(LEN('Translation-EN'!D492)>0,'Translation-EN'!D492,\"\")","v":""},"Utilisez la fonction % pour vous adapter aux différents calibres des goujons en acier."]
[{"$f":"IF(LEN('Translation-EN'!A493)>0,'Translation-EN'!A493,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B493)>0,'Translation-EN'!B493,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C493)>0,'Translation-EN'!C493,\"\")","v":"B21"},{"$f":"IF(LEN('Translation-EN'!D493)>0,'Translation-EN'!D493,\"\")","v":""},{"$f":"$E$372","v":"CHARPENTE D’ACIER, 2x6"}]
[{"$f":"IF(LEN('Translation-EN'!A494)>0,'Translation-EN'!A494,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B494)>0,'Translation-EN'!B494,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C494)>0,'Translation-EN'!C494,\"\")","v":"A22"},{"$f":"IF(LEN('Translation-EN'!D494)>0,'Translation-EN'!D494,\"\")","v":""},"Utilisez la fonction % pour vous adapter aux autres calibres des goujons en acier."]
[{"$f":"IF(LEN('Translation-EN'!A495)>0,'Translation-EN'!A495,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B495)>0,'Translation-EN'!B495,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C495)>0,'Translation-EN'!C495,\"\")","v":"C22"},{"$f":"IF(LEN('Translation-EN'!D495)>0,'Translation-EN'!D495,\"\")","v":""},{"$f":"$E$374","v":"Charpente en acier – porteur – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A496)>0,'Translation-EN'!A496,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B496)>0,'Translation-EN'!B496,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C496)>0,'Translation-EN'!C496,\"\")","v":"A28"},{"$f":"IF(LEN('Translation-EN'!D496)>0,'Translation-EN'!D496,\"\")","v":""},"MURS MITOYENS EN ÉLÉMENTS DE MAÇONNERIE EN BÉTON"]
[{"$f":"IF(LEN('Translation-EN'!A497)>0,'Translation-EN'!A497,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B497)>0,'Translation-EN'!B497,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C497)>0,'Translation-EN'!C497,\"\")","v":"A29"},{"$f":"IF(LEN('Translation-EN'!D497)>0,'Translation-EN'!D497,\"\")","v":""},"MURS MITOYENS EN EMB"]
[{"$f":"IF(LEN('Translation-EN'!A498)>0,'Translation-EN'!A498,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B498)>0,'Translation-EN'!B498,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C498)>0,'Translation-EN'!C498,\"\")","v":"B30"},{"$f":"IF(LEN('Translation-EN'!D498)>0,'Translation-EN'!D498,\"\")","v":""},"EMB 8 po – CREUX, SANS COULIS"]
[{"$f":"IF(LEN('Translation-EN'!A499)>0,'Translation-EN'!A499,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B499)>0,'Translation-EN'!B499,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C499)>0,'Translation-EN'!C499,\"\")","v":"C31"},{"$f":"IF(LEN('Translation-EN'!D499)>0,'Translation-EN'!D499,\"\")","v":""},"Murs en éléments de maçonnerie en béton"]
[{"$f":"IF(LEN('Translation-EN'!A500)>0,'Translation-EN'!A500,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B500)>0,'Translation-EN'!B500,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C500)>0,'Translation-EN'!C500,\"\")","v":"A32"},{"$f":"IF(LEN('Translation-EN'!D500)>0,'Translation-EN'!D500,\"\")","v":""},"Utilisez la fonction % pour régler d’autres épaisseurs de EMB."]
[{"$f":"IF(LEN('Translation-EN'!A501)>0,'Translation-EN'!A501,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B501)>0,'Translation-EN'!B501,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C501)>0,'Translation-EN'!C501,\"\")","v":"A38"},{"$f":"IF(LEN('Translation-EN'!D501)>0,'Translation-EN'!D501,\"\")","v":""},"BÉTON DE REMPLISSAGE POUR MURS EN EMB"]
[{"$f":"IF(LEN('Translation-EN'!A502)>0,'Translation-EN'!A502,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B502)>0,'Translation-EN'!B502,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C502)>0,'Translation-EN'!C502,\"\")","v":"D38"},{"$f":"IF(LEN('Translation-EN'!D502)>0,'Translation-EN'!D502,\"\")","v":""},"VOLUME DE BÉTON DE REMPLISSAGE"]
[{"$f":"IF(LEN('Translation-EN'!A503)>0,'Translation-EN'!A503,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B503)>0,'Translation-EN'!B503,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C503)>0,'Translation-EN'!C503,\"\")","v":"B39"},{"$f":"IF(LEN('Translation-EN'!D503)>0,'Translation-EN'!D503,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A504)>0,'Translation-EN'!A504,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B504)>0,'Translation-EN'!B504,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C504)>0,'Translation-EN'!C504,\"\")","v":"A40"},{"$f":"IF(LEN('Translation-EN'!D504)>0,'Translation-EN'!D504,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A505)>0,'Translation-EN'!A505,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B505)>0,'Translation-EN'!B505,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C505)>0,'Translation-EN'!C505,\"\")","v":"B47"},{"$f":"IF(LEN('Translation-EN'!D505)>0,'Translation-EN'!D505,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A506)>0,'Translation-EN'!A506,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B506)>0,'Translation-EN'!B506,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C506)>0,'Translation-EN'!C506,\"\")","v":"A48"},{"$f":"IF(LEN('Translation-EN'!D506)>0,'Translation-EN'!D506,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A507)>0,'Translation-EN'!A507,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B507)>0,'Translation-EN'!B507,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C507)>0,'Translation-EN'!C507,\"\")","v":"A55"},{"$f":"IF(LEN('Translation-EN'!D507)>0,'Translation-EN'!D507,\"\")","v":""},"ISOLATION DE MUR MITOYEN"]
[{"$f":"IF(LEN('Translation-EN'!A508)>0,'Translation-EN'!A508,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B508)>0,'Translation-EN'!B508,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C508)>0,'Translation-EN'!C508,\"\")","v":"A56"},{"$f":"IF(LEN('Translation-EN'!D508)>0,'Translation-EN'!D508,\"\")","v":""},{"$f":"$E$305","v":"ISOLATION DE LA CAVITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A509)>0,'Translation-EN'!A509,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B509)>0,'Translation-EN'!B509,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C509)>0,'Translation-EN'!C509,\"\")","v":"B57"},{"$f":"IF(LEN('Translation-EN'!D509)>0,'Translation-EN'!D509,\"\")","v":""},{"$f":"$E$307","v":"NATTE DE FIBRE DE VERRE"}]
[{"$f":"IF(LEN('Translation-EN'!A510)>0,'Translation-EN'!A510,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B510)>0,'Translation-EN'!B510,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C510)>0,'Translation-EN'!C510,\"\")","v":"C58"},{"$f":"IF(LEN('Translation-EN'!D510)>0,'Translation-EN'!D510,\"\")","v":""},{"$f":"$E$400","v":"Natte en fibre de verre – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A511)>0,'Translation-EN'!A511,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B511)>0,'Translation-EN'!B511,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C511)>0,'Translation-EN'!C511,\"\")","v":"B62"},{"$f":"IF(LEN('Translation-EN'!D511)>0,'Translation-EN'!D511,\"\")","v":""},{"$f":"$E$401","v":"FIBRE DE VERRE SOUFFLÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A512)>0,'Translation-EN'!A512,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B512)>0,'Translation-EN'!B512,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C512)>0,'Translation-EN'!C512,\"\")","v":"C63"},{"$f":"IF(LEN('Translation-EN'!D512)>0,'Translation-EN'!D512,\"\")","v":""},{"$f":"$E$402","v":"Fibre de verre en vrac – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A513)>0,'Translation-EN'!A513,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B513)>0,'Translation-EN'!B513,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C513)>0,'Translation-EN'!C513,\"\")","v":"B68"},{"$f":"IF(LEN('Translation-EN'!D513)>0,'Translation-EN'!D513,\"\")","v":""},{"$f":"$E$311","v":"NATTE DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A514)>0,'Translation-EN'!A514,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B514)>0,'Translation-EN'!B514,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C514)>0,'Translation-EN'!C514,\"\")","v":"B76"},{"$f":"IF(LEN('Translation-EN'!D514)>0,'Translation-EN'!D514,\"\")","v":""},{"$f":"$E$309","v":"ISOLATION EN CELLULOSE"}]
[{"$f":"IF(LEN('Translation-EN'!A515)>0,'Translation-EN'!A515,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B515)>0,'Translation-EN'!B515,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C515)>0,'Translation-EN'!C515,\"\")","v":"C77"},{"$f":"IF(LEN('Translation-EN'!D515)>0,'Translation-EN'!D515,\"\")","v":""},{"$f":"$E$405","v":"Cellulose – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A516)>0,'Translation-EN'!A516,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B516)>0,'Translation-EN'!B516,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C516)>0,'Translation-EN'!C516,\"\")","v":"B81"},{"$f":"IF(LEN('Translation-EN'!D516)>0,'Translation-EN'!D516,\"\")","v":""},{"$f":"$E$313","v":"NATTE DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A517)>0,'Translation-EN'!A517,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B517)>0,'Translation-EN'!B517,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C517)>0,'Translation-EN'!C517,\"\")","v":"C82"},{"$f":"IF(LEN('Translation-EN'!D517)>0,'Translation-EN'!D517,\"\")","v":""},{"$f":"$E$407","v":"Natte de fibres de bois – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A518)>0,'Translation-EN'!A518,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B518)>0,'Translation-EN'!B518,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C518)>0,'Translation-EN'!C518,\"\")","v":"B87"},{"$f":"IF(LEN('Translation-EN'!D518)>0,'Translation-EN'!D518,\"\")","v":""},{"$f":"$E$408","v":"AUTRES ISOLANTS EN FIBRES NATURELLES"}]
[{"$f":"IF(LEN('Translation-EN'!A519)>0,'Translation-EN'!A519,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B519)>0,'Translation-EN'!B519,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C519)>0,'Translation-EN'!C519,\"\")","v":"B93"},{"$f":"IF(LEN('Translation-EN'!D519)>0,'Translation-EN'!D519,\"\")","v":""},{"$f":"$E$409","v":"MOUSSE À PULVÉRISER – CELLULE FERMÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A520)>0,'Translation-EN'!A520,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B520)>0,'Translation-EN'!B520,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C520)>0,'Translation-EN'!C520,\"\")","v":"B97"},{"$f":"IF(LEN('Translation-EN'!D520)>0,'Translation-EN'!D520,\"\")","v":""},{"$f":"$E$410","v":"MOUSSE À PULVÉRISER – CELLULE OUVERTE"}]
[{"$f":"IF(LEN('Translation-EN'!A521)>0,'Translation-EN'!A521,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B521)>0,'Translation-EN'!B521,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C521)>0,'Translation-EN'!C521,\"\")","v":"B100"},{"$f":"IF(LEN('Translation-EN'!D521)>0,'Translation-EN'!D521,\"\")","v":""},{"$f":"$E$411","v":"BRIQUES DE CHANVRE"}]
[{"$f":"IF(LEN('Translation-EN'!A522)>0,'Translation-EN'!A522,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B522)>0,'Translation-EN'!B522,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C522)>0,'Translation-EN'!C522,\"\")","v":"C101"},{"$f":"IF(LEN('Translation-EN'!D522)>0,'Translation-EN'!D522,\"\")","v":""},{"$f":"$E$412","v":"Briques de chanvre – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A523)>0,'Translation-EN'!A523,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B523)>0,'Translation-EN'!B523,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C523)>0,'Translation-EN'!C523,\"\")","v":"A105"},{"$f":"IF(LEN('Translation-EN'!D523)>0,'Translation-EN'!D523,\"\")","v":""},"ISOLATION RIGIDE"]
[{"$f":"IF(LEN('Translation-EN'!A524)>0,'Translation-EN'!A524,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B524)>0,'Translation-EN'!B524,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C524)>0,'Translation-EN'!C524,\"\")","v":"B106"},{"$f":"IF(LEN('Translation-EN'!D524)>0,'Translation-EN'!D524,\"\")","v":""},{"$f":"$E$211","v":"PANNEAU DE MOUSSE EPS"}]
[{"$f":"IF(LEN('Translation-EN'!A525)>0,'Translation-EN'!A525,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B525)>0,'Translation-EN'!B525,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C525)>0,'Translation-EN'!C525,\"\")","v":"C107"},{"$f":"IF(LEN('Translation-EN'!D525)>0,'Translation-EN'!D525,\"\")","v":""},{"$f":"$E$212","v":"Panneau de mousse EPS – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A526)>0,'Translation-EN'!A526,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B526)>0,'Translation-EN'!B526,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C526)>0,'Translation-EN'!C526,\"\")","v":"B110"},{"$f":"IF(LEN('Translation-EN'!D526)>0,'Translation-EN'!D526,\"\")","v":""},{"$f":"$E$270","v":"PANNEAU DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A527)>0,'Translation-EN'!A527,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B527)>0,'Translation-EN'!B527,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C527)>0,'Translation-EN'!C527,\"\")","v":"C111"},{"$f":"IF(LEN('Translation-EN'!D527)>0,'Translation-EN'!D527,\"\")","v":""},{"$f":"$E$271","v":"Panneau de fibres de bois – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A528)>0,'Translation-EN'!A528,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B528)>0,'Translation-EN'!B528,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C528)>0,'Translation-EN'!C528,\"\")","v":"B117"},{"$f":"IF(LEN('Translation-EN'!D528)>0,'Translation-EN'!D528,\"\")","v":""},{"$f":"$E$213","v":"PANNEAU DE MOUSSE XPS"}]
[{"$f":"IF(LEN('Translation-EN'!A529)>0,'Translation-EN'!A529,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B529)>0,'Translation-EN'!B529,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C529)>0,'Translation-EN'!C529,\"\")","v":"C118"},{"$f":"IF(LEN('Translation-EN'!D529)>0,'Translation-EN'!D529,\"\")","v":""},{"$f":"$E$214","v":"Panneau de mousse XPS – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A530)>0,'Translation-EN'!A530,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B530)>0,'Translation-EN'!B530,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C530)>0,'Translation-EN'!C530,\"\")","v":"B123"},{"$f":"IF(LEN('Translation-EN'!D530)>0,'Translation-EN'!D530,\"\")","v":""},{"$f":"$E$420","v":"PANNEAU DE MOUSSE POLYISOCYANURATE"}]
[{"$f":"IF(LEN('Translation-EN'!A531)>0,'Translation-EN'!A531,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B531)>0,'Translation-EN'!B531,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C531)>0,'Translation-EN'!C531,\"\")","v":"C124"},{"$f":"IF(LEN('Translation-EN'!D531)>0,'Translation-EN'!D531,\"\")","v":""},{"$f":"$E$421","v":"Polyisocyanurate – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A532)>0,'Translation-EN'!A532,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B532)>0,'Translation-EN'!B532,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C532)>0,'Translation-EN'!C532,\"\")","v":"B129"},{"$f":"IF(LEN('Translation-EN'!D532)>0,'Translation-EN'!D532,\"\")","v":""},{"$f":"$E$215","v":"PANNEAU DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A533)>0,'Translation-EN'!A533,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B533)>0,'Translation-EN'!B533,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C533)>0,'Translation-EN'!C533,\"\")","v":"C130"},{"$f":"IF(LEN('Translation-EN'!D533)>0,'Translation-EN'!D533,\"\")","v":""},{"$f":"$E$423","v":"Panneau de laine minérale – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A534)>0,'Translation-EN'!A534,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B534)>0,'Translation-EN'!B534,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C534)>0,'Translation-EN'!C534,\"\")","v":"A134"},{"$f":"IF(LEN('Translation-EN'!D534)>0,'Translation-EN'!D534,\"\")","v":""},"REVÊTEMENT DE MUR MITOYEN"]
[{"$f":"IF(LEN('Translation-EN'!A535)>0,'Translation-EN'!A535,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B535)>0,'Translation-EN'!B535,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C535)>0,'Translation-EN'!C535,\"\")","v":"A135"},{"$f":"IF(LEN('Translation-EN'!D535)>0,'Translation-EN'!D535,\"\")","v":""},"REVÊTEMENT INTÉRIEUR pour les MURS MITOYENS"]
[{"$f":"IF(LEN('Translation-EN'!A536)>0,'Translation-EN'!A536,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B536)>0,'Translation-EN'!B536,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C536)>0,'Translation-EN'!C536,\"\")","v":"B136"},{"$f":"IF(LEN('Translation-EN'!D536)>0,'Translation-EN'!D536,\"\")","v":""},{"$f":"$E$320","v":"CLOISONS SÈCHES 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A537)>0,'Translation-EN'!A537,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B537)>0,'Translation-EN'!B537,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C537)>0,'Translation-EN'!C537,\"\")","v":"C137"},{"$f":"IF(LEN('Translation-EN'!D537)>0,'Translation-EN'!D537,\"\")","v":""},"Cloison sèche 1/2 po typique – Revêtement intérieur pour murs extérieurs - MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A538)>0,'Translation-EN'!A538,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B538)>0,'Translation-EN'!B538,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C538)>0,'Translation-EN'!C538,\"\")","v":"B143"},{"$f":"IF(LEN('Translation-EN'!D538)>0,'Translation-EN'!D538,\"\")","v":""},{"$f":"$E$322","v":"CLOISONS SÈCHES 5/8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A539)>0,'Translation-EN'!A539,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B539)>0,'Translation-EN'!B539,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C539)>0,'Translation-EN'!C539,\"\")","v":"B147"},{"$f":"IF(LEN('Translation-EN'!D539)>0,'Translation-EN'!D539,\"\")","v":""},{"$f":"$E$323","v":"AUTRES MATÉRIAUX DE BARDAGE"}]
[{"$f":"IF(LEN('Translation-EN'!A540)>0,'Translation-EN'!A540,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B540)>0,'Translation-EN'!B540,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C540)>0,'Translation-EN'!C540,\"\")","v":"A158"},{"$f":"IF(LEN('Translation-EN'!D540)>0,'Translation-EN'!D540,\"\")","v":""},{"$f":"$E$393","v":"PANNEAUX STRUCTURAUX"}]
[{"$f":"IF(LEN('Translation-EN'!A541)>0,'Translation-EN'!A541,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B541)>0,'Translation-EN'!B541,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C541)>0,'Translation-EN'!C541,\"\")","v":"B159"},{"$f":"IF(LEN('Translation-EN'!D541)>0,'Translation-EN'!D541,\"\")","v":""},{"$f":"$E$394","v":"PANNEAU À COPEAUX ORIENTÉS"}]
[{"$f":"IF(LEN('Translation-EN'!A542)>0,'Translation-EN'!A542,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B542)>0,'Translation-EN'!B542,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C542)>0,'Translation-EN'!C542,\"\")","v":"B164"},{"$f":"IF(LEN('Translation-EN'!D542)>0,'Translation-EN'!D542,\"\")","v":""},{"$f":"$E$395","v":"CONTREPLAQUÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A543)>0,'Translation-EN'!A543,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B543)>0,'Translation-EN'!B543,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C543)>0,'Translation-EN'!C543,\"\")","v":"B168"},{"$f":"IF(LEN('Translation-EN'!D543)>0,'Translation-EN'!D543,\"\")","v":""},{"$f":"$E$396","v":"PANNEAUX STRUCTURAUX EN GYPSE"}]
[{"$f":"IF(LEN('Translation-EN'!A544)>0,'Translation-EN'!A544,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B544)>0,'Translation-EN'!B544,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C544)>0,'Translation-EN'!C544,\"\")","v":"B172"},{"$f":"IF(LEN('Translation-EN'!D544)>0,'Translation-EN'!D544,\"\")","v":""},{"$f":"$E$397","v":"PANNEAU DE CIMENT"}]
[{"$f":"IF(LEN('Translation-EN'!A545)>0,'Translation-EN'!A545,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B545)>0,'Translation-EN'!B545,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C545)>0,'Translation-EN'!C545,\"\")","v":"A175"},{"$f":"IF(LEN('Translation-EN'!D545)>0,'Translation-EN'!D545,\"\")","v":""},"CIB DE MUR MITOYEN"]
[{"$f":"IF(LEN('Translation-EN'!A546)>0,'Translation-EN'!A546,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B546)>0,'Translation-EN'!B546,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C546)>0,'Translation-EN'!C546,\"\")","v":"A176"},{"$f":"IF(LEN('Translation-EN'!D546)>0,'Translation-EN'!D546,\"\")","v":""},{"$f":"$E$274","v":"COFFRAGES ISOLÉS EN BÉTON (CIB) – MOUSSE EPS"}]
[{"$f":"IF(LEN('Translation-EN'!A547)>0,'Translation-EN'!A547,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B547)>0,'Translation-EN'!B547,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C547)>0,'Translation-EN'!C547,\"\")","v":"A177"},{"$f":"IF(LEN('Translation-EN'!D547)>0,'Translation-EN'!D547,\"\")","v":""},{"$f":"$E$275","v":"Étape 1 : Sélectionnez la taille du CIB"}]
[{"$f":"IF(LEN('Translation-EN'!A548)>0,'Translation-EN'!A548,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B548)>0,'Translation-EN'!B548,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C548)>0,'Translation-EN'!C548,\"\")","v":"B178"},{"$f":"IF(LEN('Translation-EN'!D548)>0,'Translation-EN'!D548,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A549)>0,'Translation-EN'!A549,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B549)>0,'Translation-EN'!B549,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C549)>0,'Translation-EN'!C549,\"\")","v":"A179"},{"$f":"IF(LEN('Translation-EN'!D549)>0,'Translation-EN'!D549,\"\")","v":""},{"$f":"$E$277","v":"Étape 2 : Sélectionnez l’option de remplissage en béton."}]
[{"$f":"IF(LEN('Translation-EN'!A550)>0,'Translation-EN'!A550,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B550)>0,'Translation-EN'!B550,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C550)>0,'Translation-EN'!C550,\"\")","v":"B186"},{"$f":"IF(LEN('Translation-EN'!D550)>0,'Translation-EN'!D550,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A551)>0,'Translation-EN'!A551,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B551)>0,'Translation-EN'!B551,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C551)>0,'Translation-EN'!C551,\"\")","v":"A187"},{"$f":"IF(LEN('Translation-EN'!D551)>0,'Translation-EN'!D551,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A552)>0,'Translation-EN'!A552,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B552)>0,'Translation-EN'!B552,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C552)>0,'Translation-EN'!C552,\"\")","v":"B194"},{"$f":"IF(LEN('Translation-EN'!D552)>0,'Translation-EN'!D552,\"\")","v":""},{"$f":"$E$187","v":"BÉTON –31-35 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A553)>0,'Translation-EN'!A553,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B553)>0,'Translation-EN'!B553,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C553)>0,'Translation-EN'!C553,\"\")","v":"A195"},{"$f":"IF(LEN('Translation-EN'!D553)>0,'Translation-EN'!D553,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A554)>0,'Translation-EN'!A554,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B554)>0,'Translation-EN'!B554,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C554)>0,'Translation-EN'!C554,\"\")","v":"A202"},{"$f":"IF(LEN('Translation-EN'!D554)>0,'Translation-EN'!D554,\"\")","v":""},{"$f":"$E$282","v":"COFFRAGES ISOLÉS EN BÉTON (CIB) – COPEAUX DE BOIS/CIMENT"}]
[{"$f":"IF(LEN('Translation-EN'!A555)>0,'Translation-EN'!A555,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B555)>0,'Translation-EN'!B555,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C555)>0,'Translation-EN'!C555,\"\")","v":"A203"},{"$f":"IF(LEN('Translation-EN'!D555)>0,'Translation-EN'!D555,\"\")","v":""},{"$f":"$E$450","v":"Étape 1 : Choisir la taille et l’isolation des CIB"}]
[{"$f":"IF(LEN('Translation-EN'!A556)>0,'Translation-EN'!A556,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B556)>0,'Translation-EN'!B556,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C556)>0,'Translation-EN'!C556,\"\")","v":"B207"},{"$f":"IF(LEN('Translation-EN'!D556)>0,'Translation-EN'!D556,\"\")","v":""},{"$f":"$E$451","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A557)>0,'Translation-EN'!A557,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B557)>0,'Translation-EN'!B557,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C557)>0,'Translation-EN'!C557,\"\")","v":"A208"},{"$f":"IF(LEN('Translation-EN'!D557)>0,'Translation-EN'!D557,\"\")","v":true},{"$f":"$E$452","v":"Étape 2 : Sélectionnez l'option de remplissage en béton pour le système de mur en CIB. La quantité de béton s'adapte à la taille du CIB choisi."}]
[{"$f":"IF(LEN('Translation-EN'!A558)>0,'Translation-EN'!A558,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B558)>0,'Translation-EN'!B558,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C558)>0,'Translation-EN'!C558,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D558)>0,'Translation-EN'!D558,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A559)>0,'Translation-EN'!A559,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B559)>0,'Translation-EN'!B559,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C559)>0,'Translation-EN'!C559,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D559)>0,'Translation-EN'!D559,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A560)>0,'Translation-EN'!A560,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B560)>0,'Translation-EN'!B560,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C560)>0,'Translation-EN'!C560,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D560)>0,'Translation-EN'!D560,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A561)>0,'Translation-EN'!A561,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B561)>0,'Translation-EN'!B561,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C561)>0,'Translation-EN'!C561,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D561)>0,'Translation-EN'!D561,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A562)>0,'Translation-EN'!A562,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B562)>0,'Translation-EN'!B562,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C562)>0,'Translation-EN'!C562,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D562)>0,'Translation-EN'!D562,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A563)>0,'Translation-EN'!A563,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B563)>0,'Translation-EN'!B563,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C563)>0,'Translation-EN'!C563,\"\")","v":"B215"},{"$f":"IF(LEN('Translation-EN'!D563)>0,'Translation-EN'!D563,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A564)>0,'Translation-EN'!A564,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B564)>0,'Translation-EN'!B564,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C564)>0,'Translation-EN'!C564,\"\")","v":"A216"},{"$f":"IF(LEN('Translation-EN'!D564)>0,'Translation-EN'!D564,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A565)>0,'Translation-EN'!A565,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B565)>0,'Translation-EN'!B565,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C565)>0,'Translation-EN'!C565,\"\")","v":"B223"},{"$f":"IF(LEN('Translation-EN'!D565)>0,'Translation-EN'!D565,\"\")","v":""},{"$f":"$E$187","v":"BÉTON –31-35 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A566)>0,'Translation-EN'!A566,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B566)>0,'Translation-EN'!B566,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C566)>0,'Translation-EN'!C566,\"\")","v":"A224"},{"$f":"IF(LEN('Translation-EN'!D566)>0,'Translation-EN'!D566,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A567)>0,'Translation-EN'!A567,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B567)>0,'Translation-EN'!B567,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C567)>0,'Translation-EN'!C567,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D567)>0,'Translation-EN'!D567,\"\")","v":""},"SECTION 7 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A568)>0,'Translation-EN'!A568,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B568)>0,'Translation-EN'!B568,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C568)>0,'Translation-EN'!C568,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D568)>0,'Translation-EN'!D568,\"\")","v":""},"MURS EXTÉRIEURS – BARDAGE"]
[{"$f":"IF(LEN('Translation-EN'!A569)>0,'Translation-EN'!A569,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B569)>0,'Translation-EN'!B569,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C569)>0,'Translation-EN'!C569,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D569)>0,'Translation-EN'!D569,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A570)>0,'Translation-EN'!A570,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B570)>0,'Translation-EN'!B570,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C570)>0,'Translation-EN'!C570,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D570)>0,'Translation-EN'!D570,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A571)>0,'Translation-EN'!A571,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B571)>0,'Translation-EN'!B571,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C571)>0,'Translation-EN'!C571,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D571)>0,'Translation-EN'!D571,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A572)>0,'Translation-EN'!A572,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B572)>0,'Translation-EN'!B572,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C572)>0,'Translation-EN'!C572,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D572)>0,'Translation-EN'!D572,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A573)>0,'Translation-EN'!A573,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B573)>0,'Translation-EN'!B573,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C573)>0,'Translation-EN'!C573,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D573)>0,'Translation-EN'!D573,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A574)>0,'Translation-EN'!A574,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B574)>0,'Translation-EN'!B574,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C574)>0,'Translation-EN'!C574,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D574)>0,'Translation-EN'!D574,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A575)>0,'Translation-EN'!A575,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B575)>0,'Translation-EN'!B575,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C575)>0,'Translation-EN'!C575,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D575)>0,'Translation-EN'!D575,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A576)>0,'Translation-EN'!A576,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B576)>0,'Translation-EN'!B576,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C576)>0,'Translation-EN'!C576,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D576)>0,'Translation-EN'!D576,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A577)>0,'Translation-EN'!A577,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B577)>0,'Translation-EN'!B577,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C577)>0,'Translation-EN'!C577,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D577)>0,'Translation-EN'!D577,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A578)>0,'Translation-EN'!A578,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B578)>0,'Translation-EN'!B578,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C578)>0,'Translation-EN'!C578,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D578)>0,'Translation-EN'!D578,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A579)>0,'Translation-EN'!A579,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B579)>0,'Translation-EN'!B579,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C579)>0,'Translation-EN'!C579,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D579)>0,'Translation-EN'!D579,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A580)>0,'Translation-EN'!A580,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B580)>0,'Translation-EN'!B580,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C580)>0,'Translation-EN'!C580,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D580)>0,'Translation-EN'!D580,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A581)>0,'Translation-EN'!A581,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B581)>0,'Translation-EN'!B581,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C581)>0,'Translation-EN'!C581,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D581)>0,'Translation-EN'!D581,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A582)>0,'Translation-EN'!A582,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B582)>0,'Translation-EN'!B582,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C582)>0,'Translation-EN'!C582,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D582)>0,'Translation-EN'!D582,\"\")","v":true},"TOTAL PARTIEL POUR LE BARDAGE DES MURS EXTÉRIEURS kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A583)>0,'Translation-EN'!A583,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B583)>0,'Translation-EN'!B583,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C583)>0,'Translation-EN'!C583,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D583)>0,'Translation-EN'!D583,\"\")","v":""},"BARDAGE EXTÉRIEUR"]
[{"$f":"IF(LEN('Translation-EN'!A584)>0,'Translation-EN'!A584,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B584)>0,'Translation-EN'!B584,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C584)>0,'Translation-EN'!C584,\"\")","v":"B6"},{"$f":"IF(LEN('Translation-EN'!D584)>0,'Translation-EN'!D584,\"\")","v":""},"BRIQUE"]
[{"$f":"IF(LEN('Translation-EN'!A585)>0,'Translation-EN'!A585,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B585)>0,'Translation-EN'!B585,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C585)>0,'Translation-EN'!C585,\"\")","v":"B14"},{"$f":"IF(LEN('Translation-EN'!D585)>0,'Translation-EN'!D585,\"\")","v":""},"BARDAGE EN BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A586)>0,'Translation-EN'!A586,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B586)>0,'Translation-EN'!B586,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C586)>0,'Translation-EN'!C586,\"\")","v":"B17"},{"$f":"IF(LEN('Translation-EN'!D586)>0,'Translation-EN'!D586,\"\")","v":""},"FIBROCIMENT"]
[{"$f":"IF(LEN('Translation-EN'!A587)>0,'Translation-EN'!A587,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B587)>0,'Translation-EN'!B587,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C587)>0,'Translation-EN'!C587,\"\")","v":"C18"},{"$f":"IF(LEN('Translation-EN'!D587)>0,'Translation-EN'!D587,\"\")","v":""},"Bardage en fibrociment – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A588)>0,'Translation-EN'!A588,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B588)>0,'Translation-EN'!B588,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C588)>0,'Translation-EN'!C588,\"\")","v":"B27"},{"$f":"IF(LEN('Translation-EN'!D588)>0,'Translation-EN'!D588,\"\")","v":""},"REVÊTEMENT EN VINYLE"]
[{"$f":"IF(LEN('Translation-EN'!A589)>0,'Translation-EN'!A589,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B589)>0,'Translation-EN'!B589,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C589)>0,'Translation-EN'!C589,\"\")","v":"B29"},{"$f":"IF(LEN('Translation-EN'!D589)>0,'Translation-EN'!D589,\"\")","v":""},"REVÊTEMENT EN POLYPROPYLÈNE"]
[{"$f":"IF(LEN('Translation-EN'!A590)>0,'Translation-EN'!A590,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B590)>0,'Translation-EN'!B590,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C590)>0,'Translation-EN'!C590,\"\")","v":"C30"},{"$f":"IF(LEN('Translation-EN'!D590)>0,'Translation-EN'!D590,\"\")","v":""},"Revêtement en polypropylène – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A591)>0,'Translation-EN'!A591,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B591)>0,'Translation-EN'!B591,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C591)>0,'Translation-EN'!C591,\"\")","v":"B33"},{"$f":"IF(LEN('Translation-EN'!D591)>0,'Translation-EN'!D591,\"\")","v":""},"BARDAGE EN PANNEAUX D’ACIER"]
[{"$f":"IF(LEN('Translation-EN'!A592)>0,'Translation-EN'!A592,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B592)>0,'Translation-EN'!B592,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C592)>0,'Translation-EN'!C592,\"\")","v":"C34"},{"$f":"IF(LEN('Translation-EN'!D592)>0,'Translation-EN'!D592,\"\")","v":""},"Bardage en panneaux d’acier – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A593)>0,'Translation-EN'!A593,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B593)>0,'Translation-EN'!B593,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C593)>0,'Translation-EN'!C593,\"\")","v":"B41"},{"$f":"IF(LEN('Translation-EN'!D593)>0,'Translation-EN'!D593,\"\")","v":""},"BARDAGE EN PANNEAUX D’ALUMINIUM"]
[{"$f":"IF(LEN('Translation-EN'!A594)>0,'Translation-EN'!A594,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B594)>0,'Translation-EN'!B594,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C594)>0,'Translation-EN'!C594,\"\")","v":"C42"},{"$f":"IF(LEN('Translation-EN'!D594)>0,'Translation-EN'!D594,\"\")","v":""},"Bardage en panneaux d’aluminium – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A595)>0,'Translation-EN'!A595,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B595)>0,'Translation-EN'!B595,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C595)>0,'Translation-EN'!C595,\"\")","v":"B45"},{"$f":"IF(LEN('Translation-EN'!D595)>0,'Translation-EN'!D595,\"\")","v":""},"FINITIONS EN PLÂTRE"]
[{"$f":"IF(LEN('Translation-EN'!A596)>0,'Translation-EN'!A596,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B596)>0,'Translation-EN'!B596,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C596)>0,'Translation-EN'!C596,\"\")","v":"B50"},{"$f":"IF(LEN('Translation-EN'!D596)>0,'Translation-EN'!D596,\"\")","v":""},"BARDAGE EN BOIS D'INGÉNIERIE"]
[{"$f":"IF(LEN('Translation-EN'!A597)>0,'Translation-EN'!A597,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B597)>0,'Translation-EN'!B597,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C597)>0,'Translation-EN'!C597,\"\")","v":"A54"},{"$f":"IF(LEN('Translation-EN'!D597)>0,'Translation-EN'!D597,\"\")","v":""},"Tasseau pour écran de pluie"]
[{"$f":"IF(LEN('Translation-EN'!A598)>0,'Translation-EN'!A598,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B598)>0,'Translation-EN'!B598,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C598)>0,'Translation-EN'!C598,\"\")","v":"D54"},{"$f":"IF(LEN('Translation-EN'!D598)>0,'Translation-EN'!D598,\"\")","v":""},"ESPACEMENT DES TASSEAUX"]
[{"$f":"IF(LEN('Translation-EN'!A599)>0,'Translation-EN'!A599,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B599)>0,'Translation-EN'!B599,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C599)>0,'Translation-EN'!C599,\"\")","v":"A57"},{"$f":"IF(LEN('Translation-EN'!D599)>0,'Translation-EN'!D599,\"\")","v":""},"REVÊTEMENT INTÉRIEUR pour les MURS EXTÉRIEURS"]
[{"$f":"IF(LEN('Translation-EN'!A600)>0,'Translation-EN'!A600,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B600)>0,'Translation-EN'!B600,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C600)>0,'Translation-EN'!C600,\"\")","v":"B58"},{"$f":"IF(LEN('Translation-EN'!D600)>0,'Translation-EN'!D600,\"\")","v":""},{"$f":"$E$320","v":"CLOISONS SÈCHES 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A601)>0,'Translation-EN'!A601,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B601)>0,'Translation-EN'!B601,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C601)>0,'Translation-EN'!C601,\"\")","v":"C59"},{"$f":"IF(LEN('Translation-EN'!D601)>0,'Translation-EN'!D601,\"\")","v":""},{"$f":"$E$537","v":"Cloison sèche 1/2 po typique – Revêtement intérieur pour murs extérieurs - MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A602)>0,'Translation-EN'!A602,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B602)>0,'Translation-EN'!B602,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C602)>0,'Translation-EN'!C602,\"\")","v":"B65"},{"$f":"IF(LEN('Translation-EN'!D602)>0,'Translation-EN'!D602,\"\")","v":""},{"$f":"$E$322","v":"CLOISONS SÈCHES 5/8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A603)>0,'Translation-EN'!A603,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B603)>0,'Translation-EN'!B603,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C603)>0,'Translation-EN'!C603,\"\")","v":"B69"},{"$f":"IF(LEN('Translation-EN'!D603)>0,'Translation-EN'!D603,\"\")","v":""},{"$f":"$E$323","v":"AUTRES MATÉRIAUX DE BARDAGE"}]
[{"$f":"IF(LEN('Translation-EN'!A604)>0,'Translation-EN'!A604,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B604)>0,'Translation-EN'!B604,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C604)>0,'Translation-EN'!C604,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D604)>0,'Translation-EN'!D604,\"\")","v":""},"SECTION 8 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A605)>0,'Translation-EN'!A605,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B605)>0,'Translation-EN'!B605,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C605)>0,'Translation-EN'!C605,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D605)>0,'Translation-EN'!D605,\"\")","v":""},"FENÊTRES"]
[{"$f":"IF(LEN('Translation-EN'!A606)>0,'Translation-EN'!A606,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B606)>0,'Translation-EN'!B606,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C606)>0,'Translation-EN'!C606,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D606)>0,'Translation-EN'!D606,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A607)>0,'Translation-EN'!A607,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B607)>0,'Translation-EN'!B607,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C607)>0,'Translation-EN'!C607,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D607)>0,'Translation-EN'!D607,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A608)>0,'Translation-EN'!A608,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B608)>0,'Translation-EN'!B608,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C608)>0,'Translation-EN'!C608,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D608)>0,'Translation-EN'!D608,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A609)>0,'Translation-EN'!A609,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B609)>0,'Translation-EN'!B609,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C609)>0,'Translation-EN'!C609,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D609)>0,'Translation-EN'!D609,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A610)>0,'Translation-EN'!A610,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B610)>0,'Translation-EN'!B610,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C610)>0,'Translation-EN'!C610,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D610)>0,'Translation-EN'!D610,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A611)>0,'Translation-EN'!A611,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B611)>0,'Translation-EN'!B611,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C611)>0,'Translation-EN'!C611,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D611)>0,'Translation-EN'!D611,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A612)>0,'Translation-EN'!A612,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B612)>0,'Translation-EN'!B612,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C612)>0,'Translation-EN'!C612,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D612)>0,'Translation-EN'!D612,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A613)>0,'Translation-EN'!A613,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B613)>0,'Translation-EN'!B613,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C613)>0,'Translation-EN'!C613,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D613)>0,'Translation-EN'!D613,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A614)>0,'Translation-EN'!A614,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B614)>0,'Translation-EN'!B614,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C614)>0,'Translation-EN'!C614,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D614)>0,'Translation-EN'!D614,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A615)>0,'Translation-EN'!A615,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B615)>0,'Translation-EN'!B615,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C615)>0,'Translation-EN'!C615,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D615)>0,'Translation-EN'!D615,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A616)>0,'Translation-EN'!A616,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B616)>0,'Translation-EN'!B616,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C616)>0,'Translation-EN'!C616,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D616)>0,'Translation-EN'!D616,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A617)>0,'Translation-EN'!A617,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B617)>0,'Translation-EN'!B617,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C617)>0,'Translation-EN'!C617,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D617)>0,'Translation-EN'!D617,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A618)>0,'Translation-EN'!A618,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B618)>0,'Translation-EN'!B618,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C618)>0,'Translation-EN'!C618,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D618)>0,'Translation-EN'!D618,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A619)>0,'Translation-EN'!A619,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B619)>0,'Translation-EN'!B619,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C619)>0,'Translation-EN'!C619,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D619)>0,'Translation-EN'!D619,\"\")","v":true},"TOTAL PARTIEL POUR LES FENÊTRES kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A620)>0,'Translation-EN'!A620,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B620)>0,'Translation-EN'!B620,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C620)>0,'Translation-EN'!C620,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D620)>0,'Translation-EN'!D620,\"\")","v":""},"FENÊTRES À DOUBLE VITRAGE"]
[{"$f":"IF(LEN('Translation-EN'!A621)>0,'Translation-EN'!A621,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B621)>0,'Translation-EN'!B621,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C621)>0,'Translation-EN'!C621,\"\")","v":"A12"},{"$f":"IF(LEN('Translation-EN'!D621)>0,'Translation-EN'!D621,\"\")","v":""},"FENÊTRES À TRIPLE VITRAGE"]
[{"$f":"IF(LEN('Translation-EN'!A622)>0,'Translation-EN'!A622,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B622)>0,'Translation-EN'!B622,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C622)>0,'Translation-EN'!C622,\"\")","v":"A19"},{"$f":"IF(LEN('Translation-EN'!D622)>0,'Translation-EN'!D622,\"\")","v":""},"FENÊTRES – FABRICANTS SPÉCIFIQUES"]
[{"$f":"IF(LEN('Translation-EN'!A623)>0,'Translation-EN'!A623,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B623)>0,'Translation-EN'!B623,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C623)>0,'Translation-EN'!C623,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D623)>0,'Translation-EN'!D623,\"\")","v":""},"SECTION 9 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A624)>0,'Translation-EN'!A624,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B624)>0,'Translation-EN'!B624,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C624)>0,'Translation-EN'!C624,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D624)>0,'Translation-EN'!D624,\"\")","v":""},"MURS INTÉRIEURS"]
[{"$f":"IF(LEN('Translation-EN'!A625)>0,'Translation-EN'!A625,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B625)>0,'Translation-EN'!B625,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C625)>0,'Translation-EN'!C625,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D625)>0,'Translation-EN'!D625,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A626)>0,'Translation-EN'!A626,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B626)>0,'Translation-EN'!B626,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C626)>0,'Translation-EN'!C626,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D626)>0,'Translation-EN'!D626,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A627)>0,'Translation-EN'!A627,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B627)>0,'Translation-EN'!B627,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C627)>0,'Translation-EN'!C627,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D627)>0,'Translation-EN'!D627,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A628)>0,'Translation-EN'!A628,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B628)>0,'Translation-EN'!B628,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C628)>0,'Translation-EN'!C628,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D628)>0,'Translation-EN'!D628,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A629)>0,'Translation-EN'!A629,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B629)>0,'Translation-EN'!B629,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C629)>0,'Translation-EN'!C629,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D629)>0,'Translation-EN'!D629,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A630)>0,'Translation-EN'!A630,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B630)>0,'Translation-EN'!B630,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C630)>0,'Translation-EN'!C630,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D630)>0,'Translation-EN'!D630,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A631)>0,'Translation-EN'!A631,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B631)>0,'Translation-EN'!B631,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C631)>0,'Translation-EN'!C631,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D631)>0,'Translation-EN'!D631,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A632)>0,'Translation-EN'!A632,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B632)>0,'Translation-EN'!B632,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C632)>0,'Translation-EN'!C632,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D632)>0,'Translation-EN'!D632,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A633)>0,'Translation-EN'!A633,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B633)>0,'Translation-EN'!B633,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C633)>0,'Translation-EN'!C633,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D633)>0,'Translation-EN'!D633,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A634)>0,'Translation-EN'!A634,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B634)>0,'Translation-EN'!B634,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C634)>0,'Translation-EN'!C634,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D634)>0,'Translation-EN'!D634,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A635)>0,'Translation-EN'!A635,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B635)>0,'Translation-EN'!B635,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C635)>0,'Translation-EN'!C635,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D635)>0,'Translation-EN'!D635,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A636)>0,'Translation-EN'!A636,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B636)>0,'Translation-EN'!B636,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C636)>0,'Translation-EN'!C636,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D636)>0,'Translation-EN'!D636,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A637)>0,'Translation-EN'!A637,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B637)>0,'Translation-EN'!B637,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C637)>0,'Translation-EN'!C637,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D637)>0,'Translation-EN'!D637,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A638)>0,'Translation-EN'!A638,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B638)>0,'Translation-EN'!B638,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C638)>0,'Translation-EN'!C638,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D638)>0,'Translation-EN'!D638,\"\")","v":true},"TOTAL PARTIEL POUR LES MURS INTÉRIEURS kgCO2e "]
[{"$f":"IF(LEN('Translation-EN'!A639)>0,'Translation-EN'!A639,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B639)>0,'Translation-EN'!B639,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C639)>0,'Translation-EN'!C639,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D639)>0,'Translation-EN'!D639,\"\")","v":""},{"$f":"$E$298","v":"CONSTRUCTION EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A640)>0,'Translation-EN'!A640,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B640)>0,'Translation-EN'!B640,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C640)>0,'Translation-EN'!C640,\"\")","v":"D5"},{"$f":"IF(LEN('Translation-EN'!D640)>0,'Translation-EN'!D640,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A641)>0,'Translation-EN'!A641,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B641)>0,'Translation-EN'!B641,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C641)>0,'Translation-EN'!C641,\"\")","v":"B6"},{"$f":"IF(LEN('Translation-EN'!D641)>0,'Translation-EN'!D641,\"\")","v":""},{"$f":"$E$298","v":"CONSTRUCTION EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A642)>0,'Translation-EN'!A642,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B642)>0,'Translation-EN'!B642,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C642)>0,'Translation-EN'!C642,\"\")","v":"A10"},{"$f":"IF(LEN('Translation-EN'!D642)>0,'Translation-EN'!D642,\"\")","v":""},"CONSTRUCTION À CHARPENTE EN ACIER"]
[{"$f":"IF(LEN('Translation-EN'!A643)>0,'Translation-EN'!A643,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B643)>0,'Translation-EN'!B643,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C643)>0,'Translation-EN'!C643,\"\")","v":"D10"},{"$f":"IF(LEN('Translation-EN'!D643)>0,'Translation-EN'!D643,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A644)>0,'Translation-EN'!A644,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B644)>0,'Translation-EN'!B644,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C644)>0,'Translation-EN'!C644,\"\")","v":"B11"},{"$f":"IF(LEN('Translation-EN'!D644)>0,'Translation-EN'!D644,\"\")","v":""},{"$f":"$E$302","v":"CHARPENTE D’ACIER, 2x4"}]
[{"$f":"IF(LEN('Translation-EN'!A645)>0,'Translation-EN'!A645,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B645)>0,'Translation-EN'!B645,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C645)>0,'Translation-EN'!C645,\"\")","v":"C12"},{"$f":"IF(LEN('Translation-EN'!D645)>0,'Translation-EN'!D645,\"\")","v":""},{"$f":"$E$491","v":"Charpente en acier – murs intérieurs – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A646)>0,'Translation-EN'!A646,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B646)>0,'Translation-EN'!B646,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C646)>0,'Translation-EN'!C646,\"\")","v":"A13"},{"$f":"IF(LEN('Translation-EN'!D646)>0,'Translation-EN'!D646,\"\")","v":""},{"$f":"$E$492","v":"Utilisez la fonction % pour vous adapter aux différents calibres des goujons en acier."}]
[{"$f":"IF(LEN('Translation-EN'!A647)>0,'Translation-EN'!A647,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B647)>0,'Translation-EN'!B647,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C647)>0,'Translation-EN'!C647,\"\")","v":"A18"},{"$f":"IF(LEN('Translation-EN'!D647)>0,'Translation-EN'!D647,\"\")","v":""},{"$f":"$E$319","v":"BARDAGE DES MURS INTÉRIEURS"}]
[{"$f":"IF(LEN('Translation-EN'!A648)>0,'Translation-EN'!A648,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B648)>0,'Translation-EN'!B648,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C648)>0,'Translation-EN'!C648,\"\")","v":"B19"},{"$f":"IF(LEN('Translation-EN'!D648)>0,'Translation-EN'!D648,\"\")","v":""},{"$f":"$E$320","v":"CLOISONS SÈCHES 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A649)>0,'Translation-EN'!A649,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B649)>0,'Translation-EN'!B649,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C649)>0,'Translation-EN'!C649,\"\")","v":"C20"},{"$f":"IF(LEN('Translation-EN'!D649)>0,'Translation-EN'!D649,\"\")","v":""},"Cloison sèche 1/2 po typique – murs intérieurs – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A650)>0,'Translation-EN'!A650,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B650)>0,'Translation-EN'!B650,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C650)>0,'Translation-EN'!C650,\"\")","v":"B26"},{"$f":"IF(LEN('Translation-EN'!D650)>0,'Translation-EN'!D650,\"\")","v":""},{"$f":"$E$322","v":"CLOISONS SÈCHES 5/8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A651)>0,'Translation-EN'!A651,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B651)>0,'Translation-EN'!B651,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C651)>0,'Translation-EN'!C651,\"\")","v":"B30"},{"$f":"IF(LEN('Translation-EN'!D651)>0,'Translation-EN'!D651,\"\")","v":""},{"$f":"$E$323","v":"AUTRES MATÉRIAUX DE BARDAGE"}]
[{"$f":"IF(LEN('Translation-EN'!A652)>0,'Translation-EN'!A652,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B652)>0,'Translation-EN'!B652,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C652)>0,'Translation-EN'!C652,\"\")","v":"A41"},{"$f":"IF(LEN('Translation-EN'!D652)>0,'Translation-EN'!D652,\"\")","v":""},{"$f":"$E$305","v":"ISOLATION DE LA CAVITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A653)>0,'Translation-EN'!A653,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B653)>0,'Translation-EN'!B653,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C653)>0,'Translation-EN'!C653,\"\")","v":"B42"},{"$f":"IF(LEN('Translation-EN'!D653)>0,'Translation-EN'!D653,\"\")","v":""},{"$f":"$E$307","v":"NATTE DE FIBRE DE VERRE"}]
[{"$f":"IF(LEN('Translation-EN'!A654)>0,'Translation-EN'!A654,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B654)>0,'Translation-EN'!B654,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C654)>0,'Translation-EN'!C654,\"\")","v":"C43"},{"$f":"IF(LEN('Translation-EN'!D654)>0,'Translation-EN'!D654,\"\")","v":""},{"$f":"$E$400","v":"Natte en fibre de verre – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A655)>0,'Translation-EN'!A655,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B655)>0,'Translation-EN'!B655,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C655)>0,'Translation-EN'!C655,\"\")","v":"B47"},{"$f":"IF(LEN('Translation-EN'!D655)>0,'Translation-EN'!D655,\"\")","v":""},{"$f":"$E$401","v":"FIBRE DE VERRE SOUFFLÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A656)>0,'Translation-EN'!A656,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B656)>0,'Translation-EN'!B656,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C656)>0,'Translation-EN'!C656,\"\")","v":"C48"},{"$f":"IF(LEN('Translation-EN'!D656)>0,'Translation-EN'!D656,\"\")","v":""},{"$f":"$E$402","v":"Fibre de verre en vrac – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A657)>0,'Translation-EN'!A657,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B657)>0,'Translation-EN'!B657,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C657)>0,'Translation-EN'!C657,\"\")","v":"B53"},{"$f":"IF(LEN('Translation-EN'!D657)>0,'Translation-EN'!D657,\"\")","v":""},{"$f":"$E$311","v":"NATTE DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A658)>0,'Translation-EN'!A658,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B658)>0,'Translation-EN'!B658,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C658)>0,'Translation-EN'!C658,\"\")","v":"B61"},{"$f":"IF(LEN('Translation-EN'!D658)>0,'Translation-EN'!D658,\"\")","v":""},{"$f":"$E$309","v":"ISOLATION EN CELLULOSE"}]
[{"$f":"IF(LEN('Translation-EN'!A659)>0,'Translation-EN'!A659,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B659)>0,'Translation-EN'!B659,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C659)>0,'Translation-EN'!C659,\"\")","v":"C62"},{"$f":"IF(LEN('Translation-EN'!D659)>0,'Translation-EN'!D659,\"\")","v":""},{"$f":"$E$405","v":"Cellulose – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A660)>0,'Translation-EN'!A660,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B660)>0,'Translation-EN'!B660,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C660)>0,'Translation-EN'!C660,\"\")","v":"B66"},{"$f":"IF(LEN('Translation-EN'!D660)>0,'Translation-EN'!D660,\"\")","v":""},{"$f":"$E$313","v":"NATTE DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A661)>0,'Translation-EN'!A661,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B661)>0,'Translation-EN'!B661,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C661)>0,'Translation-EN'!C661,\"\")","v":"C67"},{"$f":"IF(LEN('Translation-EN'!D661)>0,'Translation-EN'!D661,\"\")","v":""},{"$f":"$E$407","v":"Natte de fibres de bois – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A662)>0,'Translation-EN'!A662,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B662)>0,'Translation-EN'!B662,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C662)>0,'Translation-EN'!C662,\"\")","v":"B72"},{"$f":"IF(LEN('Translation-EN'!D662)>0,'Translation-EN'!D662,\"\")","v":""},{"$f":"$E$408","v":"AUTRES ISOLANTS EN FIBRES NATURELLES"}]
[{"$f":"IF(LEN('Translation-EN'!A663)>0,'Translation-EN'!A663,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B663)>0,'Translation-EN'!B663,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C663)>0,'Translation-EN'!C663,\"\")","v":"B78"},{"$f":"IF(LEN('Translation-EN'!D663)>0,'Translation-EN'!D663,\"\")","v":""},{"$f":"$E$409","v":"MOUSSE À PULVÉRISER – CELLULE FERMÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A664)>0,'Translation-EN'!A664,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B664)>0,'Translation-EN'!B664,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C664)>0,'Translation-EN'!C664,\"\")","v":"B82"},{"$f":"IF(LEN('Translation-EN'!D664)>0,'Translation-EN'!D664,\"\")","v":""},{"$f":"$E$410","v":"MOUSSE À PULVÉRISER – CELLULE OUVERTE"}]
[{"$f":"IF(LEN('Translation-EN'!A665)>0,'Translation-EN'!A665,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B665)>0,'Translation-EN'!B665,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C665)>0,'Translation-EN'!C665,\"\")","v":"B85"},{"$f":"IF(LEN('Translation-EN'!D665)>0,'Translation-EN'!D665,\"\")","v":""},{"$f":"$E$411","v":"BRIQUES DE CHANVRE"}]
[{"$f":"IF(LEN('Translation-EN'!A666)>0,'Translation-EN'!A666,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B666)>0,'Translation-EN'!B666,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C666)>0,'Translation-EN'!C666,\"\")","v":"C86"},{"$f":"IF(LEN('Translation-EN'!D666)>0,'Translation-EN'!D666,\"\")","v":""},{"$f":"$E$412","v":"Briques de chanvre – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A667)>0,'Translation-EN'!A667,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B667)>0,'Translation-EN'!B667,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C667)>0,'Translation-EN'!C667,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D667)>0,'Translation-EN'!D667,\"\")","v":""},"SECTION 10 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A668)>0,'Translation-EN'!A668,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B668)>0,'Translation-EN'!B668,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C668)>0,'Translation-EN'!C668,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D668)>0,'Translation-EN'!D668,\"\")","v":""},"PLANCHERS"]
[{"$f":"IF(LEN('Translation-EN'!A669)>0,'Translation-EN'!A669,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B669)>0,'Translation-EN'!B669,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C669)>0,'Translation-EN'!C669,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D669)>0,'Translation-EN'!D669,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A670)>0,'Translation-EN'!A670,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B670)>0,'Translation-EN'!B670,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C670)>0,'Translation-EN'!C670,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D670)>0,'Translation-EN'!D670,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A671)>0,'Translation-EN'!A671,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B671)>0,'Translation-EN'!B671,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C671)>0,'Translation-EN'!C671,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D671)>0,'Translation-EN'!D671,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A672)>0,'Translation-EN'!A672,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B672)>0,'Translation-EN'!B672,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C672)>0,'Translation-EN'!C672,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D672)>0,'Translation-EN'!D672,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A673)>0,'Translation-EN'!A673,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B673)>0,'Translation-EN'!B673,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C673)>0,'Translation-EN'!C673,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D673)>0,'Translation-EN'!D673,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A674)>0,'Translation-EN'!A674,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B674)>0,'Translation-EN'!B674,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C674)>0,'Translation-EN'!C674,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D674)>0,'Translation-EN'!D674,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A675)>0,'Translation-EN'!A675,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B675)>0,'Translation-EN'!B675,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C675)>0,'Translation-EN'!C675,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D675)>0,'Translation-EN'!D675,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A676)>0,'Translation-EN'!A676,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B676)>0,'Translation-EN'!B676,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C676)>0,'Translation-EN'!C676,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D676)>0,'Translation-EN'!D676,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A677)>0,'Translation-EN'!A677,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B677)>0,'Translation-EN'!B677,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C677)>0,'Translation-EN'!C677,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D677)>0,'Translation-EN'!D677,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A678)>0,'Translation-EN'!A678,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B678)>0,'Translation-EN'!B678,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C678)>0,'Translation-EN'!C678,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D678)>0,'Translation-EN'!D678,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A679)>0,'Translation-EN'!A679,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B679)>0,'Translation-EN'!B679,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C679)>0,'Translation-EN'!C679,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D679)>0,'Translation-EN'!D679,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A680)>0,'Translation-EN'!A680,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B680)>0,'Translation-EN'!B680,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C680)>0,'Translation-EN'!C680,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D680)>0,'Translation-EN'!D680,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A681)>0,'Translation-EN'!A681,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B681)>0,'Translation-EN'!B681,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C681)>0,'Translation-EN'!C681,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D681)>0,'Translation-EN'!D681,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A682)>0,'Translation-EN'!A682,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B682)>0,'Translation-EN'!B682,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C682)>0,'Translation-EN'!C682,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D682)>0,'Translation-EN'!D682,\"\")","v":true},"TOTAL PARTIEL POUR LES PLANCHERS kgCO2e "]
[{"$f":"IF(LEN('Translation-EN'!A683)>0,'Translation-EN'!A683,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B683)>0,'Translation-EN'!B683,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C683)>0,'Translation-EN'!C683,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D683)>0,'Translation-EN'!D683,\"\")","v":""},"ENCADREMENT DE PLANCHER EN BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A684)>0,'Translation-EN'!A684,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B684)>0,'Translation-EN'!B684,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C684)>0,'Translation-EN'!C684,\"\")","v":"D5"},{"$f":"IF(LEN('Translation-EN'!D684)>0,'Translation-EN'!D684,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A685)>0,'Translation-EN'!A685,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B685)>0,'Translation-EN'!B685,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C685)>0,'Translation-EN'!C685,\"\")","v":"B6"},{"$f":"IF(LEN('Translation-EN'!D685)>0,'Translation-EN'!D685,\"\")","v":""},"ENCADREMENT DE PLANCHER EN BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A686)>0,'Translation-EN'!A686,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B686)>0,'Translation-EN'!B686,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C686)>0,'Translation-EN'!C686,\"\")","v":"B10"},{"$f":"IF(LEN('Translation-EN'!D686)>0,'Translation-EN'!D686,\"\")","v":""},"CHARPENTE EN BOIS DE TYPE SOLIVE-I"]
[{"$f":"IF(LEN('Translation-EN'!A687)>0,'Translation-EN'!A687,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B687)>0,'Translation-EN'!B687,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C687)>0,'Translation-EN'!C687,\"\")","v":"B11"},{"$f":"IF(LEN('Translation-EN'!D687)>0,'Translation-EN'!D687,\"\")","v":""},"9-1/2 po"]
[{"$f":"IF(LEN('Translation-EN'!A688)>0,'Translation-EN'!A688,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B688)>0,'Translation-EN'!B688,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C688)>0,'Translation-EN'!C688,\"\")","v":"B14"},{"$f":"IF(LEN('Translation-EN'!D688)>0,'Translation-EN'!D688,\"\")","v":""},"CHARPENTE À TREILLIS EN BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A689)>0,'Translation-EN'!A689,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B689)>0,'Translation-EN'!B689,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C689)>0,'Translation-EN'!C689,\"\")","v":"A16"},{"$f":"IF(LEN('Translation-EN'!D689)>0,'Translation-EN'!D689,\"\")","v":""},"CHARPENTE DE PLANCHER EN ACIER"]
[{"$f":"IF(LEN('Translation-EN'!A690)>0,'Translation-EN'!A690,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B690)>0,'Translation-EN'!B690,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C690)>0,'Translation-EN'!C690,\"\")","v":"D16"},{"$f":"IF(LEN('Translation-EN'!D690)>0,'Translation-EN'!D690,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A691)>0,'Translation-EN'!A691,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B691)>0,'Translation-EN'!B691,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C691)>0,'Translation-EN'!C691,\"\")","v":"B17"},{"$f":"IF(LEN('Translation-EN'!D691)>0,'Translation-EN'!D691,\"\")","v":""},"SOLIVE À ÂME OUVERTE EN ACIER"]
[{"$f":"IF(LEN('Translation-EN'!A692)>0,'Translation-EN'!A692,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B692)>0,'Translation-EN'!B692,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C692)>0,'Translation-EN'!C692,\"\")","v":"A19"},{"$f":"IF(LEN('Translation-EN'!D692)>0,'Translation-EN'!D692,\"\")","v":""},"SOUS-PLANCHER"]
[{"$f":"IF(LEN('Translation-EN'!A693)>0,'Translation-EN'!A693,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B693)>0,'Translation-EN'!B693,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C693)>0,'Translation-EN'!C693,\"\")","v":"A26"},{"$f":"IF(LEN('Translation-EN'!D693)>0,'Translation-EN'!D693,\"\")","v":""},"BOIS LAMELLÉ-CROISÉ (BLC)"]
[{"$f":"IF(LEN('Translation-EN'!A694)>0,'Translation-EN'!A694,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B694)>0,'Translation-EN'!B694,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C694)>0,'Translation-EN'!C694,\"\")","v":"B27"},{"$f":"IF(LEN('Translation-EN'!D694)>0,'Translation-EN'!D694,\"\")","v":""},"SYSTÈME DE PLANCHER EN BLC"]
[{"$f":"IF(LEN('Translation-EN'!A695)>0,'Translation-EN'!A695,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B695)>0,'Translation-EN'!B695,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C695)>0,'Translation-EN'!C695,\"\")","v":"C28"},{"$f":"IF(LEN('Translation-EN'!D695)>0,'Translation-EN'!D695,\"\")","v":""},"Système de plancher BLC – 3-1/2 (90 mm) – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A696)>0,'Translation-EN'!A696,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B696)>0,'Translation-EN'!B696,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C696)>0,'Translation-EN'!C696,\"\")","v":"A32"},{"$f":"IF(LEN('Translation-EN'!D696)>0,'Translation-EN'!D696,\"\")","v":""},"SYSTÈME DE PLANCHER À BASE D’ARGILE"]
[{"$f":"IF(LEN('Translation-EN'!A697)>0,'Translation-EN'!A697,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B697)>0,'Translation-EN'!B697,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C697)>0,'Translation-EN'!C697,\"\")","v":"B33"},{"$f":"IF(LEN('Translation-EN'!D697)>0,'Translation-EN'!D697,\"\")","v":""},{"$f":"$E$209","v":"PLANCHER DE TERRE"}]
[{"$f":"IF(LEN('Translation-EN'!A698)>0,'Translation-EN'!A698,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B698)>0,'Translation-EN'!B698,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C698)>0,'Translation-EN'!C698,\"\")","v":"A35"},{"$f":"IF(LEN('Translation-EN'!D698)>0,'Translation-EN'!D698,\"\")","v":""},"PLANCHER FINI"]
[{"$f":"IF(LEN('Translation-EN'!A699)>0,'Translation-EN'!A699,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B699)>0,'Translation-EN'!B699,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C699)>0,'Translation-EN'!C699,\"\")","v":"B36"},{"$f":"IF(LEN('Translation-EN'!D699)>0,'Translation-EN'!D699,\"\")","v":""},"BOIS DUR 3/4 po"]
[{"$f":"IF(LEN('Translation-EN'!A700)>0,'Translation-EN'!A700,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B700)>0,'Translation-EN'!B700,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C700)>0,'Translation-EN'!C700,\"\")","v":"C37"},{"$f":"IF(LEN('Translation-EN'!D700)>0,'Translation-EN'!D700,\"\")","v":""},{"$f":"$E$223","v":"Plancher en bois dur – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A701)>0,'Translation-EN'!A701,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B701)>0,'Translation-EN'!B701,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C701)>0,'Translation-EN'!C701,\"\")","v":"B41"},{"$f":"IF(LEN('Translation-EN'!D701)>0,'Translation-EN'!D701,\"\")","v":""},{"$f":"$E$224","v":"REVÊTEMENT DE SOL EN LINOLÉUM"}]
[{"$f":"IF(LEN('Translation-EN'!A702)>0,'Translation-EN'!A702,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B702)>0,'Translation-EN'!B702,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C702)>0,'Translation-EN'!C702,\"\")","v":"C42"},{"$f":"IF(LEN('Translation-EN'!D702)>0,'Translation-EN'!D702,\"\")","v":""},"Revêtement de sol en linoléum – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A703)>0,'Translation-EN'!A703,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B703)>0,'Translation-EN'!B703,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C703)>0,'Translation-EN'!C703,\"\")","v":"B48"},{"$f":"IF(LEN('Translation-EN'!D703)>0,'Translation-EN'!D703,\"\")","v":""},{"$f":"$E$226","v":"REVÊTEMENT DE SOL EN CARRELAGE"}]
[{"$f":"IF(LEN('Translation-EN'!A704)>0,'Translation-EN'!A704,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B704)>0,'Translation-EN'!B704,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C704)>0,'Translation-EN'!C704,\"\")","v":"C49"},{"$f":"IF(LEN('Translation-EN'!D704)>0,'Translation-EN'!D704,\"\")","v":""},"Revêtement de sol en carreaux de céramique – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A705)>0,'Translation-EN'!A705,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B705)>0,'Translation-EN'!B705,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C705)>0,'Translation-EN'!C705,\"\")","v":"B55"},{"$f":"IF(LEN('Translation-EN'!D705)>0,'Translation-EN'!D705,\"\")","v":""},{"$f":"$E$228","v":"REVÊTEMENT DE SOL EN VINYLE"}]
[{"$f":"IF(LEN('Translation-EN'!A706)>0,'Translation-EN'!A706,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B706)>0,'Translation-EN'!B706,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C706)>0,'Translation-EN'!C706,\"\")","v":"C56"},{"$f":"IF(LEN('Translation-EN'!D706)>0,'Translation-EN'!D706,\"\")","v":""},{"$f":"$E$229","v":"Revêtement de sol en vinyle – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A707)>0,'Translation-EN'!A707,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B707)>0,'Translation-EN'!B707,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C707)>0,'Translation-EN'!C707,\"\")","v":"B63"},{"$f":"IF(LEN('Translation-EN'!D707)>0,'Translation-EN'!D707,\"\")","v":""},{"$f":"$E$230","v":"PLANCHER LAMELLÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A708)>0,'Translation-EN'!A708,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B708)>0,'Translation-EN'!B708,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C708)>0,'Translation-EN'!C708,\"\")","v":"B65"},{"$f":"IF(LEN('Translation-EN'!D708)>0,'Translation-EN'!D708,\"\")","v":""},{"$f":"$E$231","v":"PLANCHER DE LIÈGE"}]
[{"$f":"IF(LEN('Translation-EN'!A709)>0,'Translation-EN'!A709,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B709)>0,'Translation-EN'!B709,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C709)>0,'Translation-EN'!C709,\"\")","v":"B68"},{"$f":"IF(LEN('Translation-EN'!D709)>0,'Translation-EN'!D709,\"\")","v":""},{"$f":"$E$232","v":"TAPIS"}]
[{"$f":"IF(LEN('Translation-EN'!A710)>0,'Translation-EN'!A710,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B710)>0,'Translation-EN'!B710,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C710)>0,'Translation-EN'!C710,\"\")","v":"B72"},{"$f":"IF(LEN('Translation-EN'!D710)>0,'Translation-EN'!D710,\"\")","v":""},"AUTRES OPTIONS DE REVÊTEMENT DE SOL"]
[{"$f":"IF(LEN('Translation-EN'!A711)>0,'Translation-EN'!A711,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B711)>0,'Translation-EN'!B711,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C711)>0,'Translation-EN'!C711,\"\")","v":"A76"},{"$f":"IF(LEN('Translation-EN'!D711)>0,'Translation-EN'!D711,\"\")","v":""},"ISOLATION DE LA CAVITÉ DE PLANCHER"]
[{"$f":"IF(LEN('Translation-EN'!A712)>0,'Translation-EN'!A712,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B712)>0,'Translation-EN'!B712,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C712)>0,'Translation-EN'!C712,\"\")","v":"B77"},{"$f":"IF(LEN('Translation-EN'!D712)>0,'Translation-EN'!D712,\"\")","v":""},{"$f":"$E$307","v":"NATTE DE FIBRE DE VERRE"}]
[{"$f":"IF(LEN('Translation-EN'!A713)>0,'Translation-EN'!A713,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B713)>0,'Translation-EN'!B713,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C713)>0,'Translation-EN'!C713,\"\")","v":"C78"},{"$f":"IF(LEN('Translation-EN'!D713)>0,'Translation-EN'!D713,\"\")","v":""},"Natte de fibre de verre – Isolation de plancher – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A714)>0,'Translation-EN'!A714,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B714)>0,'Translation-EN'!B714,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C714)>0,'Translation-EN'!C714,\"\")","v":"B82"},{"$f":"IF(LEN('Translation-EN'!D714)>0,'Translation-EN'!D714,\"\")","v":""},"FIBRE DE VERRE EN VRAC"]
[{"$f":"IF(LEN('Translation-EN'!A715)>0,'Translation-EN'!A715,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B715)>0,'Translation-EN'!B715,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C715)>0,'Translation-EN'!C715,\"\")","v":"C83"},{"$f":"IF(LEN('Translation-EN'!D715)>0,'Translation-EN'!D715,\"\")","v":""},"Fibre de verre en vrac – Isolation du plancher – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A716)>0,'Translation-EN'!A716,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B716)>0,'Translation-EN'!B716,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C716)>0,'Translation-EN'!C716,\"\")","v":"B88"},{"$f":"IF(LEN('Translation-EN'!D716)>0,'Translation-EN'!D716,\"\")","v":""},{"$f":"$E$311","v":"NATTE DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A717)>0,'Translation-EN'!A717,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B717)>0,'Translation-EN'!B717,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C717)>0,'Translation-EN'!C717,\"\")","v":"C89"},{"$f":"IF(LEN('Translation-EN'!D717)>0,'Translation-EN'!D717,\"\")","v":""},"Natte de laine minérale – Isolation du plancher – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A718)>0,'Translation-EN'!A718,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B718)>0,'Translation-EN'!B718,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C718)>0,'Translation-EN'!C718,\"\")","v":"B97"},{"$f":"IF(LEN('Translation-EN'!D718)>0,'Translation-EN'!D718,\"\")","v":""},"LAINE MINÉRALE EN VRAC"]
[{"$f":"IF(LEN('Translation-EN'!A719)>0,'Translation-EN'!A719,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B719)>0,'Translation-EN'!B719,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C719)>0,'Translation-EN'!C719,\"\")","v":"B99"},{"$f":"IF(LEN('Translation-EN'!D719)>0,'Translation-EN'!D719,\"\")","v":""},{"$f":"$E$409","v":"MOUSSE À PULVÉRISER – CELLULE FERMÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A720)>0,'Translation-EN'!A720,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B720)>0,'Translation-EN'!B720,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C720)>0,'Translation-EN'!C720,\"\")","v":"B103"},{"$f":"IF(LEN('Translation-EN'!D720)>0,'Translation-EN'!D720,\"\")","v":""},{"$f":"$E$410","v":"MOUSSE À PULVÉRISER – CELLULE OUVERTE"}]
[{"$f":"IF(LEN('Translation-EN'!A721)>0,'Translation-EN'!A721,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B721)>0,'Translation-EN'!B721,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C721)>0,'Translation-EN'!C721,\"\")","v":"B106"},{"$f":"IF(LEN('Translation-EN'!D721)>0,'Translation-EN'!D721,\"\")","v":""},{"$f":"$E$309","v":"ISOLATION EN CELLULOSE"}]
[{"$f":"IF(LEN('Translation-EN'!A722)>0,'Translation-EN'!A722,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B722)>0,'Translation-EN'!B722,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C722)>0,'Translation-EN'!C722,\"\")","v":"C107"},{"$f":"IF(LEN('Translation-EN'!D722)>0,'Translation-EN'!D722,\"\")","v":""},"Cellulose – Isolation de plancher – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A723)>0,'Translation-EN'!A723,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B723)>0,'Translation-EN'!B723,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C723)>0,'Translation-EN'!C723,\"\")","v":"B112"},{"$f":"IF(LEN('Translation-EN'!D723)>0,'Translation-EN'!D723,\"\")","v":""},{"$f":"$E$313","v":"NATTE DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A724)>0,'Translation-EN'!A724,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B724)>0,'Translation-EN'!B724,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C724)>0,'Translation-EN'!C724,\"\")","v":"C113"},{"$f":"IF(LEN('Translation-EN'!D724)>0,'Translation-EN'!D724,\"\")","v":""},"Natte de fibres de bois – Isolation du plancher – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A725)>0,'Translation-EN'!A725,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B725)>0,'Translation-EN'!B725,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C725)>0,'Translation-EN'!C725,\"\")","v":"B117"},{"$f":"IF(LEN('Translation-EN'!D725)>0,'Translation-EN'!D725,\"\")","v":""},{"$f":"$E$408","v":"AUTRES ISOLANTS EN FIBRES NATURELLES"}]
[{"$f":"IF(LEN('Translation-EN'!A726)>0,'Translation-EN'!A726,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B726)>0,'Translation-EN'!B726,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C726)>0,'Translation-EN'!C726,\"\")","v":"B124"},{"$f":"IF(LEN('Translation-EN'!D726)>0,'Translation-EN'!D726,\"\")","v":""},"BRIQUES DE CHANVRE EN VRAC"]
[{"$f":"IF(LEN('Translation-EN'!A727)>0,'Translation-EN'!A727,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B727)>0,'Translation-EN'!B727,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C727)>0,'Translation-EN'!C727,\"\")","v":"C125"},{"$f":"IF(LEN('Translation-EN'!D727)>0,'Translation-EN'!D727,\"\")","v":""},"Briques de chanvre – Isolation de plancher – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A728)>0,'Translation-EN'!A728,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B728)>0,'Translation-EN'!B728,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C728)>0,'Translation-EN'!C728,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D728)>0,'Translation-EN'!D728,\"\")","v":""},"SECTION 11 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A729)>0,'Translation-EN'!A729,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B729)>0,'Translation-EN'!B729,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C729)>0,'Translation-EN'!C729,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D729)>0,'Translation-EN'!D729,\"\")","v":""},"PLAFONDS"]
[{"$f":"IF(LEN('Translation-EN'!A730)>0,'Translation-EN'!A730,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B730)>0,'Translation-EN'!B730,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C730)>0,'Translation-EN'!C730,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D730)>0,'Translation-EN'!D730,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A731)>0,'Translation-EN'!A731,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B731)>0,'Translation-EN'!B731,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C731)>0,'Translation-EN'!C731,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D731)>0,'Translation-EN'!D731,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A732)>0,'Translation-EN'!A732,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B732)>0,'Translation-EN'!B732,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C732)>0,'Translation-EN'!C732,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D732)>0,'Translation-EN'!D732,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A733)>0,'Translation-EN'!A733,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B733)>0,'Translation-EN'!B733,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C733)>0,'Translation-EN'!C733,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D733)>0,'Translation-EN'!D733,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A734)>0,'Translation-EN'!A734,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B734)>0,'Translation-EN'!B734,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C734)>0,'Translation-EN'!C734,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D734)>0,'Translation-EN'!D734,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A735)>0,'Translation-EN'!A735,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B735)>0,'Translation-EN'!B735,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C735)>0,'Translation-EN'!C735,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D735)>0,'Translation-EN'!D735,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A736)>0,'Translation-EN'!A736,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B736)>0,'Translation-EN'!B736,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C736)>0,'Translation-EN'!C736,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D736)>0,'Translation-EN'!D736,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A737)>0,'Translation-EN'!A737,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B737)>0,'Translation-EN'!B737,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C737)>0,'Translation-EN'!C737,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D737)>0,'Translation-EN'!D737,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A738)>0,'Translation-EN'!A738,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B738)>0,'Translation-EN'!B738,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C738)>0,'Translation-EN'!C738,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D738)>0,'Translation-EN'!D738,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A739)>0,'Translation-EN'!A739,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B739)>0,'Translation-EN'!B739,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C739)>0,'Translation-EN'!C739,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D739)>0,'Translation-EN'!D739,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A740)>0,'Translation-EN'!A740,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B740)>0,'Translation-EN'!B740,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C740)>0,'Translation-EN'!C740,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D740)>0,'Translation-EN'!D740,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A741)>0,'Translation-EN'!A741,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B741)>0,'Translation-EN'!B741,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C741)>0,'Translation-EN'!C741,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D741)>0,'Translation-EN'!D741,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A742)>0,'Translation-EN'!A742,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B742)>0,'Translation-EN'!B742,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C742)>0,'Translation-EN'!C742,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D742)>0,'Translation-EN'!D742,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A743)>0,'Translation-EN'!A743,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B743)>0,'Translation-EN'!B743,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C743)>0,'Translation-EN'!C743,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D743)>0,'Translation-EN'!D743,\"\")","v":true},"TOTAL PARTIEL POUR LES PLAFONDS kgCO2e "]
[{"$f":"IF(LEN('Translation-EN'!A744)>0,'Translation-EN'!A744,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B744)>0,'Translation-EN'!B744,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C744)>0,'Translation-EN'!C744,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D744)>0,'Translation-EN'!D744,\"\")","v":""},"FNIS DE PLAFOND"]
[{"$f":"IF(LEN('Translation-EN'!A745)>0,'Translation-EN'!A745,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B745)>0,'Translation-EN'!B745,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C745)>0,'Translation-EN'!C745,\"\")","v":"B6"},{"$f":"IF(LEN('Translation-EN'!D745)>0,'Translation-EN'!D745,\"\")","v":""},{"$f":"$E$320","v":"CLOISONS SÈCHES 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A746)>0,'Translation-EN'!A746,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B746)>0,'Translation-EN'!B746,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C746)>0,'Translation-EN'!C746,\"\")","v":"C7"},{"$f":"IF(LEN('Translation-EN'!D746)>0,'Translation-EN'!D746,\"\")","v":""},"Cloison sèche 1/2 po – Plafonds – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A747)>0,'Translation-EN'!A747,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B747)>0,'Translation-EN'!B747,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C747)>0,'Translation-EN'!C747,\"\")","v":"B13"},{"$f":"IF(LEN('Translation-EN'!D747)>0,'Translation-EN'!D747,\"\")","v":""},{"$f":"$E$322","v":"CLOISONS SÈCHES 5/8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A748)>0,'Translation-EN'!A748,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B748)>0,'Translation-EN'!B748,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C748)>0,'Translation-EN'!C748,\"\")","v":"C14"},{"$f":"IF(LEN('Translation-EN'!D748)>0,'Translation-EN'!D748,\"\")","v":""},"Cloison sèche 5/8 po – Plafonds – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A749)>0,'Translation-EN'!A749,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B749)>0,'Translation-EN'!B749,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C749)>0,'Translation-EN'!C749,\"\")","v":"B18"},{"$f":"IF(LEN('Translation-EN'!D749)>0,'Translation-EN'!D749,\"\")","v":""},"AUTRES FINIS DE PLAFOND"]
[{"$f":"IF(LEN('Translation-EN'!A750)>0,'Translation-EN'!A750,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B750)>0,'Translation-EN'!B750,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C750)>0,'Translation-EN'!C750,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D750)>0,'Translation-EN'!D750,\"\")","v":""},"SECTION 12 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A751)>0,'Translation-EN'!A751,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B751)>0,'Translation-EN'!B751,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C751)>0,'Translation-EN'!C751,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D751)>0,'Translation-EN'!D751,\"\")","v":""},"TOITS"]
[{"$f":"IF(LEN('Translation-EN'!A752)>0,'Translation-EN'!A752,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B752)>0,'Translation-EN'!B752,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C752)>0,'Translation-EN'!C752,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D752)>0,'Translation-EN'!D752,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A753)>0,'Translation-EN'!A753,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B753)>0,'Translation-EN'!B753,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C753)>0,'Translation-EN'!C753,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D753)>0,'Translation-EN'!D753,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A754)>0,'Translation-EN'!A754,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B754)>0,'Translation-EN'!B754,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C754)>0,'Translation-EN'!C754,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D754)>0,'Translation-EN'!D754,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A755)>0,'Translation-EN'!A755,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B755)>0,'Translation-EN'!B755,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C755)>0,'Translation-EN'!C755,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D755)>0,'Translation-EN'!D755,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A756)>0,'Translation-EN'!A756,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B756)>0,'Translation-EN'!B756,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C756)>0,'Translation-EN'!C756,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D756)>0,'Translation-EN'!D756,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A757)>0,'Translation-EN'!A757,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B757)>0,'Translation-EN'!B757,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C757)>0,'Translation-EN'!C757,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D757)>0,'Translation-EN'!D757,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A758)>0,'Translation-EN'!A758,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B758)>0,'Translation-EN'!B758,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C758)>0,'Translation-EN'!C758,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D758)>0,'Translation-EN'!D758,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A759)>0,'Translation-EN'!A759,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B759)>0,'Translation-EN'!B759,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C759)>0,'Translation-EN'!C759,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D759)>0,'Translation-EN'!D759,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A760)>0,'Translation-EN'!A760,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B760)>0,'Translation-EN'!B760,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C760)>0,'Translation-EN'!C760,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D760)>0,'Translation-EN'!D760,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A761)>0,'Translation-EN'!A761,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B761)>0,'Translation-EN'!B761,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C761)>0,'Translation-EN'!C761,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D761)>0,'Translation-EN'!D761,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A762)>0,'Translation-EN'!A762,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B762)>0,'Translation-EN'!B762,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C762)>0,'Translation-EN'!C762,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D762)>0,'Translation-EN'!D762,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A763)>0,'Translation-EN'!A763,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B763)>0,'Translation-EN'!B763,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C763)>0,'Translation-EN'!C763,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D763)>0,'Translation-EN'!D763,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A764)>0,'Translation-EN'!A764,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B764)>0,'Translation-EN'!B764,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C764)>0,'Translation-EN'!C764,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D764)>0,'Translation-EN'!D764,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A765)>0,'Translation-EN'!A765,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B765)>0,'Translation-EN'!B765,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C765)>0,'Translation-EN'!C765,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D765)>0,'Translation-EN'!D765,\"\")","v":true},"TOTAL PARTIEL POUR LES TOITS kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A766)>0,'Translation-EN'!A766,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B766)>0,'Translation-EN'!B766,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C766)>0,'Translation-EN'!C766,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D766)>0,'Translation-EN'!D766,\"\")","v":""},"TOIT À CHARPENTE EN BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A767)>0,'Translation-EN'!A767,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B767)>0,'Translation-EN'!B767,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C767)>0,'Translation-EN'!C767,\"\")","v":"D5"},{"$f":"IF(LEN('Translation-EN'!D767)>0,'Translation-EN'!D767,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A768)>0,'Translation-EN'!A768,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B768)>0,'Translation-EN'!B768,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C768)>0,'Translation-EN'!C768,\"\")","v":"B6"},{"$f":"IF(LEN('Translation-EN'!D768)>0,'Translation-EN'!D768,\"\")","v":""},"CHARPENTE EN BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A769)>0,'Translation-EN'!A769,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B769)>0,'Translation-EN'!B769,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C769)>0,'Translation-EN'!C769,\"\")","v":"B12"},{"$f":"IF(LEN('Translation-EN'!D769)>0,'Translation-EN'!D769,\"\")","v":""},{"$f":"$E$688","v":"CHARPENTE À TREILLIS EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A770)>0,'Translation-EN'!A770,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B770)>0,'Translation-EN'!B770,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C770)>0,'Translation-EN'!C770,\"\")","v":"A13"},{"$f":"IF(LEN('Translation-EN'!D770)>0,'Translation-EN'!D770,\"\")","v":""},"Utilisez la fonction pourcentage pour ajuster le volume de bois par rapport à la conception décrite du toit."]
[{"$f":"IF(LEN('Translation-EN'!A771)>0,'Translation-EN'!A771,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B771)>0,'Translation-EN'!B771,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C771)>0,'Translation-EN'!C771,\"\")","v":"B14"},{"$f":"IF(LEN('Translation-EN'!D771)>0,'Translation-EN'!D771,\"\")","v":""},{"$f":"$E$686","v":"CHARPENTE EN BOIS DE TYPE SOLIVE-I"}]
[{"$f":"IF(LEN('Translation-EN'!A772)>0,'Translation-EN'!A772,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B772)>0,'Translation-EN'!B772,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C772)>0,'Translation-EN'!C772,\"\")","v":"A19"},{"$f":"IF(LEN('Translation-EN'!D772)>0,'Translation-EN'!D772,\"\")","v":""},"TERRASSE EN TOITURE"]
[{"$f":"IF(LEN('Translation-EN'!A773)>0,'Translation-EN'!A773,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B773)>0,'Translation-EN'!B773,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C773)>0,'Translation-EN'!C773,\"\")","v":"B20"},{"$f":"IF(LEN('Translation-EN'!D773)>0,'Translation-EN'!D773,\"\")","v":""},"PRODUITS EN FEUILLE DE BOIS –5/8 po"]
[{"$f":"IF(LEN('Translation-EN'!A774)>0,'Translation-EN'!A774,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B774)>0,'Translation-EN'!B774,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C774)>0,'Translation-EN'!C774,\"\")","v":"B23"},{"$f":"IF(LEN('Translation-EN'!D774)>0,'Translation-EN'!D774,\"\")","v":""},"PANNEAUX DE GYPSE 1/2 po"]
[{"$f":"IF(LEN('Translation-EN'!A775)>0,'Translation-EN'!A775,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B775)>0,'Translation-EN'!B775,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C775)>0,'Translation-EN'!C775,\"\")","v":"A27"},{"$f":"IF(LEN('Translation-EN'!D775)>0,'Translation-EN'!D775,\"\")","v":""},"MEMBRANE DE TOITURE"]
[{"$f":"IF(LEN('Translation-EN'!A776)>0,'Translation-EN'!A776,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B776)>0,'Translation-EN'!B776,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C776)>0,'Translation-EN'!C776,\"\")","v":"B28"},{"$f":"IF(LEN('Translation-EN'!D776)>0,'Translation-EN'!D776,\"\")","v":""},{"$f":"$E$775","v":"MEMBRANE DE TOITURE"}]
[{"$f":"IF(LEN('Translation-EN'!A777)>0,'Translation-EN'!A777,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B777)>0,'Translation-EN'!B777,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C777)>0,'Translation-EN'!C777,\"\")","v":"A33"},{"$f":"IF(LEN('Translation-EN'!D777)>0,'Translation-EN'!D777,\"\")","v":""},"GRADATION DE LA TOITURE"]
[{"$f":"IF(LEN('Translation-EN'!A778)>0,'Translation-EN'!A778,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B778)>0,'Translation-EN'!B778,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C778)>0,'Translation-EN'!C778,\"\")","v":"D33"},{"$f":"IF(LEN('Translation-EN'!D778)>0,'Translation-EN'!D778,\"\")","v":""},{"$f":"$E$598","v":"ESPACEMENT DES TASSEAUX"}]
[{"$f":"IF(LEN('Translation-EN'!A779)>0,'Translation-EN'!A779,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B779)>0,'Translation-EN'!B779,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C779)>0,'Translation-EN'!C779,\"\")","v":"B34"},{"$f":"IF(LEN('Translation-EN'!D779)>0,'Translation-EN'!D779,\"\")","v":""},"GRADATION DU BOIS"]
[{"$f":"IF(LEN('Translation-EN'!A780)>0,'Translation-EN'!A780,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B780)>0,'Translation-EN'!B780,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C780)>0,'Translation-EN'!C780,\"\")","v":"A38"},{"$f":"IF(LEN('Translation-EN'!D780)>0,'Translation-EN'!D780,\"\")","v":""},"TOITURE"]
[{"$f":"IF(LEN('Translation-EN'!A781)>0,'Translation-EN'!A781,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B781)>0,'Translation-EN'!B781,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C781)>0,'Translation-EN'!C781,\"\")","v":"B39"},{"$f":"IF(LEN('Translation-EN'!D781)>0,'Translation-EN'!D781,\"\")","v":""},"BARDEAUX D’ASPHALTE"]
[{"$f":"IF(LEN('Translation-EN'!A782)>0,'Translation-EN'!A782,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B782)>0,'Translation-EN'!B782,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C782)>0,'Translation-EN'!C782,\"\")","v":"C40"},{"$f":"IF(LEN('Translation-EN'!D782)>0,'Translation-EN'!D782,\"\")","v":""},"Bardeaux d’asphalte – Toitures – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A783)>0,'Translation-EN'!A783,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B783)>0,'Translation-EN'!B783,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C783)>0,'Translation-EN'!C783,\"\")","v":"B47"},{"$f":"IF(LEN('Translation-EN'!D783)>0,'Translation-EN'!D783,\"\")","v":""},"PLAQUE DE TOITURE D’ACIER"]
[{"$f":"IF(LEN('Translation-EN'!A784)>0,'Translation-EN'!A784,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B784)>0,'Translation-EN'!B784,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C784)>0,'Translation-EN'!C784,\"\")","v":"C48"},{"$f":"IF(LEN('Translation-EN'!D784)>0,'Translation-EN'!D784,\"\")","v":""},"Plaque de toiture d’acier – toiture – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A785)>0,'Translation-EN'!A785,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B785)>0,'Translation-EN'!B785,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C785)>0,'Translation-EN'!C785,\"\")","v":"B54"},{"$f":"IF(LEN('Translation-EN'!D785)>0,'Translation-EN'!D785,\"\")","v":""},"PLAQUE DE TOITURE D'ALUMINIUM"]
[{"$f":"IF(LEN('Translation-EN'!A786)>0,'Translation-EN'!A786,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B786)>0,'Translation-EN'!B786,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C786)>0,'Translation-EN'!C786,\"\")","v":"C55"},{"$f":"IF(LEN('Translation-EN'!D786)>0,'Translation-EN'!D786,\"\")","v":""},"Bardage en plaque d’aluminium – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A787)>0,'Translation-EN'!A787,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B787)>0,'Translation-EN'!B787,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C787)>0,'Translation-EN'!C787,\"\")","v":"B58"},{"$f":"IF(LEN('Translation-EN'!D787)>0,'Translation-EN'!D787,\"\")","v":""},"TOITURE EN FIBROCIMENT"]
[{"$f":"IF(LEN('Translation-EN'!A788)>0,'Translation-EN'!A788,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B788)>0,'Translation-EN'!B788,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C788)>0,'Translation-EN'!C788,\"\")","v":"C59"},{"$f":"IF(LEN('Translation-EN'!D788)>0,'Translation-EN'!D788,\"\")","v":""},"Bardage en fibrociment – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A789)>0,'Translation-EN'!A789,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B789)>0,'Translation-EN'!B789,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C789)>0,'Translation-EN'!C789,\"\")","v":"B63"},{"$f":"IF(LEN('Translation-EN'!D789)>0,'Translation-EN'!D789,\"\")","v":""},"AUTRES OPTIONS DE TOITURE"]
[{"$f":"IF(LEN('Translation-EN'!A790)>0,'Translation-EN'!A790,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B790)>0,'Translation-EN'!B790,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C790)>0,'Translation-EN'!C790,\"\")","v":"A65"},{"$f":"IF(LEN('Translation-EN'!D790)>0,'Translation-EN'!D790,\"\")","v":""},"ISOLATION DE LA CAVITÉ DE TOIT"]
[{"$f":"IF(LEN('Translation-EN'!A791)>0,'Translation-EN'!A791,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B791)>0,'Translation-EN'!B791,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C791)>0,'Translation-EN'!C791,\"\")","v":"F65"},{"$f":"IF(LEN('Translation-EN'!D791)>0,'Translation-EN'!D791,\"\")","v":""},"ISOLATION PARALLÈLE À :"]
[{"$f":"IF(LEN('Translation-EN'!A792)>0,'Translation-EN'!A792,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B792)>0,'Translation-EN'!B792,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C792)>0,'Translation-EN'!C792,\"\")","v":"I65"},{"$f":"IF(LEN('Translation-EN'!D792)>0,'Translation-EN'!D792,\"\")","v":""},"Surface du plafond"]
[{"$f":"IF(LEN('Translation-EN'!A793)>0,'Translation-EN'!A793,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B793)>0,'Translation-EN'!B793,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C793)>0,'Translation-EN'!C793,\"\")","v":"B66"},{"$f":"IF(LEN('Translation-EN'!D793)>0,'Translation-EN'!D793,\"\")","v":""},{"$f":"$E$307","v":"NATTE DE FIBRE DE VERRE"}]
[{"$f":"IF(LEN('Translation-EN'!A794)>0,'Translation-EN'!A794,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B794)>0,'Translation-EN'!B794,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C794)>0,'Translation-EN'!C794,\"\")","v":"C67"},{"$f":"IF(LEN('Translation-EN'!D794)>0,'Translation-EN'!D794,\"\")","v":""},"Natte de fibre de verre – Isolation de toit – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A795)>0,'Translation-EN'!A795,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B795)>0,'Translation-EN'!B795,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C795)>0,'Translation-EN'!C795,\"\")","v":"B71"},{"$f":"IF(LEN('Translation-EN'!D795)>0,'Translation-EN'!D795,\"\")","v":""},{"$f":"$E$714","v":"FIBRE DE VERRE EN VRAC"}]
[{"$f":"IF(LEN('Translation-EN'!A796)>0,'Translation-EN'!A796,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B796)>0,'Translation-EN'!B796,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C796)>0,'Translation-EN'!C796,\"\")","v":"C72"},{"$f":"IF(LEN('Translation-EN'!D796)>0,'Translation-EN'!D796,\"\")","v":""},"Fibre de verre en vrac – Isolation du toit – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A797)>0,'Translation-EN'!A797,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B797)>0,'Translation-EN'!B797,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C797)>0,'Translation-EN'!C797,\"\")","v":"B77"},{"$f":"IF(LEN('Translation-EN'!D797)>0,'Translation-EN'!D797,\"\")","v":""},{"$f":"$E$311","v":"NATTE DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A798)>0,'Translation-EN'!A798,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B798)>0,'Translation-EN'!B798,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C798)>0,'Translation-EN'!C798,\"\")","v":"C78"},{"$f":"IF(LEN('Translation-EN'!D798)>0,'Translation-EN'!D798,\"\")","v":""},"Natte de laine minérale – Isolation du toit – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A799)>0,'Translation-EN'!A799,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B799)>0,'Translation-EN'!B799,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C799)>0,'Translation-EN'!C799,\"\")","v":"B86"},{"$f":"IF(LEN('Translation-EN'!D799)>0,'Translation-EN'!D799,\"\")","v":""},{"$f":"$E$718","v":"LAINE MINÉRALE EN VRAC"}]
[{"$f":"IF(LEN('Translation-EN'!A800)>0,'Translation-EN'!A800,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B800)>0,'Translation-EN'!B800,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C800)>0,'Translation-EN'!C800,\"\")","v":"B88"},{"$f":"IF(LEN('Translation-EN'!D800)>0,'Translation-EN'!D800,\"\")","v":""},{"$f":"$E$409","v":"MOUSSE À PULVÉRISER – CELLULE FERMÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A801)>0,'Translation-EN'!A801,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B801)>0,'Translation-EN'!B801,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C801)>0,'Translation-EN'!C801,\"\")","v":"B92"},{"$f":"IF(LEN('Translation-EN'!D801)>0,'Translation-EN'!D801,\"\")","v":""},{"$f":"$E$410","v":"MOUSSE À PULVÉRISER – CELLULE OUVERTE"}]
[{"$f":"IF(LEN('Translation-EN'!A802)>0,'Translation-EN'!A802,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B802)>0,'Translation-EN'!B802,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C802)>0,'Translation-EN'!C802,\"\")","v":"B95"},{"$f":"IF(LEN('Translation-EN'!D802)>0,'Translation-EN'!D802,\"\")","v":""},{"$f":"$E$309","v":"ISOLATION EN CELLULOSE"}]
[{"$f":"IF(LEN('Translation-EN'!A803)>0,'Translation-EN'!A803,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B803)>0,'Translation-EN'!B803,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C803)>0,'Translation-EN'!C803,\"\")","v":"C96"},{"$f":"IF(LEN('Translation-EN'!D803)>0,'Translation-EN'!D803,\"\")","v":""},"Cellulose – Isolation de toit – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A804)>0,'Translation-EN'!A804,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B804)>0,'Translation-EN'!B804,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C804)>0,'Translation-EN'!C804,\"\")","v":"B101"},{"$f":"IF(LEN('Translation-EN'!D804)>0,'Translation-EN'!D804,\"\")","v":""},{"$f":"$E$313","v":"NATTE DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A805)>0,'Translation-EN'!A805,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B805)>0,'Translation-EN'!B805,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C805)>0,'Translation-EN'!C805,\"\")","v":"C102"},{"$f":"IF(LEN('Translation-EN'!D805)>0,'Translation-EN'!D805,\"\")","v":""},"Natte de fibres de bois – Isolation du toit – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A806)>0,'Translation-EN'!A806,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B806)>0,'Translation-EN'!B806,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C806)>0,'Translation-EN'!C806,\"\")","v":"B106"},{"$f":"IF(LEN('Translation-EN'!D806)>0,'Translation-EN'!D806,\"\")","v":""},{"$f":"$E$408","v":"AUTRES ISOLANTS EN FIBRES NATURELLES"}]
[{"$f":"IF(LEN('Translation-EN'!A807)>0,'Translation-EN'!A807,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B807)>0,'Translation-EN'!B807,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C807)>0,'Translation-EN'!C807,\"\")","v":"B113"},{"$f":"IF(LEN('Translation-EN'!D807)>0,'Translation-EN'!D807,\"\")","v":""},{"$f":"$E$726","v":"BRIQUES DE CHANVRE EN VRAC"}]
[{"$f":"IF(LEN('Translation-EN'!A808)>0,'Translation-EN'!A808,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B808)>0,'Translation-EN'!B808,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C808)>0,'Translation-EN'!C808,\"\")","v":"C114"},{"$f":"IF(LEN('Translation-EN'!D808)>0,'Translation-EN'!D808,\"\")","v":""},"Briques de chanvre – Isolation de toit – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A809)>0,'Translation-EN'!A809,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B809)>0,'Translation-EN'!B809,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C809)>0,'Translation-EN'!C809,\"\")","v":"B117"},{"$f":"IF(LEN('Translation-EN'!D809)>0,'Translation-EN'!D809,\"\")","v":""},{"$f":"$E$318","v":"ISOLATION À VALEUR R ÉLEVÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A810)>0,'Translation-EN'!A810,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B810)>0,'Translation-EN'!B810,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C810)>0,'Translation-EN'!C810,\"\")","v":"A120"},{"$f":"IF(LEN('Translation-EN'!D810)>0,'Translation-EN'!D810,\"\")","v":""},"BRISQUE DE CHANVRE – ISOLATION DE TOIT – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A811)>0,'Translation-EN'!A811,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B811)>0,'Translation-EN'!B811,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C811)>0,'Translation-EN'!C811,\"\")","v":"F120"},{"$f":"IF(LEN('Translation-EN'!D811)>0,'Translation-EN'!D811,\"\")","v":""},{"$f":"$E$791","v":"ISOLATION PARALLÈLE À :"}]
[{"$f":"IF(LEN('Translation-EN'!A812)>0,'Translation-EN'!A812,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B812)>0,'Translation-EN'!B812,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C812)>0,'Translation-EN'!C812,\"\")","v":"I120"},{"$f":"IF(LEN('Translation-EN'!D812)>0,'Translation-EN'!D812,\"\")","v":""},"Surface de toit"]
[{"$f":"IF(LEN('Translation-EN'!A813)>0,'Translation-EN'!A813,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B813)>0,'Translation-EN'!B813,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C813)>0,'Translation-EN'!C813,\"\")","v":"B121"},{"$f":"IF(LEN('Translation-EN'!D813)>0,'Translation-EN'!D813,\"\")","v":""},{"$f":"$E$211","v":"PANNEAU DE MOUSSE EPS"}]
[{"$f":"IF(LEN('Translation-EN'!A814)>0,'Translation-EN'!A814,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B814)>0,'Translation-EN'!B814,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C814)>0,'Translation-EN'!C814,\"\")","v":"C122"},{"$f":"IF(LEN('Translation-EN'!D814)>0,'Translation-EN'!D814,\"\")","v":""},{"$f":"$E$212","v":"Panneau de mousse EPS – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A815)>0,'Translation-EN'!A815,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B815)>0,'Translation-EN'!B815,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C815)>0,'Translation-EN'!C815,\"\")","v":"B125"},{"$f":"IF(LEN('Translation-EN'!D815)>0,'Translation-EN'!D815,\"\")","v":""},{"$f":"$E$270","v":"PANNEAU DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A816)>0,'Translation-EN'!A816,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B816)>0,'Translation-EN'!B816,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C816)>0,'Translation-EN'!C816,\"\")","v":"C126"},{"$f":"IF(LEN('Translation-EN'!D816)>0,'Translation-EN'!D816,\"\")","v":""},{"$f":"$E$271","v":"Panneau de fibres de bois – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A817)>0,'Translation-EN'!A817,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B817)>0,'Translation-EN'!B817,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C817)>0,'Translation-EN'!C817,\"\")","v":"B132"},{"$f":"IF(LEN('Translation-EN'!D817)>0,'Translation-EN'!D817,\"\")","v":""},{"$f":"$E$213","v":"PANNEAU DE MOUSSE XPS"}]
[{"$f":"IF(LEN('Translation-EN'!A818)>0,'Translation-EN'!A818,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B818)>0,'Translation-EN'!B818,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C818)>0,'Translation-EN'!C818,\"\")","v":"C133"},{"$f":"IF(LEN('Translation-EN'!D818)>0,'Translation-EN'!D818,\"\")","v":""},{"$f":"$E$214","v":"Panneau de mousse XPS – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A819)>0,'Translation-EN'!A819,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B819)>0,'Translation-EN'!B819,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C819)>0,'Translation-EN'!C819,\"\")","v":"B138"},{"$f":"IF(LEN('Translation-EN'!D819)>0,'Translation-EN'!D819,\"\")","v":""},{"$f":"$E$420","v":"PANNEAU DE MOUSSE POLYISOCYANURATE"}]
[{"$f":"IF(LEN('Translation-EN'!A820)>0,'Translation-EN'!A820,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B820)>0,'Translation-EN'!B820,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C820)>0,'Translation-EN'!C820,\"\")","v":"C139"},{"$f":"IF(LEN('Translation-EN'!D820)>0,'Translation-EN'!D820,\"\")","v":""},{"$f":"$E$421","v":"Polyisocyanurate – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A821)>0,'Translation-EN'!A821,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B821)>0,'Translation-EN'!B821,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C821)>0,'Translation-EN'!C821,\"\")","v":"B144"},{"$f":"IF(LEN('Translation-EN'!D821)>0,'Translation-EN'!D821,\"\")","v":""},{"$f":"$E$215","v":"PANNEAU DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A822)>0,'Translation-EN'!A822,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B822)>0,'Translation-EN'!B822,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C822)>0,'Translation-EN'!C822,\"\")","v":"C145"},{"$f":"IF(LEN('Translation-EN'!D822)>0,'Translation-EN'!D822,\"\")","v":""},{"$f":"$E$423","v":"Panneau de laine minérale – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A823)>0,'Translation-EN'!A823,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B823)>0,'Translation-EN'!B823,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C823)>0,'Translation-EN'!C823,\"\")","v":"A149"},{"$f":"IF(LEN('Translation-EN'!D823)>0,'Translation-EN'!D823,\"\")","v":""},"PANNEAUX DE TOITURE ISOLÉS"]
[{"$f":"IF(LEN('Translation-EN'!A824)>0,'Translation-EN'!A824,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B824)>0,'Translation-EN'!B824,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C824)>0,'Translation-EN'!C824,\"\")","v":"B150"},{"$f":"IF(LEN('Translation-EN'!D824)>0,'Translation-EN'!D824,\"\")","v":""},"PANNEAU STRUCTUREL ISOLÉ –Noyau de mousse EPS avec OSB"]
[{"$f":"IF(LEN('Translation-EN'!A825)>0,'Translation-EN'!A825,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B825)>0,'Translation-EN'!B825,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C825)>0,'Translation-EN'!C825,\"\")","v":"C151"},{"$f":"IF(LEN('Translation-EN'!D825)>0,'Translation-EN'!D825,\"\")","v":""},"Panneau structurel isolé – toiture – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A826)>0,'Translation-EN'!A826,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B826)>0,'Translation-EN'!B826,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C826)>0,'Translation-EN'!C826,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D826)>0,'Translation-EN'!D826,\"\")","v":""},"SECTION 13 ➜ COMPOSANTS ET MATÉRIAUX POUR LE"]
[{"$f":"IF(LEN('Translation-EN'!A827)>0,'Translation-EN'!A827,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B827)>0,'Translation-EN'!B827,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C827)>0,'Translation-EN'!C827,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D827)>0,'Translation-EN'!D827,\"\")","v":""},{"$f":"$E$119","v":"GARAGE"}]
[{"$f":"IF(LEN('Translation-EN'!A828)>0,'Translation-EN'!A828,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B828)>0,'Translation-EN'!B828,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C828)>0,'Translation-EN'!C828,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D828)>0,'Translation-EN'!D828,\"\")","v":true},{"$f":"$E$164","v":"INSTRUCTIONS : (double-cliquer)\nLa colonne  ÉMISSIONS NETTES de kgCO2e  (Col. I) indique le potentiel de réchauffement planétaire (PRP) de chaque matériau sur la base des informations fournies.\nVous devez spécifier la VALEUR RE, L'ÉPAISSEUR, L'ESPACE DE CADRAGE ou toute autre information requise dans les zones surlignées en JAUNE.\nEntrez « 1 » dans la colonne SÉLECTIONNER (Col. H) pour ajouter chaque matériau à votre bâtiment. Les émissions nettes de carbone pour le matériau sélectionné seront mises en évidence en  ORANGE.\nUtilisez la cellule des valeurs en pourcentage (Col. G) si nécessaire pour ajuster la quantité de matériaux présents dans le bâtiment.\nL'empreinte carbone de chaque sélection sera ajoutée à la section TOTAL PARTIEL (en haut de la Col. M) pour cette page et pour le rapport de synthèse."}]
[{"$f":"IF(LEN('Translation-EN'!A829)>0,'Translation-EN'!A829,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B829)>0,'Translation-EN'!B829,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C829)>0,'Translation-EN'!C829,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D829)>0,'Translation-EN'!D829,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A830)>0,'Translation-EN'!A830,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B830)>0,'Translation-EN'!B830,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C830)>0,'Translation-EN'!C830,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D830)>0,'Translation-EN'!D830,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A831)>0,'Translation-EN'!A831,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B831)>0,'Translation-EN'!B831,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C831)>0,'Translation-EN'!C831,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D831)>0,'Translation-EN'!D831,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A832)>0,'Translation-EN'!A832,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B832)>0,'Translation-EN'!B832,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C832)>0,'Translation-EN'!C832,\"\")","v":"H3"},{"$f":"IF(LEN('Translation-EN'!D832)>0,'Translation-EN'!D832,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A833)>0,'Translation-EN'!A833,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B833)>0,'Translation-EN'!B833,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C833)>0,'Translation-EN'!C833,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D833)>0,'Translation-EN'!D833,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A834)>0,'Translation-EN'!A834,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B834)>0,'Translation-EN'!B834,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C834)>0,'Translation-EN'!C834,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D834)>0,'Translation-EN'!D834,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A835)>0,'Translation-EN'!A835,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B835)>0,'Translation-EN'!B835,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C835)>0,'Translation-EN'!C835,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D835)>0,'Translation-EN'!D835,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A836)>0,'Translation-EN'!A836,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B836)>0,'Translation-EN'!B836,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C836)>0,'Translation-EN'!C836,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D836)>0,'Translation-EN'!D836,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A837)>0,'Translation-EN'!A837,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B837)>0,'Translation-EN'!B837,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C837)>0,'Translation-EN'!C837,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D837)>0,'Translation-EN'!D837,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A838)>0,'Translation-EN'!A838,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B838)>0,'Translation-EN'!B838,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C838)>0,'Translation-EN'!C838,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D838)>0,'Translation-EN'!D838,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A839)>0,'Translation-EN'!A839,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B839)>0,'Translation-EN'!B839,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C839)>0,'Translation-EN'!C839,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D839)>0,'Translation-EN'!D839,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A840)>0,'Translation-EN'!A840,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B840)>0,'Translation-EN'!B840,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C840)>0,'Translation-EN'!C840,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D840)>0,'Translation-EN'!D840,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A841)>0,'Translation-EN'!A841,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B841)>0,'Translation-EN'!B841,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C841)>0,'Translation-EN'!C841,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D841)>0,'Translation-EN'!D841,\"\")","v":true},"TOTAL PARTIEL POUR LE GARAGE kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A842)>0,'Translation-EN'!A842,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B842)>0,'Translation-EN'!B842,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C842)>0,'Translation-EN'!C842,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D842)>0,'Translation-EN'!D842,\"\")","v":""},"SEMELLES ET DALLES DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A843)>0,'Translation-EN'!A843,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B843)>0,'Translation-EN'!B843,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C843)>0,'Translation-EN'!C843,\"\")","v":"A6"},{"$f":"IF(LEN('Translation-EN'!D843)>0,'Translation-EN'!D843,\"\")","v":""},{"$f":"$E$178","v":"BASE DE PIERRE CONCASSÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A844)>0,'Translation-EN'!A844,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B844)>0,'Translation-EN'!B844,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C844)>0,'Translation-EN'!C844,\"\")","v":"D6"},{"$f":"IF(LEN('Translation-EN'!D844)>0,'Translation-EN'!D844,\"\")","v":""},{"$f":"$E$179","v":"ÉPAISSEUR :"}]
[{"$f":"IF(LEN('Translation-EN'!A845)>0,'Translation-EN'!A845,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B845)>0,'Translation-EN'!B845,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C845)>0,'Translation-EN'!C845,\"\")","v":"B7"},{"$f":"IF(LEN('Translation-EN'!D845)>0,'Translation-EN'!D845,\"\")","v":""},{"$f":"$E$180","v":"AGGRÉGAT"}]
[{"$f":"IF(LEN('Translation-EN'!A846)>0,'Translation-EN'!A846,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B846)>0,'Translation-EN'!B846,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C846)>0,'Translation-EN'!C846,\"\")","v":"A8"},{"$f":"IF(LEN('Translation-EN'!D846)>0,'Translation-EN'!D846,\"\")","v":""},{"$f":"$E$181","v":"Si vous ne connaissez pas l’empreinte carbone spécifique de votre agrégat, choisissez la valeur « MOYENNE »."}]
[{"$f":"IF(LEN('Translation-EN'!A847)>0,'Translation-EN'!A847,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B847)>0,'Translation-EN'!B847,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C847)>0,'Translation-EN'!C847,\"\")","v":"A13"},{"$f":"IF(LEN('Translation-EN'!D847)>0,'Translation-EN'!D847,\"\")","v":""},"PLANCHER EN DALLES DE BÉTON"]
[{"$f":"IF(LEN('Translation-EN'!A848)>0,'Translation-EN'!A848,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B848)>0,'Translation-EN'!B848,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C848)>0,'Translation-EN'!C848,\"\")","v":"D13"},{"$f":"IF(LEN('Translation-EN'!D848)>0,'Translation-EN'!D848,\"\")","v":""},{"$f":"$E$179","v":"ÉPAISSEUR :"}]
[{"$f":"IF(LEN('Translation-EN'!A849)>0,'Translation-EN'!A849,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B849)>0,'Translation-EN'!B849,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C849)>0,'Translation-EN'!C849,\"\")","v":"B14"},{"$f":"IF(LEN('Translation-EN'!D849)>0,'Translation-EN'!D849,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A850)>0,'Translation-EN'!A850,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B850)>0,'Translation-EN'!B850,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C850)>0,'Translation-EN'!C850,\"\")","v":"A15"},{"$f":"IF(LEN('Translation-EN'!D850)>0,'Translation-EN'!D850,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A851)>0,'Translation-EN'!A851,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B851)>0,'Translation-EN'!B851,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C851)>0,'Translation-EN'!C851,\"\")","v":"B22"},{"$f":"IF(LEN('Translation-EN'!D851)>0,'Translation-EN'!D851,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A852)>0,'Translation-EN'!A852,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B852)>0,'Translation-EN'!B852,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C852)>0,'Translation-EN'!C852,\"\")","v":"A23"},{"$f":"IF(LEN('Translation-EN'!D852)>0,'Translation-EN'!D852,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A853)>0,'Translation-EN'!A853,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B853)>0,'Translation-EN'!B853,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C853)>0,'Translation-EN'!C853,\"\")","v":"A30"},{"$f":"IF(LEN('Translation-EN'!D853)>0,'Translation-EN'!D853,\"\")","v":""},"GRILLAGE DE RENFORCEMENT DES DALLES"]
[{"$f":"IF(LEN('Translation-EN'!A854)>0,'Translation-EN'!A854,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B854)>0,'Translation-EN'!B854,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C854)>0,'Translation-EN'!C854,\"\")","v":"D30"},{"$f":"IF(LEN('Translation-EN'!D854)>0,'Translation-EN'!D854,\"\")","v":""},{"$f":"$E$194","v":"SURFACE PERSONNALISÉE :"}]
[{"$f":"IF(LEN('Translation-EN'!A855)>0,'Translation-EN'!A855,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B855)>0,'Translation-EN'!B855,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C855)>0,'Translation-EN'!C855,\"\")","v":"B31"},{"$f":"IF(LEN('Translation-EN'!D855)>0,'Translation-EN'!D855,\"\")","v":""},"GRILLAGE SOUDÉ"]
[{"$f":"IF(LEN('Translation-EN'!A856)>0,'Translation-EN'!A856,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B856)>0,'Translation-EN'!B856,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C856)>0,'Translation-EN'!C856,\"\")","v":"A33"},{"$f":"IF(LEN('Translation-EN'!D856)>0,'Translation-EN'!D856,\"\")","v":""},{"$f":"$E$182","v":"SEMELLES, PILIERS ET SOCLES"}]
[{"$f":"IF(LEN('Translation-EN'!A857)>0,'Translation-EN'!A857,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B857)>0,'Translation-EN'!B857,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C857)>0,'Translation-EN'!C857,\"\")","v":"B34"},{"$f":"IF(LEN('Translation-EN'!D857)>0,'Translation-EN'!D857,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A858)>0,'Translation-EN'!A858,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B858)>0,'Translation-EN'!B858,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C858)>0,'Translation-EN'!C858,\"\")","v":"A35"},{"$f":"IF(LEN('Translation-EN'!D858)>0,'Translation-EN'!D858,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A859)>0,'Translation-EN'!A859,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B859)>0,'Translation-EN'!B859,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C859)>0,'Translation-EN'!C859,\"\")","v":"B42"},{"$f":"IF(LEN('Translation-EN'!D859)>0,'Translation-EN'!D859,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A860)>0,'Translation-EN'!A860,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B860)>0,'Translation-EN'!B860,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C860)>0,'Translation-EN'!C860,\"\")","v":"A43"},{"$f":"IF(LEN('Translation-EN'!D860)>0,'Translation-EN'!D860,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A861)>0,'Translation-EN'!A861,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B861)>0,'Translation-EN'!B861,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C861)>0,'Translation-EN'!C861,\"\")","v":"A50"},{"$f":"IF(LEN('Translation-EN'!D861)>0,'Translation-EN'!D861,\"\")","v":""},{"$f":"$E$189","v":"BARRE D’ARMATURE"}]
[{"$f":"IF(LEN('Translation-EN'!A862)>0,'Translation-EN'!A862,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B862)>0,'Translation-EN'!B862,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C862)>0,'Translation-EN'!C862,\"\")","v":"D50"},{"$f":"IF(LEN('Translation-EN'!D862)>0,'Translation-EN'!D862,\"\")","v":""},"LONGUEUR ADAPTÉE :"]
[{"$f":"IF(LEN('Translation-EN'!A863)>0,'Translation-EN'!A863,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B863)>0,'Translation-EN'!B863,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C863)>0,'Translation-EN'!C863,\"\")","v":"B51"},{"$f":"IF(LEN('Translation-EN'!D863)>0,'Translation-EN'!D863,\"\")","v":""},{"$f":"$E$191","v":"BARRE D’ARMATURE DE BÉTON"}]
[{"$f":"IF(LEN('Translation-EN'!A864)>0,'Translation-EN'!A864,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B864)>0,'Translation-EN'!B864,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C864)>0,'Translation-EN'!C864,\"\")","v":"A52"},{"$f":"IF(LEN('Translation-EN'!D864)>0,'Translation-EN'!D864,\"\")","v":""},{"$f":"$E$192","v":"Indiquez une longueur totale de barres d’armature."}]
[{"$f":"IF(LEN('Translation-EN'!A865)>0,'Translation-EN'!A865,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B865)>0,'Translation-EN'!B865,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C865)>0,'Translation-EN'!C865,\"\")","v":"A60"},{"$f":"IF(LEN('Translation-EN'!D865)>0,'Translation-EN'!D865,\"\")","v":""},{"$f":"$E$196","v":"PILIERS HÉLIQUES"}]
[{"$f":"IF(LEN('Translation-EN'!A866)>0,'Translation-EN'!A866,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B866)>0,'Translation-EN'!B866,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C866)>0,'Translation-EN'!C866,\"\")","v":"D60"},{"$f":"IF(LEN('Translation-EN'!D866)>0,'Translation-EN'!D866,\"\")","v":""},{"$f":"$E$197","v":"LA LONGUEUR TOTALE DE TOUS LES PILIERS :"}]
[{"$f":"IF(LEN('Translation-EN'!A867)>0,'Translation-EN'!A867,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B867)>0,'Translation-EN'!B867,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C867)>0,'Translation-EN'!C867,\"\")","v":"B61"},{"$f":"IF(LEN('Translation-EN'!D867)>0,'Translation-EN'!D867,\"\")","v":""},{"$f":"$E$196","v":"PILIERS HÉLIQUES"}]
[{"$f":"IF(LEN('Translation-EN'!A868)>0,'Translation-EN'!A868,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B868)>0,'Translation-EN'!B868,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C868)>0,'Translation-EN'!C868,\"\")","v":"A62"},{"$f":"IF(LEN('Translation-EN'!D868)>0,'Translation-EN'!D868,\"\")","v":""},{"$f":"$E$199","v":"Indiquez la longueur totale de tous les piliers. Utiliser le % pour ajuster les différentes tailles de piliers."}]
[{"$f":"IF(LEN('Translation-EN'!A869)>0,'Translation-EN'!A869,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B869)>0,'Translation-EN'!B869,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C869)>0,'Translation-EN'!C869,\"\")","v":"A63"},{"$f":"IF(LEN('Translation-EN'!D869)>0,'Translation-EN'!D869,\"\")","v":""},"MURS DE FONDATION DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A870)>0,'Translation-EN'!A870,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B870)>0,'Translation-EN'!B870,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C870)>0,'Translation-EN'!C870,\"\")","v":"A64"},{"$f":"IF(LEN('Translation-EN'!D870)>0,'Translation-EN'!D870,\"\")","v":""},"MURS DE FONDATION EN BÉTON"]
[{"$f":"IF(LEN('Translation-EN'!A871)>0,'Translation-EN'!A871,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B871)>0,'Translation-EN'!B871,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C871)>0,'Translation-EN'!C871,\"\")","v":"D64"},{"$f":"IF(LEN('Translation-EN'!D871)>0,'Translation-EN'!D871,\"\")","v":""},{"$f":"$E$179","v":"ÉPAISSEUR :"}]
[{"$f":"IF(LEN('Translation-EN'!A872)>0,'Translation-EN'!A872,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B872)>0,'Translation-EN'!B872,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C872)>0,'Translation-EN'!C872,\"\")","v":"B65"},{"$f":"IF(LEN('Translation-EN'!D872)>0,'Translation-EN'!D872,\"\")","v":""},{"$f":"$E$183","v":"BÉTON –25 MPa ou moins"}]
[{"$f":"IF(LEN('Translation-EN'!A873)>0,'Translation-EN'!A873,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B873)>0,'Translation-EN'!B873,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C873)>0,'Translation-EN'!C873,\"\")","v":"A66"},{"$f":"IF(LEN('Translation-EN'!D873)>0,'Translation-EN'!D873,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A874)>0,'Translation-EN'!A874,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B874)>0,'Translation-EN'!B874,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C874)>0,'Translation-EN'!C874,\"\")","v":"B73"},{"$f":"IF(LEN('Translation-EN'!D874)>0,'Translation-EN'!D874,\"\")","v":""},{"$f":"$E$185","v":"BÉTON –26-30 MPa"}]
[{"$f":"IF(LEN('Translation-EN'!A875)>0,'Translation-EN'!A875,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B875)>0,'Translation-EN'!B875,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C875)>0,'Translation-EN'!C875,\"\")","v":"A74"},{"$f":"IF(LEN('Translation-EN'!D875)>0,'Translation-EN'!D875,\"\")","v":""},{"$f":"$E$184","v":"Les spécifications du mélange de béton font une grande différence dans l’empreinte carbone. Les spécifications du mélange présentées ici peuvent être utilisées pour discuter des options de mélange à faible teneur en carbone avec votre fournisseur."}]
[{"$f":"IF(LEN('Translation-EN'!A876)>0,'Translation-EN'!A876,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B876)>0,'Translation-EN'!B876,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C876)>0,'Translation-EN'!C876,\"\")","v":"A81"},{"$f":"IF(LEN('Translation-EN'!D876)>0,'Translation-EN'!D876,\"\")","v":""},"MURS DE FONDATION EN EMB"]
[{"$f":"IF(LEN('Translation-EN'!A877)>0,'Translation-EN'!A877,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B877)>0,'Translation-EN'!B877,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C877)>0,'Translation-EN'!C877,\"\")","v":"B82"},{"$f":"IF(LEN('Translation-EN'!D877)>0,'Translation-EN'!D877,\"\")","v":""},{"$f":"$E$259","v":"ÉLÉMENTS DE MAÇONNERIE EN BÉTON"}]
[{"$f":"IF(LEN('Translation-EN'!A878)>0,'Translation-EN'!A878,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B878)>0,'Translation-EN'!B878,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C878)>0,'Translation-EN'!C878,\"\")","v":"A83"},{"$f":"IF(LEN('Translation-EN'!D878)>0,'Translation-EN'!D878,\"\")","v":""},"Si un coulis de béton est utilisé dans le mur en EMB, utilisez la zone du mur en béton pour spécifier la quantité de remplissage en béton utilisée dans les EMB."]
[{"$f":"IF(LEN('Translation-EN'!A879)>0,'Translation-EN'!A879,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B879)>0,'Translation-EN'!B879,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C879)>0,'Translation-EN'!C879,\"\")","v":"C83"},{"$f":"IF(LEN('Translation-EN'!D879)>0,'Translation-EN'!D879,\"\")","v":""},"Murs en EMB 8 po creux, sans coulis – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A880)>0,'Translation-EN'!A880,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B880)>0,'Translation-EN'!B880,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C880)>0,'Translation-EN'!C880,\"\")","v":"A90"},{"$f":"IF(LEN('Translation-EN'!D880)>0,'Translation-EN'!D880,\"\")","v":""},"ÉLÉMENTS STRUCTURELS LOURDS DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A881)>0,'Translation-EN'!A881,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B881)>0,'Translation-EN'!B881,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C881)>0,'Translation-EN'!C881,\"\")","v":"A91"},{"$f":"IF(LEN('Translation-EN'!D881)>0,'Translation-EN'!D881,\"\")","v":""},"CHARPENTE EN BOIS MASSIF"]
[{"$f":"IF(LEN('Translation-EN'!A882)>0,'Translation-EN'!A882,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B882)>0,'Translation-EN'!B882,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C882)>0,'Translation-EN'!C882,\"\")","v":"B92"},{"$f":"IF(LEN('Translation-EN'!D882)>0,'Translation-EN'!D882,\"\")","v":""},{"$f":"$E$341","v":"BOIS MASSIF"}]
[{"$f":"IF(LEN('Translation-EN'!A883)>0,'Translation-EN'!A883,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B883)>0,'Translation-EN'!B883,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C883)>0,'Translation-EN'!C883,\"\")","v":"A93"},{"$f":"IF(LEN('Translation-EN'!D883)>0,'Translation-EN'!D883,\"\")","v":""},{"$f":"$E$342","v":"Utilisez la fonction % si plusieurs types de bois massifs sont utilisés."}]
[{"$f":"IF(LEN('Translation-EN'!A884)>0,'Translation-EN'!A884,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B884)>0,'Translation-EN'!B884,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C884)>0,'Translation-EN'!C884,\"\")","v":"C93"},{"$f":"IF(LEN('Translation-EN'!D884)>0,'Translation-EN'!D884,\"\")","v":""},{"$f":"$E$343","v":"Charpente lourde en bois – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A885)>0,'Translation-EN'!A885,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B885)>0,'Translation-EN'!B885,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C885)>0,'Translation-EN'!C885,\"\")","v":"A100"},{"$f":"IF(LEN('Translation-EN'!D885)>0,'Translation-EN'!D885,\"\")","v":""},{"$f":"$E$344","v":"COMPOSANTS LOURDS EN ACIER"}]
[{"$f":"IF(LEN('Translation-EN'!A886)>0,'Translation-EN'!A886,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B886)>0,'Translation-EN'!B886,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C886)>0,'Translation-EN'!C886,\"\")","v":"B101"},{"$f":"IF(LEN('Translation-EN'!D886)>0,'Translation-EN'!D886,\"\")","v":""},{"$f":"$E$345","v":"POTEAUX ET POUTRES EN ACIER"}]
[{"$f":"IF(LEN('Translation-EN'!A887)>0,'Translation-EN'!A887,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B887)>0,'Translation-EN'!B887,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C887)>0,'Translation-EN'!C887,\"\")","v":"A102"},{"$f":"IF(LEN('Translation-EN'!D887)>0,'Translation-EN'!D887,\"\")","v":""},"Sélectionnez la section de la poutre en acier dans le menu déroulant et saisissez les mètres linéaires pour chaque type de composant, car les valeurs ne proviennent pas de la feuille de saisie de l’utilisateur."]
[{"$f":"IF(LEN('Translation-EN'!A888)>0,'Translation-EN'!A888,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B888)>0,'Translation-EN'!B888,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C888)>0,'Translation-EN'!C888,\"\")","v":"C102"},{"$f":"IF(LEN('Translation-EN'!D888)>0,'Translation-EN'!D888,\"\")","v":""},{"$f":"$E$347","v":"Poutre en acier section W – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A889)>0,'Translation-EN'!A889,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B889)>0,'Translation-EN'!B889,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C889)>0,'Translation-EN'!C889,\"\")","v":"A105"},{"$f":"IF(LEN('Translation-EN'!D889)>0,'Translation-EN'!D889,\"\")","v":""},"MURS EXTÉRIEURS DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A890)>0,'Translation-EN'!A890,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B890)>0,'Translation-EN'!B890,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C890)>0,'Translation-EN'!C890,\"\")","v":"A106"},{"$f":"IF(LEN('Translation-EN'!D890)>0,'Translation-EN'!D890,\"\")","v":""},{"$f":"$E$298","v":"CONSTRUCTION EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A891)>0,'Translation-EN'!A891,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B891)>0,'Translation-EN'!B891,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C891)>0,'Translation-EN'!C891,\"\")","v":"D106"},{"$f":"IF(LEN('Translation-EN'!D891)>0,'Translation-EN'!D891,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A892)>0,'Translation-EN'!A892,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B892)>0,'Translation-EN'!B892,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C892)>0,'Translation-EN'!C892,\"\")","v":"B107"},{"$f":"IF(LEN('Translation-EN'!D892)>0,'Translation-EN'!D892,\"\")","v":""},{"$f":"$E$298","v":"CONSTRUCTION EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A893)>0,'Translation-EN'!A893,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B893)>0,'Translation-EN'!B893,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C893)>0,'Translation-EN'!C893,\"\")","v":"B111"},{"$f":"IF(LEN('Translation-EN'!D893)>0,'Translation-EN'!D893,\"\")","v":""},{"$f":"$E$299","v":"2x4 double"}]
[{"$f":"IF(LEN('Translation-EN'!A894)>0,'Translation-EN'!A894,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B894)>0,'Translation-EN'!B894,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C894)>0,'Translation-EN'!C894,\"\")","v":"A112"},{"$f":"IF(LEN('Translation-EN'!D894)>0,'Translation-EN'!D894,\"\")","v":""},{"$f":"$E$642","v":"CONSTRUCTION À CHARPENTE EN ACIER"}]
[{"$f":"IF(LEN('Translation-EN'!A895)>0,'Translation-EN'!A895,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B895)>0,'Translation-EN'!B895,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C895)>0,'Translation-EN'!C895,\"\")","v":"D112"},{"$f":"IF(LEN('Translation-EN'!D895)>0,'Translation-EN'!D895,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A896)>0,'Translation-EN'!A896,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B896)>0,'Translation-EN'!B896,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C896)>0,'Translation-EN'!C896,\"\")","v":"B113"},{"$f":"IF(LEN('Translation-EN'!D896)>0,'Translation-EN'!D896,\"\")","v":""},{"$f":"$E$372","v":"CHARPENTE D’ACIER, 2x6"}]
[{"$f":"IF(LEN('Translation-EN'!A897)>0,'Translation-EN'!A897,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B897)>0,'Translation-EN'!B897,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C897)>0,'Translation-EN'!C897,\"\")","v":"A114"},{"$f":"IF(LEN('Translation-EN'!D897)>0,'Translation-EN'!D897,\"\")","v":""},{"$f":"$E$494","v":"Utilisez la fonction % pour vous adapter aux autres calibres des goujons en acier."}]
[{"$f":"IF(LEN('Translation-EN'!A898)>0,'Translation-EN'!A898,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B898)>0,'Translation-EN'!B898,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C898)>0,'Translation-EN'!C898,\"\")","v":"C114"},{"$f":"IF(LEN('Translation-EN'!D898)>0,'Translation-EN'!D898,\"\")","v":""},{"$f":"$E$374","v":"Charpente en acier – porteur – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A899)>0,'Translation-EN'!A899,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B899)>0,'Translation-EN'!B899,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C899)>0,'Translation-EN'!C899,\"\")","v":"B120"},{"$f":"IF(LEN('Translation-EN'!D899)>0,'Translation-EN'!D899,\"\")","v":""},{"$f":"$E$302","v":"CHARPENTE D’ACIER, 2x4"}]
[{"$f":"IF(LEN('Translation-EN'!A900)>0,'Translation-EN'!A900,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B900)>0,'Translation-EN'!B900,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C900)>0,'Translation-EN'!C900,\"\")","v":"C121"},{"$f":"IF(LEN('Translation-EN'!D900)>0,'Translation-EN'!D900,\"\")","v":""},{"$f":"$E$491","v":"Charpente en acier – murs intérieurs – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A901)>0,'Translation-EN'!A901,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B901)>0,'Translation-EN'!B901,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C901)>0,'Translation-EN'!C901,\"\")","v":"A122"},{"$f":"IF(LEN('Translation-EN'!D901)>0,'Translation-EN'!D901,\"\")","v":""},{"$f":"$E$492","v":"Utilisez la fonction % pour vous adapter aux différents calibres des goujons en acier."}]
[{"$f":"IF(LEN('Translation-EN'!A902)>0,'Translation-EN'!A902,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B902)>0,'Translation-EN'!B902,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C902)>0,'Translation-EN'!C902,\"\")","v":"A127"},{"$f":"IF(LEN('Translation-EN'!D902)>0,'Translation-EN'!D902,\"\")","v":""},{"$f":"$E$393","v":"PANNEAUX STRUCTURAUX"}]
[{"$f":"IF(LEN('Translation-EN'!A903)>0,'Translation-EN'!A903,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B903)>0,'Translation-EN'!B903,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C903)>0,'Translation-EN'!C903,\"\")","v":"B128"},{"$f":"IF(LEN('Translation-EN'!D903)>0,'Translation-EN'!D903,\"\")","v":""},{"$f":"$E$394","v":"PANNEAU À COPEAUX ORIENTÉS"}]
[{"$f":"IF(LEN('Translation-EN'!A904)>0,'Translation-EN'!A904,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B904)>0,'Translation-EN'!B904,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C904)>0,'Translation-EN'!C904,\"\")","v":"B133"},{"$f":"IF(LEN('Translation-EN'!D904)>0,'Translation-EN'!D904,\"\")","v":""},{"$f":"$E$395","v":"CONTREPLAQUÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A905)>0,'Translation-EN'!A905,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B905)>0,'Translation-EN'!B905,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C905)>0,'Translation-EN'!C905,\"\")","v":"B137"},{"$f":"IF(LEN('Translation-EN'!D905)>0,'Translation-EN'!D905,\"\")","v":""},{"$f":"$E$396","v":"PANNEAUX STRUCTURAUX EN GYPSE"}]
[{"$f":"IF(LEN('Translation-EN'!A906)>0,'Translation-EN'!A906,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B906)>0,'Translation-EN'!B906,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C906)>0,'Translation-EN'!C906,\"\")","v":"A141"},{"$f":"IF(LEN('Translation-EN'!D906)>0,'Translation-EN'!D906,\"\")","v":""},"MURS EXTÉRIEURS EN EMB"]
[{"$f":"IF(LEN('Translation-EN'!A907)>0,'Translation-EN'!A907,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B907)>0,'Translation-EN'!B907,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C907)>0,'Translation-EN'!C907,\"\")","v":"B142"},{"$f":"IF(LEN('Translation-EN'!D907)>0,'Translation-EN'!D907,\"\")","v":""},"EMB DE 8 po"]
[{"$f":"IF(LEN('Translation-EN'!A908)>0,'Translation-EN'!A908,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B908)>0,'Translation-EN'!B908,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C908)>0,'Translation-EN'!C908,\"\")","v":"C143"},{"$f":"IF(LEN('Translation-EN'!D908)>0,'Translation-EN'!D908,\"\")","v":""},"Éléments de maçonnerie en béton (EMB) – MOYENNE"]
[{"$f":"IF(LEN('Translation-EN'!A909)>0,'Translation-EN'!A909,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B909)>0,'Translation-EN'!B909,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C909)>0,'Translation-EN'!C909,\"\")","v":"A144"},{"$f":"IF(LEN('Translation-EN'!D909)>0,'Translation-EN'!D909,\"\")","v":""},{"$f":"$E$500","v":"Utilisez la fonction % pour régler d’autres épaisseurs de EMB."}]
[{"$f":"IF(LEN('Translation-EN'!A910)>0,'Translation-EN'!A910,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B910)>0,'Translation-EN'!B910,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C910)>0,'Translation-EN'!C910,\"\")","v":"A150"},{"$f":"IF(LEN('Translation-EN'!D910)>0,'Translation-EN'!D910,\"\")","v":""},"ISOLATION DE LA CAVITÉ D’UN MUR DE GARAGE EXTÉRIEUR"]
[{"$f":"IF(LEN('Translation-EN'!A911)>0,'Translation-EN'!A911,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B911)>0,'Translation-EN'!B911,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C911)>0,'Translation-EN'!C911,\"\")","v":"G150"},{"$f":"IF(LEN('Translation-EN'!D911)>0,'Translation-EN'!D911,\"\")","v":""},"(Ne comprend pas la surface du mur d’attache, spécifiée séparément dans la section ci-dessous)"]
[{"$f":"IF(LEN('Translation-EN'!A912)>0,'Translation-EN'!A912,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B912)>0,'Translation-EN'!B912,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C912)>0,'Translation-EN'!C912,\"\")","v":"B151"},{"$f":"IF(LEN('Translation-EN'!D912)>0,'Translation-EN'!D912,\"\")","v":""},{"$f":"$E$307","v":"NATTE DE FIBRE DE VERRE"}]
[{"$f":"IF(LEN('Translation-EN'!A913)>0,'Translation-EN'!A913,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B913)>0,'Translation-EN'!B913,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C913)>0,'Translation-EN'!C913,\"\")","v":"C152"},{"$f":"IF(LEN('Translation-EN'!D913)>0,'Translation-EN'!D913,\"\")","v":""},{"$f":"$E$400","v":"Natte en fibre de verre – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A914)>0,'Translation-EN'!A914,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B914)>0,'Translation-EN'!B914,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C914)>0,'Translation-EN'!C914,\"\")","v":"B156"},{"$f":"IF(LEN('Translation-EN'!D914)>0,'Translation-EN'!D914,\"\")","v":""},{"$f":"$E$401","v":"FIBRE DE VERRE SOUFFLÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A915)>0,'Translation-EN'!A915,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B915)>0,'Translation-EN'!B915,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C915)>0,'Translation-EN'!C915,\"\")","v":"C157"},{"$f":"IF(LEN('Translation-EN'!D915)>0,'Translation-EN'!D915,\"\")","v":""},{"$f":"$E$402","v":"Fibre de verre en vrac – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A916)>0,'Translation-EN'!A916,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B916)>0,'Translation-EN'!B916,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C916)>0,'Translation-EN'!C916,\"\")","v":"B162"},{"$f":"IF(LEN('Translation-EN'!D916)>0,'Translation-EN'!D916,\"\")","v":""},{"$f":"$E$311","v":"NATTE DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A917)>0,'Translation-EN'!A917,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B917)>0,'Translation-EN'!B917,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C917)>0,'Translation-EN'!C917,\"\")","v":"B170"},{"$f":"IF(LEN('Translation-EN'!D917)>0,'Translation-EN'!D917,\"\")","v":""},{"$f":"$E$309","v":"ISOLATION EN CELLULOSE"}]
[{"$f":"IF(LEN('Translation-EN'!A918)>0,'Translation-EN'!A918,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B918)>0,'Translation-EN'!B918,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C918)>0,'Translation-EN'!C918,\"\")","v":"C171"},{"$f":"IF(LEN('Translation-EN'!D918)>0,'Translation-EN'!D918,\"\")","v":""},{"$f":"$E$405","v":"Cellulose – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A919)>0,'Translation-EN'!A919,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B919)>0,'Translation-EN'!B919,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C919)>0,'Translation-EN'!C919,\"\")","v":"B175"},{"$f":"IF(LEN('Translation-EN'!D919)>0,'Translation-EN'!D919,\"\")","v":""},{"$f":"$E$313","v":"NATTE DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A920)>0,'Translation-EN'!A920,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B920)>0,'Translation-EN'!B920,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C920)>0,'Translation-EN'!C920,\"\")","v":"C176"},{"$f":"IF(LEN('Translation-EN'!D920)>0,'Translation-EN'!D920,\"\")","v":""},{"$f":"$E$407","v":"Natte de fibres de bois – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A921)>0,'Translation-EN'!A921,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B921)>0,'Translation-EN'!B921,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C921)>0,'Translation-EN'!C921,\"\")","v":"B181"},{"$f":"IF(LEN('Translation-EN'!D921)>0,'Translation-EN'!D921,\"\")","v":""},{"$f":"$E$408","v":"AUTRES ISOLANTS EN FIBRES NATURELLES"}]
[{"$f":"IF(LEN('Translation-EN'!A922)>0,'Translation-EN'!A922,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B922)>0,'Translation-EN'!B922,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C922)>0,'Translation-EN'!C922,\"\")","v":"B187"},{"$f":"IF(LEN('Translation-EN'!D922)>0,'Translation-EN'!D922,\"\")","v":""},{"$f":"$E$409","v":"MOUSSE À PULVÉRISER – CELLULE FERMÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A923)>0,'Translation-EN'!A923,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B923)>0,'Translation-EN'!B923,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C923)>0,'Translation-EN'!C923,\"\")","v":"B191"},{"$f":"IF(LEN('Translation-EN'!D923)>0,'Translation-EN'!D923,\"\")","v":""},{"$f":"$E$410","v":"MOUSSE À PULVÉRISER – CELLULE OUVERTE"}]
[{"$f":"IF(LEN('Translation-EN'!A924)>0,'Translation-EN'!A924,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B924)>0,'Translation-EN'!B924,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C924)>0,'Translation-EN'!C924,\"\")","v":"B194"},{"$f":"IF(LEN('Translation-EN'!D924)>0,'Translation-EN'!D924,\"\")","v":""},{"$f":"$E$411","v":"BRIQUES DE CHANVRE"}]
[{"$f":"IF(LEN('Translation-EN'!A925)>0,'Translation-EN'!A925,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B925)>0,'Translation-EN'!B925,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C925)>0,'Translation-EN'!C925,\"\")","v":"C195"},{"$f":"IF(LEN('Translation-EN'!D925)>0,'Translation-EN'!D925,\"\")","v":""},{"$f":"$E$412","v":"Briques de chanvre – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A926)>0,'Translation-EN'!A926,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B926)>0,'Translation-EN'!B926,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C926)>0,'Translation-EN'!C926,\"\")","v":"A199"},{"$f":"IF(LEN('Translation-EN'!D926)>0,'Translation-EN'!D926,\"\")","v":""},"ISOLATION RIGIDE DU MUR EXTÉRIEUR DE GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A927)>0,'Translation-EN'!A927,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B927)>0,'Translation-EN'!B927,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C927)>0,'Translation-EN'!C927,\"\")","v":"G199"},{"$f":"IF(LEN('Translation-EN'!D927)>0,'Translation-EN'!D927,\"\")","v":""},"(Ne comprend pas la zone du mur d’attache)"]
[{"$f":"IF(LEN('Translation-EN'!A928)>0,'Translation-EN'!A928,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B928)>0,'Translation-EN'!B928,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C928)>0,'Translation-EN'!C928,\"\")","v":"B200"},{"$f":"IF(LEN('Translation-EN'!D928)>0,'Translation-EN'!D928,\"\")","v":""},{"$f":"$E$211","v":"PANNEAU DE MOUSSE EPS"}]
[{"$f":"IF(LEN('Translation-EN'!A929)>0,'Translation-EN'!A929,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B929)>0,'Translation-EN'!B929,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C929)>0,'Translation-EN'!C929,\"\")","v":"C201"},{"$f":"IF(LEN('Translation-EN'!D929)>0,'Translation-EN'!D929,\"\")","v":""},{"$f":"$E$212","v":"Panneau de mousse EPS – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A930)>0,'Translation-EN'!A930,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B930)>0,'Translation-EN'!B930,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C930)>0,'Translation-EN'!C930,\"\")","v":"B204"},{"$f":"IF(LEN('Translation-EN'!D930)>0,'Translation-EN'!D930,\"\")","v":""},{"$f":"$E$270","v":"PANNEAU DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A931)>0,'Translation-EN'!A931,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B931)>0,'Translation-EN'!B931,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C931)>0,'Translation-EN'!C931,\"\")","v":"C205"},{"$f":"IF(LEN('Translation-EN'!D931)>0,'Translation-EN'!D931,\"\")","v":""},{"$f":"$E$271","v":"Panneau de fibres de bois – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A932)>0,'Translation-EN'!A932,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B932)>0,'Translation-EN'!B932,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C932)>0,'Translation-EN'!C932,\"\")","v":"B211"},{"$f":"IF(LEN('Translation-EN'!D932)>0,'Translation-EN'!D932,\"\")","v":""},{"$f":"$E$213","v":"PANNEAU DE MOUSSE XPS"}]
[{"$f":"IF(LEN('Translation-EN'!A933)>0,'Translation-EN'!A933,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B933)>0,'Translation-EN'!B933,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C933)>0,'Translation-EN'!C933,\"\")","v":"C212"},{"$f":"IF(LEN('Translation-EN'!D933)>0,'Translation-EN'!D933,\"\")","v":""},{"$f":"$E$214","v":"Panneau de mousse XPS – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A934)>0,'Translation-EN'!A934,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B934)>0,'Translation-EN'!B934,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C934)>0,'Translation-EN'!C934,\"\")","v":"B217"},{"$f":"IF(LEN('Translation-EN'!D934)>0,'Translation-EN'!D934,\"\")","v":""},{"$f":"$E$420","v":"PANNEAU DE MOUSSE POLYISOCYANURATE"}]
[{"$f":"IF(LEN('Translation-EN'!A935)>0,'Translation-EN'!A935,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B935)>0,'Translation-EN'!B935,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C935)>0,'Translation-EN'!C935,\"\")","v":"C218"},{"$f":"IF(LEN('Translation-EN'!D935)>0,'Translation-EN'!D935,\"\")","v":""},{"$f":"$E$421","v":"Polyisocyanurate – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A936)>0,'Translation-EN'!A936,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B936)>0,'Translation-EN'!B936,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C936)>0,'Translation-EN'!C936,\"\")","v":"B223"},{"$f":"IF(LEN('Translation-EN'!D936)>0,'Translation-EN'!D936,\"\")","v":""},{"$f":"$E$215","v":"PANNEAU DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A937)>0,'Translation-EN'!A937,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B937)>0,'Translation-EN'!B937,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C937)>0,'Translation-EN'!C937,\"\")","v":"C224"},{"$f":"IF(LEN('Translation-EN'!D937)>0,'Translation-EN'!D937,\"\")","v":""},{"$f":"$E$423","v":"Panneau de laine minérale – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A938)>0,'Translation-EN'!A938,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B938)>0,'Translation-EN'!B938,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C938)>0,'Translation-EN'!C938,\"\")","v":"A228"},{"$f":"IF(LEN('Translation-EN'!D938)>0,'Translation-EN'!D938,\"\")","v":""},"ISOLATION DES MURS DE L’ANNEXE DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A939)>0,'Translation-EN'!A939,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B939)>0,'Translation-EN'!B939,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C939)>0,'Translation-EN'!C939,\"\")","v":"A229"},{"$f":"IF(LEN('Translation-EN'!D939)>0,'Translation-EN'!D939,\"\")","v":""},"ISOLATION DES CAVITÉS DES MURS DE L’ANNEXE DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A940)>0,'Translation-EN'!A940,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B940)>0,'Translation-EN'!B940,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C940)>0,'Translation-EN'!C940,\"\")","v":"B230"},{"$f":"IF(LEN('Translation-EN'!D940)>0,'Translation-EN'!D940,\"\")","v":""},{"$f":"$E$307","v":"NATTE DE FIBRE DE VERRE"}]
[{"$f":"IF(LEN('Translation-EN'!A941)>0,'Translation-EN'!A941,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B941)>0,'Translation-EN'!B941,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C941)>0,'Translation-EN'!C941,\"\")","v":"C231"},{"$f":"IF(LEN('Translation-EN'!D941)>0,'Translation-EN'!D941,\"\")","v":""},{"$f":"$E$400","v":"Natte en fibre de verre – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A942)>0,'Translation-EN'!A942,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B942)>0,'Translation-EN'!B942,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C942)>0,'Translation-EN'!C942,\"\")","v":"B235"},{"$f":"IF(LEN('Translation-EN'!D942)>0,'Translation-EN'!D942,\"\")","v":""},{"$f":"$E$401","v":"FIBRE DE VERRE SOUFFLÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A943)>0,'Translation-EN'!A943,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B943)>0,'Translation-EN'!B943,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C943)>0,'Translation-EN'!C943,\"\")","v":"C236"},{"$f":"IF(LEN('Translation-EN'!D943)>0,'Translation-EN'!D943,\"\")","v":""},{"$f":"$E$402","v":"Fibre de verre en vrac – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A944)>0,'Translation-EN'!A944,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B944)>0,'Translation-EN'!B944,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C944)>0,'Translation-EN'!C944,\"\")","v":"B241"},{"$f":"IF(LEN('Translation-EN'!D944)>0,'Translation-EN'!D944,\"\")","v":""},{"$f":"$E$311","v":"NATTE DE LAINE MINÉRALE"}]
[{"$f":"IF(LEN('Translation-EN'!A945)>0,'Translation-EN'!A945,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B945)>0,'Translation-EN'!B945,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C945)>0,'Translation-EN'!C945,\"\")","v":"B249"},{"$f":"IF(LEN('Translation-EN'!D945)>0,'Translation-EN'!D945,\"\")","v":""},{"$f":"$E$309","v":"ISOLATION EN CELLULOSE"}]
[{"$f":"IF(LEN('Translation-EN'!A946)>0,'Translation-EN'!A946,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B946)>0,'Translation-EN'!B946,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C946)>0,'Translation-EN'!C946,\"\")","v":"C250"},{"$f":"IF(LEN('Translation-EN'!D946)>0,'Translation-EN'!D946,\"\")","v":""},{"$f":"$E$405","v":"Cellulose – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A947)>0,'Translation-EN'!A947,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B947)>0,'Translation-EN'!B947,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C947)>0,'Translation-EN'!C947,\"\")","v":"B254"},{"$f":"IF(LEN('Translation-EN'!D947)>0,'Translation-EN'!D947,\"\")","v":""},{"$f":"$E$313","v":"NATTE DE FIBRES DE BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A948)>0,'Translation-EN'!A948,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B948)>0,'Translation-EN'!B948,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C948)>0,'Translation-EN'!C948,\"\")","v":"C255"},{"$f":"IF(LEN('Translation-EN'!D948)>0,'Translation-EN'!D948,\"\")","v":""},{"$f":"$E$407","v":"Natte de fibres de bois – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A949)>0,'Translation-EN'!A949,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B949)>0,'Translation-EN'!B949,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C949)>0,'Translation-EN'!C949,\"\")","v":"B260"},{"$f":"IF(LEN('Translation-EN'!D949)>0,'Translation-EN'!D949,\"\")","v":""},{"$f":"$E$408","v":"AUTRES ISOLANTS EN FIBRES NATURELLES"}]
[{"$f":"IF(LEN('Translation-EN'!A950)>0,'Translation-EN'!A950,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B950)>0,'Translation-EN'!B950,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C950)>0,'Translation-EN'!C950,\"\")","v":"B266"},{"$f":"IF(LEN('Translation-EN'!D950)>0,'Translation-EN'!D950,\"\")","v":""},{"$f":"$E$409","v":"MOUSSE À PULVÉRISER – CELLULE FERMÉE"}]
[{"$f":"IF(LEN('Translation-EN'!A951)>0,'Translation-EN'!A951,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B951)>0,'Translation-EN'!B951,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C951)>0,'Translation-EN'!C951,\"\")","v":"B270"},{"$f":"IF(LEN('Translation-EN'!D951)>0,'Translation-EN'!D951,\"\")","v":""},{"$f":"$E$410","v":"MOUSSE À PULVÉRISER – CELLULE OUVERTE"}]
[{"$f":"IF(LEN('Translation-EN'!A952)>0,'Translation-EN'!A952,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B952)>0,'Translation-EN'!B952,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C952)>0,'Translation-EN'!C952,\"\")","v":"B273"},{"$f":"IF(LEN('Translation-EN'!D952)>0,'Translation-EN'!D952,\"\")","v":""},{"$f":"$E$411","v":"BRIQUES DE CHANVRE"}]
[{"$f":"IF(LEN('Translation-EN'!A953)>0,'Translation-EN'!A953,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B953)>0,'Translation-EN'!B953,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C953)>0,'Translation-EN'!C953,\"\")","v":"C274"},{"$f":"IF(LEN('Translation-EN'!D953)>0,'Translation-EN'!D953,\"\")","v":""},{"$f":"$E$412","v":"Briques de chanvre – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A954)>0,'Translation-EN'!A954,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B954)>0,'Translation-EN'!B954,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C954)>0,'Translation-EN'!C954,\"\")","v":"A278"},{"$f":"IF(LEN('Translation-EN'!D954)>0,'Translation-EN'!D954,\"\")","v":""},"REVÊTEMENT DE GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A955)>0,'Translation-EN'!A955,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B955)>0,'Translation-EN'!B955,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C955)>0,'Translation-EN'!C955,\"\")","v":"A279"},{"$f":"IF(LEN('Translation-EN'!D955)>0,'Translation-EN'!D955,\"\")","v":""},{"$f":"$E$583","v":"BARDAGE EXTÉRIEUR"}]
[{"$f":"IF(LEN('Translation-EN'!A956)>0,'Translation-EN'!A956,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B956)>0,'Translation-EN'!B956,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C956)>0,'Translation-EN'!C956,\"\")","v":"B280"},{"$f":"IF(LEN('Translation-EN'!D956)>0,'Translation-EN'!D956,\"\")","v":""},{"$f":"$E$584","v":"BRIQUE"}]
[{"$f":"IF(LEN('Translation-EN'!A957)>0,'Translation-EN'!A957,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B957)>0,'Translation-EN'!B957,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C957)>0,'Translation-EN'!C957,\"\")","v":"B288"},{"$f":"IF(LEN('Translation-EN'!D957)>0,'Translation-EN'!D957,\"\")","v":""},{"$f":"$E$585","v":"BARDAGE EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A958)>0,'Translation-EN'!A958,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B958)>0,'Translation-EN'!B958,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C958)>0,'Translation-EN'!C958,\"\")","v":"B291"},{"$f":"IF(LEN('Translation-EN'!D958)>0,'Translation-EN'!D958,\"\")","v":""},{"$f":"$E$586","v":"FIBROCIMENT"}]
[{"$f":"IF(LEN('Translation-EN'!A959)>0,'Translation-EN'!A959,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B959)>0,'Translation-EN'!B959,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C959)>0,'Translation-EN'!C959,\"\")","v":"C292"},{"$f":"IF(LEN('Translation-EN'!D959)>0,'Translation-EN'!D959,\"\")","v":""},{"$f":"$E$587","v":"Bardage en fibrociment – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A960)>0,'Translation-EN'!A960,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B960)>0,'Translation-EN'!B960,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C960)>0,'Translation-EN'!C960,\"\")","v":"B301"},{"$f":"IF(LEN('Translation-EN'!D960)>0,'Translation-EN'!D960,\"\")","v":""},{"$f":"$E$588","v":"REVÊTEMENT EN VINYLE"}]
[{"$f":"IF(LEN('Translation-EN'!A961)>0,'Translation-EN'!A961,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B961)>0,'Translation-EN'!B961,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C961)>0,'Translation-EN'!C961,\"\")","v":"B303"},{"$f":"IF(LEN('Translation-EN'!D961)>0,'Translation-EN'!D961,\"\")","v":""},{"$f":"$E$589","v":"REVÊTEMENT EN POLYPROPYLÈNE"}]
[{"$f":"IF(LEN('Translation-EN'!A962)>0,'Translation-EN'!A962,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B962)>0,'Translation-EN'!B962,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C962)>0,'Translation-EN'!C962,\"\")","v":"C304"},{"$f":"IF(LEN('Translation-EN'!D962)>0,'Translation-EN'!D962,\"\")","v":""},{"$f":"$E$590","v":"Revêtement en polypropylène – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A963)>0,'Translation-EN'!A963,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B963)>0,'Translation-EN'!B963,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C963)>0,'Translation-EN'!C963,\"\")","v":"B307"},{"$f":"IF(LEN('Translation-EN'!D963)>0,'Translation-EN'!D963,\"\")","v":""},{"$f":"$E$591","v":"BARDAGE EN PANNEAUX D’ACIER"}]
[{"$f":"IF(LEN('Translation-EN'!A964)>0,'Translation-EN'!A964,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B964)>0,'Translation-EN'!B964,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C964)>0,'Translation-EN'!C964,\"\")","v":"C308"},{"$f":"IF(LEN('Translation-EN'!D964)>0,'Translation-EN'!D964,\"\")","v":""},{"$f":"$E$592","v":"Bardage en panneaux d’acier – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A965)>0,'Translation-EN'!A965,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B965)>0,'Translation-EN'!B965,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C965)>0,'Translation-EN'!C965,\"\")","v":"B315"},{"$f":"IF(LEN('Translation-EN'!D965)>0,'Translation-EN'!D965,\"\")","v":""},{"$f":"$E$593","v":"BARDAGE EN PANNEAUX D’ALUMINIUM"}]
[{"$f":"IF(LEN('Translation-EN'!A966)>0,'Translation-EN'!A966,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B966)>0,'Translation-EN'!B966,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C966)>0,'Translation-EN'!C966,\"\")","v":"C316"},{"$f":"IF(LEN('Translation-EN'!D966)>0,'Translation-EN'!D966,\"\")","v":""},{"$f":"$E$594","v":"Bardage en panneaux d’aluminium – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A967)>0,'Translation-EN'!A967,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B967)>0,'Translation-EN'!B967,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C967)>0,'Translation-EN'!C967,\"\")","v":"B319"},{"$f":"IF(LEN('Translation-EN'!D967)>0,'Translation-EN'!D967,\"\")","v":""},{"$f":"$E$595","v":"FINITIONS EN PLÂTRE"}]
[{"$f":"IF(LEN('Translation-EN'!A968)>0,'Translation-EN'!A968,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B968)>0,'Translation-EN'!B968,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C968)>0,'Translation-EN'!C968,\"\")","v":"B324"},{"$f":"IF(LEN('Translation-EN'!D968)>0,'Translation-EN'!D968,\"\")","v":""},{"$f":"$E$596","v":"BARDAGE EN BOIS D'INGÉNIERIE"}]
[{"$f":"IF(LEN('Translation-EN'!A969)>0,'Translation-EN'!A969,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B969)>0,'Translation-EN'!B969,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C969)>0,'Translation-EN'!C969,\"\")","v":"A328"},{"$f":"IF(LEN('Translation-EN'!D969)>0,'Translation-EN'!D969,\"\")","v":""},{"$f":"$E$597","v":"Tasseau pour écran de pluie"}]
[{"$f":"IF(LEN('Translation-EN'!A970)>0,'Translation-EN'!A970,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B970)>0,'Translation-EN'!B970,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C970)>0,'Translation-EN'!C970,\"\")","v":"D328"},{"$f":"IF(LEN('Translation-EN'!D970)>0,'Translation-EN'!D970,\"\")","v":""},{"$f":"$E$598","v":"ESPACEMENT DES TASSEAUX"}]
[{"$f":"IF(LEN('Translation-EN'!A971)>0,'Translation-EN'!A971,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B971)>0,'Translation-EN'!B971,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C971)>0,'Translation-EN'!C971,\"\")","v":"A331"},{"$f":"IF(LEN('Translation-EN'!D971)>0,'Translation-EN'!D971,\"\")","v":""},"REVÊTEMENT INTÉRIEUR pour les MURS DE GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A972)>0,'Translation-EN'!A972,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B972)>0,'Translation-EN'!B972,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C972)>0,'Translation-EN'!C972,\"\")","v":"B332"},{"$f":"IF(LEN('Translation-EN'!D972)>0,'Translation-EN'!D972,\"\")","v":""},{"$f":"$E$320","v":"CLOISONS SÈCHES 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A973)>0,'Translation-EN'!A973,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B973)>0,'Translation-EN'!B973,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C973)>0,'Translation-EN'!C973,\"\")","v":"C333"},{"$f":"IF(LEN('Translation-EN'!D973)>0,'Translation-EN'!D973,\"\")","v":""},{"$f":"$E$537","v":"Cloison sèche 1/2 po typique – Revêtement intérieur pour murs extérieurs - MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A974)>0,'Translation-EN'!A974,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B974)>0,'Translation-EN'!B974,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C974)>0,'Translation-EN'!C974,\"\")","v":"B339"},{"$f":"IF(LEN('Translation-EN'!D974)>0,'Translation-EN'!D974,\"\")","v":""},{"$f":"$E$322","v":"CLOISONS SÈCHES 5/8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A975)>0,'Translation-EN'!A975,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B975)>0,'Translation-EN'!B975,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C975)>0,'Translation-EN'!C975,\"\")","v":"B343"},{"$f":"IF(LEN('Translation-EN'!D975)>0,'Translation-EN'!D975,\"\")","v":""},{"$f":"$E$323","v":"AUTRES MATÉRIAUX DE BARDAGE"}]
[{"$f":"IF(LEN('Translation-EN'!A976)>0,'Translation-EN'!A976,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B976)>0,'Translation-EN'!B976,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C976)>0,'Translation-EN'!C976,\"\")","v":"A354"},{"$f":"IF(LEN('Translation-EN'!D976)>0,'Translation-EN'!D976,\"\")","v":""},"FENÊTRES DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A977)>0,'Translation-EN'!A977,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B977)>0,'Translation-EN'!B977,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C977)>0,'Translation-EN'!C977,\"\")","v":"A355"},{"$f":"IF(LEN('Translation-EN'!D977)>0,'Translation-EN'!D977,\"\")","v":""},{"$f":"$E$620","v":"FENÊTRES À DOUBLE VITRAGE"}]
[{"$f":"IF(LEN('Translation-EN'!A978)>0,'Translation-EN'!A978,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B978)>0,'Translation-EN'!B978,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C978)>0,'Translation-EN'!C978,\"\")","v":"A362"},{"$f":"IF(LEN('Translation-EN'!D978)>0,'Translation-EN'!D978,\"\")","v":""},{"$f":"$E$622","v":"FENÊTRES – FABRICANTS SPÉCIFIQUES"}]
[{"$f":"IF(LEN('Translation-EN'!A979)>0,'Translation-EN'!A979,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B979)>0,'Translation-EN'!B979,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C979)>0,'Translation-EN'!C979,\"\")","v":"A366"},{"$f":"IF(LEN('Translation-EN'!D979)>0,'Translation-EN'!D979,\"\")","v":""},"PLAFOND DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A980)>0,'Translation-EN'!A980,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B980)>0,'Translation-EN'!B980,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C980)>0,'Translation-EN'!C980,\"\")","v":"A367"},{"$f":"IF(LEN('Translation-EN'!D980)>0,'Translation-EN'!D980,\"\")","v":""},"REVÊTEMENT DU PLAFOND DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A981)>0,'Translation-EN'!A981,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B981)>0,'Translation-EN'!B981,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C981)>0,'Translation-EN'!C981,\"\")","v":"B368"},{"$f":"IF(LEN('Translation-EN'!D981)>0,'Translation-EN'!D981,\"\")","v":""},{"$f":"$E$320","v":"CLOISONS SÈCHES 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A982)>0,'Translation-EN'!A982,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B982)>0,'Translation-EN'!B982,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C982)>0,'Translation-EN'!C982,\"\")","v":"C369"},{"$f":"IF(LEN('Translation-EN'!D982)>0,'Translation-EN'!D982,\"\")","v":""},{"$f":"$E$746","v":"Cloison sèche 1/2 po – Plafonds – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A983)>0,'Translation-EN'!A983,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B983)>0,'Translation-EN'!B983,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C983)>0,'Translation-EN'!C983,\"\")","v":"B375"},{"$f":"IF(LEN('Translation-EN'!D983)>0,'Translation-EN'!D983,\"\")","v":""},{"$f":"$E$322","v":"CLOISONS SÈCHES 5/8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A984)>0,'Translation-EN'!A984,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B984)>0,'Translation-EN'!B984,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C984)>0,'Translation-EN'!C984,\"\")","v":"C376"},{"$f":"IF(LEN('Translation-EN'!D984)>0,'Translation-EN'!D984,\"\")","v":""},{"$f":"$E$748","v":"Cloison sèche 5/8 po – Plafonds – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A985)>0,'Translation-EN'!A985,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B985)>0,'Translation-EN'!B985,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C985)>0,'Translation-EN'!C985,\"\")","v":"B380"},{"$f":"IF(LEN('Translation-EN'!D985)>0,'Translation-EN'!D985,\"\")","v":""},{"$f":"$E$749","v":"AUTRES FINIS DE PLAFOND"}]
[{"$f":"IF(LEN('Translation-EN'!A986)>0,'Translation-EN'!A986,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B986)>0,'Translation-EN'!B986,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C986)>0,'Translation-EN'!C986,\"\")","v":"A387"},{"$f":"IF(LEN('Translation-EN'!D986)>0,'Translation-EN'!D986,\"\")","v":""},"TOIT DU GARAGE"]
[{"$f":"IF(LEN('Translation-EN'!A987)>0,'Translation-EN'!A987,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B987)>0,'Translation-EN'!B987,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C987)>0,'Translation-EN'!C987,\"\")","v":"A388"},{"$f":"IF(LEN('Translation-EN'!D987)>0,'Translation-EN'!D987,\"\")","v":""},{"$f":"$E$298","v":"CONSTRUCTION EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A988)>0,'Translation-EN'!A988,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B988)>0,'Translation-EN'!B988,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C988)>0,'Translation-EN'!C988,\"\")","v":"D388"},{"$f":"IF(LEN('Translation-EN'!D988)>0,'Translation-EN'!D988,\"\")","v":""},{"$f":"$E$297","v":"L’ESPACEMENT DES CHARPENTES :"}]
[{"$f":"IF(LEN('Translation-EN'!A989)>0,'Translation-EN'!A989,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B989)>0,'Translation-EN'!B989,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C989)>0,'Translation-EN'!C989,\"\")","v":"B389"},{"$f":"IF(LEN('Translation-EN'!D989)>0,'Translation-EN'!D989,\"\")","v":""},{"$f":"$E$768","v":"CHARPENTE EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A990)>0,'Translation-EN'!A990,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B990)>0,'Translation-EN'!B990,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C990)>0,'Translation-EN'!C990,\"\")","v":"B395"},{"$f":"IF(LEN('Translation-EN'!D990)>0,'Translation-EN'!D990,\"\")","v":""},{"$f":"$E$688","v":"CHARPENTE À TREILLIS EN BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A991)>0,'Translation-EN'!A991,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B991)>0,'Translation-EN'!B991,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C991)>0,'Translation-EN'!C991,\"\")","v":"B397"},{"$f":"IF(LEN('Translation-EN'!D991)>0,'Translation-EN'!D991,\"\")","v":""},{"$f":"$E$686","v":"CHARPENTE EN BOIS DE TYPE SOLIVE-I"}]
[{"$f":"IF(LEN('Translation-EN'!A992)>0,'Translation-EN'!A992,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B992)>0,'Translation-EN'!B992,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C992)>0,'Translation-EN'!C992,\"\")","v":"A402"},{"$f":"IF(LEN('Translation-EN'!D992)>0,'Translation-EN'!D992,\"\")","v":""},{"$f":"$E$772","v":"TERRASSE EN TOITURE"}]
[{"$f":"IF(LEN('Translation-EN'!A993)>0,'Translation-EN'!A993,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B993)>0,'Translation-EN'!B993,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C993)>0,'Translation-EN'!C993,\"\")","v":"B403"},{"$f":"IF(LEN('Translation-EN'!D993)>0,'Translation-EN'!D993,\"\")","v":""},{"$f":"$E$773","v":"PRODUITS EN FEUILLE DE BOIS –5/8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A994)>0,'Translation-EN'!A994,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B994)>0,'Translation-EN'!B994,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C994)>0,'Translation-EN'!C994,\"\")","v":"B406"},{"$f":"IF(LEN('Translation-EN'!D994)>0,'Translation-EN'!D994,\"\")","v":""},{"$f":"$E$774","v":"PANNEAUX DE GYPSE 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A995)>0,'Translation-EN'!A995,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B995)>0,'Translation-EN'!B995,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C995)>0,'Translation-EN'!C995,\"\")","v":"A410"},{"$f":"IF(LEN('Translation-EN'!D995)>0,'Translation-EN'!D995,\"\")","v":""},{"$f":"$E$775","v":"MEMBRANE DE TOITURE"}]
[{"$f":"IF(LEN('Translation-EN'!A996)>0,'Translation-EN'!A996,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B996)>0,'Translation-EN'!B996,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C996)>0,'Translation-EN'!C996,\"\")","v":"B411"},{"$f":"IF(LEN('Translation-EN'!D996)>0,'Translation-EN'!D996,\"\")","v":""},{"$f":"$E$775","v":"MEMBRANE DE TOITURE"}]
[{"$f":"IF(LEN('Translation-EN'!A997)>0,'Translation-EN'!A997,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B997)>0,'Translation-EN'!B997,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C997)>0,'Translation-EN'!C997,\"\")","v":"A416"},{"$f":"IF(LEN('Translation-EN'!D997)>0,'Translation-EN'!D997,\"\")","v":""},{"$f":"$E$777","v":"GRADATION DE LA TOITURE"}]
[{"$f":"IF(LEN('Translation-EN'!A998)>0,'Translation-EN'!A998,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B998)>0,'Translation-EN'!B998,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C998)>0,'Translation-EN'!C998,\"\")","v":"D416"},{"$f":"IF(LEN('Translation-EN'!D998)>0,'Translation-EN'!D998,\"\")","v":""},{"$f":"$E$598","v":"ESPACEMENT DES TASSEAUX"}]
[{"$f":"IF(LEN('Translation-EN'!A999)>0,'Translation-EN'!A999,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B999)>0,'Translation-EN'!B999,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C999)>0,'Translation-EN'!C999,\"\")","v":"B417"},{"$f":"IF(LEN('Translation-EN'!D999)>0,'Translation-EN'!D999,\"\")","v":""},{"$f":"$E$779","v":"GRADATION DU BOIS"}]
[{"$f":"IF(LEN('Translation-EN'!A1000)>0,'Translation-EN'!A1000,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1000)>0,'Translation-EN'!B1000,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C1000)>0,'Translation-EN'!C1000,\"\")","v":"A421"},{"$f":"IF(LEN('Translation-EN'!D1000)>0,'Translation-EN'!D1000,\"\")","v":""},{"$f":"$E$780","v":"TOITURE"}]
[{"$f":"IF(LEN('Translation-EN'!A1001)>0,'Translation-EN'!A1001,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1001)>0,'Translation-EN'!B1001,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C1001)>0,'Translation-EN'!C1001,\"\")","v":"B422"},{"$f":"IF(LEN('Translation-EN'!D1001)>0,'Translation-EN'!D1001,\"\")","v":""},{"$f":"$E$781","v":"BARDEAUX D’ASPHALTE"}]
[{"$f":"IF(LEN('Translation-EN'!A1002)>0,'Translation-EN'!A1002,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1002)>0,'Translation-EN'!B1002,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C1002)>0,'Translation-EN'!C1002,\"\")","v":"C423"},{"$f":"IF(LEN('Translation-EN'!D1002)>0,'Translation-EN'!D1002,\"\")","v":""},{"$f":"$E$782","v":"Bardeaux d’asphalte – Toitures – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A1003)>0,'Translation-EN'!A1003,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1003)>0,'Translation-EN'!B1003,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C1003)>0,'Translation-EN'!C1003,\"\")","v":"B430"},{"$f":"IF(LEN('Translation-EN'!D1003)>0,'Translation-EN'!D1003,\"\")","v":""},{"$f":"$E$783","v":"PLAQUE DE TOITURE D’ACIER"}]
[{"$f":"IF(LEN('Translation-EN'!A1004)>0,'Translation-EN'!A1004,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1004)>0,'Translation-EN'!B1004,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C1004)>0,'Translation-EN'!C1004,\"\")","v":"C431"},{"$f":"IF(LEN('Translation-EN'!D1004)>0,'Translation-EN'!D1004,\"\")","v":""},{"$f":"$E$784","v":"Plaque de toiture d’acier – toiture – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A1005)>0,'Translation-EN'!A1005,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1005)>0,'Translation-EN'!B1005,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C1005)>0,'Translation-EN'!C1005,\"\")","v":"B437"},{"$f":"IF(LEN('Translation-EN'!D1005)>0,'Translation-EN'!D1005,\"\")","v":""},{"$f":"$E$785","v":"PLAQUE DE TOITURE D'ALUMINIUM"}]
[{"$f":"IF(LEN('Translation-EN'!A1006)>0,'Translation-EN'!A1006,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1006)>0,'Translation-EN'!B1006,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C1006)>0,'Translation-EN'!C1006,\"\")","v":"C438"},{"$f":"IF(LEN('Translation-EN'!D1006)>0,'Translation-EN'!D1006,\"\")","v":""},{"$f":"$E$786","v":"Bardage en plaque d’aluminium – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A1007)>0,'Translation-EN'!A1007,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1007)>0,'Translation-EN'!B1007,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C1007)>0,'Translation-EN'!C1007,\"\")","v":"B441"},{"$f":"IF(LEN('Translation-EN'!D1007)>0,'Translation-EN'!D1007,\"\")","v":""},{"$f":"$E$787","v":"TOITURE EN FIBROCIMENT"}]
[{"$f":"IF(LEN('Translation-EN'!A1008)>0,'Translation-EN'!A1008,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1008)>0,'Translation-EN'!B1008,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C1008)>0,'Translation-EN'!C1008,\"\")","v":"C442"},{"$f":"IF(LEN('Translation-EN'!D1008)>0,'Translation-EN'!D1008,\"\")","v":""},{"$f":"$E$788","v":"Bardage en fibrociment – MOYENNE"}]
[{"$f":"IF(LEN('Translation-EN'!A1009)>0,'Translation-EN'!A1009,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1009)>0,'Translation-EN'!B1009,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C1009)>0,'Translation-EN'!C1009,\"\")","v":"B446"},{"$f":"IF(LEN('Translation-EN'!D1009)>0,'Translation-EN'!D1009,\"\")","v":""},{"$f":"$E$789","v":"AUTRES OPTIONS DE TOITURE"}]
[{"$f":"IF(LEN('Translation-EN'!A1010)>0,'Translation-EN'!A1010,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1010)>0,'Translation-EN'!B1010,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1010)>0,'Translation-EN'!C1010,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D1010)>0,'Translation-EN'!D1010,\"\")","v":""},"SECTION 14 ➜ COMPOSANTS ET MATÉRIAUX POUR LES"]
[{"$f":"IF(LEN('Translation-EN'!A1011)>0,'Translation-EN'!A1011,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1011)>0,'Translation-EN'!B1011,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1011)>0,'Translation-EN'!C1011,\"\")","v":"E1"},{"$f":"IF(LEN('Translation-EN'!D1011)>0,'Translation-EN'!D1011,\"\")","v":""},"MATÉRIAUX DÉFINIS PAR L’UTILISATEUR"]
[{"$f":"IF(LEN('Translation-EN'!A1012)>0,'Translation-EN'!A1012,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1012)>0,'Translation-EN'!B1012,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1012)>0,'Translation-EN'!C1012,\"\")","v":"B2"},{"$f":"IF(LEN('Translation-EN'!D1012)>0,'Translation-EN'!D1012,\"\")","v":true},"INSTRUCTIONS POUR L'UTILISATION D'UN MATÉRIEL DE BASE DE DONNÉES EXISTANT :         << double-cliquer >>\n- Sélectionner le matériel à partir de la cellule ayant le MENU DÉROULANT JAUNE PÂLE (colonne C) qui correspond à l'unité de mesure du matériel (volume, aire, longueur ou valeur R et aire)\n- Entrez tous les renseignements requis dans les cellules JAUNE FONCÉ pour cette ligne, y compris « 1 »dans la colonne de sélection.\n- Si vous ajoutez de l'isolation, entrer sa VALEUR R (unités I-P) totale dans la colonne B, et l'aire de surface dans la colonne D.\n"]
[{"$f":"IF(LEN('Translation-EN'!A1013)>0,'Translation-EN'!A1013,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1013)>0,'Translation-EN'!B1013,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1013)>0,'Translation-EN'!C1013,\"\")","v":"F2"},{"$f":"IF(LEN('Translation-EN'!D1013)>0,'Translation-EN'!D1013,\"\")","v":true},"INSTRUCTIONS POUR AJOUTER UN MATÉRIAU QUI NE FIGURE PAS DANS LA BASE DE DONNÉES :\n(l'utilisateur doit avoir tous les renseignements requis en main)\nDans une ligne dont la catégorie est PERSONNALISÉ, ENTREZ LES DONNÉES REQUISES dans tous les champs JAUNE FONCÉ (CATÉGORIE, MATÉRIAU, QUANTITÉ, UNITÉ, % D'ÉMISSIONS KGCO2e, STOCKAGE DE kgCO2e).\n- Utilisez uniquement les valeurs A1-A3  des DEP.\n- Le fait de changer le nom de la catégorie ne déplace pas l'entrée vers un autre total de section de bâtiment."]
[{"$f":"IF(LEN('Translation-EN'!A1014)>0,'Translation-EN'!A1014,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1014)>0,'Translation-EN'!B1014,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1014)>0,'Translation-EN'!C1014,\"\")","v":"N2"},{"$f":"IF(LEN('Translation-EN'!D1014)>0,'Translation-EN'!D1014,\"\")","v":true},"Mise en garde : Toute option définie par l'utilisateur qui n'a pas été validée et approuvée réduira la fiabilité des résultats."]
[{"$f":"IF(LEN('Translation-EN'!A1015)>0,'Translation-EN'!A1015,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1015)>0,'Translation-EN'!B1015,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1015)>0,'Translation-EN'!C1015,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D1015)>0,'Translation-EN'!D1015,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A1016)>0,'Translation-EN'!A1016,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1016)>0,'Translation-EN'!B1016,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1016)>0,'Translation-EN'!C1016,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D1016)>0,'Translation-EN'!D1016,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A1017)>0,'Translation-EN'!A1017,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1017)>0,'Translation-EN'!B1017,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1017)>0,'Translation-EN'!C1017,\"\")","v":"E3"},{"$f":"IF(LEN('Translation-EN'!D1017)>0,'Translation-EN'!D1017,\"\")","v":""},{"$f":"$E$122","v":"QUANTITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A1018)>0,'Translation-EN'!A1018,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1018)>0,'Translation-EN'!B1018,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1018)>0,'Translation-EN'!C1018,\"\")","v":"F3"},{"$f":"IF(LEN('Translation-EN'!D1018)>0,'Translation-EN'!D1018,\"\")","v":""},{"$f":"$E$72","v":"UNITÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A1019)>0,'Translation-EN'!A1019,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1019)>0,'Translation-EN'!B1019,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1019)>0,'Translation-EN'!C1019,\"\")","v":"I3"},{"$f":"IF(LEN('Translation-EN'!D1019)>0,'Translation-EN'!D1019,\"\")","v":""},{"$f":"$E$168","v":" SÉLECTIONNER"}]
[{"$f":"IF(LEN('Translation-EN'!A1020)>0,'Translation-EN'!A1020,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1020)>0,'Translation-EN'!B1020,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1020)>0,'Translation-EN'!C1020,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D1020)>0,'Translation-EN'!D1020,\"\")","v":true},{"$f":"$E$169","v":"ÉMISSIONS NETTES kgCO2e"}]
[{"$f":"IF(LEN('Translation-EN'!A1021)>0,'Translation-EN'!A1021,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1021)>0,'Translation-EN'!B1021,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C1021)>0,'Translation-EN'!C1021,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D1021)>0,'Translation-EN'!D1021,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A1022)>0,'Translation-EN'!A1022,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1022)>0,'Translation-EN'!B1022,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1022)>0,'Translation-EN'!C1022,\"\")","v":"K3"},{"$f":"IF(LEN('Translation-EN'!D1022)>0,'Translation-EN'!D1022,\"\")","v":true},{"$f":"$E$171","v":"CONTENU DE kgCO2e DANS LE MATÉRIAU SÉLECTIONNÉ"}]
[{"$f":"IF(LEN('Translation-EN'!A1023)>0,'Translation-EN'!A1023,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1023)>0,'Translation-EN'!B1023,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C1023)>0,'Translation-EN'!C1023,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D1023)>0,'Translation-EN'!D1023,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A1024)>0,'Translation-EN'!A1024,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1024)>0,'Translation-EN'!B1024,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1024)>0,'Translation-EN'!C1024,\"\")","v":"L3"},{"$f":"IF(LEN('Translation-EN'!D1024)>0,'Translation-EN'!D1024,\"\")","v":true},{"$f":"$E$173","v":"ÉMISSIONS EN kgCO2e "}]
[{"$f":"IF(LEN('Translation-EN'!A1025)>0,'Translation-EN'!A1025,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1025)>0,'Translation-EN'!B1025,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C1025)>0,'Translation-EN'!C1025,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D1025)>0,'Translation-EN'!D1025,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A1026)>0,'Translation-EN'!A1026,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1026)>0,'Translation-EN'!B1026,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1026)>0,'Translation-EN'!C1026,\"\")","v":"M3"},{"$f":"IF(LEN('Translation-EN'!D1026)>0,'Translation-EN'!D1026,\"\")","v":true},{"$f":"$E$175","v":"STOCKAGE EN kgCO2"}]
[{"$f":"IF(LEN('Translation-EN'!A1027)>0,'Translation-EN'!A1027,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1027)>0,'Translation-EN'!B1027,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C1027)>0,'Translation-EN'!C1027,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!D1027)>0,'Translation-EN'!D1027,\"\")","v":""}]
[{"$f":"IF(LEN('Translation-EN'!A1028)>0,'Translation-EN'!A1028,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1028)>0,'Translation-EN'!B1028,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1028)>0,'Translation-EN'!C1028,\"\")","v":"N3"},{"$f":"IF(LEN('Translation-EN'!D1028)>0,'Translation-EN'!D1028,\"\")","v":true},"TOTAL PARTIEL POUR LES MATÉRIAUX DÉFINIS PAR L’UTILISATEUR kgCO2e"]
[{"$f":"IF(LEN('Translation-EN'!A1029)>0,'Translation-EN'!A1029,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1029)>0,'Translation-EN'!B1029,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1029)>0,'Translation-EN'!C1029,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D1029)>0,'Translation-EN'!D1029,\"\")","v":""},"MATÉRIAUX DE LA BASE DE DONNÉES EXISTANTE"]
[{"$f":"IF(LEN('Translation-EN'!A1030)>0,'Translation-EN'!A1030,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1030)>0,'Translation-EN'!B1030,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1030)>0,'Translation-EN'!C1030,\"\")","v":"C6"},{"$f":"IF(LEN('Translation-EN'!D1030)>0,'Translation-EN'!D1030,\"\")","v":""},"MATÉRIAUX PAR VOLUME"]
[{"$f":"IF(LEN('Translation-EN'!A1031)>0,'Translation-EN'!A1031,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1031)>0,'Translation-EN'!B1031,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1031)>0,'Translation-EN'!C1031,\"\")","v":"B7"},{"$f":"IF(LEN('Translation-EN'!D1031)>0,'Translation-EN'!D1031,\"\")","v":""},"VOLUME"]
[{"$f":"IF(LEN('Translation-EN'!A1032)>0,'Translation-EN'!A1032,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1032)>0,'Translation-EN'!B1032,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1032)>0,'Translation-EN'!C1032,\"\")","v":"B8"},{"$f":"IF(LEN('Translation-EN'!D1032)>0,'Translation-EN'!D1032,\"\")","v":""},{"$f":"$E$1031","v":"VOLUME"}]
[{"$f":"IF(LEN('Translation-EN'!A1033)>0,'Translation-EN'!A1033,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1033)>0,'Translation-EN'!B1033,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1033)>0,'Translation-EN'!C1033,\"\")","v":"B9"},{"$f":"IF(LEN('Translation-EN'!D1033)>0,'Translation-EN'!D1033,\"\")","v":""},{"$f":"$E$1031","v":"VOLUME"}]
[{"$f":"IF(LEN('Translation-EN'!A1034)>0,'Translation-EN'!A1034,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1034)>0,'Translation-EN'!B1034,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1034)>0,'Translation-EN'!C1034,\"\")","v":"C10"},{"$f":"IF(LEN('Translation-EN'!D1034)>0,'Translation-EN'!D1034,\"\")","v":""},"MATÉRIAUX PAR SURFACE"]
[{"$f":"IF(LEN('Translation-EN'!A1035)>0,'Translation-EN'!A1035,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1035)>0,'Translation-EN'!B1035,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1035)>0,'Translation-EN'!C1035,\"\")","v":"B11"},{"$f":"IF(LEN('Translation-EN'!D1035)>0,'Translation-EN'!D1035,\"\")","v":""},"SURFACE"]
[{"$f":"IF(LEN('Translation-EN'!A1036)>0,'Translation-EN'!A1036,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1036)>0,'Translation-EN'!B1036,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1036)>0,'Translation-EN'!C1036,\"\")","v":"B12"},{"$f":"IF(LEN('Translation-EN'!D1036)>0,'Translation-EN'!D1036,\"\")","v":""},{"$f":"$E$1035","v":"SURFACE"}]
[{"$f":"IF(LEN('Translation-EN'!A1037)>0,'Translation-EN'!A1037,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1037)>0,'Translation-EN'!B1037,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1037)>0,'Translation-EN'!C1037,\"\")","v":"B13"},{"$f":"IF(LEN('Translation-EN'!D1037)>0,'Translation-EN'!D1037,\"\")","v":""},{"$f":"$E$1035","v":"SURFACE"}]
[{"$f":"IF(LEN('Translation-EN'!A1038)>0,'Translation-EN'!A1038,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1038)>0,'Translation-EN'!B1038,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1038)>0,'Translation-EN'!C1038,\"\")","v":"C14"},{"$f":"IF(LEN('Translation-EN'!D1038)>0,'Translation-EN'!D1038,\"\")","v":""},"MATÉRIAUX PAR LONGUEUR"]
[{"$f":"IF(LEN('Translation-EN'!A1039)>0,'Translation-EN'!A1039,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1039)>0,'Translation-EN'!B1039,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1039)>0,'Translation-EN'!C1039,\"\")","v":"B15"},{"$f":"IF(LEN('Translation-EN'!D1039)>0,'Translation-EN'!D1039,\"\")","v":""},"LONGUEUR"]
[{"$f":"IF(LEN('Translation-EN'!A1040)>0,'Translation-EN'!A1040,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1040)>0,'Translation-EN'!B1040,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1040)>0,'Translation-EN'!C1040,\"\")","v":"B16"},{"$f":"IF(LEN('Translation-EN'!D1040)>0,'Translation-EN'!D1040,\"\")","v":""},{"$f":"$E$1039","v":"LONGUEUR"}]
[{"$f":"IF(LEN('Translation-EN'!A1041)>0,'Translation-EN'!A1041,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1041)>0,'Translation-EN'!B1041,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1041)>0,'Translation-EN'!C1041,\"\")","v":"B17"},{"$f":"IF(LEN('Translation-EN'!D1041)>0,'Translation-EN'!D1041,\"\")","v":""},{"$f":"$E$1039","v":"LONGUEUR"}]
[{"$f":"IF(LEN('Translation-EN'!A1042)>0,'Translation-EN'!A1042,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1042)>0,'Translation-EN'!B1042,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1042)>0,'Translation-EN'!C1042,\"\")","v":"C18"},{"$f":"IF(LEN('Translation-EN'!D1042)>0,'Translation-EN'!D1042,\"\")","v":""},"MATÉRIAUX PAR SUPERFICIE ET VALEUR R"]
[{"$f":"IF(LEN('Translation-EN'!A1043)>0,'Translation-EN'!A1043,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1043)>0,'Translation-EN'!B1043,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1043)>0,'Translation-EN'!C1043,\"\")","v":"A22"},{"$f":"IF(LEN('Translation-EN'!D1043)>0,'Translation-EN'!D1043,\"\")","v":""},"MATÉRIAUX PERSONNALISÉS DÉFINIS PAR L’UTILISATEUR"]
[{"$f":"IF(LEN('Translation-EN'!A1044)>0,'Translation-EN'!A1044,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1044)>0,'Translation-EN'!B1044,\"\")","v":"_User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1044)>0,'Translation-EN'!C1044,\"\")","v":"B23"},{"$f":"IF(LEN('Translation-EN'!D1044)>0,'Translation-EN'!D1044,\"\")","v":"Ignore this row"},"Bardage"]
[{"$f":"IF(LEN('Translation-EN'!A1045)>0,'Translation-EN'!A1045,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1045)>0,'Translation-EN'!B1045,\"\")","v":"_User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1045)>0,'Translation-EN'!C1045,\"\")","v":"B24"},{"$f":"IF(LEN('Translation-EN'!D1045)>0,'Translation-EN'!D1045,\"\")","v":"Ignore this row"},"Défini par l’utilisateur"]
[{"$f":"IF(LEN('Translation-EN'!A1046)>0,'Translation-EN'!A1046,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1046)>0,'Translation-EN'!B1046,\"\")","v":"_User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1046)>0,'Translation-EN'!C1046,\"\")","v":"B25"},{"$f":"IF(LEN('Translation-EN'!D1046)>0,'Translation-EN'!D1046,\"\")","v":"Ignore this row"},{"$f":"$E$1045","v":"Défini par l’utilisateur"}]
[{"$f":"IF(LEN('Translation-EN'!A1047)>0,'Translation-EN'!A1047,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1047)>0,'Translation-EN'!B1047,\"\")","v":"_User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1047)>0,'Translation-EN'!C1047,\"\")","v":"B26"},{"$f":"IF(LEN('Translation-EN'!D1047)>0,'Translation-EN'!D1047,\"\")","v":"Ignore this row"},{"$f":"$E$1045","v":"Défini par l’utilisateur"}]
[{"$f":"IF(LEN('Translation-EN'!A1048)>0,'Translation-EN'!A1048,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1048)>0,'Translation-EN'!B1048,\"\")","v":"_User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1048)>0,'Translation-EN'!C1048,\"\")","v":"B27"},{"$f":"IF(LEN('Translation-EN'!D1048)>0,'Translation-EN'!D1048,\"\")","v":"Ignore this row"},{"$f":"$E$1045","v":"Défini par l’utilisateur"}]
[{"$f":"IF(LEN('Translation-EN'!A1049)>0,'Translation-EN'!A1049,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1049)>0,'Translation-EN'!B1049,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C1049)>0,'Translation-EN'!C1049,\"\")","v":"B28"},{"$f":"IF(LEN('Translation-EN'!D1049)>0,'Translation-EN'!D1049,\"\")","v":true},"Note : Les matériaux définis par l'utilisateur seront répertoriés séparément dans les rapports de synthèse."]
[{"$f":"IF(LEN('Translation-EN'!A1050)>0,'Translation-EN'!A1050,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1050)>0,'Translation-EN'!B1050,\"\")","v":"REVIEW"},{"$f":"IF(LEN('Translation-EN'!C1050)>0,'Translation-EN'!C1050,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D1050)>0,'Translation-EN'!D1050,\"\")","v":""},"SECTION 12 ➜ EXAMEN"]
[{"$f":"IF(LEN('Translation-EN'!A1051)>0,'Translation-EN'!A1051,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1051)>0,'Translation-EN'!B1051,\"\")","v":"REVIEW"},{"$f":"IF(LEN('Translation-EN'!C1051)>0,'Translation-EN'!C1051,\"\")","v":"C1"},{"$f":"IF(LEN('Translation-EN'!D1051)>0,'Translation-EN'!D1051,\"\")","v":""},"MATÉRIAUX SÉLECTIONNÉS"]
[{"$f":"IF(LEN('Translation-EN'!A1052)>0,'Translation-EN'!A1052,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1052)>0,'Translation-EN'!B1052,\"\")","v":"REVIEW"},{"$f":"IF(LEN('Translation-EN'!C1052)>0,'Translation-EN'!C1052,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D1052)>0,'Translation-EN'!D1052,\"\")","v":""},"SECTION"]
[{"$f":"IF(LEN('Translation-EN'!A1053)>0,'Translation-EN'!A1053,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1053)>0,'Translation-EN'!B1053,\"\")","v":"REVIEW"},{"$f":"IF(LEN('Translation-EN'!C1053)>0,'Translation-EN'!C1053,\"\")","v":"B2"},{"$f":"IF(LEN('Translation-EN'!D1053)>0,'Translation-EN'!D1053,\"\")","v":""},{"$f":"$E$165","v":"CATÉGORIE"}]
[{"$f":"IF(LEN('Translation-EN'!A1054)>0,'Translation-EN'!A1054,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1054)>0,'Translation-EN'!B1054,\"\")","v":"REVIEW"},{"$f":"IF(LEN('Translation-EN'!C1054)>0,'Translation-EN'!C1054,\"\")","v":"C2"},{"$f":"IF(LEN('Translation-EN'!D1054)>0,'Translation-EN'!D1054,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A1055)>0,'Translation-EN'!A1055,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1055)>0,'Translation-EN'!B1055,\"\")","v":"REVIEW"},{"$f":"IF(LEN('Translation-EN'!C1055)>0,'Translation-EN'!C1055,\"\")","v":"D2"},{"$f":"IF(LEN('Translation-EN'!D1055)>0,'Translation-EN'!D1055,\"\")","v":true},"EMPREINTE CARBONE NETTE\n[kg CO2e]"]
[{"$f":"IF(LEN('Translation-EN'!A1056)>0,'Translation-EN'!A1056,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1056)>0,'Translation-EN'!B1056,\"\")","v":"REVIEW"},{"$f":"IF(LEN('Translation-EN'!C1056)>0,'Translation-EN'!C1056,\"\")","v":"E2"},{"$f":"IF(LEN('Translation-EN'!D1056)>0,'Translation-EN'!D1056,\"\")","v":true},"ÉMISSIONS DE CARBONE\n[kg CO2e]"]
[{"$f":"IF(LEN('Translation-EN'!A1057)>0,'Translation-EN'!A1057,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1057)>0,'Translation-EN'!B1057,\"\")","v":"REVIEW"},{"$f":"IF(LEN('Translation-EN'!C1057)>0,'Translation-EN'!C1057,\"\")","v":"F2"},{"$f":"IF(LEN('Translation-EN'!D1057)>0,'Translation-EN'!D1057,\"\")","v":true},"STOCKAGE DE CARBONE\n[kg CO2e]"]
[{"$f":"IF(LEN('Translation-EN'!A1058)>0,'Translation-EN'!A1058,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1058)>0,'Translation-EN'!B1058,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1058)>0,'Translation-EN'!C1058,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D1058)>0,'Translation-EN'!D1058,\"\")","v":""},"Estimateur d'émissions de carbone des matériaux  (E2CM)"]
[{"$f":"IF(LEN('Translation-EN'!A1059)>0,'Translation-EN'!A1059,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1059)>0,'Translation-EN'!B1059,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1059)>0,'Translation-EN'!C1059,\"\")","v":"H2"},{"$f":"IF(LEN('Translation-EN'!D1059)>0,'Translation-EN'!D1059,\"\")","v":""},"Estimations d’émissions de carbone du projet"]
[{"$f":"IF(LEN('Translation-EN'!A1060)>0,'Translation-EN'!A1060,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1060)>0,'Translation-EN'!B1060,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1060)>0,'Translation-EN'!C1060,\"\")","v":"B3"},{"$f":"IF(LEN('Translation-EN'!D1060)>0,'Translation-EN'!D1060,\"\")","v":""},"RÉSUMÉ DU PROJET"]
[{"$f":"IF(LEN('Translation-EN'!A1061)>0,'Translation-EN'!A1061,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1061)>0,'Translation-EN'!B1061,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1061)>0,'Translation-EN'!C1061,\"\")","v":"E5"},{"$f":"IF(LEN('Translation-EN'!D1061)>0,'Translation-EN'!D1061,\"\")","v":""},"Projet :"]
[{"$f":"IF(LEN('Translation-EN'!A1062)>0,'Translation-EN'!A1062,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1062)>0,'Translation-EN'!B1062,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1062)>0,'Translation-EN'!C1062,\"\")","v":"E6"},{"$f":"IF(LEN('Translation-EN'!D1062)>0,'Translation-EN'!D1062,\"\")","v":""},"Évaluateur :"]
[{"$f":"IF(LEN('Translation-EN'!A1063)>0,'Translation-EN'!A1063,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1063)>0,'Translation-EN'!B1063,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1063)>0,'Translation-EN'!C1063,\"\")","v":"E7"},{"$f":"IF(LEN('Translation-EN'!D1063)>0,'Translation-EN'!D1063,\"\")","v":""},"Lieu :"]
[{"$f":"IF(LEN('Translation-EN'!A1064)>0,'Translation-EN'!A1064,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1064)>0,'Translation-EN'!B1064,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1064)>0,'Translation-EN'!C1064,\"\")","v":"E8"},{"$f":"IF(LEN('Translation-EN'!D1064)>0,'Translation-EN'!D1064,\"\")","v":""},"Description de la maison :"]
[{"$f":"IF(LEN('Translation-EN'!A1065)>0,'Translation-EN'!A1065,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1065)>0,'Translation-EN'!B1065,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1065)>0,'Translation-EN'!C1065,\"\")","v":"E9"},{"$f":"IF(LEN('Translation-EN'!D1065)>0,'Translation-EN'!D1065,\"\")","v":""},"Taille du bâtiment :"]
[{"$f":"IF(LEN('Translation-EN'!A1066)>0,'Translation-EN'!A1066,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B1066)>0,'Translation-EN'!B1066,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1066)>0,'Translation-EN'!C1066,\"\")","v":"Rectangle 3"},{"$f":"IF(LEN('Translation-EN'!D1066)>0,'Translation-EN'!D1066,\"\")","v":""},"Photo ou image du projet ici\n(Insérer -> Images) "]
[{"$f":"IF(LEN('Translation-EN'!A1067)>0,'Translation-EN'!A1067,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1067)>0,'Translation-EN'!B1067,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1067)>0,'Translation-EN'!C1067,\"\")","v":"E11"},{"$f":"IF(LEN('Translation-EN'!D1067)>0,'Translation-EN'!D1067,\"\")","v":""},{"$f":"$E$55","v":"Émissions provenant de matériaux"}]
[{"$f":"IF(LEN('Translation-EN'!A1068)>0,'Translation-EN'!A1068,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1068)>0,'Translation-EN'!B1068,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1068)>0,'Translation-EN'!C1068,\"\")","v":"H11"},{"$f":"IF(LEN('Translation-EN'!D1068)>0,'Translation-EN'!D1068,\"\")","v":""},{"$f":"$E$40","v":"Émissions opérationnelles"}]
[{"$f":"IF(LEN('Translation-EN'!A1069)>0,'Translation-EN'!A1069,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1069)>0,'Translation-EN'!B1069,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1069)>0,'Translation-EN'!C1069,\"\")","v":"E12"},{"$f":"IF(LEN('Translation-EN'!D1069)>0,'Translation-EN'!D1069,\"\")","v":true},"tonnes CO2e"]
[{"$f":"IF(LEN('Translation-EN'!A1070)>0,'Translation-EN'!A1070,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1070)>0,'Translation-EN'!B1070,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1070)>0,'Translation-EN'!C1070,\"\")","v":"F12"},{"$f":"IF(LEN('Translation-EN'!D1070)>0,'Translation-EN'!D1070,\"\")","v":true},"kg CO2e / m2"]
[{"$f":"IF(LEN('Translation-EN'!A1071)>0,'Translation-EN'!A1071,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1071)>0,'Translation-EN'!B1071,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1071)>0,'Translation-EN'!C1071,\"\")","v":"H12"},{"$f":"IF(LEN('Translation-EN'!D1071)>0,'Translation-EN'!D1071,\"\")","v":true},"tonnes CO2e / yr"]
[{"$f":"IF(LEN('Translation-EN'!A1072)>0,'Translation-EN'!A1072,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1072)>0,'Translation-EN'!B1072,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1072)>0,'Translation-EN'!C1072,\"\")","v":"I12"},{"$f":"IF(LEN('Translation-EN'!D1072)>0,'Translation-EN'!D1072,\"\")","v":true},"t CO2e / 30 yrs"]
[{"$f":"IF(LEN('Translation-EN'!A1073)>0,'Translation-EN'!A1073,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1073)>0,'Translation-EN'!B1073,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1073)>0,'Translation-EN'!C1073,\"\")","v":"B16"},{"$f":"IF(LEN('Translation-EN'!D1073)>0,'Translation-EN'!D1073,\"\")","v":""},"Notes au projet"]
[{"$f":"IF(LEN('Translation-EN'!A1074)>0,'Translation-EN'!A1074,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1074)>0,'Translation-EN'!B1074,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1074)>0,'Translation-EN'!C1074,\"\")","v":"B17"},{"$f":"IF(LEN('Translation-EN'!D1074)>0,'Translation-EN'!D1074,\"\")","v":""},"Pour cette maison, on vise à atteindre le niveau de performance XYZ..."]
[{"$f":"IF(LEN('Translation-EN'!A1075)>0,'Translation-EN'!A1075,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1075)>0,'Translation-EN'!B1075,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1075)>0,'Translation-EN'!C1075,\"\")","v":"B18"},{"$f":"IF(LEN('Translation-EN'!D1075)>0,'Translation-EN'!D1075,\"\")","v":""},"CALENDRIER D’ÉMISSION DU PROJET"]
[{"$f":"IF(LEN('Translation-EN'!A1076)>0,'Translation-EN'!A1076,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1076)>0,'Translation-EN'!B1076,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1076)>0,'Translation-EN'!C1076,\"\")","v":"B28"},{"$f":"IF(LEN('Translation-EN'!D1076)>0,'Translation-EN'!D1076,\"\")","v":""},"Informations sur le tableau"]
[{"$f":"IF(LEN('Translation-EN'!A1077)>0,'Translation-EN'!A1077,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1077)>0,'Translation-EN'!B1077,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1077)>0,'Translation-EN'!C1077,\"\")","v":"B29"},{"$f":"IF(LEN('Translation-EN'!D1077)>0,'Translation-EN'!D1077,\"\")","v":true},"Note : Dans les réseaux électrique à faible intensité de carbone, les utilisateurs de E2CM devraient envisager des mesures d'efficacité énergétique afin de réduire les charges globales sur les réseaux locaux et régionaux.  \nLe tableau des émissions cumulées de carbone offre une vue simplifiée de l'impact climatique de la fabrication des matériaux et des opérations de construction pour les 30 premières années. Ce tableau doit être utilisé comme un guide pour orienter les efforts de réduction du carbone, plutôt que comme un modèle prédictif des émissions futures. Il existe plusieurs inconnues qui peuvent entraîner des écarts par rapport à ce modèle, dont certaines sont décrites ci-dessous.\n\nNotes sur la simplification des hypothèses\n- Seules les émissions de carbone des matériaux de construction neufs du berceau à la porte sont modélisées. De manière réaliste, il y aurait des fluctuations dans le carbone matériel en raison des rénovations, de l'entretien, de la décomposition du matériel, etc.\n- Les émissions de carbone opérationnelles, la ligne grise, augmentent au même rythme annuel. Cela aussi, en réalité, variera d'une année à l'autre et surtout à mesure que le bâtiment vieillit.\n- Les émissions de GES associées aux combustibles et à la production d'électricité (par province ou territoire) sont des valeurs invariables. On peut raisonnablement s'attendre à ce que ces valeurs évoluent dans le temps."]
[{"$f":"IF(LEN('Translation-EN'!A1078)>0,'Translation-EN'!A1078,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1078)>0,'Translation-EN'!B1078,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1078)>0,'Translation-EN'!C1078,\"\")","v":"B34"},{"$f":"IF(LEN('Translation-EN'!D1078)>0,'Translation-EN'!D1078,\"\")","v":""},"Résultats des émissions de carbone du projet"]
[{"$f":"IF(LEN('Translation-EN'!A1079)>0,'Translation-EN'!A1079,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1079)>0,'Translation-EN'!B1079,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1079)>0,'Translation-EN'!C1079,\"\")","v":"B35"},{"$f":"IF(LEN('Translation-EN'!D1079)>0,'Translation-EN'!D1079,\"\")","v":""},"PAR ÉLÉMENT DE LA MAISON"]
[{"$f":"IF(LEN('Translation-EN'!A1080)>0,'Translation-EN'!A1080,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1080)>0,'Translation-EN'!B1080,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1080)>0,'Translation-EN'!C1080,\"\")","v":"B53"},{"$f":"IF(LEN('Translation-EN'!D1080)>0,'Translation-EN'!D1080,\"\")","v":""},"LES DIX MATÉRIAUX AYANT LE PLUS D’INCIDENCE"]
[{"$f":"IF(LEN('Translation-EN'!A1081)>0,'Translation-EN'!A1081,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1081)>0,'Translation-EN'!B1081,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1081)>0,'Translation-EN'!C1081,\"\")","v":"B55"},{"$f":"IF(LEN('Translation-EN'!D1081)>0,'Translation-EN'!D1081,\"\")","v":""},"Classement"]
[{"$f":"IF(LEN('Translation-EN'!A1082)>0,'Translation-EN'!A1082,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1082)>0,'Translation-EN'!B1082,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1082)>0,'Translation-EN'!C1082,\"\")","v":"C55"},{"$f":"IF(LEN('Translation-EN'!D1082)>0,'Translation-EN'!D1082,\"\")","v":true},"kg CO2e"]
[{"$f":"IF(LEN('Translation-EN'!A1083)>0,'Translation-EN'!A1083,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1083)>0,'Translation-EN'!B1083,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1083)>0,'Translation-EN'!C1083,\"\")","v":"D55"},{"$f":"IF(LEN('Translation-EN'!D1083)>0,'Translation-EN'!D1083,\"\")","v":""},"Section"]
[{"$f":"IF(LEN('Translation-EN'!A1084)>0,'Translation-EN'!A1084,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1084)>0,'Translation-EN'!B1084,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1084)>0,'Translation-EN'!C1084,\"\")","v":"F55"},{"$f":"IF(LEN('Translation-EN'!D1084)>0,'Translation-EN'!D1084,\"\")","v":""},"Matériau"]
[{"$f":"IF(LEN('Translation-EN'!A1085)>0,'Translation-EN'!A1085,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1085)>0,'Translation-EN'!B1085,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1085)>0,'Translation-EN'!C1085,\"\")","v":"B66"},{"$f":"IF(LEN('Translation-EN'!D1085)>0,'Translation-EN'!D1085,\"\")","v":""},"RECOMMANDATIONS"]
[{"$f":"IF(LEN('Translation-EN'!A1086)>0,'Translation-EN'!A1086,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1086)>0,'Translation-EN'!B1086,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1086)>0,'Translation-EN'!C1086,\"\")","v":"B68"},{"$f":"IF(LEN('Translation-EN'!D1086)>0,'Translation-EN'!D1086,\"\")","v":""},"Utilisateur ou conseiller en carbone intrinsèque pour fournir des recommandations ici..."]
[{"$f":"IF(LEN('Translation-EN'!A1087)>0,'Translation-EN'!A1087,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B1087)>0,'Translation-EN'!B1087,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1087)>0,'Translation-EN'!C1087,\"\")","v":"Rounded Rectangle 1"},{"$f":"IF(LEN('Translation-EN'!D1087)>0,'Translation-EN'!D1087,\"\")","v":""},"Enregistrer ce scénario"]
[{"$f":"IF(LEN('Translation-EN'!A1088)>0,'Translation-EN'!A1088,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B1088)>0,'Translation-EN'!B1088,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1088)>0,'Translation-EN'!C1088,\"\")","v":"Group 4,Rectangle 35"},{"$f":"IF(LEN('Translation-EN'!D1088)>0,'Translation-EN'!D1088,\"\")","v":"Shape inside another"},"  Intensité de carbone des matériaux, kg CO2/m2"]
[{"$f":"IF(LEN('Translation-EN'!A1089)>0,'Translation-EN'!A1089,\"\")","v":"Chart"},{"$f":"IF(LEN('Translation-EN'!B1089)>0,'Translation-EN'!B1089,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1089)>0,'Translation-EN'!C1089,\"\")","v":"Chart 9"},{"$f":"IF(LEN('Translation-EN'!D1089)>0,'Translation-EN'!D1089,\"\")","v":"Title"},"Émissions de carbone cumulatives"]
[{"$f":"IF(LEN('Translation-EN'!A1090)>0,'Translation-EN'!A1090,\"\")","v":"Chart"},{"$f":"IF(LEN('Translation-EN'!B1090)>0,'Translation-EN'!B1090,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1090)>0,'Translation-EN'!C1090,\"\")","v":"Chart 9"},{"$f":"IF(LEN('Translation-EN'!D1090)>0,'Translation-EN'!D1090,\"\")","v":"Y-Axis Label"},"Potentiel de réchauffement de la planète (PRP), tonnes CO2e"]
[{"$f":"IF(LEN('Translation-EN'!A1091)>0,'Translation-EN'!A1091,\"\")","v":"Chart"},{"$f":"IF(LEN('Translation-EN'!B1091)>0,'Translation-EN'!B1091,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1091)>0,'Translation-EN'!C1091,\"\")","v":"Chart 9"},{"$f":"IF(LEN('Translation-EN'!D1091)>0,'Translation-EN'!D1091,\"\")","v":"X-Axis Label"},"Années"]
[{"$f":"IF(LEN('Translation-EN'!A1092)>0,'Translation-EN'!A1092,\"\")","v":"Chart"},{"$f":"IF(LEN('Translation-EN'!B1092)>0,'Translation-EN'!B1092,\"\")","v":"RESULTS"},{"$f":"IF(LEN('Translation-EN'!C1092)>0,'Translation-EN'!C1092,\"\")","v":"Chart 42"},{"$f":"IF(LEN('Translation-EN'!D1092)>0,'Translation-EN'!D1092,\"\")","v":"Y-Axis Label"},"Émissions de carbone des matériaux, kg CO2e"]
[{"$f":"IF(LEN('Translation-EN'!A1093)>0,'Translation-EN'!A1093,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B1093)>0,'Translation-EN'!B1093,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1093)>0,'Translation-EN'!C1093,\"\")","v":"btn_reset_1"},{"$f":"IF(LEN('Translation-EN'!D1093)>0,'Translation-EN'!D1093,\"\")","v":""},"Réinitialiser le calculateur"]
[{"$f":"IF(LEN('Translation-EN'!A1094)>0,'Translation-EN'!A1094,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B1094)>0,'Translation-EN'!B1094,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1094)>0,'Translation-EN'!C1094,\"\")","v":"btn_delete_1"},{"$f":"IF(LEN('Translation-EN'!D1094)>0,'Translation-EN'!D1094,\"\")","v":""},"Supprimer le scénario"]
[{"$f":"IF(LEN('Translation-EN'!A1095)>0,'Translation-EN'!A1095,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B1095)>0,'Translation-EN'!B1095,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1095)>0,'Translation-EN'!C1095,\"\")","v":"btn_reset_all"},{"$f":"IF(LEN('Translation-EN'!D1095)>0,'Translation-EN'!D1095,\"\")","v":""},"Recalculer tous les scénarios"]
[{"$f":"IF(LEN('Translation-EN'!A1096)>0,'Translation-EN'!A1096,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1096)>0,'Translation-EN'!B1096,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1096)>0,'Translation-EN'!C1096,\"\")","v":"C2"},{"$f":"IF(LEN('Translation-EN'!D1096)>0,'Translation-EN'!D1096,\"\")","v":""},"Scénarios d’émissions de carbone du projet"]
[{"$f":"IF(LEN('Translation-EN'!A1097)>0,'Translation-EN'!A1097,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1097)>0,'Translation-EN'!B1097,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1097)>0,'Translation-EN'!C1097,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D1097)>0,'Translation-EN'!D1097,\"\")","v":""},"Comment utiliser cet onglet :"]
[{"$f":"IF(LEN('Translation-EN'!A1098)>0,'Translation-EN'!A1098,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1098)>0,'Translation-EN'!B1098,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1098)>0,'Translation-EN'!C1098,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D1098)>0,'Translation-EN'!D1098,\"\")","v":""},"1. Les utilisateurs peuvent enregistrer des scénarios sur cette page afin de comparer les résultats générés par la calculatrice."]
[{"$f":"IF(LEN('Translation-EN'!A1099)>0,'Translation-EN'!A1099,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1099)>0,'Translation-EN'!B1099,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1099)>0,'Translation-EN'!C1099,\"\")","v":"D4"},{"$f":"IF(LEN('Translation-EN'!D1099)>0,'Translation-EN'!D1099,\"\")","v":""},"2. Toutes les données associées aux scénarios sauvegardés peuvent être réintroduites dans la feuille de calcul."]
[{"$f":"IF(LEN('Translation-EN'!A1100)>0,'Translation-EN'!A1100,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1100)>0,'Translation-EN'!B1100,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1100)>0,'Translation-EN'!C1100,\"\")","v":"D5"},{"$f":"IF(LEN('Translation-EN'!D1100)>0,'Translation-EN'!D1100,\"\")","v":""},"3. Pour remplir un scénario dans l’outil d’estimation, les utilisateurs peuvent le sélectionner en cliquant sur le bouton vert intitulé « Calculateur de repos » sur la gauche."]
[{"$f":"IF(LEN('Translation-EN'!A1101)>0,'Translation-EN'!A1101,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1101)>0,'Translation-EN'!B1101,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1101)>0,'Translation-EN'!C1101,\"\")","v":"D6"},{"$f":"IF(LEN('Translation-EN'!D1101)>0,'Translation-EN'!D1101,\"\")","v":""},"4. Les utilisateurs peuvent établir des scénarios personnalisés et les appliquer à différentes maisons en chargeant une nouvelle géométrie dans la FICHE D’ENTRÉE DE L’UTILISATEUR et en cliquant sur le bouton bleu à gauche intitulé « Recalculer tous les scénarios »."]
[{"$f":"IF(LEN('Translation-EN'!A1102)>0,'Translation-EN'!A1102,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1102)>0,'Translation-EN'!B1102,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1102)>0,'Translation-EN'!C1102,\"\")","v":"D7"},{"$f":"IF(LEN('Translation-EN'!D1102)>0,'Translation-EN'!D1102,\"\")","v":""},"5 . Cela permettra de calculer les nouvelles valeurs associées à la géométrie mise à jour pour chaque scénario sauvegardé ci-dessous."]
[{"$f":"IF(LEN('Translation-EN'!A1103)>0,'Translation-EN'!A1103,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1103)>0,'Translation-EN'!B1103,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1103)>0,'Translation-EN'!C1103,\"\")","v":"B10"},{"$f":"IF(LEN('Translation-EN'!D1103)>0,'Translation-EN'!D1103,\"\")","v":""},"Notes"]
[{"$f":"IF(LEN('Translation-EN'!A1104)>0,'Translation-EN'!A1104,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1104)>0,'Translation-EN'!B1104,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1104)>0,'Translation-EN'!C1104,\"\")","v":"B11"},{"$f":"IF(LEN('Translation-EN'!D1104)>0,'Translation-EN'!D1104,\"\")","v":true},"MCE Total (tonnes CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1105)>0,'Translation-EN'!A1105,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1105)>0,'Translation-EN'!B1105,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1105)>0,'Translation-EN'!C1105,\"\")","v":"B12"},{"$f":"IF(LEN('Translation-EN'!D1105)>0,'Translation-EN'!D1105,\"\")","v":true},"Carbone intrinsèque par m2 (kg CO2e / m2)"]
[{"$f":"IF(LEN('Translation-EN'!A1106)>0,'Translation-EN'!A1106,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1106)>0,'Translation-EN'!B1106,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1106)>0,'Translation-EN'!C1106,\"\")","v":"B13"},{"$f":"IF(LEN('Translation-EN'!D1106)>0,'Translation-EN'!D1106,\"\")","v":true},"Semelles et dalles (kg CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1107)>0,'Translation-EN'!A1107,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1107)>0,'Translation-EN'!B1107,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1107)>0,'Translation-EN'!C1107,\"\")","v":"B14"},{"$f":"IF(LEN('Translation-EN'!D1107)>0,'Translation-EN'!D1107,\"\")","v":true},"Murs de fondation (kg CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1108)>0,'Translation-EN'!A1108,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1108)>0,'Translation-EN'!B1108,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1108)>0,'Translation-EN'!C1108,\"\")","v":"B15"},{"$f":"IF(LEN('Translation-EN'!D1108)>0,'Translation-EN'!D1108,\"\")","v":true},"Éléments structurels (kg CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1109)>0,'Translation-EN'!A1109,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1109)>0,'Translation-EN'!B1109,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1109)>0,'Translation-EN'!C1109,\"\")","v":"B16"},{"$f":"IF(LEN('Translation-EN'!D1109)>0,'Translation-EN'!D1109,\"\")","v":true},"Murs extérieurs (kg de CO2e/m2)"]
[{"$f":"IF(LEN('Translation-EN'!A1110)>0,'Translation-EN'!A1110,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1110)>0,'Translation-EN'!B1110,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1110)>0,'Translation-EN'!C1110,\"\")","v":"B17"},{"$f":"IF(LEN('Translation-EN'!D1110)>0,'Translation-EN'!D1110,\"\")","v":true},"Systèmes de murs extérieurs (kg CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1111)>0,'Translation-EN'!A1111,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1111)>0,'Translation-EN'!B1111,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1111)>0,'Translation-EN'!C1111,\"\")","v":"B18"},{"$f":"IF(LEN('Translation-EN'!D1111)>0,'Translation-EN'!D1111,\"\")","v":true},"Murs mitoyens (kg CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1112)>0,'Translation-EN'!A1112,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1112)>0,'Translation-EN'!B1112,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1112)>0,'Translation-EN'!C1112,\"\")","v":"B19"},{"$f":"IF(LEN('Translation-EN'!D1112)>0,'Translation-EN'!D1112,\"\")","v":true},"Bardage (kg de CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1113)>0,'Translation-EN'!A1113,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1113)>0,'Translation-EN'!B1113,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1113)>0,'Translation-EN'!C1113,\"\")","v":"B20"},{"$f":"IF(LEN('Translation-EN'!D1113)>0,'Translation-EN'!D1113,\"\")","v":true},"Fenêtre (kg de CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1114)>0,'Translation-EN'!A1114,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1114)>0,'Translation-EN'!B1114,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1114)>0,'Translation-EN'!C1114,\"\")","v":"B21"},{"$f":"IF(LEN('Translation-EN'!D1114)>0,'Translation-EN'!D1114,\"\")","v":true},"Murs intérieurs (kg CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1115)>0,'Translation-EN'!A1115,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1115)>0,'Translation-EN'!B1115,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1115)>0,'Translation-EN'!C1115,\"\")","v":"B22"},{"$f":"IF(LEN('Translation-EN'!D1115)>0,'Translation-EN'!D1115,\"\")","v":true},"Plancher (kg de CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1116)>0,'Translation-EN'!A1116,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1116)>0,'Translation-EN'!B1116,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1116)>0,'Translation-EN'!C1116,\"\")","v":"B23"},{"$f":"IF(LEN('Translation-EN'!D1116)>0,'Translation-EN'!D1116,\"\")","v":true},"Plafond (kg de CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1117)>0,'Translation-EN'!A1117,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1117)>0,'Translation-EN'!B1117,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1117)>0,'Translation-EN'!C1117,\"\")","v":"B24"},{"$f":"IF(LEN('Translation-EN'!D1117)>0,'Translation-EN'!D1117,\"\")","v":true},"Toit (kg de CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1118)>0,'Translation-EN'!A1118,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1118)>0,'Translation-EN'!B1118,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1118)>0,'Translation-EN'!C1118,\"\")","v":"B25"},{"$f":"IF(LEN('Translation-EN'!D1118)>0,'Translation-EN'!D1118,\"\")","v":true},"Garage (kg de CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1119)>0,'Translation-EN'!A1119,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1119)>0,'Translation-EN'!B1119,\"\")","v":"SCENARIOS"},{"$f":"IF(LEN('Translation-EN'!C1119)>0,'Translation-EN'!C1119,\"\")","v":"B26"},{"$f":"IF(LEN('Translation-EN'!D1119)>0,'Translation-EN'!D1119,\"\")","v":true},"Défini par l’utilisateur (kg CO2e)"]
[{"$f":"IF(LEN('Translation-EN'!A1120)>0,'Translation-EN'!A1120,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1120)>0,'Translation-EN'!B1120,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1120)>0,'Translation-EN'!C1120,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D1120)>0,'Translation-EN'!D1120,\"\")","v":""},"Épaisseur"]
[{"$f":"IF(LEN('Translation-EN'!A1121)>0,'Translation-EN'!A1121,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1121)>0,'Translation-EN'!B1121,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1121)>0,'Translation-EN'!C1121,\"\")","v":"B1"},{"$f":"IF(LEN('Translation-EN'!D1121)>0,'Translation-EN'!D1121,\"\")","v":""},"Espacement"]
[{"$f":"IF(LEN('Translation-EN'!A1122)>0,'Translation-EN'!A1122,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1122)>0,'Translation-EN'!B1122,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1122)>0,'Translation-EN'!C1122,\"\")","v":"C1"},{"$f":"IF(LEN('Translation-EN'!D1122)>0,'Translation-EN'!D1122,\"\")","v":""},"Espacement des solives en acier"]
[{"$f":"IF(LEN('Translation-EN'!A1123)>0,'Translation-EN'!A1123,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1123)>0,'Translation-EN'!B1123,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1123)>0,'Translation-EN'!C1123,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D1123)>0,'Translation-EN'!D1123,\"\")","v":""},"Isolation de la toiture parallèle au..."]
[{"$f":"IF(LEN('Translation-EN'!A1124)>0,'Translation-EN'!A1124,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1124)>0,'Translation-EN'!B1124,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1124)>0,'Translation-EN'!C1124,\"\")","v":"E1"},{"$f":"IF(LEN('Translation-EN'!D1124)>0,'Translation-EN'!D1124,\"\")","v":""},"Options définies par l’utilisateur : VOLUME – m3"]
[{"$f":"IF(LEN('Translation-EN'!A1125)>0,'Translation-EN'!A1125,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1125)>0,'Translation-EN'!B1125,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1125)>0,'Translation-EN'!C1125,\"\")","v":"F1"},{"$f":"IF(LEN('Translation-EN'!D1125)>0,'Translation-EN'!D1125,\"\")","v":""},"Options définies par l’utilisateur : AIRE DE SURFACE – m2"]
[{"$f":"IF(LEN('Translation-EN'!A1126)>0,'Translation-EN'!A1126,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1126)>0,'Translation-EN'!B1126,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1126)>0,'Translation-EN'!C1126,\"\")","v":"G1"},{"$f":"IF(LEN('Translation-EN'!D1126)>0,'Translation-EN'!D1126,\"\")","v":""},"Options définies par l’utilisateur : Longueur – m"]
[{"$f":"IF(LEN('Translation-EN'!A1127)>0,'Translation-EN'!A1127,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1127)>0,'Translation-EN'!B1127,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1127)>0,'Translation-EN'!C1127,\"\")","v":"H1"},{"$f":"IF(LEN('Translation-EN'!D1127)>0,'Translation-EN'!D1127,\"\")","v":""},"Options définies par l’utilisateur : Valeur R et aire – m2 – RTS"]
[{"$f":"IF(LEN('Translation-EN'!A1128)>0,'Translation-EN'!A1128,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1128)>0,'Translation-EN'!B1128,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1128)>0,'Translation-EN'!C1128,\"\")","v":"J1"},{"$f":"IF(LEN('Translation-EN'!D1128)>0,'Translation-EN'!D1128,\"\")","v":""},"O/ N?"]
[{"$f":"IF(LEN('Translation-EN'!A1129)>0,'Translation-EN'!A1129,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1129)>0,'Translation-EN'!B1129,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1129)>0,'Translation-EN'!C1129,\"\")","v":"D2"},{"$f":"IF(LEN('Translation-EN'!D1129)>0,'Translation-EN'!D1129,\"\")","v":""},{"$f":"$E$812","v":"Surface de toit"}]
[{"$f":"IF(LEN('Translation-EN'!A1130)>0,'Translation-EN'!A1130,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1130)>0,'Translation-EN'!B1130,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1130)>0,'Translation-EN'!C1130,\"\")","v":"J2"},{"$f":"IF(LEN('Translation-EN'!D1130)>0,'Translation-EN'!D1130,\"\")","v":""},"Oui"]
[{"$f":"IF(LEN('Translation-EN'!A1131)>0,'Translation-EN'!A1131,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1131)>0,'Translation-EN'!B1131,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1131)>0,'Translation-EN'!C1131,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D1131)>0,'Translation-EN'!D1131,\"\")","v":""},{"$f":"$E$792","v":"Surface du plafond"}]
[{"$f":"IF(LEN('Translation-EN'!A1132)>0,'Translation-EN'!A1132,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1132)>0,'Translation-EN'!B1132,\"\")","v":"Dropdown Lists"},{"$f":"IF(LEN('Translation-EN'!C1132)>0,'Translation-EN'!C1132,\"\")","v":"J3"},{"$f":"IF(LEN('Translation-EN'!D1132)>0,'Translation-EN'!D1132,\"\")","v":""},"Non"]
[{"$f":"IF(LEN('Translation-EN'!A1133)>0,'Translation-EN'!A1133,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1133)>0,'Translation-EN'!B1133,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1133)>0,'Translation-EN'!C1133,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D1133)>0,'Translation-EN'!D1133,\"\")","v":""},{"$f":"$E$1052","v":"SECTION"}]
[{"$f":"IF(LEN('Translation-EN'!A1134)>0,'Translation-EN'!A1134,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1134)>0,'Translation-EN'!B1134,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1134)>0,'Translation-EN'!C1134,\"\")","v":"B1"},{"$f":"IF(LEN('Translation-EN'!D1134)>0,'Translation-EN'!D1134,\"\")","v":""},{"$f":"$E$70","v":"  COMPOSANT"}]
[{"$f":"IF(LEN('Translation-EN'!A1135)>0,'Translation-EN'!A1135,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1135)>0,'Translation-EN'!B1135,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1135)>0,'Translation-EN'!C1135,\"\")","v":"C1"},{"$f":"IF(LEN('Translation-EN'!D1135)>0,'Translation-EN'!D1135,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A1136)>0,'Translation-EN'!A1136,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1136)>0,'Translation-EN'!B1136,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1136)>0,'Translation-EN'!C1136,\"\")","v":"H1"},{"$f":"IF(LEN('Translation-EN'!D1136)>0,'Translation-EN'!D1136,\"\")","v":""},"Articles sélectionnés"]
[{"$f":"IF(LEN('Translation-EN'!A1137)>0,'Translation-EN'!A1137,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1137)>0,'Translation-EN'!B1137,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1137)>0,'Translation-EN'!C1137,\"\")","v":"I1"},{"$f":"IF(LEN('Translation-EN'!D1137)>0,'Translation-EN'!D1137,\"\")","v":""},"CLASSEMENT"]
[{"$f":"IF(LEN('Translation-EN'!A1138)>0,'Translation-EN'!A1138,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1138)>0,'Translation-EN'!B1138,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1138)>0,'Translation-EN'!C1138,\"\")","v":"J1"},{"$f":"IF(LEN('Translation-EN'!D1138)>0,'Translation-EN'!D1138,\"\")","v":""},"CARBONE NET"]
[{"$f":"IF(LEN('Translation-EN'!A1139)>0,'Translation-EN'!A1139,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1139)>0,'Translation-EN'!B1139,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1139)>0,'Translation-EN'!C1139,\"\")","v":"K1"},{"$f":"IF(LEN('Translation-EN'!D1139)>0,'Translation-EN'!D1139,\"\")","v":""},"ONGLET"]
[{"$f":"IF(LEN('Translation-EN'!A1140)>0,'Translation-EN'!A1140,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1140)>0,'Translation-EN'!B1140,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1140)>0,'Translation-EN'!C1140,\"\")","v":"L1"},{"$f":"IF(LEN('Translation-EN'!D1140)>0,'Translation-EN'!D1140,\"\")","v":""},{"$f":"$E$1052","v":"SECTION"}]
[{"$f":"IF(LEN('Translation-EN'!A1141)>0,'Translation-EN'!A1141,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1141)>0,'Translation-EN'!B1141,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1141)>0,'Translation-EN'!C1141,\"\")","v":"M1"},{"$f":"IF(LEN('Translation-EN'!D1141)>0,'Translation-EN'!D1141,\"\")","v":""},{"$f":"$E$166","v":"MATÉRIAU"}]
[{"$f":"IF(LEN('Translation-EN'!A1142)>0,'Translation-EN'!A1142,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1142)>0,'Translation-EN'!B1142,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1142)>0,'Translation-EN'!C1142,\"\")","v":"O1"},{"$f":"IF(LEN('Translation-EN'!D1142)>0,'Translation-EN'!D1142,\"\")","v":""},"Année"]
[{"$f":"IF(LEN('Translation-EN'!A1143)>0,'Translation-EN'!A1143,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1143)>0,'Translation-EN'!B1143,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1143)>0,'Translation-EN'!C1143,\"\")","v":"P1"},{"$f":"IF(LEN('Translation-EN'!D1143)>0,'Translation-EN'!D1143,\"\")","v":""},"Matériaux"]
[{"$f":"IF(LEN('Translation-EN'!A1144)>0,'Translation-EN'!A1144,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1144)>0,'Translation-EN'!B1144,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1144)>0,'Translation-EN'!C1144,\"\")","v":"Q1"},{"$f":"IF(LEN('Translation-EN'!D1144)>0,'Translation-EN'!D1144,\"\")","v":""},"Opérations"]
[{"$f":"IF(LEN('Translation-EN'!A1145)>0,'Translation-EN'!A1145,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1145)>0,'Translation-EN'!B1145,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1145)>0,'Translation-EN'!C1145,\"\")","v":"R1"},{"$f":"IF(LEN('Translation-EN'!D1145)>0,'Translation-EN'!D1145,\"\")","v":""},"Total"]
[{"$f":"IF(LEN('Translation-EN'!A1146)>0,'Translation-EN'!A1146,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1146)>0,'Translation-EN'!B1146,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1146)>0,'Translation-EN'!C1146,\"\")","v":"T3"},{"$f":"IF(LEN('Translation-EN'!D1146)>0,'Translation-EN'!D1146,\"\")","v":""},"Émissions"]
[{"$f":"IF(LEN('Translation-EN'!A1147)>0,'Translation-EN'!A1147,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1147)>0,'Translation-EN'!B1147,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1147)>0,'Translation-EN'!C1147,\"\")","v":"U3"},{"$f":"IF(LEN('Translation-EN'!D1147)>0,'Translation-EN'!D1147,\"\")","v":""},"Barre d’émissions"]
[{"$f":"IF(LEN('Translation-EN'!A1148)>0,'Translation-EN'!A1148,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1148)>0,'Translation-EN'!B1148,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1148)>0,'Translation-EN'!C1148,\"\")","v":"V3"},{"$f":"IF(LEN('Translation-EN'!D1148)>0,'Translation-EN'!D1148,\"\")","v":""},"Échelle d’indicateur"]
[{"$f":"IF(LEN('Translation-EN'!A1149)>0,'Translation-EN'!A1149,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1149)>0,'Translation-EN'!B1149,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1149)>0,'Translation-EN'!C1149,\"\")","v":"W3"},{"$f":"IF(LEN('Translation-EN'!D1149)>0,'Translation-EN'!D1149,\"\")","v":""},"Limite inférieure"]
[{"$f":"IF(LEN('Translation-EN'!A1150)>0,'Translation-EN'!A1150,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1150)>0,'Translation-EN'!B1150,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1150)>0,'Translation-EN'!C1150,\"\")","v":"X3"},{"$f":"IF(LEN('Translation-EN'!D1150)>0,'Translation-EN'!D1150,\"\")","v":""},"Limite supérieure"]
[{"$f":"IF(LEN('Translation-EN'!A1151)>0,'Translation-EN'!A1151,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1151)>0,'Translation-EN'!B1151,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1151)>0,'Translation-EN'!C1151,\"\")","v":"K15"},{"$f":"IF(LEN('Translation-EN'!D1151)>0,'Translation-EN'!D1151,\"\")","v":""},{"$f":"$E$1083","v":"Section"}]
[{"$f":"IF(LEN('Translation-EN'!A1152)>0,'Translation-EN'!A1152,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1152)>0,'Translation-EN'!B1152,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1152)>0,'Translation-EN'!C1152,\"\")","v":"L15"},{"$f":"IF(LEN('Translation-EN'!D1152)>0,'Translation-EN'!D1152,\"\")","v":true},"Carbone intrinsèque\n[kg CO2e]"]
[{"$f":"IF(LEN('Translation-EN'!A1153)>0,'Translation-EN'!A1153,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1153)>0,'Translation-EN'!B1153,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1153)>0,'Translation-EN'!C1153,\"\")","v":"K16"},{"$f":"IF(LEN('Translation-EN'!D1153)>0,'Translation-EN'!D1153,\"\")","v":"Ignore this cell of the Data sheet"},"Semelles et dalles"]
[{"$f":"IF(LEN('Translation-EN'!A1154)>0,'Translation-EN'!A1154,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1154)>0,'Translation-EN'!B1154,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1154)>0,'Translation-EN'!C1154,\"\")","v":"K17"},{"$f":"IF(LEN('Translation-EN'!D1154)>0,'Translation-EN'!D1154,\"\")","v":"Ignore this cell of the Data sheet"},"Murs de fondation"]
[{"$f":"IF(LEN('Translation-EN'!A1155)>0,'Translation-EN'!A1155,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1155)>0,'Translation-EN'!B1155,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1155)>0,'Translation-EN'!C1155,\"\")","v":"K18"},{"$f":"IF(LEN('Translation-EN'!D1155)>0,'Translation-EN'!D1155,\"\")","v":"Ignore this cell of the Data sheet"},"Éléments structuraux"]
[{"$f":"IF(LEN('Translation-EN'!A1156)>0,'Translation-EN'!A1156,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1156)>0,'Translation-EN'!B1156,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1156)>0,'Translation-EN'!C1156,\"\")","v":"K19"},{"$f":"IF(LEN('Translation-EN'!D1156)>0,'Translation-EN'!D1156,\"\")","v":"Ignore this cell of the Data sheet"},"Murs extérieurs"]
[{"$f":"IF(LEN('Translation-EN'!A1157)>0,'Translation-EN'!A1157,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1157)>0,'Translation-EN'!B1157,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1157)>0,'Translation-EN'!C1157,\"\")","v":"K20"},{"$f":"IF(LEN('Translation-EN'!D1157)>0,'Translation-EN'!D1157,\"\")","v":"Ignore this cell of the Data sheet"},"Système de murs extérieurs"]
[{"$f":"IF(LEN('Translation-EN'!A1158)>0,'Translation-EN'!A1158,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1158)>0,'Translation-EN'!B1158,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1158)>0,'Translation-EN'!C1158,\"\")","v":"K21"},{"$f":"IF(LEN('Translation-EN'!D1158)>0,'Translation-EN'!D1158,\"\")","v":"Ignore this cell of the Data sheet"},"Murs mitoyens"]
[{"$f":"IF(LEN('Translation-EN'!A1159)>0,'Translation-EN'!A1159,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1159)>0,'Translation-EN'!B1159,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1159)>0,'Translation-EN'!C1159,\"\")","v":"K22"},{"$f":"IF(LEN('Translation-EN'!D1159)>0,'Translation-EN'!D1159,\"\")","v":"Ignore this cell of the Data sheet"},{"$f":"$E$1044","v":"Bardage"}]
[{"$f":"IF(LEN('Translation-EN'!A1160)>0,'Translation-EN'!A1160,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1160)>0,'Translation-EN'!B1160,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1160)>0,'Translation-EN'!C1160,\"\")","v":"K23"},{"$f":"IF(LEN('Translation-EN'!D1160)>0,'Translation-EN'!D1160,\"\")","v":"Ignore this cell of the Data sheet"},{"$f":"$E$93","v":"Fenêtres"}]
[{"$f":"IF(LEN('Translation-EN'!A1161)>0,'Translation-EN'!A1161,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1161)>0,'Translation-EN'!B1161,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1161)>0,'Translation-EN'!C1161,\"\")","v":"K24"},{"$f":"IF(LEN('Translation-EN'!D1161)>0,'Translation-EN'!D1161,\"\")","v":"Ignore this cell of the Data sheet"},"Murs intérieurs"]
[{"$f":"IF(LEN('Translation-EN'!A1162)>0,'Translation-EN'!A1162,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1162)>0,'Translation-EN'!B1162,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1162)>0,'Translation-EN'!C1162,\"\")","v":"K25"},{"$f":"IF(LEN('Translation-EN'!D1162)>0,'Translation-EN'!D1162,\"\")","v":"Ignore this cell of the Data sheet"},"Plancher"]
[{"$f":"IF(LEN('Translation-EN'!A1163)>0,'Translation-EN'!A1163,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1163)>0,'Translation-EN'!B1163,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1163)>0,'Translation-EN'!C1163,\"\")","v":"K26"},{"$f":"IF(LEN('Translation-EN'!D1163)>0,'Translation-EN'!D1163,\"\")","v":"Ignore this cell of the Data sheet"},"Plafonds"]
[{"$f":"IF(LEN('Translation-EN'!A1164)>0,'Translation-EN'!A1164,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1164)>0,'Translation-EN'!B1164,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1164)>0,'Translation-EN'!C1164,\"\")","v":"K27"},{"$f":"IF(LEN('Translation-EN'!D1164)>0,'Translation-EN'!D1164,\"\")","v":"Ignore this cell of the Data sheet"},"Toit"]
[{"$f":"IF(LEN('Translation-EN'!A1165)>0,'Translation-EN'!A1165,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1165)>0,'Translation-EN'!B1165,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1165)>0,'Translation-EN'!C1165,\"\")","v":"K28"},{"$f":"IF(LEN('Translation-EN'!D1165)>0,'Translation-EN'!D1165,\"\")","v":"Ignore this cell of the Data sheet"},"Garage"]
[{"$f":"IF(LEN('Translation-EN'!A1166)>0,'Translation-EN'!A1166,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1166)>0,'Translation-EN'!B1166,\"\")","v":"_Data"},{"$f":"IF(LEN('Translation-EN'!C1166)>0,'Translation-EN'!C1166,\"\")","v":"K29"},{"$f":"IF(LEN('Translation-EN'!D1166)>0,'Translation-EN'!D1166,\"\")","v":"Ignore this cell of the Data sheet"},{"$f":"$E$1045","v":"Défini par l’utilisateur"}]
[{"$f":"IF(LEN('Translation-EN'!A1167)>0,'Translation-EN'!A1167,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1167)>0,'Translation-EN'!B1167,\"\")","v":"Data"},{"$f":"IF(LEN('Translation-EN'!C1167)>0,'Translation-EN'!C1167,\"\")","v":"K30"},{"$f":"IF(LEN('Translation-EN'!D1167)>0,'Translation-EN'!D1167,\"\")","v":""},"TOTAL"]
[{"$f":"IF(LEN('Translation-EN'!A1168)>0,'Translation-EN'!A1168,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1168)>0,'Translation-EN'!B1168,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1168)>0,'Translation-EN'!C1168,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D1168)>0,'Translation-EN'!D1168,\"\")","v":""},"Produit composite"]
[{"$f":"IF(LEN('Translation-EN'!A1169)>0,'Translation-EN'!A1169,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1169)>0,'Translation-EN'!B1169,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1169)>0,'Translation-EN'!C1169,\"\")","v":"B1"},{"$f":"IF(LEN('Translation-EN'!D1169)>0,'Translation-EN'!D1169,\"\")","v":""},"Émissions composites co2"]
[{"$f":"IF(LEN('Translation-EN'!A1170)>0,'Translation-EN'!A1170,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1170)>0,'Translation-EN'!B1170,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1170)>0,'Translation-EN'!C1170,\"\")","v":"C1"},{"$f":"IF(LEN('Translation-EN'!D1170)>0,'Translation-EN'!D1170,\"\")","v":""},"Stockage composite CO2/m2"]
[{"$f":"IF(LEN('Translation-EN'!A1171)>0,'Translation-EN'!A1171,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1171)>0,'Translation-EN'!B1171,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1171)>0,'Translation-EN'!C1171,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D1171)>0,'Translation-EN'!D1171,\"\")","v":""},"Unité"]
[{"$f":"IF(LEN('Translation-EN'!A1172)>0,'Translation-EN'!A1172,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1172)>0,'Translation-EN'!B1172,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1172)>0,'Translation-EN'!C1172,\"\")","v":"E1"},{"$f":"IF(LEN('Translation-EN'!D1172)>0,'Translation-EN'!D1172,\"\")","v":""},"Matériau 1"]
[{"$f":"IF(LEN('Translation-EN'!A1173)>0,'Translation-EN'!A1173,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1173)>0,'Translation-EN'!B1173,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1173)>0,'Translation-EN'!C1173,\"\")","v":"F1"},{"$f":"IF(LEN('Translation-EN'!D1173)>0,'Translation-EN'!D1173,\"\")","v":""},"Unité entrante"]
[{"$f":"IF(LEN('Translation-EN'!A1174)>0,'Translation-EN'!A1174,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1174)>0,'Translation-EN'!B1174,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1174)>0,'Translation-EN'!C1174,\"\")","v":"G1"},{"$f":"IF(LEN('Translation-EN'!D1174)>0,'Translation-EN'!D1174,\"\")","v":""},"Émission M1"]
[{"$f":"IF(LEN('Translation-EN'!A1175)>0,'Translation-EN'!A1175,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1175)>0,'Translation-EN'!B1175,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1175)>0,'Translation-EN'!C1175,\"\")","v":"H1"},{"$f":"IF(LEN('Translation-EN'!D1175)>0,'Translation-EN'!D1175,\"\")","v":""},"Stockage M1"]
[{"$f":"IF(LEN('Translation-EN'!A1176)>0,'Translation-EN'!A1176,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1176)>0,'Translation-EN'!B1176,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1176)>0,'Translation-EN'!C1176,\"\")","v":"I1"},{"$f":"IF(LEN('Translation-EN'!D1176)>0,'Translation-EN'!D1176,\"\")","v":""},"Matériau 2"]
[{"$f":"IF(LEN('Translation-EN'!A1177)>0,'Translation-EN'!A1177,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1177)>0,'Translation-EN'!B1177,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1177)>0,'Translation-EN'!C1177,\"\")","v":"J1"},{"$f":"IF(LEN('Translation-EN'!D1177)>0,'Translation-EN'!D1177,\"\")","v":""},{"$f":"$E$1173","v":"Unité entrante"}]
[{"$f":"IF(LEN('Translation-EN'!A1178)>0,'Translation-EN'!A1178,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1178)>0,'Translation-EN'!B1178,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1178)>0,'Translation-EN'!C1178,\"\")","v":"K1"},{"$f":"IF(LEN('Translation-EN'!D1178)>0,'Translation-EN'!D1178,\"\")","v":""},"Émission M2"]
[{"$f":"IF(LEN('Translation-EN'!A1179)>0,'Translation-EN'!A1179,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1179)>0,'Translation-EN'!B1179,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1179)>0,'Translation-EN'!C1179,\"\")","v":"L1"},{"$f":"IF(LEN('Translation-EN'!D1179)>0,'Translation-EN'!D1179,\"\")","v":""},"Stockage M2"]
[{"$f":"IF(LEN('Translation-EN'!A1180)>0,'Translation-EN'!A1180,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1180)>0,'Translation-EN'!B1180,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1180)>0,'Translation-EN'!C1180,\"\")","v":"M1"},{"$f":"IF(LEN('Translation-EN'!D1180)>0,'Translation-EN'!D1180,\"\")","v":""},"Matériau 3"]
[{"$f":"IF(LEN('Translation-EN'!A1181)>0,'Translation-EN'!A1181,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1181)>0,'Translation-EN'!B1181,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1181)>0,'Translation-EN'!C1181,\"\")","v":"N1"},{"$f":"IF(LEN('Translation-EN'!D1181)>0,'Translation-EN'!D1181,\"\")","v":""},{"$f":"$E$1173","v":"Unité entrante"}]
[{"$f":"IF(LEN('Translation-EN'!A1182)>0,'Translation-EN'!A1182,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1182)>0,'Translation-EN'!B1182,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1182)>0,'Translation-EN'!C1182,\"\")","v":"O1"},{"$f":"IF(LEN('Translation-EN'!D1182)>0,'Translation-EN'!D1182,\"\")","v":""},"Émission M3"]
[{"$f":"IF(LEN('Translation-EN'!A1183)>0,'Translation-EN'!A1183,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1183)>0,'Translation-EN'!B1183,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1183)>0,'Translation-EN'!C1183,\"\")","v":"P1"},{"$f":"IF(LEN('Translation-EN'!D1183)>0,'Translation-EN'!D1183,\"\")","v":""},"Stockage M3"]
[{"$f":"IF(LEN('Translation-EN'!A1184)>0,'Translation-EN'!A1184,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1184)>0,'Translation-EN'!B1184,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1184)>0,'Translation-EN'!C1184,\"\")","v":"Q1"},{"$f":"IF(LEN('Translation-EN'!D1184)>0,'Translation-EN'!D1184,\"\")","v":""},"Matériel 4"]
[{"$f":"IF(LEN('Translation-EN'!A1185)>0,'Translation-EN'!A1185,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1185)>0,'Translation-EN'!B1185,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1185)>0,'Translation-EN'!C1185,\"\")","v":"R1"},{"$f":"IF(LEN('Translation-EN'!D1185)>0,'Translation-EN'!D1185,\"\")","v":""},{"$f":"$E$1173","v":"Unité entrante"}]
[{"$f":"IF(LEN('Translation-EN'!A1186)>0,'Translation-EN'!A1186,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1186)>0,'Translation-EN'!B1186,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1186)>0,'Translation-EN'!C1186,\"\")","v":"S1"},{"$f":"IF(LEN('Translation-EN'!D1186)>0,'Translation-EN'!D1186,\"\")","v":""},"Émission M4"]
[{"$f":"IF(LEN('Translation-EN'!A1187)>0,'Translation-EN'!A1187,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1187)>0,'Translation-EN'!B1187,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1187)>0,'Translation-EN'!C1187,\"\")","v":"T1"},{"$f":"IF(LEN('Translation-EN'!D1187)>0,'Translation-EN'!D1187,\"\")","v":""},"Stockage M4"]
[{"$f":"IF(LEN('Translation-EN'!A1188)>0,'Translation-EN'!A1188,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1188)>0,'Translation-EN'!B1188,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1188)>0,'Translation-EN'!C1188,\"\")","v":"U1"},{"$f":"IF(LEN('Translation-EN'!D1188)>0,'Translation-EN'!D1188,\"\")","v":""},"Matériau 5"]
[{"$f":"IF(LEN('Translation-EN'!A1189)>0,'Translation-EN'!A1189,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1189)>0,'Translation-EN'!B1189,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1189)>0,'Translation-EN'!C1189,\"\")","v":"V1"},{"$f":"IF(LEN('Translation-EN'!D1189)>0,'Translation-EN'!D1189,\"\")","v":""},{"$f":"$E$1173","v":"Unité entrante"}]
[{"$f":"IF(LEN('Translation-EN'!A1190)>0,'Translation-EN'!A1190,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1190)>0,'Translation-EN'!B1190,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1190)>0,'Translation-EN'!C1190,\"\")","v":"W1"},{"$f":"IF(LEN('Translation-EN'!D1190)>0,'Translation-EN'!D1190,\"\")","v":""},"Émission M5"]
[{"$f":"IF(LEN('Translation-EN'!A1191)>0,'Translation-EN'!A1191,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1191)>0,'Translation-EN'!B1191,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1191)>0,'Translation-EN'!C1191,\"\")","v":"X1"},{"$f":"IF(LEN('Translation-EN'!D1191)>0,'Translation-EN'!D1191,\"\")","v":""},"Stockage"]
[{"$f":"IF(LEN('Translation-EN'!A1192)>0,'Translation-EN'!A1192,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1192)>0,'Translation-EN'!B1192,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1192)>0,'Translation-EN'!C1192,\"\")","v":"Y1"},{"$f":"IF(LEN('Translation-EN'!D1192)>0,'Translation-EN'!D1192,\"\")","v":""},{"$f":"$E$1103","v":"Notes"}]
[{"$f":"IF(LEN('Translation-EN'!A1193)>0,'Translation-EN'!A1193,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1193)>0,'Translation-EN'!B1193,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1193)>0,'Translation-EN'!C1193,\"\")","v":"Z1"},{"$f":"IF(LEN('Translation-EN'!D1193)>0,'Translation-EN'!D1193,\"\")","v":""},"Identifiant de produit de matériau 1"]
[{"$f":"IF(LEN('Translation-EN'!A1194)>0,'Translation-EN'!A1194,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1194)>0,'Translation-EN'!B1194,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1194)>0,'Translation-EN'!C1194,\"\")","v":"AA1"},{"$f":"IF(LEN('Translation-EN'!D1194)>0,'Translation-EN'!D1194,\"\")","v":""},"Identifiant de produit de matériau 2"]
[{"$f":"IF(LEN('Translation-EN'!A1195)>0,'Translation-EN'!A1195,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1195)>0,'Translation-EN'!B1195,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1195)>0,'Translation-EN'!C1195,\"\")","v":"AB1"},{"$f":"IF(LEN('Translation-EN'!D1195)>0,'Translation-EN'!D1195,\"\")","v":""},"Identifiant de produit de matériau 3"]
[{"$f":"IF(LEN('Translation-EN'!A1196)>0,'Translation-EN'!A1196,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1196)>0,'Translation-EN'!B1196,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1196)>0,'Translation-EN'!C1196,\"\")","v":"AC1"},{"$f":"IF(LEN('Translation-EN'!D1196)>0,'Translation-EN'!D1196,\"\")","v":""},"Identifiant de produit de matériau 4"]
[{"$f":"IF(LEN('Translation-EN'!A1197)>0,'Translation-EN'!A1197,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1197)>0,'Translation-EN'!B1197,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1197)>0,'Translation-EN'!C1197,\"\")","v":"AD1"},{"$f":"IF(LEN('Translation-EN'!D1197)>0,'Translation-EN'!D1197,\"\")","v":""},"Identifiant de produit de matériau 5"]
[{"$f":"IF(LEN('Translation-EN'!A1198)>0,'Translation-EN'!A1198,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1198)>0,'Translation-EN'!B1198,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1198)>0,'Translation-EN'!C1198,\"\")","v":"A2"},{"$f":"IF(LEN('Translation-EN'!D1198)>0,'Translation-EN'!D1198,\"\")","v":""},"Mousse EPS CBI R-23, 2 feuilles de 2,75 po @ R4/po. @ R4/in., barre d’armature 15M (le noyau de béton de 6 po doit être ajouté séparément)"]
[{"$f":"IF(LEN('Translation-EN'!A1199)>0,'Translation-EN'!A1199,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1199)>0,'Translation-EN'!B1199,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1199)>0,'Translation-EN'!C1199,\"\")","v":"A3"},{"$f":"IF(LEN('Translation-EN'!D1199)>0,'Translation-EN'!D1199,\"\")","v":""},"PANNEAU STRUCTUREL ISOLÉ –R23 6,5 po – EPS 5,5 po @ R4/po, 2 feuilles d’OSB de 1/2 pouce"]
[{"$f":"IF(LEN('Translation-EN'!A1200)>0,'Translation-EN'!A1200,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1200)>0,'Translation-EN'!B1200,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1200)>0,'Translation-EN'!C1200,\"\")","v":"A4"},{"$f":"IF(LEN('Translation-EN'!D1200)>0,'Translation-EN'!D1200,\"\")","v":""},"PANNEAU STRUCTUREL ISOLÉ –R 30,25 po – EPS 7,25 po @ R4/po, 2 feuilles d’OSB de 1/2 pouce"]
[{"$f":"IF(LEN('Translation-EN'!A1201)>0,'Translation-EN'!A1201,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1201)>0,'Translation-EN'!B1201,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1201)>0,'Translation-EN'!C1201,\"\")","v":"A5"},{"$f":"IF(LEN('Translation-EN'!D1201)>0,'Translation-EN'!D1201,\"\")","v":""},"PANNEAU STRUCTUREL ISOLÉ –R38 10,5 po – EPS 9,5 po @ R4/po, 2 feuilles d’OSB de 1/2 pouce"]
[{"$f":"IF(LEN('Translation-EN'!A1202)>0,'Translation-EN'!A1202,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1202)>0,'Translation-EN'!B1202,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1202)>0,'Translation-EN'!C1202,\"\")","v":"A6"},{"$f":"IF(LEN('Translation-EN'!D1202)>0,'Translation-EN'!D1202,\"\")","v":""},"PANNEAU STRUCTUREL ISOLÉ –R48 12-7/8 po – EPS 11,875 po @ R4/po, 2 feuilles d’OSB de 1/2 pouce"]
[{"$f":"IF(LEN('Translation-EN'!A1203)>0,'Translation-EN'!A1203,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1203)>0,'Translation-EN'!B1203,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1203)>0,'Translation-EN'!C1203,\"\")","v":"A7"},{"$f":"IF(LEN('Translation-EN'!D1203)>0,'Translation-EN'!D1203,\"\")","v":""},"CIF en copeaux de bois et ciment 12 po R-22 avec INSERTS EN LAINE MINÉRALE, (3 po @ R4.2/pouce), BARRE D’ARMATURE 15M"]
[{"$f":"IF(LEN('Translation-EN'!A1204)>0,'Translation-EN'!A1204,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1204)>0,'Translation-EN'!B1204,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1204)>0,'Translation-EN'!C1204,\"\")","v":"A8"},{"$f":"IF(LEN('Translation-EN'!D1204)>0,'Translation-EN'!D1204,\"\")","v":""},"CIF en copeaux de bois et ciment 14 po R-28 avec INSERTS EN LAINE MINÉRALE, (5 po @ R4.2/pouce), BARRE D’ARMATURE 15M"]
[{"$f":"IF(LEN('Translation-EN'!A1205)>0,'Translation-EN'!A1205,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1205)>0,'Translation-EN'!B1205,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1205)>0,'Translation-EN'!C1205,\"\")","v":"A9"},{"$f":"IF(LEN('Translation-EN'!D1205)>0,'Translation-EN'!D1205,\"\")","v":""},"CIF en copeaux de bois et ciment 12 po R-21 avec INSERTS EN PANNEAU DE LIÈGE, (3 po @ R4.2/pouce), BARRE D’ARMATURE 15M"]
[{"$f":"IF(LEN('Translation-EN'!A1206)>0,'Translation-EN'!A1206,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1206)>0,'Translation-EN'!B1206,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1206)>0,'Translation-EN'!C1206,\"\")","v":"A10"},{"$f":"IF(LEN('Translation-EN'!D1206)>0,'Translation-EN'!D1206,\"\")","v":""},"CIF en copeaux de bois et ciment 14 po R-27 avec INSERTS EN PANNEAU DE LIÈGE, (5 po @ R4.2/pouce), BARRE D’ARMATURE 15M"]
[{"$f":"IF(LEN('Translation-EN'!A1207)>0,'Translation-EN'!A1207,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1207)>0,'Translation-EN'!B1207,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1207)>0,'Translation-EN'!C1207,\"\")","v":"A11"},{"$f":"IF(LEN('Translation-EN'!D1207)>0,'Translation-EN'!D1207,\"\")","v":""},"FONDATION EN BOIS TRAITÉ –charpente 2x8 à 16 po OC, revêtement en contreplaqué de 3/4 po."]
[{"$f":"IF(LEN('Translation-EN'!A1208)>0,'Translation-EN'!A1208,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1208)>0,'Translation-EN'!B1208,\"\")","v":"Composite Master Sheet"},{"$f":"IF(LEN('Translation-EN'!C1208)>0,'Translation-EN'!C1208,\"\")","v":"A12"},{"$f":"IF(LEN('Translation-EN'!D1208)>0,'Translation-EN'!D1208,\"\")","v":""},"CADRE EN BOIS avec INFILLON DE BALLES DE FER – 14 po R-46, double 2x4 @ 30 po o/c"]
[{"$f":"IF(LEN('Translation-EN'!A1209)>0,'Translation-EN'!A1209,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1209)>0,'Translation-EN'!B1209,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1209)>0,'Translation-EN'!C1209,\"\")","v":"A1"},{"$f":"IF(LEN('Translation-EN'!D1209)>0,'Translation-EN'!D1209,\"\")","v":""},"Produit"]
[{"$f":"IF(LEN('Translation-EN'!A1210)>0,'Translation-EN'!A1210,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1210)>0,'Translation-EN'!B1210,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1210)>0,'Translation-EN'!C1210,\"\")","v":"B1"},{"$f":"IF(LEN('Translation-EN'!D1210)>0,'Translation-EN'!D1210,\"\")","v":""},{"$f":"$E$1084","v":"Matériau"}]
[{"$f":"IF(LEN('Translation-EN'!A1211)>0,'Translation-EN'!A1211,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1211)>0,'Translation-EN'!B1211,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1211)>0,'Translation-EN'!C1211,\"\")","v":"C1"},{"$f":"IF(LEN('Translation-EN'!D1211)>0,'Translation-EN'!D1211,\"\")","v":""},"Société (Commissaire DEP)"]
[{"$f":"IF(LEN('Translation-EN'!A1212)>0,'Translation-EN'!A1212,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1212)>0,'Translation-EN'!B1212,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1212)>0,'Translation-EN'!C1212,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D1212)>0,'Translation-EN'!D1212,\"\")","v":""},"Marque"]
[{"$f":"IF(LEN('Translation-EN'!A1213)>0,'Translation-EN'!A1213,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1213)>0,'Translation-EN'!B1213,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1213)>0,'Translation-EN'!C1213,\"\")","v":"E1"},{"$f":"IF(LEN('Translation-EN'!D1213)>0,'Translation-EN'!D1213,\"\")","v":""},"Caractéristiques techniques"]
[{"$f":"IF(LEN('Translation-EN'!A1214)>0,'Translation-EN'!A1214,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1214)>0,'Translation-EN'!B1214,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1214)>0,'Translation-EN'!C1214,\"\")","v":"F1"},{"$f":"IF(LEN('Translation-EN'!D1214)>0,'Translation-EN'!D1214,\"\")","v":""},"No CSI"]
[{"$f":"IF(LEN('Translation-EN'!A1215)>0,'Translation-EN'!A1215,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1215)>0,'Translation-EN'!B1215,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1215)>0,'Translation-EN'!C1215,\"\")","v":"G1"},{"$f":"IF(LEN('Translation-EN'!D1215)>0,'Translation-EN'!D1215,\"\")","v":""},"Catégorie"]
[{"$f":"IF(LEN('Translation-EN'!A1216)>0,'Translation-EN'!A1216,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1216)>0,'Translation-EN'!B1216,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1216)>0,'Translation-EN'!C1216,\"\")","v":"H1"},{"$f":"IF(LEN('Translation-EN'!D1216)>0,'Translation-EN'!D1216,\"\")","v":""},{"$f":"$E$1103","v":"Notes"}]
[{"$f":"IF(LEN('Translation-EN'!A1217)>0,'Translation-EN'!A1217,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1217)>0,'Translation-EN'!B1217,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1217)>0,'Translation-EN'!C1217,\"\")","v":"I1"},{"$f":"IF(LEN('Translation-EN'!D1217)>0,'Translation-EN'!D1217,\"\")","v":""},"Pays de fabrication"]
[{"$f":"IF(LEN('Translation-EN'!A1218)>0,'Translation-EN'!A1218,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1218)>0,'Translation-EN'!B1218,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1218)>0,'Translation-EN'!C1218,\"\")","v":"J1"},{"$f":"IF(LEN('Translation-EN'!D1218)>0,'Translation-EN'!D1218,\"\")","v":""},"RNCan"]
[{"$f":"IF(LEN('Translation-EN'!A1219)>0,'Translation-EN'!A1219,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1219)>0,'Translation-EN'!B1219,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1219)>0,'Translation-EN'!C1219,\"\")","v":"K1"},{"$f":"IF(LEN('Translation-EN'!D1219)>0,'Translation-EN'!D1219,\"\")","v":""},"DEP déclaré kgCO2e/unité"]
[{"$f":"IF(LEN('Translation-EN'!A1220)>0,'Translation-EN'!A1220,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1220)>0,'Translation-EN'!B1220,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1220)>0,'Translation-EN'!C1220,\"\")","v":"L1"},{"$f":"IF(LEN('Translation-EN'!D1220)>0,'Translation-EN'!D1220,\"\")","v":""},"Unités DEP kgCO2e par"]
[{"$f":"IF(LEN('Translation-EN'!A1221)>0,'Translation-EN'!A1221,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1221)>0,'Translation-EN'!B1221,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1221)>0,'Translation-EN'!C1221,\"\")","v":"M1"},{"$f":"IF(LEN('Translation-EN'!D1221)>0,'Translation-EN'!D1221,\"\")","v":""},"Émissions communes kgCO2e/unité"]
[{"$f":"IF(LEN('Translation-EN'!A1222)>0,'Translation-EN'!A1222,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1222)>0,'Translation-EN'!B1222,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1222)>0,'Translation-EN'!C1222,\"\")","v":"N1"},{"$f":"IF(LEN('Translation-EN'!D1222)>0,'Translation-EN'!D1222,\"\")","v":""},"Unités : kgCO2e par"]
[{"$f":"IF(LEN('Translation-EN'!A1223)>0,'Translation-EN'!A1223,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1223)>0,'Translation-EN'!B1223,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1223)>0,'Translation-EN'!C1223,\"\")","v":"O1"},{"$f":"IF(LEN('Translation-EN'!D1223)>0,'Translation-EN'!D1223,\"\")","v":""},"No DEP"]
[{"$f":"IF(LEN('Translation-EN'!A1224)>0,'Translation-EN'!A1224,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1224)>0,'Translation-EN'!B1224,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1224)>0,'Translation-EN'!C1224,\"\")","v":"P1"},{"$f":"IF(LEN('Translation-EN'!D1224)>0,'Translation-EN'!D1224,\"\")","v":""},"Organisme de vérification"]
[{"$f":"IF(LEN('Translation-EN'!A1225)>0,'Translation-EN'!A1225,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1225)>0,'Translation-EN'!B1225,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1225)>0,'Translation-EN'!C1225,\"\")","v":"Q1"},{"$f":"IF(LEN('Translation-EN'!D1225)>0,'Translation-EN'!D1225,\"\")","v":""},"Année d’exp."]
[{"$f":"IF(LEN('Translation-EN'!A1226)>0,'Translation-EN'!A1226,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1226)>0,'Translation-EN'!B1226,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1226)>0,'Translation-EN'!C1226,\"\")","v":"R1"},{"$f":"IF(LEN('Translation-EN'!D1226)>0,'Translation-EN'!D1226,\"\")","v":""},"Densité"]
[{"$f":"IF(LEN('Translation-EN'!A1227)>0,'Translation-EN'!A1227,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1227)>0,'Translation-EN'!B1227,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1227)>0,'Translation-EN'!C1227,\"\")","v":"S1"},{"$f":"IF(LEN('Translation-EN'!D1227)>0,'Translation-EN'!D1227,\"\")","v":""},"Unités"]
[{"$f":"IF(LEN('Translation-EN'!A1228)>0,'Translation-EN'!A1228,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1228)>0,'Translation-EN'!B1228,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1228)>0,'Translation-EN'!C1228,\"\")","v":"T1"},{"$f":"IF(LEN('Translation-EN'!D1228)>0,'Translation-EN'!D1228,\"\")","v":""},"Facteurs additionnels"]
[{"$f":"IF(LEN('Translation-EN'!A1229)>0,'Translation-EN'!A1229,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1229)>0,'Translation-EN'!B1229,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1229)>0,'Translation-EN'!C1229,\"\")","v":"U1"},{"$f":"IF(LEN('Translation-EN'!D1229)>0,'Translation-EN'!D1229,\"\")","v":""},{"$f":"$E$1227","v":"Unités"}]
[{"$f":"IF(LEN('Translation-EN'!A1230)>0,'Translation-EN'!A1230,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1230)>0,'Translation-EN'!B1230,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1230)>0,'Translation-EN'!C1230,\"\")","v":"V1"},{"$f":"IF(LEN('Translation-EN'!D1230)>0,'Translation-EN'!D1230,\"\")","v":""},"Valeur R/po"]
[{"$f":"IF(LEN('Translation-EN'!A1231)>0,'Translation-EN'!A1231,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1231)>0,'Translation-EN'!B1231,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1231)>0,'Translation-EN'!C1231,\"\")","v":"W1"},{"$f":"IF(LEN('Translation-EN'!D1231)>0,'Translation-EN'!D1231,\"\")","v":""},"Cond. thermiques"]
[{"$f":"IF(LEN('Translation-EN'!A1232)>0,'Translation-EN'!A1232,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1232)>0,'Translation-EN'!B1232,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1232)>0,'Translation-EN'!C1232,\"\")","v":"X1"},{"$f":"IF(LEN('Translation-EN'!D1232)>0,'Translation-EN'!D1232,\"\")","v":""},{"$f":"$E$1227","v":"Unités"}]
[{"$f":"IF(LEN('Translation-EN'!A1233)>0,'Translation-EN'!A1233,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1233)>0,'Translation-EN'!B1233,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1233)>0,'Translation-EN'!C1233,\"\")","v":"Y1"},{"$f":"IF(LEN('Translation-EN'!D1233)>0,'Translation-EN'!D1233,\"\")","v":""},"Facteur de carbone biogénique"]
[{"$f":"IF(LEN('Translation-EN'!A1234)>0,'Translation-EN'!A1234,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1234)>0,'Translation-EN'!B1234,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1234)>0,'Translation-EN'!C1234,\"\")","v":"Z1"},{"$f":"IF(LEN('Translation-EN'!D1234)>0,'Translation-EN'!D1234,\"\")","v":""},"% Teneur en carbone (kgC/kg)"]
[{"$f":"IF(LEN('Translation-EN'!A1235)>0,'Translation-EN'!A1235,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1235)>0,'Translation-EN'!B1235,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1235)>0,'Translation-EN'!C1235,\"\")","v":"AA1"},{"$f":"IF(LEN('Translation-EN'!D1235)>0,'Translation-EN'!D1235,\"\")","v":""},"Stockage biogénique kgCO2/unité"]
[{"$f":"IF(LEN('Translation-EN'!A1236)>0,'Translation-EN'!A1236,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1236)>0,'Translation-EN'!B1236,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1236)>0,'Translation-EN'!C1236,\"\")","v":"AB1"},{"$f":"IF(LEN('Translation-EN'!D1236)>0,'Translation-EN'!D1236,\"\")","v":""},{"$f":"$E$1222","v":"Unités : kgCO2e par"}]
[{"$f":"IF(LEN('Translation-EN'!A1237)>0,'Translation-EN'!A1237,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1237)>0,'Translation-EN'!B1237,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1237)>0,'Translation-EN'!C1237,\"\")","v":"AC1"},{"$f":"IF(LEN('Translation-EN'!D1237)>0,'Translation-EN'!D1237,\"\")","v":""},"Facteur de stockage WWF kgCO2/kgC"]
[{"$f":"IF(LEN('Translation-EN'!A1238)>0,'Translation-EN'!A1238,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1238)>0,'Translation-EN'!B1238,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1238)>0,'Translation-EN'!C1238,\"\")","v":"AD1"},{"$f":"IF(LEN('Translation-EN'!D1238)>0,'Translation-EN'!D1238,\"\")","v":""},"Teneur en carbone kgC/unité"]
[{"$f":"IF(LEN('Translation-EN'!A1239)>0,'Translation-EN'!A1239,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1239)>0,'Translation-EN'!B1239,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1239)>0,'Translation-EN'!C1239,\"\")","v":"AE1"},{"$f":"IF(LEN('Translation-EN'!D1239)>0,'Translation-EN'!D1239,\"\")","v":""},{"$f":"$E$1227","v":"Unités"}]
[{"$f":"IF(LEN('Translation-EN'!A1240)>0,'Translation-EN'!A1240,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1240)>0,'Translation-EN'!B1240,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1240)>0,'Translation-EN'!C1240,\"\")","v":"AF1"},{"$f":"IF(LEN('Translation-EN'!D1240)>0,'Translation-EN'!D1240,\"\")","v":""},"CO2 biogénique en kg – valeur C complète"]
[{"$f":"IF(LEN('Translation-EN'!A1241)>0,'Translation-EN'!A1241,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1241)>0,'Translation-EN'!B1241,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1241)>0,'Translation-EN'!C1241,\"\")","v":"AG1"},{"$f":"IF(LEN('Translation-EN'!D1241)>0,'Translation-EN'!D1241,\"\")","v":""},"Hauteur (m)"]
[{"$f":"IF(LEN('Translation-EN'!A1242)>0,'Translation-EN'!A1242,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1242)>0,'Translation-EN'!B1242,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1242)>0,'Translation-EN'!C1242,\"\")","v":"AH1"},{"$f":"IF(LEN('Translation-EN'!D1242)>0,'Translation-EN'!D1242,\"\")","v":""},"Longueur (m)"]
[{"$f":"IF(LEN('Translation-EN'!A1243)>0,'Translation-EN'!A1243,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1243)>0,'Translation-EN'!B1243,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1243)>0,'Translation-EN'!C1243,\"\")","v":"AI1"},{"$f":"IF(LEN('Translation-EN'!D1243)>0,'Translation-EN'!D1243,\"\")","v":""},"Largeur (m)"]
[{"$f":"IF(LEN('Translation-EN'!A1244)>0,'Translation-EN'!A1244,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1244)>0,'Translation-EN'!B1244,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1244)>0,'Translation-EN'!C1244,\"\")","v":"AJ1"},{"$f":"IF(LEN('Translation-EN'!D1244)>0,'Translation-EN'!D1244,\"\")","v":""},"Volume unitaire (m3)"]
[{"$f":"IF(LEN('Translation-EN'!A1245)>0,'Translation-EN'!A1245,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1245)>0,'Translation-EN'!B1245,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1245)>0,'Translation-EN'!C1245,\"\")","v":"AK1"},{"$f":"IF(LEN('Translation-EN'!D1245)>0,'Translation-EN'!D1245,\"\")","v":""},"Unités/m2"]
[{"$f":"IF(LEN('Translation-EN'!A1246)>0,'Translation-EN'!A1246,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1246)>0,'Translation-EN'!B1246,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1246)>0,'Translation-EN'!C1246,\"\")","v":"AL1"},{"$f":"IF(LEN('Translation-EN'!D1246)>0,'Translation-EN'!D1246,\"\")","v":""},"Identifiant de produit"]
[{"$f":"IF(LEN('Translation-EN'!A1247)>0,'Translation-EN'!A1247,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1247)>0,'Translation-EN'!B1247,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1247)>0,'Translation-EN'!C1247,\"\")","v":"AP1"},{"$f":"IF(LEN('Translation-EN'!D1247)>0,'Translation-EN'!D1247,\"\")","v":""},"Notre DEP"]
[{"$f":"IF(LEN('Translation-EN'!A1248)>0,'Translation-EN'!A1248,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1248)>0,'Translation-EN'!B1248,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1248)>0,'Translation-EN'!C1248,\"\")","v":"B2"},{"$f":"IF(LEN('Translation-EN'!D1248)>0,'Translation-EN'!D1248,\"\")","v":""},"Traitement du bois par ACQ"]
[{"$f":"IF(LEN('Translation-EN'!A1249)>0,'Translation-EN'!A1249,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1249)>0,'Translation-EN'!B1249,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1249)>0,'Translation-EN'!C1249,\"\")","v":"B3"},{"$f":"IF(LEN('Translation-EN'!D1249)>0,'Translation-EN'!D1249,\"\")","v":""},"Block d’adobe"]
[{"$f":"IF(LEN('Translation-EN'!A1250)>0,'Translation-EN'!A1250,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1250)>0,'Translation-EN'!B1250,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1250)>0,'Translation-EN'!C1250,\"\")","v":"D3"},{"$f":"IF(LEN('Translation-EN'!D1250)>0,'Translation-EN'!D1250,\"\")","v":""},"Mur de bloc de 8 pi"]
[{"$f":"IF(LEN('Translation-EN'!A1251)>0,'Translation-EN'!A1251,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1251)>0,'Translation-EN'!B1251,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1251)>0,'Translation-EN'!C1251,\"\")","v":"E3"},{"$f":"IF(LEN('Translation-EN'!D1251)>0,'Translation-EN'!D1251,\"\")","v":""},"Moyenne des produits fabriqués sur place et en usine (Chypre)"]
[{"$f":"IF(LEN('Translation-EN'!A1252)>0,'Translation-EN'!A1252,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1252)>0,'Translation-EN'!B1252,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1252)>0,'Translation-EN'!C1252,\"\")","v":"B4"},{"$f":"IF(LEN('Translation-EN'!D1252)>0,'Translation-EN'!D1252,\"\")","v":""},"Couverture d’aérogel"]
[{"$f":"IF(LEN('Translation-EN'!A1253)>0,'Translation-EN'!A1253,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1253)>0,'Translation-EN'!B1253,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1253)>0,'Translation-EN'!C1253,\"\")","v":"C4"},{"$f":"IF(LEN('Translation-EN'!D1253)>0,'Translation-EN'!D1253,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Aérogels d’Aspen"]
[{"$f":"IF(LEN('Translation-EN'!A1254)>0,'Translation-EN'!A1254,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1254)>0,'Translation-EN'!B1254,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1254)>0,'Translation-EN'!C1254,\"\")","v":"E4"},{"$f":"IF(LEN('Translation-EN'!D1254)>0,'Translation-EN'!D1254,\"\")","v":""},"R 9,6/pouce, couverture blanche/grise"]
[{"$f":"IF(LEN('Translation-EN'!A1255)>0,'Translation-EN'!A1255,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1255)>0,'Translation-EN'!B1255,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1255)>0,'Translation-EN'!C1255,\"\")","v":"B5"},{"$f":"IF(LEN('Translation-EN'!D1255)>0,'Translation-EN'!D1255,\"\")","v":""},"Agrégat"]
[{"$f":"IF(LEN('Translation-EN'!A1256)>0,'Translation-EN'!A1256,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1256)>0,'Translation-EN'!B1256,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1256)>0,'Translation-EN'!C1256,\"\")","v":"E5"},{"$f":"IF(LEN('Translation-EN'!D1256)>0,'Translation-EN'!D1256,\"\")","v":""},"Moyenne des agrégats de construction (gravier et sable)"]
[{"$f":"IF(LEN('Translation-EN'!A1257)>0,'Translation-EN'!A1257,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1257)>0,'Translation-EN'!B1257,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1257)>0,'Translation-EN'!C1257,\"\")","v":"B6"},{"$f":"IF(LEN('Translation-EN'!D1257)>0,'Translation-EN'!D1257,\"\")","v":""},{"$f":"$E$1255","v":"Agrégat"}]
[{"$f":"IF(LEN('Translation-EN'!A1258)>0,'Translation-EN'!A1258,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1258)>0,'Translation-EN'!B1258,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1258)>0,'Translation-EN'!C1258,\"\")","v":"C6"},{"$f":"IF(LEN('Translation-EN'!D1258)>0,'Translation-EN'!D1258,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Kangley Rock & Recycling"]
[{"$f":"IF(LEN('Translation-EN'!A1259)>0,'Translation-EN'!A1259,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1259)>0,'Translation-EN'!B1259,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1259)>0,'Translation-EN'!C1259,\"\")","v":"E6"},{"$f":"IF(LEN('Translation-EN'!D1259)>0,'Translation-EN'!D1259,\"\")","v":""},{"$f":"$E$1256","v":"Moyenne des agrégats de construction (gravier et sable)"}]
[{"$f":"IF(LEN('Translation-EN'!A1260)>0,'Translation-EN'!A1260,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1260)>0,'Translation-EN'!B1260,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1260)>0,'Translation-EN'!C1260,\"\")","v":"B7"},{"$f":"IF(LEN('Translation-EN'!D1260)>0,'Translation-EN'!D1260,\"\")","v":""},{"$f":"$E$1255","v":"Agrégat"}]
[{"$f":"IF(LEN('Translation-EN'!A1261)>0,'Translation-EN'!A1261,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1261)>0,'Translation-EN'!B1261,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1261)>0,'Translation-EN'!C1261,\"\")","v":"C7"},{"$f":"IF(LEN('Translation-EN'!D1261)>0,'Translation-EN'!D1261,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Martin Marietta"]
[{"$f":"IF(LEN('Translation-EN'!A1262)>0,'Translation-EN'!A1262,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1262)>0,'Translation-EN'!B1262,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1262)>0,'Translation-EN'!C1262,\"\")","v":"E7"},{"$f":"IF(LEN('Translation-EN'!D1262)>0,'Translation-EN'!D1262,\"\")","v":""},{"$f":"$E$1256","v":"Moyenne des agrégats de construction (gravier et sable)"}]
[{"$f":"IF(LEN('Translation-EN'!A1263)>0,'Translation-EN'!A1263,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1263)>0,'Translation-EN'!B1263,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1263)>0,'Translation-EN'!C1263,\"\")","v":"B8"},{"$f":"IF(LEN('Translation-EN'!D1263)>0,'Translation-EN'!D1263,\"\")","v":""},{"$f":"$E$1255","v":"Agrégat"}]
[{"$f":"IF(LEN('Translation-EN'!A1264)>0,'Translation-EN'!A1264,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1264)>0,'Translation-EN'!B1264,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1264)>0,'Translation-EN'!C1264,\"\")","v":"C8"},{"$f":"IF(LEN('Translation-EN'!D1264)>0,'Translation-EN'!D1264,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Polaris Mtls Corp."]
[{"$f":"IF(LEN('Translation-EN'!A1265)>0,'Translation-EN'!A1265,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1265)>0,'Translation-EN'!B1265,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1265)>0,'Translation-EN'!C1265,\"\")","v":"E8"},{"$f":"IF(LEN('Translation-EN'!D1265)>0,'Translation-EN'!D1265,\"\")","v":""},{"$f":"$E$1256","v":"Moyenne des agrégats de construction (gravier et sable)"}]
[{"$f":"IF(LEN('Translation-EN'!A1266)>0,'Translation-EN'!A1266,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1266)>0,'Translation-EN'!B1266,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1266)>0,'Translation-EN'!C1266,\"\")","v":"B9"},{"$f":"IF(LEN('Translation-EN'!D1266)>0,'Translation-EN'!D1266,\"\")","v":""},{"$f":"$E$1255","v":"Agrégat"}]
[{"$f":"IF(LEN('Translation-EN'!A1267)>0,'Translation-EN'!A1267,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1267)>0,'Translation-EN'!B1267,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1267)>0,'Translation-EN'!C1267,\"\")","v":"C9"},{"$f":"IF(LEN('Translation-EN'!D1267)>0,'Translation-EN'!D1267,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Vulcan Mtls Co."]
[{"$f":"IF(LEN('Translation-EN'!A1268)>0,'Translation-EN'!A1268,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1268)>0,'Translation-EN'!B1268,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1268)>0,'Translation-EN'!C1268,\"\")","v":"E9"},{"$f":"IF(LEN('Translation-EN'!D1268)>0,'Translation-EN'!D1268,\"\")","v":""},{"$f":"$E$1256","v":"Moyenne des agrégats de construction (gravier et sable)"}]
[{"$f":"IF(LEN('Translation-EN'!A1269)>0,'Translation-EN'!A1269,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1269)>0,'Translation-EN'!B1269,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1269)>0,'Translation-EN'!C1269,\"\")","v":"B10"},{"$f":"IF(LEN('Translation-EN'!D1269)>0,'Translation-EN'!D1269,\"\")","v":""},"Barrière d’air"]
[{"$f":"IF(LEN('Translation-EN'!A1270)>0,'Translation-EN'!A1270,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1270)>0,'Translation-EN'!B1270,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1270)>0,'Translation-EN'!C1270,\"\")","v":"C10"},{"$f":"IF(LEN('Translation-EN'!D1270)>0,'Translation-EN'!D1270,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Dupont"]
[{"$f":"IF(LEN('Translation-EN'!A1271)>0,'Translation-EN'!A1271,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1271)>0,'Translation-EN'!B1271,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1271)>0,'Translation-EN'!C1271,\"\")","v":"D10"},{"$f":"IF(LEN('Translation-EN'!D1271)>0,'Translation-EN'!D1271,\"\")","v":""},"Système de barrière contre les intempéries à base de tyvek fluide appliquée – toutes les composantes"]
[{"$f":"IF(LEN('Translation-EN'!A1272)>0,'Translation-EN'!A1272,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1272)>0,'Translation-EN'!B1272,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1272)>0,'Translation-EN'!C1272,\"\")","v":"E10"},{"$f":"IF(LEN('Translation-EN'!D1272)>0,'Translation-EN'!D1272,\"\")","v":""},"25 Perms"]
[{"$f":"IF(LEN('Translation-EN'!A1273)>0,'Translation-EN'!A1273,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1273)>0,'Translation-EN'!B1273,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1273)>0,'Translation-EN'!C1273,\"\")","v":"B11"},{"$f":"IF(LEN('Translation-EN'!D1273)>0,'Translation-EN'!D1273,\"\")","v":""},{"$f":"$E$1269","v":"Barrière d’air"}]
[{"$f":"IF(LEN('Translation-EN'!A1274)>0,'Translation-EN'!A1274,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1274)>0,'Translation-EN'!B1274,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1274)>0,'Translation-EN'!C1274,\"\")","v":"C11"},{"$f":"IF(LEN('Translation-EN'!D1274)>0,'Translation-EN'!D1274,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1270","v":"Dupont"}]
[{"$f":"IF(LEN('Translation-EN'!A1275)>0,'Translation-EN'!A1275,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1275)>0,'Translation-EN'!B1275,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1275)>0,'Translation-EN'!C1275,\"\")","v":"D11"},{"$f":"IF(LEN('Translation-EN'!D1275)>0,'Translation-EN'!D1275,\"\")","v":""},"Tyvek HomeWrap "]
[{"$f":"IF(LEN('Translation-EN'!A1276)>0,'Translation-EN'!A1276,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1276)>0,'Translation-EN'!B1276,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1276)>0,'Translation-EN'!C1276,\"\")","v":"E11"},{"$f":"IF(LEN('Translation-EN'!D1276)>0,'Translation-EN'!D1276,\"\")","v":""},"54 Perms"]
[{"$f":"IF(LEN('Translation-EN'!A1277)>0,'Translation-EN'!A1277,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1277)>0,'Translation-EN'!B1277,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1277)>0,'Translation-EN'!C1277,\"\")","v":"B12"},{"$f":"IF(LEN('Translation-EN'!D1277)>0,'Translation-EN'!D1277,\"\")","v":""},{"$f":"$E$1269","v":"Barrière d’air"}]
[{"$f":"IF(LEN('Translation-EN'!A1278)>0,'Translation-EN'!A1278,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1278)>0,'Translation-EN'!B1278,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1278)>0,'Translation-EN'!C1278,\"\")","v":"C12"},{"$f":"IF(LEN('Translation-EN'!D1278)>0,'Translation-EN'!D1278,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"GCP"]
[{"$f":"IF(LEN('Translation-EN'!A1279)>0,'Translation-EN'!A1279,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1279)>0,'Translation-EN'!B1279,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1279)>0,'Translation-EN'!C1279,\"\")","v":"D12"},{"$f":"IF(LEN('Translation-EN'!D1279)>0,'Translation-EN'!D1279,\"\")","v":""},"Barrière perméable appliquée en liquide Perm-a-Barrier VPL"]
[{"$f":"IF(LEN('Translation-EN'!A1280)>0,'Translation-EN'!A1280,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1280)>0,'Translation-EN'!B1280,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1280)>0,'Translation-EN'!C1280,\"\")","v":"E12"},{"$f":"IF(LEN('Translation-EN'!D1280)>0,'Translation-EN'!D1280,\"\")","v":""},"15 Perms, 40 mils d’épaisseur"]
[{"$f":"IF(LEN('Translation-EN'!A1281)>0,'Translation-EN'!A1281,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1281)>0,'Translation-EN'!B1281,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1281)>0,'Translation-EN'!C1281,\"\")","v":"B13"},{"$f":"IF(LEN('Translation-EN'!D1281)>0,'Translation-EN'!D1281,\"\")","v":""},"Bardeaux d’asphalte"]
[{"$f":"IF(LEN('Translation-EN'!A1282)>0,'Translation-EN'!A1282,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1282)>0,'Translation-EN'!B1282,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1282)>0,'Translation-EN'!C1282,\"\")","v":"C13"},{"$f":"IF(LEN('Translation-EN'!D1282)>0,'Translation-EN'!D1282,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Inclus : Atlas, BP, CertainTeed, GAF, IKO, Malarkey, Owens Corning, Pabco"]
[{"$f":"IF(LEN('Translation-EN'!A1283)>0,'Translation-EN'!A1283,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1283)>0,'Translation-EN'!B1283,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1283)>0,'Translation-EN'!C1283,\"\")","v":"B14"},{"$f":"IF(LEN('Translation-EN'!D1283)>0,'Translation-EN'!D1283,\"\")","v":""},{"$f":"$E$1281","v":"Bardeaux d’asphalte"}]
[{"$f":"IF(LEN('Translation-EN'!A1284)>0,'Translation-EN'!A1284,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1284)>0,'Translation-EN'!B1284,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1284)>0,'Translation-EN'!C1284,\"\")","v":"C14"},{"$f":"IF(LEN('Translation-EN'!D1284)>0,'Translation-EN'!D1284,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"GAF"]
[{"$f":"IF(LEN('Translation-EN'!A1285)>0,'Translation-EN'!A1285,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1285)>0,'Translation-EN'!B1285,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1285)>0,'Translation-EN'!C1285,\"\")","v":"D14"},{"$f":"IF(LEN('Translation-EN'!D1285)>0,'Translation-EN'!D1285,\"\")","v":""},"Timberline"]
[{"$f":"IF(LEN('Translation-EN'!A1286)>0,'Translation-EN'!A1286,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1286)>0,'Translation-EN'!B1286,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1286)>0,'Translation-EN'!C1286,\"\")","v":"E14"},{"$f":"IF(LEN('Translation-EN'!D1286)>0,'Translation-EN'!D1286,\"\")","v":""},{"$f":"$E$1285","v":"Timberline"}]
[{"$f":"IF(LEN('Translation-EN'!A1287)>0,'Translation-EN'!A1287,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1287)>0,'Translation-EN'!B1287,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1287)>0,'Translation-EN'!C1287,\"\")","v":"B15"},{"$f":"IF(LEN('Translation-EN'!D1287)>0,'Translation-EN'!D1287,\"\")","v":""},{"$f":"$E$1281","v":"Bardeaux d’asphalte"}]
[{"$f":"IF(LEN('Translation-EN'!A1288)>0,'Translation-EN'!A1288,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1288)>0,'Translation-EN'!B1288,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1288)>0,'Translation-EN'!C1288,\"\")","v":"C15"},{"$f":"IF(LEN('Translation-EN'!D1288)>0,'Translation-EN'!D1288,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Owens Corning"]
[{"$f":"IF(LEN('Translation-EN'!A1289)>0,'Translation-EN'!A1289,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1289)>0,'Translation-EN'!B1289,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1289)>0,'Translation-EN'!C1289,\"\")","v":"D15"},{"$f":"IF(LEN('Translation-EN'!D1289)>0,'Translation-EN'!D1289,\"\")","v":""},"Durée"]
[{"$f":"IF(LEN('Translation-EN'!A1290)>0,'Translation-EN'!A1290,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1290)>0,'Translation-EN'!B1290,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1290)>0,'Translation-EN'!C1290,\"\")","v":"B16"},{"$f":"IF(LEN('Translation-EN'!D1290)>0,'Translation-EN'!D1290,\"\")","v":""},{"$f":"$E$1281","v":"Bardeaux d’asphalte"}]
[{"$f":"IF(LEN('Translation-EN'!A1291)>0,'Translation-EN'!A1291,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1291)>0,'Translation-EN'!B1291,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1291)>0,'Translation-EN'!C1291,\"\")","v":"C16"},{"$f":"IF(LEN('Translation-EN'!D1291)>0,'Translation-EN'!D1291,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1288","v":"Owens Corning"}]
[{"$f":"IF(LEN('Translation-EN'!A1292)>0,'Translation-EN'!A1292,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1292)>0,'Translation-EN'!B1292,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1292)>0,'Translation-EN'!C1292,\"\")","v":"D16"},{"$f":"IF(LEN('Translation-EN'!D1292)>0,'Translation-EN'!D1292,\"\")","v":""},"Oakridge"]
[{"$f":"IF(LEN('Translation-EN'!A1293)>0,'Translation-EN'!A1293,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1293)>0,'Translation-EN'!B1293,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1293)>0,'Translation-EN'!C1293,\"\")","v":"B17"},{"$f":"IF(LEN('Translation-EN'!D1293)>0,'Translation-EN'!D1293,\"\")","v":""},{"$f":"$E$1281","v":"Bardeaux d’asphalte"}]
[{"$f":"IF(LEN('Translation-EN'!A1294)>0,'Translation-EN'!A1294,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1294)>0,'Translation-EN'!B1294,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1294)>0,'Translation-EN'!C1294,\"\")","v":"C17"},{"$f":"IF(LEN('Translation-EN'!D1294)>0,'Translation-EN'!D1294,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1288","v":"Owens Corning"}]
[{"$f":"IF(LEN('Translation-EN'!A1295)>0,'Translation-EN'!A1295,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1295)>0,'Translation-EN'!B1295,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1295)>0,'Translation-EN'!C1295,\"\")","v":"D17"},{"$f":"IF(LEN('Translation-EN'!D1295)>0,'Translation-EN'!D1295,\"\")","v":""},"Supreme"]
[{"$f":"IF(LEN('Translation-EN'!A1296)>0,'Translation-EN'!A1296,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1296)>0,'Translation-EN'!B1296,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1296)>0,'Translation-EN'!C1296,\"\")","v":"B18"},{"$f":"IF(LEN('Translation-EN'!D1296)>0,'Translation-EN'!D1296,\"\")","v":""},"Contreplaqué de bambou"]
[{"$f":"IF(LEN('Translation-EN'!A1297)>0,'Translation-EN'!A1297,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1297)>0,'Translation-EN'!B1297,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1297)>0,'Translation-EN'!C1297,\"\")","v":"C18"},{"$f":"IF(LEN('Translation-EN'!D1297)>0,'Translation-EN'!D1297,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Smith & Fong"]
[{"$f":"IF(LEN('Translation-EN'!A1298)>0,'Translation-EN'!A1298,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1298)>0,'Translation-EN'!B1298,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1298)>0,'Translation-EN'!C1298,\"\")","v":"D18"},{"$f":"IF(LEN('Translation-EN'!D1298)>0,'Translation-EN'!D1298,\"\")","v":""},"Plyboo"]
[{"$f":"IF(LEN('Translation-EN'!A1299)>0,'Translation-EN'!A1299,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1299)>0,'Translation-EN'!B1299,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1299)>0,'Translation-EN'!C1299,\"\")","v":"E18"},{"$f":"IF(LEN('Translation-EN'!D1299)>0,'Translation-EN'!D1299,\"\")","v":""},"1/2 po (12,7 mm)"]
[{"$f":"IF(LEN('Translation-EN'!A1300)>0,'Translation-EN'!A1300,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1300)>0,'Translation-EN'!B1300,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1300)>0,'Translation-EN'!C1300,\"\")","v":"B19"},{"$f":"IF(LEN('Translation-EN'!D1300)>0,'Translation-EN'!D1300,\"\")","v":""},"Tuile BioBased"]
[{"$f":"IF(LEN('Translation-EN'!A1301)>0,'Translation-EN'!A1301,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1301)>0,'Translation-EN'!B1301,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1301)>0,'Translation-EN'!C1301,\"\")","v":"C19"},{"$f":"IF(LEN('Translation-EN'!D1301)>0,'Translation-EN'!D1301,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Armstrong"]
[{"$f":"IF(LEN('Translation-EN'!A1302)>0,'Translation-EN'!A1302,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1302)>0,'Translation-EN'!B1302,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1302)>0,'Translation-EN'!C1302,\"\")","v":"D19"},{"$f":"IF(LEN('Translation-EN'!D1302)>0,'Translation-EN'!D1302,\"\")","v":""},{"$f":"$E$1300","v":"Tuile BioBased"}]
[{"$f":"IF(LEN('Translation-EN'!A1303)>0,'Translation-EN'!A1303,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1303)>0,'Translation-EN'!B1303,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1303)>0,'Translation-EN'!C1303,\"\")","v":"E19"},{"$f":"IF(LEN('Translation-EN'!D1303)>0,'Translation-EN'!D1303,\"\")","v":""},"Non-PVC avec liant polyester BioStride, Striations BBT et Migrations BBT"]
[{"$f":"IF(LEN('Translation-EN'!A1304)>0,'Translation-EN'!A1304,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1304)>0,'Translation-EN'!B1304,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1304)>0,'Translation-EN'!C1304,\"\")","v":"B20"},{"$f":"IF(LEN('Translation-EN'!D1304)>0,'Translation-EN'!D1304,\"\")","v":""},"Brique, silicate de calcium"]
[{"$f":"IF(LEN('Translation-EN'!A1305)>0,'Translation-EN'!A1305,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1305)>0,'Translation-EN'!B1305,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1305)>0,'Translation-EN'!C1305,\"\")","v":"C20"},{"$f":"IF(LEN('Translation-EN'!D1305)>0,'Translation-EN'!D1305,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Arriscraft"]
[{"$f":"IF(LEN('Translation-EN'!A1306)>0,'Translation-EN'!A1306,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1306)>0,'Translation-EN'!B1306,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1306)>0,'Translation-EN'!C1306,\"\")","v":"D20"},{"$f":"IF(LEN('Translation-EN'!D1306)>0,'Translation-EN'!D1306,\"\")","v":""},"Brique contemporaine"]
[{"$f":"IF(LEN('Translation-EN'!A1307)>0,'Translation-EN'!A1307,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1307)>0,'Translation-EN'!B1307,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1307)>0,'Translation-EN'!C1307,\"\")","v":"E20"},{"$f":"IF(LEN('Translation-EN'!D1307)>0,'Translation-EN'!D1307,\"\")","v":""},"3-1/8 po x 3-1/2 po x n’importe quelle longueur, mortier et attaches inclus"]
[{"$f":"IF(LEN('Translation-EN'!A1308)>0,'Translation-EN'!A1308,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1308)>0,'Translation-EN'!B1308,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1308)>0,'Translation-EN'!C1308,\"\")","v":"B21"},{"$f":"IF(LEN('Translation-EN'!D1308)>0,'Translation-EN'!D1308,\"\")","v":""},"Brique, ciment"]
[{"$f":"IF(LEN('Translation-EN'!A1309)>0,'Translation-EN'!A1309,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1309)>0,'Translation-EN'!B1309,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1309)>0,'Translation-EN'!C1309,\"\")","v":"C21"},{"$f":"IF(LEN('Translation-EN'!D1309)>0,'Translation-EN'!D1309,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"MidWest"]
[{"$f":"IF(LEN('Translation-EN'!A1310)>0,'Translation-EN'!A1310,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1310)>0,'Translation-EN'!B1310,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1310)>0,'Translation-EN'!C1310,\"\")","v":"D21"},{"$f":"IF(LEN('Translation-EN'!D1310)>0,'Translation-EN'!D1310,\"\")","v":""},"Brique de façade architecturale"]
[{"$f":"IF(LEN('Translation-EN'!A1311)>0,'Translation-EN'!A1311,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1311)>0,'Translation-EN'!B1311,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1311)>0,'Translation-EN'!C1311,\"\")","v":"E21"},{"$f":"IF(LEN('Translation-EN'!D1311)>0,'Translation-EN'!D1311,\"\")","v":""},"3-5/8 po x 2-3/4 po x 7-5/8 po (92 x 70 x 194 mm), mortier de 3/8 po inclus3-5/8 po x 2-3/4 po x 7-5/8 po (92 x 70 x 194 mm) avec mortier de 3/8 po "]
[{"$f":"IF(LEN('Translation-EN'!A1312)>0,'Translation-EN'!A1312,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1312)>0,'Translation-EN'!B1312,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1312)>0,'Translation-EN'!C1312,\"\")","v":"B22"},{"$f":"IF(LEN('Translation-EN'!D1312)>0,'Translation-EN'!D1312,\"\")","v":""},"Brique, argile"]
[{"$f":"IF(LEN('Translation-EN'!A1313)>0,'Translation-EN'!A1313,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1313)>0,'Translation-EN'!B1313,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1313)>0,'Translation-EN'!C1313,\"\")","v":"C22"},{"$f":"IF(LEN('Translation-EN'!D1313)>0,'Translation-EN'!D1313,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Interstate"]
[{"$f":"IF(LEN('Translation-EN'!A1314)>0,'Translation-EN'!A1314,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1314)>0,'Translation-EN'!B1314,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1314)>0,'Translation-EN'!C1314,\"\")","v":"D22"},{"$f":"IF(LEN('Translation-EN'!D1314)>0,'Translation-EN'!D1314,\"\")","v":""},"Brique moyenne de façade"]
[{"$f":"IF(LEN('Translation-EN'!A1315)>0,'Translation-EN'!A1315,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1315)>0,'Translation-EN'!B1315,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1315)>0,'Translation-EN'!C1315,\"\")","v":"E22"},{"$f":"IF(LEN('Translation-EN'!D1315)>0,'Translation-EN'!D1315,\"\")","v":""},{"$f":"$E$1311","v":"3-5/8 po x 2-3/4 po x 7-5/8 po (92 x 70 x 194 mm), mortier de 3/8 po inclus3-5/8 po x 2-3/4 po x 7-5/8 po (92 x 70 x 194 mm) avec mortier de 3/8 po "}]
[{"$f":"IF(LEN('Translation-EN'!A1316)>0,'Translation-EN'!A1316,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1316)>0,'Translation-EN'!B1316,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1316)>0,'Translation-EN'!C1316,\"\")","v":"B23"},{"$f":"IF(LEN('Translation-EN'!D1316)>0,'Translation-EN'!D1316,\"\")","v":""},{"$f":"$E$1312","v":"Brique, argile"}]
[{"$f":"IF(LEN('Translation-EN'!A1317)>0,'Translation-EN'!A1317,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1317)>0,'Translation-EN'!B1317,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1317)>0,'Translation-EN'!C1317,\"\")","v":"C23"},{"$f":"IF(LEN('Translation-EN'!D1317)>0,'Translation-EN'!D1317,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1313","v":"Interstate"}]
[{"$f":"IF(LEN('Translation-EN'!A1318)>0,'Translation-EN'!A1318,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1318)>0,'Translation-EN'!B1318,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1318)>0,'Translation-EN'!C1318,\"\")","v":"D23"},{"$f":"IF(LEN('Translation-EN'!D1318)>0,'Translation-EN'!D1318,\"\")","v":""},"Brique moyenne mince de façade"]
[{"$f":"IF(LEN('Translation-EN'!A1319)>0,'Translation-EN'!A1319,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1319)>0,'Translation-EN'!B1319,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1319)>0,'Translation-EN'!C1319,\"\")","v":"E23"},{"$f":"IF(LEN('Translation-EN'!D1319)>0,'Translation-EN'!D1319,\"\")","v":""},"3-9/16 po x 5/8 po x 11-5/8 po (90 x 16 mm x 295) avec mortier de 3/8 po."]
[{"$f":"IF(LEN('Translation-EN'!A1320)>0,'Translation-EN'!A1320,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1320)>0,'Translation-EN'!B1320,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1320)>0,'Translation-EN'!C1320,\"\")","v":"B24"},{"$f":"IF(LEN('Translation-EN'!D1320)>0,'Translation-EN'!D1320,\"\")","v":""},"Brique, argile, générique modulaire"]
[{"$f":"IF(LEN('Translation-EN'!A1321)>0,'Translation-EN'!A1321,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1321)>0,'Translation-EN'!B1321,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1321)>0,'Translation-EN'!C1321,\"\")","v":"C24"},{"$f":"IF(LEN('Translation-EN'!D1321)>0,'Translation-EN'!D1321,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Association de l’industrie de la brique"]
[{"$f":"IF(LEN('Translation-EN'!A1322)>0,'Translation-EN'!A1322,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1322)>0,'Translation-EN'!B1322,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1322)>0,'Translation-EN'!C1322,\"\")","v":"D24"},{"$f":"IF(LEN('Translation-EN'!D1322)>0,'Translation-EN'!D1322,\"\")","v":""},"Moyenne de l’industrie États-Unis–Canada"]
[{"$f":"IF(LEN('Translation-EN'!A1323)>0,'Translation-EN'!A1323,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1323)>0,'Translation-EN'!B1323,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1323)>0,'Translation-EN'!C1323,\"\")","v":"E24"},{"$f":"IF(LEN('Translation-EN'!D1323)>0,'Translation-EN'!D1323,\"\")","v":""},"3-5/8 po x 2-3/4 po x 7-5/8 po, avec mortier de 3/8 po "]
[{"$f":"IF(LEN('Translation-EN'!A1324)>0,'Translation-EN'!A1324,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1324)>0,'Translation-EN'!B1324,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1324)>0,'Translation-EN'!C1324,\"\")","v":"B25"},{"$f":"IF(LEN('Translation-EN'!D1324)>0,'Translation-EN'!D1324,\"\")","v":""},{"$f":"$E$1312","v":"Brique, argile"}]
[{"$f":"IF(LEN('Translation-EN'!A1325)>0,'Translation-EN'!A1325,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1325)>0,'Translation-EN'!B1325,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1325)>0,'Translation-EN'!C1325,\"\")","v":"C25"},{"$f":"IF(LEN('Translation-EN'!D1325)>0,'Translation-EN'!D1325,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1321","v":"Association de l’industrie de la brique"}]
[{"$f":"IF(LEN('Translation-EN'!A1326)>0,'Translation-EN'!A1326,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1326)>0,'Translation-EN'!B1326,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1326)>0,'Translation-EN'!C1326,\"\")","v":"D25"},{"$f":"IF(LEN('Translation-EN'!D1326)>0,'Translation-EN'!D1326,\"\")","v":""},"Moyenne de l’industrie États-Unis–Canada"]
[{"$f":"IF(LEN('Translation-EN'!A1327)>0,'Translation-EN'!A1327,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1327)>0,'Translation-EN'!B1327,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1327)>0,'Translation-EN'!C1327,\"\")","v":"B26"},{"$f":"IF(LEN('Translation-EN'!D1327)>0,'Translation-EN'!D1327,\"\")","v":""},"Tapis"]
[{"$f":"IF(LEN('Translation-EN'!A1328)>0,'Translation-EN'!A1328,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1328)>0,'Translation-EN'!B1328,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1328)>0,'Translation-EN'!C1328,\"\")","v":"E26"},{"$f":"IF(LEN('Translation-EN'!D1328)>0,'Translation-EN'!D1328,\"\")","v":""},"Moyenne de 150 échantillons dans la base de données EC3"]
[{"$f":"IF(LEN('Translation-EN'!A1329)>0,'Translation-EN'!A1329,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1329)>0,'Translation-EN'!B1329,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1329)>0,'Translation-EN'!C1329,\"\")","v":"B27"},{"$f":"IF(LEN('Translation-EN'!D1329)>0,'Translation-EN'!D1329,\"\")","v":""},{"$f":"$E$1327","v":"Tapis"}]
[{"$f":"IF(LEN('Translation-EN'!A1330)>0,'Translation-EN'!A1330,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1330)>0,'Translation-EN'!B1330,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1330)>0,'Translation-EN'!C1330,\"\")","v":"D27"},{"$f":"IF(LEN('Translation-EN'!D1330)>0,'Translation-EN'!D1330,\"\")","v":""},"Réalisable à partir d’EC3"]
[{"$f":"IF(LEN('Translation-EN'!A1331)>0,'Translation-EN'!A1331,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1331)>0,'Translation-EN'!B1331,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1331)>0,'Translation-EN'!C1331,\"\")","v":"E27"},{"$f":"IF(LEN('Translation-EN'!D1331)>0,'Translation-EN'!D1331,\"\")","v":""},"Réalisable à partir de 150 échantillons dans la base de données EC3"]
[{"$f":"IF(LEN('Translation-EN'!A1332)>0,'Translation-EN'!A1332,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1332)>0,'Translation-EN'!B1332,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1332)>0,'Translation-EN'!C1332,\"\")","v":"B28"},{"$f":"IF(LEN('Translation-EN'!D1332)>0,'Translation-EN'!D1332,\"\")","v":""},{"$f":"$E$1327","v":"Tapis"}]
[{"$f":"IF(LEN('Translation-EN'!A1333)>0,'Translation-EN'!A1333,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1333)>0,'Translation-EN'!B1333,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1333)>0,'Translation-EN'!C1333,\"\")","v":"D28"},{"$f":"IF(LEN('Translation-EN'!D1333)>0,'Translation-EN'!D1333,\"\")","v":""},"Conservateur à partir d’EC3"]
[{"$f":"IF(LEN('Translation-EN'!A1334)>0,'Translation-EN'!A1334,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1334)>0,'Translation-EN'!B1334,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1334)>0,'Translation-EN'!C1334,\"\")","v":"E28"},{"$f":"IF(LEN('Translation-EN'!D1334)>0,'Translation-EN'!D1334,\"\")","v":""},"Conservateur à partir de 150 échantillons dans la base de données EC3"]
[{"$f":"IF(LEN('Translation-EN'!A1335)>0,'Translation-EN'!A1335,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1335)>0,'Translation-EN'!B1335,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1335)>0,'Translation-EN'!C1335,\"\")","v":"B29"},{"$f":"IF(LEN('Translation-EN'!D1335)>0,'Translation-EN'!D1335,\"\")","v":""},{"$f":"$E$1327","v":"Tapis"}]
[{"$f":"IF(LEN('Translation-EN'!A1336)>0,'Translation-EN'!A1336,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1336)>0,'Translation-EN'!B1336,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1336)>0,'Translation-EN'!C1336,\"\")","v":"C29"},{"$f":"IF(LEN('Translation-EN'!D1336)>0,'Translation-EN'!D1336,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Interface"]
[{"$f":"IF(LEN('Translation-EN'!A1337)>0,'Translation-EN'!A1337,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1337)>0,'Translation-EN'!B1337,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1337)>0,'Translation-EN'!C1337,\"\")","v":"D29"},{"$f":"IF(LEN('Translation-EN'!D1337)>0,'Translation-EN'!D1337,\"\")","v":""},"GLASBAC® RE, Nylon"]
[{"$f":"IF(LEN('Translation-EN'!A1338)>0,'Translation-EN'!A1338,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1338)>0,'Translation-EN'!B1338,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1338)>0,'Translation-EN'!C1338,\"\")","v":"E29"},{"$f":"IF(LEN('Translation-EN'!D1338)>0,'Translation-EN'!D1338,\"\")","v":""},"Tapis en dalles modulaires (recyclage en circuit fermé)"]
[{"$f":"IF(LEN('Translation-EN'!A1339)>0,'Translation-EN'!A1339,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1339)>0,'Translation-EN'!B1339,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1339)>0,'Translation-EN'!C1339,\"\")","v":"B30"},{"$f":"IF(LEN('Translation-EN'!D1339)>0,'Translation-EN'!D1339,\"\")","v":""},{"$f":"$E$1327","v":"Tapis"}]
[{"$f":"IF(LEN('Translation-EN'!A1340)>0,'Translation-EN'!A1340,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1340)>0,'Translation-EN'!B1340,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1340)>0,'Translation-EN'!C1340,\"\")","v":"C30"},{"$f":"IF(LEN('Translation-EN'!D1340)>0,'Translation-EN'!D1340,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1336","v":"Interface"}]
[{"$f":"IF(LEN('Translation-EN'!A1341)>0,'Translation-EN'!A1341,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1341)>0,'Translation-EN'!B1341,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1341)>0,'Translation-EN'!C1341,\"\")","v":"D30"},{"$f":"IF(LEN('Translation-EN'!D1341)>0,'Translation-EN'!D1341,\"\")","v":""},"Cquest BioX"]
[{"$f":"IF(LEN('Translation-EN'!A1342)>0,'Translation-EN'!A1342,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1342)>0,'Translation-EN'!B1342,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1342)>0,'Translation-EN'!C1342,\"\")","v":"E30"},{"$f":"IF(LEN('Translation-EN'!D1342)>0,'Translation-EN'!D1342,\"\")","v":""},"1,5 mm Tapis à dalles modulaires"]
[{"$f":"IF(LEN('Translation-EN'!A1343)>0,'Translation-EN'!A1343,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1343)>0,'Translation-EN'!B1343,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1343)>0,'Translation-EN'!C1343,\"\")","v":"B31"},{"$f":"IF(LEN('Translation-EN'!D1343)>0,'Translation-EN'!D1343,\"\")","v":""},"Bardeaux/bardeaux en fentes en cèdre"]
[{"$f":"IF(LEN('Translation-EN'!A1344)>0,'Translation-EN'!A1344,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1344)>0,'Translation-EN'!B1344,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1344)>0,'Translation-EN'!C1344,\"\")","v":"E31"},{"$f":"IF(LEN('Translation-EN'!D1344)>0,'Translation-EN'!D1344,\"\")","v":""},"couverture 3/4 po."]
[{"$f":"IF(LEN('Translation-EN'!A1345)>0,'Translation-EN'!A1345,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1345)>0,'Translation-EN'!B1345,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1345)>0,'Translation-EN'!C1345,\"\")","v":"B32"},{"$f":"IF(LEN('Translation-EN'!D1345)>0,'Translation-EN'!D1345,\"\")","v":""},"Bardage de cèdre"]
[{"$f":"IF(LEN('Translation-EN'!A1346)>0,'Translation-EN'!A1346,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1346)>0,'Translation-EN'!B1346,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1346)>0,'Translation-EN'!C1346,\"\")","v":"C32"},{"$f":"IF(LEN('Translation-EN'!D1346)>0,'Translation-EN'!D1346,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Western Red Cedar Lumber Assn"]
[{"$f":"IF(LEN('Translation-EN'!A1347)>0,'Translation-EN'!A1347,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1347)>0,'Translation-EN'!B1347,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1347)>0,'Translation-EN'!C1347,\"\")","v":"E32"},{"$f":"IF(LEN('Translation-EN'!D1347)>0,'Translation-EN'!D1347,\"\")","v":""},"Planches 1 x 6"]
[{"$f":"IF(LEN('Translation-EN'!A1348)>0,'Translation-EN'!A1348,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1348)>0,'Translation-EN'!B1348,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1348)>0,'Translation-EN'!C1348,\"\")","v":"B33"},{"$f":"IF(LEN('Translation-EN'!D1348)>0,'Translation-EN'!D1348,\"\")","v":""},"Cellulose – Natte"]
[{"$f":"IF(LEN('Translation-EN'!A1349)>0,'Translation-EN'!A1349,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1349)>0,'Translation-EN'!B1349,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1349)>0,'Translation-EN'!C1349,\"\")","v":"C33"},{"$f":"IF(LEN('Translation-EN'!D1349)>0,'Translation-EN'!D1349,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"CMS"]
[{"$f":"IF(LEN('Translation-EN'!A1350)>0,'Translation-EN'!A1350,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1350)>0,'Translation-EN'!B1350,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1350)>0,'Translation-EN'!C1350,\"\")","v":"D33"},{"$f":"IF(LEN('Translation-EN'!D1350)>0,'Translation-EN'!D1350,\"\")","v":""},"EcoCell"]
[{"$f":"IF(LEN('Translation-EN'!A1351)>0,'Translation-EN'!A1351,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1351)>0,'Translation-EN'!B1351,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1351)>0,'Translation-EN'!C1351,\"\")","v":"E33"},{"$f":"IF(LEN('Translation-EN'!D1351)>0,'Translation-EN'!D1351,\"\")","v":""},"R 3,6/po"]
[{"$f":"IF(LEN('Translation-EN'!A1352)>0,'Translation-EN'!A1352,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1352)>0,'Translation-EN'!B1352,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1352)>0,'Translation-EN'!C1352,\"\")","v":"B34"},{"$f":"IF(LEN('Translation-EN'!D1352)>0,'Translation-EN'!D1352,\"\")","v":""},"Cellulose – paquet dense"]
[{"$f":"IF(LEN('Translation-EN'!A1353)>0,'Translation-EN'!A1353,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1353)>0,'Translation-EN'!B1353,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1353)>0,'Translation-EN'!C1353,\"\")","v":"D34"},{"$f":"IF(LEN('Translation-EN'!D1353)>0,'Translation-EN'!D1353,\"\")","v":""},"Inclus : AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"]
[{"$f":"IF(LEN('Translation-EN'!A1354)>0,'Translation-EN'!A1354,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1354)>0,'Translation-EN'!B1354,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1354)>0,'Translation-EN'!C1354,\"\")","v":"E34"},{"$f":"IF(LEN('Translation-EN'!D1354)>0,'Translation-EN'!D1354,\"\")","v":""},"R 3,7/po"]
[{"$f":"IF(LEN('Translation-EN'!A1355)>0,'Translation-EN'!A1355,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1355)>0,'Translation-EN'!B1355,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1355)>0,'Translation-EN'!C1355,\"\")","v":"B35"},{"$f":"IF(LEN('Translation-EN'!D1355)>0,'Translation-EN'!D1355,\"\")","v":""},"Cellulose en vrac"]
[{"$f":"IF(LEN('Translation-EN'!A1356)>0,'Translation-EN'!A1356,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1356)>0,'Translation-EN'!B1356,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1356)>0,'Translation-EN'!C1356,\"\")","v":"D35"},{"$f":"IF(LEN('Translation-EN'!D1356)>0,'Translation-EN'!D1356,\"\")","v":""},"Inclus : AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"]
[{"$f":"IF(LEN('Translation-EN'!A1357)>0,'Translation-EN'!A1357,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1357)>0,'Translation-EN'!B1357,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1357)>0,'Translation-EN'!C1357,\"\")","v":"E35"},{"$f":"IF(LEN('Translation-EN'!D1357)>0,'Translation-EN'!D1357,\"\")","v":""},{"$f":"$E$1354","v":"R 3,7/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1358)>0,'Translation-EN'!A1358,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1358)>0,'Translation-EN'!B1358,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1358)>0,'Translation-EN'!C1358,\"\")","v":"B36"},{"$f":"IF(LEN('Translation-EN'!D1358)>0,'Translation-EN'!D1358,\"\")","v":""},"Cellulose – appliquée par pulvérisation"]
[{"$f":"IF(LEN('Translation-EN'!A1359)>0,'Translation-EN'!A1359,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1359)>0,'Translation-EN'!B1359,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1359)>0,'Translation-EN'!C1359,\"\")","v":"C36"},{"$f":"IF(LEN('Translation-EN'!D1359)>0,'Translation-EN'!D1359,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"International Cellulose Corp."]
[{"$f":"IF(LEN('Translation-EN'!A1360)>0,'Translation-EN'!A1360,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1360)>0,'Translation-EN'!B1360,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1360)>0,'Translation-EN'!C1360,\"\")","v":"D36"},{"$f":"IF(LEN('Translation-EN'!D1360)>0,'Translation-EN'!D1360,\"\")","v":""},"K-13, ThermoCon"]
[{"$f":"IF(LEN('Translation-EN'!A1361)>0,'Translation-EN'!A1361,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1361)>0,'Translation-EN'!B1361,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1361)>0,'Translation-EN'!C1361,\"\")","v":"E36"},{"$f":"IF(LEN('Translation-EN'!D1361)>0,'Translation-EN'!D1361,\"\")","v":""},"R 3,75/po"]
[{"$f":"IF(LEN('Translation-EN'!A1362)>0,'Translation-EN'!A1362,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1362)>0,'Translation-EN'!B1362,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1362)>0,'Translation-EN'!C1362,\"\")","v":"B37"},{"$f":"IF(LEN('Translation-EN'!D1362)>0,'Translation-EN'!D1362,\"\")","v":""},"Panneau de ciment 1/2 po"]
[{"$f":"IF(LEN('Translation-EN'!A1363)>0,'Translation-EN'!A1363,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1363)>0,'Translation-EN'!B1363,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1363)>0,'Translation-EN'!C1363,\"\")","v":"C37"},{"$f":"IF(LEN('Translation-EN'!D1363)>0,'Translation-EN'!D1363,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"USG"]
[{"$f":"IF(LEN('Translation-EN'!A1364)>0,'Translation-EN'!A1364,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1364)>0,'Translation-EN'!B1364,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1364)>0,'Translation-EN'!C1364,\"\")","v":"D37"},{"$f":"IF(LEN('Translation-EN'!D1364)>0,'Translation-EN'!D1364,\"\")","v":""},"Durock (132)"]
[{"$f":"IF(LEN('Translation-EN'!A1365)>0,'Translation-EN'!A1365,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1365)>0,'Translation-EN'!B1365,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1365)>0,'Translation-EN'!C1365,\"\")","v":"E37"},{"$f":"IF(LEN('Translation-EN'!D1365)>0,'Translation-EN'!D1365,\"\")","v":""},{"$f":"$E$1299","v":"1/2 po (12,7 mm)"}]
[{"$f":"IF(LEN('Translation-EN'!A1366)>0,'Translation-EN'!A1366,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1366)>0,'Translation-EN'!B1366,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1366)>0,'Translation-EN'!C1366,\"\")","v":"B38"},{"$f":"IF(LEN('Translation-EN'!D1366)>0,'Translation-EN'!D1366,\"\")","v":""},{"$f":"$E$1362","v":"Panneau de ciment 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A1367)>0,'Translation-EN'!A1367,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1367)>0,'Translation-EN'!B1367,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1367)>0,'Translation-EN'!C1367,\"\")","v":"C38"},{"$f":"IF(LEN('Translation-EN'!D1367)>0,'Translation-EN'!D1367,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1363","v":"USG"}]
[{"$f":"IF(LEN('Translation-EN'!A1368)>0,'Translation-EN'!A1368,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1368)>0,'Translation-EN'!B1368,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1368)>0,'Translation-EN'!C1368,\"\")","v":"D38"},{"$f":"IF(LEN('Translation-EN'!D1368)>0,'Translation-EN'!D1368,\"\")","v":""},"Durock (133)"]
[{"$f":"IF(LEN('Translation-EN'!A1369)>0,'Translation-EN'!A1369,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1369)>0,'Translation-EN'!B1369,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1369)>0,'Translation-EN'!C1369,\"\")","v":"E38"},{"$f":"IF(LEN('Translation-EN'!D1369)>0,'Translation-EN'!D1369,\"\")","v":""},{"$f":"$E$1299","v":"1/2 po (12,7 mm)"}]
[{"$f":"IF(LEN('Translation-EN'!A1370)>0,'Translation-EN'!A1370,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1370)>0,'Translation-EN'!B1370,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1370)>0,'Translation-EN'!C1370,\"\")","v":"B39"},{"$f":"IF(LEN('Translation-EN'!D1370)>0,'Translation-EN'!D1370,\"\")","v":""},"Mortier de ciment, carreaux"]
[{"$f":"IF(LEN('Translation-EN'!A1371)>0,'Translation-EN'!A1371,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1371)>0,'Translation-EN'!B1371,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1371)>0,'Translation-EN'!C1371,\"\")","v":"C39"},{"$f":"IF(LEN('Translation-EN'!D1371)>0,'Translation-EN'!D1371,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Conseil des carreaux d’Amérique du Nord"]
[{"$f":"IF(LEN('Translation-EN'!A1372)>0,'Translation-EN'!A1372,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1372)>0,'Translation-EN'!B1372,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1372)>0,'Translation-EN'!C1372,\"\")","v":"E39"},{"$f":"IF(LEN('Translation-EN'!D1372)>0,'Translation-EN'!D1372,\"\")","v":""},"Moyenne de l’industrie. Comprend les mortiers de ciment à prise sèche, à prise sèche modifiée et à prise sèche modifiée améliorée."]
[{"$f":"IF(LEN('Translation-EN'!A1373)>0,'Translation-EN'!A1373,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1373)>0,'Translation-EN'!B1373,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1373)>0,'Translation-EN'!C1373,\"\")","v":"B40"},{"$f":"IF(LEN('Translation-EN'!D1373)>0,'Translation-EN'!D1373,\"\")","v":""},"Carreaux en céramique"]
[{"$f":"IF(LEN('Translation-EN'!A1374)>0,'Translation-EN'!A1374,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1374)>0,'Translation-EN'!B1374,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1374)>0,'Translation-EN'!C1374,\"\")","v":"C40"},{"$f":"IF(LEN('Translation-EN'!D1374)>0,'Translation-EN'!D1374,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Crossville"]
[{"$f":"IF(LEN('Translation-EN'!A1375)>0,'Translation-EN'!A1375,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1375)>0,'Translation-EN'!B1375,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1375)>0,'Translation-EN'!C1375,\"\")","v":"D40"},{"$f":"IF(LEN('Translation-EN'!D1375)>0,'Translation-EN'!D1375,\"\")","v":""},"Porcelaine"]
[{"$f":"IF(LEN('Translation-EN'!A1376)>0,'Translation-EN'!A1376,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1376)>0,'Translation-EN'!B1376,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1376)>0,'Translation-EN'!C1376,\"\")","v":"E40"},{"$f":"IF(LEN('Translation-EN'!D1376)>0,'Translation-EN'!D1376,\"\")","v":""},"Grade standard"]
[{"$f":"IF(LEN('Translation-EN'!A1377)>0,'Translation-EN'!A1377,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1377)>0,'Translation-EN'!B1377,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1377)>0,'Translation-EN'!C1377,\"\")","v":"B41"},{"$f":"IF(LEN('Translation-EN'!D1377)>0,'Translation-EN'!D1377,\"\")","v":""},{"$f":"$E$1373","v":"Carreaux en céramique"}]
[{"$f":"IF(LEN('Translation-EN'!A1378)>0,'Translation-EN'!A1378,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1378)>0,'Translation-EN'!B1378,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1378)>0,'Translation-EN'!C1378,\"\")","v":"C41"},{"$f":"IF(LEN('Translation-EN'!D1378)>0,'Translation-EN'!D1378,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"StonePeak "]
[{"$f":"IF(LEN('Translation-EN'!A1379)>0,'Translation-EN'!A1379,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1379)>0,'Translation-EN'!B1379,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1379)>0,'Translation-EN'!C1379,\"\")","v":"D41"},{"$f":"IF(LEN('Translation-EN'!D1379)>0,'Translation-EN'!D1379,\"\")","v":""},{"$f":"$E$1375","v":"Porcelaine"}]
[{"$f":"IF(LEN('Translation-EN'!A1380)>0,'Translation-EN'!A1380,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1380)>0,'Translation-EN'!B1380,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1380)>0,'Translation-EN'!C1380,\"\")","v":"E41"},{"$f":"IF(LEN('Translation-EN'!D1380)>0,'Translation-EN'!D1380,\"\")","v":""},"Porcelaine, grade standard"]
[{"$f":"IF(LEN('Translation-EN'!A1381)>0,'Translation-EN'!A1381,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1381)>0,'Translation-EN'!B1381,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1381)>0,'Translation-EN'!C1381,\"\")","v":"B42"},{"$f":"IF(LEN('Translation-EN'!D1381)>0,'Translation-EN'!D1381,\"\")","v":""},{"$f":"$E$1373","v":"Carreaux en céramique"}]
[{"$f":"IF(LEN('Translation-EN'!A1382)>0,'Translation-EN'!A1382,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1382)>0,'Translation-EN'!B1382,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1382)>0,'Translation-EN'!C1382,\"\")","v":"C42"},{"$f":"IF(LEN('Translation-EN'!D1382)>0,'Translation-EN'!D1382,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1371","v":"Conseil des carreaux d’Amérique du Nord"}]
[{"$f":"IF(LEN('Translation-EN'!A1383)>0,'Translation-EN'!A1383,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1383)>0,'Translation-EN'!B1383,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1383)>0,'Translation-EN'!C1383,\"\")","v":"E42"},{"$f":"IF(LEN('Translation-EN'!D1383)>0,'Translation-EN'!D1383,\"\")","v":""},"Moyenne de l’industrie. Comprend les carreaux de porcelaine, les carreaux pressés, les mosaïques et les carreaux de carrière."]
[{"$f":"IF(LEN('Translation-EN'!A1384)>0,'Translation-EN'!A1384,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1384)>0,'Translation-EN'!B1384,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1384)>0,'Translation-EN'!C1384,\"\")","v":"B43"},{"$f":"IF(LEN('Translation-EN'!D1384)>0,'Translation-EN'!D1384,\"\")","v":""},"Plâtre d’argile"]
[{"$f":"IF(LEN('Translation-EN'!A1385)>0,'Translation-EN'!A1385,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1385)>0,'Translation-EN'!B1385,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1385)>0,'Translation-EN'!C1385,\"\")","v":"C43"},{"$f":"IF(LEN('Translation-EN'!D1385)>0,'Translation-EN'!D1385,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Mélangé sur place"]
[{"$f":"IF(LEN('Translation-EN'!A1386)>0,'Translation-EN'!A1386,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1386)>0,'Translation-EN'!B1386,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1386)>0,'Translation-EN'!C1386,\"\")","v":"E43"},{"$f":"IF(LEN('Translation-EN'!D1386)>0,'Translation-EN'!D1386,\"\")","v":""},"15 mm"]
[{"$f":"IF(LEN('Translation-EN'!A1387)>0,'Translation-EN'!A1387,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1387)>0,'Translation-EN'!B1387,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1387)>0,'Translation-EN'!C1387,\"\")","v":"B44"},{"$f":"IF(LEN('Translation-EN'!D1387)>0,'Translation-EN'!D1387,\"\")","v":""},"Tuiles en terre cuite"]
[{"$f":"IF(LEN('Translation-EN'!A1388)>0,'Translation-EN'!A1388,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1388)>0,'Translation-EN'!B1388,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1388)>0,'Translation-EN'!C1388,\"\")","v":"C44"},{"$f":"IF(LEN('Translation-EN'!D1388)>0,'Translation-EN'!D1388,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"HISPALYT"]
[{"$f":"IF(LEN('Translation-EN'!A1389)>0,'Translation-EN'!A1389,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1389)>0,'Translation-EN'!B1389,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1389)>0,'Translation-EN'!C1389,\"\")","v":"B45"},{"$f":"IF(LEN('Translation-EN'!D1389)>0,'Translation-EN'!D1389,\"\")","v":""},"EMB –légers"]
[{"$f":"IF(LEN('Translation-EN'!A1390)>0,'Translation-EN'!A1390,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1390)>0,'Translation-EN'!B1390,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1390)>0,'Translation-EN'!C1390,\"\")","v":"C45"},{"$f":"IF(LEN('Translation-EN'!D1390)>0,'Translation-EN'!D1390,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Angelus Block Co."]
[{"$f":"IF(LEN('Translation-EN'!A1391)>0,'Translation-EN'!A1391,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1391)>0,'Translation-EN'!B1391,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1391)>0,'Translation-EN'!C1391,\"\")","v":"D45"},{"$f":"IF(LEN('Translation-EN'!D1391)>0,'Translation-EN'!D1391,\"\")","v":""},"Blocs légers de 8 po"]
[{"$f":"IF(LEN('Translation-EN'!A1392)>0,'Translation-EN'!A1392,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1392)>0,'Translation-EN'!B1392,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1392)>0,'Translation-EN'!C1392,\"\")","v":"E45"},{"$f":"IF(LEN('Translation-EN'!D1392)>0,'Translation-EN'!D1392,\"\")","v":""},"Précision 9 x 8 x 16 "]
[{"$f":"IF(LEN('Translation-EN'!A1393)>0,'Translation-EN'!A1393,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1393)>0,'Translation-EN'!B1393,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1393)>0,'Translation-EN'!C1393,\"\")","v":"B46"},{"$f":"IF(LEN('Translation-EN'!D1393)>0,'Translation-EN'!D1393,\"\")","v":""},{"$f":"$E$1389","v":"EMB –légers"}]
[{"$f":"IF(LEN('Translation-EN'!A1394)>0,'Translation-EN'!A1394,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1394)>0,'Translation-EN'!B1394,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1394)>0,'Translation-EN'!C1394,\"\")","v":"C46"},{"$f":"IF(LEN('Translation-EN'!D1394)>0,'Translation-EN'!D1394,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Brique Brampton"]
[{"$f":"IF(LEN('Translation-EN'!A1395)>0,'Translation-EN'!A1395,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1395)>0,'Translation-EN'!B1395,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1395)>0,'Translation-EN'!C1395,\"\")","v":"D46"},{"$f":"IF(LEN('Translation-EN'!D1395)>0,'Translation-EN'!D1395,\"\")","v":""},"Blocs légers 8 po avec traitement au carbone"]
[{"$f":"IF(LEN('Translation-EN'!A1396)>0,'Translation-EN'!A1396,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1396)>0,'Translation-EN'!B1396,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1396)>0,'Translation-EN'!C1396,\"\")","v":"E46"},{"$f":"IF(LEN('Translation-EN'!D1396)>0,'Translation-EN'!D1396,\"\")","v":""},"Traitement au carbone 15 MPa"]
[{"$f":"IF(LEN('Translation-EN'!A1397)>0,'Translation-EN'!A1397,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1397)>0,'Translation-EN'!B1397,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1397)>0,'Translation-EN'!C1397,\"\")","v":"B47"},{"$f":"IF(LEN('Translation-EN'!D1397)>0,'Translation-EN'!D1397,\"\")","v":""},{"$f":"$E$1389","v":"EMB –légers"}]
[{"$f":"IF(LEN('Translation-EN'!A1398)>0,'Translation-EN'!A1398,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1398)>0,'Translation-EN'!B1398,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1398)>0,'Translation-EN'!C1398,\"\")","v":"C47"},{"$f":"IF(LEN('Translation-EN'!D1398)>0,'Translation-EN'!D1398,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Association canadienne des producteurs de maçonnerie en béton"]
[{"$f":"IF(LEN('Translation-EN'!A1399)>0,'Translation-EN'!A1399,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1399)>0,'Translation-EN'!B1399,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1399)>0,'Translation-EN'!C1399,\"\")","v":"D47"},{"$f":"IF(LEN('Translation-EN'!D1399)>0,'Translation-EN'!D1399,\"\")","v":""},{"$f":"$E$1391","v":"Blocs légers de 8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A1400)>0,'Translation-EN'!A1400,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1400)>0,'Translation-EN'!B1400,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1400)>0,'Translation-EN'!C1400,\"\")","v":"E47"},{"$f":"IF(LEN('Translation-EN'!D1400)>0,'Translation-EN'!D1400,\"\")","v":""},"390 x 190 x 190 mm"]
[{"$f":"IF(LEN('Translation-EN'!A1401)>0,'Translation-EN'!A1401,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1401)>0,'Translation-EN'!B1401,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1401)>0,'Translation-EN'!C1401,\"\")","v":"B49"},{"$f":"IF(LEN('Translation-EN'!D1401)>0,'Translation-EN'!D1401,\"\")","v":""},"EMB –poids normal"]
[{"$f":"IF(LEN('Translation-EN'!A1402)>0,'Translation-EN'!A1402,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1402)>0,'Translation-EN'!B1402,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1402)>0,'Translation-EN'!C1402,\"\")","v":"C49"},{"$f":"IF(LEN('Translation-EN'!D1402)>0,'Translation-EN'!D1402,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1390","v":"Angelus Block Co."}]
[{"$f":"IF(LEN('Translation-EN'!A1403)>0,'Translation-EN'!A1403,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1403)>0,'Translation-EN'!B1403,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1403)>0,'Translation-EN'!C1403,\"\")","v":"D49"},{"$f":"IF(LEN('Translation-EN'!D1403)>0,'Translation-EN'!D1403,\"\")","v":""},"Blocs de poids normal de 8 po"]
[{"$f":"IF(LEN('Translation-EN'!A1404)>0,'Translation-EN'!A1404,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1404)>0,'Translation-EN'!B1404,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1404)>0,'Translation-EN'!C1404,\"\")","v":"E49"},{"$f":"IF(LEN('Translation-EN'!D1404)>0,'Translation-EN'!D1404,\"\")","v":""},"Précision 8 x 8 x 16"]
[{"$f":"IF(LEN('Translation-EN'!A1405)>0,'Translation-EN'!A1405,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1405)>0,'Translation-EN'!B1405,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1405)>0,'Translation-EN'!C1405,\"\")","v":"B50"},{"$f":"IF(LEN('Translation-EN'!D1405)>0,'Translation-EN'!D1405,\"\")","v":""},{"$f":"$E$1401","v":"EMB –poids normal"}]
[{"$f":"IF(LEN('Translation-EN'!A1406)>0,'Translation-EN'!A1406,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1406)>0,'Translation-EN'!B1406,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1406)>0,'Translation-EN'!C1406,\"\")","v":"C50"},{"$f":"IF(LEN('Translation-EN'!D1406)>0,'Translation-EN'!D1406,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1398","v":"Association canadienne des producteurs de maçonnerie en béton"}]
[{"$f":"IF(LEN('Translation-EN'!A1407)>0,'Translation-EN'!A1407,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1407)>0,'Translation-EN'!B1407,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1407)>0,'Translation-EN'!C1407,\"\")","v":"D50"},{"$f":"IF(LEN('Translation-EN'!D1407)>0,'Translation-EN'!D1407,\"\")","v":""},{"$f":"$E$1403","v":"Blocs de poids normal de 8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A1408)>0,'Translation-EN'!A1408,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1408)>0,'Translation-EN'!B1408,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1408)>0,'Translation-EN'!C1408,\"\")","v":"E50"},{"$f":"IF(LEN('Translation-EN'!D1408)>0,'Translation-EN'!D1408,\"\")","v":""},"390 x 190 x 190 mm"]
[{"$f":"IF(LEN('Translation-EN'!A1409)>0,'Translation-EN'!A1409,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1409)>0,'Translation-EN'!B1409,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1409)>0,'Translation-EN'!C1409,\"\")","v":"B52"},{"$f":"IF(LEN('Translation-EN'!D1409)>0,'Translation-EN'!D1409,\"\")","v":""},{"$f":"$E$1401","v":"EMB –poids normal"}]
[{"$f":"IF(LEN('Translation-EN'!A1410)>0,'Translation-EN'!A1410,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1410)>0,'Translation-EN'!B1410,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1410)>0,'Translation-EN'!C1410,\"\")","v":"C52"},{"$f":"IF(LEN('Translation-EN'!D1410)>0,'Translation-EN'!D1410,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Permacon"]
[{"$f":"IF(LEN('Translation-EN'!A1411)>0,'Translation-EN'!A1411,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1411)>0,'Translation-EN'!B1411,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1411)>0,'Translation-EN'!C1411,\"\")","v":"D52"},{"$f":"IF(LEN('Translation-EN'!D1411)>0,'Translation-EN'!D1411,\"\")","v":""},{"$f":"$E$1403","v":"Blocs de poids normal de 8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A1412)>0,'Translation-EN'!A1412,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1412)>0,'Translation-EN'!B1412,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1412)>0,'Translation-EN'!C1412,\"\")","v":"E52"},{"$f":"IF(LEN('Translation-EN'!D1412)>0,'Translation-EN'!D1412,\"\")","v":""},"NW STD 20 CM GLPW"]
[{"$f":"IF(LEN('Translation-EN'!A1413)>0,'Translation-EN'!A1413,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1413)>0,'Translation-EN'!B1413,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1413)>0,'Translation-EN'!C1413,\"\")","v":"B53"},{"$f":"IF(LEN('Translation-EN'!D1413)>0,'Translation-EN'!D1413,\"\")","v":""},"EMB –Terre battue"]
[{"$f":"IF(LEN('Translation-EN'!A1414)>0,'Translation-EN'!A1414,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1414)>0,'Translation-EN'!B1414,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1414)>0,'Translation-EN'!C1414,\"\")","v":"C53"},{"$f":"IF(LEN('Translation-EN'!D1414)>0,'Translation-EN'!D1414,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Matériaux Watershed"]
[{"$f":"IF(LEN('Translation-EN'!A1415)>0,'Translation-EN'!A1415,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1415)>0,'Translation-EN'!B1415,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1415)>0,'Translation-EN'!C1415,\"\")","v":"D53"},{"$f":"IF(LEN('Translation-EN'!D1415)>0,'Translation-EN'!D1415,\"\")","v":""},"Bloc Watershed"]
[{"$f":"IF(LEN('Translation-EN'!A1416)>0,'Translation-EN'!A1416,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1416)>0,'Translation-EN'!B1416,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1416)>0,'Translation-EN'!C1416,\"\")","v":"B54"},{"$f":"IF(LEN('Translation-EN'!D1416)>0,'Translation-EN'!D1416,\"\")","v":""},{"$f":"$E$1413","v":"EMB –Terre battue"}]
[{"$f":"IF(LEN('Translation-EN'!A1417)>0,'Translation-EN'!A1417,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1417)>0,'Translation-EN'!B1417,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1417)>0,'Translation-EN'!C1417,\"\")","v":"C54"},{"$f":"IF(LEN('Translation-EN'!D1417)>0,'Translation-EN'!D1417,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1414","v":"Matériaux Watershed"}]
[{"$f":"IF(LEN('Translation-EN'!A1418)>0,'Translation-EN'!A1418,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1418)>0,'Translation-EN'!B1418,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1418)>0,'Translation-EN'!C1418,\"\")","v":"D54"},{"$f":"IF(LEN('Translation-EN'!D1418)>0,'Translation-EN'!D1418,\"\")","v":""},"ZeroBlock Watershed"]
[{"$f":"IF(LEN('Translation-EN'!A1419)>0,'Translation-EN'!A1419,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1419)>0,'Translation-EN'!B1419,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1419)>0,'Translation-EN'!C1419,\"\")","v":"B55"},{"$f":"IF(LEN('Translation-EN'!D1419)>0,'Translation-EN'!D1419,\"\")","v":""},"Plancher de terre"]
[{"$f":"IF(LEN('Translation-EN'!A1420)>0,'Translation-EN'!A1420,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1420)>0,'Translation-EN'!B1420,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1420)>0,'Translation-EN'!C1420,\"\")","v":"C55"},{"$f":"IF(LEN('Translation-EN'!D1420)>0,'Translation-EN'!D1420,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Fait sur place"]
[{"$f":"IF(LEN('Translation-EN'!A1421)>0,'Translation-EN'!A1421,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1421)>0,'Translation-EN'!B1421,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1421)>0,'Translation-EN'!C1421,\"\")","v":"E55"},{"$f":"IF(LEN('Translation-EN'!D1421)>0,'Translation-EN'!D1421,\"\")","v":""},"3 po torchis, 1 po plâtre d’argile"]
[{"$f":"IF(LEN('Translation-EN'!A1422)>0,'Translation-EN'!A1422,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1422)>0,'Translation-EN'!B1422,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1422)>0,'Translation-EN'!C1422,\"\")","v":"B56"},{"$f":"IF(LEN('Translation-EN'!D1422)>0,'Translation-EN'!D1422,\"\")","v":""},"Mur de torchis"]
[{"$f":"IF(LEN('Translation-EN'!A1423)>0,'Translation-EN'!A1423,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1423)>0,'Translation-EN'!B1423,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1423)>0,'Translation-EN'!C1423,\"\")","v":"C56"},{"$f":"IF(LEN('Translation-EN'!D1423)>0,'Translation-EN'!D1423,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1385","v":"Mélangé sur place"}]
[{"$f":"IF(LEN('Translation-EN'!A1424)>0,'Translation-EN'!A1424,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1424)>0,'Translation-EN'!B1424,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1424)>0,'Translation-EN'!C1424,\"\")","v":"E56"},{"$f":"IF(LEN('Translation-EN'!D1424)>0,'Translation-EN'!D1424,\"\")","v":""},"18 po (457 mm) épaisseur moyenne"]
[{"$f":"IF(LEN('Translation-EN'!A1425)>0,'Translation-EN'!A1425,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1425)>0,'Translation-EN'!B1425,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1425)>0,'Translation-EN'!C1425,\"\")","v":"B57"},{"$f":"IF(LEN('Translation-EN'!D1425)>0,'Translation-EN'!D1425,\"\")","v":""},"Bloc de terre comprimée"]
[{"$f":"IF(LEN('Translation-EN'!A1426)>0,'Translation-EN'!A1426,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1426)>0,'Translation-EN'!B1426,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1426)>0,'Translation-EN'!C1426,\"\")","v":"C57"},{"$f":"IF(LEN('Translation-EN'!D1426)>0,'Translation-EN'!D1426,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Fabriqué en usine"]
[{"$f":"IF(LEN('Translation-EN'!A1427)>0,'Translation-EN'!A1427,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1427)>0,'Translation-EN'!B1427,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1427)>0,'Translation-EN'!C1427,\"\")","v":"D57"},{"$f":"IF(LEN('Translation-EN'!D1427)>0,'Translation-EN'!D1427,\"\")","v":""},"Stabilisé avec 6,5 % de CHN"]
[{"$f":"IF(LEN('Translation-EN'!A1428)>0,'Translation-EN'!A1428,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1428)>0,'Translation-EN'!B1428,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1428)>0,'Translation-EN'!C1428,\"\")","v":"E57"},{"$f":"IF(LEN('Translation-EN'!D1428)>0,'Translation-EN'!D1428,\"\")","v":""},"31,5 x 6 x 2,75 po (300 x 150 x 70 mm)"]
[{"$f":"IF(LEN('Translation-EN'!A1429)>0,'Translation-EN'!A1429,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1429)>0,'Translation-EN'!B1429,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1429)>0,'Translation-EN'!C1429,\"\")","v":"B58"},{"$f":"IF(LEN('Translation-EN'!D1429)>0,'Translation-EN'!D1429,\"\")","v":""},"Panneau de paille comprimée"]
[{"$f":"IF(LEN('Translation-EN'!A1430)>0,'Translation-EN'!A1430,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1430)>0,'Translation-EN'!B1430,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1430)>0,'Translation-EN'!C1430,\"\")","v":"C58"},{"$f":"IF(LEN('Translation-EN'!D1430)>0,'Translation-EN'!D1430,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Stramit"]
[{"$f":"IF(LEN('Translation-EN'!A1431)>0,'Translation-EN'!A1431,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1431)>0,'Translation-EN'!B1431,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1431)>0,'Translation-EN'!C1431,\"\")","v":"D58"},{"$f":"IF(LEN('Translation-EN'!D1431)>0,'Translation-EN'!D1431,\"\")","v":""},"Planche de 60 mm"]
[{"$f":"IF(LEN('Translation-EN'!A1432)>0,'Translation-EN'!A1432,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1432)>0,'Translation-EN'!B1432,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1432)>0,'Translation-EN'!C1432,\"\")","v":"E58"},{"$f":"IF(LEN('Translation-EN'!D1432)>0,'Translation-EN'!D1432,\"\")","v":""},"R 3,9/po"]
[{"$f":"IF(LEN('Translation-EN'!A1433)>0,'Translation-EN'!A1433,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1433)>0,'Translation-EN'!B1433,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1433)>0,'Translation-EN'!C1433,\"\")","v":"B59"},{"$f":"IF(LEN('Translation-EN'!D1433)>0,'Translation-EN'!D1433,\"\")","v":""},"Béton"]
[{"$f":"IF(LEN('Translation-EN'!A1434)>0,'Translation-EN'!A1434,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1434)>0,'Translation-EN'!B1434,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1434)>0,'Translation-EN'!C1434,\"\")","v":"C59"},{"$f":"IF(LEN('Translation-EN'!D1434)>0,'Translation-EN'!D1434,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Béton Butler"]
[{"$f":"IF(LEN('Translation-EN'!A1435)>0,'Translation-EN'!A1435,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1435)>0,'Translation-EN'!B1435,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1435)>0,'Translation-EN'!C1435,\"\")","v":"D59"},{"$f":"IF(LEN('Translation-EN'!D1435)>0,'Translation-EN'!D1435,\"\")","v":""},"Moyenne de 19 mélanges différents de 25 MPa"]
[{"$f":"IF(LEN('Translation-EN'!A1436)>0,'Translation-EN'!A1436,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1436)>0,'Translation-EN'!B1436,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1436)>0,'Translation-EN'!C1436,\"\")","v":"B60"},{"$f":"IF(LEN('Translation-EN'!D1436)>0,'Translation-EN'!D1436,\"\")","v":""},"Béton – 0-25 MPa, référence moyenne de l’industrie"]
[{"$f":"IF(LEN('Translation-EN'!A1437)>0,'Translation-EN'!A1437,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1437)>0,'Translation-EN'!B1437,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1437)>0,'Translation-EN'!C1437,\"\")","v":"C60"},{"$f":"IF(LEN('Translation-EN'!D1437)>0,'Translation-EN'!D1437,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"ANBP"]
[{"$f":"IF(LEN('Translation-EN'!A1438)>0,'Translation-EN'!A1438,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1438)>0,'Translation-EN'!B1438,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1438)>0,'Translation-EN'!C1438,\"\")","v":"D60"},{"$f":"IF(LEN('Translation-EN'!D1438)>0,'Translation-EN'!D1438,\"\")","v":""},"Moy. can."]
[{"$f":"IF(LEN('Translation-EN'!A1439)>0,'Translation-EN'!A1439,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1439)>0,'Translation-EN'!B1439,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1439)>0,'Translation-EN'!C1439,\"\")","v":"B61"},{"$f":"IF(LEN('Translation-EN'!D1439)>0,'Translation-EN'!D1439,\"\")","v":""},"Béton – 0-25 MPa, 0-14 % FA/SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1440)>0,'Translation-EN'!A1440,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1440)>0,'Translation-EN'!B1440,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1440)>0,'Translation-EN'!C1440,\"\")","v":"C61"},{"$f":"IF(LEN('Translation-EN'!D1440)>0,'Translation-EN'!D1440,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1441)>0,'Translation-EN'!A1441,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1441)>0,'Translation-EN'!B1441,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1441)>0,'Translation-EN'!C1441,\"\")","v":"D61"},{"$f":"IF(LEN('Translation-EN'!D1441)>0,'Translation-EN'!D1441,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1442)>0,'Translation-EN'!A1442,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1442)>0,'Translation-EN'!B1442,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1442)>0,'Translation-EN'!C1442,\"\")","v":"B62"},{"$f":"IF(LEN('Translation-EN'!D1442)>0,'Translation-EN'!D1442,\"\")","v":""},"Béton – 0-25 MPa, 15-29 % de cendres volantes, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1443)>0,'Translation-EN'!A1443,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1443)>0,'Translation-EN'!B1443,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1443)>0,'Translation-EN'!C1443,\"\")","v":"C62"},{"$f":"IF(LEN('Translation-EN'!D1443)>0,'Translation-EN'!D1443,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1444)>0,'Translation-EN'!A1444,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1444)>0,'Translation-EN'!B1444,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1444)>0,'Translation-EN'!C1444,\"\")","v":"D62"},{"$f":"IF(LEN('Translation-EN'!D1444)>0,'Translation-EN'!D1444,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1445)>0,'Translation-EN'!A1445,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1445)>0,'Translation-EN'!B1445,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1445)>0,'Translation-EN'!C1445,\"\")","v":"B63"},{"$f":"IF(LEN('Translation-EN'!D1445)>0,'Translation-EN'!D1445,\"\")","v":""},"Béton – 0-25 MPa, 30-40 % de cendres volantes, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1446)>0,'Translation-EN'!A1446,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1446)>0,'Translation-EN'!B1446,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1446)>0,'Translation-EN'!C1446,\"\")","v":"C63"},{"$f":"IF(LEN('Translation-EN'!D1446)>0,'Translation-EN'!D1446,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1447)>0,'Translation-EN'!A1447,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1447)>0,'Translation-EN'!B1447,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1447)>0,'Translation-EN'!C1447,\"\")","v":"D63"},{"$f":"IF(LEN('Translation-EN'!D1447)>0,'Translation-EN'!D1447,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1448)>0,'Translation-EN'!A1448,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1448)>0,'Translation-EN'!B1448,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1448)>0,'Translation-EN'!C1448,\"\")","v":"B64"},{"$f":"IF(LEN('Translation-EN'!D1448)>0,'Translation-EN'!D1448,\"\")","v":""},"Béton – 0-25 MPa, 25-34 % de scories, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1449)>0,'Translation-EN'!A1449,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1449)>0,'Translation-EN'!B1449,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1449)>0,'Translation-EN'!C1449,\"\")","v":"C64"},{"$f":"IF(LEN('Translation-EN'!D1449)>0,'Translation-EN'!D1449,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1450)>0,'Translation-EN'!A1450,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1450)>0,'Translation-EN'!B1450,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1450)>0,'Translation-EN'!C1450,\"\")","v":"D64"},{"$f":"IF(LEN('Translation-EN'!D1450)>0,'Translation-EN'!D1450,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1451)>0,'Translation-EN'!A1451,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1451)>0,'Translation-EN'!B1451,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1451)>0,'Translation-EN'!C1451,\"\")","v":"B65"},{"$f":"IF(LEN('Translation-EN'!D1451)>0,'Translation-EN'!D1451,\"\")","v":""},"Béton – 0-25 MPa, 35-50 % de scories, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1452)>0,'Translation-EN'!A1452,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1452)>0,'Translation-EN'!B1452,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1452)>0,'Translation-EN'!C1452,\"\")","v":"C65"},{"$f":"IF(LEN('Translation-EN'!D1452)>0,'Translation-EN'!D1452,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1453)>0,'Translation-EN'!A1453,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1453)>0,'Translation-EN'!B1453,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1453)>0,'Translation-EN'!C1453,\"\")","v":"D65"},{"$f":"IF(LEN('Translation-EN'!D1453)>0,'Translation-EN'!D1453,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1454)>0,'Translation-EN'!A1454,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1454)>0,'Translation-EN'!B1454,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1454)>0,'Translation-EN'!C1454,\"\")","v":"B66"},{"$f":"IF(LEN('Translation-EN'!D1454)>0,'Translation-EN'!D1454,\"\")","v":""},"Béton – 26-30 MPa, moyenne de référence canadienne"]
[{"$f":"IF(LEN('Translation-EN'!A1455)>0,'Translation-EN'!A1455,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1455)>0,'Translation-EN'!B1455,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1455)>0,'Translation-EN'!C1455,\"\")","v":"C66"},{"$f":"IF(LEN('Translation-EN'!D1455)>0,'Translation-EN'!D1455,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1456)>0,'Translation-EN'!A1456,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1456)>0,'Translation-EN'!B1456,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1456)>0,'Translation-EN'!C1456,\"\")","v":"D66"},{"$f":"IF(LEN('Translation-EN'!D1456)>0,'Translation-EN'!D1456,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1457)>0,'Translation-EN'!A1457,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1457)>0,'Translation-EN'!B1457,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1457)>0,'Translation-EN'!C1457,\"\")","v":"B67"},{"$f":"IF(LEN('Translation-EN'!D1457)>0,'Translation-EN'!D1457,\"\")","v":""},"Béton – 26-30 MPa, 0-14 % FA/SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1458)>0,'Translation-EN'!A1458,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1458)>0,'Translation-EN'!B1458,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1458)>0,'Translation-EN'!C1458,\"\")","v":"C67"},{"$f":"IF(LEN('Translation-EN'!D1458)>0,'Translation-EN'!D1458,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1459)>0,'Translation-EN'!A1459,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1459)>0,'Translation-EN'!B1459,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1459)>0,'Translation-EN'!C1459,\"\")","v":"D67"},{"$f":"IF(LEN('Translation-EN'!D1459)>0,'Translation-EN'!D1459,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1460)>0,'Translation-EN'!A1460,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1460)>0,'Translation-EN'!B1460,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1460)>0,'Translation-EN'!C1460,\"\")","v":"B68"},{"$f":"IF(LEN('Translation-EN'!D1460)>0,'Translation-EN'!D1460,\"\")","v":""},"Béton – 26-30 MPa, 15-29 % de cendres volantes, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1461)>0,'Translation-EN'!A1461,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1461)>0,'Translation-EN'!B1461,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1461)>0,'Translation-EN'!C1461,\"\")","v":"C68"},{"$f":"IF(LEN('Translation-EN'!D1461)>0,'Translation-EN'!D1461,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1462)>0,'Translation-EN'!A1462,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1462)>0,'Translation-EN'!B1462,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1462)>0,'Translation-EN'!C1462,\"\")","v":"D68"},{"$f":"IF(LEN('Translation-EN'!D1462)>0,'Translation-EN'!D1462,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1463)>0,'Translation-EN'!A1463,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1463)>0,'Translation-EN'!B1463,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1463)>0,'Translation-EN'!C1463,\"\")","v":"B69"},{"$f":"IF(LEN('Translation-EN'!D1463)>0,'Translation-EN'!D1463,\"\")","v":""},"Béton – 26-30 MPa, 30-40 % de cendres volantes, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1464)>0,'Translation-EN'!A1464,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1464)>0,'Translation-EN'!B1464,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1464)>0,'Translation-EN'!C1464,\"\")","v":"C69"},{"$f":"IF(LEN('Translation-EN'!D1464)>0,'Translation-EN'!D1464,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1465)>0,'Translation-EN'!A1465,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1465)>0,'Translation-EN'!B1465,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1465)>0,'Translation-EN'!C1465,\"\")","v":"D69"},{"$f":"IF(LEN('Translation-EN'!D1465)>0,'Translation-EN'!D1465,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1466)>0,'Translation-EN'!A1466,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1466)>0,'Translation-EN'!B1466,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1466)>0,'Translation-EN'!C1466,\"\")","v":"B70"},{"$f":"IF(LEN('Translation-EN'!D1466)>0,'Translation-EN'!D1466,\"\")","v":""},"Béton – 26-30 MPa, 25-34 % de scories, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1467)>0,'Translation-EN'!A1467,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1467)>0,'Translation-EN'!B1467,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1467)>0,'Translation-EN'!C1467,\"\")","v":"C70"},{"$f":"IF(LEN('Translation-EN'!D1467)>0,'Translation-EN'!D1467,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1468)>0,'Translation-EN'!A1468,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1468)>0,'Translation-EN'!B1468,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1468)>0,'Translation-EN'!C1468,\"\")","v":"D70"},{"$f":"IF(LEN('Translation-EN'!D1468)>0,'Translation-EN'!D1468,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1469)>0,'Translation-EN'!A1469,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1469)>0,'Translation-EN'!B1469,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1469)>0,'Translation-EN'!C1469,\"\")","v":"B71"},{"$f":"IF(LEN('Translation-EN'!D1469)>0,'Translation-EN'!D1469,\"\")","v":""},"Béton – 26-30 MPa, 35-50 % de scories, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1470)>0,'Translation-EN'!A1470,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1470)>0,'Translation-EN'!B1470,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1470)>0,'Translation-EN'!C1470,\"\")","v":"C71"},{"$f":"IF(LEN('Translation-EN'!D1470)>0,'Translation-EN'!D1470,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1471)>0,'Translation-EN'!A1471,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1471)>0,'Translation-EN'!B1471,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1471)>0,'Translation-EN'!C1471,\"\")","v":"D71"},{"$f":"IF(LEN('Translation-EN'!D1471)>0,'Translation-EN'!D1471,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1472)>0,'Translation-EN'!A1472,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1472)>0,'Translation-EN'!B1472,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1472)>0,'Translation-EN'!C1472,\"\")","v":"B72"},{"$f":"IF(LEN('Translation-EN'!D1472)>0,'Translation-EN'!D1472,\"\")","v":""},"Béton – 31-35 MPa, moyenne de référence canadienne"]
[{"$f":"IF(LEN('Translation-EN'!A1473)>0,'Translation-EN'!A1473,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1473)>0,'Translation-EN'!B1473,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1473)>0,'Translation-EN'!C1473,\"\")","v":"C72"},{"$f":"IF(LEN('Translation-EN'!D1473)>0,'Translation-EN'!D1473,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1474)>0,'Translation-EN'!A1474,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1474)>0,'Translation-EN'!B1474,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1474)>0,'Translation-EN'!C1474,\"\")","v":"D72"},{"$f":"IF(LEN('Translation-EN'!D1474)>0,'Translation-EN'!D1474,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1475)>0,'Translation-EN'!A1475,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1475)>0,'Translation-EN'!B1475,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1475)>0,'Translation-EN'!C1475,\"\")","v":"B73"},{"$f":"IF(LEN('Translation-EN'!D1475)>0,'Translation-EN'!D1475,\"\")","v":""},"Béton – 31-35 MPa, 0-14 % FA/SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1476)>0,'Translation-EN'!A1476,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1476)>0,'Translation-EN'!B1476,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1476)>0,'Translation-EN'!C1476,\"\")","v":"C73"},{"$f":"IF(LEN('Translation-EN'!D1476)>0,'Translation-EN'!D1476,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1477)>0,'Translation-EN'!A1477,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1477)>0,'Translation-EN'!B1477,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1477)>0,'Translation-EN'!C1477,\"\")","v":"D73"},{"$f":"IF(LEN('Translation-EN'!D1477)>0,'Translation-EN'!D1477,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1478)>0,'Translation-EN'!A1478,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1478)>0,'Translation-EN'!B1478,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1478)>0,'Translation-EN'!C1478,\"\")","v":"B74"},{"$f":"IF(LEN('Translation-EN'!D1478)>0,'Translation-EN'!D1478,\"\")","v":""},"Béton – 31-35 MPa, 15-29 % de cendres volantes, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1479)>0,'Translation-EN'!A1479,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1479)>0,'Translation-EN'!B1479,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1479)>0,'Translation-EN'!C1479,\"\")","v":"C74"},{"$f":"IF(LEN('Translation-EN'!D1479)>0,'Translation-EN'!D1479,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1480)>0,'Translation-EN'!A1480,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1480)>0,'Translation-EN'!B1480,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1480)>0,'Translation-EN'!C1480,\"\")","v":"D74"},{"$f":"IF(LEN('Translation-EN'!D1480)>0,'Translation-EN'!D1480,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1481)>0,'Translation-EN'!A1481,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1481)>0,'Translation-EN'!B1481,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1481)>0,'Translation-EN'!C1481,\"\")","v":"B75"},{"$f":"IF(LEN('Translation-EN'!D1481)>0,'Translation-EN'!D1481,\"\")","v":""},"Béton – 31-35 MPa, 30-40 % de cendres volantes, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1482)>0,'Translation-EN'!A1482,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1482)>0,'Translation-EN'!B1482,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1482)>0,'Translation-EN'!C1482,\"\")","v":"C75"},{"$f":"IF(LEN('Translation-EN'!D1482)>0,'Translation-EN'!D1482,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1483)>0,'Translation-EN'!A1483,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1483)>0,'Translation-EN'!B1483,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1483)>0,'Translation-EN'!C1483,\"\")","v":"D75"},{"$f":"IF(LEN('Translation-EN'!D1483)>0,'Translation-EN'!D1483,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1484)>0,'Translation-EN'!A1484,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1484)>0,'Translation-EN'!B1484,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1484)>0,'Translation-EN'!C1484,\"\")","v":"B76"},{"$f":"IF(LEN('Translation-EN'!D1484)>0,'Translation-EN'!D1484,\"\")","v":""},"Béton – 31-35 MPa, 25-34 % de scories, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1485)>0,'Translation-EN'!A1485,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1485)>0,'Translation-EN'!B1485,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1485)>0,'Translation-EN'!C1485,\"\")","v":"C76"},{"$f":"IF(LEN('Translation-EN'!D1485)>0,'Translation-EN'!D1485,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1486)>0,'Translation-EN'!A1486,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1486)>0,'Translation-EN'!B1486,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1486)>0,'Translation-EN'!C1486,\"\")","v":"D76"},{"$f":"IF(LEN('Translation-EN'!D1486)>0,'Translation-EN'!D1486,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1487)>0,'Translation-EN'!A1487,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1487)>0,'Translation-EN'!B1487,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1487)>0,'Translation-EN'!C1487,\"\")","v":"B77"},{"$f":"IF(LEN('Translation-EN'!D1487)>0,'Translation-EN'!D1487,\"\")","v":""},"Béton – 31-35 MPa, 35-50 % de scories, GU"]
[{"$f":"IF(LEN('Translation-EN'!A1488)>0,'Translation-EN'!A1488,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1488)>0,'Translation-EN'!B1488,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1488)>0,'Translation-EN'!C1488,\"\")","v":"C77"},{"$f":"IF(LEN('Translation-EN'!D1488)>0,'Translation-EN'!D1488,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1437","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1489)>0,'Translation-EN'!A1489,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1489)>0,'Translation-EN'!B1489,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1489)>0,'Translation-EN'!C1489,\"\")","v":"D77"},{"$f":"IF(LEN('Translation-EN'!D1489)>0,'Translation-EN'!D1489,\"\")","v":""},{"$f":"$E$1438","v":"Moy. can."}]
[{"$f":"IF(LEN('Translation-EN'!A1490)>0,'Translation-EN'!A1490,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1490)>0,'Translation-EN'!B1490,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1490)>0,'Translation-EN'!C1490,\"\")","v":"B78"},{"$f":"IF(LEN('Translation-EN'!D1490)>0,'Translation-EN'!D1490,\"\")","v":""},"Béton – 20 MPa, mélange standard"]
[{"$f":"IF(LEN('Translation-EN'!A1491)>0,'Translation-EN'!A1491,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1491)>0,'Translation-EN'!B1491,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1491)>0,'Translation-EN'!C1491,\"\")","v":"C78"},{"$f":"IF(LEN('Translation-EN'!D1491)>0,'Translation-EN'!D1491,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"ANBP"]
[{"$f":"IF(LEN('Translation-EN'!A1492)>0,'Translation-EN'!A1492,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1492)>0,'Translation-EN'!B1492,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1492)>0,'Translation-EN'!C1492,\"\")","v":"D78"},{"$f":"IF(LEN('Translation-EN'!D1492)>0,'Translation-EN'!D1492,\"\")","v":""},"Moy. É.-U."]
[{"$f":"IF(LEN('Translation-EN'!A1493)>0,'Translation-EN'!A1493,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1493)>0,'Translation-EN'!B1493,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1493)>0,'Translation-EN'!C1493,\"\")","v":"B79"},{"$f":"IF(LEN('Translation-EN'!D1493)>0,'Translation-EN'!D1493,\"\")","v":""},"Béton – 20 MPa, 20-30 % de cendres volantes"]
[{"$f":"IF(LEN('Translation-EN'!A1494)>0,'Translation-EN'!A1494,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1494)>0,'Translation-EN'!B1494,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1494)>0,'Translation-EN'!C1494,\"\")","v":"C79"},{"$f":"IF(LEN('Translation-EN'!D1494)>0,'Translation-EN'!D1494,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1491","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1495)>0,'Translation-EN'!A1495,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1495)>0,'Translation-EN'!B1495,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1495)>0,'Translation-EN'!C1495,\"\")","v":"D79"},{"$f":"IF(LEN('Translation-EN'!D1495)>0,'Translation-EN'!D1495,\"\")","v":""},{"$f":"$E$1492","v":"Moy. É.-U."}]
[{"$f":"IF(LEN('Translation-EN'!A1496)>0,'Translation-EN'!A1496,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1496)>0,'Translation-EN'!B1496,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1496)>0,'Translation-EN'!C1496,\"\")","v":"B80"},{"$f":"IF(LEN('Translation-EN'!D1496)>0,'Translation-EN'!D1496,\"\")","v":""},"Béton – 20 MPa, 30-40 % FA/SL"]
[{"$f":"IF(LEN('Translation-EN'!A1497)>0,'Translation-EN'!A1497,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1497)>0,'Translation-EN'!B1497,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1497)>0,'Translation-EN'!C1497,\"\")","v":"C80"},{"$f":"IF(LEN('Translation-EN'!D1497)>0,'Translation-EN'!D1497,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1491","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1498)>0,'Translation-EN'!A1498,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1498)>0,'Translation-EN'!B1498,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1498)>0,'Translation-EN'!C1498,\"\")","v":"D80"},{"$f":"IF(LEN('Translation-EN'!D1498)>0,'Translation-EN'!D1498,\"\")","v":""},{"$f":"$E$1492","v":"Moy. É.-U."}]
[{"$f":"IF(LEN('Translation-EN'!A1499)>0,'Translation-EN'!A1499,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1499)>0,'Translation-EN'!B1499,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1499)>0,'Translation-EN'!C1499,\"\")","v":"B81"},{"$f":"IF(LEN('Translation-EN'!D1499)>0,'Translation-EN'!D1499,\"\")","v":""},"Béton – 20 MPa mélange 40-50 % FA/SL"]
[{"$f":"IF(LEN('Translation-EN'!A1500)>0,'Translation-EN'!A1500,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1500)>0,'Translation-EN'!B1500,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1500)>0,'Translation-EN'!C1500,\"\")","v":"C81"},{"$f":"IF(LEN('Translation-EN'!D1500)>0,'Translation-EN'!D1500,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1491","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1501)>0,'Translation-EN'!A1501,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1501)>0,'Translation-EN'!B1501,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1501)>0,'Translation-EN'!C1501,\"\")","v":"D81"},{"$f":"IF(LEN('Translation-EN'!D1501)>0,'Translation-EN'!D1501,\"\")","v":""},{"$f":"$E$1492","v":"Moy. É.-U."}]
[{"$f":"IF(LEN('Translation-EN'!A1502)>0,'Translation-EN'!A1502,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1502)>0,'Translation-EN'!B1502,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1502)>0,'Translation-EN'!C1502,\"\")","v":"B82"},{"$f":"IF(LEN('Translation-EN'!D1502)>0,'Translation-EN'!D1502,\"\")","v":""},"Béton – 20 MPa, >50 % de mélange SCM"]
[{"$f":"IF(LEN('Translation-EN'!A1503)>0,'Translation-EN'!A1503,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1503)>0,'Translation-EN'!B1503,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1503)>0,'Translation-EN'!C1503,\"\")","v":"C82"},{"$f":"IF(LEN('Translation-EN'!D1503)>0,'Translation-EN'!D1503,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1491","v":"ANBP"}]
[{"$f":"IF(LEN('Translation-EN'!A1504)>0,'Translation-EN'!A1504,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1504)>0,'Translation-EN'!B1504,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1504)>0,'Translation-EN'!C1504,\"\")","v":"D82"},{"$f":"IF(LEN('Translation-EN'!D1504)>0,'Translation-EN'!D1504,\"\")","v":""},{"$f":"$E$1492","v":"Moy. É.-U."}]
[{"$f":"IF(LEN('Translation-EN'!A1505)>0,'Translation-EN'!A1505,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1505)>0,'Translation-EN'!B1505,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1505)>0,'Translation-EN'!C1505,\"\")","v":"B83"},{"$f":"IF(LEN('Translation-EN'!D1505)>0,'Translation-EN'!D1505,\"\")","v":""},"Isolation en panneaux de liège"]
[{"$f":"IF(LEN('Translation-EN'!A1506)>0,'Translation-EN'!A1506,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1506)>0,'Translation-EN'!B1506,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1506)>0,'Translation-EN'!C1506,\"\")","v":"C83"},{"$f":"IF(LEN('Translation-EN'!D1506)>0,'Translation-EN'!D1506,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Amorim "]
[{"$f":"IF(LEN('Translation-EN'!A1507)>0,'Translation-EN'!A1507,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1507)>0,'Translation-EN'!B1507,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1507)>0,'Translation-EN'!C1507,\"\")","v":"D83"},{"$f":"IF(LEN('Translation-EN'!D1507)>0,'Translation-EN'!D1507,\"\")","v":""},"Isolamentos"]
[{"$f":"IF(LEN('Translation-EN'!A1508)>0,'Translation-EN'!A1508,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1508)>0,'Translation-EN'!B1508,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1508)>0,'Translation-EN'!C1508,\"\")","v":"E83"},{"$f":"IF(LEN('Translation-EN'!D1508)>0,'Translation-EN'!D1508,\"\")","v":""},"R4/po"]
[{"$f":"IF(LEN('Translation-EN'!A1509)>0,'Translation-EN'!A1509,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1509)>0,'Translation-EN'!B1509,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1509)>0,'Translation-EN'!C1509,\"\")","v":"B84"},{"$f":"IF(LEN('Translation-EN'!D1509)>0,'Translation-EN'!D1509,\"\")","v":""},"Plancher de liège"]
[{"$f":"IF(LEN('Translation-EN'!A1510)>0,'Translation-EN'!A1510,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1510)>0,'Translation-EN'!B1510,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1510)>0,'Translation-EN'!C1510,\"\")","v":"C84"},{"$f":"IF(LEN('Translation-EN'!D1510)>0,'Translation-EN'!D1510,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1506","v":"Amorim "}]
[{"$f":"IF(LEN('Translation-EN'!A1511)>0,'Translation-EN'!A1511,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1511)>0,'Translation-EN'!B1511,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1511)>0,'Translation-EN'!C1511,\"\")","v":"D84"},{"$f":"IF(LEN('Translation-EN'!D1511)>0,'Translation-EN'!D1511,\"\")","v":""}," Revestimentos S.A."]
[{"$f":"IF(LEN('Translation-EN'!A1512)>0,'Translation-EN'!A1512,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1512)>0,'Translation-EN'!B1512,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1512)>0,'Translation-EN'!C1512,\"\")","v":"E84"},{"$f":"IF(LEN('Translation-EN'!D1512)>0,'Translation-EN'!D1512,\"\")","v":""},"Planches de plancher flottant en liège"]
[{"$f":"IF(LEN('Translation-EN'!A1513)>0,'Translation-EN'!A1513,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1513)>0,'Translation-EN'!B1513,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1513)>0,'Translation-EN'!C1513,\"\")","v":"B85"},{"$f":"IF(LEN('Translation-EN'!D1513)>0,'Translation-EN'!D1513,\"\")","v":""},{"$f":"$E$1509","v":"Plancher de liège"}]
[{"$f":"IF(LEN('Translation-EN'!A1514)>0,'Translation-EN'!A1514,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1514)>0,'Translation-EN'!B1514,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1514)>0,'Translation-EN'!C1514,\"\")","v":"C85"},{"$f":"IF(LEN('Translation-EN'!D1514)>0,'Translation-EN'!D1514,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Institut européen des fabricants de revêtements de sol résilients"]
[{"$f":"IF(LEN('Translation-EN'!A1515)>0,'Translation-EN'!A1515,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1515)>0,'Translation-EN'!B1515,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1515)>0,'Translation-EN'!C1515,\"\")","v":"D85"},{"$f":"IF(LEN('Translation-EN'!D1515)>0,'Translation-EN'!D1515,\"\")","v":""},"Inclus : Altro, Amorim, Amtico, Artigo, Aspecta, BeauFlor, Dickson, Mflor, Forbo, Gerflor, IVC, Nora, Polyflor, Tarkett, Kahrs, Windmoller"]
[{"$f":"IF(LEN('Translation-EN'!A1516)>0,'Translation-EN'!A1516,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1516)>0,'Translation-EN'!B1516,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1516)>0,'Translation-EN'!C1516,\"\")","v":"E85"},{"$f":"IF(LEN('Translation-EN'!D1516)>0,'Translation-EN'!D1516,\"\")","v":""},"Carreaux de sol en liège"]
[{"$f":"IF(LEN('Translation-EN'!A1517)>0,'Translation-EN'!A1517,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1517)>0,'Translation-EN'!B1517,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1517)>0,'Translation-EN'!C1517,\"\")","v":"B86"},{"$f":"IF(LEN('Translation-EN'!D1517)>0,'Translation-EN'!D1517,\"\")","v":""},"Bois lamellé-croisé (BLC)"]
[{"$f":"IF(LEN('Translation-EN'!A1518)>0,'Translation-EN'!A1518,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1518)>0,'Translation-EN'!B1518,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1518)>0,'Translation-EN'!C1518,\"\")","v":"C86"},{"$f":"IF(LEN('Translation-EN'!D1518)>0,'Translation-EN'!D1518,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Pays nordiques"]
[{"$f":"IF(LEN('Translation-EN'!A1519)>0,'Translation-EN'!A1519,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1519)>0,'Translation-EN'!B1519,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1519)>0,'Translation-EN'!C1519,\"\")","v":"D86"},{"$f":"IF(LEN('Translation-EN'!D1519)>0,'Translation-EN'!D1519,\"\")","v":""},"X- Lam"]
[{"$f":"IF(LEN('Translation-EN'!A1520)>0,'Translation-EN'!A1520,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1520)>0,'Translation-EN'!B1520,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1520)>0,'Translation-EN'!C1520,\"\")","v":"E86"},{"$f":"IF(LEN('Translation-EN'!D1520)>0,'Translation-EN'!D1520,\"\")","v":""},"3-1/2 po (90 mm) d’épaisseur"]
[{"$f":"IF(LEN('Translation-EN'!A1521)>0,'Translation-EN'!A1521,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1521)>0,'Translation-EN'!B1521,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1521)>0,'Translation-EN'!C1521,\"\")","v":"B87"},{"$f":"IF(LEN('Translation-EN'!D1521)>0,'Translation-EN'!D1521,\"\")","v":""},{"$f":"$E$1517","v":"Bois lamellé-croisé (BLC)"}]
[{"$f":"IF(LEN('Translation-EN'!A1522)>0,'Translation-EN'!A1522,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1522)>0,'Translation-EN'!B1522,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1522)>0,'Translation-EN'!C1522,\"\")","v":"C87"},{"$f":"IF(LEN('Translation-EN'!D1522)>0,'Translation-EN'!D1522,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Structurlam"]
[{"$f":"IF(LEN('Translation-EN'!A1523)>0,'Translation-EN'!A1523,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1523)>0,'Translation-EN'!B1523,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1523)>0,'Translation-EN'!C1523,\"\")","v":"D87"},{"$f":"IF(LEN('Translation-EN'!D1523)>0,'Translation-EN'!D1523,\"\")","v":""},"CrossLam"]
[{"$f":"IF(LEN('Translation-EN'!A1524)>0,'Translation-EN'!A1524,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1524)>0,'Translation-EN'!B1524,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1524)>0,'Translation-EN'!C1524,\"\")","v":"E87"},{"$f":"IF(LEN('Translation-EN'!D1524)>0,'Translation-EN'!D1524,\"\")","v":""},{"$f":"$E$1520","v":"3-1/2 po (90 mm) d’épaisseur"}]
[{"$f":"IF(LEN('Translation-EN'!A1525)>0,'Translation-EN'!A1525,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1525)>0,'Translation-EN'!B1525,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1525)>0,'Translation-EN'!C1525,\"\")","v":"B88"},{"$f":"IF(LEN('Translation-EN'!D1525)>0,'Translation-EN'!D1525,\"\")","v":""},"Dowel Laminated Timber"]
[{"$f":"IF(LEN('Translation-EN'!A1526)>0,'Translation-EN'!A1526,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1526)>0,'Translation-EN'!B1526,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1526)>0,'Translation-EN'!C1526,\"\")","v":"C88"},{"$f":"IF(LEN('Translation-EN'!D1526)>0,'Translation-EN'!D1526,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"StructureCraft"]
[{"$f":"IF(LEN('Translation-EN'!A1527)>0,'Translation-EN'!A1527,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1527)>0,'Translation-EN'!B1527,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1527)>0,'Translation-EN'!C1527,\"\")","v":"D88"},{"$f":"IF(LEN('Translation-EN'!D1527)>0,'Translation-EN'!D1527,\"\")","v":""},"DowelLam"]
[{"$f":"IF(LEN('Translation-EN'!A1528)>0,'Translation-EN'!A1528,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1528)>0,'Translation-EN'!B1528,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1528)>0,'Translation-EN'!C1528,\"\")","v":"E88"},{"$f":"IF(LEN('Translation-EN'!D1528)>0,'Translation-EN'!D1528,\"\")","v":""},{"$f":"$E$1520","v":"3-1/2 po (90 mm) d’épaisseur"}]
[{"$f":"IF(LEN('Translation-EN'!A1529)>0,'Translation-EN'!A1529,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1529)>0,'Translation-EN'!B1529,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1529)>0,'Translation-EN'!C1529,\"\")","v":"B89"},{"$f":"IF(LEN('Translation-EN'!D1529)>0,'Translation-EN'!D1529,\"\")","v":""},"Cloisons sèches 1/2 po"]
[{"$f":"IF(LEN('Translation-EN'!A1530)>0,'Translation-EN'!A1530,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1530)>0,'Translation-EN'!B1530,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1530)>0,'Translation-EN'!C1530,\"\")","v":"C89"},{"$f":"IF(LEN('Translation-EN'!D1530)>0,'Translation-EN'!D1530,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"CertainTeed"]
[{"$f":"IF(LEN('Translation-EN'!A1531)>0,'Translation-EN'!A1531,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1531)>0,'Translation-EN'!B1531,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1531)>0,'Translation-EN'!C1531,\"\")","v":"D89"},{"$f":"IF(LEN('Translation-EN'!D1531)>0,'Translation-EN'!D1531,\"\")","v":""},"AirRenew"]
[{"$f":"IF(LEN('Translation-EN'!A1532)>0,'Translation-EN'!A1532,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1532)>0,'Translation-EN'!B1532,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1532)>0,'Translation-EN'!C1532,\"\")","v":"E89"},{"$f":"IF(LEN('Translation-EN'!D1532)>0,'Translation-EN'!D1532,\"\")","v":""},{"$f":"$E$1299","v":"1/2 po (12,7 mm)"}]
[{"$f":"IF(LEN('Translation-EN'!A1533)>0,'Translation-EN'!A1533,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1533)>0,'Translation-EN'!B1533,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1533)>0,'Translation-EN'!C1533,\"\")","v":"B90"},{"$f":"IF(LEN('Translation-EN'!D1533)>0,'Translation-EN'!D1533,\"\")","v":""},{"$f":"$E$1529","v":"Cloisons sèches 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A1534)>0,'Translation-EN'!A1534,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1534)>0,'Translation-EN'!B1534,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1534)>0,'Translation-EN'!C1534,\"\")","v":"C90"},{"$f":"IF(LEN('Translation-EN'!D1534)>0,'Translation-EN'!D1534,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1530","v":"CertainTeed"}]
[{"$f":"IF(LEN('Translation-EN'!A1535)>0,'Translation-EN'!A1535,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1535)>0,'Translation-EN'!B1535,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1535)>0,'Translation-EN'!C1535,\"\")","v":"D90"},{"$f":"IF(LEN('Translation-EN'!D1535)>0,'Translation-EN'!D1535,\"\")","v":""},"Easi-Lite"]
[{"$f":"IF(LEN('Translation-EN'!A1536)>0,'Translation-EN'!A1536,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1536)>0,'Translation-EN'!B1536,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1536)>0,'Translation-EN'!C1536,\"\")","v":"E90"},{"$f":"IF(LEN('Translation-EN'!D1536)>0,'Translation-EN'!D1536,\"\")","v":""},{"$f":"$E$1299","v":"1/2 po (12,7 mm)"}]
[{"$f":"IF(LEN('Translation-EN'!A1537)>0,'Translation-EN'!A1537,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1537)>0,'Translation-EN'!B1537,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1537)>0,'Translation-EN'!C1537,\"\")","v":"B91"},{"$f":"IF(LEN('Translation-EN'!D1537)>0,'Translation-EN'!D1537,\"\")","v":""},{"$f":"$E$1529","v":"Cloisons sèches 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A1538)>0,'Translation-EN'!A1538,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1538)>0,'Translation-EN'!B1538,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1538)>0,'Translation-EN'!C1538,\"\")","v":"C91"},{"$f":"IF(LEN('Translation-EN'!D1538)>0,'Translation-EN'!D1538,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1530","v":"CertainTeed"}]
[{"$f":"IF(LEN('Translation-EN'!A1539)>0,'Translation-EN'!A1539,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1539)>0,'Translation-EN'!B1539,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1539)>0,'Translation-EN'!C1539,\"\")","v":"D91"},{"$f":"IF(LEN('Translation-EN'!D1539)>0,'Translation-EN'!D1539,\"\")","v":""},"M2Tech résistant à l’humidité"]
[{"$f":"IF(LEN('Translation-EN'!A1540)>0,'Translation-EN'!A1540,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1540)>0,'Translation-EN'!B1540,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1540)>0,'Translation-EN'!C1540,\"\")","v":"E91"},{"$f":"IF(LEN('Translation-EN'!D1540)>0,'Translation-EN'!D1540,\"\")","v":""},{"$f":"$E$1299","v":"1/2 po (12,7 mm)"}]
[{"$f":"IF(LEN('Translation-EN'!A1541)>0,'Translation-EN'!A1541,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1541)>0,'Translation-EN'!B1541,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1541)>0,'Translation-EN'!C1541,\"\")","v":"B92"},{"$f":"IF(LEN('Translation-EN'!D1541)>0,'Translation-EN'!D1541,\"\")","v":""},{"$f":"$E$1529","v":"Cloisons sèches 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A1542)>0,'Translation-EN'!A1542,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1542)>0,'Translation-EN'!B1542,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1542)>0,'Translation-EN'!C1542,\"\")","v":"C92"},{"$f":"IF(LEN('Translation-EN'!D1542)>0,'Translation-EN'!D1542,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Pabco"]
[{"$f":"IF(LEN('Translation-EN'!A1543)>0,'Translation-EN'!A1543,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1543)>0,'Translation-EN'!B1543,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1543)>0,'Translation-EN'!C1543,\"\")","v":"D92"},{"$f":"IF(LEN('Translation-EN'!D1543)>0,'Translation-EN'!D1543,\"\")","v":""},"QuietRock"]
[{"$f":"IF(LEN('Translation-EN'!A1544)>0,'Translation-EN'!A1544,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1544)>0,'Translation-EN'!B1544,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1544)>0,'Translation-EN'!C1544,\"\")","v":"E92"},{"$f":"IF(LEN('Translation-EN'!D1544)>0,'Translation-EN'!D1544,\"\")","v":""},"QuietRock 1/2 po"]
[{"$f":"IF(LEN('Translation-EN'!A1545)>0,'Translation-EN'!A1545,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1545)>0,'Translation-EN'!B1545,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1545)>0,'Translation-EN'!C1545,\"\")","v":"B93"},{"$f":"IF(LEN('Translation-EN'!D1545)>0,'Translation-EN'!D1545,\"\")","v":""},"Cloisons sèches 5/8 po"]
[{"$f":"IF(LEN('Translation-EN'!A1546)>0,'Translation-EN'!A1546,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1546)>0,'Translation-EN'!B1546,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1546)>0,'Translation-EN'!C1546,\"\")","v":"D93"},{"$f":"IF(LEN('Translation-EN'!D1546)>0,'Translation-EN'!D1546,\"\")","v":""},"Inclus : American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC"]
[{"$f":"IF(LEN('Translation-EN'!A1547)>0,'Translation-EN'!A1547,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1547)>0,'Translation-EN'!B1547,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1547)>0,'Translation-EN'!C1547,\"\")","v":"B94"},{"$f":"IF(LEN('Translation-EN'!D1547)>0,'Translation-EN'!D1547,\"\")","v":""},{"$f":"$E$1545","v":"Cloisons sèches 5/8 po"}]
[{"$f":"IF(LEN('Translation-EN'!A1548)>0,'Translation-EN'!A1548,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1548)>0,'Translation-EN'!B1548,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1548)>0,'Translation-EN'!C1548,\"\")","v":"C94"},{"$f":"IF(LEN('Translation-EN'!D1548)>0,'Translation-EN'!D1548,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1363","v":"USG"}]
[{"$f":"IF(LEN('Translation-EN'!A1549)>0,'Translation-EN'!A1549,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1549)>0,'Translation-EN'!B1549,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1549)>0,'Translation-EN'!C1549,\"\")","v":"D94"},{"$f":"IF(LEN('Translation-EN'!D1549)>0,'Translation-EN'!D1549,\"\")","v":""},"Code-incendie EcoSmart"]
[{"$f":"IF(LEN('Translation-EN'!A1550)>0,'Translation-EN'!A1550,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1550)>0,'Translation-EN'!B1550,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1550)>0,'Translation-EN'!C1550,\"\")","v":"B95"},{"$f":"IF(LEN('Translation-EN'!D1550)>0,'Translation-EN'!D1550,\"\")","v":""},"Membrane d’étanchéité EPDM"]
[{"$f":"IF(LEN('Translation-EN'!A1551)>0,'Translation-EN'!A1551,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1551)>0,'Translation-EN'!B1551,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1551)>0,'Translation-EN'!C1551,\"\")","v":"C95"},{"$f":"IF(LEN('Translation-EN'!D1551)>0,'Translation-EN'!D1551,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"SPRI"]
[{"$f":"IF(LEN('Translation-EN'!A1552)>0,'Translation-EN'!A1552,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1552)>0,'Translation-EN'!B1552,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1552)>0,'Translation-EN'!C1552,\"\")","v":"B96"},{"$f":"IF(LEN('Translation-EN'!D1552)>0,'Translation-EN'!D1552,\"\")","v":""},"Panneau en mousse EPS"]
[{"$f":"IF(LEN('Translation-EN'!A1553)>0,'Translation-EN'!A1553,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1553)>0,'Translation-EN'!B1553,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1553)>0,'Translation-EN'!C1553,\"\")","v":"C96"},{"$f":"IF(LEN('Translation-EN'!D1553)>0,'Translation-EN'!D1553,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Alliance industrielle EPS"]
[{"$f":"IF(LEN('Translation-EN'!A1554)>0,'Translation-EN'!A1554,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1554)>0,'Translation-EN'!B1554,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1554)>0,'Translation-EN'!C1554,\"\")","v":"E96"},{"$f":"IF(LEN('Translation-EN'!D1554)>0,'Translation-EN'!D1554,\"\")","v":""},"R 4,6/pouce, Type IX, 25 psi (Type 3, 140 kPa)"]
[{"$f":"IF(LEN('Translation-EN'!A1555)>0,'Translation-EN'!A1555,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1555)>0,'Translation-EN'!B1555,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1555)>0,'Translation-EN'!C1555,\"\")","v":"B97"},{"$f":"IF(LEN('Translation-EN'!D1555)>0,'Translation-EN'!D1555,\"\")","v":""},{"$f":"$E$1552","v":"Panneau en mousse EPS"}]
[{"$f":"IF(LEN('Translation-EN'!A1556)>0,'Translation-EN'!A1556,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1556)>0,'Translation-EN'!B1556,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1556)>0,'Translation-EN'!C1556,\"\")","v":"C97"},{"$f":"IF(LEN('Translation-EN'!D1556)>0,'Translation-EN'!D1556,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1553","v":"Alliance industrielle EPS"}]
[{"$f":"IF(LEN('Translation-EN'!A1557)>0,'Translation-EN'!A1557,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1557)>0,'Translation-EN'!B1557,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1557)>0,'Translation-EN'!C1557,\"\")","v":"E97"},{"$f":"IF(LEN('Translation-EN'!D1557)>0,'Translation-EN'!D1557,\"\")","v":""},"R 4/pouce, Type II, 15 psi (Type 2, 110 kPa)"]
[{"$f":"IF(LEN('Translation-EN'!A1558)>0,'Translation-EN'!A1558,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1558)>0,'Translation-EN'!B1558,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1558)>0,'Translation-EN'!C1558,\"\")","v":"B98"},{"$f":"IF(LEN('Translation-EN'!D1558)>0,'Translation-EN'!D1558,\"\")","v":""},"Panneau de mousse EPS avec graphite"]
[{"$f":"IF(LEN('Translation-EN'!A1559)>0,'Translation-EN'!A1559,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1559)>0,'Translation-EN'!B1559,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1559)>0,'Translation-EN'!C1559,\"\")","v":"C98"},{"$f":"IF(LEN('Translation-EN'!D1559)>0,'Translation-EN'!D1559,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"BASF"]
[{"$f":"IF(LEN('Translation-EN'!A1560)>0,'Translation-EN'!A1560,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1560)>0,'Translation-EN'!B1560,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1560)>0,'Translation-EN'!C1560,\"\")","v":"D98"},{"$f":"IF(LEN('Translation-EN'!D1560)>0,'Translation-EN'!D1560,\"\")","v":""},"Neopor"]
[{"$f":"IF(LEN('Translation-EN'!A1561)>0,'Translation-EN'!A1561,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1561)>0,'Translation-EN'!B1561,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1561)>0,'Translation-EN'!C1561,\"\")","v":"E98"},{"$f":"IF(LEN('Translation-EN'!D1561)>0,'Translation-EN'!D1561,\"\")","v":""},"R 4,7/pouce, Type IXR 4.7/po, Type IX"]
[{"$f":"IF(LEN('Translation-EN'!A1562)>0,'Translation-EN'!A1562,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1562)>0,'Translation-EN'!B1562,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1562)>0,'Translation-EN'!C1562,\"\")","v":"B99"},{"$f":"IF(LEN('Translation-EN'!D1562)>0,'Translation-EN'!D1562,\"\")","v":""},{"$f":"$E$1558","v":"Panneau de mousse EPS avec graphite"}]
[{"$f":"IF(LEN('Translation-EN'!A1563)>0,'Translation-EN'!A1563,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1563)>0,'Translation-EN'!B1563,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1563)>0,'Translation-EN'!C1563,\"\")","v":"C99"},{"$f":"IF(LEN('Translation-EN'!D1563)>0,'Translation-EN'!D1563,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1559","v":"BASF"}]
[{"$f":"IF(LEN('Translation-EN'!A1564)>0,'Translation-EN'!A1564,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1564)>0,'Translation-EN'!B1564,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1564)>0,'Translation-EN'!C1564,\"\")","v":"D99"},{"$f":"IF(LEN('Translation-EN'!D1564)>0,'Translation-EN'!D1564,\"\")","v":""},{"$f":"$E$1560","v":"Neopor"}]
[{"$f":"IF(LEN('Translation-EN'!A1565)>0,'Translation-EN'!A1565,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1565)>0,'Translation-EN'!B1565,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1565)>0,'Translation-EN'!C1565,\"\")","v":"E99"},{"$f":"IF(LEN('Translation-EN'!D1565)>0,'Translation-EN'!D1565,\"\")","v":""},"R 4,7/pouce, Type II, 15 psi (Type 2, 110 kPa)"]
[{"$f":"IF(LEN('Translation-EN'!A1566)>0,'Translation-EN'!A1566,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1566)>0,'Translation-EN'!B1566,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1566)>0,'Translation-EN'!C1566,\"\")","v":"B100"},{"$f":"IF(LEN('Translation-EN'!D1566)>0,'Translation-EN'!D1566,\"\")","v":""},"Toiture en fibrociment"]
[{"$f":"IF(LEN('Translation-EN'!A1567)>0,'Translation-EN'!A1567,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1567)>0,'Translation-EN'!B1567,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1567)>0,'Translation-EN'!C1567,\"\")","v":"C100"},{"$f":"IF(LEN('Translation-EN'!D1567)>0,'Translation-EN'!D1567,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Cembrit"]
[{"$f":"IF(LEN('Translation-EN'!A1568)>0,'Translation-EN'!A1568,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1568)>0,'Translation-EN'!B1568,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1568)>0,'Translation-EN'!C1568,\"\")","v":"D100"},{"$f":"IF(LEN('Translation-EN'!D1568)>0,'Translation-EN'!D1568,\"\")","v":""},"Tôles ondulées"]
[{"$f":"IF(LEN('Translation-EN'!A1569)>0,'Translation-EN'!A1569,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1569)>0,'Translation-EN'!B1569,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1569)>0,'Translation-EN'!C1569,\"\")","v":"E100"},{"$f":"IF(LEN('Translation-EN'!D1569)>0,'Translation-EN'!D1569,\"\")","v":""},"6,5 mm"]
[{"$f":"IF(LEN('Translation-EN'!A1570)>0,'Translation-EN'!A1570,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1570)>0,'Translation-EN'!B1570,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1570)>0,'Translation-EN'!C1570,\"\")","v":"B101"},{"$f":"IF(LEN('Translation-EN'!D1570)>0,'Translation-EN'!D1570,\"\")","v":""},{"$f":"$E$1566","v":"Toiture en fibrociment"}]
[{"$f":"IF(LEN('Translation-EN'!A1571)>0,'Translation-EN'!A1571,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1571)>0,'Translation-EN'!B1571,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1571)>0,'Translation-EN'!C1571,\"\")","v":"C101"},{"$f":"IF(LEN('Translation-EN'!D1571)>0,'Translation-EN'!D1571,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1567","v":"Cembrit"}]
[{"$f":"IF(LEN('Translation-EN'!A1572)>0,'Translation-EN'!A1572,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1572)>0,'Translation-EN'!B1572,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1572)>0,'Translation-EN'!C1572,\"\")","v":"D101"},{"$f":"IF(LEN('Translation-EN'!D1572)>0,'Translation-EN'!D1572,\"\")","v":""},"Ardoises"]
[{"$f":"IF(LEN('Translation-EN'!A1573)>0,'Translation-EN'!A1573,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1573)>0,'Translation-EN'!B1573,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1573)>0,'Translation-EN'!C1573,\"\")","v":"E101"},{"$f":"IF(LEN('Translation-EN'!D1573)>0,'Translation-EN'!D1573,\"\")","v":""},"4 mm"]
[{"$f":"IF(LEN('Translation-EN'!A1574)>0,'Translation-EN'!A1574,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1574)>0,'Translation-EN'!B1574,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1574)>0,'Translation-EN'!C1574,\"\")","v":"B102"},{"$f":"IF(LEN('Translation-EN'!D1574)>0,'Translation-EN'!D1574,\"\")","v":""},{"$f":"$E$1566","v":"Toiture en fibrociment"}]
[{"$f":"IF(LEN('Translation-EN'!A1575)>0,'Translation-EN'!A1575,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1575)>0,'Translation-EN'!B1575,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1575)>0,'Translation-EN'!C1575,\"\")","v":"C102"},{"$f":"IF(LEN('Translation-EN'!D1575)>0,'Translation-EN'!D1575,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Mahaphant "]
[{"$f":"IF(LEN('Translation-EN'!A1576)>0,'Translation-EN'!A1576,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1576)>0,'Translation-EN'!B1576,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1576)>0,'Translation-EN'!C1576,\"\")","v":"D102"},{"$f":"IF(LEN('Translation-EN'!D1576)>0,'Translation-EN'!D1576,\"\")","v":""},"Fibrociment"]
[{"$f":"IF(LEN('Translation-EN'!A1577)>0,'Translation-EN'!A1577,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1577)>0,'Translation-EN'!B1577,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1577)>0,'Translation-EN'!C1577,\"\")","v":"E102"},{"$f":"IF(LEN('Translation-EN'!D1577)>0,'Translation-EN'!D1577,\"\")","v":""},"5 mm"]
[{"$f":"IF(LEN('Translation-EN'!A1578)>0,'Translation-EN'!A1578,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1578)>0,'Translation-EN'!B1578,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1578)>0,'Translation-EN'!C1578,\"\")","v":"B103"},{"$f":"IF(LEN('Translation-EN'!D1578)>0,'Translation-EN'!D1578,\"\")","v":""},"Bardage en fibrociment"]
[{"$f":"IF(LEN('Translation-EN'!A1579)>0,'Translation-EN'!A1579,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1579)>0,'Translation-EN'!B1579,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1579)>0,'Translation-EN'!C1579,\"\")","v":"C103"},{"$f":"IF(LEN('Translation-EN'!D1579)>0,'Translation-EN'!D1579,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1567","v":"Cembrit"}]
[{"$f":"IF(LEN('Translation-EN'!A1580)>0,'Translation-EN'!A1580,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1580)>0,'Translation-EN'!B1580,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1580)>0,'Translation-EN'!C1580,\"\")","v":"D103"},{"$f":"IF(LEN('Translation-EN'!D1580)>0,'Translation-EN'!D1580,\"\")","v":""},"Patina"]
[{"$f":"IF(LEN('Translation-EN'!A1581)>0,'Translation-EN'!A1581,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1581)>0,'Translation-EN'!B1581,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1581)>0,'Translation-EN'!C1581,\"\")","v":"B104"},{"$f":"IF(LEN('Translation-EN'!D1581)>0,'Translation-EN'!D1581,\"\")","v":""},{"$f":"$E$1578","v":"Bardage en fibrociment"}]
[{"$f":"IF(LEN('Translation-EN'!A1582)>0,'Translation-EN'!A1582,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1582)>0,'Translation-EN'!B1582,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1582)>0,'Translation-EN'!C1582,\"\")","v":"C104"},{"$f":"IF(LEN('Translation-EN'!D1582)>0,'Translation-EN'!D1582,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1567","v":"Cembrit"}]
[{"$f":"IF(LEN('Translation-EN'!A1583)>0,'Translation-EN'!A1583,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1583)>0,'Translation-EN'!B1583,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1583)>0,'Translation-EN'!C1583,\"\")","v":"D104"},{"$f":"IF(LEN('Translation-EN'!D1583)>0,'Translation-EN'!D1583,\"\")","v":""},"Solid & Express"]
[{"$f":"IF(LEN('Translation-EN'!A1584)>0,'Translation-EN'!A1584,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1584)>0,'Translation-EN'!B1584,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1584)>0,'Translation-EN'!C1584,\"\")","v":"B105"},{"$f":"IF(LEN('Translation-EN'!D1584)>0,'Translation-EN'!D1584,\"\")","v":""},"Natte en fibre de verre"]
[{"$f":"IF(LEN('Translation-EN'!A1585)>0,'Translation-EN'!A1585,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1585)>0,'Translation-EN'!B1585,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1585)>0,'Translation-EN'!C1585,\"\")","v":"C105"},{"$f":"IF(LEN('Translation-EN'!D1585)>0,'Translation-EN'!D1585,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1530","v":"CertainTeed"}]
[{"$f":"IF(LEN('Translation-EN'!A1586)>0,'Translation-EN'!A1586,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1586)>0,'Translation-EN'!B1586,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1586)>0,'Translation-EN'!C1586,\"\")","v":"D105"},{"$f":"IF(LEN('Translation-EN'!D1586)>0,'Translation-EN'!D1586,\"\")","v":""},"Isolation durable"]
[{"$f":"IF(LEN('Translation-EN'!A1587)>0,'Translation-EN'!A1587,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1587)>0,'Translation-EN'!B1587,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1587)>0,'Translation-EN'!C1587,\"\")","v":"E105"},{"$f":"IF(LEN('Translation-EN'!D1587)>0,'Translation-EN'!D1587,\"\")","v":""},{"$f":"$E$1351","v":"R 3,6/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1588)>0,'Translation-EN'!A1588,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1588)>0,'Translation-EN'!B1588,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1588)>0,'Translation-EN'!C1588,\"\")","v":"B106"},{"$f":"IF(LEN('Translation-EN'!D1588)>0,'Translation-EN'!D1588,\"\")","v":""},{"$f":"$E$1584","v":"Natte en fibre de verre"}]
[{"$f":"IF(LEN('Translation-EN'!A1589)>0,'Translation-EN'!A1589,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1589)>0,'Translation-EN'!B1589,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1589)>0,'Translation-EN'!C1589,\"\")","v":"C106"},{"$f":"IF(LEN('Translation-EN'!D1589)>0,'Translation-EN'!D1589,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Knauf"]
[{"$f":"IF(LEN('Translation-EN'!A1590)>0,'Translation-EN'!A1590,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1590)>0,'Translation-EN'!B1590,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1590)>0,'Translation-EN'!C1590,\"\")","v":"D106"},{"$f":"IF(LEN('Translation-EN'!D1590)>0,'Translation-EN'!D1590,\"\")","v":""},"EcoBatt"]
[{"$f":"IF(LEN('Translation-EN'!A1591)>0,'Translation-EN'!A1591,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1591)>0,'Translation-EN'!B1591,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1591)>0,'Translation-EN'!C1591,\"\")","v":"E106"},{"$f":"IF(LEN('Translation-EN'!D1591)>0,'Translation-EN'!D1591,\"\")","v":""},{"$f":"$E$1351","v":"R 3,6/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1592)>0,'Translation-EN'!A1592,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1592)>0,'Translation-EN'!B1592,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1592)>0,'Translation-EN'!C1592,\"\")","v":"B107"},{"$f":"IF(LEN('Translation-EN'!D1592)>0,'Translation-EN'!D1592,\"\")","v":""},{"$f":"$E$1584","v":"Natte en fibre de verre"}]
[{"$f":"IF(LEN('Translation-EN'!A1593)>0,'Translation-EN'!A1593,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1593)>0,'Translation-EN'!B1593,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1593)>0,'Translation-EN'!C1593,\"\")","v":"C107"},{"$f":"IF(LEN('Translation-EN'!D1593)>0,'Translation-EN'!D1593,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1288","v":"Owens Corning"}]
[{"$f":"IF(LEN('Translation-EN'!A1594)>0,'Translation-EN'!A1594,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1594)>0,'Translation-EN'!B1594,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1594)>0,'Translation-EN'!C1594,\"\")","v":"D107"},{"$f":"IF(LEN('Translation-EN'!D1594)>0,'Translation-EN'!D1594,\"\")","v":""},"EcoTouch Pink batt and roll"]
[{"$f":"IF(LEN('Translation-EN'!A1595)>0,'Translation-EN'!A1595,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1595)>0,'Translation-EN'!B1595,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1595)>0,'Translation-EN'!C1595,\"\")","v":"E107"},{"$f":"IF(LEN('Translation-EN'!D1595)>0,'Translation-EN'!D1595,\"\")","v":""},{"$f":"$E$1351","v":"R 3,6/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1596)>0,'Translation-EN'!A1596,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1596)>0,'Translation-EN'!B1596,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1596)>0,'Translation-EN'!C1596,\"\")","v":"B108"},{"$f":"IF(LEN('Translation-EN'!D1596)>0,'Translation-EN'!D1596,\"\")","v":""},"Fibre de verre en vrac"]
[{"$f":"IF(LEN('Translation-EN'!A1597)>0,'Translation-EN'!A1597,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1597)>0,'Translation-EN'!B1597,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1597)>0,'Translation-EN'!C1597,\"\")","v":"C108"},{"$f":"IF(LEN('Translation-EN'!D1597)>0,'Translation-EN'!D1597,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1530","v":"CertainTeed"}]
[{"$f":"IF(LEN('Translation-EN'!A1598)>0,'Translation-EN'!A1598,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1598)>0,'Translation-EN'!B1598,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1598)>0,'Translation-EN'!C1598,\"\")","v":"D108"},{"$f":"IF(LEN('Translation-EN'!D1598)>0,'Translation-EN'!D1598,\"\")","v":""},"InsulSafe, Optima, TruComfort"]
[{"$f":"IF(LEN('Translation-EN'!A1599)>0,'Translation-EN'!A1599,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1599)>0,'Translation-EN'!B1599,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1599)>0,'Translation-EN'!C1599,\"\")","v":"E108"},{"$f":"IF(LEN('Translation-EN'!D1599)>0,'Translation-EN'!D1599,\"\")","v":""},"R 2,6/po"]
[{"$f":"IF(LEN('Translation-EN'!A1600)>0,'Translation-EN'!A1600,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1600)>0,'Translation-EN'!B1600,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1600)>0,'Translation-EN'!C1600,\"\")","v":"B109"},{"$f":"IF(LEN('Translation-EN'!D1600)>0,'Translation-EN'!D1600,\"\")","v":""},{"$f":"$E$1596","v":"Fibre de verre en vrac"}]
[{"$f":"IF(LEN('Translation-EN'!A1601)>0,'Translation-EN'!A1601,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1601)>0,'Translation-EN'!B1601,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1601)>0,'Translation-EN'!C1601,\"\")","v":"C109"},{"$f":"IF(LEN('Translation-EN'!D1601)>0,'Translation-EN'!D1601,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1589","v":"Knauf"}]
[{"$f":"IF(LEN('Translation-EN'!A1602)>0,'Translation-EN'!A1602,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1602)>0,'Translation-EN'!B1602,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1602)>0,'Translation-EN'!C1602,\"\")","v":"D109"},{"$f":"IF(LEN('Translation-EN'!D1602)>0,'Translation-EN'!D1602,\"\")","v":""},"Jet Stream ULTRA"]
[{"$f":"IF(LEN('Translation-EN'!A1603)>0,'Translation-EN'!A1603,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1603)>0,'Translation-EN'!B1603,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1603)>0,'Translation-EN'!C1603,\"\")","v":"E109"},{"$f":"IF(LEN('Translation-EN'!D1603)>0,'Translation-EN'!D1603,\"\")","v":""},"R 2,2/po"]
[{"$f":"IF(LEN('Translation-EN'!A1604)>0,'Translation-EN'!A1604,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1604)>0,'Translation-EN'!B1604,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1604)>0,'Translation-EN'!C1604,\"\")","v":"B110"},{"$f":"IF(LEN('Translation-EN'!D1604)>0,'Translation-EN'!D1604,\"\")","v":""},{"$f":"$E$1596","v":"Fibre de verre en vrac"}]
[{"$f":"IF(LEN('Translation-EN'!A1605)>0,'Translation-EN'!A1605,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1605)>0,'Translation-EN'!B1605,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1605)>0,'Translation-EN'!C1605,\"\")","v":"C110"},{"$f":"IF(LEN('Translation-EN'!D1605)>0,'Translation-EN'!D1605,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1288","v":"Owens Corning"}]
[{"$f":"IF(LEN('Translation-EN'!A1606)>0,'Translation-EN'!A1606,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1606)>0,'Translation-EN'!B1606,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1606)>0,'Translation-EN'!C1606,\"\")","v":"D110"},{"$f":"IF(LEN('Translation-EN'!D1606)>0,'Translation-EN'!D1606,\"\")","v":""},"AttiCat, ProCat, ProPink"]
[{"$f":"IF(LEN('Translation-EN'!A1607)>0,'Translation-EN'!A1607,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1607)>0,'Translation-EN'!B1607,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1607)>0,'Translation-EN'!C1607,\"\")","v":"E110"},{"$f":"IF(LEN('Translation-EN'!D1607)>0,'Translation-EN'!D1607,\"\")","v":""},"R 2,8/po"]
[{"$f":"IF(LEN('Translation-EN'!A1608)>0,'Translation-EN'!A1608,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1608)>0,'Translation-EN'!B1608,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1608)>0,'Translation-EN'!C1608,\"\")","v":"B111"},{"$f":"IF(LEN('Translation-EN'!D1608)>0,'Translation-EN'!D1608,\"\")","v":""},"Agrégat de mousse de verre"]
[{"$f":"IF(LEN('Translation-EN'!A1609)>0,'Translation-EN'!A1609,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1609)>0,'Translation-EN'!B1609,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1609)>0,'Translation-EN'!C1609,\"\")","v":"C111"},{"$f":"IF(LEN('Translation-EN'!D1609)>0,'Translation-EN'!D1609,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Glasopor AS"]
[{"$f":"IF(LEN('Translation-EN'!A1610)>0,'Translation-EN'!A1610,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1610)>0,'Translation-EN'!B1610,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1610)>0,'Translation-EN'!C1610,\"\")","v":"E111"},{"$f":"IF(LEN('Translation-EN'!D1610)>0,'Translation-EN'!D1610,\"\")","v":""},"R 1,7/po, 10-60 mm"]
[{"$f":"IF(LEN('Translation-EN'!A1611)>0,'Translation-EN'!A1611,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1611)>0,'Translation-EN'!B1611,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1611)>0,'Translation-EN'!C1611,\"\")","v":"B112"},{"$f":"IF(LEN('Translation-EN'!D1611)>0,'Translation-EN'!D1611,\"\")","v":""},{"$f":"$E$1608","v":"Agrégat de mousse de verre"}]
[{"$f":"IF(LEN('Translation-EN'!A1612)>0,'Translation-EN'!A1612,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1612)>0,'Translation-EN'!B1612,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1612)>0,'Translation-EN'!C1612,\"\")","v":"C112"},{"$f":"IF(LEN('Translation-EN'!D1612)>0,'Translation-EN'!D1612,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Hasopor"]
[{"$f":"IF(LEN('Translation-EN'!A1613)>0,'Translation-EN'!A1613,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1613)>0,'Translation-EN'!B1613,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1613)>0,'Translation-EN'!C1613,\"\")","v":"E112"},{"$f":"IF(LEN('Translation-EN'!D1613)>0,'Translation-EN'!D1613,\"\")","v":""},{"$f":"$E$1610","v":"R 1,7/po, 10-60 mm"}]
[{"$f":"IF(LEN('Translation-EN'!A1614)>0,'Translation-EN'!A1614,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1614)>0,'Translation-EN'!B1614,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1614)>0,'Translation-EN'!C1614,\"\")","v":"B113"},{"$f":"IF(LEN('Translation-EN'!D1614)>0,'Translation-EN'!D1614,\"\")","v":""},{"$f":"$E$1608","v":"Agrégat de mousse de verre"}]
[{"$f":"IF(LEN('Translation-EN'!A1615)>0,'Translation-EN'!A1615,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1615)>0,'Translation-EN'!B1615,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1615)>0,'Translation-EN'!C1615,\"\")","v":"C113"},{"$f":"IF(LEN('Translation-EN'!D1615)>0,'Translation-EN'!D1615,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Misapor "]
[{"$f":"IF(LEN('Translation-EN'!A1616)>0,'Translation-EN'!A1616,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1616)>0,'Translation-EN'!B1616,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1616)>0,'Translation-EN'!C1616,\"\")","v":"D113"},{"$f":"IF(LEN('Translation-EN'!D1616)>0,'Translation-EN'!D1616,\"\")","v":""},"Glavel"]
[{"$f":"IF(LEN('Translation-EN'!A1617)>0,'Translation-EN'!A1617,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1617)>0,'Translation-EN'!B1617,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1617)>0,'Translation-EN'!C1617,\"\")","v":"E113"},{"$f":"IF(LEN('Translation-EN'!D1617)>0,'Translation-EN'!D1617,\"\")","v":""},{"$f":"$E$1610","v":"R 1,7/po, 10-60 mm"}]
[{"$f":"IF(LEN('Translation-EN'!A1618)>0,'Translation-EN'!A1618,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1618)>0,'Translation-EN'!B1618,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1618)>0,'Translation-EN'!C1618,\"\")","v":"B114"},{"$f":"IF(LEN('Translation-EN'!D1618)>0,'Translation-EN'!D1618,\"\")","v":""},"Panneau de mousse de verre"]
[{"$f":"IF(LEN('Translation-EN'!A1619)>0,'Translation-EN'!A1619,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1619)>0,'Translation-EN'!B1619,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1619)>0,'Translation-EN'!C1619,\"\")","v":"C114"},{"$f":"IF(LEN('Translation-EN'!D1619)>0,'Translation-EN'!D1619,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Pittsburgh Corning Europe"]
[{"$f":"IF(LEN('Translation-EN'!A1620)>0,'Translation-EN'!A1620,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1620)>0,'Translation-EN'!B1620,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1620)>0,'Translation-EN'!C1620,\"\")","v":"D114"},{"$f":"IF(LEN('Translation-EN'!D1620)>0,'Translation-EN'!D1620,\"\")","v":""},"Foamglas T4"]
[{"$f":"IF(LEN('Translation-EN'!A1621)>0,'Translation-EN'!A1621,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1621)>0,'Translation-EN'!B1621,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1621)>0,'Translation-EN'!C1621,\"\")","v":"E114"},{"$f":"IF(LEN('Translation-EN'!D1621)>0,'Translation-EN'!D1621,\"\")","v":""},"R 3,7/po"]
[{"$f":"IF(LEN('Translation-EN'!A1622)>0,'Translation-EN'!A1622,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1622)>0,'Translation-EN'!B1622,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1622)>0,'Translation-EN'!C1622,\"\")","v":"B115"},{"$f":"IF(LEN('Translation-EN'!D1622)>0,'Translation-EN'!D1622,\"\")","v":""},{"$f":"$E$1618","v":"Panneau de mousse de verre"}]
[{"$f":"IF(LEN('Translation-EN'!A1623)>0,'Translation-EN'!A1623,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1623)>0,'Translation-EN'!B1623,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1623)>0,'Translation-EN'!C1623,\"\")","v":"C115"},{"$f":"IF(LEN('Translation-EN'!D1623)>0,'Translation-EN'!D1623,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1619","v":"Pittsburgh Corning Europe"}]
[{"$f":"IF(LEN('Translation-EN'!A1624)>0,'Translation-EN'!A1624,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1624)>0,'Translation-EN'!B1624,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1624)>0,'Translation-EN'!C1624,\"\")","v":"D115"},{"$f":"IF(LEN('Translation-EN'!D1624)>0,'Translation-EN'!D1624,\"\")","v":""},"Foamglas W+F, Foamglas T3"]
[{"$f":"IF(LEN('Translation-EN'!A1625)>0,'Translation-EN'!A1625,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1625)>0,'Translation-EN'!B1625,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1625)>0,'Translation-EN'!C1625,\"\")","v":"E115"},{"$f":"IF(LEN('Translation-EN'!D1625)>0,'Translation-EN'!D1625,\"\")","v":""},{"$f":"$E$1508","v":"R4/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1626)>0,'Translation-EN'!A1626,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1626)>0,'Translation-EN'!B1626,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1626)>0,'Translation-EN'!C1626,\"\")","v":"B116"},{"$f":"IF(LEN('Translation-EN'!D1626)>0,'Translation-EN'!D1626,\"\")","v":""},"Bois lamellé-collé"]
[{"$f":"IF(LEN('Translation-EN'!A1627)>0,'Translation-EN'!A1627,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1627)>0,'Translation-EN'!B1627,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1627)>0,'Translation-EN'!C1627,\"\")","v":"C116"},{"$f":"IF(LEN('Translation-EN'!D1627)>0,'Translation-EN'!D1627,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Conseil américain du bois et Conseil canadien du bois"]
[{"$f":"IF(LEN('Translation-EN'!A1628)>0,'Translation-EN'!A1628,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1628)>0,'Translation-EN'!B1628,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1628)>0,'Translation-EN'!C1628,\"\")","v":"B117"},{"$f":"IF(LEN('Translation-EN'!D1628)>0,'Translation-EN'!D1628,\"\")","v":""},{"$f":"$E$1626","v":"Bois lamellé-collé"}]
[{"$f":"IF(LEN('Translation-EN'!A1629)>0,'Translation-EN'!A1629,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1629)>0,'Translation-EN'!B1629,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1629)>0,'Translation-EN'!C1629,\"\")","v":"C117"},{"$f":"IF(LEN('Translation-EN'!D1629)>0,'Translation-EN'!D1629,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1522","v":"Structurlam"}]
[{"$f":"IF(LEN('Translation-EN'!A1630)>0,'Translation-EN'!A1630,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1630)>0,'Translation-EN'!B1630,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1630)>0,'Translation-EN'!C1630,\"\")","v":"D117"},{"$f":"IF(LEN('Translation-EN'!D1630)>0,'Translation-EN'!D1630,\"\")","v":""},"Glulam Plus"]
[{"$f":"IF(LEN('Translation-EN'!A1631)>0,'Translation-EN'!A1631,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1631)>0,'Translation-EN'!B1631,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1631)>0,'Translation-EN'!C1631,\"\")","v":"E117"},{"$f":"IF(LEN('Translation-EN'!D1631)>0,'Translation-EN'!D1631,\"\")","v":""},{"$f":"$E$1520","v":"3-1/2 po (90 mm) d’épaisseur"}]
[{"$f":"IF(LEN('Translation-EN'!A1632)>0,'Translation-EN'!A1632,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1632)>0,'Translation-EN'!B1632,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1632)>0,'Translation-EN'!C1632,\"\")","v":"B118"},{"$f":"IF(LEN('Translation-EN'!D1632)>0,'Translation-EN'!D1632,\"\")","v":""},"Panneaux de gypse – matelas de verre"]
[{"$f":"IF(LEN('Translation-EN'!A1633)>0,'Translation-EN'!A1633,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1633)>0,'Translation-EN'!B1633,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1633)>0,'Translation-EN'!C1633,\"\")","v":"D118"},{"$f":"IF(LEN('Translation-EN'!D1633)>0,'Translation-EN'!D1633,\"\")","v":""},{"$f":"$E$1546","v":"Inclus : American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC"}]
[{"$f":"IF(LEN('Translation-EN'!A1634)>0,'Translation-EN'!A1634,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1634)>0,'Translation-EN'!B1634,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1634)>0,'Translation-EN'!C1634,\"\")","v":"B119"},{"$f":"IF(LEN('Translation-EN'!D1634)>0,'Translation-EN'!D1634,\"\")","v":""},{"$f":"$E$1632","v":"Panneaux de gypse – matelas de verre"}]
[{"$f":"IF(LEN('Translation-EN'!A1635)>0,'Translation-EN'!A1635,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1635)>0,'Translation-EN'!B1635,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1635)>0,'Translation-EN'!C1635,\"\")","v":"C119"},{"$f":"IF(LEN('Translation-EN'!D1635)>0,'Translation-EN'!D1635,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1363","v":"USG"}]
[{"$f":"IF(LEN('Translation-EN'!A1636)>0,'Translation-EN'!A1636,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1636)>0,'Translation-EN'!B1636,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1636)>0,'Translation-EN'!C1636,\"\")","v":"D119"},{"$f":"IF(LEN('Translation-EN'!D1636)>0,'Translation-EN'!D1636,\"\")","v":""},"Securock ExoAir 430"]
[{"$f":"IF(LEN('Translation-EN'!A1637)>0,'Translation-EN'!A1637,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1637)>0,'Translation-EN'!B1637,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1637)>0,'Translation-EN'!C1637,\"\")","v":"B120"},{"$f":"IF(LEN('Translation-EN'!D1637)>0,'Translation-EN'!D1637,\"\")","v":""},"Plancher en bois dur"]
[{"$f":"IF(LEN('Translation-EN'!A1638)>0,'Translation-EN'!A1638,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1638)>0,'Translation-EN'!B1638,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1638)>0,'Translation-EN'!C1638,\"\")","v":"C120"},{"$f":"IF(LEN('Translation-EN'!D1638)>0,'Translation-EN'!D1638,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Action Floor Systems"]
[{"$f":"IF(LEN('Translation-EN'!A1639)>0,'Translation-EN'!A1639,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1639)>0,'Translation-EN'!B1639,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1639)>0,'Translation-EN'!C1639,\"\")","v":"E120"},{"$f":"IF(LEN('Translation-EN'!D1639)>0,'Translation-EN'!D1639,\"\")","v":""},"25/32 po x 3-1/4 po certifié FSC"]
[{"$f":"IF(LEN('Translation-EN'!A1640)>0,'Translation-EN'!A1640,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1640)>0,'Translation-EN'!B1640,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1640)>0,'Translation-EN'!C1640,\"\")","v":"B121"},{"$f":"IF(LEN('Translation-EN'!D1640)>0,'Translation-EN'!D1640,\"\")","v":""},{"$f":"$E$1637","v":"Plancher en bois dur"}]
[{"$f":"IF(LEN('Translation-EN'!A1641)>0,'Translation-EN'!A1641,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1641)>0,'Translation-EN'!B1641,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1641)>0,'Translation-EN'!C1641,\"\")","v":"C121"},{"$f":"IF(LEN('Translation-EN'!D1641)>0,'Translation-EN'!D1641,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"mafi"]
[{"$f":"IF(LEN('Translation-EN'!A1642)>0,'Translation-EN'!A1642,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1642)>0,'Translation-EN'!B1642,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1642)>0,'Translation-EN'!C1642,\"\")","v":"D121"},{"$f":"IF(LEN('Translation-EN'!D1642)>0,'Translation-EN'!D1642,\"\")","v":""},"Planches de bois dur naturel"]
[{"$f":"IF(LEN('Translation-EN'!A1643)>0,'Translation-EN'!A1643,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1643)>0,'Translation-EN'!B1643,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1643)>0,'Translation-EN'!C1643,\"\")","v":"E121"},{"$f":"IF(LEN('Translation-EN'!D1643)>0,'Translation-EN'!D1643,\"\")","v":""},"3/4 po, massif laminé 3 plis, préfini à l’huile"]
[{"$f":"IF(LEN('Translation-EN'!A1644)>0,'Translation-EN'!A1644,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1644)>0,'Translation-EN'!B1644,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1644)>0,'Translation-EN'!C1644,\"\")","v":"B122"},{"$f":"IF(LEN('Translation-EN'!D1644)>0,'Translation-EN'!D1644,\"\")","v":""},{"$f":"$E$1637","v":"Plancher en bois dur"}]
[{"$f":"IF(LEN('Translation-EN'!A1645)>0,'Translation-EN'!A1645,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1645)>0,'Translation-EN'!B1645,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1645)>0,'Translation-EN'!C1645,\"\")","v":"C122"},{"$f":"IF(LEN('Translation-EN'!D1645)>0,'Translation-EN'!D1645,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Typique de l’Est canadien, massif, préfini"]
[{"$f":"IF(LEN('Translation-EN'!A1646)>0,'Translation-EN'!A1646,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1646)>0,'Translation-EN'!B1646,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1646)>0,'Translation-EN'!C1646,\"\")","v":"E122"},{"$f":"IF(LEN('Translation-EN'!D1646)>0,'Translation-EN'!D1646,\"\")","v":""},"3-12 po x 3/4 po préfinis"]
[{"$f":"IF(LEN('Translation-EN'!A1647)>0,'Translation-EN'!A1647,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1647)>0,'Translation-EN'!B1647,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1647)>0,'Translation-EN'!C1647,\"\")","v":"B123"},{"$f":"IF(LEN('Translation-EN'!D1647)>0,'Translation-EN'!D1647,\"\")","v":""},"Piliers héliques"]
[{"$f":"IF(LEN('Translation-EN'!A1648)>0,'Translation-EN'!A1648,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1648)>0,'Translation-EN'!B1648,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1648)>0,'Translation-EN'!C1648,\"\")","v":"C123"},{"$f":"IF(LEN('Translation-EN'!D1648)>0,'Translation-EN'!D1648,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Générique"]
[{"$f":"IF(LEN('Translation-EN'!A1649)>0,'Translation-EN'!A1649,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1649)>0,'Translation-EN'!B1649,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1649)>0,'Translation-EN'!C1649,\"\")","v":"E123"},{"$f":"IF(LEN('Translation-EN'!D1649)>0,'Translation-EN'!D1649,\"\")","v":""},"Tuyau nominal 3 po, 3,5 x 3/16 po (89 x 5,5 mm), hélice 10 po, acier galvanisé Sched 40 STD"]
[{"$f":"IF(LEN('Translation-EN'!A1650)>0,'Translation-EN'!A1650,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1650)>0,'Translation-EN'!B1650,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1650)>0,'Translation-EN'!C1650,\"\")","v":"B124"},{"$f":"IF(LEN('Translation-EN'!D1650)>0,'Translation-EN'!D1650,\"\")","v":""},"Natte de fibres de chanvre"]
[{"$f":"IF(LEN('Translation-EN'!A1651)>0,'Translation-EN'!A1651,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1651)>0,'Translation-EN'!B1651,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1651)>0,'Translation-EN'!C1651,\"\")","v":"C124"},{"$f":"IF(LEN('Translation-EN'!D1651)>0,'Translation-EN'!D1651,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"NaturFibre"]
[{"$f":"IF(LEN('Translation-EN'!A1652)>0,'Translation-EN'!A1652,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1652)>0,'Translation-EN'!B1652,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1652)>0,'Translation-EN'!C1652,\"\")","v":"D124"},{"$f":"IF(LEN('Translation-EN'!D1652)>0,'Translation-EN'!D1652,\"\")","v":""},"Laine de chanvre"]
[{"$f":"IF(LEN('Translation-EN'!A1653)>0,'Translation-EN'!A1653,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1653)>0,'Translation-EN'!B1653,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1653)>0,'Translation-EN'!C1653,\"\")","v":"E124"},{"$f":"IF(LEN('Translation-EN'!D1653)>0,'Translation-EN'!D1653,\"\")","v":""},{"$f":"$E$1354","v":"R 3,7/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1654)>0,'Translation-EN'!A1654,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1654)>0,'Translation-EN'!B1654,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1654)>0,'Translation-EN'!C1654,\"\")","v":"B125"},{"$f":"IF(LEN('Translation-EN'!D1654)>0,'Translation-EN'!D1654,\"\")","v":""},"Briques de chanvre"]
[{"$f":"IF(LEN('Translation-EN'!A1655)>0,'Translation-EN'!A1655,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1655)>0,'Translation-EN'!B1655,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1655)>0,'Translation-EN'!C1655,\"\")","v":"C125"},{"$f":"IF(LEN('Translation-EN'!D1655)>0,'Translation-EN'!D1655,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"IsoHemp"]
[{"$f":"IF(LEN('Translation-EN'!A1656)>0,'Translation-EN'!A1656,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1656)>0,'Translation-EN'!B1656,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1656)>0,'Translation-EN'!C1656,\"\")","v":"D125"},{"$f":"IF(LEN('Translation-EN'!D1656)>0,'Translation-EN'!D1656,\"\")","v":""},"Europe"]
[{"$f":"IF(LEN('Translation-EN'!A1657)>0,'Translation-EN'!A1657,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1657)>0,'Translation-EN'!B1657,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1657)>0,'Translation-EN'!C1657,\"\")","v":"E125"},{"$f":"IF(LEN('Translation-EN'!D1657)>0,'Translation-EN'!D1657,\"\")","v":""},"R 2,1/po"]
[{"$f":"IF(LEN('Translation-EN'!A1658)>0,'Translation-EN'!A1658,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1658)>0,'Translation-EN'!B1658,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1658)>0,'Translation-EN'!C1658,\"\")","v":"B126"},{"$f":"IF(LEN('Translation-EN'!D1658)>0,'Translation-EN'!D1658,\"\")","v":""},{"$f":"$E$1654","v":"Briques de chanvre"}]
[{"$f":"IF(LEN('Translation-EN'!A1659)>0,'Translation-EN'!A1659,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1659)>0,'Translation-EN'!B1659,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1659)>0,'Translation-EN'!C1659,\"\")","v":"C126"},{"$f":"IF(LEN('Translation-EN'!D1659)>0,'Translation-EN'!D1659,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1385","v":"Mélangé sur place"}]
[{"$f":"IF(LEN('Translation-EN'!A1660)>0,'Translation-EN'!A1660,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1660)>0,'Translation-EN'!B1660,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1660)>0,'Translation-EN'!C1660,\"\")","v":"D126"},{"$f":"IF(LEN('Translation-EN'!D1660)>0,'Translation-EN'!D1660,\"\")","v":""},{"$f":"$E$1656","v":"Europe"}]
[{"$f":"IF(LEN('Translation-EN'!A1661)>0,'Translation-EN'!A1661,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1661)>0,'Translation-EN'!B1661,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1661)>0,'Translation-EN'!C1661,\"\")","v":"E126"},{"$f":"IF(LEN('Translation-EN'!D1661)>0,'Translation-EN'!D1661,\"\")","v":""},"R 2,/po, Moyenne de 9 mélanges"]
[{"$f":"IF(LEN('Translation-EN'!A1662)>0,'Translation-EN'!A1662,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1662)>0,'Translation-EN'!B1662,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1662)>0,'Translation-EN'!C1662,\"\")","v":"B127"},{"$f":"IF(LEN('Translation-EN'!D1662)>0,'Translation-EN'!D1662,\"\")","v":""},{"$f":"$E$1654","v":"Briques de chanvre"}]
[{"$f":"IF(LEN('Translation-EN'!A1663)>0,'Translation-EN'!A1663,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1663)>0,'Translation-EN'!B1663,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1663)>0,'Translation-EN'!C1663,\"\")","v":"C127"},{"$f":"IF(LEN('Translation-EN'!D1663)>0,'Translation-EN'!D1663,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1385","v":"Mélangé sur place"}]
[{"$f":"IF(LEN('Translation-EN'!A1664)>0,'Translation-EN'!A1664,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1664)>0,'Translation-EN'!B1664,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1664)>0,'Translation-EN'!C1664,\"\")","v":"D127"},{"$f":"IF(LEN('Translation-EN'!D1664)>0,'Translation-EN'!D1664,\"\")","v":""},"États-Unis"]
[{"$f":"IF(LEN('Translation-EN'!A1665)>0,'Translation-EN'!A1665,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1665)>0,'Translation-EN'!B1665,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1665)>0,'Translation-EN'!C1665,\"\")","v":"E127"},{"$f":"IF(LEN('Translation-EN'!D1665)>0,'Translation-EN'!D1665,\"\")","v":""},"R 2,/po mélange moyen utilisant CHN et PHL"]
[{"$f":"IF(LEN('Translation-EN'!A1666)>0,'Translation-EN'!A1666,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1666)>0,'Translation-EN'!B1666,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1666)>0,'Translation-EN'!C1666,\"\")","v":"B128"},{"$f":"IF(LEN('Translation-EN'!D1666)>0,'Translation-EN'!D1666,\"\")","v":""},"Plancher lamellé"]
[{"$f":"IF(LEN('Translation-EN'!A1667)>0,'Translation-EN'!A1667,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1667)>0,'Translation-EN'!B1667,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1667)>0,'Translation-EN'!C1667,\"\")","v":"C128"},{"$f":"IF(LEN('Translation-EN'!D1667)>0,'Translation-EN'!D1667,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Novalis"]
[{"$f":"IF(LEN('Translation-EN'!A1668)>0,'Translation-EN'!A1668,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1668)>0,'Translation-EN'!B1668,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1668)>0,'Translation-EN'!C1668,\"\")","v":"D128"},{"$f":"IF(LEN('Translation-EN'!D1668)>0,'Translation-EN'!D1668,\"\")","v":""},"LVT"]
[{"$f":"IF(LEN('Translation-EN'!A1669)>0,'Translation-EN'!A1669,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1669)>0,'Translation-EN'!B1669,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1669)>0,'Translation-EN'!C1669,\"\")","v":"B130"},{"$f":"IF(LEN('Translation-EN'!D1669)>0,'Translation-EN'!D1669,\"\")","v":""},"Bois de longs copeaux lamellés"]
[{"$f":"IF(LEN('Translation-EN'!A1670)>0,'Translation-EN'!A1670,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1670)>0,'Translation-EN'!B1670,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1670)>0,'Translation-EN'!C1670,\"\")","v":"C130"},{"$f":"IF(LEN('Translation-EN'!D1670)>0,'Translation-EN'!D1670,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1627","v":"Conseil américain du bois et Conseil canadien du bois"}]
[{"$f":"IF(LEN('Translation-EN'!A1671)>0,'Translation-EN'!A1671,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1671)>0,'Translation-EN'!B1671,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1671)>0,'Translation-EN'!C1671,\"\")","v":"B131"},{"$f":"IF(LEN('Translation-EN'!D1671)>0,'Translation-EN'!D1671,\"\")","v":""},"Bois en placage stratifié"]
[{"$f":"IF(LEN('Translation-EN'!A1672)>0,'Translation-EN'!A1672,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1672)>0,'Translation-EN'!B1672,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1672)>0,'Translation-EN'!C1672,\"\")","v":"C131"},{"$f":"IF(LEN('Translation-EN'!D1672)>0,'Translation-EN'!D1672,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1627","v":"Conseil américain du bois et Conseil canadien du bois"}]
[{"$f":"IF(LEN('Translation-EN'!A1673)>0,'Translation-EN'!A1673,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1673)>0,'Translation-EN'!B1673,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1673)>0,'Translation-EN'!C1673,\"\")","v":"B132"},{"$f":"IF(LEN('Translation-EN'!D1673)>0,'Translation-EN'!D1673,\"\")","v":""},{"$f":"$E$1671","v":"Bois en placage stratifié"}]
[{"$f":"IF(LEN('Translation-EN'!A1674)>0,'Translation-EN'!A1674,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1674)>0,'Translation-EN'!B1674,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1674)>0,'Translation-EN'!C1674,\"\")","v":"C132"},{"$f":"IF(LEN('Translation-EN'!D1674)>0,'Translation-EN'!D1674,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"RedBuilt"]
[{"$f":"IF(LEN('Translation-EN'!A1675)>0,'Translation-EN'!A1675,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1675)>0,'Translation-EN'!B1675,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1675)>0,'Translation-EN'!C1675,\"\")","v":"D132"},{"$f":"IF(LEN('Translation-EN'!D1675)>0,'Translation-EN'!D1675,\"\")","v":""},"RedLam"]
[{"$f":"IF(LEN('Translation-EN'!A1676)>0,'Translation-EN'!A1676,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1676)>0,'Translation-EN'!B1676,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1676)>0,'Translation-EN'!C1676,\"\")","v":"B133"},{"$f":"IF(LEN('Translation-EN'!D1676)>0,'Translation-EN'!D1676,\"\")","v":""},"Plâtre à la chaux"]
[{"$f":"IF(LEN('Translation-EN'!A1677)>0,'Translation-EN'!A1677,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1677)>0,'Translation-EN'!B1677,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1677)>0,'Translation-EN'!C1677,\"\")","v":"C133"},{"$f":"IF(LEN('Translation-EN'!D1677)>0,'Translation-EN'!D1677,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Mapei"]
[{"$f":"IF(LEN('Translation-EN'!A1678)>0,'Translation-EN'!A1678,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1678)>0,'Translation-EN'!B1678,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1678)>0,'Translation-EN'!C1678,\"\")","v":"D133"},{"$f":"IF(LEN('Translation-EN'!D1678)>0,'Translation-EN'!D1678,\"\")","v":""},"MapeWall Muratura"]
[{"$f":"IF(LEN('Translation-EN'!A1679)>0,'Translation-EN'!A1679,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1679)>0,'Translation-EN'!B1679,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1679)>0,'Translation-EN'!C1679,\"\")","v":"E133"},{"$f":"IF(LEN('Translation-EN'!D1679)>0,'Translation-EN'!D1679,\"\")","v":""},"Chaux hydraulique naturelle (CHN) 3/4 po"]
[{"$f":"IF(LEN('Translation-EN'!A1680)>0,'Translation-EN'!A1680,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1680)>0,'Translation-EN'!B1680,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1680)>0,'Translation-EN'!C1680,\"\")","v":"B134"},{"$f":"IF(LEN('Translation-EN'!D1680)>0,'Translation-EN'!D1680,\"\")","v":""},"Plâtre à la chaux/au liège"]
[{"$f":"IF(LEN('Translation-EN'!A1681)>0,'Translation-EN'!A1681,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1681)>0,'Translation-EN'!B1681,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1681)>0,'Translation-EN'!C1681,\"\")","v":"C134"},{"$f":"IF(LEN('Translation-EN'!D1681)>0,'Translation-EN'!D1681,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Diasen"]
[{"$f":"IF(LEN('Translation-EN'!A1682)>0,'Translation-EN'!A1682,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1682)>0,'Translation-EN'!B1682,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1682)>0,'Translation-EN'!C1682,\"\")","v":"D134"},{"$f":"IF(LEN('Translation-EN'!D1682)>0,'Translation-EN'!D1682,\"\")","v":""},"Diathonite Evolution"]
[{"$f":"IF(LEN('Translation-EN'!A1683)>0,'Translation-EN'!A1683,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1683)>0,'Translation-EN'!B1683,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1683)>0,'Translation-EN'!C1683,\"\")","v":"E134"},{"$f":"IF(LEN('Translation-EN'!D1683)>0,'Translation-EN'!D1683,\"\")","v":""},"Revêtement extérieur en plâtre, 3/4 po."]
[{"$f":"IF(LEN('Translation-EN'!A1684)>0,'Translation-EN'!A1684,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1684)>0,'Translation-EN'!B1684,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1684)>0,'Translation-EN'!C1684,\"\")","v":"B135"},{"$f":"IF(LEN('Translation-EN'!D1684)>0,'Translation-EN'!D1684,\"\")","v":""},"Revêtement de plancher en linoléum"]
[{"$f":"IF(LEN('Translation-EN'!A1685)>0,'Translation-EN'!A1685,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1685)>0,'Translation-EN'!B1685,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1685)>0,'Translation-EN'!C1685,\"\")","v":"C135"},{"$f":"IF(LEN('Translation-EN'!D1685)>0,'Translation-EN'!D1685,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1301","v":"Armstrong"}]
[{"$f":"IF(LEN('Translation-EN'!A1686)>0,'Translation-EN'!A1686,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1686)>0,'Translation-EN'!B1686,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1686)>0,'Translation-EN'!C1686,\"\")","v":"D135"},{"$f":"IF(LEN('Translation-EN'!D1686)>0,'Translation-EN'!D1686,\"\")","v":""},"Style en feuille"]
[{"$f":"IF(LEN('Translation-EN'!A1687)>0,'Translation-EN'!A1687,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1687)>0,'Translation-EN'!B1687,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1687)>0,'Translation-EN'!C1687,\"\")","v":"E135"},{"$f":"IF(LEN('Translation-EN'!D1687)>0,'Translation-EN'!D1687,\"\")","v":""},"linoléum en feuille de 2,5 mm"]
[{"$f":"IF(LEN('Translation-EN'!A1688)>0,'Translation-EN'!A1688,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1688)>0,'Translation-EN'!B1688,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1688)>0,'Translation-EN'!C1688,\"\")","v":"B136"},{"$f":"IF(LEN('Translation-EN'!D1688)>0,'Translation-EN'!D1688,\"\")","v":""},{"$f":"$E$1684","v":"Revêtement de plancher en linoléum"}]
[{"$f":"IF(LEN('Translation-EN'!A1689)>0,'Translation-EN'!A1689,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1689)>0,'Translation-EN'!B1689,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1689)>0,'Translation-EN'!C1689,\"\")","v":"C136"},{"$f":"IF(LEN('Translation-EN'!D1689)>0,'Translation-EN'!D1689,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Forbo "]
[{"$f":"IF(LEN('Translation-EN'!A1690)>0,'Translation-EN'!A1690,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1690)>0,'Translation-EN'!B1690,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1690)>0,'Translation-EN'!C1690,\"\")","v":"D136"},{"$f":"IF(LEN('Translation-EN'!D1690)>0,'Translation-EN'!D1690,\"\")","v":""},"Marmoleum"]
[{"$f":"IF(LEN('Translation-EN'!A1691)>0,'Translation-EN'!A1691,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1691)>0,'Translation-EN'!B1691,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1691)>0,'Translation-EN'!C1691,\"\")","v":"E136"},{"$f":"IF(LEN('Translation-EN'!D1691)>0,'Translation-EN'!D1691,\"\")","v":""},{"$f":"$E$1687","v":"linoléum en feuille de 2,5 mm"}]
[{"$f":"IF(LEN('Translation-EN'!A1692)>0,'Translation-EN'!A1692,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1692)>0,'Translation-EN'!B1692,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1692)>0,'Translation-EN'!C1692,\"\")","v":"B137"},{"$f":"IF(LEN('Translation-EN'!D1692)>0,'Translation-EN'!D1692,\"\")","v":""},{"$f":"$E$1684","v":"Revêtement de plancher en linoléum"}]
[{"$f":"IF(LEN('Translation-EN'!A1693)>0,'Translation-EN'!A1693,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1693)>0,'Translation-EN'!B1693,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1693)>0,'Translation-EN'!C1693,\"\")","v":"C137"},{"$f":"IF(LEN('Translation-EN'!D1693)>0,'Translation-EN'!D1693,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1689","v":"Forbo "}]
[{"$f":"IF(LEN('Translation-EN'!A1694)>0,'Translation-EN'!A1694,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1694)>0,'Translation-EN'!B1694,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1694)>0,'Translation-EN'!C1694,\"\")","v":"D137"},{"$f":"IF(LEN('Translation-EN'!D1694)>0,'Translation-EN'!D1694,\"\")","v":""},"Marmoleum Striato"]
[{"$f":"IF(LEN('Translation-EN'!A1695)>0,'Translation-EN'!A1695,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1695)>0,'Translation-EN'!B1695,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1695)>0,'Translation-EN'!C1695,\"\")","v":"E137"},{"$f":"IF(LEN('Translation-EN'!D1695)>0,'Translation-EN'!D1695,\"\")","v":""},{"$f":"$E$1687","v":"linoléum en feuille de 2,5 mm"}]
[{"$f":"IF(LEN('Translation-EN'!A1696)>0,'Translation-EN'!A1696,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1696)>0,'Translation-EN'!B1696,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1696)>0,'Translation-EN'!C1696,\"\")","v":"B138"},{"$f":"IF(LEN('Translation-EN'!D1696)>0,'Translation-EN'!D1696,\"\")","v":""},{"$f":"$E$1684","v":"Revêtement de plancher en linoléum"}]
[{"$f":"IF(LEN('Translation-EN'!A1697)>0,'Translation-EN'!A1697,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1697)>0,'Translation-EN'!B1697,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1697)>0,'Translation-EN'!C1697,\"\")","v":"C138"},{"$f":"IF(LEN('Translation-EN'!D1697)>0,'Translation-EN'!D1697,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Gerflor "]
[{"$f":"IF(LEN('Translation-EN'!A1698)>0,'Translation-EN'!A1698,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1698)>0,'Translation-EN'!B1698,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1698)>0,'Translation-EN'!C1698,\"\")","v":"D138"},{"$f":"IF(LEN('Translation-EN'!D1698)>0,'Translation-EN'!D1698,\"\")","v":""},"DLW Linoleum Acousticplus"]
[{"$f":"IF(LEN('Translation-EN'!A1699)>0,'Translation-EN'!A1699,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1699)>0,'Translation-EN'!B1699,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1699)>0,'Translation-EN'!C1699,\"\")","v":"E138"},{"$f":"IF(LEN('Translation-EN'!D1699)>0,'Translation-EN'!D1699,\"\")","v":""},"linoléum en feuille de 4,0 mm"]
[{"$f":"IF(LEN('Translation-EN'!A1700)>0,'Translation-EN'!A1700,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1700)>0,'Translation-EN'!B1700,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1700)>0,'Translation-EN'!C1700,\"\")","v":"B140"},{"$f":"IF(LEN('Translation-EN'!D1700)>0,'Translation-EN'!D1700,\"\")","v":""},"Revêtement de plancher en linoléum liquide"]
[{"$f":"IF(LEN('Translation-EN'!A1701)>0,'Translation-EN'!A1701,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1701)>0,'Translation-EN'!B1701,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1701)>0,'Translation-EN'!C1701,\"\")","v":"C140"},{"$f":"IF(LEN('Translation-EN'!D1701)>0,'Translation-EN'!D1701,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Duracryl Corques"]
[{"$f":"IF(LEN('Translation-EN'!A1702)>0,'Translation-EN'!A1702,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1702)>0,'Translation-EN'!B1702,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1702)>0,'Translation-EN'!C1702,\"\")","v":"D140"},{"$f":"IF(LEN('Translation-EN'!D1702)>0,'Translation-EN'!D1702,\"\")","v":""},"Liquid Lino"]
[{"$f":"IF(LEN('Translation-EN'!A1703)>0,'Translation-EN'!A1703,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1703)>0,'Translation-EN'!B1703,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1703)>0,'Translation-EN'!C1703,\"\")","v":"E140"},{"$f":"IF(LEN('Translation-EN'!D1703)>0,'Translation-EN'!D1703,\"\")","v":""},"2,0 mm appliqué liquide"]
[{"$f":"IF(LEN('Translation-EN'!A1704)>0,'Translation-EN'!A1704,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1704)>0,'Translation-EN'!B1704,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1704)>0,'Translation-EN'!C1704,\"\")","v":"B141"},{"$f":"IF(LEN('Translation-EN'!D1704)>0,'Translation-EN'!D1704,\"\")","v":""},"Ciment de maçonnerie"]
[{"$f":"IF(LEN('Translation-EN'!A1705)>0,'Translation-EN'!A1705,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1705)>0,'Translation-EN'!B1705,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1705)>0,'Translation-EN'!C1705,\"\")","v":"C141"},{"$f":"IF(LEN('Translation-EN'!D1705)>0,'Translation-EN'!D1705,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Portland Cement Association"]
[{"$f":"IF(LEN('Translation-EN'!A1706)>0,'Translation-EN'!A1706,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1706)>0,'Translation-EN'!B1706,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1706)>0,'Translation-EN'!C1706,\"\")","v":"D141"},{"$f":"IF(LEN('Translation-EN'!D1706)>0,'Translation-EN'!D1706,\"\")","v":""},"Inclus : Argos, Buzzi, CalPortland, Capitol Aggregates, Cemex, Essroc, LafargeHolcim, Monarch, St. Mary's, Titan"]
[{"$f":"IF(LEN('Translation-EN'!A1707)>0,'Translation-EN'!A1707,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1707)>0,'Translation-EN'!B1707,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1707)>0,'Translation-EN'!C1707,\"\")","v":"B142"},{"$f":"IF(LEN('Translation-EN'!D1707)>0,'Translation-EN'!D1707,\"\")","v":""},"Mélange de mortier de maçonnerie"]
[{"$f":"IF(LEN('Translation-EN'!A1708)>0,'Translation-EN'!A1708,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1708)>0,'Translation-EN'!B1708,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1708)>0,'Translation-EN'!C1708,\"\")","v":"C142"},{"$f":"IF(LEN('Translation-EN'!D1708)>0,'Translation-EN'!D1708,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"1 part de ciment de maçonnerie"]
[{"$f":"IF(LEN('Translation-EN'!A1709)>0,'Translation-EN'!A1709,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1709)>0,'Translation-EN'!B1709,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1709)>0,'Translation-EN'!C1709,\"\")","v":"D142"},{"$f":"IF(LEN('Translation-EN'!D1709)>0,'Translation-EN'!D1709,\"\")","v":""},"3 parts de sable ordinaire"]
[{"$f":"IF(LEN('Translation-EN'!A1710)>0,'Translation-EN'!A1710,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1710)>0,'Translation-EN'!B1710,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1710)>0,'Translation-EN'!C1710,\"\")","v":"B143"},{"$f":"IF(LEN('Translation-EN'!D1710)>0,'Translation-EN'!D1710,\"\")","v":""},"Panneaux métalliques – Aluminium"]
[{"$f":"IF(LEN('Translation-EN'!A1711)>0,'Translation-EN'!A1711,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1711)>0,'Translation-EN'!B1711,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1711)>0,'Translation-EN'!C1711,\"\")","v":"C143"},{"$f":"IF(LEN('Translation-EN'!D1711)>0,'Translation-EN'!D1711,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Association des métaux de construction"]
[{"$f":"IF(LEN('Translation-EN'!A1712)>0,'Translation-EN'!A1712,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1712)>0,'Translation-EN'!B1712,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1712)>0,'Translation-EN'!C1712,\"\")","v":"D143"},{"$f":"IF(LEN('Translation-EN'!D1712)>0,'Translation-EN'!D1712,\"\")","v":""},"Inclus : ATAS, DMI, Englert, Fabral, McElroy, Pac-Clad"]
[{"$f":"IF(LEN('Translation-EN'!A1713)>0,'Translation-EN'!A1713,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1713)>0,'Translation-EN'!B1713,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1713)>0,'Translation-EN'!C1713,\"\")","v":"E143"},{"$f":"IF(LEN('Translation-EN'!D1713)>0,'Translation-EN'!D1713,\"\")","v":""},"22 jauge"]
[{"$f":"IF(LEN('Translation-EN'!A1714)>0,'Translation-EN'!A1714,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1714)>0,'Translation-EN'!B1714,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1714)>0,'Translation-EN'!C1714,\"\")","v":"B144"},{"$f":"IF(LEN('Translation-EN'!D1714)>0,'Translation-EN'!D1714,\"\")","v":""},{"$f":"$E$1710","v":"Panneaux métalliques – Aluminium"}]
[{"$f":"IF(LEN('Translation-EN'!A1715)>0,'Translation-EN'!A1715,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1715)>0,'Translation-EN'!B1715,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1715)>0,'Translation-EN'!C1715,\"\")","v":"C144"},{"$f":"IF(LEN('Translation-EN'!D1715)>0,'Translation-EN'!D1715,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Petersen Aluminum Corp"]
[{"$f":"IF(LEN('Translation-EN'!A1716)>0,'Translation-EN'!A1716,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1716)>0,'Translation-EN'!B1716,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1716)>0,'Translation-EN'!C1716,\"\")","v":"D144"},{"$f":"IF(LEN('Translation-EN'!D1716)>0,'Translation-EN'!D1716,\"\")","v":""},"Pac-Clad"]
[{"$f":"IF(LEN('Translation-EN'!A1717)>0,'Translation-EN'!A1717,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1717)>0,'Translation-EN'!B1717,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1717)>0,'Translation-EN'!C1717,\"\")","v":"E144"},{"$f":"IF(LEN('Translation-EN'!D1717)>0,'Translation-EN'!D1717,\"\")","v":""},"20EQ jauge"]
[{"$f":"IF(LEN('Translation-EN'!A1718)>0,'Translation-EN'!A1718,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1718)>0,'Translation-EN'!B1718,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1718)>0,'Translation-EN'!C1718,\"\")","v":"B145"},{"$f":"IF(LEN('Translation-EN'!D1718)>0,'Translation-EN'!D1718,\"\")","v":""},"Panneaux métalliques – acier"]
[{"$f":"IF(LEN('Translation-EN'!A1719)>0,'Translation-EN'!A1719,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1719)>0,'Translation-EN'!B1719,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1719)>0,'Translation-EN'!C1719,\"\")","v":"C145"},{"$f":"IF(LEN('Translation-EN'!D1719)>0,'Translation-EN'!D1719,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"AEP Span"]
[{"$f":"IF(LEN('Translation-EN'!A1720)>0,'Translation-EN'!A1720,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1720)>0,'Translation-EN'!B1720,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1720)>0,'Translation-EN'!C1720,\"\")","v":"D145"},{"$f":"IF(LEN('Translation-EN'!D1720)>0,'Translation-EN'!D1720,\"\")","v":""},"Tous les produits"]
[{"$f":"IF(LEN('Translation-EN'!A1721)>0,'Translation-EN'!A1721,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1721)>0,'Translation-EN'!B1721,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1721)>0,'Translation-EN'!C1721,\"\")","v":"E145"},{"$f":"IF(LEN('Translation-EN'!D1721)>0,'Translation-EN'!D1721,\"\")","v":""},"24 jauge"]
[{"$f":"IF(LEN('Translation-EN'!A1722)>0,'Translation-EN'!A1722,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1722)>0,'Translation-EN'!B1722,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1722)>0,'Translation-EN'!C1722,\"\")","v":"B146"},{"$f":"IF(LEN('Translation-EN'!D1722)>0,'Translation-EN'!D1722,\"\")","v":""},{"$f":"$E$1718","v":"Panneaux métalliques – acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1723)>0,'Translation-EN'!A1723,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1723)>0,'Translation-EN'!B1723,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1723)>0,'Translation-EN'!C1723,\"\")","v":"C146"},{"$f":"IF(LEN('Translation-EN'!D1723)>0,'Translation-EN'!D1723,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"ArcelorMittal"]
[{"$f":"IF(LEN('Translation-EN'!A1724)>0,'Translation-EN'!A1724,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1724)>0,'Translation-EN'!B1724,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1724)>0,'Translation-EN'!C1724,\"\")","v":"D146"},{"$f":"IF(LEN('Translation-EN'!D1724)>0,'Translation-EN'!D1724,\"\")","v":""},{"$f":"$E$1720","v":"Tous les produits"}]
[{"$f":"IF(LEN('Translation-EN'!A1725)>0,'Translation-EN'!A1725,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1725)>0,'Translation-EN'!B1725,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1725)>0,'Translation-EN'!C1725,\"\")","v":"E146"},{"$f":"IF(LEN('Translation-EN'!D1725)>0,'Translation-EN'!D1725,\"\")","v":""},{"$f":"$E$1721","v":"24 jauge"}]
[{"$f":"IF(LEN('Translation-EN'!A1726)>0,'Translation-EN'!A1726,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1726)>0,'Translation-EN'!B1726,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1726)>0,'Translation-EN'!C1726,\"\")","v":"B147"},{"$f":"IF(LEN('Translation-EN'!D1726)>0,'Translation-EN'!D1726,\"\")","v":""},{"$f":"$E$1718","v":"Panneaux métalliques – acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1727)>0,'Translation-EN'!A1727,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1727)>0,'Translation-EN'!B1727,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1727)>0,'Translation-EN'!C1727,\"\")","v":"C147"},{"$f":"IF(LEN('Translation-EN'!D1727)>0,'Translation-EN'!D1727,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Institut canadien de la tôle d’acier pour le bâtiment"]
[{"$f":"IF(LEN('Translation-EN'!A1728)>0,'Translation-EN'!A1728,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1728)>0,'Translation-EN'!B1728,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1728)>0,'Translation-EN'!C1728,\"\")","v":"D147"},{"$f":"IF(LEN('Translation-EN'!D1728)>0,'Translation-EN'!D1728,\"\")","v":""},"Inclus : Agway, Bailey, Behlen, Canam,DASS, DCM, Duchesne, EB, Exsteel, Ideal Roofing, Imperial, LKME, Manugypse, Metal Up, Scotia, Steel Tile Co, Steelway, Trebor, Vicwest, Vulcraft, Westform, Westman"]
[{"$f":"IF(LEN('Translation-EN'!A1729)>0,'Translation-EN'!A1729,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1729)>0,'Translation-EN'!B1729,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1729)>0,'Translation-EN'!C1729,\"\")","v":"E147"},{"$f":"IF(LEN('Translation-EN'!D1729)>0,'Translation-EN'!D1729,\"\")","v":""},{"$f":"$E$1721","v":"24 jauge"}]
[{"$f":"IF(LEN('Translation-EN'!A1730)>0,'Translation-EN'!A1730,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1730)>0,'Translation-EN'!B1730,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1730)>0,'Translation-EN'!C1730,\"\")","v":"B148"},{"$f":"IF(LEN('Translation-EN'!D1730)>0,'Translation-EN'!D1730,\"\")","v":""},{"$f":"$E$1718","v":"Panneaux métalliques – acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1731)>0,'Translation-EN'!A1731,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1731)>0,'Translation-EN'!B1731,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1731)>0,'Translation-EN'!C1731,\"\")","v":"C148"},{"$f":"IF(LEN('Translation-EN'!D1731)>0,'Translation-EN'!D1731,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Association des fabricants de matériaux de bâtiments métalliques"]
[{"$f":"IF(LEN('Translation-EN'!A1732)>0,'Translation-EN'!A1732,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1732)>0,'Translation-EN'!B1732,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1732)>0,'Translation-EN'!C1732,\"\")","v":"D148"},{"$f":"IF(LEN('Translation-EN'!D1732)>0,'Translation-EN'!D1732,\"\")","v":""},"Voir tous les membres"]
[{"$f":"IF(LEN('Translation-EN'!A1733)>0,'Translation-EN'!A1733,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1733)>0,'Translation-EN'!B1733,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1733)>0,'Translation-EN'!C1733,\"\")","v":"E148"},{"$f":"IF(LEN('Translation-EN'!D1733)>0,'Translation-EN'!D1733,\"\")","v":""},{"$f":"$E$1721","v":"24 jauge"}]
[{"$f":"IF(LEN('Translation-EN'!A1734)>0,'Translation-EN'!A1734,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1734)>0,'Translation-EN'!B1734,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1734)>0,'Translation-EN'!C1734,\"\")","v":"B149"},{"$f":"IF(LEN('Translation-EN'!D1734)>0,'Translation-EN'!D1734,\"\")","v":""},{"$f":"$E$1718","v":"Panneaux métalliques – acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1735)>0,'Translation-EN'!A1735,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1735)>0,'Translation-EN'!B1735,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1735)>0,'Translation-EN'!C1735,\"\")","v":"C149"},{"$f":"IF(LEN('Translation-EN'!D1735)>0,'Translation-EN'!D1735,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1711","v":"Association des métaux de construction"}]
[{"$f":"IF(LEN('Translation-EN'!A1736)>0,'Translation-EN'!A1736,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1736)>0,'Translation-EN'!B1736,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1736)>0,'Translation-EN'!C1736,\"\")","v":"D149"},{"$f":"IF(LEN('Translation-EN'!D1736)>0,'Translation-EN'!D1736,\"\")","v":""},{"$f":"$E$1712","v":"Inclus : ATAS, DMI, Englert, Fabral, McElroy, Pac-Clad"}]
[{"$f":"IF(LEN('Translation-EN'!A1737)>0,'Translation-EN'!A1737,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1737)>0,'Translation-EN'!B1737,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1737)>0,'Translation-EN'!C1737,\"\")","v":"E149"},{"$f":"IF(LEN('Translation-EN'!D1737)>0,'Translation-EN'!D1737,\"\")","v":""},{"$f":"$E$1721","v":"24 jauge"}]
[{"$f":"IF(LEN('Translation-EN'!A1738)>0,'Translation-EN'!A1738,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1738)>0,'Translation-EN'!B1738,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1738)>0,'Translation-EN'!C1738,\"\")","v":"B150"},{"$f":"IF(LEN('Translation-EN'!D1738)>0,'Translation-EN'!D1738,\"\")","v":""},{"$f":"$E$1718","v":"Panneaux métalliques – acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1739)>0,'Translation-EN'!A1739,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1739)>0,'Translation-EN'!B1739,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1739)>0,'Translation-EN'!C1739,\"\")","v":"C150"},{"$f":"IF(LEN('Translation-EN'!D1739)>0,'Translation-EN'!D1739,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1715","v":"Petersen Aluminum Corp"}]
[{"$f":"IF(LEN('Translation-EN'!A1740)>0,'Translation-EN'!A1740,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1740)>0,'Translation-EN'!B1740,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1740)>0,'Translation-EN'!C1740,\"\")","v":"D150"},{"$f":"IF(LEN('Translation-EN'!D1740)>0,'Translation-EN'!D1740,\"\")","v":""},"PAC-CLAD"]
[{"$f":"IF(LEN('Translation-EN'!A1741)>0,'Translation-EN'!A1741,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1741)>0,'Translation-EN'!B1741,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1741)>0,'Translation-EN'!C1741,\"\")","v":"E150"},{"$f":"IF(LEN('Translation-EN'!D1741)>0,'Translation-EN'!D1741,\"\")","v":""},{"$f":"$E$1721","v":"24 jauge"}]
[{"$f":"IF(LEN('Translation-EN'!A1742)>0,'Translation-EN'!A1742,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1742)>0,'Translation-EN'!B1742,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1742)>0,'Translation-EN'!C1742,\"\")","v":"B151"},{"$f":"IF(LEN('Translation-EN'!D1742)>0,'Translation-EN'!D1742,\"\")","v":""},"Panneau de MG 1/2 po"]
[{"$f":"IF(LEN('Translation-EN'!A1743)>0,'Translation-EN'!A1743,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1743)>0,'Translation-EN'!B1743,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1743)>0,'Translation-EN'!C1743,\"\")","v":"C151"},{"$f":"IF(LEN('Translation-EN'!D1743)>0,'Translation-EN'!D1743,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"North American MgO"]
[{"$f":"IF(LEN('Translation-EN'!A1744)>0,'Translation-EN'!A1744,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1744)>0,'Translation-EN'!B1744,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1744)>0,'Translation-EN'!C1744,\"\")","v":"D151"},{"$f":"IF(LEN('Translation-EN'!D1744)>0,'Translation-EN'!D1744,\"\")","v":""},"MagTech Ultra"]
[{"$f":"IF(LEN('Translation-EN'!A1745)>0,'Translation-EN'!A1745,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1745)>0,'Translation-EN'!B1745,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1745)>0,'Translation-EN'!C1745,\"\")","v":"B152"},{"$f":"IF(LEN('Translation-EN'!D1745)>0,'Translation-EN'!D1745,\"\")","v":""},"Natte de laine minérale"]
[{"$f":"IF(LEN('Translation-EN'!A1746)>0,'Translation-EN'!A1746,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1746)>0,'Translation-EN'!B1746,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1746)>0,'Translation-EN'!C1746,\"\")","v":"C152"},{"$f":"IF(LEN('Translation-EN'!D1746)>0,'Translation-EN'!D1746,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1288","v":"Owens Corning"}]
[{"$f":"IF(LEN('Translation-EN'!A1747)>0,'Translation-EN'!A1747,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1747)>0,'Translation-EN'!B1747,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1747)>0,'Translation-EN'!C1747,\"\")","v":"D152"},{"$f":"IF(LEN('Translation-EN'!D1747)>0,'Translation-EN'!D1747,\"\")","v":""},"Thermafiber UltraBatt"]
[{"$f":"IF(LEN('Translation-EN'!A1748)>0,'Translation-EN'!A1748,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1748)>0,'Translation-EN'!B1748,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1748)>0,'Translation-EN'!C1748,\"\")","v":"E152"},{"$f":"IF(LEN('Translation-EN'!D1748)>0,'Translation-EN'!D1748,\"\")","v":""},"R 4,3/po"]
[{"$f":"IF(LEN('Translation-EN'!A1749)>0,'Translation-EN'!A1749,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1749)>0,'Translation-EN'!B1749,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1749)>0,'Translation-EN'!C1749,\"\")","v":"B153"},{"$f":"IF(LEN('Translation-EN'!D1749)>0,'Translation-EN'!D1749,\"\")","v":""},{"$f":"$E$1745","v":"Natte de laine minérale"}]
[{"$f":"IF(LEN('Translation-EN'!A1750)>0,'Translation-EN'!A1750,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1750)>0,'Translation-EN'!B1750,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1750)>0,'Translation-EN'!C1750,\"\")","v":"C153"},{"$f":"IF(LEN('Translation-EN'!D1750)>0,'Translation-EN'!D1750,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Rockwool"]
[{"$f":"IF(LEN('Translation-EN'!A1751)>0,'Translation-EN'!A1751,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1751)>0,'Translation-EN'!B1751,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1751)>0,'Translation-EN'!C1751,\"\")","v":"D153"},{"$f":"IF(LEN('Translation-EN'!D1751)>0,'Translation-EN'!D1751,\"\")","v":""},"Safe'n'Sound, ComfortBatt"]
[{"$f":"IF(LEN('Translation-EN'!A1752)>0,'Translation-EN'!A1752,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1752)>0,'Translation-EN'!B1752,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1752)>0,'Translation-EN'!C1752,\"\")","v":"E153"},{"$f":"IF(LEN('Translation-EN'!D1752)>0,'Translation-EN'!D1752,\"\")","v":""},"R 3,8/po"]
[{"$f":"IF(LEN('Translation-EN'!A1753)>0,'Translation-EN'!A1753,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1753)>0,'Translation-EN'!B1753,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1753)>0,'Translation-EN'!C1753,\"\")","v":"B154"},{"$f":"IF(LEN('Translation-EN'!D1753)>0,'Translation-EN'!D1753,\"\")","v":""},"Panneau de laine minérale – forte densité"]
[{"$f":"IF(LEN('Translation-EN'!A1754)>0,'Translation-EN'!A1754,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1754)>0,'Translation-EN'!B1754,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1754)>0,'Translation-EN'!C1754,\"\")","v":"C154"},{"$f":"IF(LEN('Translation-EN'!D1754)>0,'Translation-EN'!D1754,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"NAIMA "]
[{"$f":"IF(LEN('Translation-EN'!A1755)>0,'Translation-EN'!A1755,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1755)>0,'Translation-EN'!B1755,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1755)>0,'Translation-EN'!C1755,\"\")","v":"D154"},{"$f":"IF(LEN('Translation-EN'!D1755)>0,'Translation-EN'!D1755,\"\")","v":""},"Inclus : Rolan, Armstrong, Rockwool, Thermafiber, American Rock Wool, IIG, Delta, USG"]
[{"$f":"IF(LEN('Translation-EN'!A1756)>0,'Translation-EN'!A1756,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1756)>0,'Translation-EN'!B1756,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1756)>0,'Translation-EN'!C1756,\"\")","v":"E154"},{"$f":"IF(LEN('Translation-EN'!D1756)>0,'Translation-EN'!D1756,\"\")","v":""},"R 4,2/po"]
[{"$f":"IF(LEN('Translation-EN'!A1757)>0,'Translation-EN'!A1757,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1757)>0,'Translation-EN'!B1757,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1757)>0,'Translation-EN'!C1757,\"\")","v":"B155"},{"$f":"IF(LEN('Translation-EN'!D1757)>0,'Translation-EN'!D1757,\"\")","v":""},"Panneau de laine minérale"]
[{"$f":"IF(LEN('Translation-EN'!A1758)>0,'Translation-EN'!A1758,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1758)>0,'Translation-EN'!B1758,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1758)>0,'Translation-EN'!C1758,\"\")","v":"C155"},{"$f":"IF(LEN('Translation-EN'!D1758)>0,'Translation-EN'!D1758,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1750","v":"Rockwool"}]
[{"$f":"IF(LEN('Translation-EN'!A1759)>0,'Translation-EN'!A1759,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1759)>0,'Translation-EN'!B1759,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1759)>0,'Translation-EN'!C1759,\"\")","v":"D155"},{"$f":"IF(LEN('Translation-EN'!D1759)>0,'Translation-EN'!D1759,\"\")","v":""},"Rockboard 60"]
[{"$f":"IF(LEN('Translation-EN'!A1760)>0,'Translation-EN'!A1760,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1760)>0,'Translation-EN'!B1760,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1760)>0,'Translation-EN'!C1760,\"\")","v":"E155"},{"$f":"IF(LEN('Translation-EN'!D1760)>0,'Translation-EN'!D1760,\"\")","v":""},{"$f":"$E$1748","v":"R 4,3/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1761)>0,'Translation-EN'!A1761,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1761)>0,'Translation-EN'!B1761,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1761)>0,'Translation-EN'!C1761,\"\")","v":"B156"},{"$f":"IF(LEN('Translation-EN'!D1761)>0,'Translation-EN'!D1761,\"\")","v":""},"Panneau de laine minérale – faible densité"]
[{"$f":"IF(LEN('Translation-EN'!A1762)>0,'Translation-EN'!A1762,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1762)>0,'Translation-EN'!B1762,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1762)>0,'Translation-EN'!C1762,\"\")","v":"C156"},{"$f":"IF(LEN('Translation-EN'!D1762)>0,'Translation-EN'!D1762,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1754","v":"NAIMA "}]
[{"$f":"IF(LEN('Translation-EN'!A1763)>0,'Translation-EN'!A1763,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1763)>0,'Translation-EN'!B1763,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1763)>0,'Translation-EN'!C1763,\"\")","v":"D156"},{"$f":"IF(LEN('Translation-EN'!D1763)>0,'Translation-EN'!D1763,\"\")","v":""},{"$f":"$E$1755","v":"Inclus : Rolan, Armstrong, Rockwool, Thermafiber, American Rock Wool, IIG, Delta, USG"}]
[{"$f":"IF(LEN('Translation-EN'!A1764)>0,'Translation-EN'!A1764,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1764)>0,'Translation-EN'!B1764,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1764)>0,'Translation-EN'!C1764,\"\")","v":"E156"},{"$f":"IF(LEN('Translation-EN'!D1764)>0,'Translation-EN'!D1764,\"\")","v":""},{"$f":"$E$1354","v":"R 3,7/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1765)>0,'Translation-EN'!A1765,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1765)>0,'Translation-EN'!B1765,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1765)>0,'Translation-EN'!C1765,\"\")","v":"B157"},{"$f":"IF(LEN('Translation-EN'!D1765)>0,'Translation-EN'!D1765,\"\")","v":""},"Laine minérale en vrac"]
[{"$f":"IF(LEN('Translation-EN'!A1766)>0,'Translation-EN'!A1766,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1766)>0,'Translation-EN'!B1766,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1766)>0,'Translation-EN'!C1766,\"\")","v":"C157"},{"$f":"IF(LEN('Translation-EN'!D1766)>0,'Translation-EN'!D1766,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1754","v":"NAIMA "}]
[{"$f":"IF(LEN('Translation-EN'!A1767)>0,'Translation-EN'!A1767,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1767)>0,'Translation-EN'!B1767,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1767)>0,'Translation-EN'!C1767,\"\")","v":"D157"},{"$f":"IF(LEN('Translation-EN'!D1767)>0,'Translation-EN'!D1767,\"\")","v":""},{"$f":"$E$1755","v":"Inclus : Rolan, Armstrong, Rockwool, Thermafiber, American Rock Wool, IIG, Delta, USG"}]
[{"$f":"IF(LEN('Translation-EN'!A1768)>0,'Translation-EN'!A1768,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1768)>0,'Translation-EN'!B1768,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1768)>0,'Translation-EN'!C1768,\"\")","v":"E157"},{"$f":"IF(LEN('Translation-EN'!D1768)>0,'Translation-EN'!D1768,\"\")","v":""},"R 3/po"]
[{"$f":"IF(LEN('Translation-EN'!A1769)>0,'Translation-EN'!A1769,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1769)>0,'Translation-EN'!B1769,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1769)>0,'Translation-EN'!C1769,\"\")","v":"B158"},{"$f":"IF(LEN('Translation-EN'!D1769)>0,'Translation-EN'!D1769,\"\")","v":""},"Panneau de mycélium"]
[{"$f":"IF(LEN('Translation-EN'!A1770)>0,'Translation-EN'!A1770,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1770)>0,'Translation-EN'!B1770,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1770)>0,'Translation-EN'!C1770,\"\")","v":"C158"},{"$f":"IF(LEN('Translation-EN'!D1770)>0,'Translation-EN'!D1770,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Ecovative"]
[{"$f":"IF(LEN('Translation-EN'!A1771)>0,'Translation-EN'!A1771,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1771)>0,'Translation-EN'!B1771,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1771)>0,'Translation-EN'!C1771,\"\")","v":"D158"},{"$f":"IF(LEN('Translation-EN'!D1771)>0,'Translation-EN'!D1771,\"\")","v":""},"Mycofoam"]
[{"$f":"IF(LEN('Translation-EN'!A1772)>0,'Translation-EN'!A1772,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1772)>0,'Translation-EN'!B1772,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1772)>0,'Translation-EN'!C1772,\"\")","v":"E158"},{"$f":"IF(LEN('Translation-EN'!D1772)>0,'Translation-EN'!D1772,\"\")","v":""},{"$f":"$E$1354","v":"R 3,7/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1773)>0,'Translation-EN'!A1773,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1773)>0,'Translation-EN'!B1773,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1773)>0,'Translation-EN'!C1773,\"\")","v":"B159"},{"$f":"IF(LEN('Translation-EN'!D1773)>0,'Translation-EN'!D1773,\"\")","v":""},"Panneau à copeaux orientés"]
[{"$f":"IF(LEN('Translation-EN'!A1774)>0,'Translation-EN'!A1774,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1774)>0,'Translation-EN'!B1774,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1774)>0,'Translation-EN'!C1774,\"\")","v":"C159"},{"$f":"IF(LEN('Translation-EN'!D1774)>0,'Translation-EN'!D1774,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1627","v":"Conseil américain du bois et Conseil canadien du bois"}]
[{"$f":"IF(LEN('Translation-EN'!A1775)>0,'Translation-EN'!A1775,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1775)>0,'Translation-EN'!B1775,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1775)>0,'Translation-EN'!C1775,\"\")","v":"B160"},{"$f":"IF(LEN('Translation-EN'!D1775)>0,'Translation-EN'!D1775,\"\")","v":""},{"$f":"$E$1773","v":"Panneau à copeaux orientés"}]
[{"$f":"IF(LEN('Translation-EN'!A1776)>0,'Translation-EN'!A1776,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1776)>0,'Translation-EN'!B1776,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1776)>0,'Translation-EN'!C1776,\"\")","v":"C160"},{"$f":"IF(LEN('Translation-EN'!D1776)>0,'Translation-EN'!D1776,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1627","v":"Conseil américain du bois et Conseil canadien du bois"}]
[{"$f":"IF(LEN('Translation-EN'!A1777)>0,'Translation-EN'!A1777,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1777)>0,'Translation-EN'!B1777,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1777)>0,'Translation-EN'!C1777,\"\")","v":"B161"},{"$f":"IF(LEN('Translation-EN'!D1777)>0,'Translation-EN'!D1777,\"\")","v":""},{"$f":"$E$1773","v":"Panneau à copeaux orientés"}]
[{"$f":"IF(LEN('Translation-EN'!A1778)>0,'Translation-EN'!A1778,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1778)>0,'Translation-EN'!B1778,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1778)>0,'Translation-EN'!C1778,\"\")","v":"C161"},{"$f":"IF(LEN('Translation-EN'!D1778)>0,'Translation-EN'!D1778,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Huber "]
[{"$f":"IF(LEN('Translation-EN'!A1779)>0,'Translation-EN'!A1779,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1779)>0,'Translation-EN'!B1779,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1779)>0,'Translation-EN'!C1779,\"\")","v":"D161"},{"$f":"IF(LEN('Translation-EN'!D1779)>0,'Translation-EN'!D1779,\"\")","v":""},"AdvanTech"]
[{"$f":"IF(LEN('Translation-EN'!A1780)>0,'Translation-EN'!A1780,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1780)>0,'Translation-EN'!B1780,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1780)>0,'Translation-EN'!C1780,\"\")","v":"E161"},{"$f":"IF(LEN('Translation-EN'!D1780)>0,'Translation-EN'!D1780,\"\")","v":""},"Panneau 1/2 po"]
[{"$f":"IF(LEN('Translation-EN'!A1781)>0,'Translation-EN'!A1781,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1781)>0,'Translation-EN'!B1781,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1781)>0,'Translation-EN'!C1781,\"\")","v":"B163"},{"$f":"IF(LEN('Translation-EN'!D1781)>0,'Translation-EN'!D1781,\"\")","v":""},{"$f":"$E$1773","v":"Panneau à copeaux orientés"}]
[{"$f":"IF(LEN('Translation-EN'!A1782)>0,'Translation-EN'!A1782,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1782)>0,'Translation-EN'!B1782,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1782)>0,'Translation-EN'!C1782,\"\")","v":"C163"},{"$f":"IF(LEN('Translation-EN'!D1782)>0,'Translation-EN'!D1782,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1778","v":"Huber "}]
[{"$f":"IF(LEN('Translation-EN'!A1783)>0,'Translation-EN'!A1783,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1783)>0,'Translation-EN'!B1783,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1783)>0,'Translation-EN'!C1783,\"\")","v":"D163"},{"$f":"IF(LEN('Translation-EN'!D1783)>0,'Translation-EN'!D1783,\"\")","v":""},"ZIP System"]
[{"$f":"IF(LEN('Translation-EN'!A1784)>0,'Translation-EN'!A1784,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1784)>0,'Translation-EN'!B1784,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1784)>0,'Translation-EN'!C1784,\"\")","v":"E163"},{"$f":"IF(LEN('Translation-EN'!D1784)>0,'Translation-EN'!D1784,\"\")","v":""},"Panneau 7/16 po, barrière de protection et ruban adhésif"]
[{"$f":"IF(LEN('Translation-EN'!A1785)>0,'Translation-EN'!A1785,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1785)>0,'Translation-EN'!B1785,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1785)>0,'Translation-EN'!C1785,\"\")","v":"B165"},{"$f":"IF(LEN('Translation-EN'!D1785)>0,'Translation-EN'!D1785,\"\")","v":""},"Panneau à copeaux orientés pour sous-plancher"]
[{"$f":"IF(LEN('Translation-EN'!A1786)>0,'Translation-EN'!A1786,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1786)>0,'Translation-EN'!B1786,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1786)>0,'Translation-EN'!C1786,\"\")","v":"C165"},{"$f":"IF(LEN('Translation-EN'!D1786)>0,'Translation-EN'!D1786,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1778","v":"Huber "}]
[{"$f":"IF(LEN('Translation-EN'!A1787)>0,'Translation-EN'!A1787,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1787)>0,'Translation-EN'!B1787,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1787)>0,'Translation-EN'!C1787,\"\")","v":"D165"},{"$f":"IF(LEN('Translation-EN'!D1787)>0,'Translation-EN'!D1787,\"\")","v":""},{"$f":"$E$1779","v":"AdvanTech"}]
[{"$f":"IF(LEN('Translation-EN'!A1788)>0,'Translation-EN'!A1788,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1788)>0,'Translation-EN'!B1788,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1788)>0,'Translation-EN'!C1788,\"\")","v":"E165"},{"$f":"IF(LEN('Translation-EN'!D1788)>0,'Translation-EN'!D1788,\"\")","v":""},"Sous-plancher 19/32 po"]
[{"$f":"IF(LEN('Translation-EN'!A1789)>0,'Translation-EN'!A1789,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1789)>0,'Translation-EN'!B1789,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1789)>0,'Translation-EN'!C1789,\"\")","v":"B167"},{"$f":"IF(LEN('Translation-EN'!D1789)>0,'Translation-EN'!D1789,\"\")","v":""},"Contreplaqué"]
[{"$f":"IF(LEN('Translation-EN'!A1790)>0,'Translation-EN'!A1790,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1790)>0,'Translation-EN'!B1790,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1790)>0,'Translation-EN'!C1790,\"\")","v":"C167"},{"$f":"IF(LEN('Translation-EN'!D1790)>0,'Translation-EN'!D1790,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1627","v":"Conseil américain du bois et Conseil canadien du bois"}]
[{"$f":"IF(LEN('Translation-EN'!A1791)>0,'Translation-EN'!A1791,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1791)>0,'Translation-EN'!B1791,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1791)>0,'Translation-EN'!C1791,\"\")","v":"B168"},{"$f":"IF(LEN('Translation-EN'!D1791)>0,'Translation-EN'!D1791,\"\")","v":""},{"$f":"$E$1789","v":"Contreplaqué"}]
[{"$f":"IF(LEN('Translation-EN'!A1792)>0,'Translation-EN'!A1792,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1792)>0,'Translation-EN'!B1792,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1792)>0,'Translation-EN'!C1792,\"\")","v":"C168"},{"$f":"IF(LEN('Translation-EN'!D1792)>0,'Translation-EN'!D1792,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1627","v":"Conseil américain du bois et Conseil canadien du bois"}]
[{"$f":"IF(LEN('Translation-EN'!A1793)>0,'Translation-EN'!A1793,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1793)>0,'Translation-EN'!B1793,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1793)>0,'Translation-EN'!C1793,\"\")","v":"B169"},{"$f":"IF(LEN('Translation-EN'!D1793)>0,'Translation-EN'!D1793,\"\")","v":""},{"$f":"$E$1789","v":"Contreplaqué"}]
[{"$f":"IF(LEN('Translation-EN'!A1794)>0,'Translation-EN'!A1794,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1794)>0,'Translation-EN'!B1794,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1794)>0,'Translation-EN'!C1794,\"\")","v":"C169"},{"$f":"IF(LEN('Translation-EN'!D1794)>0,'Translation-EN'!D1794,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1627","v":"Conseil américain du bois et Conseil canadien du bois"}]
[{"$f":"IF(LEN('Translation-EN'!A1795)>0,'Translation-EN'!A1795,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1795)>0,'Translation-EN'!B1795,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1795)>0,'Translation-EN'!C1795,\"\")","v":"B170"},{"$f":"IF(LEN('Translation-EN'!D1795)>0,'Translation-EN'!D1795,\"\")","v":""},"Polyiso – panneaux de toiture"]
[{"$f":"IF(LEN('Translation-EN'!A1796)>0,'Translation-EN'!A1796,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1796)>0,'Translation-EN'!B1796,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1796)>0,'Translation-EN'!C1796,\"\")","v":"C170"},{"$f":"IF(LEN('Translation-EN'!D1796)>0,'Translation-EN'!D1796,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Carlisle"]
[{"$f":"IF(LEN('Translation-EN'!A1797)>0,'Translation-EN'!A1797,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1797)>0,'Translation-EN'!B1797,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1797)>0,'Translation-EN'!C1797,\"\")","v":"D170"},{"$f":"IF(LEN('Translation-EN'!D1797)>0,'Translation-EN'!D1797,\"\")","v":""},"GRF cellulosic facer"]
[{"$f":"IF(LEN('Translation-EN'!A1798)>0,'Translation-EN'!A1798,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1798)>0,'Translation-EN'!B1798,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1798)>0,'Translation-EN'!C1798,\"\")","v":"E170"},{"$f":"IF(LEN('Translation-EN'!D1798)>0,'Translation-EN'!D1798,\"\")","v":""},"R 5,8/po"]
[{"$f":"IF(LEN('Translation-EN'!A1799)>0,'Translation-EN'!A1799,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1799)>0,'Translation-EN'!B1799,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1799)>0,'Translation-EN'!C1799,\"\")","v":"B172"},{"$f":"IF(LEN('Translation-EN'!D1799)>0,'Translation-EN'!D1799,\"\")","v":""},{"$f":"$E$1795","v":"Polyiso – panneaux de toiture"}]
[{"$f":"IF(LEN('Translation-EN'!A1800)>0,'Translation-EN'!A1800,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1800)>0,'Translation-EN'!B1800,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1800)>0,'Translation-EN'!C1800,\"\")","v":"C172"},{"$f":"IF(LEN('Translation-EN'!D1800)>0,'Translation-EN'!D1800,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Hunter"]
[{"$f":"IF(LEN('Translation-EN'!A1801)>0,'Translation-EN'!A1801,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1801)>0,'Translation-EN'!B1801,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1801)>0,'Translation-EN'!C1801,\"\")","v":"D172"},{"$f":"IF(LEN('Translation-EN'!D1801)>0,'Translation-EN'!D1801,\"\")","v":""},"Polyiso - panneaux de toiture"]
[{"$f":"IF(LEN('Translation-EN'!A1802)>0,'Translation-EN'!A1802,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1802)>0,'Translation-EN'!B1802,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1802)>0,'Translation-EN'!C1802,\"\")","v":"E172"},{"$f":"IF(LEN('Translation-EN'!D1802)>0,'Translation-EN'!D1802,\"\")","v":""},{"$f":"$E$1798","v":"R 5,8/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1803)>0,'Translation-EN'!A1803,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1803)>0,'Translation-EN'!B1803,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1803)>0,'Translation-EN'!C1803,\"\")","v":"B174"},{"$f":"IF(LEN('Translation-EN'!D1803)>0,'Translation-EN'!D1803,\"\")","v":""},{"$f":"$E$1795","v":"Polyiso – panneaux de toiture"}]
[{"$f":"IF(LEN('Translation-EN'!A1804)>0,'Translation-EN'!A1804,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1804)>0,'Translation-EN'!B1804,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1804)>0,'Translation-EN'!C1804,\"\")","v":"C174"},{"$f":"IF(LEN('Translation-EN'!D1804)>0,'Translation-EN'!D1804,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"PIMA"]
[{"$f":"IF(LEN('Translation-EN'!A1805)>0,'Translation-EN'!A1805,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1805)>0,'Translation-EN'!B1805,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1805)>0,'Translation-EN'!C1805,\"\")","v":"D174"},{"$f":"IF(LEN('Translation-EN'!D1805)>0,'Translation-EN'!D1805,\"\")","v":""},"Inclus : Atlas, Firestone, GAF, Johns Manville, Rmax"]
[{"$f":"IF(LEN('Translation-EN'!A1806)>0,'Translation-EN'!A1806,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1806)>0,'Translation-EN'!B1806,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1806)>0,'Translation-EN'!C1806,\"\")","v":"E174"},{"$f":"IF(LEN('Translation-EN'!D1806)>0,'Translation-EN'!D1806,\"\")","v":""},{"$f":"$E$1798","v":"R 5,8/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1807)>0,'Translation-EN'!A1807,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1807)>0,'Translation-EN'!B1807,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1807)>0,'Translation-EN'!C1807,\"\")","v":"B175"},{"$f":"IF(LEN('Translation-EN'!D1807)>0,'Translation-EN'!D1807,\"\")","v":""},{"$f":"$E$1795","v":"Polyiso – panneaux de toiture"}]
[{"$f":"IF(LEN('Translation-EN'!A1808)>0,'Translation-EN'!A1808,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1808)>0,'Translation-EN'!B1808,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1808)>0,'Translation-EN'!C1808,\"\")","v":"C175"},{"$f":"IF(LEN('Translation-EN'!D1808)>0,'Translation-EN'!D1808,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Versico"]
[{"$f":"IF(LEN('Translation-EN'!A1809)>0,'Translation-EN'!A1809,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1809)>0,'Translation-EN'!B1809,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1809)>0,'Translation-EN'!C1809,\"\")","v":"D175"},{"$f":"IF(LEN('Translation-EN'!D1809)>0,'Translation-EN'!D1809,\"\")","v":""},"VersiCore, SecurShield, DuraFaceR"]
[{"$f":"IF(LEN('Translation-EN'!A1810)>0,'Translation-EN'!A1810,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1810)>0,'Translation-EN'!B1810,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1810)>0,'Translation-EN'!C1810,\"\")","v":"E175"},{"$f":"IF(LEN('Translation-EN'!D1810)>0,'Translation-EN'!D1810,\"\")","v":""},{"$f":"$E$1798","v":"R 5,8/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1811)>0,'Translation-EN'!A1811,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1811)>0,'Translation-EN'!B1811,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1811)>0,'Translation-EN'!C1811,\"\")","v":"B176"},{"$f":"IF(LEN('Translation-EN'!D1811)>0,'Translation-EN'!D1811,\"\")","v":""},"Polyiso – panneaux de toiture"]
[{"$f":"IF(LEN('Translation-EN'!A1812)>0,'Translation-EN'!A1812,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1812)>0,'Translation-EN'!B1812,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1812)>0,'Translation-EN'!C1812,\"\")","v":"C176"},{"$f":"IF(LEN('Translation-EN'!D1812)>0,'Translation-EN'!D1812,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Dow Chemical Company"]
[{"$f":"IF(LEN('Translation-EN'!A1813)>0,'Translation-EN'!A1813,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1813)>0,'Translation-EN'!B1813,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1813)>0,'Translation-EN'!C1813,\"\")","v":"D176"},{"$f":"IF(LEN('Translation-EN'!D1813)>0,'Translation-EN'!D1813,\"\")","v":""},"Tuff-R, Super Tuff-R, Thermax"]
[{"$f":"IF(LEN('Translation-EN'!A1814)>0,'Translation-EN'!A1814,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1814)>0,'Translation-EN'!B1814,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1814)>0,'Translation-EN'!C1814,\"\")","v":"E176"},{"$f":"IF(LEN('Translation-EN'!D1814)>0,'Translation-EN'!D1814,\"\")","v":""},"R 6,5/po"]
[{"$f":"IF(LEN('Translation-EN'!A1815)>0,'Translation-EN'!A1815,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1815)>0,'Translation-EN'!B1815,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1815)>0,'Translation-EN'!C1815,\"\")","v":"B177"},{"$f":"IF(LEN('Translation-EN'!D1815)>0,'Translation-EN'!D1815,\"\")","v":""},{"$f":"$E$1811","v":"Polyiso – panneaux de toiture"}]
[{"$f":"IF(LEN('Translation-EN'!A1816)>0,'Translation-EN'!A1816,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1816)>0,'Translation-EN'!B1816,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1816)>0,'Translation-EN'!C1816,\"\")","v":"C177"},{"$f":"IF(LEN('Translation-EN'!D1816)>0,'Translation-EN'!D1816,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1800","v":"Hunter"}]
[{"$f":"IF(LEN('Translation-EN'!A1817)>0,'Translation-EN'!A1817,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1817)>0,'Translation-EN'!B1817,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1817)>0,'Translation-EN'!C1817,\"\")","v":"D177"},{"$f":"IF(LEN('Translation-EN'!D1817)>0,'Translation-EN'!D1817,\"\")","v":""},"Polyiso - panneaux de mur"]
[{"$f":"IF(LEN('Translation-EN'!A1818)>0,'Translation-EN'!A1818,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1818)>0,'Translation-EN'!B1818,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1818)>0,'Translation-EN'!C1818,\"\")","v":"E177"},{"$f":"IF(LEN('Translation-EN'!D1818)>0,'Translation-EN'!D1818,\"\")","v":""},{"$f":"$E$1814","v":"R 6,5/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1819)>0,'Translation-EN'!A1819,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1819)>0,'Translation-EN'!B1819,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1819)>0,'Translation-EN'!C1819,\"\")","v":"B179"},{"$f":"IF(LEN('Translation-EN'!D1819)>0,'Translation-EN'!D1819,\"\")","v":""},{"$f":"$E$1811","v":"Polyiso – panneaux de toiture"}]
[{"$f":"IF(LEN('Translation-EN'!A1820)>0,'Translation-EN'!A1820,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1820)>0,'Translation-EN'!B1820,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1820)>0,'Translation-EN'!C1820,\"\")","v":"C179"},{"$f":"IF(LEN('Translation-EN'!D1820)>0,'Translation-EN'!D1820,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1804","v":"PIMA"}]
[{"$f":"IF(LEN('Translation-EN'!A1821)>0,'Translation-EN'!A1821,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1821)>0,'Translation-EN'!B1821,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1821)>0,'Translation-EN'!C1821,\"\")","v":"D179"},{"$f":"IF(LEN('Translation-EN'!D1821)>0,'Translation-EN'!D1821,\"\")","v":""},{"$f":"$E$1805","v":"Inclus : Atlas, Firestone, GAF, Johns Manville, Rmax"}]
[{"$f":"IF(LEN('Translation-EN'!A1822)>0,'Translation-EN'!A1822,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1822)>0,'Translation-EN'!B1822,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1822)>0,'Translation-EN'!C1822,\"\")","v":"E179"},{"$f":"IF(LEN('Translation-EN'!D1822)>0,'Translation-EN'!D1822,\"\")","v":""},{"$f":"$E$1814","v":"R 6,5/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1823)>0,'Translation-EN'!A1823,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1823)>0,'Translation-EN'!B1823,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1823)>0,'Translation-EN'!C1823,\"\")","v":"B180"},{"$f":"IF(LEN('Translation-EN'!D1823)>0,'Translation-EN'!D1823,\"\")","v":""},"Revêtement en polypropylène"]
[{"$f":"IF(LEN('Translation-EN'!A1824)>0,'Translation-EN'!A1824,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1824)>0,'Translation-EN'!B1824,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1824)>0,'Translation-EN'!C1824,\"\")","v":"C180"},{"$f":"IF(LEN('Translation-EN'!D1824)>0,'Translation-EN'!D1824,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Novik"]
[{"$f":"IF(LEN('Translation-EN'!A1825)>0,'Translation-EN'!A1825,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1825)>0,'Translation-EN'!B1825,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1825)>0,'Translation-EN'!C1825,\"\")","v":"D180"},{"$f":"IF(LEN('Translation-EN'!D1825)>0,'Translation-EN'!D1825,\"\")","v":""},"NovikStone, NovikShake"]
[{"$f":"IF(LEN('Translation-EN'!A1826)>0,'Translation-EN'!A1826,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1826)>0,'Translation-EN'!B1826,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1826)>0,'Translation-EN'!C1826,\"\")","v":"E180"},{"$f":"IF(LEN('Translation-EN'!D1826)>0,'Translation-EN'!D1826,\"\")","v":""},"Moyenne de 5 produits"]
[{"$f":"IF(LEN('Translation-EN'!A1827)>0,'Translation-EN'!A1827,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1827)>0,'Translation-EN'!B1827,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1827)>0,'Translation-EN'!C1827,\"\")","v":"B181"},{"$f":"IF(LEN('Translation-EN'!D1827)>0,'Translation-EN'!D1827,\"\")","v":""},{"$f":"$E$1823","v":"Revêtement en polypropylène"}]
[{"$f":"IF(LEN('Translation-EN'!A1828)>0,'Translation-EN'!A1828,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1828)>0,'Translation-EN'!B1828,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1828)>0,'Translation-EN'!C1828,\"\")","v":"C181"},{"$f":"IF(LEN('Translation-EN'!D1828)>0,'Translation-EN'!D1828,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Institut de revêtement en vinyle"]
[{"$f":"IF(LEN('Translation-EN'!A1829)>0,'Translation-EN'!A1829,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1829)>0,'Translation-EN'!B1829,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1829)>0,'Translation-EN'!C1829,\"\")","v":"E181"},{"$f":"IF(LEN('Translation-EN'!D1829)>0,'Translation-EN'!D1829,\"\")","v":""},"0,085 po bardeau de fente simple \"Cèdre\" 7 po"]
[{"$f":"IF(LEN('Translation-EN'!A1830)>0,'Translation-EN'!A1830,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1830)>0,'Translation-EN'!B1830,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1830)>0,'Translation-EN'!C1830,\"\")","v":"B183"},{"$f":"IF(LEN('Translation-EN'!D1830)>0,'Translation-EN'!D1830,\"\")","v":""},"Sangle CBI en polypropylène"]
[{"$f":"IF(LEN('Translation-EN'!A1831)>0,'Translation-EN'!A1831,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1831)>0,'Translation-EN'!B1831,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1831)>0,'Translation-EN'!C1831,\"\")","v":"B184"},{"$f":"IF(LEN('Translation-EN'!D1831)>0,'Translation-EN'!D1831,\"\")","v":""},"Membrane de toiture en PVC"]
[{"$f":"IF(LEN('Translation-EN'!A1832)>0,'Translation-EN'!A1832,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1832)>0,'Translation-EN'!B1832,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1832)>0,'Translation-EN'!C1832,\"\")","v":"C184"},{"$f":"IF(LEN('Translation-EN'!D1832)>0,'Translation-EN'!D1832,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"CIFA"]
[{"$f":"IF(LEN('Translation-EN'!A1833)>0,'Translation-EN'!A1833,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1833)>0,'Translation-EN'!B1833,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1833)>0,'Translation-EN'!C1833,\"\")","v":"D184"},{"$f":"IF(LEN('Translation-EN'!D1833)>0,'Translation-EN'!D1833,\"\")","v":""},"Inclus : Canadian General-Tower, Duro-Last, FiberTite"]
[{"$f":"IF(LEN('Translation-EN'!A1834)>0,'Translation-EN'!A1834,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1834)>0,'Translation-EN'!B1834,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1834)>0,'Translation-EN'!C1834,\"\")","v":"E184"},{"$f":"IF(LEN('Translation-EN'!D1834)>0,'Translation-EN'!D1834,\"\")","v":""},"48 mils"]
[{"$f":"IF(LEN('Translation-EN'!A1835)>0,'Translation-EN'!A1835,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1835)>0,'Translation-EN'!B1835,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1835)>0,'Translation-EN'!C1835,\"\")","v":"B185"},{"$f":"IF(LEN('Translation-EN'!D1835)>0,'Translation-EN'!D1835,\"\")","v":""},"Terre battue"]
[{"$f":"IF(LEN('Translation-EN'!A1836)>0,'Translation-EN'!A1836,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1836)>0,'Translation-EN'!B1836,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1836)>0,'Translation-EN'!C1836,\"\")","v":"D185"},{"$f":"IF(LEN('Translation-EN'!D1836)>0,'Translation-EN'!D1836,\"\")","v":""},"Stabilisé avec 3 % de CHN"]
[{"$f":"IF(LEN('Translation-EN'!A1837)>0,'Translation-EN'!A1837,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1837)>0,'Translation-EN'!B1837,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1837)>0,'Translation-EN'!C1837,\"\")","v":"B186"},{"$f":"IF(LEN('Translation-EN'!D1837)>0,'Translation-EN'!D1837,\"\")","v":""},{"$f":"$E$1835","v":"Terre battue"}]
[{"$f":"IF(LEN('Translation-EN'!A1838)>0,'Translation-EN'!A1838,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1838)>0,'Translation-EN'!B1838,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1838)>0,'Translation-EN'!C1838,\"\")","v":"D186"},{"$f":"IF(LEN('Translation-EN'!D1838)>0,'Translation-EN'!D1838,\"\")","v":""},"Stabilisé avec 5 % de ciment"]
[{"$f":"IF(LEN('Translation-EN'!A1839)>0,'Translation-EN'!A1839,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1839)>0,'Translation-EN'!B1839,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1839)>0,'Translation-EN'!C1839,\"\")","v":"B187"},{"$f":"IF(LEN('Translation-EN'!D1839)>0,'Translation-EN'!D1839,\"\")","v":""},{"$f":"$E$1835","v":"Terre battue"}]
[{"$f":"IF(LEN('Translation-EN'!A1840)>0,'Translation-EN'!A1840,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1840)>0,'Translation-EN'!B1840,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1840)>0,'Translation-EN'!C1840,\"\")","v":"D187"},{"$f":"IF(LEN('Translation-EN'!D1840)>0,'Translation-EN'!D1840,\"\")","v":""},"Stabilisé avec 8 % de ciment"]
[{"$f":"IF(LEN('Translation-EN'!A1841)>0,'Translation-EN'!A1841,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1841)>0,'Translation-EN'!B1841,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1841)>0,'Translation-EN'!C1841,\"\")","v":"B188"},{"$f":"IF(LEN('Translation-EN'!D1841)>0,'Translation-EN'!D1841,\"\")","v":""},"Barre d’armature"]
[{"$f":"IF(LEN('Translation-EN'!A1842)>0,'Translation-EN'!A1842,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1842)>0,'Translation-EN'!B1842,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1842)>0,'Translation-EN'!C1842,\"\")","v":"C188"},{"$f":"IF(LEN('Translation-EN'!D1842)>0,'Translation-EN'!D1842,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Institut de l’acier pour béton armé"]
[{"$f":"IF(LEN('Translation-EN'!A1843)>0,'Translation-EN'!A1843,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1843)>0,'Translation-EN'!B1843,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1843)>0,'Translation-EN'!C1843,\"\")","v":"E188"},{"$f":"IF(LEN('Translation-EN'!D1843)>0,'Translation-EN'!D1843,\"\")","v":""},"10M"]
[{"$f":"IF(LEN('Translation-EN'!A1844)>0,'Translation-EN'!A1844,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1844)>0,'Translation-EN'!B1844,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1844)>0,'Translation-EN'!C1844,\"\")","v":"B189"},{"$f":"IF(LEN('Translation-EN'!D1844)>0,'Translation-EN'!D1844,\"\")","v":""},{"$f":"$E$1841","v":"Barre d’armature"}]
[{"$f":"IF(LEN('Translation-EN'!A1845)>0,'Translation-EN'!A1845,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1845)>0,'Translation-EN'!B1845,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1845)>0,'Translation-EN'!C1845,\"\")","v":"C189"},{"$f":"IF(LEN('Translation-EN'!D1845)>0,'Translation-EN'!D1845,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1842","v":"Institut de l’acier pour béton armé"}]
[{"$f":"IF(LEN('Translation-EN'!A1846)>0,'Translation-EN'!A1846,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1846)>0,'Translation-EN'!B1846,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1846)>0,'Translation-EN'!C1846,\"\")","v":"E189"},{"$f":"IF(LEN('Translation-EN'!D1846)>0,'Translation-EN'!D1846,\"\")","v":""},"15M"]
[{"$f":"IF(LEN('Translation-EN'!A1847)>0,'Translation-EN'!A1847,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1847)>0,'Translation-EN'!B1847,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1847)>0,'Translation-EN'!C1847,\"\")","v":"B190"},{"$f":"IF(LEN('Translation-EN'!D1847)>0,'Translation-EN'!D1847,\"\")","v":""},"Revêtement de plancher en caoutchouc"]
[{"$f":"IF(LEN('Translation-EN'!A1848)>0,'Translation-EN'!A1848,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1848)>0,'Translation-EN'!B1848,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1848)>0,'Translation-EN'!C1848,\"\")","v":"C190"},{"$f":"IF(LEN('Translation-EN'!D1848)>0,'Translation-EN'!D1848,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"ECOsurfaces"]
[{"$f":"IF(LEN('Translation-EN'!A1849)>0,'Translation-EN'!A1849,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1849)>0,'Translation-EN'!B1849,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1849)>0,'Translation-EN'!C1849,\"\")","v":"D190"},{"$f":"IF(LEN('Translation-EN'!D1849)>0,'Translation-EN'!D1849,\"\")","v":""},{"$f":"$E$1848","v":"ECOsurfaces"}]
[{"$f":"IF(LEN('Translation-EN'!A1850)>0,'Translation-EN'!A1850,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1850)>0,'Translation-EN'!B1850,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1850)>0,'Translation-EN'!C1850,\"\")","v":"B191"},{"$f":"IF(LEN('Translation-EN'!D1850)>0,'Translation-EN'!D1850,\"\")","v":""},{"$f":"$E$1847","v":"Revêtement de plancher en caoutchouc"}]
[{"$f":"IF(LEN('Translation-EN'!A1851)>0,'Translation-EN'!A1851,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1851)>0,'Translation-EN'!B1851,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1851)>0,'Translation-EN'!C1851,\"\")","v":"C191"},{"$f":"IF(LEN('Translation-EN'!D1851)>0,'Translation-EN'!D1851,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Institut des revêtements de sol résilients"]
[{"$f":"IF(LEN('Translation-EN'!A1852)>0,'Translation-EN'!A1852,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1852)>0,'Translation-EN'!B1852,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1852)>0,'Translation-EN'!C1852,\"\")","v":"D191"},{"$f":"IF(LEN('Translation-EN'!D1852)>0,'Translation-EN'!D1852,\"\")","v":""},"Comprend des carreaux et des rouleaux d’American Biltrite, Armstrong, Burke, FLEXCO, Johnsonite, Mannington, Roppe et Tarkett."]
[{"$f":"IF(LEN('Translation-EN'!A1853)>0,'Translation-EN'!A1853,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1853)>0,'Translation-EN'!B1853,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1853)>0,'Translation-EN'!C1853,\"\")","v":"B192"},{"$f":"IF(LEN('Translation-EN'!D1853)>0,'Translation-EN'!D1853,\"\")","v":""},"Toitures en bitume modifié SBS"]
[{"$f":"IF(LEN('Translation-EN'!A1854)>0,'Translation-EN'!A1854,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1854)>0,'Translation-EN'!B1854,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1854)>0,'Translation-EN'!C1854,\"\")","v":"C192"},{"$f":"IF(LEN('Translation-EN'!D1854)>0,'Translation-EN'!D1854,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"ARMA"]
[{"$f":"IF(LEN('Translation-EN'!A1855)>0,'Translation-EN'!A1855,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1855)>0,'Translation-EN'!B1855,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1855)>0,'Translation-EN'!C1855,\"\")","v":"D192"},{"$f":"IF(LEN('Translation-EN'!D1855)>0,'Translation-EN'!D1855,\"\")","v":""},"Inclus : CertainTeed, Firestone, GAF, Henry, IKO, Johns Mansville, Malarkey, Siplast, Soprema"]
[{"$f":"IF(LEN('Translation-EN'!A1856)>0,'Translation-EN'!A1856,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1856)>0,'Translation-EN'!B1856,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1856)>0,'Translation-EN'!C1856,\"\")","v":"B193"},{"$f":"IF(LEN('Translation-EN'!D1856)>0,'Translation-EN'!D1856,\"\")","v":""},"Panneau structurel isolé – Noyau de mousse EPS "]
[{"$f":"IF(LEN('Translation-EN'!A1857)>0,'Translation-EN'!A1857,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1857)>0,'Translation-EN'!B1857,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1857)>0,'Translation-EN'!C1857,\"\")","v":"E193"},{"$f":"IF(LEN('Translation-EN'!D1857)>0,'Translation-EN'!D1857,\"\")","v":""},"OSB 7/16 po, EPS de type II"]
[{"$f":"IF(LEN('Translation-EN'!A1858)>0,'Translation-EN'!A1858,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1858)>0,'Translation-EN'!B1858,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1858)>0,'Translation-EN'!C1858,\"\")","v":"B194"},{"$f":"IF(LEN('Translation-EN'!D1858)>0,'Translation-EN'!D1858,\"\")","v":""},"Panneau structurel isolé – Noyau de paille"]
[{"$f":"IF(LEN('Translation-EN'!A1859)>0,'Translation-EN'!A1859,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1859)>0,'Translation-EN'!B1859,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1859)>0,'Translation-EN'!C1859,\"\")","v":"C194"},{"$f":"IF(LEN('Translation-EN'!D1859)>0,'Translation-EN'!D1859,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Agriboard"]
[{"$f":"IF(LEN('Translation-EN'!A1860)>0,'Translation-EN'!A1860,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1860)>0,'Translation-EN'!B1860,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1860)>0,'Translation-EN'!C1860,\"\")","v":"D194"},{"$f":"IF(LEN('Translation-EN'!D1860)>0,'Translation-EN'!D1860,\"\")","v":""},"Agriboard 7-7/8 po"]
[{"$f":"IF(LEN('Translation-EN'!A1861)>0,'Translation-EN'!A1861,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1861)>0,'Translation-EN'!B1861,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1861)>0,'Translation-EN'!C1861,\"\")","v":"E194"},{"$f":"IF(LEN('Translation-EN'!D1861)>0,'Translation-EN'!D1861,\"\")","v":""},"R?/po"]
[{"$f":"IF(LEN('Translation-EN'!A1862)>0,'Translation-EN'!A1862,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1862)>0,'Translation-EN'!B1862,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1862)>0,'Translation-EN'!C1862,\"\")","v":"B195"},{"$f":"IF(LEN('Translation-EN'!D1862)>0,'Translation-EN'!D1862,\"\")","v":""},"Mousse de polyuréthane pulvérisée – Cellule fermée (HFC)"]
[{"$f":"IF(LEN('Translation-EN'!A1863)>0,'Translation-EN'!A1863,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1863)>0,'Translation-EN'!B1863,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1863)>0,'Translation-EN'!C1863,\"\")","v":"C195"},{"$f":"IF(LEN('Translation-EN'!D1863)>0,'Translation-EN'!D1863,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"AMPP"]
[{"$f":"IF(LEN('Translation-EN'!A1864)>0,'Translation-EN'!A1864,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1864)>0,'Translation-EN'!B1864,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1864)>0,'Translation-EN'!C1864,\"\")","v":"E195"},{"$f":"IF(LEN('Translation-EN'!D1864)>0,'Translation-EN'!D1864,\"\")","v":""},"R 6,6/po"]
[{"$f":"IF(LEN('Translation-EN'!A1865)>0,'Translation-EN'!A1865,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1865)>0,'Translation-EN'!B1865,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1865)>0,'Translation-EN'!C1865,\"\")","v":"B196"},{"$f":"IF(LEN('Translation-EN'!D1865)>0,'Translation-EN'!D1865,\"\")","v":""},"Isolant mousse de polyuréthane giclée - structure alvéolaire fermée - à gas HFO"]
[{"$f":"IF(LEN('Translation-EN'!A1866)>0,'Translation-EN'!A1866,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1866)>0,'Translation-EN'!B1866,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1866)>0,'Translation-EN'!C1866,\"\")","v":"C196"},{"$f":"IF(LEN('Translation-EN'!D1866)>0,'Translation-EN'!D1866,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1863","v":"AMPP"}]
[{"$f":"IF(LEN('Translation-EN'!A1867)>0,'Translation-EN'!A1867,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1867)>0,'Translation-EN'!B1867,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1867)>0,'Translation-EN'!C1867,\"\")","v":"E196"},{"$f":"IF(LEN('Translation-EN'!D1867)>0,'Translation-EN'!D1867,\"\")","v":""},{"$f":"$E$1864","v":"R 6,6/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1868)>0,'Translation-EN'!A1868,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1868)>0,'Translation-EN'!B1868,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1868)>0,'Translation-EN'!C1868,\"\")","v":"B198"},{"$f":"IF(LEN('Translation-EN'!D1868)>0,'Translation-EN'!D1868,\"\")","v":""},"Mousse de polyuréthane pulvérisée – Haute densité (HFC)"]
[{"$f":"IF(LEN('Translation-EN'!A1869)>0,'Translation-EN'!A1869,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1869)>0,'Translation-EN'!B1869,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1869)>0,'Translation-EN'!C1869,\"\")","v":"C198"},{"$f":"IF(LEN('Translation-EN'!D1869)>0,'Translation-EN'!D1869,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1863","v":"AMPP"}]
[{"$f":"IF(LEN('Translation-EN'!A1870)>0,'Translation-EN'!A1870,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1870)>0,'Translation-EN'!B1870,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1870)>0,'Translation-EN'!C1870,\"\")","v":"E198"},{"$f":"IF(LEN('Translation-EN'!D1870)>0,'Translation-EN'!D1870,\"\")","v":""},"R 6,3/po"]
[{"$f":"IF(LEN('Translation-EN'!A1871)>0,'Translation-EN'!A1871,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1871)>0,'Translation-EN'!B1871,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1871)>0,'Translation-EN'!C1871,\"\")","v":"B199"},{"$f":"IF(LEN('Translation-EN'!D1871)>0,'Translation-EN'!D1871,\"\")","v":""},"Isolant mousse de polyuréthane giclée - haute densité - à gas HFO"]
[{"$f":"IF(LEN('Translation-EN'!A1872)>0,'Translation-EN'!A1872,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1872)>0,'Translation-EN'!B1872,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1872)>0,'Translation-EN'!C1872,\"\")","v":"C199"},{"$f":"IF(LEN('Translation-EN'!D1872)>0,'Translation-EN'!D1872,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1863","v":"AMPP"}]
[{"$f":"IF(LEN('Translation-EN'!A1873)>0,'Translation-EN'!A1873,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1873)>0,'Translation-EN'!B1873,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1873)>0,'Translation-EN'!C1873,\"\")","v":"E199"},{"$f":"IF(LEN('Translation-EN'!D1873)>0,'Translation-EN'!D1873,\"\")","v":""},{"$f":"$E$1814","v":"R 6,5/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1874)>0,'Translation-EN'!A1874,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1874)>0,'Translation-EN'!B1874,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1874)>0,'Translation-EN'!C1874,\"\")","v":"B201"},{"$f":"IF(LEN('Translation-EN'!D1874)>0,'Translation-EN'!D1874,\"\")","v":""},"Mousse de polyuréthane pulvérisée – Cellule ouverte (HFC)"]
[{"$f":"IF(LEN('Translation-EN'!A1875)>0,'Translation-EN'!A1875,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1875)>0,'Translation-EN'!B1875,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1875)>0,'Translation-EN'!C1875,\"\")","v":"C201"},{"$f":"IF(LEN('Translation-EN'!D1875)>0,'Translation-EN'!D1875,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1863","v":"AMPP"}]
[{"$f":"IF(LEN('Translation-EN'!A1876)>0,'Translation-EN'!A1876,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1876)>0,'Translation-EN'!B1876,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1876)>0,'Translation-EN'!C1876,\"\")","v":"E201"},{"$f":"IF(LEN('Translation-EN'!D1876)>0,'Translation-EN'!D1876,\"\")","v":""},"R 4,1/po"]
[{"$f":"IF(LEN('Translation-EN'!A1877)>0,'Translation-EN'!A1877,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1877)>0,'Translation-EN'!B1877,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1877)>0,'Translation-EN'!C1877,\"\")","v":"B202"},{"$f":"IF(LEN('Translation-EN'!D1877)>0,'Translation-EN'!D1877,\"\")","v":""},"Isolant mousse de polyuréthane giclée - structure alvéolaire ouverte - à gas HFO"]
[{"$f":"IF(LEN('Translation-EN'!A1878)>0,'Translation-EN'!A1878,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1878)>0,'Translation-EN'!B1878,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1878)>0,'Translation-EN'!C1878,\"\")","v":"C202"},{"$f":"IF(LEN('Translation-EN'!D1878)>0,'Translation-EN'!D1878,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1863","v":"AMPP"}]
[{"$f":"IF(LEN('Translation-EN'!A1879)>0,'Translation-EN'!A1879,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1879)>0,'Translation-EN'!B1879,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1879)>0,'Translation-EN'!C1879,\"\")","v":"E202"},{"$f":"IF(LEN('Translation-EN'!D1879)>0,'Translation-EN'!D1879,\"\")","v":""},{"$f":"$E$1876","v":"R 4,1/po"}]
[{"$f":"IF(LEN('Translation-EN'!A1880)>0,'Translation-EN'!A1880,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1880)>0,'Translation-EN'!B1880,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1880)>0,'Translation-EN'!C1880,\"\")","v":"B204"},{"$f":"IF(LEN('Translation-EN'!D1880)>0,'Translation-EN'!D1880,\"\")","v":""},"Poutre en acier"]
[{"$f":"IF(LEN('Translation-EN'!A1881)>0,'Translation-EN'!A1881,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1881)>0,'Translation-EN'!B1881,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1881)>0,'Translation-EN'!C1881,\"\")","v":"C204"},{"$f":"IF(LEN('Translation-EN'!D1881)>0,'Translation-EN'!D1881,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Institut américain de la construction métallique"]
[{"$f":"IF(LEN('Translation-EN'!A1882)>0,'Translation-EN'!A1882,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1882)>0,'Translation-EN'!B1882,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1882)>0,'Translation-EN'!C1882,\"\")","v":"D204"},{"$f":"IF(LEN('Translation-EN'!D1882)>0,'Translation-EN'!D1882,\"\")","v":""},"Acier de construction laminé à chaud"]
[{"$f":"IF(LEN('Translation-EN'!A1883)>0,'Translation-EN'!A1883,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1883)>0,'Translation-EN'!B1883,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1883)>0,'Translation-EN'!C1883,\"\")","v":"E204"},{"$f":"IF(LEN('Translation-EN'!D1883)>0,'Translation-EN'!D1883,\"\")","v":""},"W150x22 (W6x15)"]
[{"$f":"IF(LEN('Translation-EN'!A1884)>0,'Translation-EN'!A1884,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1884)>0,'Translation-EN'!B1884,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1884)>0,'Translation-EN'!C1884,\"\")","v":"B205"},{"$f":"IF(LEN('Translation-EN'!D1884)>0,'Translation-EN'!D1884,\"\")","v":""},{"$f":"$E$1880","v":"Poutre en acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1885)>0,'Translation-EN'!A1885,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1885)>0,'Translation-EN'!B1885,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1885)>0,'Translation-EN'!C1885,\"\")","v":"C205"},{"$f":"IF(LEN('Translation-EN'!D1885)>0,'Translation-EN'!D1885,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1881","v":"Institut américain de la construction métallique"}]
[{"$f":"IF(LEN('Translation-EN'!A1886)>0,'Translation-EN'!A1886,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1886)>0,'Translation-EN'!B1886,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1886)>0,'Translation-EN'!C1886,\"\")","v":"D205"},{"$f":"IF(LEN('Translation-EN'!D1886)>0,'Translation-EN'!D1886,\"\")","v":""},{"$f":"$E$1882","v":"Acier de construction laminé à chaud"}]
[{"$f":"IF(LEN('Translation-EN'!A1887)>0,'Translation-EN'!A1887,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1887)>0,'Translation-EN'!B1887,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1887)>0,'Translation-EN'!C1887,\"\")","v":"E205"},{"$f":"IF(LEN('Translation-EN'!D1887)>0,'Translation-EN'!D1887,\"\")","v":""},"W200x22 (W8x15)"]
[{"$f":"IF(LEN('Translation-EN'!A1888)>0,'Translation-EN'!A1888,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1888)>0,'Translation-EN'!B1888,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1888)>0,'Translation-EN'!C1888,\"\")","v":"B206"},{"$f":"IF(LEN('Translation-EN'!D1888)>0,'Translation-EN'!D1888,\"\")","v":""},{"$f":"$E$1880","v":"Poutre en acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1889)>0,'Translation-EN'!A1889,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1889)>0,'Translation-EN'!B1889,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1889)>0,'Translation-EN'!C1889,\"\")","v":"C206"},{"$f":"IF(LEN('Translation-EN'!D1889)>0,'Translation-EN'!D1889,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1881","v":"Institut américain de la construction métallique"}]
[{"$f":"IF(LEN('Translation-EN'!A1890)>0,'Translation-EN'!A1890,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1890)>0,'Translation-EN'!B1890,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1890)>0,'Translation-EN'!C1890,\"\")","v":"D206"},{"$f":"IF(LEN('Translation-EN'!D1890)>0,'Translation-EN'!D1890,\"\")","v":""},{"$f":"$E$1882","v":"Acier de construction laminé à chaud"}]
[{"$f":"IF(LEN('Translation-EN'!A1891)>0,'Translation-EN'!A1891,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1891)>0,'Translation-EN'!B1891,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1891)>0,'Translation-EN'!C1891,\"\")","v":"E206"},{"$f":"IF(LEN('Translation-EN'!D1891)>0,'Translation-EN'!D1891,\"\")","v":""},"W200x27 (W8x18)"]
[{"$f":"IF(LEN('Translation-EN'!A1892)>0,'Translation-EN'!A1892,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1892)>0,'Translation-EN'!B1892,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1892)>0,'Translation-EN'!C1892,\"\")","v":"B207"},{"$f":"IF(LEN('Translation-EN'!D1892)>0,'Translation-EN'!D1892,\"\")","v":""},{"$f":"$E$1880","v":"Poutre en acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1893)>0,'Translation-EN'!A1893,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1893)>0,'Translation-EN'!B1893,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1893)>0,'Translation-EN'!C1893,\"\")","v":"C207"},{"$f":"IF(LEN('Translation-EN'!D1893)>0,'Translation-EN'!D1893,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1881","v":"Institut américain de la construction métallique"}]
[{"$f":"IF(LEN('Translation-EN'!A1894)>0,'Translation-EN'!A1894,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1894)>0,'Translation-EN'!B1894,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1894)>0,'Translation-EN'!C1894,\"\")","v":"D207"},{"$f":"IF(LEN('Translation-EN'!D1894)>0,'Translation-EN'!D1894,\"\")","v":""},{"$f":"$E$1882","v":"Acier de construction laminé à chaud"}]
[{"$f":"IF(LEN('Translation-EN'!A1895)>0,'Translation-EN'!A1895,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1895)>0,'Translation-EN'!B1895,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1895)>0,'Translation-EN'!C1895,\"\")","v":"E207"},{"$f":"IF(LEN('Translation-EN'!D1895)>0,'Translation-EN'!D1895,\"\")","v":""},"W200x31 (W8x21)"]
[{"$f":"IF(LEN('Translation-EN'!A1896)>0,'Translation-EN'!A1896,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1896)>0,'Translation-EN'!B1896,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1896)>0,'Translation-EN'!C1896,\"\")","v":"B208"},{"$f":"IF(LEN('Translation-EN'!D1896)>0,'Translation-EN'!D1896,\"\")","v":""},{"$f":"$E$1880","v":"Poutre en acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1897)>0,'Translation-EN'!A1897,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1897)>0,'Translation-EN'!B1897,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1897)>0,'Translation-EN'!C1897,\"\")","v":"C208"},{"$f":"IF(LEN('Translation-EN'!D1897)>0,'Translation-EN'!D1897,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1881","v":"Institut américain de la construction métallique"}]
[{"$f":"IF(LEN('Translation-EN'!A1898)>0,'Translation-EN'!A1898,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1898)>0,'Translation-EN'!B1898,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1898)>0,'Translation-EN'!C1898,\"\")","v":"D208"},{"$f":"IF(LEN('Translation-EN'!D1898)>0,'Translation-EN'!D1898,\"\")","v":""},{"$f":"$E$1882","v":"Acier de construction laminé à chaud"}]
[{"$f":"IF(LEN('Translation-EN'!A1899)>0,'Translation-EN'!A1899,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1899)>0,'Translation-EN'!B1899,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1899)>0,'Translation-EN'!C1899,\"\")","v":"E208"},{"$f":"IF(LEN('Translation-EN'!D1899)>0,'Translation-EN'!D1899,\"\")","v":""},"W250x25 (W10x17)"]
[{"$f":"IF(LEN('Translation-EN'!A1900)>0,'Translation-EN'!A1900,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1900)>0,'Translation-EN'!B1900,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1900)>0,'Translation-EN'!C1900,\"\")","v":"B209"},{"$f":"IF(LEN('Translation-EN'!D1900)>0,'Translation-EN'!D1900,\"\")","v":""},{"$f":"$E$1880","v":"Poutre en acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1901)>0,'Translation-EN'!A1901,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1901)>0,'Translation-EN'!B1901,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1901)>0,'Translation-EN'!C1901,\"\")","v":"C209"},{"$f":"IF(LEN('Translation-EN'!D1901)>0,'Translation-EN'!D1901,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1881","v":"Institut américain de la construction métallique"}]
[{"$f":"IF(LEN('Translation-EN'!A1902)>0,'Translation-EN'!A1902,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1902)>0,'Translation-EN'!B1902,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1902)>0,'Translation-EN'!C1902,\"\")","v":"D209"},{"$f":"IF(LEN('Translation-EN'!D1902)>0,'Translation-EN'!D1902,\"\")","v":""},{"$f":"$E$1882","v":"Acier de construction laminé à chaud"}]
[{"$f":"IF(LEN('Translation-EN'!A1903)>0,'Translation-EN'!A1903,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1903)>0,'Translation-EN'!B1903,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1903)>0,'Translation-EN'!C1903,\"\")","v":"E209"},{"$f":"IF(LEN('Translation-EN'!D1903)>0,'Translation-EN'!D1903,\"\")","v":""},"W250x33 (W10x22)"]
[{"$f":"IF(LEN('Translation-EN'!A1904)>0,'Translation-EN'!A1904,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1904)>0,'Translation-EN'!B1904,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1904)>0,'Translation-EN'!C1904,\"\")","v":"B210"},{"$f":"IF(LEN('Translation-EN'!D1904)>0,'Translation-EN'!D1904,\"\")","v":""},{"$f":"$E$1880","v":"Poutre en acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1905)>0,'Translation-EN'!A1905,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1905)>0,'Translation-EN'!B1905,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1905)>0,'Translation-EN'!C1905,\"\")","v":"C210"},{"$f":"IF(LEN('Translation-EN'!D1905)>0,'Translation-EN'!D1905,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1881","v":"Institut américain de la construction métallique"}]
[{"$f":"IF(LEN('Translation-EN'!A1906)>0,'Translation-EN'!A1906,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1906)>0,'Translation-EN'!B1906,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1906)>0,'Translation-EN'!C1906,\"\")","v":"D210"},{"$f":"IF(LEN('Translation-EN'!D1906)>0,'Translation-EN'!D1906,\"\")","v":""},{"$f":"$E$1882","v":"Acier de construction laminé à chaud"}]
[{"$f":"IF(LEN('Translation-EN'!A1907)>0,'Translation-EN'!A1907,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1907)>0,'Translation-EN'!B1907,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1907)>0,'Translation-EN'!C1907,\"\")","v":"E210"},{"$f":"IF(LEN('Translation-EN'!D1907)>0,'Translation-EN'!D1907,\"\")","v":""},"W250x39 (W10x26)"]
[{"$f":"IF(LEN('Translation-EN'!A1908)>0,'Translation-EN'!A1908,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1908)>0,'Translation-EN'!B1908,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1908)>0,'Translation-EN'!C1908,\"\")","v":"B211"},{"$f":"IF(LEN('Translation-EN'!D1908)>0,'Translation-EN'!D1908,\"\")","v":""},{"$f":"$E$1880","v":"Poutre en acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1909)>0,'Translation-EN'!A1909,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1909)>0,'Translation-EN'!B1909,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1909)>0,'Translation-EN'!C1909,\"\")","v":"C211"},{"$f":"IF(LEN('Translation-EN'!D1909)>0,'Translation-EN'!D1909,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1881","v":"Institut américain de la construction métallique"}]
[{"$f":"IF(LEN('Translation-EN'!A1910)>0,'Translation-EN'!A1910,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1910)>0,'Translation-EN'!B1910,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1910)>0,'Translation-EN'!C1910,\"\")","v":"D211"},{"$f":"IF(LEN('Translation-EN'!D1910)>0,'Translation-EN'!D1910,\"\")","v":""},{"$f":"$E$1882","v":"Acier de construction laminé à chaud"}]
[{"$f":"IF(LEN('Translation-EN'!A1911)>0,'Translation-EN'!A1911,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1911)>0,'Translation-EN'!B1911,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1911)>0,'Translation-EN'!C1911,\"\")","v":"E211"},{"$f":"IF(LEN('Translation-EN'!D1911)>0,'Translation-EN'!D1911,\"\")","v":""},"W310x33 (W12x22)"]
[{"$f":"IF(LEN('Translation-EN'!A1912)>0,'Translation-EN'!A1912,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1912)>0,'Translation-EN'!B1912,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1912)>0,'Translation-EN'!C1912,\"\")","v":"B212"},{"$f":"IF(LEN('Translation-EN'!D1912)>0,'Translation-EN'!D1912,\"\")","v":""},{"$f":"$E$1880","v":"Poutre en acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1913)>0,'Translation-EN'!A1913,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1913)>0,'Translation-EN'!B1913,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1913)>0,'Translation-EN'!C1913,\"\")","v":"C212"},{"$f":"IF(LEN('Translation-EN'!D1913)>0,'Translation-EN'!D1913,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1881","v":"Institut américain de la construction métallique"}]
[{"$f":"IF(LEN('Translation-EN'!A1914)>0,'Translation-EN'!A1914,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1914)>0,'Translation-EN'!B1914,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1914)>0,'Translation-EN'!C1914,\"\")","v":"D212"},{"$f":"IF(LEN('Translation-EN'!D1914)>0,'Translation-EN'!D1914,\"\")","v":""},{"$f":"$E$1882","v":"Acier de construction laminé à chaud"}]
[{"$f":"IF(LEN('Translation-EN'!A1915)>0,'Translation-EN'!A1915,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1915)>0,'Translation-EN'!B1915,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1915)>0,'Translation-EN'!C1915,\"\")","v":"E212"},{"$f":"IF(LEN('Translation-EN'!D1915)>0,'Translation-EN'!D1915,\"\")","v":""},"W310x39 (W12x26)"]
[{"$f":"IF(LEN('Translation-EN'!A1916)>0,'Translation-EN'!A1916,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1916)>0,'Translation-EN'!B1916,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1916)>0,'Translation-EN'!C1916,\"\")","v":"B213"},{"$f":"IF(LEN('Translation-EN'!D1916)>0,'Translation-EN'!D1916,\"\")","v":""},"Poutrelle en acier, âme ouverte"]
[{"$f":"IF(LEN('Translation-EN'!A1917)>0,'Translation-EN'!A1917,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1917)>0,'Translation-EN'!B1917,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1917)>0,'Translation-EN'!C1917,\"\")","v":"C213"},{"$f":"IF(LEN('Translation-EN'!D1917)>0,'Translation-EN'!D1917,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Institut de la poutrelle en acier"]
[{"$f":"IF(LEN('Translation-EN'!A1918)>0,'Translation-EN'!A1918,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1918)>0,'Translation-EN'!B1918,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1918)>0,'Translation-EN'!C1918,\"\")","v":"E213"},{"$f":"IF(LEN('Translation-EN'!D1918)>0,'Translation-EN'!D1918,\"\")","v":""},"Poutrelle 12 po 12K3 "]
[{"$f":"IF(LEN('Translation-EN'!A1919)>0,'Translation-EN'!A1919,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1919)>0,'Translation-EN'!B1919,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1919)>0,'Translation-EN'!C1919,\"\")","v":"B214"},{"$f":"IF(LEN('Translation-EN'!D1919)>0,'Translation-EN'!D1919,\"\")","v":""},"Poteau en acier"]
[{"$f":"IF(LEN('Translation-EN'!A1920)>0,'Translation-EN'!A1920,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1920)>0,'Translation-EN'!B1920,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1920)>0,'Translation-EN'!C1920,\"\")","v":"C214"},{"$f":"IF(LEN('Translation-EN'!D1920)>0,'Translation-EN'!D1920,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1648","v":"Générique"}]
[{"$f":"IF(LEN('Translation-EN'!A1921)>0,'Translation-EN'!A1921,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1921)>0,'Translation-EN'!B1921,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1921)>0,'Translation-EN'!C1921,\"\")","v":"E214"},{"$f":"IF(LEN('Translation-EN'!D1921)>0,'Translation-EN'!D1921,\"\")","v":""},"3,5 x 0,216 po (89 x 5,5 mm), Sched 40 STD"]
[{"$f":"IF(LEN('Translation-EN'!A1922)>0,'Translation-EN'!A1922,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1922)>0,'Translation-EN'!B1922,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1922)>0,'Translation-EN'!C1922,\"\")","v":"B215"},{"$f":"IF(LEN('Translation-EN'!D1922)>0,'Translation-EN'!D1922,\"\")","v":""},"Plots en acier – porteurs"]
[{"$f":"IF(LEN('Translation-EN'!A1923)>0,'Translation-EN'!A1923,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1923)>0,'Translation-EN'!B1923,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1923)>0,'Translation-EN'!C1923,\"\")","v":"C215"},{"$f":"IF(LEN('Translation-EN'!D1923)>0,'Translation-EN'!D1923,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"ClarkDietrich"]
[{"$f":"IF(LEN('Translation-EN'!A1924)>0,'Translation-EN'!A1924,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1924)>0,'Translation-EN'!B1924,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1924)>0,'Translation-EN'!C1924,\"\")","v":"E215"},{"$f":"IF(LEN('Translation-EN'!D1924)>0,'Translation-EN'!D1924,\"\")","v":""},"600-S-137-54, 16 jauge"]
[{"$f":"IF(LEN('Translation-EN'!A1925)>0,'Translation-EN'!A1925,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1925)>0,'Translation-EN'!B1925,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1925)>0,'Translation-EN'!C1925,\"\")","v":"B217"},{"$f":"IF(LEN('Translation-EN'!D1925)>0,'Translation-EN'!D1925,\"\")","v":""},{"$f":"$E$1922","v":"Plots en acier – porteurs"}]
[{"$f":"IF(LEN('Translation-EN'!A1926)>0,'Translation-EN'!A1926,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1926)>0,'Translation-EN'!B1926,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1926)>0,'Translation-EN'!C1926,\"\")","v":"C217"},{"$f":"IF(LEN('Translation-EN'!D1926)>0,'Translation-EN'!D1926,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"MarinoWARE"]
[{"$f":"IF(LEN('Translation-EN'!A1927)>0,'Translation-EN'!A1927,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1927)>0,'Translation-EN'!B1927,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1927)>0,'Translation-EN'!C1927,\"\")","v":"D217"},{"$f":"IF(LEN('Translation-EN'!D1927)>0,'Translation-EN'!D1927,\"\")","v":""},"Poteaux et rails structurels"]
[{"$f":"IF(LEN('Translation-EN'!A1928)>0,'Translation-EN'!A1928,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1928)>0,'Translation-EN'!B1928,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1928)>0,'Translation-EN'!C1928,\"\")","v":"E217"},{"$f":"IF(LEN('Translation-EN'!D1928)>0,'Translation-EN'!D1928,\"\")","v":""},"600-S-137-54, 16 gauge, \"2x6\""]
[{"$f":"IF(LEN('Translation-EN'!A1929)>0,'Translation-EN'!A1929,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1929)>0,'Translation-EN'!B1929,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1929)>0,'Translation-EN'!C1929,\"\")","v":"B219"},{"$f":"IF(LEN('Translation-EN'!D1929)>0,'Translation-EN'!D1929,\"\")","v":""},{"$f":"$E$1922","v":"Plots en acier – porteurs"}]
[{"$f":"IF(LEN('Translation-EN'!A1930)>0,'Translation-EN'!A1930,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1930)>0,'Translation-EN'!B1930,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1930)>0,'Translation-EN'!C1930,\"\")","v":"C219"},{"$f":"IF(LEN('Translation-EN'!D1930)>0,'Translation-EN'!D1930,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"MBA Building Supplies"]
[{"$f":"IF(LEN('Translation-EN'!A1931)>0,'Translation-EN'!A1931,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1931)>0,'Translation-EN'!B1931,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1931)>0,'Translation-EN'!C1931,\"\")","v":"E219"},{"$f":"IF(LEN('Translation-EN'!D1931)>0,'Translation-EN'!D1931,\"\")","v":""},{"$f":"$E$1924","v":"600-S-137-54, 16 jauge"}]
[{"$f":"IF(LEN('Translation-EN'!A1932)>0,'Translation-EN'!A1932,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1932)>0,'Translation-EN'!B1932,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1932)>0,'Translation-EN'!C1932,\"\")","v":"B220"},{"$f":"IF(LEN('Translation-EN'!D1932)>0,'Translation-EN'!D1932,\"\")","v":""},{"$f":"$E$1922","v":"Plots en acier – porteurs"}]
[{"$f":"IF(LEN('Translation-EN'!A1933)>0,'Translation-EN'!A1933,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1933)>0,'Translation-EN'!B1933,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1933)>0,'Translation-EN'!C1933,\"\")","v":"C220"},{"$f":"IF(LEN('Translation-EN'!D1933)>0,'Translation-EN'!D1933,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Scafco"]
[{"$f":"IF(LEN('Translation-EN'!A1934)>0,'Translation-EN'!A1934,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1934)>0,'Translation-EN'!B1934,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1934)>0,'Translation-EN'!C1934,\"\")","v":"E220"},{"$f":"IF(LEN('Translation-EN'!D1934)>0,'Translation-EN'!D1934,\"\")","v":""},{"$f":"$E$1924","v":"600-S-137-54, 16 jauge"}]
[{"$f":"IF(LEN('Translation-EN'!A1935)>0,'Translation-EN'!A1935,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1935)>0,'Translation-EN'!B1935,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1935)>0,'Translation-EN'!C1935,\"\")","v":"B221"},{"$f":"IF(LEN('Translation-EN'!D1935)>0,'Translation-EN'!D1935,\"\")","v":""},{"$f":"$E$1922","v":"Plots en acier – porteurs"}]
[{"$f":"IF(LEN('Translation-EN'!A1936)>0,'Translation-EN'!A1936,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1936)>0,'Translation-EN'!B1936,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1936)>0,'Translation-EN'!C1936,\"\")","v":"C221"},{"$f":"IF(LEN('Translation-EN'!D1936)>0,'Translation-EN'!D1936,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Institut du recyclage de l’acier"]
[{"$f":"IF(LEN('Translation-EN'!A1937)>0,'Translation-EN'!A1937,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1937)>0,'Translation-EN'!B1937,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1937)>0,'Translation-EN'!C1937,\"\")","v":"E221"},{"$f":"IF(LEN('Translation-EN'!D1937)>0,'Translation-EN'!D1937,\"\")","v":""},{"$f":"$E$1924","v":"600-S-137-54, 16 jauge"}]
[{"$f":"IF(LEN('Translation-EN'!A1938)>0,'Translation-EN'!A1938,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1938)>0,'Translation-EN'!B1938,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1938)>0,'Translation-EN'!C1938,\"\")","v":"B222"},{"$f":"IF(LEN('Translation-EN'!D1938)>0,'Translation-EN'!D1938,\"\")","v":""},"Goujons en acier – Non porteurs"]
[{"$f":"IF(LEN('Translation-EN'!A1939)>0,'Translation-EN'!A1939,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1939)>0,'Translation-EN'!B1939,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1939)>0,'Translation-EN'!C1939,\"\")","v":"C222"},{"$f":"IF(LEN('Translation-EN'!D1939)>0,'Translation-EN'!D1939,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1923","v":"ClarkDietrich"}]
[{"$f":"IF(LEN('Translation-EN'!A1940)>0,'Translation-EN'!A1940,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1940)>0,'Translation-EN'!B1940,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1940)>0,'Translation-EN'!C1940,\"\")","v":"E222"},{"$f":"IF(LEN('Translation-EN'!D1940)>0,'Translation-EN'!D1940,\"\")","v":""},"362-S-125-18, 20EQ gauge, \"2x4\""]
[{"$f":"IF(LEN('Translation-EN'!A1941)>0,'Translation-EN'!A1941,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1941)>0,'Translation-EN'!B1941,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1941)>0,'Translation-EN'!C1941,\"\")","v":"B224"},{"$f":"IF(LEN('Translation-EN'!D1941)>0,'Translation-EN'!D1941,\"\")","v":""},{"$f":"$E$1938","v":"Goujons en acier – Non porteurs"}]
[{"$f":"IF(LEN('Translation-EN'!A1942)>0,'Translation-EN'!A1942,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1942)>0,'Translation-EN'!B1942,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1942)>0,'Translation-EN'!C1942,\"\")","v":"C224"},{"$f":"IF(LEN('Translation-EN'!D1942)>0,'Translation-EN'!D1942,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1926","v":"MarinoWARE"}]
[{"$f":"IF(LEN('Translation-EN'!A1943)>0,'Translation-EN'!A1943,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1943)>0,'Translation-EN'!B1943,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1943)>0,'Translation-EN'!C1943,\"\")","v":"D224"},{"$f":"IF(LEN('Translation-EN'!D1943)>0,'Translation-EN'!D1943,\"\")","v":""},"Viper Stud Viper 20"]
[{"$f":"IF(LEN('Translation-EN'!A1944)>0,'Translation-EN'!A1944,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1944)>0,'Translation-EN'!B1944,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1944)>0,'Translation-EN'!C1944,\"\")","v":"E224"},{"$f":"IF(LEN('Translation-EN'!D1944)>0,'Translation-EN'!D1944,\"\")","v":""},{"$f":"$E$1940","v":"362-S-125-18, 20EQ gauge, \"2x4\""}]
[{"$f":"IF(LEN('Translation-EN'!A1945)>0,'Translation-EN'!A1945,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1945)>0,'Translation-EN'!B1945,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1945)>0,'Translation-EN'!C1945,\"\")","v":"B226"},{"$f":"IF(LEN('Translation-EN'!D1945)>0,'Translation-EN'!D1945,\"\")","v":""},{"$f":"$E$1938","v":"Goujons en acier – Non porteurs"}]
[{"$f":"IF(LEN('Translation-EN'!A1946)>0,'Translation-EN'!A1946,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1946)>0,'Translation-EN'!B1946,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1946)>0,'Translation-EN'!C1946,\"\")","v":"C226"},{"$f":"IF(LEN('Translation-EN'!D1946)>0,'Translation-EN'!D1946,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1930","v":"MBA Building Supplies"}]
[{"$f":"IF(LEN('Translation-EN'!A1947)>0,'Translation-EN'!A1947,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1947)>0,'Translation-EN'!B1947,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1947)>0,'Translation-EN'!C1947,\"\")","v":"E226"},{"$f":"IF(LEN('Translation-EN'!D1947)>0,'Translation-EN'!D1947,\"\")","v":""},"362-S-125-18, 20EQ jauge, ProSTUD, ProTRAK"]
[{"$f":"IF(LEN('Translation-EN'!A1948)>0,'Translation-EN'!A1948,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1948)>0,'Translation-EN'!B1948,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1948)>0,'Translation-EN'!C1948,\"\")","v":"B227"},{"$f":"IF(LEN('Translation-EN'!D1948)>0,'Translation-EN'!D1948,\"\")","v":""},{"$f":"$E$1938","v":"Goujons en acier – Non porteurs"}]
[{"$f":"IF(LEN('Translation-EN'!A1949)>0,'Translation-EN'!A1949,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1949)>0,'Translation-EN'!B1949,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1949)>0,'Translation-EN'!C1949,\"\")","v":"C227"},{"$f":"IF(LEN('Translation-EN'!D1949)>0,'Translation-EN'!D1949,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1933","v":"Scafco"}]
[{"$f":"IF(LEN('Translation-EN'!A1950)>0,'Translation-EN'!A1950,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1950)>0,'Translation-EN'!B1950,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1950)>0,'Translation-EN'!C1950,\"\")","v":"E227"},{"$f":"IF(LEN('Translation-EN'!D1950)>0,'Translation-EN'!D1950,\"\")","v":""},"362VS125-18, 20EQ jauge"]
[{"$f":"IF(LEN('Translation-EN'!A1951)>0,'Translation-EN'!A1951,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1951)>0,'Translation-EN'!B1951,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1951)>0,'Translation-EN'!C1951,\"\")","v":"B228"},{"$f":"IF(LEN('Translation-EN'!D1951)>0,'Translation-EN'!D1951,\"\")","v":""},{"$f":"$E$1938","v":"Goujons en acier – Non porteurs"}]
[{"$f":"IF(LEN('Translation-EN'!A1952)>0,'Translation-EN'!A1952,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1952)>0,'Translation-EN'!B1952,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1952)>0,'Translation-EN'!C1952,\"\")","v":"C228"},{"$f":"IF(LEN('Translation-EN'!D1952)>0,'Translation-EN'!D1952,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1936","v":"Institut du recyclage de l’acier"}]
[{"$f":"IF(LEN('Translation-EN'!A1953)>0,'Translation-EN'!A1953,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1953)>0,'Translation-EN'!B1953,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1953)>0,'Translation-EN'!C1953,\"\")","v":"E228"},{"$f":"IF(LEN('Translation-EN'!D1953)>0,'Translation-EN'!D1953,\"\")","v":""},{"$f":"$E$1940","v":"362-S-125-18, 20EQ gauge, \"2x4\""}]
[{"$f":"IF(LEN('Translation-EN'!A1954)>0,'Translation-EN'!A1954,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1954)>0,'Translation-EN'!B1954,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1954)>0,'Translation-EN'!C1954,\"\")","v":"B229"},{"$f":"IF(LEN('Translation-EN'!D1954)>0,'Translation-EN'!D1954,\"\")","v":""},"Balle de paille"]
[{"$f":"IF(LEN('Translation-EN'!A1955)>0,'Translation-EN'!A1955,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1955)>0,'Translation-EN'!B1955,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1955)>0,'Translation-EN'!C1955,\"\")","v":"D229"},{"$f":"IF(LEN('Translation-EN'!D1955)>0,'Translation-EN'!D1955,\"\")","v":""},"Paille de blé et de seigle"]
[{"$f":"IF(LEN('Translation-EN'!A1956)>0,'Translation-EN'!A1956,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1956)>0,'Translation-EN'!B1956,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1956)>0,'Translation-EN'!C1956,\"\")","v":"E229"},{"$f":"IF(LEN('Translation-EN'!D1956)>0,'Translation-EN'!D1956,\"\")","v":""},"R 3,3/po"]
[{"$f":"IF(LEN('Translation-EN'!A1957)>0,'Translation-EN'!A1957,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1957)>0,'Translation-EN'!B1957,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1957)>0,'Translation-EN'!C1957,\"\")","v":"B230"},{"$f":"IF(LEN('Translation-EN'!D1957)>0,'Translation-EN'!D1957,\"\")","v":""},"Panneaux de paille"]
[{"$f":"IF(LEN('Translation-EN'!A1958)>0,'Translation-EN'!A1958,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1958)>0,'Translation-EN'!B1958,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1958)>0,'Translation-EN'!C1958,\"\")","v":"C230"},{"$f":"IF(LEN('Translation-EN'!D1958)>0,'Translation-EN'!D1958,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"EcoCocon"]
[{"$f":"IF(LEN('Translation-EN'!A1959)>0,'Translation-EN'!A1959,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1959)>0,'Translation-EN'!B1959,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1959)>0,'Translation-EN'!C1959,\"\")","v":"E230"},{"$f":"IF(LEN('Translation-EN'!D1959)>0,'Translation-EN'!D1959,\"\")","v":""},"R 2,9/po"]
[{"$f":"IF(LEN('Translation-EN'!A1960)>0,'Translation-EN'!A1960,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1960)>0,'Translation-EN'!B1960,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1960)>0,'Translation-EN'!C1960,\"\")","v":"B231"},{"$f":"IF(LEN('Translation-EN'!D1960)>0,'Translation-EN'!D1960,\"\")","v":""},"Finition acrylique stucco texturée"]
[{"$f":"IF(LEN('Translation-EN'!A1961)>0,'Translation-EN'!A1961,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1961)>0,'Translation-EN'!B1961,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1961)>0,'Translation-EN'!C1961,\"\")","v":"C231"},{"$f":"IF(LEN('Translation-EN'!D1961)>0,'Translation-EN'!D1961,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Sto"]
[{"$f":"IF(LEN('Translation-EN'!A1962)>0,'Translation-EN'!A1962,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1962)>0,'Translation-EN'!B1962,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1962)>0,'Translation-EN'!C1962,\"\")","v":"D231"},{"$f":"IF(LEN('Translation-EN'!D1962)>0,'Translation-EN'!D1962,\"\")","v":""},"Stolit 1,0, Stolit 1,5, Stolit Freeform"]
[{"$f":"IF(LEN('Translation-EN'!A1963)>0,'Translation-EN'!A1963,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1963)>0,'Translation-EN'!B1963,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1963)>0,'Translation-EN'!C1963,\"\")","v":"B232"},{"$f":"IF(LEN('Translation-EN'!D1963)>0,'Translation-EN'!D1963,\"\")","v":""},"Membrane de toiture TPO"]
[{"$f":"IF(LEN('Translation-EN'!A1964)>0,'Translation-EN'!A1964,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1964)>0,'Translation-EN'!B1964,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1964)>0,'Translation-EN'!C1964,\"\")","v":"C232"},{"$f":"IF(LEN('Translation-EN'!D1964)>0,'Translation-EN'!D1964,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1796","v":"Carlisle"}]
[{"$f":"IF(LEN('Translation-EN'!A1965)>0,'Translation-EN'!A1965,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1965)>0,'Translation-EN'!B1965,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1965)>0,'Translation-EN'!C1965,\"\")","v":"E232"},{"$f":"IF(LEN('Translation-EN'!D1965)>0,'Translation-EN'!D1965,\"\")","v":""},"60 mils"]
[{"$f":"IF(LEN('Translation-EN'!A1966)>0,'Translation-EN'!A1966,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1966)>0,'Translation-EN'!B1966,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1966)>0,'Translation-EN'!C1966,\"\")","v":"B233"},{"$f":"IF(LEN('Translation-EN'!D1966)>0,'Translation-EN'!D1966,\"\")","v":""},"Panneau à isolation sous vide"]
[{"$f":"IF(LEN('Translation-EN'!A1967)>0,'Translation-EN'!A1967,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1967)>0,'Translation-EN'!B1967,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1967)>0,'Translation-EN'!C1967,\"\")","v":"C233"},{"$f":"IF(LEN('Translation-EN'!D1967)>0,'Translation-EN'!D1967,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Porextherm"]
[{"$f":"IF(LEN('Translation-EN'!A1968)>0,'Translation-EN'!A1968,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1968)>0,'Translation-EN'!B1968,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1968)>0,'Translation-EN'!C1968,\"\")","v":"D233"},{"$f":"IF(LEN('Translation-EN'!D1968)>0,'Translation-EN'!D1968,\"\")","v":""},"Vacupor"]
[{"$f":"IF(LEN('Translation-EN'!A1969)>0,'Translation-EN'!A1969,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1969)>0,'Translation-EN'!B1969,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1969)>0,'Translation-EN'!C1969,\"\")","v":"E233"},{"$f":"IF(LEN('Translation-EN'!D1969)>0,'Translation-EN'!D1969,\"\")","v":""},"R 30/po"]
[{"$f":"IF(LEN('Translation-EN'!A1970)>0,'Translation-EN'!A1970,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1970)>0,'Translation-EN'!B1970,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1970)>0,'Translation-EN'!C1970,\"\")","v":"B234"},{"$f":"IF(LEN('Translation-EN'!D1970)>0,'Translation-EN'!D1970,\"\")","v":""},"Revêtement de plancher en vinyle"]
[{"$f":"IF(LEN('Translation-EN'!A1971)>0,'Translation-EN'!A1971,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1971)>0,'Translation-EN'!B1971,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1971)>0,'Translation-EN'!C1971,\"\")","v":"C234"},{"$f":"IF(LEN('Translation-EN'!D1971)>0,'Translation-EN'!D1971,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Altro"]
[{"$f":"IF(LEN('Translation-EN'!A1972)>0,'Translation-EN'!A1972,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1972)>0,'Translation-EN'!B1972,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1972)>0,'Translation-EN'!C1972,\"\")","v":"D234"},{"$f":"IF(LEN('Translation-EN'!D1972)>0,'Translation-EN'!D1972,\"\")","v":""},"Altro Lavencia Click"]
[{"$f":"IF(LEN('Translation-EN'!A1973)>0,'Translation-EN'!A1973,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1973)>0,'Translation-EN'!B1973,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1973)>0,'Translation-EN'!C1973,\"\")","v":"B235"},{"$f":"IF(LEN('Translation-EN'!D1973)>0,'Translation-EN'!D1973,\"\")","v":""},{"$f":"$E$1970","v":"Revêtement de plancher en vinyle"}]
[{"$f":"IF(LEN('Translation-EN'!A1974)>0,'Translation-EN'!A1974,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1974)>0,'Translation-EN'!B1974,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1974)>0,'Translation-EN'!C1974,\"\")","v":"C235"},{"$f":"IF(LEN('Translation-EN'!D1974)>0,'Translation-EN'!D1974,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1971","v":"Altro"}]
[{"$f":"IF(LEN('Translation-EN'!A1975)>0,'Translation-EN'!A1975,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1975)>0,'Translation-EN'!B1975,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1975)>0,'Translation-EN'!C1975,\"\")","v":"D235"},{"$f":"IF(LEN('Translation-EN'!D1975)>0,'Translation-EN'!D1975,\"\")","v":""},"Altro Lavencia Plus"]
[{"$f":"IF(LEN('Translation-EN'!A1976)>0,'Translation-EN'!A1976,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1976)>0,'Translation-EN'!B1976,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1976)>0,'Translation-EN'!C1976,\"\")","v":"B236"},{"$f":"IF(LEN('Translation-EN'!D1976)>0,'Translation-EN'!D1976,\"\")","v":""},{"$f":"$E$1970","v":"Revêtement de plancher en vinyle"}]
[{"$f":"IF(LEN('Translation-EN'!A1977)>0,'Translation-EN'!A1977,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1977)>0,'Translation-EN'!B1977,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1977)>0,'Translation-EN'!C1977,\"\")","v":"C236"},{"$f":"IF(LEN('Translation-EN'!D1977)>0,'Translation-EN'!D1977,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1697","v":"Gerflor "}]
[{"$f":"IF(LEN('Translation-EN'!A1978)>0,'Translation-EN'!A1978,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1978)>0,'Translation-EN'!B1978,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1978)>0,'Translation-EN'!C1978,\"\")","v":"D236"},{"$f":"IF(LEN('Translation-EN'!D1978)>0,'Translation-EN'!D1978,\"\")","v":""},"Creation 70 CLIC"]
[{"$f":"IF(LEN('Translation-EN'!A1979)>0,'Translation-EN'!A1979,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1979)>0,'Translation-EN'!B1979,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1979)>0,'Translation-EN'!C1979,\"\")","v":"B237"},{"$f":"IF(LEN('Translation-EN'!D1979)>0,'Translation-EN'!D1979,\"\")","v":""},{"$f":"$E$1970","v":"Revêtement de plancher en vinyle"}]
[{"$f":"IF(LEN('Translation-EN'!A1980)>0,'Translation-EN'!A1980,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1980)>0,'Translation-EN'!B1980,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1980)>0,'Translation-EN'!C1980,\"\")","v":"C237"},{"$f":"IF(LEN('Translation-EN'!D1980)>0,'Translation-EN'!D1980,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1851","v":"Institut des revêtements de sol résilients"}]
[{"$f":"IF(LEN('Translation-EN'!A1981)>0,'Translation-EN'!A1981,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1981)>0,'Translation-EN'!B1981,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1981)>0,'Translation-EN'!C1981,\"\")","v":"D237"},{"$f":"IF(LEN('Translation-EN'!D1981)>0,'Translation-EN'!D1981,\"\")","v":""},"Comprend les produits de carrelage d’Armstrong, Congoleum, Tarkett."]
[{"$f":"IF(LEN('Translation-EN'!A1982)>0,'Translation-EN'!A1982,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1982)>0,'Translation-EN'!B1982,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1982)>0,'Translation-EN'!C1982,\"\")","v":"B238"},{"$f":"IF(LEN('Translation-EN'!D1982)>0,'Translation-EN'!D1982,\"\")","v":""},"Revêtement en vinyle"]
[{"$f":"IF(LEN('Translation-EN'!A1983)>0,'Translation-EN'!A1983,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1983)>0,'Translation-EN'!B1983,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1983)>0,'Translation-EN'!C1983,\"\")","v":"C238"},{"$f":"IF(LEN('Translation-EN'!D1983)>0,'Translation-EN'!D1983,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1828","v":"Institut de revêtement en vinyle"}]
[{"$f":"IF(LEN('Translation-EN'!A1984)>0,'Translation-EN'!A1984,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1984)>0,'Translation-EN'!B1984,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1984)>0,'Translation-EN'!C1984,\"\")","v":"D238"},{"$f":"IF(LEN('Translation-EN'!D1984)>0,'Translation-EN'!D1984,\"\")","v":""},"Produits Double 4,5 po de : American Original, Associated Materials, CertainTeed, Novik, Ply Gem"]
[{"$f":"IF(LEN('Translation-EN'!A1985)>0,'Translation-EN'!A1985,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1985)>0,'Translation-EN'!B1985,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1985)>0,'Translation-EN'!C1985,\"\")","v":"E238"},{"$f":"IF(LEN('Translation-EN'!D1985)>0,'Translation-EN'!D1985,\"\")","v":""},"0,040 po Double 4,5 po"]
[{"$f":"IF(LEN('Translation-EN'!A1986)>0,'Translation-EN'!A1986,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1986)>0,'Translation-EN'!B1986,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1986)>0,'Translation-EN'!C1986,\"\")","v":"B240"},{"$f":"IF(LEN('Translation-EN'!D1986)>0,'Translation-EN'!D1986,\"\")","v":""},"Adhésif pour membrane d’étanchéité"]
[{"$f":"IF(LEN('Translation-EN'!A1987)>0,'Translation-EN'!A1987,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1987)>0,'Translation-EN'!B1987,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1987)>0,'Translation-EN'!C1987,\"\")","v":"C240"},{"$f":"IF(LEN('Translation-EN'!D1987)>0,'Translation-EN'!D1987,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1278","v":"GCP"}]
[{"$f":"IF(LEN('Translation-EN'!A1988)>0,'Translation-EN'!A1988,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1988)>0,'Translation-EN'!B1988,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1988)>0,'Translation-EN'!C1988,\"\")","v":"D240"},{"$f":"IF(LEN('Translation-EN'!D1988)>0,'Translation-EN'!D1988,\"\")","v":""},"Bituthene"]
[{"$f":"IF(LEN('Translation-EN'!A1989)>0,'Translation-EN'!A1989,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1989)>0,'Translation-EN'!B1989,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1989)>0,'Translation-EN'!C1989,\"\")","v":"B241"},{"$f":"IF(LEN('Translation-EN'!D1989)>0,'Translation-EN'!D1989,\"\")","v":""},"Grillage soudé"]
[{"$f":"IF(LEN('Translation-EN'!A1990)>0,'Translation-EN'!A1990,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1990)>0,'Translation-EN'!B1990,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1990)>0,'Translation-EN'!C1990,\"\")","v":"C241"},{"$f":"IF(LEN('Translation-EN'!D1990)>0,'Translation-EN'!D1990,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Serfas"]
[{"$f":"IF(LEN('Translation-EN'!A1991)>0,'Translation-EN'!A1991,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1991)>0,'Translation-EN'!B1991,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1991)>0,'Translation-EN'!C1991,\"\")","v":"E241"},{"$f":"IF(LEN('Translation-EN'!D1991)>0,'Translation-EN'!D1991,\"\")","v":""},"6 po x 6 po x 6/6 g"]
[{"$f":"IF(LEN('Translation-EN'!A1992)>0,'Translation-EN'!A1992,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1992)>0,'Translation-EN'!B1992,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1992)>0,'Translation-EN'!C1992,\"\")","v":"B242"},{"$f":"IF(LEN('Translation-EN'!D1992)>0,'Translation-EN'!D1992,\"\")","v":""},"Fenêtre – sous-fenêtre double"]
[{"$f":"IF(LEN('Translation-EN'!A1993)>0,'Translation-EN'!A1993,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1993)>0,'Translation-EN'!B1993,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1993)>0,'Translation-EN'!C1993,\"\")","v":"E242"},{"$f":"IF(LEN('Translation-EN'!D1993)>0,'Translation-EN'!D1993,\"\")","v":""},"Cadre en fibre de verre"]
[{"$f":"IF(LEN('Translation-EN'!A1994)>0,'Translation-EN'!A1994,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1994)>0,'Translation-EN'!B1994,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1994)>0,'Translation-EN'!C1994,\"\")","v":"B243"},{"$f":"IF(LEN('Translation-EN'!D1994)>0,'Translation-EN'!D1994,\"\")","v":""},{"$f":"$E$1992","v":"Fenêtre – sous-fenêtre double"}]
[{"$f":"IF(LEN('Translation-EN'!A1995)>0,'Translation-EN'!A1995,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B1995)>0,'Translation-EN'!B1995,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1995)>0,'Translation-EN'!C1995,\"\")","v":"C243"},{"$f":"IF(LEN('Translation-EN'!D1995)>0,'Translation-EN'!D1995,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Andersen"]
[{"$f":"IF(LEN('Translation-EN'!A1996)>0,'Translation-EN'!A1996,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1996)>0,'Translation-EN'!B1996,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1996)>0,'Translation-EN'!C1996,\"\")","v":"D243"},{"$f":"IF(LEN('Translation-EN'!D1996)>0,'Translation-EN'!D1996,\"\")","v":""},"Fibrex"]
[{"$f":"IF(LEN('Translation-EN'!A1997)>0,'Translation-EN'!A1997,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1997)>0,'Translation-EN'!B1997,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1997)>0,'Translation-EN'!C1997,\"\")","v":"E243"},{"$f":"IF(LEN('Translation-EN'!D1997)>0,'Translation-EN'!D1997,\"\")","v":""},"PVC et bois composite"]
[{"$f":"IF(LEN('Translation-EN'!A1998)>0,'Translation-EN'!A1998,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1998)>0,'Translation-EN'!B1998,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1998)>0,'Translation-EN'!C1998,\"\")","v":"B244"},{"$f":"IF(LEN('Translation-EN'!D1998)>0,'Translation-EN'!D1998,\"\")","v":""},{"$f":"$E$1992","v":"Fenêtre – sous-fenêtre double"}]
[{"$f":"IF(LEN('Translation-EN'!A1999)>0,'Translation-EN'!A1999,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B1999)>0,'Translation-EN'!B1999,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C1999)>0,'Translation-EN'!C1999,\"\")","v":"E244"},{"$f":"IF(LEN('Translation-EN'!D1999)>0,'Translation-EN'!D1999,\"\")","v":""},"Charpente en vinyle"]
[{"$f":"IF(LEN('Translation-EN'!A2000)>0,'Translation-EN'!A2000,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2000)>0,'Translation-EN'!B2000,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2000)>0,'Translation-EN'!C2000,\"\")","v":"B245"},{"$f":"IF(LEN('Translation-EN'!D2000)>0,'Translation-EN'!D2000,\"\")","v":""},{"$f":"$E$1992","v":"Fenêtre – sous-fenêtre double"}]
[{"$f":"IF(LEN('Translation-EN'!A2001)>0,'Translation-EN'!A2001,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2001)>0,'Translation-EN'!B2001,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2001)>0,'Translation-EN'!C2001,\"\")","v":"E245"},{"$f":"IF(LEN('Translation-EN'!D2001)>0,'Translation-EN'!D2001,\"\")","v":""},"Charpente en bois"]
[{"$f":"IF(LEN('Translation-EN'!A2002)>0,'Translation-EN'!A2002,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2002)>0,'Translation-EN'!B2002,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2002)>0,'Translation-EN'!C2002,\"\")","v":"B246"},{"$f":"IF(LEN('Translation-EN'!D2002)>0,'Translation-EN'!D2002,\"\")","v":""},{"$f":"$E$1992","v":"Fenêtre – sous-fenêtre double"}]
[{"$f":"IF(LEN('Translation-EN'!A2003)>0,'Translation-EN'!A2003,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2003)>0,'Translation-EN'!B2003,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2003)>0,'Translation-EN'!C2003,\"\")","v":"E246"},{"$f":"IF(LEN('Translation-EN'!D2003)>0,'Translation-EN'!D2003,\"\")","v":""},{"$f":"$E$2001","v":"Charpente en bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2004)>0,'Translation-EN'!A2004,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2004)>0,'Translation-EN'!B2004,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2004)>0,'Translation-EN'!C2004,\"\")","v":"B247"},{"$f":"IF(LEN('Translation-EN'!D2004)>0,'Translation-EN'!D2004,\"\")","v":""},{"$f":"$E$1992","v":"Fenêtre – sous-fenêtre double"}]
[{"$f":"IF(LEN('Translation-EN'!A2005)>0,'Translation-EN'!A2005,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2005)>0,'Translation-EN'!B2005,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2005)>0,'Translation-EN'!C2005,\"\")","v":"E247"},{"$f":"IF(LEN('Translation-EN'!D2005)>0,'Translation-EN'!D2005,\"\")","v":""},"Charpente en bois, revêtement en aluminium"]
[{"$f":"IF(LEN('Translation-EN'!A2006)>0,'Translation-EN'!A2006,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2006)>0,'Translation-EN'!B2006,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2006)>0,'Translation-EN'!C2006,\"\")","v":"B248"},{"$f":"IF(LEN('Translation-EN'!D2006)>0,'Translation-EN'!D2006,\"\")","v":""},{"$f":"$E$1992","v":"Fenêtre – sous-fenêtre double"}]
[{"$f":"IF(LEN('Translation-EN'!A2007)>0,'Translation-EN'!A2007,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2007)>0,'Translation-EN'!B2007,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2007)>0,'Translation-EN'!C2007,\"\")","v":"E248"},{"$f":"IF(LEN('Translation-EN'!D2007)>0,'Translation-EN'!D2007,\"\")","v":""},{"$f":"$E$2005","v":"Charpente en bois, revêtement en aluminium"}]
[{"$f":"IF(LEN('Translation-EN'!A2008)>0,'Translation-EN'!A2008,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2008)>0,'Translation-EN'!B2008,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2008)>0,'Translation-EN'!C2008,\"\")","v":"B249"},{"$f":"IF(LEN('Translation-EN'!D2008)>0,'Translation-EN'!D2008,\"\")","v":""},"Fenêtre – sous-fenêtre triple"]
[{"$f":"IF(LEN('Translation-EN'!A2009)>0,'Translation-EN'!A2009,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2009)>0,'Translation-EN'!B2009,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2009)>0,'Translation-EN'!C2009,\"\")","v":"E249"},{"$f":"IF(LEN('Translation-EN'!D2009)>0,'Translation-EN'!D2009,\"\")","v":""},{"$f":"$E$1993","v":"Cadre en fibre de verre"}]
[{"$f":"IF(LEN('Translation-EN'!A2010)>0,'Translation-EN'!A2010,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2010)>0,'Translation-EN'!B2010,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2010)>0,'Translation-EN'!C2010,\"\")","v":"B250"},{"$f":"IF(LEN('Translation-EN'!D2010)>0,'Translation-EN'!D2010,\"\")","v":""},{"$f":"$E$2008","v":"Fenêtre – sous-fenêtre triple"}]
[{"$f":"IF(LEN('Translation-EN'!A2011)>0,'Translation-EN'!A2011,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2011)>0,'Translation-EN'!B2011,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2011)>0,'Translation-EN'!C2011,\"\")","v":"E250"},{"$f":"IF(LEN('Translation-EN'!D2011)>0,'Translation-EN'!D2011,\"\")","v":""},{"$f":"$E$1999","v":"Charpente en vinyle"}]
[{"$f":"IF(LEN('Translation-EN'!A2012)>0,'Translation-EN'!A2012,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2012)>0,'Translation-EN'!B2012,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2012)>0,'Translation-EN'!C2012,\"\")","v":"B251"},{"$f":"IF(LEN('Translation-EN'!D2012)>0,'Translation-EN'!D2012,\"\")","v":""},{"$f":"$E$2008","v":"Fenêtre – sous-fenêtre triple"}]
[{"$f":"IF(LEN('Translation-EN'!A2013)>0,'Translation-EN'!A2013,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2013)>0,'Translation-EN'!B2013,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2013)>0,'Translation-EN'!C2013,\"\")","v":"E251"},{"$f":"IF(LEN('Translation-EN'!D2013)>0,'Translation-EN'!D2013,\"\")","v":""},{"$f":"$E$2001","v":"Charpente en bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2014)>0,'Translation-EN'!A2014,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2014)>0,'Translation-EN'!B2014,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2014)>0,'Translation-EN'!C2014,\"\")","v":"B252"},{"$f":"IF(LEN('Translation-EN'!D2014)>0,'Translation-EN'!D2014,\"\")","v":""},{"$f":"$E$2008","v":"Fenêtre – sous-fenêtre triple"}]
[{"$f":"IF(LEN('Translation-EN'!A2015)>0,'Translation-EN'!A2015,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2015)>0,'Translation-EN'!B2015,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2015)>0,'Translation-EN'!C2015,\"\")","v":"E252"},{"$f":"IF(LEN('Translation-EN'!D2015)>0,'Translation-EN'!D2015,\"\")","v":""},{"$f":"$E$2001","v":"Charpente en bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2016)>0,'Translation-EN'!A2016,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2016)>0,'Translation-EN'!B2016,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2016)>0,'Translation-EN'!C2016,\"\")","v":"B253"},{"$f":"IF(LEN('Translation-EN'!D2016)>0,'Translation-EN'!D2016,\"\")","v":""},{"$f":"$E$2008","v":"Fenêtre – sous-fenêtre triple"}]
[{"$f":"IF(LEN('Translation-EN'!A2017)>0,'Translation-EN'!A2017,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2017)>0,'Translation-EN'!B2017,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2017)>0,'Translation-EN'!C2017,\"\")","v":"E253"},{"$f":"IF(LEN('Translation-EN'!D2017)>0,'Translation-EN'!D2017,\"\")","v":""},{"$f":"$E$2005","v":"Charpente en bois, revêtement en aluminium"}]
[{"$f":"IF(LEN('Translation-EN'!A2018)>0,'Translation-EN'!A2018,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2018)>0,'Translation-EN'!B2018,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2018)>0,'Translation-EN'!C2018,\"\")","v":"B254"},{"$f":"IF(LEN('Translation-EN'!D2018)>0,'Translation-EN'!D2018,\"\")","v":""},{"$f":"$E$2008","v":"Fenêtre – sous-fenêtre triple"}]
[{"$f":"IF(LEN('Translation-EN'!A2019)>0,'Translation-EN'!A2019,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2019)>0,'Translation-EN'!B2019,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2019)>0,'Translation-EN'!C2019,\"\")","v":"E254"},{"$f":"IF(LEN('Translation-EN'!D2019)>0,'Translation-EN'!D2019,\"\")","v":""},{"$f":"$E$2005","v":"Charpente en bois, revêtement en aluminium"}]
[{"$f":"IF(LEN('Translation-EN'!A2020)>0,'Translation-EN'!A2020,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2020)>0,'Translation-EN'!B2020,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2020)>0,'Translation-EN'!C2020,\"\")","v":"B255"},{"$f":"IF(LEN('Translation-EN'!D2020)>0,'Translation-EN'!D2020,\"\")","v":""},"Fenêtre – triple vitrage"]
[{"$f":"IF(LEN('Translation-EN'!A2021)>0,'Translation-EN'!A2021,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2021)>0,'Translation-EN'!B2021,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2021)>0,'Translation-EN'!C2021,\"\")","v":"C255"},{"$f":"IF(LEN('Translation-EN'!D2021)>0,'Translation-EN'!D2021,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Isospan"]
[{"$f":"IF(LEN('Translation-EN'!A2022)>0,'Translation-EN'!A2022,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2022)>0,'Translation-EN'!B2022,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2022)>0,'Translation-EN'!C2022,\"\")","v":"D255"},{"$f":"IF(LEN('Translation-EN'!D2022)>0,'Translation-EN'!D2022,\"\")","v":""},"Okopur"]
[{"$f":"IF(LEN('Translation-EN'!A2023)>0,'Translation-EN'!A2023,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2023)>0,'Translation-EN'!B2023,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2023)>0,'Translation-EN'!C2023,\"\")","v":"E255"},{"$f":"IF(LEN('Translation-EN'!D2023)>0,'Translation-EN'!D2023,\"\")","v":""},"RÉVISION DES BESOINS"]
[{"$f":"IF(LEN('Translation-EN'!A2024)>0,'Translation-EN'!A2024,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2024)>0,'Translation-EN'!B2024,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2024)>0,'Translation-EN'!C2024,\"\")","v":"B256"},{"$f":"IF(LEN('Translation-EN'!D2024)>0,'Translation-EN'!D2024,\"\")","v":""},{"$f":"$E$2020","v":"Fenêtre – triple vitrage"}]
[{"$f":"IF(LEN('Translation-EN'!A2025)>0,'Translation-EN'!A2025,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2025)>0,'Translation-EN'!B2025,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2025)>0,'Translation-EN'!C2025,\"\")","v":"C256"},{"$f":"IF(LEN('Translation-EN'!D2025)>0,'Translation-EN'!D2025,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Nexcem, Faswall"]
[{"$f":"IF(LEN('Translation-EN'!A2026)>0,'Translation-EN'!A2026,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2026)>0,'Translation-EN'!B2026,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2026)>0,'Translation-EN'!C2026,\"\")","v":"E256"},{"$f":"IF(LEN('Translation-EN'!D2026)>0,'Translation-EN'!D2026,\"\")","v":""},"Bloc 12 po R22"]
[{"$f":"IF(LEN('Translation-EN'!A2027)>0,'Translation-EN'!A2027,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2027)>0,'Translation-EN'!B2027,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2027)>0,'Translation-EN'!C2027,\"\")","v":"B257"},{"$f":"IF(LEN('Translation-EN'!D2027)>0,'Translation-EN'!D2027,\"\")","v":""},{"$f":"$E$2020","v":"Fenêtre – triple vitrage"}]
[{"$f":"IF(LEN('Translation-EN'!A2028)>0,'Translation-EN'!A2028,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2028)>0,'Translation-EN'!B2028,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2028)>0,'Translation-EN'!C2028,\"\")","v":"C257"},{"$f":"IF(LEN('Translation-EN'!D2028)>0,'Translation-EN'!D2028,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$2025","v":"Nexcem, Faswall"}]
[{"$f":"IF(LEN('Translation-EN'!A2029)>0,'Translation-EN'!A2029,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2029)>0,'Translation-EN'!B2029,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2029)>0,'Translation-EN'!C2029,\"\")","v":"E257"},{"$f":"IF(LEN('Translation-EN'!D2029)>0,'Translation-EN'!D2029,\"\")","v":""},"Bloc 14 po R28"]
[{"$f":"IF(LEN('Translation-EN'!A2030)>0,'Translation-EN'!A2030,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2030)>0,'Translation-EN'!B2030,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2030)>0,'Translation-EN'!C2030,\"\")","v":"B258"},{"$f":"IF(LEN('Translation-EN'!D2030)>0,'Translation-EN'!D2030,\"\")","v":""},"Fibre de bois – en vrac"]
[{"$f":"IF(LEN('Translation-EN'!A2031)>0,'Translation-EN'!A2031,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2031)>0,'Translation-EN'!B2031,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2031)>0,'Translation-EN'!C2031,\"\")","v":"C258"},{"$f":"IF(LEN('Translation-EN'!D2031)>0,'Translation-EN'!D2031,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"GUTEX"]
[{"$f":"IF(LEN('Translation-EN'!A2032)>0,'Translation-EN'!A2032,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2032)>0,'Translation-EN'!B2032,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2032)>0,'Translation-EN'!C2032,\"\")","v":"D258"},{"$f":"IF(LEN('Translation-EN'!D2032)>0,'Translation-EN'!D2032,\"\")","v":""},"ThermoFiber"]
[{"$f":"IF(LEN('Translation-EN'!A2033)>0,'Translation-EN'!A2033,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2033)>0,'Translation-EN'!B2033,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2033)>0,'Translation-EN'!C2033,\"\")","v":"E258"},{"$f":"IF(LEN('Translation-EN'!D2033)>0,'Translation-EN'!D2033,\"\")","v":""},{"$f":"$E$1351","v":"R 3,6/po"}]
[{"$f":"IF(LEN('Translation-EN'!A2034)>0,'Translation-EN'!A2034,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2034)>0,'Translation-EN'!B2034,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2034)>0,'Translation-EN'!C2034,\"\")","v":"B260"},{"$f":"IF(LEN('Translation-EN'!D2034)>0,'Translation-EN'!D2034,\"\")","v":""},"Natte de fibres de bois"]
[{"$f":"IF(LEN('Translation-EN'!A2035)>0,'Translation-EN'!A2035,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2035)>0,'Translation-EN'!B2035,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2035)>0,'Translation-EN'!C2035,\"\")","v":"C260"},{"$f":"IF(LEN('Translation-EN'!D2035)>0,'Translation-EN'!D2035,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$2031","v":"GUTEX"}]
[{"$f":"IF(LEN('Translation-EN'!A2036)>0,'Translation-EN'!A2036,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2036)>0,'Translation-EN'!B2036,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2036)>0,'Translation-EN'!C2036,\"\")","v":"D260"},{"$f":"IF(LEN('Translation-EN'!D2036)>0,'Translation-EN'!D2036,\"\")","v":""},"ThermoFlex"]
[{"$f":"IF(LEN('Translation-EN'!A2037)>0,'Translation-EN'!A2037,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2037)>0,'Translation-EN'!B2037,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2037)>0,'Translation-EN'!C2037,\"\")","v":"E260"},{"$f":"IF(LEN('Translation-EN'!D2037)>0,'Translation-EN'!D2037,\"\")","v":""},"R 4/po"]
[{"$f":"IF(LEN('Translation-EN'!A2038)>0,'Translation-EN'!A2038,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2038)>0,'Translation-EN'!B2038,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2038)>0,'Translation-EN'!C2038,\"\")","v":"B261"},{"$f":"IF(LEN('Translation-EN'!D2038)>0,'Translation-EN'!D2038,\"\")","v":""},{"$f":"$E$2034","v":"Natte de fibres de bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2039)>0,'Translation-EN'!A2039,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2039)>0,'Translation-EN'!B2039,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2039)>0,'Translation-EN'!C2039,\"\")","v":"C261"},{"$f":"IF(LEN('Translation-EN'!D2039)>0,'Translation-EN'!D2039,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Pavatex"]
[{"$f":"IF(LEN('Translation-EN'!A2040)>0,'Translation-EN'!A2040,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2040)>0,'Translation-EN'!B2040,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2040)>0,'Translation-EN'!C2040,\"\")","v":"D261"},{"$f":"IF(LEN('Translation-EN'!D2040)>0,'Translation-EN'!D2040,\"\")","v":""},"Pavaflex"]
[{"$f":"IF(LEN('Translation-EN'!A2041)>0,'Translation-EN'!A2041,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2041)>0,'Translation-EN'!B2041,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2041)>0,'Translation-EN'!C2041,\"\")","v":"E261"},{"$f":"IF(LEN('Translation-EN'!D2041)>0,'Translation-EN'!D2041,\"\")","v":""},{"$f":"$E$1752","v":"R 3,8/po"}]
[{"$f":"IF(LEN('Translation-EN'!A2042)>0,'Translation-EN'!A2042,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2042)>0,'Translation-EN'!B2042,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2042)>0,'Translation-EN'!C2042,\"\")","v":"B262"},{"$f":"IF(LEN('Translation-EN'!D2042)>0,'Translation-EN'!D2042,\"\")","v":""},{"$f":"$E$2034","v":"Natte de fibres de bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2043)>0,'Translation-EN'!A2043,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2043)>0,'Translation-EN'!B2043,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2043)>0,'Translation-EN'!C2043,\"\")","v":"C262"},{"$f":"IF(LEN('Translation-EN'!D2043)>0,'Translation-EN'!D2043,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Steico"]
[{"$f":"IF(LEN('Translation-EN'!A2044)>0,'Translation-EN'!A2044,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2044)>0,'Translation-EN'!B2044,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2044)>0,'Translation-EN'!C2044,\"\")","v":"D262"},{"$f":"IF(LEN('Translation-EN'!D2044)>0,'Translation-EN'!D2044,\"\")","v":""},"SteicoFlex"]
[{"$f":"IF(LEN('Translation-EN'!A2045)>0,'Translation-EN'!A2045,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2045)>0,'Translation-EN'!B2045,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2045)>0,'Translation-EN'!C2045,\"\")","v":"E262"},{"$f":"IF(LEN('Translation-EN'!D2045)>0,'Translation-EN'!D2045,\"\")","v":""},{"$f":"$E$1752","v":"R 3,8/po"}]
[{"$f":"IF(LEN('Translation-EN'!A2046)>0,'Translation-EN'!A2046,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2046)>0,'Translation-EN'!B2046,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2046)>0,'Translation-EN'!C2046,\"\")","v":"B263"},{"$f":"IF(LEN('Translation-EN'!D2046)>0,'Translation-EN'!D2046,\"\")","v":""},"Panneau de fibres de bois"]
[{"$f":"IF(LEN('Translation-EN'!A2047)>0,'Translation-EN'!A2047,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2047)>0,'Translation-EN'!B2047,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2047)>0,'Translation-EN'!C2047,\"\")","v":"C263"},{"$f":"IF(LEN('Translation-EN'!D2047)>0,'Translation-EN'!D2047,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Conseil canadien du bois/Conseil américain du bois"]
[{"$f":"IF(LEN('Translation-EN'!A2048)>0,'Translation-EN'!A2048,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2048)>0,'Translation-EN'!B2048,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2048)>0,'Translation-EN'!C2048,\"\")","v":"D263"},{"$f":"IF(LEN('Translation-EN'!D2048)>0,'Translation-EN'!D2048,\"\")","v":""},"Inclus : Georgia Pacific, Louisville, BPC, Temple-Inland, Blue Ridge, Int'l Bildrite"]
[{"$f":"IF(LEN('Translation-EN'!A2049)>0,'Translation-EN'!A2049,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2049)>0,'Translation-EN'!B2049,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2049)>0,'Translation-EN'!C2049,\"\")","v":"E263"},{"$f":"IF(LEN('Translation-EN'!D2049)>0,'Translation-EN'!D2049,\"\")","v":""},"R 2,7/po"]
[{"$f":"IF(LEN('Translation-EN'!A2050)>0,'Translation-EN'!A2050,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2050)>0,'Translation-EN'!B2050,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2050)>0,'Translation-EN'!C2050,\"\")","v":"B264"},{"$f":"IF(LEN('Translation-EN'!D2050)>0,'Translation-EN'!D2050,\"\")","v":""},{"$f":"$E$2046","v":"Panneau de fibres de bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2051)>0,'Translation-EN'!A2051,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2051)>0,'Translation-EN'!B2051,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2051)>0,'Translation-EN'!C2051,\"\")","v":"C264"},{"$f":"IF(LEN('Translation-EN'!D2051)>0,'Translation-EN'!D2051,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$2031","v":"GUTEX"}]
[{"$f":"IF(LEN('Translation-EN'!A2052)>0,'Translation-EN'!A2052,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2052)>0,'Translation-EN'!B2052,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2052)>0,'Translation-EN'!C2052,\"\")","v":"D264"},{"$f":"IF(LEN('Translation-EN'!D2052)>0,'Translation-EN'!D2052,\"\")","v":""},"Multi-Therm"]
[{"$f":"IF(LEN('Translation-EN'!A2053)>0,'Translation-EN'!A2053,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2053)>0,'Translation-EN'!B2053,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2053)>0,'Translation-EN'!C2053,\"\")","v":"E264"},{"$f":"IF(LEN('Translation-EN'!D2053)>0,'Translation-EN'!D2053,\"\")","v":""},"R 3.6/po, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm"]
[{"$f":"IF(LEN('Translation-EN'!A2054)>0,'Translation-EN'!A2054,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2054)>0,'Translation-EN'!B2054,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2054)>0,'Translation-EN'!C2054,\"\")","v":"B266"},{"$f":"IF(LEN('Translation-EN'!D2054)>0,'Translation-EN'!D2054,\"\")","v":""},{"$f":"$E$2046","v":"Panneau de fibres de bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2055)>0,'Translation-EN'!A2055,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2055)>0,'Translation-EN'!B2055,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2055)>0,'Translation-EN'!C2055,\"\")","v":"C266"},{"$f":"IF(LEN('Translation-EN'!D2055)>0,'Translation-EN'!D2055,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$2039","v":"Pavatex"}]
[{"$f":"IF(LEN('Translation-EN'!A2056)>0,'Translation-EN'!A2056,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2056)>0,'Translation-EN'!B2056,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2056)>0,'Translation-EN'!C2056,\"\")","v":"D266"},{"$f":"IF(LEN('Translation-EN'!D2056)>0,'Translation-EN'!D2056,\"\")","v":""},"Pavatherm"]
[{"$f":"IF(LEN('Translation-EN'!A2057)>0,'Translation-EN'!A2057,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2057)>0,'Translation-EN'!B2057,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2057)>0,'Translation-EN'!C2057,\"\")","v":"E266"},{"$f":"IF(LEN('Translation-EN'!D2057)>0,'Translation-EN'!D2057,\"\")","v":""},"R 3,4/po"]
[{"$f":"IF(LEN('Translation-EN'!A2058)>0,'Translation-EN'!A2058,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2058)>0,'Translation-EN'!B2058,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2058)>0,'Translation-EN'!C2058,\"\")","v":"B267"},{"$f":"IF(LEN('Translation-EN'!D2058)>0,'Translation-EN'!D2058,\"\")","v":""},{"$f":"$E$2046","v":"Panneau de fibres de bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2059)>0,'Translation-EN'!A2059,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2059)>0,'Translation-EN'!B2059,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2059)>0,'Translation-EN'!C2059,\"\")","v":"C267"},{"$f":"IF(LEN('Translation-EN'!D2059)>0,'Translation-EN'!D2059,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$2043","v":"Steico"}]
[{"$f":"IF(LEN('Translation-EN'!A2060)>0,'Translation-EN'!A2060,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2060)>0,'Translation-EN'!B2060,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2060)>0,'Translation-EN'!C2060,\"\")","v":"D267"},{"$f":"IF(LEN('Translation-EN'!D2060)>0,'Translation-EN'!D2060,\"\")","v":""},"Special Dry"]
[{"$f":"IF(LEN('Translation-EN'!A2061)>0,'Translation-EN'!A2061,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2061)>0,'Translation-EN'!B2061,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2061)>0,'Translation-EN'!C2061,\"\")","v":"E267"},{"$f":"IF(LEN('Translation-EN'!D2061)>0,'Translation-EN'!D2061,\"\")","v":""},"R 3,6/po, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm"]
[{"$f":"IF(LEN('Translation-EN'!A2062)>0,'Translation-EN'!A2062,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2062)>0,'Translation-EN'!B2062,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2062)>0,'Translation-EN'!C2062,\"\")","v":"B268"},{"$f":"IF(LEN('Translation-EN'!D2062)>0,'Translation-EN'!D2062,\"\")","v":""},"Charpente en bois – Bois tendre"]
[{"$f":"IF(LEN('Translation-EN'!A2063)>0,'Translation-EN'!A2063,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2063)>0,'Translation-EN'!B2063,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2063)>0,'Translation-EN'!C2063,\"\")","v":"C268"},{"$f":"IF(LEN('Translation-EN'!D2063)>0,'Translation-EN'!D2063,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Roseburg"]
[{"$f":"IF(LEN('Translation-EN'!A2064)>0,'Translation-EN'!A2064,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2064)>0,'Translation-EN'!B2064,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2064)>0,'Translation-EN'!C2064,\"\")","v":"B269"},{"$f":"IF(LEN('Translation-EN'!D2064)>0,'Translation-EN'!D2064,\"\")","v":""},"Charpente et bardage en bois – Séquoia"]
[{"$f":"IF(LEN('Translation-EN'!A2065)>0,'Translation-EN'!A2065,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2065)>0,'Translation-EN'!B2065,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2065)>0,'Translation-EN'!C2065,\"\")","v":"C269"},{"$f":"IF(LEN('Translation-EN'!D2065)>0,'Translation-EN'!D2065,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1627","v":"Conseil américain du bois et Conseil canadien du bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2066)>0,'Translation-EN'!A2066,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2066)>0,'Translation-EN'!B2066,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2066)>0,'Translation-EN'!C2066,\"\")","v":"B270"},{"$f":"IF(LEN('Translation-EN'!D2066)>0,'Translation-EN'!D2066,\"\")","v":""},"Charpente et bardage en bois – EPS"]
[{"$f":"IF(LEN('Translation-EN'!A2067)>0,'Translation-EN'!A2067,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2067)>0,'Translation-EN'!B2067,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2067)>0,'Translation-EN'!C2067,\"\")","v":"C270"},{"$f":"IF(LEN('Translation-EN'!D2067)>0,'Translation-EN'!D2067,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1627","v":"Conseil américain du bois et Conseil canadien du bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2068)>0,'Translation-EN'!A2068,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2068)>0,'Translation-EN'!B2068,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2068)>0,'Translation-EN'!C2068,\"\")","v":"B271"},{"$f":"IF(LEN('Translation-EN'!D2068)>0,'Translation-EN'!D2068,\"\")","v":""},"Poutrelle en I en bois"]
[{"$f":"IF(LEN('Translation-EN'!A2069)>0,'Translation-EN'!A2069,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2069)>0,'Translation-EN'!B2069,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2069)>0,'Translation-EN'!C2069,\"\")","v":"C271"},{"$f":"IF(LEN('Translation-EN'!D2069)>0,'Translation-EN'!D2069,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1627","v":"Conseil américain du bois et Conseil canadien du bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2070)>0,'Translation-EN'!A2070,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2070)>0,'Translation-EN'!B2070,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2070)>0,'Translation-EN'!C2070,\"\")","v":"E271"},{"$f":"IF(LEN('Translation-EN'!D2070)>0,'Translation-EN'!D2070,\"\")","v":""},"TJI 230/360"]
[{"$f":"IF(LEN('Translation-EN'!A2071)>0,'Translation-EN'!A2071,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2071)>0,'Translation-EN'!B2071,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2071)>0,'Translation-EN'!C2071,\"\")","v":"B272"},{"$f":"IF(LEN('Translation-EN'!D2071)>0,'Translation-EN'!D2071,\"\")","v":""},{"$f":"$E$2068","v":"Poutrelle en I en bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2072)>0,'Translation-EN'!A2072,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2072)>0,'Translation-EN'!B2072,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2072)>0,'Translation-EN'!C2072,\"\")","v":"C272"},{"$f":"IF(LEN('Translation-EN'!D2072)>0,'Translation-EN'!D2072,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$2063","v":"Roseburg"}]
[{"$f":"IF(LEN('Translation-EN'!A2073)>0,'Translation-EN'!A2073,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2073)>0,'Translation-EN'!B2073,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2073)>0,'Translation-EN'!C2073,\"\")","v":"D272"},{"$f":"IF(LEN('Translation-EN'!D2073)>0,'Translation-EN'!D2073,\"\")","v":""},"Poutrelle RFPI"]
[{"$f":"IF(LEN('Translation-EN'!A2074)>0,'Translation-EN'!A2074,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2074)>0,'Translation-EN'!B2074,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2074)>0,'Translation-EN'!C2074,\"\")","v":"B273"},{"$f":"IF(LEN('Translation-EN'!D2074)>0,'Translation-EN'!D2074,\"\")","v":""},"Poutrelle de plancher en bois – préfabriquée"]
[{"$f":"IF(LEN('Translation-EN'!A2075)>0,'Translation-EN'!A2075,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2075)>0,'Translation-EN'!B2075,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2075)>0,'Translation-EN'!C2075,\"\")","v":"C273"},{"$f":"IF(LEN('Translation-EN'!D2075)>0,'Translation-EN'!D2075,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Bureau de promotion des produits du bois du Québec"]
[{"$f":"IF(LEN('Translation-EN'!A2076)>0,'Translation-EN'!A2076,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2076)>0,'Translation-EN'!B2076,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2076)>0,'Translation-EN'!C2076,\"\")","v":"D273"},{"$f":"IF(LEN('Translation-EN'!D2076)>0,'Translation-EN'!D2076,\"\")","v":""},"Modèle de toile commun (Warren, 45 deg)"]
[{"$f":"IF(LEN('Translation-EN'!A2077)>0,'Translation-EN'!A2077,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2077)>0,'Translation-EN'!B2077,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2077)>0,'Translation-EN'!C2077,\"\")","v":"E273"},{"$f":"IF(LEN('Translation-EN'!D2077)>0,'Translation-EN'!D2077,\"\")","v":""},"Palier de la membrure supérieure, profondeur variable"]
[{"$f":"IF(LEN('Translation-EN'!A2078)>0,'Translation-EN'!A2078,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2078)>0,'Translation-EN'!B2078,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2078)>0,'Translation-EN'!C2078,\"\")","v":"B274"},{"$f":"IF(LEN('Translation-EN'!D2078)>0,'Translation-EN'!D2078,\"\")","v":""},"Poutrelle de toit en bois – préfabriquée"]
[{"$f":"IF(LEN('Translation-EN'!A2079)>0,'Translation-EN'!A2079,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2079)>0,'Translation-EN'!B2079,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2079)>0,'Translation-EN'!C2079,\"\")","v":"C274"},{"$f":"IF(LEN('Translation-EN'!D2079)>0,'Translation-EN'!D2079,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$2075","v":"Bureau de promotion des produits du bois du Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2080)>0,'Translation-EN'!A2080,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2080)>0,'Translation-EN'!B2080,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2080)>0,'Translation-EN'!C2080,\"\")","v":"D274"},{"$f":"IF(LEN('Translation-EN'!D2080)>0,'Translation-EN'!D2080,\"\")","v":""},"Toit en gabarit commun (Double Howe)"]
[{"$f":"IF(LEN('Translation-EN'!A2081)>0,'Translation-EN'!A2081,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2081)>0,'Translation-EN'!B2081,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2081)>0,'Translation-EN'!C2081,\"\")","v":"E274"},{"$f":"IF(LEN('Translation-EN'!D2081)>0,'Translation-EN'!D2081,\"\")","v":""},"Cordes 2x6, toiles 2x4, pas de 4:12, portée de 40 pieds, porte-à-faux de 20 po."]
[{"$f":"IF(LEN('Translation-EN'!A2082)>0,'Translation-EN'!A2082,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2082)>0,'Translation-EN'!B2082,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2082)>0,'Translation-EN'!C2082,\"\")","v":"B275"},{"$f":"IF(LEN('Translation-EN'!D2082)>0,'Translation-EN'!D2082,\"\")","v":""},"Panneau de fibres de laine"]
[{"$f":"IF(LEN('Translation-EN'!A2083)>0,'Translation-EN'!A2083,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2083)>0,'Translation-EN'!B2083,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2083)>0,'Translation-EN'!C2083,\"\")","v":"C275"},{"$f":"IF(LEN('Translation-EN'!D2083)>0,'Translation-EN'!D2083,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1301","v":"Armstrong"}]
[{"$f":"IF(LEN('Translation-EN'!A2084)>0,'Translation-EN'!A2084,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2084)>0,'Translation-EN'!B2084,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2084)>0,'Translation-EN'!C2084,\"\")","v":"D275"},{"$f":"IF(LEN('Translation-EN'!D2084)>0,'Translation-EN'!D2084,\"\")","v":""},"Tectum"]
[{"$f":"IF(LEN('Translation-EN'!A2085)>0,'Translation-EN'!A2085,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2085)>0,'Translation-EN'!B2085,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2085)>0,'Translation-EN'!C2085,\"\")","v":"E275"},{"$f":"IF(LEN('Translation-EN'!D2085)>0,'Translation-EN'!D2085,\"\")","v":""},"2 po (50,8 mm)"]
[{"$f":"IF(LEN('Translation-EN'!A2086)>0,'Translation-EN'!A2086,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2086)>0,'Translation-EN'!B2086,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2086)>0,'Translation-EN'!C2086,\"\")","v":"B276"},{"$f":"IF(LEN('Translation-EN'!D2086)>0,'Translation-EN'!D2086,\"\")","v":""},"Natte de laine"]
[{"$f":"IF(LEN('Translation-EN'!A2087)>0,'Translation-EN'!A2087,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2087)>0,'Translation-EN'!B2087,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2087)>0,'Translation-EN'!C2087,\"\")","v":"C276"},{"$f":"IF(LEN('Translation-EN'!D2087)>0,'Translation-EN'!D2087,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},"Laine Havelock"]
[{"$f":"IF(LEN('Translation-EN'!A2088)>0,'Translation-EN'!A2088,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2088)>0,'Translation-EN'!B2088,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2088)>0,'Translation-EN'!C2088,\"\")","v":"E276"},{"$f":"IF(LEN('Translation-EN'!D2088)>0,'Translation-EN'!D2088,\"\")","v":""},{"$f":"$E$1351","v":"R 3,6/po"}]
[{"$f":"IF(LEN('Translation-EN'!A2089)>0,'Translation-EN'!A2089,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2089)>0,'Translation-EN'!B2089,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2089)>0,'Translation-EN'!C2089,\"\")","v":"B277"},{"$f":"IF(LEN('Translation-EN'!D2089)>0,'Translation-EN'!D2089,\"\")","v":""},"Laine en vrac"]
[{"$f":"IF(LEN('Translation-EN'!A2090)>0,'Translation-EN'!A2090,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2090)>0,'Translation-EN'!B2090,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2090)>0,'Translation-EN'!C2090,\"\")","v":"C277"},{"$f":"IF(LEN('Translation-EN'!D2090)>0,'Translation-EN'!D2090,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$2087","v":"Laine Havelock"}]
[{"$f":"IF(LEN('Translation-EN'!A2091)>0,'Translation-EN'!A2091,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2091)>0,'Translation-EN'!B2091,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2091)>0,'Translation-EN'!C2091,\"\")","v":"E277"},{"$f":"IF(LEN('Translation-EN'!D2091)>0,'Translation-EN'!D2091,\"\")","v":""},"R 4,4/po"]
[{"$f":"IF(LEN('Translation-EN'!A2092)>0,'Translation-EN'!A2092,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2092)>0,'Translation-EN'!B2092,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2092)>0,'Translation-EN'!C2092,\"\")","v":"B278"},{"$f":"IF(LEN('Translation-EN'!D2092)>0,'Translation-EN'!D2092,\"\")","v":""},"Panneau en mousse XPS"]
[{"$f":"IF(LEN('Translation-EN'!A2093)>0,'Translation-EN'!A2093,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2093)>0,'Translation-EN'!B2093,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2093)>0,'Translation-EN'!C2093,\"\")","v":"C278"},{"$f":"IF(LEN('Translation-EN'!D2093)>0,'Translation-EN'!D2093,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1812","v":"Dow Chemical Company"}]
[{"$f":"IF(LEN('Translation-EN'!A2094)>0,'Translation-EN'!A2094,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2094)>0,'Translation-EN'!B2094,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2094)>0,'Translation-EN'!C2094,\"\")","v":"D278"},{"$f":"IF(LEN('Translation-EN'!D2094)>0,'Translation-EN'!D2094,\"\")","v":""},"Styromousse SM"]
[{"$f":"IF(LEN('Translation-EN'!A2095)>0,'Translation-EN'!A2095,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2095)>0,'Translation-EN'!B2095,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2095)>0,'Translation-EN'!C2095,\"\")","v":"E278"},{"$f":"IF(LEN('Translation-EN'!D2095)>0,'Translation-EN'!D2095,\"\")","v":""},"R 5/po"]
[{"$f":"IF(LEN('Translation-EN'!A2096)>0,'Translation-EN'!A2096,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2096)>0,'Translation-EN'!B2096,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2096)>0,'Translation-EN'!C2096,\"\")","v":"B279"},{"$f":"IF(LEN('Translation-EN'!D2096)>0,'Translation-EN'!D2096,\"\")","v":""},{"$f":"$E$2092","v":"Panneau en mousse XPS"}]
[{"$f":"IF(LEN('Translation-EN'!A2097)>0,'Translation-EN'!A2097,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2097)>0,'Translation-EN'!B2097,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2097)>0,'Translation-EN'!C2097,\"\")","v":"C279"},{"$f":"IF(LEN('Translation-EN'!D2097)>0,'Translation-EN'!D2097,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1288","v":"Owens Corning"}]
[{"$f":"IF(LEN('Translation-EN'!A2098)>0,'Translation-EN'!A2098,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2098)>0,'Translation-EN'!B2098,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2098)>0,'Translation-EN'!C2098,\"\")","v":"D279"},{"$f":"IF(LEN('Translation-EN'!D2098)>0,'Translation-EN'!D2098,\"\")","v":""},"Foamular 250 "]
[{"$f":"IF(LEN('Translation-EN'!A2099)>0,'Translation-EN'!A2099,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2099)>0,'Translation-EN'!B2099,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2099)>0,'Translation-EN'!C2099,\"\")","v":"E279"},{"$f":"IF(LEN('Translation-EN'!D2099)>0,'Translation-EN'!D2099,\"\")","v":""},{"$f":"$E$2095","v":"R 5/po"}]
[{"$f":"IF(LEN('Translation-EN'!A2100)>0,'Translation-EN'!A2100,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2100)>0,'Translation-EN'!B2100,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2100)>0,'Translation-EN'!C2100,\"\")","v":"B280"},{"$f":"IF(LEN('Translation-EN'!D2100)>0,'Translation-EN'!D2100,\"\")","v":""},{"$f":"$E$2092","v":"Panneau en mousse XPS"}]
[{"$f":"IF(LEN('Translation-EN'!A2101)>0,'Translation-EN'!A2101,\"\")","v":"-"},{"$f":"IF(LEN('Translation-EN'!B2101)>0,'Translation-EN'!B2101,\"\")","v":"_Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2101)>0,'Translation-EN'!C2101,\"\")","v":"C280"},{"$f":"IF(LEN('Translation-EN'!D2101)>0,'Translation-EN'!D2101,\"\")","v":"Ignore this cell of Master sheet. Company is not translatable"},{"$f":"$E$1288","v":"Owens Corning"}]
[{"$f":"IF(LEN('Translation-EN'!A2102)>0,'Translation-EN'!A2102,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2102)>0,'Translation-EN'!B2102,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2102)>0,'Translation-EN'!C2102,\"\")","v":"D280"},{"$f":"IF(LEN('Translation-EN'!D2102)>0,'Translation-EN'!D2102,\"\")","v":""},"Foamular NGX 250 "]
[{"$f":"IF(LEN('Translation-EN'!A2103)>0,'Translation-EN'!A2103,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2103)>0,'Translation-EN'!B2103,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2103)>0,'Translation-EN'!C2103,\"\")","v":"E280"},{"$f":"IF(LEN('Translation-EN'!D2103)>0,'Translation-EN'!D2103,\"\")","v":""},{"$f":"$E$2095","v":"R 5/po"}]
[{"$f":"IF(LEN('Translation-EN'!A2104)>0,'Translation-EN'!A2104,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2104)>0,'Translation-EN'!B2104,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2104)>0,'Translation-EN'!C2104,\"\")","v":"B281"},{"$f":"IF(LEN('Translation-EN'!D2104)>0,'Translation-EN'!D2104,\"\")","v":""},"De la feuille maîtresse composite"]
[{"$f":"IF(LEN('Translation-EN'!A2105)>0,'Translation-EN'!A2105,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2105)>0,'Translation-EN'!B2105,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2105)>0,'Translation-EN'!C2105,\"\")","v":"B282"},{"$f":"IF(LEN('Translation-EN'!D2105)>0,'Translation-EN'!D2105,\"\")","v":""},{"$f":"$E$2104","v":"De la feuille maîtresse composite"}]
[{"$f":"IF(LEN('Translation-EN'!A2106)>0,'Translation-EN'!A2106,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2106)>0,'Translation-EN'!B2106,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2106)>0,'Translation-EN'!C2106,\"\")","v":"B283"},{"$f":"IF(LEN('Translation-EN'!D2106)>0,'Translation-EN'!D2106,\"\")","v":""},"De la feuille maîtresse composite"]
[{"$f":"IF(LEN('Translation-EN'!A2107)>0,'Translation-EN'!A2107,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2107)>0,'Translation-EN'!B2107,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2107)>0,'Translation-EN'!C2107,\"\")","v":"B284"},{"$f":"IF(LEN('Translation-EN'!D2107)>0,'Translation-EN'!D2107,\"\")","v":""},"De la feuille maîtresse composite"]
[{"$f":"IF(LEN('Translation-EN'!A2108)>0,'Translation-EN'!A2108,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2108)>0,'Translation-EN'!B2108,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2108)>0,'Translation-EN'!C2108,\"\")","v":"B285"},{"$f":"IF(LEN('Translation-EN'!D2108)>0,'Translation-EN'!D2108,\"\")","v":""},"De la feuille maîtresse composite"]
[{"$f":"IF(LEN('Translation-EN'!A2109)>0,'Translation-EN'!A2109,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2109)>0,'Translation-EN'!B2109,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2109)>0,'Translation-EN'!C2109,\"\")","v":"B286"},{"$f":"IF(LEN('Translation-EN'!D2109)>0,'Translation-EN'!D2109,\"\")","v":""},"De la feuille maîtresse composite"]
[{"$f":"IF(LEN('Translation-EN'!A2110)>0,'Translation-EN'!A2110,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2110)>0,'Translation-EN'!B2110,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2110)>0,'Translation-EN'!C2110,\"\")","v":"B287"},{"$f":"IF(LEN('Translation-EN'!D2110)>0,'Translation-EN'!D2110,\"\")","v":""},"De la feuille maîtresse composite"]
[{"$f":"IF(LEN('Translation-EN'!A2111)>0,'Translation-EN'!A2111,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2111)>0,'Translation-EN'!B2111,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2111)>0,'Translation-EN'!C2111,\"\")","v":"B288"},{"$f":"IF(LEN('Translation-EN'!D2111)>0,'Translation-EN'!D2111,\"\")","v":""},"De la feuille maîtresse composite"]
[{"$f":"IF(LEN('Translation-EN'!A2112)>0,'Translation-EN'!A2112,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2112)>0,'Translation-EN'!B2112,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2112)>0,'Translation-EN'!C2112,\"\")","v":"B289"},{"$f":"IF(LEN('Translation-EN'!D2112)>0,'Translation-EN'!D2112,\"\")","v":""},"De la feuille maîtresse composite"]
[{"$f":"IF(LEN('Translation-EN'!A2113)>0,'Translation-EN'!A2113,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2113)>0,'Translation-EN'!B2113,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2113)>0,'Translation-EN'!C2113,\"\")","v":"B290"},{"$f":"IF(LEN('Translation-EN'!D2113)>0,'Translation-EN'!D2113,\"\")","v":""},"De la feuille maîtresse composite"]
[{"$f":"IF(LEN('Translation-EN'!A2114)>0,'Translation-EN'!A2114,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2114)>0,'Translation-EN'!B2114,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2114)>0,'Translation-EN'!C2114,\"\")","v":"B291"},{"$f":"IF(LEN('Translation-EN'!D2114)>0,'Translation-EN'!D2114,\"\")","v":""},"De la feuille maîtresse composite"]
[{"$f":"IF(LEN('Translation-EN'!A2115)>0,'Translation-EN'!A2115,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2115)>0,'Translation-EN'!B2115,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2115)>0,'Translation-EN'!C2115,\"\")","v":"B292"},{"$f":"IF(LEN('Translation-EN'!D2115)>0,'Translation-EN'!D2115,\"\")","v":""},"Béton - 25 MPs, Moyenne de référence du Québec"]
[{"$f":"IF(LEN('Translation-EN'!A2116)>0,'Translation-EN'!A2116,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2116)>0,'Translation-EN'!B2116,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2116)>0,'Translation-EN'!C2116,\"\")","v":"D292"},{"$f":"IF(LEN('Translation-EN'!D2116)>0,'Translation-EN'!D2116,\"\")","v":""},"Can. Moyenne Québec"]
[{"$f":"IF(LEN('Translation-EN'!A2117)>0,'Translation-EN'!A2117,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2117)>0,'Translation-EN'!B2117,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2117)>0,'Translation-EN'!C2117,\"\")","v":"B293"},{"$f":"IF(LEN('Translation-EN'!D2117)>0,'Translation-EN'!D2117,\"\")","v":""},"Béton - 25 MPa, 10% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2118)>0,'Translation-EN'!A2118,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2118)>0,'Translation-EN'!B2118,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2118)>0,'Translation-EN'!C2118,\"\")","v":"D293"},{"$f":"IF(LEN('Translation-EN'!D2118)>0,'Translation-EN'!D2118,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2119)>0,'Translation-EN'!A2119,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2119)>0,'Translation-EN'!B2119,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2119)>0,'Translation-EN'!C2119,\"\")","v":"B294"},{"$f":"IF(LEN('Translation-EN'!D2119)>0,'Translation-EN'!D2119,\"\")","v":""},"Béton -  25 MPa, 10% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2120)>0,'Translation-EN'!A2120,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2120)>0,'Translation-EN'!B2120,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2120)>0,'Translation-EN'!C2120,\"\")","v":"D294"},{"$f":"IF(LEN('Translation-EN'!D2120)>0,'Translation-EN'!D2120,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2121)>0,'Translation-EN'!A2121,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2121)>0,'Translation-EN'!B2121,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2121)>0,'Translation-EN'!C2121,\"\")","v":"B295"},{"$f":"IF(LEN('Translation-EN'!D2121)>0,'Translation-EN'!D2121,\"\")","v":""},"Béton - 25 MPa, 20% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2122)>0,'Translation-EN'!A2122,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2122)>0,'Translation-EN'!B2122,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2122)>0,'Translation-EN'!C2122,\"\")","v":"D295"},{"$f":"IF(LEN('Translation-EN'!D2122)>0,'Translation-EN'!D2122,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2123)>0,'Translation-EN'!A2123,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2123)>0,'Translation-EN'!B2123,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2123)>0,'Translation-EN'!C2123,\"\")","v":"B296"},{"$f":"IF(LEN('Translation-EN'!D2123)>0,'Translation-EN'!D2123,\"\")","v":""},"Béton - 25 MPa, 20% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2124)>0,'Translation-EN'!A2124,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2124)>0,'Translation-EN'!B2124,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2124)>0,'Translation-EN'!C2124,\"\")","v":"D296"},{"$f":"IF(LEN('Translation-EN'!D2124)>0,'Translation-EN'!D2124,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2125)>0,'Translation-EN'!A2125,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2125)>0,'Translation-EN'!B2125,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2125)>0,'Translation-EN'!C2125,\"\")","v":"B297"},{"$f":"IF(LEN('Translation-EN'!D2125)>0,'Translation-EN'!D2125,\"\")","v":""},"Béton - 25 MPa, 30% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2126)>0,'Translation-EN'!A2126,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2126)>0,'Translation-EN'!B2126,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2126)>0,'Translation-EN'!C2126,\"\")","v":"D297"},{"$f":"IF(LEN('Translation-EN'!D2126)>0,'Translation-EN'!D2126,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2127)>0,'Translation-EN'!A2127,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2127)>0,'Translation-EN'!B2127,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2127)>0,'Translation-EN'!C2127,\"\")","v":"B298"},{"$f":"IF(LEN('Translation-EN'!D2127)>0,'Translation-EN'!D2127,\"\")","v":""},"Béton - 25 MPa, 30% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2128)>0,'Translation-EN'!A2128,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2128)>0,'Translation-EN'!B2128,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2128)>0,'Translation-EN'!C2128,\"\")","v":"D298"},{"$f":"IF(LEN('Translation-EN'!D2128)>0,'Translation-EN'!D2128,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2129)>0,'Translation-EN'!A2129,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2129)>0,'Translation-EN'!B2129,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2129)>0,'Translation-EN'!C2129,\"\")","v":"B299"},{"$f":"IF(LEN('Translation-EN'!D2129)>0,'Translation-EN'!D2129,\"\")","v":""},"Béton - 30 MPs, Moyenne de référence du Québec"]
[{"$f":"IF(LEN('Translation-EN'!A2130)>0,'Translation-EN'!A2130,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2130)>0,'Translation-EN'!B2130,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2130)>0,'Translation-EN'!C2130,\"\")","v":"D299"},{"$f":"IF(LEN('Translation-EN'!D2130)>0,'Translation-EN'!D2130,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2131)>0,'Translation-EN'!A2131,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2131)>0,'Translation-EN'!B2131,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2131)>0,'Translation-EN'!C2131,\"\")","v":"B300"},{"$f":"IF(LEN('Translation-EN'!D2131)>0,'Translation-EN'!D2131,\"\")","v":""},"Béton - 30 MPa, 10% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2132)>0,'Translation-EN'!A2132,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2132)>0,'Translation-EN'!B2132,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2132)>0,'Translation-EN'!C2132,\"\")","v":"D300"},{"$f":"IF(LEN('Translation-EN'!D2132)>0,'Translation-EN'!D2132,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2133)>0,'Translation-EN'!A2133,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2133)>0,'Translation-EN'!B2133,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2133)>0,'Translation-EN'!C2133,\"\")","v":"B301"},{"$f":"IF(LEN('Translation-EN'!D2133)>0,'Translation-EN'!D2133,\"\")","v":""},"Béton -  30 MPa, 10% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2134)>0,'Translation-EN'!A2134,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2134)>0,'Translation-EN'!B2134,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2134)>0,'Translation-EN'!C2134,\"\")","v":"D301"},{"$f":"IF(LEN('Translation-EN'!D2134)>0,'Translation-EN'!D2134,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2135)>0,'Translation-EN'!A2135,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2135)>0,'Translation-EN'!B2135,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2135)>0,'Translation-EN'!C2135,\"\")","v":"B302"},{"$f":"IF(LEN('Translation-EN'!D2135)>0,'Translation-EN'!D2135,\"\")","v":""},"Béton - 30 MPa, 20% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2136)>0,'Translation-EN'!A2136,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2136)>0,'Translation-EN'!B2136,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2136)>0,'Translation-EN'!C2136,\"\")","v":"D302"},{"$f":"IF(LEN('Translation-EN'!D2136)>0,'Translation-EN'!D2136,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2137)>0,'Translation-EN'!A2137,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2137)>0,'Translation-EN'!B2137,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2137)>0,'Translation-EN'!C2137,\"\")","v":"B303"},{"$f":"IF(LEN('Translation-EN'!D2137)>0,'Translation-EN'!D2137,\"\")","v":""},"Béton - 30 MPa, 20% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2138)>0,'Translation-EN'!A2138,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2138)>0,'Translation-EN'!B2138,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2138)>0,'Translation-EN'!C2138,\"\")","v":"D303"},{"$f":"IF(LEN('Translation-EN'!D2138)>0,'Translation-EN'!D2138,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2139)>0,'Translation-EN'!A2139,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2139)>0,'Translation-EN'!B2139,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2139)>0,'Translation-EN'!C2139,\"\")","v":"B304"},{"$f":"IF(LEN('Translation-EN'!D2139)>0,'Translation-EN'!D2139,\"\")","v":""},"Béton - 30 MPa, 30% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2140)>0,'Translation-EN'!A2140,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2140)>0,'Translation-EN'!B2140,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2140)>0,'Translation-EN'!C2140,\"\")","v":"D304"},{"$f":"IF(LEN('Translation-EN'!D2140)>0,'Translation-EN'!D2140,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2141)>0,'Translation-EN'!A2141,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2141)>0,'Translation-EN'!B2141,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2141)>0,'Translation-EN'!C2141,\"\")","v":"B305"},{"$f":"IF(LEN('Translation-EN'!D2141)>0,'Translation-EN'!D2141,\"\")","v":""},"Béton - 30 MPa, 30% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2142)>0,'Translation-EN'!A2142,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2142)>0,'Translation-EN'!B2142,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2142)>0,'Translation-EN'!C2142,\"\")","v":"D305"},{"$f":"IF(LEN('Translation-EN'!D2142)>0,'Translation-EN'!D2142,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2143)>0,'Translation-EN'!A2143,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2143)>0,'Translation-EN'!B2143,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2143)>0,'Translation-EN'!C2143,\"\")","v":"B306"},{"$f":"IF(LEN('Translation-EN'!D2143)>0,'Translation-EN'!D2143,\"\")","v":""},"Béton - 35 MPs, Moyenne de référence du Québec"]
[{"$f":"IF(LEN('Translation-EN'!A2144)>0,'Translation-EN'!A2144,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2144)>0,'Translation-EN'!B2144,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2144)>0,'Translation-EN'!C2144,\"\")","v":"D306"},{"$f":"IF(LEN('Translation-EN'!D2144)>0,'Translation-EN'!D2144,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2145)>0,'Translation-EN'!A2145,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2145)>0,'Translation-EN'!B2145,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2145)>0,'Translation-EN'!C2145,\"\")","v":"B307"},{"$f":"IF(LEN('Translation-EN'!D2145)>0,'Translation-EN'!D2145,\"\")","v":""},"Béton - 35 MPa, 10% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2146)>0,'Translation-EN'!A2146,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2146)>0,'Translation-EN'!B2146,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2146)>0,'Translation-EN'!C2146,\"\")","v":"D307"},{"$f":"IF(LEN('Translation-EN'!D2146)>0,'Translation-EN'!D2146,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2147)>0,'Translation-EN'!A2147,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2147)>0,'Translation-EN'!B2147,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2147)>0,'Translation-EN'!C2147,\"\")","v":"B308"},{"$f":"IF(LEN('Translation-EN'!D2147)>0,'Translation-EN'!D2147,\"\")","v":""},"Béton -  35 MPa, 10% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2148)>0,'Translation-EN'!A2148,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2148)>0,'Translation-EN'!B2148,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2148)>0,'Translation-EN'!C2148,\"\")","v":"D308"},{"$f":"IF(LEN('Translation-EN'!D2148)>0,'Translation-EN'!D2148,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2149)>0,'Translation-EN'!A2149,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2149)>0,'Translation-EN'!B2149,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2149)>0,'Translation-EN'!C2149,\"\")","v":"B309"},{"$f":"IF(LEN('Translation-EN'!D2149)>0,'Translation-EN'!D2149,\"\")","v":""},"Béton - 35 MPa, 20% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2150)>0,'Translation-EN'!A2150,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2150)>0,'Translation-EN'!B2150,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2150)>0,'Translation-EN'!C2150,\"\")","v":"D309"},{"$f":"IF(LEN('Translation-EN'!D2150)>0,'Translation-EN'!D2150,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2151)>0,'Translation-EN'!A2151,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2151)>0,'Translation-EN'!B2151,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2151)>0,'Translation-EN'!C2151,\"\")","v":"B310"},{"$f":"IF(LEN('Translation-EN'!D2151)>0,'Translation-EN'!D2151,\"\")","v":""},"Béton - 35 MPa, 20% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2152)>0,'Translation-EN'!A2152,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2152)>0,'Translation-EN'!B2152,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2152)>0,'Translation-EN'!C2152,\"\")","v":"D310"},{"$f":"IF(LEN('Translation-EN'!D2152)>0,'Translation-EN'!D2152,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2153)>0,'Translation-EN'!A2153,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2153)>0,'Translation-EN'!B2153,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2153)>0,'Translation-EN'!C2153,\"\")","v":"B311"},{"$f":"IF(LEN('Translation-EN'!D2153)>0,'Translation-EN'!D2153,\"\")","v":""},"Béton - 35 MPa, 30% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2154)>0,'Translation-EN'!A2154,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2154)>0,'Translation-EN'!B2154,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2154)>0,'Translation-EN'!C2154,\"\")","v":"D311"},{"$f":"IF(LEN('Translation-EN'!D2154)>0,'Translation-EN'!D2154,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2155)>0,'Translation-EN'!A2155,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2155)>0,'Translation-EN'!B2155,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2155)>0,'Translation-EN'!C2155,\"\")","v":"B312"},{"$f":"IF(LEN('Translation-EN'!D2155)>0,'Translation-EN'!D2155,\"\")","v":""},"Béton - 35 MPa, 30% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2156)>0,'Translation-EN'!A2156,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2156)>0,'Translation-EN'!B2156,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2156)>0,'Translation-EN'!C2156,\"\")","v":"D312"},{"$f":"IF(LEN('Translation-EN'!D2156)>0,'Translation-EN'!D2156,\"\")","v":""},{"$f":"$E$2116","v":"Can. Moyenne Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2157)>0,'Translation-EN'!A2157,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2157)>0,'Translation-EN'!B2157,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2157)>0,'Translation-EN'!C2157,\"\")","v":"B313"},{"$f":"IF(LEN('Translation-EN'!D2157)>0,'Translation-EN'!D2157,\"\")","v":""},"Béton - 25 MPa, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2158)>0,'Translation-EN'!A2158,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2158)>0,'Translation-EN'!B2158,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2158)>0,'Translation-EN'!C2158,\"\")","v":"D313"},{"$f":"IF(LEN('Translation-EN'!D2158)>0,'Translation-EN'!D2158,\"\")","v":""},"Can. Moyenne Ontario"]
[{"$f":"IF(LEN('Translation-EN'!A2159)>0,'Translation-EN'!A2159,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2159)>0,'Translation-EN'!B2159,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2159)>0,'Translation-EN'!C2159,\"\")","v":"B314"},{"$f":"IF(LEN('Translation-EN'!D2159)>0,'Translation-EN'!D2159,\"\")","v":""},"Béton - 25 MPa, 15% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2160)>0,'Translation-EN'!A2160,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2160)>0,'Translation-EN'!B2160,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2160)>0,'Translation-EN'!C2160,\"\")","v":"D314"},{"$f":"IF(LEN('Translation-EN'!D2160)>0,'Translation-EN'!D2160,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2161)>0,'Translation-EN'!A2161,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2161)>0,'Translation-EN'!B2161,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2161)>0,'Translation-EN'!C2161,\"\")","v":"B315"},{"$f":"IF(LEN('Translation-EN'!D2161)>0,'Translation-EN'!D2161,\"\")","v":""},"Béton - 25 MPa, 25% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2162)>0,'Translation-EN'!A2162,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2162)>0,'Translation-EN'!B2162,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2162)>0,'Translation-EN'!C2162,\"\")","v":"D315"},{"$f":"IF(LEN('Translation-EN'!D2162)>0,'Translation-EN'!D2162,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2163)>0,'Translation-EN'!A2163,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2163)>0,'Translation-EN'!B2163,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2163)>0,'Translation-EN'!C2163,\"\")","v":"B316"},{"$f":"IF(LEN('Translation-EN'!D2163)>0,'Translation-EN'!D2163,\"\")","v":""},"Béton - 25 MPa, 35% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2164)>0,'Translation-EN'!A2164,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2164)>0,'Translation-EN'!B2164,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2164)>0,'Translation-EN'!C2164,\"\")","v":"D316"},{"$f":"IF(LEN('Translation-EN'!D2164)>0,'Translation-EN'!D2164,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2165)>0,'Translation-EN'!A2165,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2165)>0,'Translation-EN'!B2165,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2165)>0,'Translation-EN'!C2165,\"\")","v":"B317"},{"$f":"IF(LEN('Translation-EN'!D2165)>0,'Translation-EN'!D2165,\"\")","v":""},"Béton - 25 MPa, 50% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2166)>0,'Translation-EN'!A2166,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2166)>0,'Translation-EN'!B2166,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2166)>0,'Translation-EN'!C2166,\"\")","v":"D317"},{"$f":"IF(LEN('Translation-EN'!D2166)>0,'Translation-EN'!D2166,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2167)>0,'Translation-EN'!A2167,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2167)>0,'Translation-EN'!B2167,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2167)>0,'Translation-EN'!C2167,\"\")","v":"B318"},{"$f":"IF(LEN('Translation-EN'!D2167)>0,'Translation-EN'!D2167,\"\")","v":""},"Béton - 30 MPa, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2168)>0,'Translation-EN'!A2168,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2168)>0,'Translation-EN'!B2168,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2168)>0,'Translation-EN'!C2168,\"\")","v":"D318"},{"$f":"IF(LEN('Translation-EN'!D2168)>0,'Translation-EN'!D2168,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2169)>0,'Translation-EN'!A2169,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2169)>0,'Translation-EN'!B2169,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2169)>0,'Translation-EN'!C2169,\"\")","v":"B319"},{"$f":"IF(LEN('Translation-EN'!D2169)>0,'Translation-EN'!D2169,\"\")","v":""},"Béton - 30 MPa, 15% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2170)>0,'Translation-EN'!A2170,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2170)>0,'Translation-EN'!B2170,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2170)>0,'Translation-EN'!C2170,\"\")","v":"D319"},{"$f":"IF(LEN('Translation-EN'!D2170)>0,'Translation-EN'!D2170,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2171)>0,'Translation-EN'!A2171,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2171)>0,'Translation-EN'!B2171,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2171)>0,'Translation-EN'!C2171,\"\")","v":"B320"},{"$f":"IF(LEN('Translation-EN'!D2171)>0,'Translation-EN'!D2171,\"\")","v":""},"Béton - 30 MPa, 25% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2172)>0,'Translation-EN'!A2172,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2172)>0,'Translation-EN'!B2172,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2172)>0,'Translation-EN'!C2172,\"\")","v":"D320"},{"$f":"IF(LEN('Translation-EN'!D2172)>0,'Translation-EN'!D2172,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2173)>0,'Translation-EN'!A2173,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2173)>0,'Translation-EN'!B2173,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2173)>0,'Translation-EN'!C2173,\"\")","v":"B321"},{"$f":"IF(LEN('Translation-EN'!D2173)>0,'Translation-EN'!D2173,\"\")","v":""},"Béton - 30 MPa, 35% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2174)>0,'Translation-EN'!A2174,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2174)>0,'Translation-EN'!B2174,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2174)>0,'Translation-EN'!C2174,\"\")","v":"D321"},{"$f":"IF(LEN('Translation-EN'!D2174)>0,'Translation-EN'!D2174,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2175)>0,'Translation-EN'!A2175,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2175)>0,'Translation-EN'!B2175,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2175)>0,'Translation-EN'!C2175,\"\")","v":"B322"},{"$f":"IF(LEN('Translation-EN'!D2175)>0,'Translation-EN'!D2175,\"\")","v":""},"Béton - 30 MPa, 50% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2176)>0,'Translation-EN'!A2176,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2176)>0,'Translation-EN'!B2176,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2176)>0,'Translation-EN'!C2176,\"\")","v":"D322"},{"$f":"IF(LEN('Translation-EN'!D2176)>0,'Translation-EN'!D2176,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2177)>0,'Translation-EN'!A2177,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2177)>0,'Translation-EN'!B2177,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2177)>0,'Translation-EN'!C2177,\"\")","v":"B323"},{"$f":"IF(LEN('Translation-EN'!D2177)>0,'Translation-EN'!D2177,\"\")","v":""},"Béton - 35 MPa, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2178)>0,'Translation-EN'!A2178,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2178)>0,'Translation-EN'!B2178,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2178)>0,'Translation-EN'!C2178,\"\")","v":"D323"},{"$f":"IF(LEN('Translation-EN'!D2178)>0,'Translation-EN'!D2178,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2179)>0,'Translation-EN'!A2179,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2179)>0,'Translation-EN'!B2179,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2179)>0,'Translation-EN'!C2179,\"\")","v":"B324"},{"$f":"IF(LEN('Translation-EN'!D2179)>0,'Translation-EN'!D2179,\"\")","v":""},"Béton - 35 MPa, 15% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2180)>0,'Translation-EN'!A2180,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2180)>0,'Translation-EN'!B2180,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2180)>0,'Translation-EN'!C2180,\"\")","v":"D324"},{"$f":"IF(LEN('Translation-EN'!D2180)>0,'Translation-EN'!D2180,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2181)>0,'Translation-EN'!A2181,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2181)>0,'Translation-EN'!B2181,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2181)>0,'Translation-EN'!C2181,\"\")","v":"B325"},{"$f":"IF(LEN('Translation-EN'!D2181)>0,'Translation-EN'!D2181,\"\")","v":""},"Béton - 35 MPa, 25% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2182)>0,'Translation-EN'!A2182,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2182)>0,'Translation-EN'!B2182,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2182)>0,'Translation-EN'!C2182,\"\")","v":"D325"},{"$f":"IF(LEN('Translation-EN'!D2182)>0,'Translation-EN'!D2182,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2183)>0,'Translation-EN'!A2183,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2183)>0,'Translation-EN'!B2183,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2183)>0,'Translation-EN'!C2183,\"\")","v":"B326"},{"$f":"IF(LEN('Translation-EN'!D2183)>0,'Translation-EN'!D2183,\"\")","v":""},"Béton - 35 MPa, 35% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2184)>0,'Translation-EN'!A2184,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2184)>0,'Translation-EN'!B2184,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2184)>0,'Translation-EN'!C2184,\"\")","v":"D326"},{"$f":"IF(LEN('Translation-EN'!D2184)>0,'Translation-EN'!D2184,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2185)>0,'Translation-EN'!A2185,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2185)>0,'Translation-EN'!B2185,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2185)>0,'Translation-EN'!C2185,\"\")","v":"B327"},{"$f":"IF(LEN('Translation-EN'!D2185)>0,'Translation-EN'!D2185,\"\")","v":""},"Béton - 35 MPa, 50% SL, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2186)>0,'Translation-EN'!A2186,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2186)>0,'Translation-EN'!B2186,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2186)>0,'Translation-EN'!C2186,\"\")","v":"D327"},{"$f":"IF(LEN('Translation-EN'!D2186)>0,'Translation-EN'!D2186,\"\")","v":""},{"$f":"$E$2158","v":"Can. Moyenne Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2187)>0,'Translation-EN'!A2187,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2187)>0,'Translation-EN'!B2187,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2187)>0,'Translation-EN'!C2187,\"\")","v":"B328"},{"$f":"IF(LEN('Translation-EN'!D2187)>0,'Translation-EN'!D2187,\"\")","v":""},{"$f":"$E$2157","v":"Béton - 25 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2188)>0,'Translation-EN'!A2188,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2188)>0,'Translation-EN'!B2188,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2188)>0,'Translation-EN'!C2188,\"\")","v":"D328"},{"$f":"IF(LEN('Translation-EN'!D2188)>0,'Translation-EN'!D2188,\"\")","v":""},"Can. Moyenne Saskatchewan"]
[{"$f":"IF(LEN('Translation-EN'!A2189)>0,'Translation-EN'!A2189,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2189)>0,'Translation-EN'!B2189,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2189)>0,'Translation-EN'!C2189,\"\")","v":"B329"},{"$f":"IF(LEN('Translation-EN'!D2189)>0,'Translation-EN'!D2189,\"\")","v":""},{"$f":"$E$2119","v":"Béton -  25 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2190)>0,'Translation-EN'!A2190,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2190)>0,'Translation-EN'!B2190,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2190)>0,'Translation-EN'!C2190,\"\")","v":"D329"},{"$f":"IF(LEN('Translation-EN'!D2190)>0,'Translation-EN'!D2190,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2191)>0,'Translation-EN'!A2191,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2191)>0,'Translation-EN'!B2191,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2191)>0,'Translation-EN'!C2191,\"\")","v":"B330"},{"$f":"IF(LEN('Translation-EN'!D2191)>0,'Translation-EN'!D2191,\"\")","v":""},{"$f":"$E$2123","v":"Béton - 25 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2192)>0,'Translation-EN'!A2192,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2192)>0,'Translation-EN'!B2192,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2192)>0,'Translation-EN'!C2192,\"\")","v":"D330"},{"$f":"IF(LEN('Translation-EN'!D2192)>0,'Translation-EN'!D2192,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2193)>0,'Translation-EN'!A2193,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2193)>0,'Translation-EN'!B2193,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2193)>0,'Translation-EN'!C2193,\"\")","v":"B331"},{"$f":"IF(LEN('Translation-EN'!D2193)>0,'Translation-EN'!D2193,\"\")","v":""},{"$f":"$E$2127","v":"Béton - 25 MPa, 30% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2194)>0,'Translation-EN'!A2194,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2194)>0,'Translation-EN'!B2194,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2194)>0,'Translation-EN'!C2194,\"\")","v":"D331"},{"$f":"IF(LEN('Translation-EN'!D2194)>0,'Translation-EN'!D2194,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2195)>0,'Translation-EN'!A2195,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2195)>0,'Translation-EN'!B2195,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2195)>0,'Translation-EN'!C2195,\"\")","v":"B332"},{"$f":"IF(LEN('Translation-EN'!D2195)>0,'Translation-EN'!D2195,\"\")","v":""},"Béton - 25 MPa, 40% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2196)>0,'Translation-EN'!A2196,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2196)>0,'Translation-EN'!B2196,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2196)>0,'Translation-EN'!C2196,\"\")","v":"D332"},{"$f":"IF(LEN('Translation-EN'!D2196)>0,'Translation-EN'!D2196,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2197)>0,'Translation-EN'!A2197,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2197)>0,'Translation-EN'!B2197,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2197)>0,'Translation-EN'!C2197,\"\")","v":"B333"},{"$f":"IF(LEN('Translation-EN'!D2197)>0,'Translation-EN'!D2197,\"\")","v":""},{"$f":"$E$2167","v":"Béton - 30 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2198)>0,'Translation-EN'!A2198,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2198)>0,'Translation-EN'!B2198,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2198)>0,'Translation-EN'!C2198,\"\")","v":"D333"},{"$f":"IF(LEN('Translation-EN'!D2198)>0,'Translation-EN'!D2198,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2199)>0,'Translation-EN'!A2199,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2199)>0,'Translation-EN'!B2199,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2199)>0,'Translation-EN'!C2199,\"\")","v":"B334"},{"$f":"IF(LEN('Translation-EN'!D2199)>0,'Translation-EN'!D2199,\"\")","v":""},{"$f":"$E$2133","v":"Béton -  30 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2200)>0,'Translation-EN'!A2200,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2200)>0,'Translation-EN'!B2200,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2200)>0,'Translation-EN'!C2200,\"\")","v":"D334"},{"$f":"IF(LEN('Translation-EN'!D2200)>0,'Translation-EN'!D2200,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2201)>0,'Translation-EN'!A2201,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2201)>0,'Translation-EN'!B2201,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2201)>0,'Translation-EN'!C2201,\"\")","v":"B335"},{"$f":"IF(LEN('Translation-EN'!D2201)>0,'Translation-EN'!D2201,\"\")","v":""},{"$f":"$E$2137","v":"Béton - 30 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2202)>0,'Translation-EN'!A2202,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2202)>0,'Translation-EN'!B2202,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2202)>0,'Translation-EN'!C2202,\"\")","v":"D335"},{"$f":"IF(LEN('Translation-EN'!D2202)>0,'Translation-EN'!D2202,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2203)>0,'Translation-EN'!A2203,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2203)>0,'Translation-EN'!B2203,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2203)>0,'Translation-EN'!C2203,\"\")","v":"B336"},{"$f":"IF(LEN('Translation-EN'!D2203)>0,'Translation-EN'!D2203,\"\")","v":""},{"$f":"$E$2141","v":"Béton - 30 MPa, 30% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2204)>0,'Translation-EN'!A2204,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2204)>0,'Translation-EN'!B2204,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2204)>0,'Translation-EN'!C2204,\"\")","v":"D336"},{"$f":"IF(LEN('Translation-EN'!D2204)>0,'Translation-EN'!D2204,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2205)>0,'Translation-EN'!A2205,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2205)>0,'Translation-EN'!B2205,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2205)>0,'Translation-EN'!C2205,\"\")","v":"B337"},{"$f":"IF(LEN('Translation-EN'!D2205)>0,'Translation-EN'!D2205,\"\")","v":""},"Béton - 30 MPa, 40% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2206)>0,'Translation-EN'!A2206,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2206)>0,'Translation-EN'!B2206,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2206)>0,'Translation-EN'!C2206,\"\")","v":"D337"},{"$f":"IF(LEN('Translation-EN'!D2206)>0,'Translation-EN'!D2206,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2207)>0,'Translation-EN'!A2207,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2207)>0,'Translation-EN'!B2207,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2207)>0,'Translation-EN'!C2207,\"\")","v":"B338"},{"$f":"IF(LEN('Translation-EN'!D2207)>0,'Translation-EN'!D2207,\"\")","v":""},{"$f":"$E$2177","v":"Béton - 35 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2208)>0,'Translation-EN'!A2208,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2208)>0,'Translation-EN'!B2208,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2208)>0,'Translation-EN'!C2208,\"\")","v":"D338"},{"$f":"IF(LEN('Translation-EN'!D2208)>0,'Translation-EN'!D2208,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2209)>0,'Translation-EN'!A2209,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2209)>0,'Translation-EN'!B2209,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2209)>0,'Translation-EN'!C2209,\"\")","v":"B339"},{"$f":"IF(LEN('Translation-EN'!D2209)>0,'Translation-EN'!D2209,\"\")","v":""},{"$f":"$E$2147","v":"Béton -  35 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2210)>0,'Translation-EN'!A2210,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2210)>0,'Translation-EN'!B2210,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2210)>0,'Translation-EN'!C2210,\"\")","v":"D339"},{"$f":"IF(LEN('Translation-EN'!D2210)>0,'Translation-EN'!D2210,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2211)>0,'Translation-EN'!A2211,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2211)>0,'Translation-EN'!B2211,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2211)>0,'Translation-EN'!C2211,\"\")","v":"B340"},{"$f":"IF(LEN('Translation-EN'!D2211)>0,'Translation-EN'!D2211,\"\")","v":""},{"$f":"$E$2151","v":"Béton - 35 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2212)>0,'Translation-EN'!A2212,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2212)>0,'Translation-EN'!B2212,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2212)>0,'Translation-EN'!C2212,\"\")","v":"D340"},{"$f":"IF(LEN('Translation-EN'!D2212)>0,'Translation-EN'!D2212,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2213)>0,'Translation-EN'!A2213,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2213)>0,'Translation-EN'!B2213,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2213)>0,'Translation-EN'!C2213,\"\")","v":"B341"},{"$f":"IF(LEN('Translation-EN'!D2213)>0,'Translation-EN'!D2213,\"\")","v":""},{"$f":"$E$2155","v":"Béton - 35 MPa, 30% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2214)>0,'Translation-EN'!A2214,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2214)>0,'Translation-EN'!B2214,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2214)>0,'Translation-EN'!C2214,\"\")","v":"D341"},{"$f":"IF(LEN('Translation-EN'!D2214)>0,'Translation-EN'!D2214,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2215)>0,'Translation-EN'!A2215,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2215)>0,'Translation-EN'!B2215,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2215)>0,'Translation-EN'!C2215,\"\")","v":"B342"},{"$f":"IF(LEN('Translation-EN'!D2215)>0,'Translation-EN'!D2215,\"\")","v":""},"Béton - 35 MPa, 40% FA, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2216)>0,'Translation-EN'!A2216,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2216)>0,'Translation-EN'!B2216,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2216)>0,'Translation-EN'!C2216,\"\")","v":"D342"},{"$f":"IF(LEN('Translation-EN'!D2216)>0,'Translation-EN'!D2216,\"\")","v":""},{"$f":"$E$2188","v":"Can. Moyenne Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2217)>0,'Translation-EN'!A2217,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2217)>0,'Translation-EN'!B2217,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2217)>0,'Translation-EN'!C2217,\"\")","v":"B343"},{"$f":"IF(LEN('Translation-EN'!D2217)>0,'Translation-EN'!D2217,\"\")","v":""},{"$f":"$E$2157","v":"Béton - 25 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2218)>0,'Translation-EN'!A2218,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2218)>0,'Translation-EN'!B2218,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2218)>0,'Translation-EN'!C2218,\"\")","v":"D343"},{"$f":"IF(LEN('Translation-EN'!D2218)>0,'Translation-EN'!D2218,\"\")","v":""},"Can. Moyenne Manitoba"]
[{"$f":"IF(LEN('Translation-EN'!A2219)>0,'Translation-EN'!A2219,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2219)>0,'Translation-EN'!B2219,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2219)>0,'Translation-EN'!C2219,\"\")","v":"B344"},{"$f":"IF(LEN('Translation-EN'!D2219)>0,'Translation-EN'!D2219,\"\")","v":""},{"$f":"$E$2119","v":"Béton -  25 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2220)>0,'Translation-EN'!A2220,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2220)>0,'Translation-EN'!B2220,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2220)>0,'Translation-EN'!C2220,\"\")","v":"D344"},{"$f":"IF(LEN('Translation-EN'!D2220)>0,'Translation-EN'!D2220,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2221)>0,'Translation-EN'!A2221,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2221)>0,'Translation-EN'!B2221,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2221)>0,'Translation-EN'!C2221,\"\")","v":"B345"},{"$f":"IF(LEN('Translation-EN'!D2221)>0,'Translation-EN'!D2221,\"\")","v":""},{"$f":"$E$2123","v":"Béton - 25 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2222)>0,'Translation-EN'!A2222,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2222)>0,'Translation-EN'!B2222,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2222)>0,'Translation-EN'!C2222,\"\")","v":"D345"},{"$f":"IF(LEN('Translation-EN'!D2222)>0,'Translation-EN'!D2222,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2223)>0,'Translation-EN'!A2223,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2223)>0,'Translation-EN'!B2223,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2223)>0,'Translation-EN'!C2223,\"\")","v":"B346"},{"$f":"IF(LEN('Translation-EN'!D2223)>0,'Translation-EN'!D2223,\"\")","v":""},{"$f":"$E$2127","v":"Béton - 25 MPa, 30% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2224)>0,'Translation-EN'!A2224,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2224)>0,'Translation-EN'!B2224,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2224)>0,'Translation-EN'!C2224,\"\")","v":"D346"},{"$f":"IF(LEN('Translation-EN'!D2224)>0,'Translation-EN'!D2224,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2225)>0,'Translation-EN'!A2225,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2225)>0,'Translation-EN'!B2225,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2225)>0,'Translation-EN'!C2225,\"\")","v":"B347"},{"$f":"IF(LEN('Translation-EN'!D2225)>0,'Translation-EN'!D2225,\"\")","v":""},{"$f":"$E$2195","v":"Béton - 25 MPa, 40% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2226)>0,'Translation-EN'!A2226,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2226)>0,'Translation-EN'!B2226,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2226)>0,'Translation-EN'!C2226,\"\")","v":"D347"},{"$f":"IF(LEN('Translation-EN'!D2226)>0,'Translation-EN'!D2226,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2227)>0,'Translation-EN'!A2227,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2227)>0,'Translation-EN'!B2227,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2227)>0,'Translation-EN'!C2227,\"\")","v":"B348"},{"$f":"IF(LEN('Translation-EN'!D2227)>0,'Translation-EN'!D2227,\"\")","v":""},{"$f":"$E$2167","v":"Béton - 30 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2228)>0,'Translation-EN'!A2228,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2228)>0,'Translation-EN'!B2228,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2228)>0,'Translation-EN'!C2228,\"\")","v":"D348"},{"$f":"IF(LEN('Translation-EN'!D2228)>0,'Translation-EN'!D2228,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2229)>0,'Translation-EN'!A2229,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2229)>0,'Translation-EN'!B2229,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2229)>0,'Translation-EN'!C2229,\"\")","v":"B349"},{"$f":"IF(LEN('Translation-EN'!D2229)>0,'Translation-EN'!D2229,\"\")","v":""},{"$f":"$E$2133","v":"Béton -  30 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2230)>0,'Translation-EN'!A2230,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2230)>0,'Translation-EN'!B2230,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2230)>0,'Translation-EN'!C2230,\"\")","v":"D349"},{"$f":"IF(LEN('Translation-EN'!D2230)>0,'Translation-EN'!D2230,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2231)>0,'Translation-EN'!A2231,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2231)>0,'Translation-EN'!B2231,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2231)>0,'Translation-EN'!C2231,\"\")","v":"B350"},{"$f":"IF(LEN('Translation-EN'!D2231)>0,'Translation-EN'!D2231,\"\")","v":""},{"$f":"$E$2137","v":"Béton - 30 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2232)>0,'Translation-EN'!A2232,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2232)>0,'Translation-EN'!B2232,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2232)>0,'Translation-EN'!C2232,\"\")","v":"D350"},{"$f":"IF(LEN('Translation-EN'!D2232)>0,'Translation-EN'!D2232,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2233)>0,'Translation-EN'!A2233,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2233)>0,'Translation-EN'!B2233,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2233)>0,'Translation-EN'!C2233,\"\")","v":"B351"},{"$f":"IF(LEN('Translation-EN'!D2233)>0,'Translation-EN'!D2233,\"\")","v":""},{"$f":"$E$2141","v":"Béton - 30 MPa, 30% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2234)>0,'Translation-EN'!A2234,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2234)>0,'Translation-EN'!B2234,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2234)>0,'Translation-EN'!C2234,\"\")","v":"D351"},{"$f":"IF(LEN('Translation-EN'!D2234)>0,'Translation-EN'!D2234,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2235)>0,'Translation-EN'!A2235,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2235)>0,'Translation-EN'!B2235,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2235)>0,'Translation-EN'!C2235,\"\")","v":"B352"},{"$f":"IF(LEN('Translation-EN'!D2235)>0,'Translation-EN'!D2235,\"\")","v":""},{"$f":"$E$2205","v":"Béton - 30 MPa, 40% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2236)>0,'Translation-EN'!A2236,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2236)>0,'Translation-EN'!B2236,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2236)>0,'Translation-EN'!C2236,\"\")","v":"D352"},{"$f":"IF(LEN('Translation-EN'!D2236)>0,'Translation-EN'!D2236,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2237)>0,'Translation-EN'!A2237,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2237)>0,'Translation-EN'!B2237,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2237)>0,'Translation-EN'!C2237,\"\")","v":"B353"},{"$f":"IF(LEN('Translation-EN'!D2237)>0,'Translation-EN'!D2237,\"\")","v":""},{"$f":"$E$2177","v":"Béton - 35 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2238)>0,'Translation-EN'!A2238,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2238)>0,'Translation-EN'!B2238,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2238)>0,'Translation-EN'!C2238,\"\")","v":"D353"},{"$f":"IF(LEN('Translation-EN'!D2238)>0,'Translation-EN'!D2238,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2239)>0,'Translation-EN'!A2239,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2239)>0,'Translation-EN'!B2239,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2239)>0,'Translation-EN'!C2239,\"\")","v":"B354"},{"$f":"IF(LEN('Translation-EN'!D2239)>0,'Translation-EN'!D2239,\"\")","v":""},{"$f":"$E$2147","v":"Béton -  35 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2240)>0,'Translation-EN'!A2240,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2240)>0,'Translation-EN'!B2240,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2240)>0,'Translation-EN'!C2240,\"\")","v":"D354"},{"$f":"IF(LEN('Translation-EN'!D2240)>0,'Translation-EN'!D2240,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2241)>0,'Translation-EN'!A2241,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2241)>0,'Translation-EN'!B2241,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2241)>0,'Translation-EN'!C2241,\"\")","v":"B355"},{"$f":"IF(LEN('Translation-EN'!D2241)>0,'Translation-EN'!D2241,\"\")","v":""},{"$f":"$E$2151","v":"Béton - 35 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2242)>0,'Translation-EN'!A2242,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2242)>0,'Translation-EN'!B2242,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2242)>0,'Translation-EN'!C2242,\"\")","v":"D355"},{"$f":"IF(LEN('Translation-EN'!D2242)>0,'Translation-EN'!D2242,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2243)>0,'Translation-EN'!A2243,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2243)>0,'Translation-EN'!B2243,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2243)>0,'Translation-EN'!C2243,\"\")","v":"B356"},{"$f":"IF(LEN('Translation-EN'!D2243)>0,'Translation-EN'!D2243,\"\")","v":""},{"$f":"$E$2155","v":"Béton - 35 MPa, 30% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2244)>0,'Translation-EN'!A2244,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2244)>0,'Translation-EN'!B2244,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2244)>0,'Translation-EN'!C2244,\"\")","v":"D356"},{"$f":"IF(LEN('Translation-EN'!D2244)>0,'Translation-EN'!D2244,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2245)>0,'Translation-EN'!A2245,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2245)>0,'Translation-EN'!B2245,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2245)>0,'Translation-EN'!C2245,\"\")","v":"B357"},{"$f":"IF(LEN('Translation-EN'!D2245)>0,'Translation-EN'!D2245,\"\")","v":""},{"$f":"$E$2215","v":"Béton - 35 MPa, 40% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2246)>0,'Translation-EN'!A2246,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2246)>0,'Translation-EN'!B2246,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2246)>0,'Translation-EN'!C2246,\"\")","v":"D357"},{"$f":"IF(LEN('Translation-EN'!D2246)>0,'Translation-EN'!D2246,\"\")","v":""},{"$f":"$E$2218","v":"Can. Moyenne Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2247)>0,'Translation-EN'!A2247,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2247)>0,'Translation-EN'!B2247,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2247)>0,'Translation-EN'!C2247,\"\")","v":"B358"},{"$f":"IF(LEN('Translation-EN'!D2247)>0,'Translation-EN'!D2247,\"\")","v":""},{"$f":"$E$2157","v":"Béton - 25 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2248)>0,'Translation-EN'!A2248,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2248)>0,'Translation-EN'!B2248,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2248)>0,'Translation-EN'!C2248,\"\")","v":"D358"},{"$f":"IF(LEN('Translation-EN'!D2248)>0,'Translation-EN'!D2248,\"\")","v":""},"Can. Moyenne Colombie Britanique"]
[{"$f":"IF(LEN('Translation-EN'!A2249)>0,'Translation-EN'!A2249,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2249)>0,'Translation-EN'!B2249,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2249)>0,'Translation-EN'!C2249,\"\")","v":"B359"},{"$f":"IF(LEN('Translation-EN'!D2249)>0,'Translation-EN'!D2249,\"\")","v":""},"Béton - 25 MPa, 15% SCM, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2250)>0,'Translation-EN'!A2250,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2250)>0,'Translation-EN'!B2250,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2250)>0,'Translation-EN'!C2250,\"\")","v":"D359"},{"$f":"IF(LEN('Translation-EN'!D2250)>0,'Translation-EN'!D2250,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2251)>0,'Translation-EN'!A2251,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2251)>0,'Translation-EN'!B2251,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2251)>0,'Translation-EN'!C2251,\"\")","v":"B360"},{"$f":"IF(LEN('Translation-EN'!D2251)>0,'Translation-EN'!D2251,\"\")","v":""},"Béton - 25 MPa, 25% SCM, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2252)>0,'Translation-EN'!A2252,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2252)>0,'Translation-EN'!B2252,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2252)>0,'Translation-EN'!C2252,\"\")","v":"D360"},{"$f":"IF(LEN('Translation-EN'!D2252)>0,'Translation-EN'!D2252,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2253)>0,'Translation-EN'!A2253,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2253)>0,'Translation-EN'!B2253,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2253)>0,'Translation-EN'!C2253,\"\")","v":"B361"},{"$f":"IF(LEN('Translation-EN'!D2253)>0,'Translation-EN'!D2253,\"\")","v":""},"Béton - 25 MPa, 40% SCM, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2254)>0,'Translation-EN'!A2254,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2254)>0,'Translation-EN'!B2254,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2254)>0,'Translation-EN'!C2254,\"\")","v":"D361"},{"$f":"IF(LEN('Translation-EN'!D2254)>0,'Translation-EN'!D2254,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2255)>0,'Translation-EN'!A2255,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2255)>0,'Translation-EN'!B2255,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2255)>0,'Translation-EN'!C2255,\"\")","v":"B362"},{"$f":"IF(LEN('Translation-EN'!D2255)>0,'Translation-EN'!D2255,\"\")","v":""},{"$f":"$E$2167","v":"Béton - 30 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2256)>0,'Translation-EN'!A2256,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2256)>0,'Translation-EN'!B2256,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2256)>0,'Translation-EN'!C2256,\"\")","v":"D362"},{"$f":"IF(LEN('Translation-EN'!D2256)>0,'Translation-EN'!D2256,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2257)>0,'Translation-EN'!A2257,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2257)>0,'Translation-EN'!B2257,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2257)>0,'Translation-EN'!C2257,\"\")","v":"B363"},{"$f":"IF(LEN('Translation-EN'!D2257)>0,'Translation-EN'!D2257,\"\")","v":""},"Béton - 30 MPa, 15% SCM, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2258)>0,'Translation-EN'!A2258,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2258)>0,'Translation-EN'!B2258,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2258)>0,'Translation-EN'!C2258,\"\")","v":"D363"},{"$f":"IF(LEN('Translation-EN'!D2258)>0,'Translation-EN'!D2258,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2259)>0,'Translation-EN'!A2259,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2259)>0,'Translation-EN'!B2259,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2259)>0,'Translation-EN'!C2259,\"\")","v":"B364"},{"$f":"IF(LEN('Translation-EN'!D2259)>0,'Translation-EN'!D2259,\"\")","v":""},"Béton - 30 MPa, 25% SCM, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2260)>0,'Translation-EN'!A2260,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2260)>0,'Translation-EN'!B2260,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2260)>0,'Translation-EN'!C2260,\"\")","v":"D364"},{"$f":"IF(LEN('Translation-EN'!D2260)>0,'Translation-EN'!D2260,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2261)>0,'Translation-EN'!A2261,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2261)>0,'Translation-EN'!B2261,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2261)>0,'Translation-EN'!C2261,\"\")","v":"B365"},{"$f":"IF(LEN('Translation-EN'!D2261)>0,'Translation-EN'!D2261,\"\")","v":""},"Béton - 30 MPa, 40% SCM, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2262)>0,'Translation-EN'!A2262,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2262)>0,'Translation-EN'!B2262,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2262)>0,'Translation-EN'!C2262,\"\")","v":"D365"},{"$f":"IF(LEN('Translation-EN'!D2262)>0,'Translation-EN'!D2262,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2263)>0,'Translation-EN'!A2263,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2263)>0,'Translation-EN'!B2263,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2263)>0,'Translation-EN'!C2263,\"\")","v":"B366"},{"$f":"IF(LEN('Translation-EN'!D2263)>0,'Translation-EN'!D2263,\"\")","v":""},{"$f":"$E$2177","v":"Béton - 35 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2264)>0,'Translation-EN'!A2264,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2264)>0,'Translation-EN'!B2264,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2264)>0,'Translation-EN'!C2264,\"\")","v":"D366"},{"$f":"IF(LEN('Translation-EN'!D2264)>0,'Translation-EN'!D2264,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2265)>0,'Translation-EN'!A2265,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2265)>0,'Translation-EN'!B2265,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2265)>0,'Translation-EN'!C2265,\"\")","v":"B367"},{"$f":"IF(LEN('Translation-EN'!D2265)>0,'Translation-EN'!D2265,\"\")","v":""},"Béton - 35 MPa, 15% SCM, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2266)>0,'Translation-EN'!A2266,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2266)>0,'Translation-EN'!B2266,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2266)>0,'Translation-EN'!C2266,\"\")","v":"D367"},{"$f":"IF(LEN('Translation-EN'!D2266)>0,'Translation-EN'!D2266,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2267)>0,'Translation-EN'!A2267,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2267)>0,'Translation-EN'!B2267,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2267)>0,'Translation-EN'!C2267,\"\")","v":"B368"},{"$f":"IF(LEN('Translation-EN'!D2267)>0,'Translation-EN'!D2267,\"\")","v":""},"Béton - 35 MPa, 25% SCM, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2268)>0,'Translation-EN'!A2268,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2268)>0,'Translation-EN'!B2268,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2268)>0,'Translation-EN'!C2268,\"\")","v":"D368"},{"$f":"IF(LEN('Translation-EN'!D2268)>0,'Translation-EN'!D2268,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2269)>0,'Translation-EN'!A2269,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2269)>0,'Translation-EN'!B2269,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2269)>0,'Translation-EN'!C2269,\"\")","v":"B369"},{"$f":"IF(LEN('Translation-EN'!D2269)>0,'Translation-EN'!D2269,\"\")","v":""},"Béton - 35 MPa, 40% SCM, GU"]
[{"$f":"IF(LEN('Translation-EN'!A2270)>0,'Translation-EN'!A2270,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2270)>0,'Translation-EN'!B2270,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2270)>0,'Translation-EN'!C2270,\"\")","v":"D369"},{"$f":"IF(LEN('Translation-EN'!D2270)>0,'Translation-EN'!D2270,\"\")","v":""},{"$f":"$E$2248","v":"Can. Moyenne Colombie Britanique"}]
[{"$f":"IF(LEN('Translation-EN'!A2271)>0,'Translation-EN'!A2271,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2271)>0,'Translation-EN'!B2271,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2271)>0,'Translation-EN'!C2271,\"\")","v":"B370"},{"$f":"IF(LEN('Translation-EN'!D2271)>0,'Translation-EN'!D2271,\"\")","v":""},{"$f":"$E$2157","v":"Béton - 25 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2272)>0,'Translation-EN'!A2272,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2272)>0,'Translation-EN'!B2272,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2272)>0,'Translation-EN'!C2272,\"\")","v":"D370"},{"$f":"IF(LEN('Translation-EN'!D2272)>0,'Translation-EN'!D2272,\"\")","v":""},"Can. Moyenne prov. Atlantique"]
[{"$f":"IF(LEN('Translation-EN'!A2273)>0,'Translation-EN'!A2273,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2273)>0,'Translation-EN'!B2273,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2273)>0,'Translation-EN'!C2273,\"\")","v":"B371"},{"$f":"IF(LEN('Translation-EN'!D2273)>0,'Translation-EN'!D2273,\"\")","v":""},{"$f":"$E$2119","v":"Béton -  25 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2274)>0,'Translation-EN'!A2274,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2274)>0,'Translation-EN'!B2274,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2274)>0,'Translation-EN'!C2274,\"\")","v":"D371"},{"$f":"IF(LEN('Translation-EN'!D2274)>0,'Translation-EN'!D2274,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2275)>0,'Translation-EN'!A2275,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2275)>0,'Translation-EN'!B2275,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2275)>0,'Translation-EN'!C2275,\"\")","v":"B372"},{"$f":"IF(LEN('Translation-EN'!D2275)>0,'Translation-EN'!D2275,\"\")","v":""},{"$f":"$E$2123","v":"Béton - 25 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2276)>0,'Translation-EN'!A2276,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2276)>0,'Translation-EN'!B2276,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2276)>0,'Translation-EN'!C2276,\"\")","v":"D372"},{"$f":"IF(LEN('Translation-EN'!D2276)>0,'Translation-EN'!D2276,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2277)>0,'Translation-EN'!A2277,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2277)>0,'Translation-EN'!B2277,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2277)>0,'Translation-EN'!C2277,\"\")","v":"B373"},{"$f":"IF(LEN('Translation-EN'!D2277)>0,'Translation-EN'!D2277,\"\")","v":""},{"$f":"$E$2127","v":"Béton - 25 MPa, 30% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2278)>0,'Translation-EN'!A2278,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2278)>0,'Translation-EN'!B2278,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2278)>0,'Translation-EN'!C2278,\"\")","v":"D373"},{"$f":"IF(LEN('Translation-EN'!D2278)>0,'Translation-EN'!D2278,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2279)>0,'Translation-EN'!A2279,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2279)>0,'Translation-EN'!B2279,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2279)>0,'Translation-EN'!C2279,\"\")","v":"B374"},{"$f":"IF(LEN('Translation-EN'!D2279)>0,'Translation-EN'!D2279,\"\")","v":""},{"$f":"$E$2195","v":"Béton - 25 MPa, 40% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2280)>0,'Translation-EN'!A2280,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2280)>0,'Translation-EN'!B2280,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2280)>0,'Translation-EN'!C2280,\"\")","v":"D374"},{"$f":"IF(LEN('Translation-EN'!D2280)>0,'Translation-EN'!D2280,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2281)>0,'Translation-EN'!A2281,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2281)>0,'Translation-EN'!B2281,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2281)>0,'Translation-EN'!C2281,\"\")","v":"B375"},{"$f":"IF(LEN('Translation-EN'!D2281)>0,'Translation-EN'!D2281,\"\")","v":""},{"$f":"$E$2167","v":"Béton - 30 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2282)>0,'Translation-EN'!A2282,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2282)>0,'Translation-EN'!B2282,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2282)>0,'Translation-EN'!C2282,\"\")","v":"D375"},{"$f":"IF(LEN('Translation-EN'!D2282)>0,'Translation-EN'!D2282,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2283)>0,'Translation-EN'!A2283,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2283)>0,'Translation-EN'!B2283,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2283)>0,'Translation-EN'!C2283,\"\")","v":"B376"},{"$f":"IF(LEN('Translation-EN'!D2283)>0,'Translation-EN'!D2283,\"\")","v":""},{"$f":"$E$2133","v":"Béton -  30 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2284)>0,'Translation-EN'!A2284,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2284)>0,'Translation-EN'!B2284,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2284)>0,'Translation-EN'!C2284,\"\")","v":"D376"},{"$f":"IF(LEN('Translation-EN'!D2284)>0,'Translation-EN'!D2284,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2285)>0,'Translation-EN'!A2285,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2285)>0,'Translation-EN'!B2285,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2285)>0,'Translation-EN'!C2285,\"\")","v":"B377"},{"$f":"IF(LEN('Translation-EN'!D2285)>0,'Translation-EN'!D2285,\"\")","v":""},{"$f":"$E$2137","v":"Béton - 30 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2286)>0,'Translation-EN'!A2286,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2286)>0,'Translation-EN'!B2286,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2286)>0,'Translation-EN'!C2286,\"\")","v":"D377"},{"$f":"IF(LEN('Translation-EN'!D2286)>0,'Translation-EN'!D2286,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2287)>0,'Translation-EN'!A2287,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2287)>0,'Translation-EN'!B2287,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2287)>0,'Translation-EN'!C2287,\"\")","v":"B378"},{"$f":"IF(LEN('Translation-EN'!D2287)>0,'Translation-EN'!D2287,\"\")","v":""},{"$f":"$E$2141","v":"Béton - 30 MPa, 30% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2288)>0,'Translation-EN'!A2288,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2288)>0,'Translation-EN'!B2288,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2288)>0,'Translation-EN'!C2288,\"\")","v":"D378"},{"$f":"IF(LEN('Translation-EN'!D2288)>0,'Translation-EN'!D2288,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2289)>0,'Translation-EN'!A2289,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2289)>0,'Translation-EN'!B2289,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2289)>0,'Translation-EN'!C2289,\"\")","v":"B379"},{"$f":"IF(LEN('Translation-EN'!D2289)>0,'Translation-EN'!D2289,\"\")","v":""},{"$f":"$E$2205","v":"Béton - 30 MPa, 40% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2290)>0,'Translation-EN'!A2290,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2290)>0,'Translation-EN'!B2290,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2290)>0,'Translation-EN'!C2290,\"\")","v":"D379"},{"$f":"IF(LEN('Translation-EN'!D2290)>0,'Translation-EN'!D2290,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2291)>0,'Translation-EN'!A2291,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2291)>0,'Translation-EN'!B2291,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2291)>0,'Translation-EN'!C2291,\"\")","v":"B380"},{"$f":"IF(LEN('Translation-EN'!D2291)>0,'Translation-EN'!D2291,\"\")","v":""},{"$f":"$E$2177","v":"Béton - 35 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2292)>0,'Translation-EN'!A2292,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2292)>0,'Translation-EN'!B2292,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2292)>0,'Translation-EN'!C2292,\"\")","v":"D380"},{"$f":"IF(LEN('Translation-EN'!D2292)>0,'Translation-EN'!D2292,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2293)>0,'Translation-EN'!A2293,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2293)>0,'Translation-EN'!B2293,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2293)>0,'Translation-EN'!C2293,\"\")","v":"B381"},{"$f":"IF(LEN('Translation-EN'!D2293)>0,'Translation-EN'!D2293,\"\")","v":""},{"$f":"$E$2147","v":"Béton -  35 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2294)>0,'Translation-EN'!A2294,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2294)>0,'Translation-EN'!B2294,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2294)>0,'Translation-EN'!C2294,\"\")","v":"D381"},{"$f":"IF(LEN('Translation-EN'!D2294)>0,'Translation-EN'!D2294,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2295)>0,'Translation-EN'!A2295,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2295)>0,'Translation-EN'!B2295,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2295)>0,'Translation-EN'!C2295,\"\")","v":"B382"},{"$f":"IF(LEN('Translation-EN'!D2295)>0,'Translation-EN'!D2295,\"\")","v":""},{"$f":"$E$2151","v":"Béton - 35 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2296)>0,'Translation-EN'!A2296,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2296)>0,'Translation-EN'!B2296,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2296)>0,'Translation-EN'!C2296,\"\")","v":"D382"},{"$f":"IF(LEN('Translation-EN'!D2296)>0,'Translation-EN'!D2296,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2297)>0,'Translation-EN'!A2297,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2297)>0,'Translation-EN'!B2297,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2297)>0,'Translation-EN'!C2297,\"\")","v":"B383"},{"$f":"IF(LEN('Translation-EN'!D2297)>0,'Translation-EN'!D2297,\"\")","v":""},{"$f":"$E$2155","v":"Béton - 35 MPa, 30% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2298)>0,'Translation-EN'!A2298,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2298)>0,'Translation-EN'!B2298,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2298)>0,'Translation-EN'!C2298,\"\")","v":"D383"},{"$f":"IF(LEN('Translation-EN'!D2298)>0,'Translation-EN'!D2298,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2299)>0,'Translation-EN'!A2299,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2299)>0,'Translation-EN'!B2299,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2299)>0,'Translation-EN'!C2299,\"\")","v":"B384"},{"$f":"IF(LEN('Translation-EN'!D2299)>0,'Translation-EN'!D2299,\"\")","v":""},{"$f":"$E$2215","v":"Béton - 35 MPa, 40% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2300)>0,'Translation-EN'!A2300,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2300)>0,'Translation-EN'!B2300,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2300)>0,'Translation-EN'!C2300,\"\")","v":"D384"},{"$f":"IF(LEN('Translation-EN'!D2300)>0,'Translation-EN'!D2300,\"\")","v":""},{"$f":"$E$2272","v":"Can. Moyenne prov. Atlantique"}]
[{"$f":"IF(LEN('Translation-EN'!A2301)>0,'Translation-EN'!A2301,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2301)>0,'Translation-EN'!B2301,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2301)>0,'Translation-EN'!C2301,\"\")","v":"B385"},{"$f":"IF(LEN('Translation-EN'!D2301)>0,'Translation-EN'!D2301,\"\")","v":""},{"$f":"$E$2157","v":"Béton - 25 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2302)>0,'Translation-EN'!A2302,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2302)>0,'Translation-EN'!B2302,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2302)>0,'Translation-EN'!C2302,\"\")","v":"D385"},{"$f":"IF(LEN('Translation-EN'!D2302)>0,'Translation-EN'!D2302,\"\")","v":""},"Can. Moyenne Alberta"]
[{"$f":"IF(LEN('Translation-EN'!A2303)>0,'Translation-EN'!A2303,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2303)>0,'Translation-EN'!B2303,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2303)>0,'Translation-EN'!C2303,\"\")","v":"B386"},{"$f":"IF(LEN('Translation-EN'!D2303)>0,'Translation-EN'!D2303,\"\")","v":""},{"$f":"$E$2119","v":"Béton -  25 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2304)>0,'Translation-EN'!A2304,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2304)>0,'Translation-EN'!B2304,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2304)>0,'Translation-EN'!C2304,\"\")","v":"D386"},{"$f":"IF(LEN('Translation-EN'!D2304)>0,'Translation-EN'!D2304,\"\")","v":""},{"$f":"$E$2302","v":"Can. Moyenne Alberta"}]
[{"$f":"IF(LEN('Translation-EN'!A2305)>0,'Translation-EN'!A2305,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2305)>0,'Translation-EN'!B2305,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2305)>0,'Translation-EN'!C2305,\"\")","v":"B387"},{"$f":"IF(LEN('Translation-EN'!D2305)>0,'Translation-EN'!D2305,\"\")","v":""},{"$f":"$E$2123","v":"Béton - 25 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2306)>0,'Translation-EN'!A2306,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2306)>0,'Translation-EN'!B2306,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2306)>0,'Translation-EN'!C2306,\"\")","v":"D387"},{"$f":"IF(LEN('Translation-EN'!D2306)>0,'Translation-EN'!D2306,\"\")","v":""},{"$f":"$E$2302","v":"Can. Moyenne Alberta"}]
[{"$f":"IF(LEN('Translation-EN'!A2307)>0,'Translation-EN'!A2307,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2307)>0,'Translation-EN'!B2307,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2307)>0,'Translation-EN'!C2307,\"\")","v":"B388"},{"$f":"IF(LEN('Translation-EN'!D2307)>0,'Translation-EN'!D2307,\"\")","v":""},{"$f":"$E$2167","v":"Béton - 30 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2308)>0,'Translation-EN'!A2308,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2308)>0,'Translation-EN'!B2308,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2308)>0,'Translation-EN'!C2308,\"\")","v":"D388"},{"$f":"IF(LEN('Translation-EN'!D2308)>0,'Translation-EN'!D2308,\"\")","v":""},{"$f":"$E$2302","v":"Can. Moyenne Alberta"}]
[{"$f":"IF(LEN('Translation-EN'!A2309)>0,'Translation-EN'!A2309,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2309)>0,'Translation-EN'!B2309,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2309)>0,'Translation-EN'!C2309,\"\")","v":"B389"},{"$f":"IF(LEN('Translation-EN'!D2309)>0,'Translation-EN'!D2309,\"\")","v":""},{"$f":"$E$2133","v":"Béton -  30 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2310)>0,'Translation-EN'!A2310,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2310)>0,'Translation-EN'!B2310,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2310)>0,'Translation-EN'!C2310,\"\")","v":"D389"},{"$f":"IF(LEN('Translation-EN'!D2310)>0,'Translation-EN'!D2310,\"\")","v":""},{"$f":"$E$2302","v":"Can. Moyenne Alberta"}]
[{"$f":"IF(LEN('Translation-EN'!A2311)>0,'Translation-EN'!A2311,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2311)>0,'Translation-EN'!B2311,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2311)>0,'Translation-EN'!C2311,\"\")","v":"B390"},{"$f":"IF(LEN('Translation-EN'!D2311)>0,'Translation-EN'!D2311,\"\")","v":""},{"$f":"$E$2137","v":"Béton - 30 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2312)>0,'Translation-EN'!A2312,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2312)>0,'Translation-EN'!B2312,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2312)>0,'Translation-EN'!C2312,\"\")","v":"D390"},{"$f":"IF(LEN('Translation-EN'!D2312)>0,'Translation-EN'!D2312,\"\")","v":""},{"$f":"$E$2302","v":"Can. Moyenne Alberta"}]
[{"$f":"IF(LEN('Translation-EN'!A2313)>0,'Translation-EN'!A2313,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2313)>0,'Translation-EN'!B2313,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2313)>0,'Translation-EN'!C2313,\"\")","v":"B391"},{"$f":"IF(LEN('Translation-EN'!D2313)>0,'Translation-EN'!D2313,\"\")","v":""},{"$f":"$E$2177","v":"Béton - 35 MPa, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2314)>0,'Translation-EN'!A2314,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2314)>0,'Translation-EN'!B2314,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2314)>0,'Translation-EN'!C2314,\"\")","v":"D391"},{"$f":"IF(LEN('Translation-EN'!D2314)>0,'Translation-EN'!D2314,\"\")","v":""},{"$f":"$E$2302","v":"Can. Moyenne Alberta"}]
[{"$f":"IF(LEN('Translation-EN'!A2315)>0,'Translation-EN'!A2315,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2315)>0,'Translation-EN'!B2315,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2315)>0,'Translation-EN'!C2315,\"\")","v":"B392"},{"$f":"IF(LEN('Translation-EN'!D2315)>0,'Translation-EN'!D2315,\"\")","v":""},{"$f":"$E$2147","v":"Béton -  35 MPa, 10% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2316)>0,'Translation-EN'!A2316,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2316)>0,'Translation-EN'!B2316,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2316)>0,'Translation-EN'!C2316,\"\")","v":"D392"},{"$f":"IF(LEN('Translation-EN'!D2316)>0,'Translation-EN'!D2316,\"\")","v":""},{"$f":"$E$2302","v":"Can. Moyenne Alberta"}]
[{"$f":"IF(LEN('Translation-EN'!A2317)>0,'Translation-EN'!A2317,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2317)>0,'Translation-EN'!B2317,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2317)>0,'Translation-EN'!C2317,\"\")","v":"B393"},{"$f":"IF(LEN('Translation-EN'!D2317)>0,'Translation-EN'!D2317,\"\")","v":""},{"$f":"$E$2151","v":"Béton - 35 MPa, 20% FA, GU"}]
[{"$f":"IF(LEN('Translation-EN'!A2318)>0,'Translation-EN'!A2318,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2318)>0,'Translation-EN'!B2318,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2318)>0,'Translation-EN'!C2318,\"\")","v":"D393"},{"$f":"IF(LEN('Translation-EN'!D2318)>0,'Translation-EN'!D2318,\"\")","v":""},{"$f":"$E$2302","v":"Can. Moyenne Alberta"}]
[{"$f":"IF(LEN('Translation-EN'!A2319)>0,'Translation-EN'!A2319,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2319)>0,'Translation-EN'!B2319,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2319)>0,'Translation-EN'!C2319,\"\")","v":"B394"},{"$f":"IF(LEN('Translation-EN'!D2319)>0,'Translation-EN'!D2319,\"\")","v":""},{"$f":"$E$1970","v":"Revêtement de plancher en vinyle"}]
[{"$f":"IF(LEN('Translation-EN'!A2320)>0,'Translation-EN'!A2320,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2320)>0,'Translation-EN'!B2320,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2320)>0,'Translation-EN'!C2320,\"\")","v":"D394"},{"$f":"IF(LEN('Translation-EN'!D2320)>0,'Translation-EN'!D2320,\"\")","v":""},"Carreau de vinyle de luxe"]
[{"$f":"IF(LEN('Translation-EN'!A2321)>0,'Translation-EN'!A2321,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2321)>0,'Translation-EN'!B2321,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2321)>0,'Translation-EN'!C2321,\"\")","v":"B395"},{"$f":"IF(LEN('Translation-EN'!D2321)>0,'Translation-EN'!D2321,\"\")","v":""},{"$f":"$E$1684","v":"Revêtement de plancher en linoléum"}]
[{"$f":"IF(LEN('Translation-EN'!A2322)>0,'Translation-EN'!A2322,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2322)>0,'Translation-EN'!B2322,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2322)>0,'Translation-EN'!C2322,\"\")","v":"D395"},{"$f":"IF(LEN('Translation-EN'!D2322)>0,'Translation-EN'!D2322,\"\")","v":""},"Linoleum Compact DLW"]
[{"$f":"IF(LEN('Translation-EN'!A2323)>0,'Translation-EN'!A2323,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2323)>0,'Translation-EN'!B2323,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2323)>0,'Translation-EN'!C2323,\"\")","v":"E395"},{"$f":"IF(LEN('Translation-EN'!D2323)>0,'Translation-EN'!D2323,\"\")","v":""},{"$f":"$E$1687","v":"linoléum en feuille de 2,5 mm"}]
[{"$f":"IF(LEN('Translation-EN'!A2324)>0,'Translation-EN'!A2324,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2324)>0,'Translation-EN'!B2324,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2324)>0,'Translation-EN'!C2324,\"\")","v":"B396"},{"$f":"IF(LEN('Translation-EN'!D2324)>0,'Translation-EN'!D2324,\"\")","v":""},{"$f":"$E$1596","v":"Fibre de verre en vrac"}]
[{"$f":"IF(LEN('Translation-EN'!A2325)>0,'Translation-EN'!A2325,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2325)>0,'Translation-EN'!B2325,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2325)>0,'Translation-EN'!C2325,\"\")","v":"D396"},{"$f":"IF(LEN('Translation-EN'!D2325)>0,'Translation-EN'!D2325,\"\")","v":""},"Climate Pro, Protecteur de grenier, JM Spider PLUS (Canada)"]
[{"$f":"IF(LEN('Translation-EN'!A2326)>0,'Translation-EN'!A2326,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2326)>0,'Translation-EN'!B2326,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2326)>0,'Translation-EN'!C2326,\"\")","v":"E396"},{"$f":"IF(LEN('Translation-EN'!D2326)>0,'Translation-EN'!D2326,\"\")","v":""},"R 2,8/po, sans Formaldehyde"]
[{"$f":"IF(LEN('Translation-EN'!A2327)>0,'Translation-EN'!A2327,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2327)>0,'Translation-EN'!B2327,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2327)>0,'Translation-EN'!C2327,\"\")","v":"B397"},{"$f":"IF(LEN('Translation-EN'!D2327)>0,'Translation-EN'!D2327,\"\")","v":""},{"$f":"$E$1992","v":"Fenêtre – sous-fenêtre double"}]
[{"$f":"IF(LEN('Translation-EN'!A2328)>0,'Translation-EN'!A2328,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2328)>0,'Translation-EN'!B2328,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2328)>0,'Translation-EN'!C2328,\"\")","v":"D397"},{"$f":"IF(LEN('Translation-EN'!D2328)>0,'Translation-EN'!D2328,\"\")","v":""},"Série-E (moyenne guillotine double/Auvent/Panoramique)"]
[{"$f":"IF(LEN('Translation-EN'!A2329)>0,'Translation-EN'!A2329,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2329)>0,'Translation-EN'!B2329,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2329)>0,'Translation-EN'!C2329,\"\")","v":"E397"},{"$f":"IF(LEN('Translation-EN'!D2329)>0,'Translation-EN'!D2329,\"\")","v":""},{"$f":"$E$2005","v":"Charpente en bois, revêtement en aluminium"}]
[{"$f":"IF(LEN('Translation-EN'!A2330)>0,'Translation-EN'!A2330,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2330)>0,'Translation-EN'!B2330,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2330)>0,'Translation-EN'!C2330,\"\")","v":"B398"},{"$f":"IF(LEN('Translation-EN'!D2330)>0,'Translation-EN'!D2330,\"\")","v":""},{"$f":"$E$1529","v":"Cloisons sèches 1/2 po"}]
[{"$f":"IF(LEN('Translation-EN'!A2331)>0,'Translation-EN'!A2331,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2331)>0,'Translation-EN'!B2331,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2331)>0,'Translation-EN'!C2331,\"\")","v":"D398"},{"$f":"IF(LEN('Translation-EN'!D2331)>0,'Translation-EN'!D2331,\"\")","v":""},"Panneaux de gypse Gold Bond XP"]
[{"$f":"IF(LEN('Translation-EN'!A2332)>0,'Translation-EN'!A2332,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2332)>0,'Translation-EN'!B2332,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2332)>0,'Translation-EN'!C2332,\"\")","v":"B399"},{"$f":"IF(LEN('Translation-EN'!D2332)>0,'Translation-EN'!D2332,\"\")","v":""},"Gypse 5/8\" Type X"]
[{"$f":"IF(LEN('Translation-EN'!A2333)>0,'Translation-EN'!A2333,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2333)>0,'Translation-EN'!B2333,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2333)>0,'Translation-EN'!C2333,\"\")","v":"D399"},{"$f":"IF(LEN('Translation-EN'!D2333)>0,'Translation-EN'!D2333,\"\")","v":""},"Panneaux de gypse Gold Bond XP pare-feu"]
[{"$f":"IF(LEN('Translation-EN'!A2334)>0,'Translation-EN'!A2334,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2334)>0,'Translation-EN'!B2334,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2334)>0,'Translation-EN'!C2334,\"\")","v":"E399"},{"$f":"IF(LEN('Translation-EN'!D2334)>0,'Translation-EN'!D2334,\"\")","v":""},"5/8'' type X"]
[{"$f":"IF(LEN('Translation-EN'!A2335)>0,'Translation-EN'!A2335,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2335)>0,'Translation-EN'!B2335,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2335)>0,'Translation-EN'!C2335,\"\")","v":"B400"},{"$f":"IF(LEN('Translation-EN'!D2335)>0,'Translation-EN'!D2335,\"\")","v":""},{"$f":"$E$1327","v":"Tapis"}]
[{"$f":"IF(LEN('Translation-EN'!A2336)>0,'Translation-EN'!A2336,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2336)>0,'Translation-EN'!B2336,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2336)>0,'Translation-EN'!C2336,\"\")","v":"D400"},{"$f":"IF(LEN('Translation-EN'!D2336)>0,'Translation-EN'!D2336,\"\")","v":""},"Envers standard"]
[{"$f":"IF(LEN('Translation-EN'!A2337)>0,'Translation-EN'!A2337,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2337)>0,'Translation-EN'!B2337,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2337)>0,'Translation-EN'!C2337,\"\")","v":"E400"},{"$f":"IF(LEN('Translation-EN'!D2337)>0,'Translation-EN'!D2337,\"\")","v":""},"Tapis style grande largeur"]
[{"$f":"IF(LEN('Translation-EN'!A2338)>0,'Translation-EN'!A2338,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2338)>0,'Translation-EN'!B2338,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2338)>0,'Translation-EN'!C2338,\"\")","v":"B401"},{"$f":"IF(LEN('Translation-EN'!D2338)>0,'Translation-EN'!D2338,\"\")","v":""},{"$f":"$E$1970","v":"Revêtement de plancher en vinyle"}]
[{"$f":"IF(LEN('Translation-EN'!A2339)>0,'Translation-EN'!A2339,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2339)>0,'Translation-EN'!B2339,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2339)>0,'Translation-EN'!C2339,\"\")","v":"D401"},{"$f":"IF(LEN('Translation-EN'!D2339)>0,'Translation-EN'!D2339,\"\")","v":""},{"$f":"$E$2320","v":"Carreau de vinyle de luxe"}]
[{"$f":"IF(LEN('Translation-EN'!A2340)>0,'Translation-EN'!A2340,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2340)>0,'Translation-EN'!B2340,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2340)>0,'Translation-EN'!C2340,\"\")","v":"E401"},{"$f":"IF(LEN('Translation-EN'!D2340)>0,'Translation-EN'!D2340,\"\")","v":""},"Tuiles et planches 2,5 mm"]
[{"$f":"IF(LEN('Translation-EN'!A2341)>0,'Translation-EN'!A2341,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2341)>0,'Translation-EN'!B2341,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2341)>0,'Translation-EN'!C2341,\"\")","v":"B402"},{"$f":"IF(LEN('Translation-EN'!D2341)>0,'Translation-EN'!D2341,\"\")","v":""},{"$f":"$E$1281","v":"Bardeaux d’asphalte"}]
[{"$f":"IF(LEN('Translation-EN'!A2342)>0,'Translation-EN'!A2342,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2342)>0,'Translation-EN'!B2342,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2342)>0,'Translation-EN'!C2342,\"\")","v":"D402"},{"$f":"IF(LEN('Translation-EN'!D2342)>0,'Translation-EN'!D2342,\"\")","v":true},"Bardeaux TimberlineMD CS"]
[{"$f":"IF(LEN('Translation-EN'!A2343)>0,'Translation-EN'!A2343,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2343)>0,'Translation-EN'!B2343,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2343)>0,'Translation-EN'!C2343,\"\")","v":"B403"},{"$f":"IF(LEN('Translation-EN'!D2343)>0,'Translation-EN'!D2343,\"\")","v":""},{"$f":"$E$1684","v":"Revêtement de plancher en linoléum"}]
[{"$f":"IF(LEN('Translation-EN'!A2344)>0,'Translation-EN'!A2344,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2344)>0,'Translation-EN'!B2344,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2344)>0,'Translation-EN'!C2344,\"\")","v":"D403"},{"$f":"IF(LEN('Translation-EN'!D2344)>0,'Translation-EN'!D2344,\"\")","v":""},"Plancher Legato"]
[{"$f":"IF(LEN('Translation-EN'!A2345)>0,'Translation-EN'!A2345,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2345)>0,'Translation-EN'!B2345,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2345)>0,'Translation-EN'!C2345,\"\")","v":"E403"},{"$f":"IF(LEN('Translation-EN'!D2345)>0,'Translation-EN'!D2345,\"\")","v":""},"liquide appliqué"]
[{"$f":"IF(LEN('Translation-EN'!A2346)>0,'Translation-EN'!A2346,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2346)>0,'Translation-EN'!B2346,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2346)>0,'Translation-EN'!C2346,\"\")","v":"B404"},{"$f":"IF(LEN('Translation-EN'!D2346)>0,'Translation-EN'!D2346,\"\")","v":""},{"$f":"$E$1373","v":"Carreaux en céramique"}]
[{"$f":"IF(LEN('Translation-EN'!A2347)>0,'Translation-EN'!A2347,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2347)>0,'Translation-EN'!B2347,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2347)>0,'Translation-EN'!C2347,\"\")","v":"D404"},{"$f":"IF(LEN('Translation-EN'!D2347)>0,'Translation-EN'!D2347,\"\")","v":""},"Céramique – contenu recyclé"]
[{"$f":"IF(LEN('Translation-EN'!A2348)>0,'Translation-EN'!A2348,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2348)>0,'Translation-EN'!B2348,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2348)>0,'Translation-EN'!C2348,\"\")","v":"E404"},{"$f":"IF(LEN('Translation-EN'!D2348)>0,'Translation-EN'!D2348,\"\")","v":""},"Grade standard et second"]
[{"$f":"IF(LEN('Translation-EN'!A2349)>0,'Translation-EN'!A2349,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2349)>0,'Translation-EN'!B2349,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2349)>0,'Translation-EN'!C2349,\"\")","v":"B405"},{"$f":"IF(LEN('Translation-EN'!D2349)>0,'Translation-EN'!D2349,\"\")","v":""},{"$f":"$E$1373","v":"Carreaux en céramique"}]
[{"$f":"IF(LEN('Translation-EN'!A2350)>0,'Translation-EN'!A2350,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2350)>0,'Translation-EN'!B2350,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2350)>0,'Translation-EN'!C2350,\"\")","v":"D405"},{"$f":"IF(LEN('Translation-EN'!D2350)>0,'Translation-EN'!D2350,\"\")","v":""},"Porcelaine – contenu recyclé"]
[{"$f":"IF(LEN('Translation-EN'!A2351)>0,'Translation-EN'!A2351,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2351)>0,'Translation-EN'!B2351,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2351)>0,'Translation-EN'!C2351,\"\")","v":"E405"},{"$f":"IF(LEN('Translation-EN'!D2351)>0,'Translation-EN'!D2351,\"\")","v":""},{"$f":"$E$2348","v":"Grade standard et second"}]
[{"$f":"IF(LEN('Translation-EN'!A2352)>0,'Translation-EN'!A2352,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2352)>0,'Translation-EN'!B2352,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2352)>0,'Translation-EN'!C2352,\"\")","v":"B406"},{"$f":"IF(LEN('Translation-EN'!D2352)>0,'Translation-EN'!D2352,\"\")","v":""},{"$f":"$E$1578","v":"Bardage en fibrociment"}]
[{"$f":"IF(LEN('Translation-EN'!A2353)>0,'Translation-EN'!A2353,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2353)>0,'Translation-EN'!B2353,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2353)>0,'Translation-EN'!C2353,\"\")","v":"D406"},{"$f":"IF(LEN('Translation-EN'!D2353)>0,'Translation-EN'!D2353,\"\")","v":""},"Pictura et Natura Pro"]
[{"$f":"IF(LEN('Translation-EN'!A2354)>0,'Translation-EN'!A2354,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2354)>0,'Translation-EN'!B2354,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2354)>0,'Translation-EN'!C2354,\"\")","v":"B407"},{"$f":"IF(LEN('Translation-EN'!D2354)>0,'Translation-EN'!D2354,\"\")","v":""},{"$f":"$E$1578","v":"Bardage en fibrociment"}]
[{"$f":"IF(LEN('Translation-EN'!A2355)>0,'Translation-EN'!A2355,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2355)>0,'Translation-EN'!B2355,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2355)>0,'Translation-EN'!C2355,\"\")","v":"D407"},{"$f":"IF(LEN('Translation-EN'!D2355)>0,'Translation-EN'!D2355,\"\")","v":""},"Tectiva"]
[{"$f":"IF(LEN('Translation-EN'!A2356)>0,'Translation-EN'!A2356,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2356)>0,'Translation-EN'!B2356,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2356)>0,'Translation-EN'!C2356,\"\")","v":"B408"},{"$f":"IF(LEN('Translation-EN'!D2356)>0,'Translation-EN'!D2356,\"\")","v":""},{"$f":"$E$1578","v":"Bardage en fibrociment"}]
[{"$f":"IF(LEN('Translation-EN'!A2357)>0,'Translation-EN'!A2357,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2357)>0,'Translation-EN'!B2357,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2357)>0,'Translation-EN'!C2357,\"\")","v":"D408"},{"$f":"IF(LEN('Translation-EN'!D2357)>0,'Translation-EN'!D2357,\"\")","v":""},"Natura, Textura et Materia"]
[{"$f":"IF(LEN('Translation-EN'!A2358)>0,'Translation-EN'!A2358,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2358)>0,'Translation-EN'!B2358,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2358)>0,'Translation-EN'!C2358,\"\")","v":"B409"},{"$f":"IF(LEN('Translation-EN'!D2358)>0,'Translation-EN'!D2358,\"\")","v":""},{"$f":"$E$1957","v":"Panneaux de paille"}]
[{"$f":"IF(LEN('Translation-EN'!A2359)>0,'Translation-EN'!A2359,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2359)>0,'Translation-EN'!B2359,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2359)>0,'Translation-EN'!C2359,\"\")","v":"D409"},{"$f":"IF(LEN('Translation-EN'!D2359)>0,'Translation-EN'!D2359,\"\")","v":""},"Panneaux standard et de renfort"]
[{"$f":"IF(LEN('Translation-EN'!A2360)>0,'Translation-EN'!A2360,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2360)>0,'Translation-EN'!B2360,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2360)>0,'Translation-EN'!C2360,\"\")","v":"E409"},{"$f":"IF(LEN('Translation-EN'!D2360)>0,'Translation-EN'!D2360,\"\")","v":""},"40cm R16, panneau seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2361)>0,'Translation-EN'!A2361,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2361)>0,'Translation-EN'!B2361,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2361)>0,'Translation-EN'!C2361,\"\")","v":"B410"},{"$f":"IF(LEN('Translation-EN'!D2361)>0,'Translation-EN'!D2361,\"\")","v":""},{"$f":"$E$1312","v":"Brique, argile"}]
[{"$f":"IF(LEN('Translation-EN'!A2362)>0,'Translation-EN'!A2362,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2362)>0,'Translation-EN'!B2362,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2362)>0,'Translation-EN'!C2362,\"\")","v":"D410"},{"$f":"IF(LEN('Translation-EN'!D2362)>0,'Translation-EN'!D2362,\"\")","v":""},"Mince – Brique à face mince"]
[{"$f":"IF(LEN('Translation-EN'!A2363)>0,'Translation-EN'!A2363,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2363)>0,'Translation-EN'!B2363,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2363)>0,'Translation-EN'!C2363,\"\")","v":"E410"},{"$f":"IF(LEN('Translation-EN'!D2363)>0,'Translation-EN'!D2363,\"\")","v":""},"2 1/4\" x 1/2\" x 7-1/2\" (57 x 12.7 mm x 190) incl. 3/8\" mortier"]
[{"$f":"IF(LEN('Translation-EN'!A2364)>0,'Translation-EN'!A2364,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2364)>0,'Translation-EN'!B2364,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2364)>0,'Translation-EN'!C2364,\"\")","v":"B411"},{"$f":"IF(LEN('Translation-EN'!D2364)>0,'Translation-EN'!D2364,\"\")","v":""},{"$f":"$E$1312","v":"Brique, argile"}]
[{"$f":"IF(LEN('Translation-EN'!A2365)>0,'Translation-EN'!A2365,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2365)>0,'Translation-EN'!B2365,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2365)>0,'Translation-EN'!C2365,\"\")","v":"D411"},{"$f":"IF(LEN('Translation-EN'!D2365)>0,'Translation-EN'!D2365,\"\")","v":""},{"$f":"$E$1314","v":"Brique moyenne de façade"}]
[{"$f":"IF(LEN('Translation-EN'!A2366)>0,'Translation-EN'!A2366,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2366)>0,'Translation-EN'!B2366,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2366)>0,'Translation-EN'!C2366,\"\")","v":"E411"},{"$f":"IF(LEN('Translation-EN'!D2366)>0,'Translation-EN'!D2366,\"\")","v":""},{"$f":"$E$1311","v":"3-5/8 po x 2-3/4 po x 7-5/8 po (92 x 70 x 194 mm), mortier de 3/8 po inclus3-5/8 po x 2-3/4 po x 7-5/8 po (92 x 70 x 194 mm) avec mortier de 3/8 po "}]
[{"$f":"IF(LEN('Translation-EN'!A2367)>0,'Translation-EN'!A2367,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2367)>0,'Translation-EN'!B2367,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2367)>0,'Translation-EN'!C2367,\"\")","v":"B412"},{"$f":"IF(LEN('Translation-EN'!D2367)>0,'Translation-EN'!D2367,\"\")","v":""},{"$f":"$E$1841","v":"Barre d’armature"}]
[{"$f":"IF(LEN('Translation-EN'!A2368)>0,'Translation-EN'!A2368,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2368)>0,'Translation-EN'!B2368,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2368)>0,'Translation-EN'!C2368,\"\")","v":"D412"},{"$f":"IF(LEN('Translation-EN'!D2368)>0,'Translation-EN'!D2368,\"\")","v":""},"Dimensions canadiennes"]
[{"$f":"IF(LEN('Translation-EN'!A2369)>0,'Translation-EN'!A2369,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2369)>0,'Translation-EN'!B2369,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2369)>0,'Translation-EN'!C2369,\"\")","v":"B413"},{"$f":"IF(LEN('Translation-EN'!D2369)>0,'Translation-EN'!D2369,\"\")","v":""},{"$f":"$E$1841","v":"Barre d’armature"}]
[{"$f":"IF(LEN('Translation-EN'!A2370)>0,'Translation-EN'!A2370,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2370)>0,'Translation-EN'!B2370,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2370)>0,'Translation-EN'!C2370,\"\")","v":"D413"},{"$f":"IF(LEN('Translation-EN'!D2370)>0,'Translation-EN'!D2370,\"\")","v":""},{"$f":"$E$2368","v":"Dimensions canadiennes"}]
[{"$f":"IF(LEN('Translation-EN'!A2371)>0,'Translation-EN'!A2371,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2371)>0,'Translation-EN'!B2371,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2371)>0,'Translation-EN'!C2371,\"\")","v":"B414"},{"$f":"IF(LEN('Translation-EN'!D2371)>0,'Translation-EN'!D2371,\"\")","v":""},{"$f":"$E$1841","v":"Barre d’armature"}]
[{"$f":"IF(LEN('Translation-EN'!A2372)>0,'Translation-EN'!A2372,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2372)>0,'Translation-EN'!B2372,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2372)>0,'Translation-EN'!C2372,\"\")","v":"D414"},{"$f":"IF(LEN('Translation-EN'!D2372)>0,'Translation-EN'!D2372,\"\")","v":""},{"$f":"$E$2368","v":"Dimensions canadiennes"}]
[{"$f":"IF(LEN('Translation-EN'!A2373)>0,'Translation-EN'!A2373,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2373)>0,'Translation-EN'!B2373,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2373)>0,'Translation-EN'!C2373,\"\")","v":"B415"},{"$f":"IF(LEN('Translation-EN'!D2373)>0,'Translation-EN'!D2373,\"\")","v":""},{"$f":"$E$1841","v":"Barre d’armature"}]
[{"$f":"IF(LEN('Translation-EN'!A2374)>0,'Translation-EN'!A2374,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2374)>0,'Translation-EN'!B2374,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2374)>0,'Translation-EN'!C2374,\"\")","v":"D415"},{"$f":"IF(LEN('Translation-EN'!D2374)>0,'Translation-EN'!D2374,\"\")","v":""},{"$f":"$E$2368","v":"Dimensions canadiennes"}]
[{"$f":"IF(LEN('Translation-EN'!A2375)>0,'Translation-EN'!A2375,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2375)>0,'Translation-EN'!B2375,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2375)>0,'Translation-EN'!C2375,\"\")","v":"B416"},{"$f":"IF(LEN('Translation-EN'!D2375)>0,'Translation-EN'!D2375,\"\")","v":""},{"$f":"$E$1841","v":"Barre d’armature"}]
[{"$f":"IF(LEN('Translation-EN'!A2376)>0,'Translation-EN'!A2376,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2376)>0,'Translation-EN'!B2376,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2376)>0,'Translation-EN'!C2376,\"\")","v":"D416"},{"$f":"IF(LEN('Translation-EN'!D2376)>0,'Translation-EN'!D2376,\"\")","v":""},{"$f":"$E$2368","v":"Dimensions canadiennes"}]
[{"$f":"IF(LEN('Translation-EN'!A2377)>0,'Translation-EN'!A2377,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2377)>0,'Translation-EN'!B2377,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2377)>0,'Translation-EN'!C2377,\"\")","v":"B417"},{"$f":"IF(LEN('Translation-EN'!D2377)>0,'Translation-EN'!D2377,\"\")","v":""},{"$f":"$E$1841","v":"Barre d’armature"}]
[{"$f":"IF(LEN('Translation-EN'!A2378)>0,'Translation-EN'!A2378,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2378)>0,'Translation-EN'!B2378,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2378)>0,'Translation-EN'!C2378,\"\")","v":"D417"},{"$f":"IF(LEN('Translation-EN'!D2378)>0,'Translation-EN'!D2378,\"\")","v":""},{"$f":"$E$2368","v":"Dimensions canadiennes"}]
[{"$f":"IF(LEN('Translation-EN'!A2379)>0,'Translation-EN'!A2379,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2379)>0,'Translation-EN'!B2379,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2379)>0,'Translation-EN'!C2379,\"\")","v":"B418"},{"$f":"IF(LEN('Translation-EN'!D2379)>0,'Translation-EN'!D2379,\"\")","v":""},{"$f":"$E$2046","v":"Panneau de fibres de bois"}]
[{"$f":"IF(LEN('Translation-EN'!A2380)>0,'Translation-EN'!A2380,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2380)>0,'Translation-EN'!B2380,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2380)>0,'Translation-EN'!C2380,\"\")","v":"D418"},{"$f":"IF(LEN('Translation-EN'!D2380)>0,'Translation-EN'!D2380,\"\")","v":""},"Inclus : MSL, Blue Ridge Fiberboard Inc."]
[{"$f":"IF(LEN('Translation-EN'!A2381)>0,'Translation-EN'!A2381,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2381)>0,'Translation-EN'!B2381,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2381)>0,'Translation-EN'!C2381,\"\")","v":"B419"},{"$f":"IF(LEN('Translation-EN'!D2381)>0,'Translation-EN'!D2381,\"\")","v":""},"(ARCHIVÉ 2023) Panneau de mousse XPS"]
[{"$f":"IF(LEN('Translation-EN'!A2382)>0,'Translation-EN'!A2382,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2382)>0,'Translation-EN'!B2382,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2382)>0,'Translation-EN'!C2382,\"\")","v":"D419"},{"$f":"IF(LEN('Translation-EN'!D2382)>0,'Translation-EN'!D2382,\"\")","v":""},"Styrofoam (bleu) (formule anciennne)"]
[{"$f":"IF(LEN('Translation-EN'!A2383)>0,'Translation-EN'!A2383,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2383)>0,'Translation-EN'!B2383,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2383)>0,'Translation-EN'!C2383,\"\")","v":"E419"},{"$f":"IF(LEN('Translation-EN'!D2383)>0,'Translation-EN'!D2383,\"\")","v":""},"R 5,6/po"]
[{"$f":"IF(LEN('Translation-EN'!A2384)>0,'Translation-EN'!A2384,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2384)>0,'Translation-EN'!B2384,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2384)>0,'Translation-EN'!C2384,\"\")","v":"B420"},{"$f":"IF(LEN('Translation-EN'!D2384)>0,'Translation-EN'!D2384,\"\")","v":""},{"$f":"$E$2092","v":"Panneau en mousse XPS"}]
[{"$f":"IF(LEN('Translation-EN'!A2385)>0,'Translation-EN'!A2385,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2385)>0,'Translation-EN'!B2385,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2385)>0,'Translation-EN'!C2385,\"\")","v":"D420"},{"$f":"IF(LEN('Translation-EN'!D2385)>0,'Translation-EN'!D2385,\"\")","v":""},"Styrofoam (Grisy, PRP Réduit)"]
[{"$f":"IF(LEN('Translation-EN'!A2386)>0,'Translation-EN'!A2386,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2386)>0,'Translation-EN'!B2386,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2386)>0,'Translation-EN'!C2386,\"\")","v":"E420"},{"$f":"IF(LEN('Translation-EN'!D2386)>0,'Translation-EN'!D2386,\"\")","v":""},{"$f":"$E$2383","v":"R 5,6/po"}]
[{"$f":"IF(LEN('Translation-EN'!A2387)>0,'Translation-EN'!A2387,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2387)>0,'Translation-EN'!B2387,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2387)>0,'Translation-EN'!C2387,\"\")","v":"B421"},{"$f":"IF(LEN('Translation-EN'!D2387)>0,'Translation-EN'!D2387,\"\")","v":""},{"$f":"$E$2092","v":"Panneau en mousse XPS"}]
[{"$f":"IF(LEN('Translation-EN'!A2388)>0,'Translation-EN'!A2388,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2388)>0,'Translation-EN'!B2388,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2388)>0,'Translation-EN'!C2388,\"\")","v":"D421"},{"$f":"IF(LEN('Translation-EN'!D2388)>0,'Translation-EN'!D2388,\"\")","v":""},"Styrofoam gris à PPR réduit (même que ST-100)"]
[{"$f":"IF(LEN('Translation-EN'!A2389)>0,'Translation-EN'!A2389,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2389)>0,'Translation-EN'!B2389,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2389)>0,'Translation-EN'!C2389,\"\")","v":"B422"},{"$f":"IF(LEN('Translation-EN'!D2389)>0,'Translation-EN'!D2389,\"\")","v":""},{"$f":"$E$2092","v":"Panneau en mousse XPS"}]
[{"$f":"IF(LEN('Translation-EN'!A2390)>0,'Translation-EN'!A2390,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2390)>0,'Translation-EN'!B2390,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2390)>0,'Translation-EN'!C2390,\"\")","v":"D422"},{"$f":"IF(LEN('Translation-EN'!D2390)>0,'Translation-EN'!D2390,\"\")","v":""},"SOPRA-XPS"]
[{"$f":"IF(LEN('Translation-EN'!A2391)>0,'Translation-EN'!A2391,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2391)>0,'Translation-EN'!B2391,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2391)>0,'Translation-EN'!C2391,\"\")","v":"B423"},{"$f":"IF(LEN('Translation-EN'!D2391)>0,'Translation-EN'!D2391,\"\")","v":""},{"$f":"$E$1745","v":"Natte de laine minérale"}]
[{"$f":"IF(LEN('Translation-EN'!A2392)>0,'Translation-EN'!A2392,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2392)>0,'Translation-EN'!B2392,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2392)>0,'Translation-EN'!C2392,\"\")","v":"D423"},{"$f":"IF(LEN('Translation-EN'!D2392)>0,'Translation-EN'!D2392,\"\")","v":""},"ComfortBatt R14"]
[{"$f":"IF(LEN('Translation-EN'!A2393)>0,'Translation-EN'!A2393,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2393)>0,'Translation-EN'!B2393,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2393)>0,'Translation-EN'!C2393,\"\")","v":"B424"},{"$f":"IF(LEN('Translation-EN'!D2393)>0,'Translation-EN'!D2393,\"\")","v":""},{"$f":"$E$1745","v":"Natte de laine minérale"}]
[{"$f":"IF(LEN('Translation-EN'!A2394)>0,'Translation-EN'!A2394,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2394)>0,'Translation-EN'!B2394,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2394)>0,'Translation-EN'!C2394,\"\")","v":"D424"},{"$f":"IF(LEN('Translation-EN'!D2394)>0,'Translation-EN'!D2394,\"\")","v":""},"ComfortBatt R15"]
[{"$f":"IF(LEN('Translation-EN'!A2395)>0,'Translation-EN'!A2395,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2395)>0,'Translation-EN'!B2395,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2395)>0,'Translation-EN'!C2395,\"\")","v":"B425"},{"$f":"IF(LEN('Translation-EN'!D2395)>0,'Translation-EN'!D2395,\"\")","v":""},{"$f":"$E$1745","v":"Natte de laine minérale"}]
[{"$f":"IF(LEN('Translation-EN'!A2396)>0,'Translation-EN'!A2396,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2396)>0,'Translation-EN'!B2396,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2396)>0,'Translation-EN'!C2396,\"\")","v":"D425"},{"$f":"IF(LEN('Translation-EN'!D2396)>0,'Translation-EN'!D2396,\"\")","v":""},"ComfortBatt R22"]
[{"$f":"IF(LEN('Translation-EN'!A2397)>0,'Translation-EN'!A2397,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2397)>0,'Translation-EN'!B2397,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2397)>0,'Translation-EN'!C2397,\"\")","v":"B426"},{"$f":"IF(LEN('Translation-EN'!D2397)>0,'Translation-EN'!D2397,\"\")","v":""},{"$f":"$E$1745","v":"Natte de laine minérale"}]
[{"$f":"IF(LEN('Translation-EN'!A2398)>0,'Translation-EN'!A2398,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2398)>0,'Translation-EN'!B2398,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2398)>0,'Translation-EN'!C2398,\"\")","v":"D426"},{"$f":"IF(LEN('Translation-EN'!D2398)>0,'Translation-EN'!D2398,\"\")","v":""},"ComfortBatt R24"]
[{"$f":"IF(LEN('Translation-EN'!A2399)>0,'Translation-EN'!A2399,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2399)>0,'Translation-EN'!B2399,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2399)>0,'Translation-EN'!C2399,\"\")","v":"B427"},{"$f":"IF(LEN('Translation-EN'!D2399)>0,'Translation-EN'!D2399,\"\")","v":""},{"$f":"$E$1745","v":"Natte de laine minérale"}]
[{"$f":"IF(LEN('Translation-EN'!A2400)>0,'Translation-EN'!A2400,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2400)>0,'Translation-EN'!B2400,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2400)>0,'Translation-EN'!C2400,\"\")","v":"D427"},{"$f":"IF(LEN('Translation-EN'!D2400)>0,'Translation-EN'!D2400,\"\")","v":""},"ComfortBatt R24 SS"]
[{"$f":"IF(LEN('Translation-EN'!A2401)>0,'Translation-EN'!A2401,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2401)>0,'Translation-EN'!B2401,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2401)>0,'Translation-EN'!C2401,\"\")","v":"E427"},{"$f":"IF(LEN('Translation-EN'!D2401)>0,'Translation-EN'!D2401,\"\")","v":""},"R 4,0/pouce, montants en acier de 6 pouces"]
[{"$f":"IF(LEN('Translation-EN'!A2402)>0,'Translation-EN'!A2402,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2402)>0,'Translation-EN'!B2402,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2402)>0,'Translation-EN'!C2402,\"\")","v":"B428"},{"$f":"IF(LEN('Translation-EN'!D2402)>0,'Translation-EN'!D2402,\"\")","v":""},{"$f":"$E$1757","v":"Panneau de laine minérale"}]
[{"$f":"IF(LEN('Translation-EN'!A2403)>0,'Translation-EN'!A2403,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2403)>0,'Translation-EN'!B2403,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2403)>0,'Translation-EN'!C2403,\"\")","v":"D428"},{"$f":"IF(LEN('Translation-EN'!D2403)>0,'Translation-EN'!D2403,\"\")","v":""},"Comfortboard 80"]
[{"$f":"IF(LEN('Translation-EN'!A2404)>0,'Translation-EN'!A2404,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2404)>0,'Translation-EN'!B2404,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2404)>0,'Translation-EN'!C2404,\"\")","v":"B429"},{"$f":"IF(LEN('Translation-EN'!D2404)>0,'Translation-EN'!D2404,\"\")","v":""},{"$f":"$E$1811","v":"Polyiso – panneaux de toiture"}]
[{"$f":"IF(LEN('Translation-EN'!A2405)>0,'Translation-EN'!A2405,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2405)>0,'Translation-EN'!B2405,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2405)>0,'Translation-EN'!C2405,\"\")","v":"D429"},{"$f":"IF(LEN('Translation-EN'!D2405)>0,'Translation-EN'!D2405,\"\")","v":""},"Thermax"]
[{"$f":"IF(LEN('Translation-EN'!A2406)>0,'Translation-EN'!A2406,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2406)>0,'Translation-EN'!B2406,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2406)>0,'Translation-EN'!C2406,\"\")","v":"B430"},{"$f":"IF(LEN('Translation-EN'!D2406)>0,'Translation-EN'!D2406,\"\")","v":""},"Bois en placage stratifié"]
[{"$f":"IF(LEN('Translation-EN'!A2407)>0,'Translation-EN'!A2407,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2407)>0,'Translation-EN'!B2407,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2407)>0,'Translation-EN'!C2407,\"\")","v":"D430"},{"$f":"IF(LEN('Translation-EN'!D2407)>0,'Translation-EN'!D2407,\"\")","v":""},"RigidLam LVL"]
[{"$f":"IF(LEN('Translation-EN'!A2408)>0,'Translation-EN'!A2408,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2408)>0,'Translation-EN'!B2408,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2408)>0,'Translation-EN'!C2408,\"\")","v":"B431"},{"$f":"IF(LEN('Translation-EN'!D2408)>0,'Translation-EN'!D2408,\"\")","v":""},"Isolant mousse de polyuréthane giclée – structure alvéolaire fermée (HFO)"]
[{"$f":"IF(LEN('Translation-EN'!A2409)>0,'Translation-EN'!A2409,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2409)>0,'Translation-EN'!B2409,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2409)>0,'Translation-EN'!C2409,\"\")","v":"D431"},{"$f":"IF(LEN('Translation-EN'!D2409)>0,'Translation-EN'!D2409,\"\")","v":""},"Airmétic HFO & Airmétic Soya HFO"]
[{"$f":"IF(LEN('Translation-EN'!A2410)>0,'Translation-EN'!A2410,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2410)>0,'Translation-EN'!B2410,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2410)>0,'Translation-EN'!C2410,\"\")","v":"B432"},{"$f":"IF(LEN('Translation-EN'!D2410)>0,'Translation-EN'!D2410,\"\")","v":""},{"$f":"$E$1811","v":"Polyiso – panneaux de toiture"}]
[{"$f":"IF(LEN('Translation-EN'!A2411)>0,'Translation-EN'!A2411,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2411)>0,'Translation-EN'!B2411,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2411)>0,'Translation-EN'!C2411,\"\")","v":"D432"},{"$f":"IF(LEN('Translation-EN'!D2411)>0,'Translation-EN'!D2411,\"\")","v":""},"Inclus: Atlas, Firestone, GAF, Johns Manville, Rmax, Carlisle, Iko, Soprema"]
[{"$f":"IF(LEN('Translation-EN'!A2412)>0,'Translation-EN'!A2412,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2412)>0,'Translation-EN'!B2412,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2412)>0,'Translation-EN'!C2412,\"\")","v":"B433"},{"$f":"IF(LEN('Translation-EN'!D2412)>0,'Translation-EN'!D2412,\"\")","v":""},{"$f":"$E$1954","v":"Balle de paille"}]
[{"$f":"IF(LEN('Translation-EN'!A2413)>0,'Translation-EN'!A2413,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2413)>0,'Translation-EN'!B2413,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2413)>0,'Translation-EN'!C2413,\"\")","v":"D433"},{"$f":"IF(LEN('Translation-EN'!D2413)>0,'Translation-EN'!D2413,\"\")","v":""},"Paille de blé et d'orge"]
[{"$f":"IF(LEN('Translation-EN'!A2414)>0,'Translation-EN'!A2414,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2414)>0,'Translation-EN'!B2414,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2414)>0,'Translation-EN'!C2414,\"\")","v":"B434"},{"$f":"IF(LEN('Translation-EN'!D2414)>0,'Translation-EN'!D2414,\"\")","v":""},"Bardage et moulures en bois d'ingénierie"]
[{"$f":"IF(LEN('Translation-EN'!A2415)>0,'Translation-EN'!A2415,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2415)>0,'Translation-EN'!B2415,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2415)>0,'Translation-EN'!C2415,\"\")","v":"D434"},{"$f":"IF(LEN('Translation-EN'!D2415)>0,'Translation-EN'!D2415,\"\")","v":""},"SmartSide"]
[{"$f":"IF(LEN('Translation-EN'!A2416)>0,'Translation-EN'!A2416,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2416)>0,'Translation-EN'!B2416,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2416)>0,'Translation-EN'!C2416,\"\")","v":"B435"},{"$f":"IF(LEN('Translation-EN'!D2416)>0,'Translation-EN'!D2416,\"\")","v":""},{"$f":"$E$2414","v":"Bardage et moulures en bois d'ingénierie"}]
[{"$f":"IF(LEN('Translation-EN'!A2417)>0,'Translation-EN'!A2417,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2417)>0,'Translation-EN'!B2417,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2417)>0,'Translation-EN'!C2417,\"\")","v":"D435"},{"$f":"IF(LEN('Translation-EN'!D2417)>0,'Translation-EN'!D2417,\"\")","v":""},{"$f":"$E$2415","v":"SmartSide"}]
[{"$f":"IF(LEN('Translation-EN'!A2418)>0,'Translation-EN'!A2418,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2418)>0,'Translation-EN'!B2418,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2418)>0,'Translation-EN'!C2418,\"\")","v":"B436"},{"$f":"IF(LEN('Translation-EN'!D2418)>0,'Translation-EN'!D2418,\"\")","v":""},{"$f":"$E$2414","v":"Bardage et moulures en bois d'ingénierie"}]
[{"$f":"IF(LEN('Translation-EN'!A2419)>0,'Translation-EN'!A2419,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2419)>0,'Translation-EN'!B2419,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2419)>0,'Translation-EN'!C2419,\"\")","v":"D436"},{"$f":"IF(LEN('Translation-EN'!D2419)>0,'Translation-EN'!D2419,\"\")","v":""},{"$f":"$E$2415","v":"SmartSide"}]
[{"$f":"IF(LEN('Translation-EN'!A2420)>0,'Translation-EN'!A2420,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2420)>0,'Translation-EN'!B2420,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2420)>0,'Translation-EN'!C2420,\"\")","v":"B437"},{"$f":"IF(LEN('Translation-EN'!D2420)>0,'Translation-EN'!D2420,\"\")","v":""},{"$f":"$E$1992","v":"Fenêtre – sous-fenêtre double"}]
[{"$f":"IF(LEN('Translation-EN'!A2421)>0,'Translation-EN'!A2421,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2421)>0,'Translation-EN'!B2421,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2421)>0,'Translation-EN'!C2421,\"\")","v":"D437"},{"$f":"IF(LEN('Translation-EN'!D2421)>0,'Translation-EN'!D2421,\"\")","v":""},"300 series oscillo-battante, 300 series fixed, 325 series auvent/battant, 325 series Fixed, et 400 series"]
[{"$f":"IF(LEN('Translation-EN'!A2422)>0,'Translation-EN'!A2422,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2422)>0,'Translation-EN'!B2422,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2422)>0,'Translation-EN'!C2422,\"\")","v":"E437"},{"$f":"IF(LEN('Translation-EN'!D2422)>0,'Translation-EN'!D2422,\"\")","v":""},{"$f":"$E$1993","v":"Cadre en fibre de verre"}]
[{"$f":"IF(LEN('Translation-EN'!A2423)>0,'Translation-EN'!A2423,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2423)>0,'Translation-EN'!B2423,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2423)>0,'Translation-EN'!C2423,\"\")","v":"B438"},{"$f":"IF(LEN('Translation-EN'!D2423)>0,'Translation-EN'!D2423,\"\")","v":""},{"$f":"$E$1578","v":"Bardage en fibrociment"}]
[{"$f":"IF(LEN('Translation-EN'!A2424)>0,'Translation-EN'!A2424,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2424)>0,'Translation-EN'!B2424,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2424)>0,'Translation-EN'!C2424,\"\")","v":"D438"},{"$f":"IF(LEN('Translation-EN'!D2424)>0,'Translation-EN'!D2424,\"\")","v":true},"HardiePanel®"]
[{"$f":"IF(LEN('Translation-EN'!A2425)>0,'Translation-EN'!A2425,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2425)>0,'Translation-EN'!B2425,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2425)>0,'Translation-EN'!C2425,\"\")","v":"B439"},{"$f":"IF(LEN('Translation-EN'!D2425)>0,'Translation-EN'!D2425,\"\")","v":""},{"$f":"$E$1632","v":"Panneaux de gypse – matelas de verre"}]
[{"$f":"IF(LEN('Translation-EN'!A2426)>0,'Translation-EN'!A2426,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2426)>0,'Translation-EN'!B2426,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2426)>0,'Translation-EN'!C2426,\"\")","v":"D439"},{"$f":"IF(LEN('Translation-EN'!D2426)>0,'Translation-EN'!D2426,\"\")","v":""},"Panneaux de gypse GlasRoc "]
[{"$f":"IF(LEN('Translation-EN'!A2427)>0,'Translation-EN'!A2427,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2427)>0,'Translation-EN'!B2427,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2427)>0,'Translation-EN'!C2427,\"\")","v":"B440"},{"$f":"IF(LEN('Translation-EN'!D2427)>0,'Translation-EN'!D2427,\"\")","v":""},{"$f":"$E$1578","v":"Bardage en fibrociment"}]
[{"$f":"IF(LEN('Translation-EN'!A2428)>0,'Translation-EN'!A2428,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2428)>0,'Translation-EN'!B2428,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2428)>0,'Translation-EN'!C2428,\"\")","v":"D440"},{"$f":"IF(LEN('Translation-EN'!D2428)>0,'Translation-EN'!D2428,\"\")","v":""},"Hardie VL Plank"]
[{"$f":"IF(LEN('Translation-EN'!A2429)>0,'Translation-EN'!A2429,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2429)>0,'Translation-EN'!B2429,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2429)>0,'Translation-EN'!C2429,\"\")","v":"B441"},{"$f":"IF(LEN('Translation-EN'!D2429)>0,'Translation-EN'!D2429,\"\")","v":""},{"$f":"$E$1578","v":"Bardage en fibrociment"}]
[{"$f":"IF(LEN('Translation-EN'!A2430)>0,'Translation-EN'!A2430,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2430)>0,'Translation-EN'!B2430,\"\")","v":"Master sheet"},{"$f":"IF(LEN('Translation-EN'!C2430)>0,'Translation-EN'!C2430,\"\")","v":"D441"},{"$f":"IF(LEN('Translation-EN'!D2430)>0,'Translation-EN'!D2430,\"\")","v":""},"HardiePlank"]
[{"$f":"IF(LEN('Translation-EN'!A2431)>0,'Translation-EN'!A2431,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2431)>0,'Translation-EN'!B2431,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2431)>0,'Translation-EN'!C2431,\"\")","v":"C1"},{"$f":"IF(LEN('Translation-EN'!D2431)>0,'Translation-EN'!D2431,\"\")","v":""},"Province"]
[{"$f":"IF(LEN('Translation-EN'!A2432)>0,'Translation-EN'!A2432,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2432)>0,'Translation-EN'!B2432,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2432)>0,'Translation-EN'!C2432,\"\")","v":"D1"},{"$f":"IF(LEN('Translation-EN'!D2432)>0,'Translation-EN'!D2432,\"\")","v":""},"Facteur de GES – Électricité"]
[{"$f":"IF(LEN('Translation-EN'!A2433)>0,'Translation-EN'!A2433,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2433)>0,'Translation-EN'!B2433,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2433)>0,'Translation-EN'!C2433,\"\")","v":"E1"},{"$f":"IF(LEN('Translation-EN'!D2433)>0,'Translation-EN'!D2433,\"\")","v":""},"Facteur de GES – Gaz naturel"]
[{"$f":"IF(LEN('Translation-EN'!A2434)>0,'Translation-EN'!A2434,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2434)>0,'Translation-EN'!B2434,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2434)>0,'Translation-EN'!C2434,\"\")","v":"F1"},{"$f":"IF(LEN('Translation-EN'!D2434)>0,'Translation-EN'!D2434,\"\")","v":""},"Facteur de GES – Mazout"]
[{"$f":"IF(LEN('Translation-EN'!A2435)>0,'Translation-EN'!A2435,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2435)>0,'Translation-EN'!B2435,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2435)>0,'Translation-EN'!C2435,\"\")","v":"G1"},{"$f":"IF(LEN('Translation-EN'!D2435)>0,'Translation-EN'!D2435,\"\")","v":""},"Facteur de GES – Propane"]
[{"$f":"IF(LEN('Translation-EN'!A2436)>0,'Translation-EN'!A2436,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2436)>0,'Translation-EN'!B2436,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2436)>0,'Translation-EN'!C2436,\"\")","v":"H1"},{"$f":"IF(LEN('Translation-EN'!D2436)>0,'Translation-EN'!D2436,\"\")","v":""},"Facteur de GES – Bois"]
[{"$f":"IF(LEN('Translation-EN'!A2437)>0,'Translation-EN'!A2437,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2437)>0,'Translation-EN'!B2437,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2437)>0,'Translation-EN'!C2437,\"\")","v":"C2"},{"$f":"IF(LEN('Translation-EN'!D2437)>0,'Translation-EN'!D2437,\"\")","v":""},"Terre-Neuve-et-Labrador"]
[{"$f":"IF(LEN('Translation-EN'!A2438)>0,'Translation-EN'!A2438,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2438)>0,'Translation-EN'!B2438,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2438)>0,'Translation-EN'!C2438,\"\")","v":"C3"},{"$f":"IF(LEN('Translation-EN'!D2438)>0,'Translation-EN'!D2438,\"\")","v":""},"Île-du-Prince-Édouard"]
[{"$f":"IF(LEN('Translation-EN'!A2439)>0,'Translation-EN'!A2439,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2439)>0,'Translation-EN'!B2439,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2439)>0,'Translation-EN'!C2439,\"\")","v":"C4"},{"$f":"IF(LEN('Translation-EN'!D2439)>0,'Translation-EN'!D2439,\"\")","v":""},"Nouvelle-Écosse"]
[{"$f":"IF(LEN('Translation-EN'!A2440)>0,'Translation-EN'!A2440,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2440)>0,'Translation-EN'!B2440,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2440)>0,'Translation-EN'!C2440,\"\")","v":"C5"},{"$f":"IF(LEN('Translation-EN'!D2440)>0,'Translation-EN'!D2440,\"\")","v":""},"Nouveau-Brunswick"]
[{"$f":"IF(LEN('Translation-EN'!A2441)>0,'Translation-EN'!A2441,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2441)>0,'Translation-EN'!B2441,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2441)>0,'Translation-EN'!C2441,\"\")","v":"C6"},{"$f":"IF(LEN('Translation-EN'!D2441)>0,'Translation-EN'!D2441,\"\")","v":""},"Québec"]
[{"$f":"IF(LEN('Translation-EN'!A2442)>0,'Translation-EN'!A2442,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2442)>0,'Translation-EN'!B2442,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2442)>0,'Translation-EN'!C2442,\"\")","v":"C7"},{"$f":"IF(LEN('Translation-EN'!D2442)>0,'Translation-EN'!D2442,\"\")","v":""},"Ontario"]
[{"$f":"IF(LEN('Translation-EN'!A2443)>0,'Translation-EN'!A2443,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2443)>0,'Translation-EN'!B2443,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2443)>0,'Translation-EN'!C2443,\"\")","v":"C8"},{"$f":"IF(LEN('Translation-EN'!D2443)>0,'Translation-EN'!D2443,\"\")","v":""},"Manitoba"]
[{"$f":"IF(LEN('Translation-EN'!A2444)>0,'Translation-EN'!A2444,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2444)>0,'Translation-EN'!B2444,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2444)>0,'Translation-EN'!C2444,\"\")","v":"C9"},{"$f":"IF(LEN('Translation-EN'!D2444)>0,'Translation-EN'!D2444,\"\")","v":""},"Saskatchewan"]
[{"$f":"IF(LEN('Translation-EN'!A2445)>0,'Translation-EN'!A2445,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2445)>0,'Translation-EN'!B2445,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2445)>0,'Translation-EN'!C2445,\"\")","v":"C10"},{"$f":"IF(LEN('Translation-EN'!D2445)>0,'Translation-EN'!D2445,\"\")","v":""},"Alberta"]
[{"$f":"IF(LEN('Translation-EN'!A2446)>0,'Translation-EN'!A2446,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2446)>0,'Translation-EN'!B2446,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2446)>0,'Translation-EN'!C2446,\"\")","v":"C11"},{"$f":"IF(LEN('Translation-EN'!D2446)>0,'Translation-EN'!D2446,\"\")","v":""},"Colombie-Britannique"]
[{"$f":"IF(LEN('Translation-EN'!A2447)>0,'Translation-EN'!A2447,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2447)>0,'Translation-EN'!B2447,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2447)>0,'Translation-EN'!C2447,\"\")","v":"C12"},{"$f":"IF(LEN('Translation-EN'!D2447)>0,'Translation-EN'!D2447,\"\")","v":""},"Yukon"]
[{"$f":"IF(LEN('Translation-EN'!A2448)>0,'Translation-EN'!A2448,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2448)>0,'Translation-EN'!B2448,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2448)>0,'Translation-EN'!C2448,\"\")","v":"C13"},{"$f":"IF(LEN('Translation-EN'!D2448)>0,'Translation-EN'!D2448,\"\")","v":""},"Territoires du Nord-Ouest"]
[{"$f":"IF(LEN('Translation-EN'!A2449)>0,'Translation-EN'!A2449,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2449)>0,'Translation-EN'!B2449,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2449)>0,'Translation-EN'!C2449,\"\")","v":"C14"},{"$f":"IF(LEN('Translation-EN'!D2449)>0,'Translation-EN'!D2449,\"\")","v":""},"Nunavut"]
[{"$f":"IF(LEN('Translation-EN'!A2450)>0,'Translation-EN'!A2450,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2450)>0,'Translation-EN'!B2450,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2450)>0,'Translation-EN'!C2450,\"\")","v":"C15"},{"$f":"IF(LEN('Translation-EN'!D2450)>0,'Translation-EN'!D2450,\"\")","v":""},"Remplacer la province"]
[{"$f":"IF(LEN('Translation-EN'!A2451)>0,'Translation-EN'!A2451,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2451)>0,'Translation-EN'!B2451,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2451)>0,'Translation-EN'!C2451,\"\")","v":"C16"},{"$f":"IF(LEN('Translation-EN'!D2451)>0,'Translation-EN'!D2451,\"\")","v":""},"Remplacer la valeur"]
[{"$f":"IF(LEN('Translation-EN'!A2452)>0,'Translation-EN'!A2452,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2452)>0,'Translation-EN'!B2452,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2452)>0,'Translation-EN'!C2452,\"\")","v":"C17"},{"$f":"IF(LEN('Translation-EN'!D2452)>0,'Translation-EN'!D2452,\"\")","v":""},"Source d’information"]
[{"$f":"IF(LEN('Translation-EN'!A2453)>0,'Translation-EN'!A2453,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2453)>0,'Translation-EN'!B2453,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2453)>0,'Translation-EN'!C2453,\"\")","v":"C19"},{"$f":"IF(LEN('Translation-EN'!D2453)>0,'Translation-EN'!D2453,\"\")","v":""},"Résultats des calculs de GES"]
[{"$f":"IF(LEN('Translation-EN'!A2454)>0,'Translation-EN'!A2454,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2454)>0,'Translation-EN'!B2454,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2454)>0,'Translation-EN'!C2454,\"\")","v":"A20"},{"$f":"IF(LEN('Translation-EN'!D2454)>0,'Translation-EN'!D2454,\"\")","v":""},"Consommation de carburant à partir du fichier h2k "]
[{"$f":"IF(LEN('Translation-EN'!A2455)>0,'Translation-EN'!A2455,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2455)>0,'Translation-EN'!B2455,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2455)>0,'Translation-EN'!C2455,\"\")","v":"C20"},{"$f":"IF(LEN('Translation-EN'!D2455)>0,'Translation-EN'!D2455,\"\")","v":""},{"$f":"$E$2431","v":"Province"}]
[{"$f":"IF(LEN('Translation-EN'!A2456)>0,'Translation-EN'!A2456,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2456)>0,'Translation-EN'!B2456,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2456)>0,'Translation-EN'!C2456,\"\")","v":"D20"},{"$f":"IF(LEN('Translation-EN'!D2456)>0,'Translation-EN'!D2456,\"\")","v":""},"Électricité"]
[{"$f":"IF(LEN('Translation-EN'!A2457)>0,'Translation-EN'!A2457,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2457)>0,'Translation-EN'!B2457,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2457)>0,'Translation-EN'!C2457,\"\")","v":"E20"},{"$f":"IF(LEN('Translation-EN'!D2457)>0,'Translation-EN'!D2457,\"\")","v":""},"Gaz naturel"]
[{"$f":"IF(LEN('Translation-EN'!A2458)>0,'Translation-EN'!A2458,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2458)>0,'Translation-EN'!B2458,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2458)>0,'Translation-EN'!C2458,\"\")","v":"F20"},{"$f":"IF(LEN('Translation-EN'!D2458)>0,'Translation-EN'!D2458,\"\")","v":""},"Mazout"]
[{"$f":"IF(LEN('Translation-EN'!A2459)>0,'Translation-EN'!A2459,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2459)>0,'Translation-EN'!B2459,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2459)>0,'Translation-EN'!C2459,\"\")","v":"G20"},{"$f":"IF(LEN('Translation-EN'!D2459)>0,'Translation-EN'!D2459,\"\")","v":""},"Propane"]
[{"$f":"IF(LEN('Translation-EN'!A2460)>0,'Translation-EN'!A2460,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2460)>0,'Translation-EN'!B2460,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2460)>0,'Translation-EN'!C2460,\"\")","v":"H20"},{"$f":"IF(LEN('Translation-EN'!D2460)>0,'Translation-EN'!D2460,\"\")","v":""},"Bois"]
[{"$f":"IF(LEN('Translation-EN'!A2461)>0,'Translation-EN'!A2461,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2461)>0,'Translation-EN'!B2461,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2461)>0,'Translation-EN'!C2461,\"\")","v":"I20"},{"$f":"IF(LEN('Translation-EN'!D2461)>0,'Translation-EN'!D2461,\"\")","v":""},{"$f":"$E$1145","v":"Total"}]
[{"$f":"IF(LEN('Translation-EN'!A2462)>0,'Translation-EN'!A2462,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2462)>0,'Translation-EN'!B2462,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2462)>0,'Translation-EN'!C2462,\"\")","v":"A21"},{"$f":"IF(LEN('Translation-EN'!D2462)>0,'Translation-EN'!D2462,\"\")","v":""},"Électricité_kWh"]
[{"$f":"IF(LEN('Translation-EN'!A2463)>0,'Translation-EN'!A2463,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2463)>0,'Translation-EN'!B2463,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2463)>0,'Translation-EN'!C2463,\"\")","v":"C21"},{"$f":"IF(LEN('Translation-EN'!D2463)>0,'Translation-EN'!D2463,\"\")","v":""},{"$f":"$E$2437","v":"Terre-Neuve-et-Labrador"}]
[{"$f":"IF(LEN('Translation-EN'!A2464)>0,'Translation-EN'!A2464,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2464)>0,'Translation-EN'!B2464,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2464)>0,'Translation-EN'!C2464,\"\")","v":"A22"},{"$f":"IF(LEN('Translation-EN'!D2464)>0,'Translation-EN'!D2464,\"\")","v":""},"Gaz naturel_m3"]
[{"$f":"IF(LEN('Translation-EN'!A2465)>0,'Translation-EN'!A2465,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2465)>0,'Translation-EN'!B2465,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2465)>0,'Translation-EN'!C2465,\"\")","v":"C22"},{"$f":"IF(LEN('Translation-EN'!D2465)>0,'Translation-EN'!D2465,\"\")","v":""},{"$f":"$E$2438","v":"Île-du-Prince-Édouard"}]
[{"$f":"IF(LEN('Translation-EN'!A2466)>0,'Translation-EN'!A2466,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2466)>0,'Translation-EN'!B2466,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2466)>0,'Translation-EN'!C2466,\"\")","v":"A23"},{"$f":"IF(LEN('Translation-EN'!D2466)>0,'Translation-EN'!D2466,\"\")","v":""},"Mazout_Litres"]
[{"$f":"IF(LEN('Translation-EN'!A2467)>0,'Translation-EN'!A2467,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2467)>0,'Translation-EN'!B2467,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2467)>0,'Translation-EN'!C2467,\"\")","v":"C23"},{"$f":"IF(LEN('Translation-EN'!D2467)>0,'Translation-EN'!D2467,\"\")","v":""},{"$f":"$E$2439","v":"Nouvelle-Écosse"}]
[{"$f":"IF(LEN('Translation-EN'!A2468)>0,'Translation-EN'!A2468,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2468)>0,'Translation-EN'!B2468,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2468)>0,'Translation-EN'!C2468,\"\")","v":"A24"},{"$f":"IF(LEN('Translation-EN'!D2468)>0,'Translation-EN'!D2468,\"\")","v":""},"Propane_Litres"]
[{"$f":"IF(LEN('Translation-EN'!A2469)>0,'Translation-EN'!A2469,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2469)>0,'Translation-EN'!B2469,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2469)>0,'Translation-EN'!C2469,\"\")","v":"C24"},{"$f":"IF(LEN('Translation-EN'!D2469)>0,'Translation-EN'!D2469,\"\")","v":""},{"$f":"$E$2440","v":"Nouveau-Brunswick"}]
[{"$f":"IF(LEN('Translation-EN'!A2470)>0,'Translation-EN'!A2470,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2470)>0,'Translation-EN'!B2470,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2470)>0,'Translation-EN'!C2470,\"\")","v":"A25"},{"$f":"IF(LEN('Translation-EN'!D2470)>0,'Translation-EN'!D2470,\"\")","v":""},"Bois_Kg"]
[{"$f":"IF(LEN('Translation-EN'!A2471)>0,'Translation-EN'!A2471,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2471)>0,'Translation-EN'!B2471,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2471)>0,'Translation-EN'!C2471,\"\")","v":"C25"},{"$f":"IF(LEN('Translation-EN'!D2471)>0,'Translation-EN'!D2471,\"\")","v":""},{"$f":"$E$2441","v":"Québec"}]
[{"$f":"IF(LEN('Translation-EN'!A2472)>0,'Translation-EN'!A2472,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2472)>0,'Translation-EN'!B2472,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2472)>0,'Translation-EN'!C2472,\"\")","v":"C26"},{"$f":"IF(LEN('Translation-EN'!D2472)>0,'Translation-EN'!D2472,\"\")","v":""},{"$f":"$E$2442","v":"Ontario"}]
[{"$f":"IF(LEN('Translation-EN'!A2473)>0,'Translation-EN'!A2473,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2473)>0,'Translation-EN'!B2473,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2473)>0,'Translation-EN'!C2473,\"\")","v":"C27"},{"$f":"IF(LEN('Translation-EN'!D2473)>0,'Translation-EN'!D2473,\"\")","v":""},{"$f":"$E$2443","v":"Manitoba"}]
[{"$f":"IF(LEN('Translation-EN'!A2474)>0,'Translation-EN'!A2474,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2474)>0,'Translation-EN'!B2474,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2474)>0,'Translation-EN'!C2474,\"\")","v":"C28"},{"$f":"IF(LEN('Translation-EN'!D2474)>0,'Translation-EN'!D2474,\"\")","v":""},{"$f":"$E$2444","v":"Saskatchewan"}]
[{"$f":"IF(LEN('Translation-EN'!A2475)>0,'Translation-EN'!A2475,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2475)>0,'Translation-EN'!B2475,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2475)>0,'Translation-EN'!C2475,\"\")","v":"C29"},{"$f":"IF(LEN('Translation-EN'!D2475)>0,'Translation-EN'!D2475,\"\")","v":""},{"$f":"$E$2445","v":"Alberta"}]
[{"$f":"IF(LEN('Translation-EN'!A2476)>0,'Translation-EN'!A2476,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2476)>0,'Translation-EN'!B2476,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2476)>0,'Translation-EN'!C2476,\"\")","v":"C30"},{"$f":"IF(LEN('Translation-EN'!D2476)>0,'Translation-EN'!D2476,\"\")","v":""},{"$f":"$E$2446","v":"Colombie-Britannique"}]
[{"$f":"IF(LEN('Translation-EN'!A2477)>0,'Translation-EN'!A2477,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2477)>0,'Translation-EN'!B2477,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2477)>0,'Translation-EN'!C2477,\"\")","v":"C31"},{"$f":"IF(LEN('Translation-EN'!D2477)>0,'Translation-EN'!D2477,\"\")","v":""},{"$f":"$E$2447","v":"Yukon"}]
[{"$f":"IF(LEN('Translation-EN'!A2478)>0,'Translation-EN'!A2478,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2478)>0,'Translation-EN'!B2478,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2478)>0,'Translation-EN'!C2478,\"\")","v":"A32"},{"$f":"IF(LEN('Translation-EN'!D2478)>0,'Translation-EN'!D2478,\"\")","v":""},"Renouvelables_GJ"]
[{"$f":"IF(LEN('Translation-EN'!A2479)>0,'Translation-EN'!A2479,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2479)>0,'Translation-EN'!B2479,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2479)>0,'Translation-EN'!C2479,\"\")","v":"C32"},{"$f":"IF(LEN('Translation-EN'!D2479)>0,'Translation-EN'!D2479,\"\")","v":""},{"$f":"$E$2448","v":"Territoires du Nord-Ouest"}]
[{"$f":"IF(LEN('Translation-EN'!A2480)>0,'Translation-EN'!A2480,\"\")","v":"Range"},{"$f":"IF(LEN('Translation-EN'!B2480)>0,'Translation-EN'!B2480,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2480)>0,'Translation-EN'!C2480,\"\")","v":"C33"},{"$f":"IF(LEN('Translation-EN'!D2480)>0,'Translation-EN'!D2480,\"\")","v":""},{"$f":"$E$2449","v":"Nunavut"}]
[{"$f":"IF(LEN('Translation-EN'!A2481)>0,'Translation-EN'!A2481,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2481)>0,'Translation-EN'!B2481,\"\")","v":"Introduction"},{"$f":"IF(LEN('Translation-EN'!C2481)>0,'Translation-EN'!C2481,\"\")","v":"TextBox 8"},{"$f":"IF(LEN('Translation-EN'!D2481)>0,'Translation-EN'!D2481,\"\")","v":true},"RNCan tient à souligner la contribution fondamentale de Chris Magwood et de l’équipe de Builders for Climate Action. L’estimateur d’émissions de carbone des matériaux (MCE2) a été créé conjointement par l’équipe de Builders for Climate Action (https://www.buildersforclimateaction.org/) et RNCan. Il soutient la mission de Builders for Climate Action qui consiste à : « offrir aux générations futures nos meilleurs efforts pour freiner les pires effets du changement climatique par une action intelligente, coordonnée et efficace pour réduire les émissions du secteur tout en créant un monde juste et équitable » et le mandat de RNCan qui consiste à aider l’industrie à prendre des décisions éclairées en matière de performance énergétique et de réduction de carbone dans l’environnement bâti.  "]
[{"$f":"IF(LEN('Translation-EN'!A2482)>0,'Translation-EN'!A2482,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2482)>0,'Translation-EN'!B2482,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2482)>0,'Translation-EN'!C2482,\"\")","v":"msgBVT"},{"$f":"IF(LEN('Translation-EN'!D2482)>0,'Translation-EN'!D2482,\"\")","v":""},"Attention : le bâtiment est modélisé avec un nombre particulier d'étages (<~NoOfStoreys~>). Veuillez spécifier manuellement la surface totale du plafond."]
[{"$f":"IF(LEN('Translation-EN'!A2483)>0,'Translation-EN'!A2483,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2483)>0,'Translation-EN'!B2483,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2483)>0,'Translation-EN'!C2483,\"\")","v":"msgCTR"},{"$f":"IF(LEN('Translation-EN'!D2483)>0,'Translation-EN'!D2483,\"\")","v":""},"Erreur : aucun résultat n'a été trouvé. Veuillez exécuter 'calculs' dans HOT2000 et réessayer."]
[{"$f":"IF(LEN('Translation-EN'!A2484)>0,'Translation-EN'!A2484,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2484)>0,'Translation-EN'!B2484,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2484)>0,'Translation-EN'!C2484,\"\")","v":"msgVIU"},{"$f":"IF(LEN('Translation-EN'!D2484)>0,'Translation-EN'!D2484,\"\")","v":""},"Erreur : Veuillez sélectionner un fichier .h2k"]
[{"$f":"IF(LEN('Translation-EN'!A2485)>0,'Translation-EN'!A2485,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2485)>0,'Translation-EN'!B2485,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2485)>0,'Translation-EN'!C2485,\"\")","v":"msgXRT"},{"$f":"IF(LEN('Translation-EN'!D2485)>0,'Translation-EN'!D2485,\"\")","v":""},"Le scénario '<~new_SCN_Name~>' existe déjà. Veuillez sélectionner un nouveau nom."]
[{"$f":"IF(LEN('Translation-EN'!A2486)>0,'Translation-EN'!A2486,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2486)>0,'Translation-EN'!B2486,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2486)>0,'Translation-EN'!C2486,\"\")","v":"msgCTI"},{"$f":"IF(LEN('Translation-EN'!D2486)>0,'Translation-EN'!D2486,\"\")","v":""},"Vous avez déjà créé '<~MAX_SCENARIOS~>' scénarios. L'outil ne prend pas en charge les scénarios supplémentaires. Vous pouvez supprimer un scénario et réessayer."]
[{"$f":"IF(LEN('Translation-EN'!A2487)>0,'Translation-EN'!A2487,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2487)>0,'Translation-EN'!B2487,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2487)>0,'Translation-EN'!C2487,\"\")","v":"msgMTD"},{"$f":"IF(LEN('Translation-EN'!D2487)>0,'Translation-EN'!D2487,\"\")","v":""},"Le scénario '<~scn_Name~>' n'existe pas. Veuillez réessayer.","Nom de scénario"]
[{"$f":"IF(LEN('Translation-EN'!A2488)>0,'Translation-EN'!A2488,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2488)>0,'Translation-EN'!B2488,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2488)>0,'Translation-EN'!C2488,\"\")","v":"msgUOQ"},{"$f":"IF(LEN('Translation-EN'!D2488)>0,'Translation-EN'!D2488,\"\")","v":""},"Le scénario '<~scn_Name~>' est introuvable. Veuillez réessayer."]
[{"$f":"IF(LEN('Translation-EN'!A2489)>0,'Translation-EN'!A2489,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2489)>0,'Translation-EN'!B2489,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2489)>0,'Translation-EN'!C2489,\"\")","v":"msgVCU"},{"$f":"IF(LEN('Translation-EN'!D2489)>0,'Translation-EN'!D2489,\"\")","v":""},"Etes-vous sûr de vouloir supprimer le scénario '<~scn_Name~>' ?"," "]
[{"$f":"IF(LEN('Translation-EN'!A2490)>0,'Translation-EN'!A2490,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2490)>0,'Translation-EN'!B2490,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2490)>0,'Translation-EN'!C2490,\"\")","v":"msgUIM"},{"$f":"IF(LEN('Translation-EN'!D2490)>0,'Translation-EN'!D2490,\"\")","v":""},"L'adresse des cellules orange est enregistrée dans la feuille <~scnDBSh.Name~>."]
[{"$f":"IF(LEN('Translation-EN'!A2491)>0,'Translation-EN'!A2491,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2491)>0,'Translation-EN'!B2491,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2491)>0,'Translation-EN'!C2491,\"\")","v":"msgFVT"},{"$f":"IF(LEN('Translation-EN'!D2491)>0,'Translation-EN'!D2491,\"\")","v":""},"Veuillez entrer un nom pour votre scénario","Nom de scénario"]
[{"$f":"IF(LEN('Translation-EN'!A2492)>0,'Translation-EN'!A2492,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2492)>0,'Translation-EN'!B2492,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2492)>0,'Translation-EN'!C2492,\"\")","v":"msgEVU"},{"$f":"IF(LEN('Translation-EN'!D2492)>0,'Translation-EN'!D2492,\"\")","v":""},"Sélectionnez le fichier de maison (h2k)"]
[{"$f":"IF(LEN('Translation-EN'!A2493)>0,'Translation-EN'!A2493,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2493)>0,'Translation-EN'!B2493,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2493)>0,'Translation-EN'!C2493,\"\")","v":"msgVRG"},{"$f":"IF(LEN('Translation-EN'!D2493)>0,'Translation-EN'!D2493,\"\")","v":""},"Toutes les données sur la fiche \"SCÉNARIOS\" seront perdues.  Voulez-vous continuer ?","Alerte"]
[{"$f":"IF(LEN('Translation-EN'!A2494)>0,'Translation-EN'!A2494,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2494)>0,'Translation-EN'!B2494,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2494)>0,'Translation-EN'!C2494,\"\")","v":"msgCYT"},{"$f":"IF(LEN('Translation-EN'!D2494)>0,'Translation-EN'!D2494,\"\")","v":""},"Le changement de province modifie à la fois le facteur d'intensité des GES du réseau électrique et les mélanges de béton disponibles dans la région.  Si vous continuez, vos sélections actuelles de béton pour la <~Province_Name~> seront sauvegardées pour une utilisation ultérieure.  Vous devrez faire de nouvelles sélections de béton basées sur les mélanges disponibles dans la région pour la province de votre choix."]
[{"$f":"IF(LEN('Translation-EN'!A2495)>0,'Translation-EN'!A2495,\"\")","v":"MsgBox"},{"$f":"IF(LEN('Translation-EN'!B2495)>0,'Translation-EN'!B2495,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2495)>0,'Translation-EN'!C2495,\"\")","v":"msgNTR"},{"$f":"IF(LEN('Translation-EN'!D2495)>0,'Translation-EN'!D2495,\"\")","v":""},"Le changement de province modifie à la fois le facteur d'intensité des GES du réseau électrique et les mélanges de béton disponibles dans la région.  Les mélanges de béton sélectionnés précédemment pour la <~Province_Name~> seront chargés."]
[{"$f":"IF(LEN('Translation-EN'!A2496)>0,'Translation-EN'!A2496,\"\")","v":"Forms"},{"$f":"IF(LEN('Translation-EN'!B2496)>0,'Translation-EN'!B2496,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2496)>0,'Translation-EN'!C2496,\"\")","v":"frmSelectScenario"},{"$f":"IF(LEN('Translation-EN'!D2496)>0,'Translation-EN'!D2496,\"\")","v":""},"Sélectionnez un scénario"]
[{"$f":"IF(LEN('Translation-EN'!A2497)>0,'Translation-EN'!A2497,\"\")","v":"Forms"},{"$f":"IF(LEN('Translation-EN'!B2497)>0,'Translation-EN'!B2497,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2497)>0,'Translation-EN'!C2497,\"\")","v":"lblSelectScenToDelete"},{"$f":"IF(LEN('Translation-EN'!D2497)>0,'Translation-EN'!D2497,\"\")","v":"delete"},"Sélectionnez un scénario à supprimer"]
[{"$f":"IF(LEN('Translation-EN'!A2498)>0,'Translation-EN'!A2498,\"\")","v":"Forms"},{"$f":"IF(LEN('Translation-EN'!B2498)>0,'Translation-EN'!B2498,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2498)>0,'Translation-EN'!C2498,\"\")","v":"lblSelectScenToDelete"},{"$f":"IF(LEN('Translation-EN'!D2498)>0,'Translation-EN'!D2498,\"\")","v":"restore"},"Sélectionnez un scénario à restaurer"]
[{"$f":"IF(LEN('Translation-EN'!A2499)>0,'Translation-EN'!A2499,\"\")","v":"Forms"},{"$f":"IF(LEN('Translation-EN'!B2499)>0,'Translation-EN'!B2499,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2499)>0,'Translation-EN'!C2499,\"\")","v":"cmdCancel"},{"$f":"IF(LEN('Translation-EN'!D2499)>0,'Translation-EN'!D2499,\"\")","v":""},"Annuler"]
[{"$f":"IF(LEN('Translation-EN'!A2500)>0,'Translation-EN'!A2500,\"\")","v":"Forms"},{"$f":"IF(LEN('Translation-EN'!B2500)>0,'Translation-EN'!B2500,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2500)>0,'Translation-EN'!C2500,\"\")","v":"cmdOk"},{"$f":"IF(LEN('Translation-EN'!D2500)>0,'Translation-EN'!D2500,\"\")","v":""},"Sélectionnez"]
[{"$f":"IF(LEN('Translation-EN'!A2501)>0,'Translation-EN'!A2501,\"\")","v":"Forms"},{"$f":"IF(LEN('Translation-EN'!B2501)>0,'Translation-EN'!B2501,\"\")","v":""},{"$f":"IF(LEN('Translation-EN'!C2501)>0,'Translation-EN'!C2501,\"\")","v":"lblWaitMessage"},{"$f":"IF(LEN('Translation-EN'!D2501)>0,'Translation-EN'!D2501,\"\")","v":""},"Un moment s'il vous plaît…"]
[{"$f":"IF(LEN('Translation-EN'!A2502)>0,'Translation-EN'!A2502,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2502)>0,'Translation-EN'!B2502,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C2502)>0,'Translation-EN'!C2502,\"\")","v":"D19"},{"$f":"IF(LEN('Translation-EN'!D2502)>0,'Translation-EN'!D2502,\"\")","v":""},"Sélectionnez l'isolation parmi la liste déroulante, entrez la valeur R (à gauche, en unités impériales) et la superficie (à droite, en mètres carrés)."]
[{"$f":"IF(LEN('Translation-EN'!A2503)>0,'Translation-EN'!A2503,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2503)>0,'Translation-EN'!B2503,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C2503)>0,'Translation-EN'!C2503,\"\")","v":"D20"},{"$f":"IF(LEN('Translation-EN'!D2503)>0,'Translation-EN'!D2503,\"\")","v":""},{"$f":"$E$2502","v":"Sélectionnez l'isolation parmi la liste déroulante, entrez la valeur R (à gauche, en unités impériales) et la superficie (à droite, en mètres carrés)."}]
[{"$f":"IF(LEN('Translation-EN'!A2504)>0,'Translation-EN'!A2504,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2504)>0,'Translation-EN'!B2504,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C2504)>0,'Translation-EN'!C2504,\"\")","v":"D21"},{"$f":"IF(LEN('Translation-EN'!D2504)>0,'Translation-EN'!D2504,\"\")","v":""},{"$f":"$E$2502","v":"Sélectionnez l'isolation parmi la liste déroulante, entrez la valeur R (à gauche, en unités impériales) et la superficie (à droite, en mètres carrés)."}]
[{"$f":"IF(LEN('Translation-EN'!A2505)>0,'Translation-EN'!A2505,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2505)>0,'Translation-EN'!B2505,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2505)>0,'Translation-EN'!C2505,\"\")","v":"D15"},{"$f":"IF(LEN('Translation-EN'!D2505)>0,'Translation-EN'!D2505,\"\")","v":""},"Sélectionnez une province dont vous voulez remplacer le facteur de GES, puis entrez la nouvelle valeur de l'intensité des GES dans la cellule correspondante ci-dessous.\n  \nNote : un seul type de carburant d'une province peut être remplacé à la fois."]
[{"$f":"IF(LEN('Translation-EN'!A2506)>0,'Translation-EN'!A2506,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2506)>0,'Translation-EN'!B2506,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2506)>0,'Translation-EN'!C2506,\"\")","v":"E15"},{"$f":"IF(LEN('Translation-EN'!D2506)>0,'Translation-EN'!D2506,\"\")","v":""},{"$f":"E2505","v":"Sélectionnez une province dont vous voulez remplacer le facteur de GES, puis entrez la nouvelle valeur de l'intensité des GES dans la cellule correspondante ci-dessous.\n  \nNote : un seul type de carburant d'une province peut être remplacé à la fois."}]
[{"$f":"IF(LEN('Translation-EN'!A2507)>0,'Translation-EN'!A2507,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2507)>0,'Translation-EN'!B2507,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2507)>0,'Translation-EN'!C2507,\"\")","v":"F15"},{"$f":"IF(LEN('Translation-EN'!D2507)>0,'Translation-EN'!D2507,\"\")","v":""},{"$f":"E2505","v":"Sélectionnez une province dont vous voulez remplacer le facteur de GES, puis entrez la nouvelle valeur de l'intensité des GES dans la cellule correspondante ci-dessous.\n  \nNote : un seul type de carburant d'une province peut être remplacé à la fois."}]
[{"$f":"IF(LEN('Translation-EN'!A2508)>0,'Translation-EN'!A2508,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2508)>0,'Translation-EN'!B2508,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2508)>0,'Translation-EN'!C2508,\"\")","v":"G15"},{"$f":"IF(LEN('Translation-EN'!D2508)>0,'Translation-EN'!D2508,\"\")","v":""},"Sélectionnez une province dont vous voulez remplacer le facteur de GES, puis entrez la nouvelle valeur de l'intensité des GES dans la cellule correspondante ci-dessous.\n  \nNote : un seul type de carburant d'une province peut être remplacé à la fois."]
[{"$f":"IF(LEN('Translation-EN'!A2509)>0,'Translation-EN'!A2509,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2509)>0,'Translation-EN'!B2509,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2509)>0,'Translation-EN'!C2509,\"\")","v":"H15"},{"$f":"IF(LEN('Translation-EN'!D2509)>0,'Translation-EN'!D2509,\"\")","v":""},"Sélectionnez une province dont vous voulez remplacer le facteur de GES, puis entrez la nouvelle valeur de l'intensité des GES dans la cellule correspondante ci-dessous.\n  \nNote : un seul type de carburant d'une province peut être remplacé à la fois."]
[{"$f":"IF(LEN('Translation-EN'!A2510)>0,'Translation-EN'!A2510,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2510)>0,'Translation-EN'!B2510,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2510)>0,'Translation-EN'!C2510,\"\")","v":"D17"},{"$f":"IF(LEN('Translation-EN'!D2510)>0,'Translation-EN'!D2510,\"\")","v":""},"Indiquez la source d'information utilisée pour la valeur de remplacement. Un lien Internet est préférable, s'il est disponible."]
[{"$f":"IF(LEN('Translation-EN'!A2511)>0,'Translation-EN'!A2511,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2511)>0,'Translation-EN'!B2511,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2511)>0,'Translation-EN'!C2511,\"\")","v":"E17"},{"$f":"IF(LEN('Translation-EN'!D2511)>0,'Translation-EN'!D2511,\"\")","v":""},{"$f":"$E$2510","v":"Indiquez la source d'information utilisée pour la valeur de remplacement. Un lien Internet est préférable, s'il est disponible."}]
[{"$f":"IF(LEN('Translation-EN'!A2512)>0,'Translation-EN'!A2512,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2512)>0,'Translation-EN'!B2512,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2512)>0,'Translation-EN'!C2512,\"\")","v":"F17"},{"$f":"IF(LEN('Translation-EN'!D2512)>0,'Translation-EN'!D2512,\"\")","v":""},{"$f":"$E$2510","v":"Indiquez la source d'information utilisée pour la valeur de remplacement. Un lien Internet est préférable, s'il est disponible."}]
[{"$f":"IF(LEN('Translation-EN'!A2513)>0,'Translation-EN'!A2513,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2513)>0,'Translation-EN'!B2513,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2513)>0,'Translation-EN'!C2513,\"\")","v":"G17"},{"$f":"IF(LEN('Translation-EN'!D2513)>0,'Translation-EN'!D2513,\"\")","v":""},{"$f":"$E$2510","v":"Indiquez la source d'information utilisée pour la valeur de remplacement. Un lien Internet est préférable, s'il est disponible."}]
[{"$f":"IF(LEN('Translation-EN'!A2514)>0,'Translation-EN'!A2514,\"\")","v":"Validation.InputMessage"},{"$f":"IF(LEN('Translation-EN'!B2514)>0,'Translation-EN'!B2514,\"\")","v":"Energy GHG"},{"$f":"IF(LEN('Translation-EN'!C2514)>0,'Translation-EN'!C2514,\"\")","v":"H17"},{"$f":"IF(LEN('Translation-EN'!D2514)>0,'Translation-EN'!D2514,\"\")","v":""},{"$f":"$E$2510","v":"Indiquez la source d'information utilisée pour la valeur de remplacement. Un lien Internet est préférable, s'il est disponible."}]
[{"$f":"IF(LEN('Translation-EN'!A2515)>0,'Translation-EN'!A2515,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2515)>0,'Translation-EN'!B2515,\"\")","v":"Footings & Slabs"},{"$f":"IF(LEN('Translation-EN'!C2515)>0,'Translation-EN'!C2515,\"\")","v":"Rounded Rectangle 2||Rectangle: Rounded Corners 2"},{"$f":"IF(LEN('Translation-EN'!D2515)>0,'Translation-EN'!D2515,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2516)>0,'Translation-EN'!A2516,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2516)>0,'Translation-EN'!B2516,\"\")","v":"Foundation Walls"},{"$f":"IF(LEN('Translation-EN'!C2516)>0,'Translation-EN'!C2516,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2516)>0,'Translation-EN'!D2516,\"\")","v":""},{"$f":"$E$2515","v":"Effacer cette fiche seulement"}]
[{"$f":"IF(LEN('Translation-EN'!A2517)>0,'Translation-EN'!A2517,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2517)>0,'Translation-EN'!B2517,\"\")","v":"Structural Elements"},{"$f":"IF(LEN('Translation-EN'!C2517)>0,'Translation-EN'!C2517,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2517)>0,'Translation-EN'!D2517,\"\")","v":""},{"$f":"$E$2515","v":"Effacer cette fiche seulement"}]
[{"$f":"IF(LEN('Translation-EN'!A2518)>0,'Translation-EN'!A2518,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2518)>0,'Translation-EN'!B2518,\"\")","v":"Ext. Walls"},{"$f":"IF(LEN('Translation-EN'!C2518)>0,'Translation-EN'!C2518,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2518)>0,'Translation-EN'!D2518,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2519)>0,'Translation-EN'!A2519,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2519)>0,'Translation-EN'!B2519,\"\")","v":"Ext. Wall Systems"},{"$f":"IF(LEN('Translation-EN'!C2519)>0,'Translation-EN'!C2519,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2519)>0,'Translation-EN'!D2519,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2520)>0,'Translation-EN'!A2520,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2520)>0,'Translation-EN'!B2520,\"\")","v":"Party Walls"},{"$f":"IF(LEN('Translation-EN'!C2520)>0,'Translation-EN'!C2520,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2520)>0,'Translation-EN'!D2520,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2521)>0,'Translation-EN'!A2521,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2521)>0,'Translation-EN'!B2521,\"\")","v":"Cladding"},{"$f":"IF(LEN('Translation-EN'!C2521)>0,'Translation-EN'!C2521,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2521)>0,'Translation-EN'!D2521,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2522)>0,'Translation-EN'!A2522,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2522)>0,'Translation-EN'!B2522,\"\")","v":"Windows"},{"$f":"IF(LEN('Translation-EN'!C2522)>0,'Translation-EN'!C2522,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2522)>0,'Translation-EN'!D2522,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2523)>0,'Translation-EN'!A2523,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2523)>0,'Translation-EN'!B2523,\"\")","v":"Int. Walls"},{"$f":"IF(LEN('Translation-EN'!C2523)>0,'Translation-EN'!C2523,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2523)>0,'Translation-EN'!D2523,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2524)>0,'Translation-EN'!A2524,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2524)>0,'Translation-EN'!B2524,\"\")","v":"Floors"},{"$f":"IF(LEN('Translation-EN'!C2524)>0,'Translation-EN'!C2524,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2524)>0,'Translation-EN'!D2524,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2525)>0,'Translation-EN'!A2525,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2525)>0,'Translation-EN'!B2525,\"\")","v":"Ceilings"},{"$f":"IF(LEN('Translation-EN'!C2525)>0,'Translation-EN'!C2525,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2525)>0,'Translation-EN'!D2525,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2526)>0,'Translation-EN'!A2526,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2526)>0,'Translation-EN'!B2526,\"\")","v":"Roof"},{"$f":"IF(LEN('Translation-EN'!C2526)>0,'Translation-EN'!C2526,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2526)>0,'Translation-EN'!D2526,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2527)>0,'Translation-EN'!A2527,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2527)>0,'Translation-EN'!B2527,\"\")","v":"Garage"},{"$f":"IF(LEN('Translation-EN'!C2527)>0,'Translation-EN'!C2527,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2527)>0,'Translation-EN'!D2527,\"\")","v":""},"Effacer cette fiche seulement"]
[{"$f":"IF(LEN('Translation-EN'!A2528)>0,'Translation-EN'!A2528,\"\")","v":"Shape"},{"$f":"IF(LEN('Translation-EN'!B2528)>0,'Translation-EN'!B2528,\"\")","v":"User-Defined"},{"$f":"IF(LEN('Translation-EN'!C2528)>0,'Translation-EN'!C2528,\"\")","v":"Rounded Rectangle 1||Rectangle: Rounded Corners 1"},{"$f":"IF(LEN('Translation-EN'!D2528)>0,'Translation-EN'!D2528,\"\")","v":""},"Effacer cette fiche seulement"]
[]
[null,null,null,null,null,null,null,"© His Majesty the king in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,null,null,null,null,null,null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Cover_Couverture","index":2,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[[38,4,38,11],[7,2,17,5],[7,7,15,10],[18,2,35,5],[37,4,37,11],[18,7,35,10]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,"Material Carbon Emissions Estimator (MCE2)",null,null,null,null,"Estimateur d'émissions de carbone des matériaux  (E2CM)"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Disclaimer:\nNeither Natural Resources Canada nor any of its employees makes any warranty express or implied, or assumes any legal liability or responsibility for the accuracy, completeness or usefulness of its contents. Reference in the tool to any specific commercial product, process, service or organization does not necessarily constitute or imply endorsement, recommendation or favouring by Natural Resources Canada. The views and opinions of authors expressed in this tool do not necessarily state or reflect those of Natural Resources Canada.\n\nFunding for this work was provided by Natural Resources Canada through the Program of Energy Research and Development, Green Infrastructure program and the Office of Energy Efficiency, Housing and Communities Division.\n\nThis spreadsheet has been optimized for use in Microsoft Windows Excel versions 2016 onwards. Running the software on legacy versions of Microsoft Excel or other operating systems may not work.",null,null,null,null,"Avertissement :\nRessources naturelles Canada et aucun de ses employés ne font aucune garantie, formelle ou tacite, et n’assument aucune responsabilité légale ou autre à l’égard de l’exactitude, de l’exhaustivité ou de l’utilité du contenu du rapport. Toute référence dans l'outil à quelque produit, processus, service ou organisation que ce soit ne constitue pas nécessairement une approbation, une recommandation ou une préférence de la part de Ressources naturelles Canada. Les points de vue et les opinions exprimés par les auteurs dans cet outil ne sont pas et ne reflètent pas nécessairement ceux de Ressources naturelles Canada. \n\nCes travaux ont été réalisés grâce au financement fourni par Ressources naturelles Canada dans le cadre du Programme de recherche et de développement énergétiques, du programme Infrastructures vertes et de l’Office de l'efficacité énergétique, Division du logement et des collectivités.\n\nCette feuille de calcul a été optimisée pour être utilisée dans les versions 2016 et suivantes de Microsoft Windows Excel. L'exécution du logiciel sur des versions antérieures de Microsoft Excel ou d'autres systèmes d'exploitation pourrait ne pas fonctionner. "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,null,null,null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"License","index":3,"n_rows":57,"n_cols":5,"rows_kept":57,"cut":false,"hidden":false,"merged":[]}
[]
[null,"License Agreement",null,null,"Accord de licence"]
[]
[null,"THIS END-USER LICENCE AGREEMENT (EULA) IS A LEGAL AGREEMENT BETWEEN YOU, THE END-USER, IN YOUR CAPACITY AS AN INDIVIDUAL AND/OR AS AN AGENT FOR YOUR COMPANY, INSTITUTION OR OTHER ENTITY (hereinafter referred to as the \"Licensee\"), AND HER MAJESTY THE QUEEN IN RIGHT OF CANADA AS REPRESENTED BY THE MINISTER OF NATURAL RESOURCES (hereinafter referred to as \"NRCan\")",null,null,"LE PRÉSENT CONTRAT DE LICENCE D’UTILISATEUR FINAL (CLUF) EST UN ACCORD JURIDIQUE ENTRE VOUS, L’UTILISATEUR FINAL, EN VOTRE QUALITÉ DE PERSONNE PHYSIQUE ET/OU D’AGENT DE VOTRE ENTREPRISE, INSTITUTION OU AUTRE ENTITÉ (ci-après dénommé le « Licencié »), ET SA MAJESTÉ LA REINE DU CHEF DU CANADA, REPRÉSENTÉE PAR LE MINISTRE DES RESSOURCES NATURELLES (ci -après dénommé « RNCan »)\n"]
[]
[null,"WHEREAS NRCAN HAS THE RIGHT TO GRANT A LICENSE FOR THE NRCAN MATERIALS EMISSIONS ESTIMATOR, AN EXCEL BASED MATERIALS EMISSIONS CALCULATOR THAT ALLOWS USERS TO ESTIMATE THE FIRST CARBON IMPACT OF THEIR HOMES, COMPARE THIS WITH THE OPERATIONAL CARBON ESTIMATES DERIVED FROM HOT2000, AND ENABLE INDUSTRY TO CONSIDER TRADE-OFFS ON MATERIAL SELECTIONS THAT WILL RESULT IN A LOWER CARBON FOOTPRINT OF THE HOME (hereinafter referred to as the “Software”)",null,null,"ATTENDU QUE RNCAN AFFIRME QU’IL A TOUS LES POUVOIRS NÉCESSAIRES POUR OCTROYER UNE LICENCE POUR UN ESTIMATEUR D'ÉMISSIONS DE MATIÈRES DE RNCAN, UN CALCULATEUR D'ÉMISSIONS DE MATIÈRES BASÉ SUR EXCEL QUI PERMET AUX UTILISATEURS D'ESTIMER LE PREMIER IMPACT DE CARBONE DE LEURS MAISONS, LE COMPARER AVEC LES ESTIMATIONS OPÉRATIONNELLES DE CARBONE DÉRIVÉES DE HOT2000, ET PERMET À L'INDUSTRIE D'ENVISAGER DES COMPROMIS SUR LES SÉLECTIONS DE MATÉRIAUX AFIN DE RÉDUIRE L'EMPREINTE DE CARBONE DE LA MAISON (ci-après appelé le « Logiciel »)\n"]
[]
[null,"BY DOWNLOADING, INSTALLING, USING OR COPYING THE SOFTWARE THE LICENSEE HEREBY AGREES TO ADHERE TO THE TERMS AND CONDITIONS BELOW:\n",null,null,"EN TÉLÉCHARGEANT, INSTALLANT, UTILISANT OU COPIANT LE LOGICIEL LE LICENCIÉ CONVIENT PAR LES PRÉSENTES D’ADHÉRER AUX CONDITIONS GÉNÉRALES CI-DESSOUS:"]
[]
[1," GRANT OF LICENSE",null,1,"OCTROI DE LA LICENCE"]
[1.1000000000000001," Upon the terms and conditions hereinafter set forth, NRCan hereby grants to you, the Licensee, a non-exclusive license to use the Software. ",null,1.1000000000000001,"Aux termes des conditions générales énoncées ci-après, RNCan accorde par les présentes, à vous le Licencié, une licence non exclusive d’utilisation du Logiciel."]
[1.2,"The Licensee shall not disclose, modify, sell, sublicense, loan, transfer, reverse-engineer the Software, or otherwise assign any rights under this EULA to any third party.",null,1.2,"Le Licencié ne doit pas divulguer, modifier, vendre, prêter ou transférer le Logiciel, accorder une sous-licence à son égard ou en faire l’ingénierie inverse ni céder de toute autre manière à un tiers les droits prévus par le présent CLUF.\n"]
[1.3," Subject to Article 8.2, the Licensee shall not make more than one (1) backup copy of the Software. The backup copy shall be held confidential and shall be used only for the purpose of backup.",null,1.3,"Sous réserve de l’article 8.2, le Licencié ne peut faire plus d’une (1) copie de sauvegarde du Logiciel. La copie de sauvegarde doit être tenue confidentielle et n’être utilisée qu’à des fins de sauvegarde.\n"]
[]
[2," TERM",null,2,"DURÉE"]
[2.1," This EULA shall come into force upon the first instance that the Software is used by the Licensee or comes into the possession of the Licensee, and shall remain in force until the Licensee destroys all copies of the Software.",null,2.1,"Le présent CLUF entre en vigueur dès la première utilisation du Logiciel par le Licencié ou dès que le Licencié en prend possession et demeure en vigueur jusqu’à ce qu’il soit résilié par le Licencié à la suite de la destruction par celui-ci de toutes les copies du Logiciel."]
[]
[3," OBLIGATIONS OF THE LICENSEE",null,3,"OBLIGATIONS DU LICENCIÉ"]
[3.1," The Licensee shall not make any statement or representation indicating that NRCan or the Government of Canada endorses or approves any recommendation, study, report, product, service or course of action as a result of the Licensee's use of the Software.",null,3.1,"Le Licencié ne doit faire aucune déclaration ni représentation indiquant que RNCan ou le Gouvernement du Canada appuie ou approuve une recommandation, une étude, un rapport, un produit, un service ou une ligne de conduite à la suite de l’utilisation du Logiciel par le Licencié.\n"]
[3.2," The Licensee’s publications referring to the Software must state the origin of the Software using the following text: \"NRCan’s Materials Emissions Estimator is owned by Her Majesty the Queen in Right of Canada as represented by the Minister Natural Resources © 2021\". The Licensee shall seek prior written approval for any other statements concerning NRCan beyond the origin of the Software.",null,3.2,"Les publications du Licencié faisant référence au Logiciel doivent indiquer l’origine du Logiciel au moyen du texte suivant : « Le logiciel Estimateur D'Émissions De Matières appartient à Sa Majesté la Reine du chef du Canada représentée par le Ministre des Ressources naturelles © 2021 ». Le Licencié doit demandé l’approbation écrite préalable pour toute autre déclaration concernant RNCan qui va au-delà de l’origine du Logiciel."]
[]
[4," MAINTENANCE AND SUPPORT ",null,4," MAINTENANCE ET SOUTIEN\n"]
[4.0999999999999996,"The parties understand and agree that while the Licensee may report any bugs or technical malfunctions in the Software to NRCan, NRCan is under no obligation to provide technical support, maintenance services, update services, notices of latent defects, or correction of defects for the Software.",null,4.0999999999999996,"Les parties comprennent et conviennent que, bien que le Licencié puisse signaler à RNCan tout bogue ou toute défectuosité technique du Logiciel, RNCan n’est pas tenu de fournir un soutien technique, des services de maintenance, des services de mise à jour, des avis de vices cachés ni d’assurer la correction de défauts pour le Logiciel.\n"]
[]
[5," TITLE ",null,5," TITRE\n"]
[5.0999999999999996,"The Licensee agrees that the Software is and shall at all times remain the property of NRCan. The Licensee shall have no right, title and interest therein or thereto, except as expressly set forth in this EULA. ",null,5.0999999999999996,"Le Licencié convient que le Logiciel est, et demeurera en tout temps, la propriété de RNCan. Le Licencié n’a aucun droit, titre ni intérêt à son égard et s’y afférant, sauf dans la mesure expressément prévue dans le présent CLUF."]
[5.2," The Licensee acknowledges that the Software is protected under the Copyright Act.",null,5.2,"Le Licencié reconnaît que le Logiciel est protégé par la Loi sur le droit d’auteur."]
[]
[6," WARRANTY AND INDEMNITY",null,6,"GARANTIE ET INDEMNISATION"]
[6.1,"The Software is licensed on an \"AS IS\" basis. NRCan makes no guarantees, representations, or warranties respecting the Software, either express or implied, arising by law or otherwise, including but not limited to effectiveness, completeness, accuracy, or fitness for a particular purpose. ",null,6.1,"Une licence est octroyée pour le Logiciel « tel quel ». RNCan ne fait à l’égard du Logiciel aucune représentation ou garantie, expresse ou tacite, découlant de la loi ou d’autres sources, y compris, mais sans toutefois s’y limiter son efficacité, son intégralité, son exactitude ou son utilité à des fins particulières. "]
[6.2," NRCan shall not be liable in respect of any claim, demand or action, irrespective of the nature of the cause of the claim, demand or action alleging any loss, injury or damages, direct or indirect, which may result from the Licensee’s use or possession of the Software. NRCan shall not be liable in any way for loss of revenue or contracts, or any other consequential loss of any kind resulting from the Licensee’s use or possession of the Software. ",null,6.2,"RNCan ne peut être tenu responsable en cas de réclamations, de revendications ou d’actions en justice, quelle qu’en soit la nature de la cause, alléguant des pertes, des préjudices ou des dommages, directs ou indirects, pouvant résulter de la possession ou de l ’utilisation du Logiciel par le Licencié. RNCan ne peut aucunement être tenu responsable de la perte de revenus ou de contrats, ou de toute autre perte conséquente de quelque nature que ce soit, découlant de la possession ou de l ’utilisation du Logiciel par le Licencié. "]
[6.3," The Licensee shall indemnify and defend NRCan, its employees, contractors, agents and suppliers, from and against all claims, demands, losses, damages, costs (including legal fees and costs on a substantial indemnity basis), actions, suits or proceedings brought by any third party, that are in any manner based upon, arising out of, or attributable to the use, possession, or performance of the Software by the Licensee, or it’s employees or agents.",null,6.3," Le Licencié indemnisera et défendra RNCan, ses employés, ses contractants, ses mandataires et ses fournisseurs en cas de réclamations, demandes, pertes, dommages, coûts (y compris les frais juridiques et les coûts sur une base d’indemnité substantielle), actions, poursuites ou procédures intentées par un tiers, étant de quelque manière que ce soit fondés sur, attribuables à ou issus de la possession, l’utilisation ou de la performance du Logiciel par le Licencié, ses employés ou ses mandataires."]
[]
[7," TERMINATION",null,7,"RÉSILIATION"]
[7.1," Subject to Article 8.2, if the Licensee breaches any obligation under this EULA and fails to remedy the breach within thirty (30) calendar days, the present EULA is deemed to be terminated immediately without any notice. ",null,7.1,"Sous réserve de l’article 8.2, si le Licencié manque à une obligation en vertu du présent CLUF et n’y remédie pas dans un délai de trente (30) jours civils, le présent CLUF est réputé avoir été résilié immédiatement sans préavis."]
[7.2," Notwithstanding any other provisions in this agreement, Articles 3.1 and 3.2 shall survive termination of this EULA.",null,7.2," Nonobstant toute autre disposition du présent contrat, les articles 3.1 et 3.2 restent en vigueur après la fin du présent CLUF.\n"]
[]
[8," DESTRUCTION ",null,8,"DESTRUCTION"]
[8.1," Prior to assigning, selling or otherwise disposing of any media, the Licensee shall completely erase or otherwise destroy any Software contained on such media. ",null,8.1,"Avant de céder, de vendre ou d’aliéner autrement un médium (électronique ou autre), le Licencié doit effacer ou autrement détruire toute version du Logiciel contenue sur ce médium.\n"]
[8.1999999999999993," Upon termination of the Agreement, the Licensee agrees to either: ",null,8.1999999999999993,"À la résiliation ou à l’expiration du CLUF, le Licencié convient de ce qui suit :"]
[null,"(1) Return to NRCan immediately all copies of the Software and any related documentation and completely erase or otherwise destroy the backup copy of the Software provided for under Article 1.3 on the Licensee’s media; or ",null,null,"(1) retourner immédiatement à RNCan toutes les copies du Logiciel et toute documentation connexe, et effacer complètement ou détruire de toute autre manière la copie de sauvegarde du Logiciel prévue à l’article 1.3 sur le médium du Licencié, ou"]
[null,"(2) Completely erase or otherwise destroy all copies of the Software, including but not limited to the backup copy provided for under Article 1.3, as well as any related documentation on the Licensee’s media.",null,null,"(2) effacer complètement ou détruire de toute autre manière toutes les copies du Logiciel, y compris, sans toutefois s’y limiter, la copie de sauvegarde prévue à l’article 1.3, ainsi que toute documentation connexe sur le médium du Licencié.\n"]
[]
[9," APPLICABLE LAW",null,9," DROIT APPLICABLE"]
[9.1," This EULA shall be interpreted in accordance with the provincial or territorial laws in force in Ontario, Canada.",null,9.1,"  Le présent CLUF est interprété conformément aux lois provinciales ou territoriales en vigueur en Ontario, au Canada."]
[]
[10," NOTICES ",null,10,"AVIS"]
[10.1,"All notices, inquiries and other communications hereunder shall be in writing and shall be deemed to have been duly given once confirmation is received after sending to NRCan:",null,10.1,"Les avis, les demandes de renseignements et les autres communications mentionnées aux présentes doivent se faire par écrit et sont réputés avoir été dûment donnés une fois que RNCan en a confirmé réception:"]
[]
[null,"Natural Resources Canada",null,null,"Ressources naturelles Canada\n"]
[null,"Intellectual Property Division",null,null,"Division de la propriété intellectuelle\n"]
[null,"NRCan.ipd-dpi.rncan@canada.ca",null,null,"NRCan.ipd-dpi.rncan@canada.ca"]
[]
[]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Introduction","index":4,"n_rows":71,"n_cols":2,"rows_kept":71,"cut":false,"hidden":false,"merged":[[59,1,59,2],[60,1,60,2],[62,1,62,2],[63,1,63,2],[66,1,66,2],[61,1,61,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[15,1,15,2],[3,1,3,2],[9,1,9,2],[4,1,4,2],[5,1,5,2],[7,1,7,2],[8,1,8,2],[10,1,10,2],[0,15,0,16],[0,17,0,18],[1,10,1,14],[1,15,1,16],[1,17,1,18],[16,1,16,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[17,1,17,2],[41,1,41,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[29,1,29,2],[33,1,33,2],[37,1,37,2],[38,1,38,2],[40,1,40,2]]}
["English"]
["November \n2023","Material Carbon Emissions Estimator (MCE2)"]
[null,"Notes on the use of this calculator:"]
[null,"1 - The results from this calculator are an estimate of the material carbon emissions (MCEs) of your finished construction project. These results can be considered in a similar vein as the results of a basic energy model for a home. Just as a simple energy model is a relatively good predictor of the comparative effectiveness of different efficiency strategies, such a model won’t necessarily tell you exactly how much energy the building will eventually use.  This calculator should be used to gauge the relative MCEs of different construction approaches to a home or renovation project. "]
[null,"2 - This calculator is not intended to be used as a program or compliance tool.  The calculator is intended to provide the homebuilding and renovating industry with knowledge tools to support decisions regarding to the relative MCEs of different construction approaches.  "]
[null,"3 - This calculator provides a range of possible material and construction technologies, but does not include every material available. Every effort has been made to include the most relevant information on common materials and systems at the time of publication.  Product manufacturers and suppliers whose product data is not included can provide NRCan with relevant Environmental Product Declaration (EPD) and product documentation, and these will be reviewed and included in a scheduled update (timing TBD)."]
[null,"Overview and Context:"]
[null,"This calculator is designed to compare the greenhouse gas (GHG) emissions of different building materials for residential construction. The comparative results can help users to make material selections to reduce the carbon footprint of the homes and renovations they are planning. "]
[null,"By combining the annual operational energy data from HOT2000 with this tool's estimate of their project's upfront MCEs, users will be able to review a plot of the cumulative carbon footprint of their home and renovation projects."]
[null,"This calculator allows users to compare materials on a component-by-component basis, as well by whole assemblies. The majority of a building’s high impact materials are represented in the calculator. NRCan has included a wide range of structure and enclosure assemblies and materials, as well as the main cladding, sheathing and finishing materials for residential construction."]
[null,"This calculator focuses on material carbon emissions (MCEs - often referred to as “embodied carbon”) because the high volume of emissions arising directly from the harvesting and production of building materials, represents a key opportunity to drive major emission reductions. Low-rise residential buildings average 150-400 kg of GHGs per square metre of floor area (25-75 tonnes for a 2,000 square foot home). Multiplied across all of the low-rise residential buildings constructed each year in Canada, this produces emissions that are equivalent to approximately 2 coal fired power plants."]
[null,"Canada recognizes this considerable source of GHGs. This calculator is designed to support the homebuilding and renovation industries in making informed material choices to reduce up-front carbon emission.  "]
[null,"By making informed material choices, a building with the same size, function and energy performance can dramatically reduce its MCEs. In fact, it is possible with materials available today to get the MCEs of buildings close to – and even below – zero. "]
[null,"This calculator is intended to open up a dialogue, and allows industry to take a leading role in moving the residential building industry from a driver of climate change, to a leader in carbon drawdown."]
[null,"Data for calculations:"]
[null,"The data for this calculator comes from published Environmental Product Declarations (EPDs). These documents provide the results of a “life cycle assessment” (LCA) that has been performed and reported according to product category rules (PCRs) defined and regulated by ISO standards. EPDs are performed or verified by a third party. EPDs cannot compare materials intended for different uses (ie. dimensional lumber to floor tiles). Even within the same product category, it can be difficult to compare EPD figures because the values expressed for each material may not be directly comparable (ie. kilograms of brick can’t be compared to square metres of wood siding). This calculator normalizes all of the values expressed in the source EPDs to ensure that appropriate types of materials are being compared in appropriate quantities (ie. square metres of brick and square metres of wood siding)."]
[null,"NRCan has worked to ensure that all material comparisons are equivalent, using standard product sizes, code norms and best practice to make this an “apples to apples” comparison. "]
[null,"Material options with pastel highlights in column M have received their carbon emissions data from sources other than an EPD and are denoted by the following legend:"]
[]
[null,"Data source: EPD includes phases A1-A3 and B1 (VOC off-gassing) "]
[null,"Data source: LCA Study"]
[null,"Data source: ICE Database (UK)"]
[null,"Data source: other than EPD, LCA or database."]
[null,"Data source: recently expired EPD"]
[]
[]
[]
[]
[null,"Limitations of This Calculator"]
[null,"It is important to note that this calculator has a number of limitations of which you should be aware. Please read this section carefully so that you are fully informed. "]
[]
[null,"There are several factors to keep in mind regarding this calculators’ accuracy:"]
[null,"1. All the data is based on publicly available Environmental Product Declarations (EPDs). "]
[null,"The calculations used to create an EPD can be compared to calculating the fuel mileage for a car or truck. A series of assumptions and generic data are used to predict the carbon footprint of a material. The rules for making EPDs ensure that these assumptions are similar for all products in a particular category, but this does not necessarily guarantee that the actual figure is a perfect representation of the actual emissions from manufacturing the material."]
[null,"A range of uncertainty from 5-25% is typical in EPDs."]
[]
[null,"2. Calculations may not reflect your practices."]
[null,"In order to make the calculator simple to use and to minimize the number of inputs, numerous assumptions have been made in the calculations for material quantities. To the best of our ability we have chosen factors that are well-established industry norms, but these norms may not reflect the actual design or execution of your building."]
[null,"While the quantities of materials we estimate in the calculator are unlikely to be a perfect match to your actual material use, the quantities are consistent between all the options we present. This means that the comparison of emissions between materials is accurate. For example, you may use more or less framing material than we have estimated for your project but the relative difference between the framing options as depicted by the calculator will be accurate."]
[null,"3. No waste factor for materials is included."]
[null,"Every construction project generates offcuts and waste. None of our calculations assume any waste factors due to the wide variation in on-site practices."]
[null,"If you would like your total emissions to reflect waste factors, you can add an appropriate percentage to each material category using the percentage function in Column F. "]
[null,"4. We have not included data for all of the components in a building."]
[null,"There are many materials that will go into your building that are not included here:"]
[null,"Mechanical, electrical and plumbing (MEP) systems and components"]
[null,"Damp-proofing, air/vapour barriers and membranes"]
[null,"Flashing, sealants, adhesives"]
[null,"Fasteners"]
[null,"Appliances and fixtures "]
[null,"Millwork, cabinetry and stairs"]
[null,"Paints, stains and surface finishes"]
[null,"There is currently limited data available in some of these categories and/or the quantities of materials and emissions would be quite similar (e.g. toilets and washing machines don’t have much variation in emissions for comparison according to the available data). "]
[null,"The total of all these missing elements could be quite sizable, so it shouldn’t be assumed that the results from this calculator accurately reflect the entire carbon footprint of the building. Even a carbon-banking result may actually be a net emitter if all of these materials were included in the total."]
[null,"NRCan will consider updating the calculator with EPDs in these categories as they become available."]
[null,"5. We have only included data for “cradle-to-gate” (A1-A3) emissions, not transportation to site, product use emissions/off-gassing or job site emissions."]
[null,"Getting building materials from the factory to the job site can add a significant quantity of emissions to the overall project. Typically, transportation to the construction site adds 5-10% to the total material emissions."]
[null,"We encourage you to understand your supply chains and to attempt to do your own transportation emission calculations. The emissions from a construction site are likewise difficult to estimate, but average between 5-10% of the total materials emissions, and will depend on emissions factors associated with the energy source on the job site (electricity grid versus diesel generator)"]
[null,"It should be noted that some job site emissions (A5) and/or product use emissions (B1) have been included in MCE calculations for those materials that have a necessary, sizable and very predictable volume of emissions in those life cycle phases. Examples include emissions from site-mixed foam insulation and GHG off-gasing from some rigid insulations. These types of emissions are included in A5 or B1 in many EPDs but are more related to the static emission profile of the product than to construction site or product use specific activity."]
[null,"6. No end of life emissions calculated"]
[null,"There are emission impacts at the end of life for a building component or a whole building, and these are important considerations when making climate-related material choices. Despite the value of considering \"future emissions\" today, this tool excludes end of life estimates for a few reasons:"]
[null,"End of life scenarios for buildings and materials are difficult, if not impossible, to predict. Thus, focusing on the reasonably measurable and predictable cradle-to-gate phases greatly reduces uncertainty and speculation by excluding later life cycle phases. "]
[null,"The data and methodology for counting end-of-life and replacement emissions is not as refined or widely available as today's A1-A3 emissions."]
[null,"The actual service life of a material or whole building is rarely the cause for replacement or demolition; instead factors like property value, aesthetics and planning issues tend to bring about the demise of materials and buildings, not the expected service life. "]
[null,"When considering the 30-year project emissions timeline provided on the results page of MCE2, consider the potential need for replacement of materials that may not last 30 years. Estimates of replacement emissions can be made using today's A1-A3 values and adding them to the emissions timeline at an appropriate year."]
[]
[null,"7. No costing information."]
[null,"No attempt has been made to include material costs in this calculator. Builders should use external costing information to understand the impact of alternative materials in their own projects. "]
[]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Introduction-FR","index":5,"n_rows":71,"n_cols":5,"rows_kept":71,"cut":false,"hidden":true,"merged":[[66,1,66,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[59,1,59,2],[60,1,60,2],[62,1,62,2],[63,1,63,2],[41,1,41,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[29,1,29,2],[33,1,33,2],[37,1,37,2],[38,1,38,2],[40,1,40,2],[10,1,10,2],[0,15,0,16],[0,17,0,18],[1,10,1,14],[1,15,1,16],[1,17,1,18],[3,1,3,2],[4,1,4,2],[5,1,5,2],[7,1,7,2],[8,1,8,2],[9,1,9,2]]}
["French"]
["Novembre \n2023","Outil d’estimation d’émissions de carbone des matériaux (E2CM)"]
[null,"Notes sur l’utilisation de cet outil d’estimation"]
[null,"1 – Les résultats de cet outil sont une estimation des émissions de carbone des matériaux (ECM) de votre projet de construction fini.\nCes résultats peuvent être considérés de la même manière que les résultats d’un modèle énergétique de base pour une maison. De même qu’un modèle énergétique simple permet de prédire relativement bien l’efficacité comparative de différentes stratégies d’efficacité, un tel modèle ne vous dira pas nécessairement combien d’énergie le bâtiment consommera finalement. Cet outil d’estimation doit être utilisé pour évaluer les ECM relatives de différentes approches de construction pour un projet de maison ou de rénovation."]
[null,"2 – Cet outil n’est pas destiné à être utilisé comme un outil de programme ou de conformité. L’outil est destiné à fournir à l’industrie de la construction et de la rénovation de maisons des outils de connaissance pour soutenir les décisions concernant les ECM relatives de différentes approches de construction."]
[null,"3 – Cet outil fournit une gamme de matériaux et de technologies de construction possibles, mais n’inclut pas tous les matériaux sur le marché. Tous les efforts ont été faits pour inclure les informations les plus pertinentes sur les matériaux et systèmes courants au moment de la publication. Les fabricants et les fournisseurs de produits dont les données ne sont pas incluses peuvent fournir à RNCan la documentation pertinente sur les Déclarations Environnementale de Produit (DEP) et les produits, qui sera examinée et incluse dans une mise à jour prévue (date à déterminer)."]
[null,"Vue d’ensemble et contexte"]
[null,"Cet outil d’estimation est conçu pour comparer les émissions de gaz à effet de serre (GES) de différents matériaux de construction pour la construction résidentielle. Les résultats comparatifs peuvent aider les utilisateurs à faire des choix de matériaux pour réduire l’empreinte carbone des maisons et des rénovations qu’ils envisagent."]
[null,"En combinant les données énergétiques opérationnelles annuelles de HOT2000 avec l’estimation par cet outil des ECM initiaux de leur projet, les utilisateurs pourront examiner un graphique de l’empreinte carbone cumulée de leur maison et de leurs projets de rénovation."]
[null,"Cet outil permet aux utilisateurs de comparer les matériaux sur une base composant par composant, ainsi que par ensembles entiers. La majorité des matériaux à fort impact d’un bâtiment sont représentés dans l’outil. RNCan a inclus une vaste gamme d’assemblages et de matériaux de structure et d’enceinte, ainsi que les principaux matériaux de revêtement, de gainage et de finition pour la construction résidentielle.",null,null,"\n"]
[null,"Cet outil d’estimation porte sur les émissions de carbone des matériaux (ECM – souvent appelé « carbone incorporé ») parce que le volume élevé d’émissions provenant directement de la récolte et de la production de matériaux de construction représente une opportunité clé pour réduire considérablement les émissions. Les bâtiments résidentiels de faible hauteur émettent en moyenne 150 à 400 kg de GES par mètre carré de surface de plancher (25 à 75 tonnes pour une maison de 2 000 pieds carrés). Si l’on multiplie ces émissions par celles de tous les immeubles résidentiels de faible hauteur construits chaque année au Canada, on obtient des émissions équivalentes à celles d’environ deux centrales électriques au charbon."]
[null,"Le Canada reconnaît cette source considérable de GES. Cet outil est conçu pour aider les industries de la construction et de la rénovation de maisons à faire des choix de matériaux éclairés afin de réduire les émissions de carbone initiales."]
[null,"En choisissant les matériaux en connaissance de cause, un bâtiment ayant la même taille, la même fonction et la même performance énergétique peut réduire considérablement ses ECM. En fait, il est possible, avec les matériaux disponibles aujourd’hui, de faire en sorte que les ECM des bâtiments soient proches de zéro, voire inférieurs."]
[null,"Cet outil d’estimation a pour but d’ouvrir le dialogue et de permettre à l’industrie de jouer un rôle de premier plan pour faire passer le secteur de la construction résidentielle du statut de moteur du changement climatique à celui de leader en matière de réduction des émissions de carbone."]
[null,"Données pour les calculs"]
[null,"Les données de cet outil d’estimation proviennent des déclarations environnementales de produits (DEP) publiées.\nCes documents fournissent les résultats d’une « analyse du cycle de vie » (ACV) qui a été réalisée et rapportée selon les règles de catégories de produits (RCP) définies et réglementées par les normes ISO. Les DEP sont réalisées ou vérifiées par une tierce partie. Les DEP ne peuvent pas comparer des matériaux destinés à des usages différents (par exemple, du bois de construction à des carreaux de sol). Même au sein d’une même catégorie de produits, il peut être difficile de comparer les chiffres de la DEP, car les valeurs exprimées pour chaque matériau peuvent ne pas être directement comparables (par exemple, les kilogrammes de briques ne peuvent être comparés aux mètres carrés de bardage en bois). Cet outil d’estimation normalise toutes les valeurs exprimées dans les DEP sources afin de s’assurer que les types de matériaux appropriés sont comparés dans les quantités appropriées (c’est-à-dire les mètres carrés de briques et les mètres carrés de bardage en bois)."]
[null,"RNCan s’est efforcé de s’assurer que toutes les comparaisons de matériaux sont équivalentes, en utilisant des tailles de produits standard, des normes de code et des pratiques exemplaires pour faire en sorte qu’on « compare des pommes avec des pommes »."]
[null,"Les options de matériaux avec des surlignages pastel dans la colonne M ont reçu leurs données d’émissions de carbone de sources autres qu’une DEP et sont indiquées par la légende suivante :"]
[]
[null,"Source de données : la DEP comprend les phases A1-A3 et B1 (dégagement de COV)."]
[null,"Source de données : étude ACV"]
[null,"Source de données : base de données ICE (R. U.)"]
[null,"Source des données : autre que DEP, ACV ou base de données."]
[null,"Source des données : DEP récemment expiré"]
[]
[]
[]
[]
[null,"Limites de l’outil"]
[null,"Il est important de noter que cet outil présente un certain nombre de limites dont vous devez savoir. Veuillez lire attentivement cette section afin d’être pleinement informé."]
[]
[null,"Il y a plusieurs facteurs à garder à l’esprit concernant la précision de cet outil d’estimation :"]
[null,"1. Toutes les données sont basées sur des déclarations environnementales de produits (DEP) accessibles au public."]
[null,"Les calculs utilisés pour créer une DEP peuvent être comparés au calcul de la consommation de carburant d’une voiture ou d’un camion. Une série d’hypothèses et de données génériques sont utilisées pour prédire l’empreinte carbone d’un matériau. Les règles d’élaboration des DEP garantissent que ces hypothèses sont similaires pour tous les produits d’une catégorie donnée, mais cela ne garantit pas nécessairement que le chiffre réel soit une représentation parfaite des émissions effectives dues à la fabrication du matériau."]
[null,"Une fourchette d’incertitude de 5 à 25 % est typique des DEP."]
[]
[null,"2. Les calculs peuvent ne pas refléter vos pratiques."]
[null,"Afin de rendre l’outil d’estimation simple à utiliser et de minimiser le nombre d’entrées, de nombreuses hypothèses ont été faites dans les calculs des quantités de matériaux. Dans la mesure de nos possibilités, nous avons choisi des facteurs qui sont des normes industrielles bien établies, mais ces normes peuvent ne pas refléter la conception ou l’exécution réelle de votre bâtiment."]
[null,"Bien qu’il soit peu probable que les quantités de matériaux que nous estimons dans l’outil correspondent parfaitement à votre utilisation réelle de matériaux, les quantités sont cohérentes entre toutes les options que nous présentons.\nCela signifie que la comparaison des émissions entre les matériaux est exacte. Par exemple, vous pouvez utiliser plus ou moins de matériaux d’encadrement que ce que nous avons estimé pour votre projet, mais la différence relative entre les options d’encadrement, telle qu’elle est représentée par l’outil, sera exacte."]
[null,"3. Aucun facteur de gaspillage pour les matériaux n’est inclus."]
[null,"Tout projet de construction génère des retailles et des déchets. Aucun de nos calculs ne suppose de facteurs de gaspillage en raison de la grande variation des pratiques sur site."]
[null,"Si vous souhaitez que vos émissions totales reflètent les facteurs de déchets, vous pouvez ajouter un pourcentage approprié à chaque catégorie de matériau en utilisant la fonction de pourcentage de la colonne F."]
[null,"4. Nous n’avons pas inclus de données pour tous les composants d’un bâtiment."]
[null,"Il y a beaucoup de matériaux qui entrent dans la construction de votre bâtiment et qui ne sont pas inclus ici :"]
[null,"Systèmes et composants mécaniques, électriques et de plomberie"]
[null,"Imperméabilisation, pare-air/pare-vapeur et membranes"]
[null,"Solins, mastics, adhésifs"]
[null,"Attaches"]
[null,"Appareils et accessoires"]
[null,"Menuiserie, ébénisterie et escaliers"]
[null,"Peintures, teintures et finitions de surface"]
[null,"Les données disponibles sont actuellement limitées dans certaines de ces catégories ou les quantités de matériaux et d’émissions seraient assez similaires (par exemple, les toilettes et les machines à laver n’ont pas beaucoup de variation dans les émissions pour la comparaison selon les données disponibles)."]
[null,"Le total de tous ces éléments manquants peut être assez important, il ne faut donc pas croire que les résultats de cet outil d’estimation reflètent avec précision l’empreinte carbone totale du bâtiment.\nMême le résultat d’une banque de carbone peut en fait être un émetteur net si toutes ces matières étaient incluses dans le total."]
[null,"RNCan envisagera de mettre à jour l’outil d’estimation avec les DEP dans ces catégories dès qu’ils seront disponibles."]
[null,"5. Nous n’avons inclus que les données relatives aux émissions « du berceau à la porte » (A1-A3), et non le transport jusqu’au site, les émissions/le dégazage de l’utilisation du produit ou les émissions sur le chantier."]
[null,"Le transport des matériaux de construction de l’usine au chantier peut ajouter une quantité importante d’émissions au projet global. En général, le transport vers le site de construction ajoute 5 à 10 % aux émissions totales des matériaux."]
[null,"Nous vous encourageons à comprendre vos chaînes d’approvisionnement et à essayer de faire vos propres calculs d’émissions de transport. Les émissions d’un chantier de construction sont également difficiles à estimer, mais représentent en moyenne entre 5 et 10 % des émissions totales des matériaux, et dépendent des facteurs d’émissions associés à la source d’énergie du chantier (réseau électrique ou générateur diesel)."]
[null,"Il convient de noter que certaines émissions du chantier (A5) ou des émissions liées à l’utilisation du produit (B1) ont été incluses dans les calculs de l’ECM pour les matériaux dont le volume d’émissions est nécessaire, important et très prévisible au cours de ces phases du cycle de vie. Il s’agit par exemple des émissions provenant de la mousse isolante mélangée sur place et des gaz à effet de serre émis par certains isolants rigides. Ces types d’émissions sont inclus en A5 ou B1 dans de nombreuses DEP mais sont davantage liés au profil d’émission statique du produit qu’à une activité spécifique au site de construction ou à l’utilisation du produit."]
[null,"6. Aucune émission en fin de vie n’est calculée"]
[null,"Il y a des impacts d'émissions en fin de vie pour une composante de bâtiment ou pour l'ensemble d'un bâtiment, et ceux-ci sont des considérations importantes lors du choix des matériaux liés au climat. Malgré la valeur de la prise en compte des \"émissions futures\" aujourd'hui, cet outil exclut les estimations en fin de vie pour quelques raisons :"]
[null,"Les scénarios de fin de vie pour les bâtiments et les matériaux sont difficiles, voire impossibles, à prévoir. Ainsi, se concentrer sur les phases du berceau à la porte de l’usine raisonnablement mesurables et prévisibles réduit considérablement l'incertitude et la spéculation en excluant les phases ultérieures du cycle de vie."]
[null,"Les données et la méthodologie pour comptabiliser les émissions en fin de vie et de remplacement ne sont pas aussi affinées ou largement disponibles que les émissions A1-A3 d'aujourd'hui."]
[null,"La durée de vie effective d'un matériau ou d'un bâtiment entier est rarement la cause du remplacement ou de la démolition ; ce sont plutôt des facteurs tels que la valeur immobilière, l'esthétique et les problèmes de planification qui ont tendance à causer la disparition des matériaux et des bâtiments, et non la durée de vie prévue."]
[null,"Lorsque vous examinez le calendrier d’émission du projet sur 30 ans fourni sur la page de résultats de E2CM, tenez compte du besoin potentiel de remplacement des matériaux qui pourraient ne pas durer 30 ans. Des estimations des émissions de remplacement peuvent être réalisées en utilisant les valeurs A1-A3 d'aujourd'hui et en les ajoutant à la chronologie des émissions à l'année appropriée."]
[]
[null,"7. Aucune information sur les coûts."]
[null,"Aucune tentative n’a été faite pour inclure les coûts des matériaux dans cet outil d’estimation. Il incombe aux constructeurs de trouver des sources d’information sur les coûts pour comprendre l’impact des matériaux équivalents dans leurs propres projets."]
[]
[]
[null,"© His Majesty the king in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"USER INPUT SHEET","index":6,"n_rows":71,"n_cols":32,"rows_kept":71,"cut":false,"hidden":false,"merged":[[0,16,0,31],[2,16,2,20],[2,22,2,25],[2,27,2,30],[3,17,3,18],[3,19,3,20],[3,23,3,24],[3,28,3,29],[66,1,66,12],[15,7,15,10],[15,12,16,12],[15,13,16,13],[16,7,16,10],[17,7,17,10],[17,12,17,13],[18,12,19,12],[18,13,19,13],[29,5,29,10],[29,12,29,14],[30,5,30,10],[20,12,21,12],[20,13,21,13],[26,1,27,1],[26,2,27,2],[46,1,47,1],[46,2,47,2],[46,4,47,4],[46,12,47,14],[40,1,40,14],[42,1,42,11],[45,5,45,10],[45,12,45,14],[43,5,43,10],[43,12,43,14],[54,5,54,10],[54,12,54,14],[51,5,51,10],[51,12,51,14],[52,5,52,10],[52,12,52,14],[53,5,53,10],[53,12,53,14],[36,12,36,14],[53,15,53,19],[48,5,48,10],[48,12,48,14],[49,5,49,10],[49,12,49,14],[50,5,50,10],[50,12,50,14],[37,5,37,10],[37,12,37,14],[36,5,36,10],[1,0,5,0],[1,1,5,9],[1,10,5,14],[38,5,38,10],[38,12,38,14],[28,5,28,10],[28,12,28,14],[34,12,34,14],[30,12,30,14],[31,5,31,10],[31,12,31,14],[32,5,32,10],[32,12,32,14],[33,5,33,10],[33,12,33,14],[34,5,34,10],[4,28,4,29],[35,5,35,10],[35,12,35,14],[23,4,23,11],[23,12,23,14],[13,12,13,13],[14,7,14,10],[6,12,6,13],[6,17,6,24],[7,17,8,24],[26,4,27,4],[26,12,27,14],[24,5,24,10],[24,12,24,14],[4,17,4,18],[13,17,16,24],[10,17,12,24],[18,7,18,10],[35,16,35,22],[4,19,4,20],[4,23,4,24]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UNIT CONVERSIONS"]
["November\n2023","Material Carbon Emissions Estimator (MCE2)",null,null,null,null,null,null,null,null,"Project Carbon Content"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Volume",null,null,null,null,null,"Area",null,null,null,null,"Length"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,"m3 à",null,{"$f":"Q4/0.0283168","v":176.57362413832072},null,"pi/ft3",628,"m2 à",null,{"$f":"W4*10.7639","v":6759.7291999999998},"pi/ft2",1,"m à",null,{"$f":"AB4*3.28084","v":3.28084},"ft"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,45,"ft3 à",null,{"$f":"Q5/35.3147","v":1.2742568958535681},null,"m3",26,"ft2à",null,{"$f":"W5*0.092903","v":2.4154779999999998},"m2",100,"ft à",null,{"$f":"AB5*0.3048","v":30.48},"m"]
[]
["Step","      Import project data from HOT2000 (If no HOT2000 file, skip to Step 2)",null,null,null,null,null,null,null,null,null,null,"Energy Consumption",null,"Energy Generation",null,null,"Notes on Energy Consumption"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Elec. kWh/yr","N. Gas m3/yr","Elec. kWh/yr",null,null,"Electricity generated on-site has already been subtracted from the total energy consumption in cell M9."]
[null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Note: kg/m2 comes from total kg divided by habitable floor area"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Propane L/yr","Oil L/yr","Wood kg/yr",null,null,"Energy consumption reflects values from HOT2000, users should manually update values if using a different modeling software. "]
[null,null,null,null,null,null,null,null,null,null,null,null,0,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,"To override energy GHG intensities, use the Energy GHG tab."]
["Step","      Confirm or enter project information",null,null,null,null,null,null,null,null,null,null,"Operational Emissions",null,null,null,null,"When considering different scenarios, users should ensure that thermal resistances of assemblies are consistent, as these will determine the energy consumption of the home. Where these change, users should also revise the energy model and update the energy consumption values."]
[null,"Address:",null,null,"Province:",null,null,null,null,null,null,null,"tonnes CO2e / yr","t CO2e / 30 yrs"]
[null,"City:",null,null,"Postal code:",null,null,null,null,null,null,null,{"$f":"IFERROR(INDEX('Energy GHG'!I21:I33,MATCH('USER INPUT SHEET'!H15,'Energy GHG'!C21:C33,0),),)","v":0},{"$f":"M16*30","v":0}]
[null,"Building Type:",null,null,"Evaluation date:"]
[null,"Storeys:",null,null,"File ID:",null,null,null,null,null,null,null,"Material Emissions"]
[null,"Year Built:",null,null,"File name:",null,null,null,null,null,null,null,"tonnes CO2e","kg CO2e / m2"]
[null,"Heated Floor Area (above grade, m2):"]
[null,"Heated Floor Area (below grade, m2):",null,null,null,null,null,null,null,null,null,null,{"$f":"IFERROR(Summary[[#Totals],[Embodied Carbon \n'[kg CO2e']]]/10^3,)","v":0},{"$f":"IFERROR(ROUND(Summary[[#Totals],[Embodied Carbon \n'[kg CO2e']]]/(C20+C21),1),)","v":0}]
[null,"Heating Degree Days:",null,null,null,null,null,null,null,null,null,null,{"$f":"Summary[[#Totals],[Embodied Carbon \n'[kg CO2e']]]","v":0}]
[]
["Step","      Confirm or enter project dimensions",null,null,"HOT2000 values are imported to the BLUE cells below. \nIf no HOT2000 file imported, then enter values into the BLUE cells. ",null,null,null,null,null,null,null,"For all YELLOW cells below, manually enter all relevant values. Exclude any garage quantities.",null,null,"YOUR DATA"]
[null,"COMPONENT","AREA/\nVOLUME",null,"UNIT","APPLICATION OF INPUT VALUE",null,null,null,null,null,null,"DESCRIPTION OF REQUIRED UNITS"]
[]
[null,"FOOTINGS, PADS & PIERS",{"$f":"F28*H28*J28","v":0},null,"m3","Footing Length",null,"Footing Depth",null,"Footing Width",null,null,"Total cubic metres of all footings, piers and posts"]
[null,null,null,null,null,null,"X",null,"X"]
[null,"FOUNDATION WALL AREA",null,null,"m2","Foundation wall, exterior continuous insulation, interior framing, interior insulation, interior wall finish",null,null,null,null,null,null,"Total wall area (exclude windows and doors)"]
[null,"FOUNDATION SLAB/FLOOR AREA",null,null,"m2","Slab, aggregate base, sub-slab insulation, basement flooring",null,null,null,null,null,null,"Square metres"]
[null,"EXTERIOR WALL AREA",null,null,"m2","Framing, insulation, sheathing, exterior cladding, interior cladding of exterior walls only",null,null,null,null,null,null,"Total exterior wall area (include gable ends; exclude window & door openings). Exclude all garage wall, garage partition wall and party wall areas"]
[null,"WINDOW AREA",null,null,"m2","Windows",null,null,null,null,null,null,"Square metres (include full area of glazing units)"]
[null,"INTERIOR WALL AREA",null,null,"m2","Framing, insulation and interior cladding of interior walls",null,null,null,null,null,null,"Square metres (one side only) of all interior walls. Quantity will be doubled for cladding materials"]
[null,"FRAMED FLOOR AREA",null,null,"m2","Floor framing, subfloor, floor insulation, flooring",null,null,null,null,null,null,"Square metres (includes all levels, excludes basement slab, stairs and other openings)"]
[null,"CEILING AREA",{"$f":"C20+C21","v":0},null,"m2","Ceiling cladding/coverings",null,null,null,null,null,null,"Square metres (all levels; include basement ceiling if applicable)"]
[null,"ROOFING AREA",null,null,"m2","Roof framing,  decking, roofing, and insulation parallel to roof deck",null,null,null,null,null,null,"Square metres (Include sloped and flat roofs; exclude overhangs and gable ends)",null,null,null,"HEAVY TIMBER BEAM VOLUME CALCULATOR"]
[null,"ROOF INSULATION AREA",null,null,"m2","Roof insulation parallel to ceiling",null,null,null,null,null,null,"Square metres of insulation in the roof cavity. Typically this is equal to the attic floor or top floor ceiling area.",null,null,null,"Beam Length (M)",null,"Beam Depth (mm)",null,"Beam Width (mm)",null,"Beam Volume (m3)"]
[null,"HEAVY TIMBER ELEMENTS",null,null,"m3","Heavy timber framing members (e.g. posts and beams)",null,null,null,null,null,null,"Cubic metres of total wood volume in posts & beams. (Heavy steel members input in Structural Elements tab)",null,null,null,12,"X",305,"X",75,"=",{"$f":"Q38*(S38/1000)*(U38/1000)","v":0.27450000000000002}]
[null,"PARTY WALL AREA",null,null,"m2","Party wall framing, insulation, sheathing, interior cladding.",null,null,null,null,null,null,"Square meters of wall area that partitions one dwelling from another. Used for row housing units, apartment units, etc."]
[]
[null,"If this building includes a GARAGE, click the PLUS symbol on the left to expand the Garage section. "]
[null,"GARAGE"]
[null,"Enter garage measurements in the YELLOW cells below. "]
[null,"COMPONENT","QUANTITY",null,"UNIT","APPLICATION OF INPUT VALUE",null,null,null,null,null,null,"DESCRIPTION OF REQUIRED UNITS"]
[]
[null,"ATTACHED GARAGE WALL AREA",null,null,"m2","Exterior wall framing, interior wall cladding, partition wall insulation (hover cursor for details)",null,null,null,null,null,null,"Area of wall that attaches the garage to the building (excludes openings and exterior garage walls).\nIf the garage is detached, leave this cell blank."]
[null,"GARAGE FOOTINGS & PADS",{"$f":"F48*H48*J48","v":0},null,"m3","Footing Length",null,"Footing Depth",null,"Footing Width",null,null,"Cubic metres. Only include volume additional to main building footings, pads and piers"]
[null,null,null,null,null,null,"X",null,"X"]
[null,"GARAGE FOUNDATION WALL AREA",null,null,"m2","Garage foundation wall, interior framing, interior wall finish",null,null,null,null,null,null,"Square metres (exclude windows and doors). Only include foundation area additional to main building foundation"]
[null,"GARAGE SLAB/FLOOR AREA",null,null,"m2","Slab, aggregate base",null,null,null,null,null,null,"Square metres"]
[null,"GARAGE EXTERIOR WALL AREA",null,null,"m2","Framing, sheathing, exterior cladding, interior cladding",null,null,null,null,null,null,"Exterior garage wall area (include gable area, exclude window & door openings) Exclude attached wall area"]
[null,"GARAGE WINDOW AREA",null,null,"m2","Windows",null,null,null,null,null,null,"Square metres (full area of glazing units)"]
[null,"GARAGE FINISHED CEILING AREA",null,null,"m2","Ceiling cladding/coverings",null,null,null,null,null,null,"Square metres (all levels)"]
[null,"GARAGE ROOFING AREA",null,null,"m2","Roof framing, decking, roofing. HOT2000 users: see Note (hover cursor)",null,null,null,null,null,null,"Square metres (Includes sloped and flat roofs; excludes overhangs)"]
[null,"GARAGE HEAVY TIMBERS",null,null,"m3","Heavy timber framing members (e.g. posts and beams)",null,null,null,null,null,null,"Cubic metres of total wood volume in posts & beams. (Heavy steel members input in Structural Elements tab)"]
[]
[]
["Step","      Define all building assemblies in the following building section tabs."]
[]
[]
["Step","      Review the selected materials in the REVIEW tab. "]
[]
[]
["Step","      View the carbon emissions report in the RESULTS tabs."]
[]
[]
[null,"Helpful Notes:\n- See the Glossary tab for descriptions of unfamiliar terms or acronyms.\n- Use the User-Defined tab for any materials you wish to add but that could not be included in the section tabs.\n- To jump to a tab, right-click the arrows in the lower left corner and select the tab.\n- All framing spacing is 24 inches on centre by default, even when Framing Spacing value is blank"]
[]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Conctete Selections","index":7,"n_rows":2,"n_cols":14,"rows_kept":2,"cut":false,"hidden":true,"merged":[]}
["About This Sheet",null,"Previously selected Province:"]
["Material",{"$f":"'Energy GHG'!$C2","v":"Newfoundland and Labrador"},{"$f":"'Energy GHG'!$C3","v":"Prince Edward Island"},{"$f":"'Energy GHG'!$C4","v":"Nova Scotia"},{"$f":"'Energy GHG'!$C5","v":"New Brunswick"},{"$f":"'Energy GHG'!$C6","v":"Quebec"},{"$f":"'Energy GHG'!$C7","v":"Ontario"},{"$f":"'Energy GHG'!$C8","v":"Manitoba"},{"$f":"'Energy GHG'!$C9","v":"Saskatchewan"},{"$f":"'Energy GHG'!$C10","v":"Alberta"},{"$f":"'Energy GHG'!$C11","v":"British Columbia"},{"$f":"'Energy GHG'!$C12","v":"Yukon"},{"$f":"'Energy GHG'!$C13","v":"Northwest Territories"},{"$f":"'Energy GHG'!$C14","v":"Nunavut"}]

{"sheet":"Footings & Slabs","index":8,"n_rows":146,"n_cols":16,"rows_kept":146,"cut":false,"hidden":false,"merged":[[98,1,98,2],[85,1,85,2],[92,0,92,1],[95,0,97,1],[50,1,50,2],[81,1,81,2],[82,0,84,1],[87,0,90,1],[91,1,91,2],[93,1,93,2],[49,0,49,2],[51,0,51,1],[52,0,52,2],[80,0,80,2],[78,1,78,2],[53,1,53,2],[54,0,60,1],[77,0,77,2],[70,0,76,1],[61,1,61,2],[62,0,68,1],[69,1,69,2],[4,0,4,2],[11,0,11,2],[6,0,10,1],[46,0,46,2],[47,1,47,2],[20,1,20,2],[21,0,27,1],[28,1,28,2],[29,0,35,1],[12,1,12,2],[13,0,19,1],[36,0,36,2],[5,1,5,2],[37,1,37,2],[38,0,45,1],[0,0,0,2],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,5,3,5],[2,6,3,6],[2,2,3,2],[2,0,3,1],[0,3,0,11],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[142,0,142,1],[126,0,131,1],[133,0,133,1],[135,0,136,1],[141,1,141,2],[137,1,137,2],[132,1,132,2],[134,1,134,2],[107,0,109,1],[138,0,140,1],[119,0,123,1],[100,0,101,1],[103,0,103,1],[104,0,104,2],[105,1,105,2],[110,1,110,2],[102,1,102,2],[117,1,117,2],[111,0,116,1],[124,1,124,2]]}
["SECTION 1 ➜ COMPONENT MATERIALS FOR",null,null,"FOUNDATION - FOOTINGS & SLABS"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR FOUNDATION FOOTINGS & SLAB"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0},null,"Category","Subcategory"]
["CRUSHED STONE BASE",null,null,"THICKNESS:",null,"in","=",{"$f":"IF(F5=\"mm\",E5/1000,E5*0.0254)","v":0},"m"]
[null,"AGGREGATE"]
["If you do not know the specific carbon footprint of your aggregate, chose the \"AVERAGE\" value",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(4,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate /  /  / Avg construction aggregate (gravel & sand)"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K7-L7","v":0},{"$f":"IF(H7=1,I7,\"\")","v":""},{"$f":"$D7*$H$5*$F7*VLOOKUP($C7,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D7*$H$5*$F7*VLOOKUP($C7,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","CRUSHED STONE BASE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(5,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Kangley Rock & Recycling /  / Avg construction aggregate (gravel & sand)"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K8-L8","v":0},{"$f":"IF(H8=1,I8,\"\")","v":""},{"$f":"$D8*$H$5*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D8*$H$5*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","CRUSHED STONE BASE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(6,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Martin Marietta /  / Avg construction aggregate (gravel & sand)"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K9-L9","v":0},{"$f":"IF(H9=1,I9,\"\")","v":""},{"$f":"$D9*$H$5*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D9*$H$5*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","CRUSHED STONE BASE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(7,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Polaris Mtls Corp. /  / Avg construction aggregate (gravel & sand)"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K10-L10","v":0},{"$f":"IF(H10=1,I10,\"\")","v":""},{"$f":"$D10*$H$5*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D10*$H$5*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","CRUSHED STONE BASE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(8,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Vulcan Mtls Co. /  / Avg construction aggregate (gravel & sand)"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K11-L11","v":0},{"$f":"IF(H11=1,I11,\"\")","v":""},{"$f":"$D11*$H$5*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D11*$H$5*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - FOOTINGS & SLABS","CRUSHED STONE BASE"]
["FOOTINGS, PIERS & PADS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CONCRETE – 25 MPa or less",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,{"$f":"K14-L14","v":0},{"$f":"IF(H14=1,I14,\"\")","v":""},{"$f":"$D14*$F14*VLOOKUP($C14,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D14*$F14*VLOOKUP($C14,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D15*$F15*VLOOKUP($C15,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D15*$F15*VLOOKUP($C15,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D16*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D16*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D17*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D17*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D18*$F18*VLOOKUP($C18,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D18*$F18*VLOOKUP($C18,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,{"$f":"K19-L19","v":0},{"$f":"IF(H19=1,I19,\"\")","v":""},{"$f":"$D19*$F19*VLOOKUP($C19,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D19*$F19*VLOOKUP($C19,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,{"$f":"K22-L22","v":0},{"$f":"IF(H22=1,I22,\"\")","v":""},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D23*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D23*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D26*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D26*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,{"$f":"K27-L27","v":0},{"$f":"IF(H27=1,I27,\"\")","v":""},{"$f":"$D27*$F27*VLOOKUP($C27,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D27*$F27*VLOOKUP($C27,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D28*$F28*VLOOKUP($C28,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D28*$F28*VLOOKUP($C28,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,"CONCRETE – 31-35 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,{"$f":"K30-L30","v":0},{"$f":"IF(H30=1,I30,\"\")","v":""},{"$f":"$D30*$F30*VLOOKUP($C30,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D30*$F30*VLOOKUP($C30,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,0,"",{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,{"$f":"K35-L35","v":0},{"$f":"IF(H35=1,I35,\"\")","v":""},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$27","v":0},{"$f":"'USER INPUT SHEET'!$E$27","v":"m3"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","FOOTINGS & PADS"]
["REBAR",null,null,"CUSTOM LENGTH",null,"m",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CONCRETE REINFORCING BAR",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Specify an overall rebar length.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(176,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Concrete Reinforcing Steel Institute /  / 10M"},{"$f":"IF(E$37>0,E$37,'USER INPUT SHEET'!$F$28)","v":0},{"$f":"$F$37","v":"m"},1,null,null,{"$f":"K39-L39","v":0},{"$f":"IF(H39=1,I39,\"\")","v":""},{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS",{"$f":"$A$37","v":"REBAR"}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(177,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Concrete Reinforcing Steel Institute /  / 15M"},{"$f":"IF(E$37>0,E$37,'USER INPUT SHEET'!$F$28)","v":0},"m",1,null,null,0,"",{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(390,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Nucor Corporation / Canadian sizes / 10M"},{"$f":"IF(E$37>0,E$37,'USER INPUT SHEET'!$F$28)","v":0},"m",1,null,null,0,"",{"$f":"$D41*$F41*VLOOKUP($C41,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D41*$F41*VLOOKUP($C41,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(391,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Nucor Corporation / Canadian sizes / 15M"},{"$f":"IF(E$37>0,E$37,'USER INPUT SHEET'!$F$28)","v":0},"m",1,null,null,0,"",{"$f":"$D42*$F42*VLOOKUP($C42,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D42*$F42*VLOOKUP($C42,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(392,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Nucor Corporation / Canadian sizes / 20M"},{"$f":"IF(E$37>0,E$37,'USER INPUT SHEET'!$F$28)","v":0},"m",1,null,null,0,"",{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(393,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 10M"},{"$f":"IF(E$37>0,E$37,'USER INPUT SHEET'!$F$28)","v":0},"m",1,null,null,0,"",{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(394,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 15M"},{"$f":"IF(E$37>0,E$37,'USER INPUT SHEET'!$F$28)","v":0},"m",1,null,null,0,"",{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(395,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 20M"},{"$f":"IF(E$37>0,E$37,'USER INPUT SHEET'!$F$28)","v":0},"m",1,null,null,0,"",{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","REBAR"]
["STEEL REINFORCING MESH",null,null,"CUSTOM AREA:",null,"m2",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"WELDED WIRE MESH",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(221,'Master sheet'!$AL$1:$AL$441,0))","v":"Welded wire mesh / Serfas /  / 6\" x 6\" x 6/6g / Norway"},{"$f":"IF(E47>0,E47,'USER INPUT SHEET'!$C$30)","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K49-L49","v":0},{"$f":"IF(H49=1,I49,\"\")","v":""},{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - FOOTINGS & SLABS",{"$f":"A47","v":"STEEL REINFORCING MESH"}]
["HELICAL PIERS",null,null,"TOTAL LENGTH OF ALL PIERS:",null,"m",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"HELICAL PIERS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Specify the total length of all piers. Use % to adjust for different sized piers",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(120,'Master sheet'!$AL$1:$AL$441,0))","v":"Helical pier / Generic /  / 3\" Nominal Pipe, 3.5 x 3/16\" (89 x 5.5 mm), 10\" Helix, Sched 40 STD Galvanized steel"},{"$f":"E$50","v":0},{"$f":"F$50","v":"m"},1,null,null,{"$f":"K52-L52","v":0},{"$f":"IF(H52=1,I52,\"\")","v":""},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - FOOTINGS & SLABS",{"$f":"A50","v":"HELICAL PIERS"}]
["CONCRETE SLAB FLOOR(S)",null,null,"THICKNESS:",null,"in","=",{"$f":"IF(F53=\"mm\",E53/1000,E53*0.0254)","v":0},"m",null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CONCRETE – 25 MPa or less",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K55-L55","v":0},{"$f":"IF(H55=1,I55,\"\")","v":""},{"$f":"$D55*$F55*$H$53*VLOOKUP($C55,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D55*$F55*$H$53*VLOOKUP($C55,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D56*$F56*$H$53*VLOOKUP($C56,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D56*$F56*$H$53*VLOOKUP($C56,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D57*$F57*$H$53*VLOOKUP($C57,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D57*$F57*$H$53*VLOOKUP($C57,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D58*$F58*$H$53*VLOOKUP($C58,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D58*$F58*$H$53*VLOOKUP($C58,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D59*$F59*$H$53*VLOOKUP($C59,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D59*$F59*$H$53*VLOOKUP($C59,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K60-L60","v":0},{"$f":"IF(H60=1,I60,\"\")","v":""},{"$f":"$D60*$F60*$H$53*VLOOKUP($C60,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D60*$F60*$H$53*VLOOKUP($C60,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D61*$F61*$H$53*VLOOKUP($C61,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D61*$F61*$H$53*VLOOKUP($C61,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K63-L63","v":0},{"$f":"IF(H63=1,I63,\"\")","v":""},{"$f":"$D63*$F63*$H$53*VLOOKUP($C63,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D63*$F63*$H$53*VLOOKUP($C63,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D64*$F64*$H$53*VLOOKUP($C64,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D64*$F64*$H$53*VLOOKUP($C64,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D65*$F65*$H$53*VLOOKUP($C65,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D65*$F65*$H$53*VLOOKUP($C65,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D66*$F66*$H$53*VLOOKUP($C66,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D66*$F66*$H$53*VLOOKUP($C66,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D67*$F67*$H$53*VLOOKUP($C67,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D67*$F67*$H$53*VLOOKUP($C67,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K68-L68","v":0},{"$f":"IF(H68=1,I68,\"\")","v":""},{"$f":"$D68*$F68*$H$53*VLOOKUP($C68,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D68*$F68*$H$53*VLOOKUP($C68,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D69*$F69*$H$53*VLOOKUP($C69,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D69*$F69*$H$53*VLOOKUP($C69,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,"CONCRETE – 31-35 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K71-L71","v":0},{"$f":"IF(H71=1,I71,\"\")","v":""},{"$f":"$D71*$F71*$H$53*VLOOKUP($C71,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D71*$F71*$H$53*VLOOKUP($C71,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D72*$F72*$H$53*VLOOKUP($C72,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D72*$F72*$H$53*VLOOKUP($C72,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D73*$F73*$H$53*VLOOKUP($C73,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D73*$F73*$H$53*VLOOKUP($C73,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D74*$F74*$H$53*VLOOKUP($C74,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D74*$F74*$H$53*VLOOKUP($C74,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D75*$F75*$H$53*VLOOKUP($C75,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D75*$F75*$H$53*VLOOKUP($C75,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K76-L76","v":0},{"$f":"IF(H76=1,I76,\"\")","v":""},{"$f":"$D76*$F76*$H$53*VLOOKUP($C76,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D76*$F76*$H$53*VLOOKUP($C76,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D77*$F77*$H$53*VLOOKUP($C77,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D77*$F77*$H$53*VLOOKUP($C77,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
["OTHER SLAB FLOOR(S)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"EARTHEN FLOOR",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(52,'Master sheet'!$AL$1:$AL$441,0))","v":"Earthen Floor / Site made /  / 3\" cob, 1\" clay plaster"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K80-L80","v":0},{"$f":"IF(H80=1,I80,\"\")","v":""},{"$f":"$D80*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D80*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Adapted from peer-reviewed LCA, 2019"},null,"FOUNDATION - FOOTINGS & SLABS","SLAB FLOOR(S)"]
["SUB-SLAB INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"EPS FOAM BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"EPS foam board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K83-L83","v":0},{"$f":"IF(H83=1,I83,\"\")","v":""},{"$f":"$F83*AVERAGE(K84:K85)","v":0},{"$f":"$F83*AVERAGE(L84:L85)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(93,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board / EPS Industry Alliance /  / R 4.6/inch, Type IX, 25 psi (Type 3, 140 kPa)"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K84-L84","v":0},"",{"$f":"$D84*($E$82/5.678)*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D84*($E$82/5.678)*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(95,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board with graphite / BASF / Neopor / R 4.7/inch, Type IX"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K85-L85","v":0},"",{"$f":"$D85*($E$82/5.678)*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D85*($E$82/5.678)*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,"XPS FOAM BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"XPS foam board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K87-L87","v":0},"",{"$f":"$F87*AVERAGE(K88:K90)","v":0},{"$f":"$F87*AVERAGE(L88:L90)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(258,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Owens Corning / Foamular NGX 250  / R 5/inch"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,{"$f":"IF(H88=1,I88,\"\")","v":""},{"$f":"$D88*($E$86/5.678)*$F88*VLOOKUP($C88,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D88*($E$86/5.678)*$F88*VLOOKUP($C88,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(401,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Soprema / SOPRA-XPS / R 5.0/inch"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D89*($E$86/5.678)*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D89*($E$86/5.678)*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(400,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / DuPont / Reduced GWP Grey Styrofoam™ (same as ST-100) / R 5.0/inch"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D90*($E$86/5.678)*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D90*($E$86/5.678)*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(399,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) XPS foam board / DuPont / Styrofoam (Grey, Reduced GWP) / R 5.6/inch"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},"This is archived and can be deleted (BSUP)","FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,"MINERAL WOOL BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(149,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board - heavy density / NAIMA / R 4.2/inch"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K93-L93","v":0},{"$f":"IF(H93=1,I93,\"\")","v":""},{"$f":"$D93*($E$92/5.678)*$F93*VLOOKUP($C93,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D93*($E$92/5.678)*$F93*VLOOKUP($C93,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,"FOAMGLASS AGGREGATE",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Foam glass aggregate - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K95-L95","v":0},{"$f":"IF(H95=1,I95,\"\")","v":""},{"$f":"$F95*AVERAGE(K96:K98)","v":0},{"$f":"$F95*AVERAGE(L96:L98)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(108,'Master sheet'!$AL$1:$AL$441,0))","v":"Foam glass aggregate / Glasopor AS /  / R 1.7/inch, 10-60 mm"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K96-L96","v":0},{"$f":"IF(H96=1,I96,\"\")","v":""},{"$f":"$D96*($E$94/5.678)*$F96*VLOOKUP($C96,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D96*($E$94/5.678)*$F96*VLOOKUP($C96,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(109,'Master sheet'!$AL$1:$AL$441,0))","v":"Foam glass aggregate / Hasopor /  / R 1.7/inch, 10-60 mm"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K97-L97","v":0},{"$f":"IF(H97=1,I97,\"\")","v":""},{"$f":"$D97*($E$94/5.678)*$F97*VLOOKUP($C97,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D97*($E$94/5.678)*$F97*VLOOKUP($C97,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(110,'Master sheet'!$AL$1:$AL$441,0))","v":"Foam glass aggregate / Misapor / Glavel / R 1.7/inch, 10-60 mm"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K98-L98","v":0},{"$f":"IF(H98=1,I98,\"\")","v":""},{"$f":"$D98*($E$94/5.678)*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D98*($E$94/5.678)*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,"FOAMGLASS BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Foam glass board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K100-L100","v":0},{"$f":"IF(H100=1,I100,\"\")","v":""},{"$f":"$F100*AVERAGE(K101:K102)","v":0},{"$f":"$F100*AVERAGE(L101:L102)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(111,'Master sheet'!$AL$1:$AL$441,0))","v":"Foam glass board / Pittsburgh Corning Europe / Foamglas T4 / R3.7/inch"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K101-L101","v":0},{"$f":"IF(H101=1,I101,\"\")","v":""},{"$f":"$D101*($E$99/5.678)*$F101*VLOOKUP($C101,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D101*($E$99/5.678)*$F101*VLOOKUP($C101,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(112,'Master sheet'!$AL$1:$AL$441,0))","v":"Foam glass board / Pittsburgh Corning Europe / Foamglas W+F, Foamglas T3 / R4/inch"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K102-L102","v":0},{"$f":"IF(H102=1,I102,\"\")","v":""},{"$f":"$D102*($E$99/5.678)*$F102*VLOOKUP($C102,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D102*($E$99/5.678)*$F102*VLOOKUP($C102,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
[null,"CORK BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(80,'Master sheet'!$AL$1:$AL$441,0))","v":"Cork board insulation / Amorim / Isolamentos / R4/inch"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K104-L104","v":0},{"$f":"IF(H104=1,I104,\"\")","v":""},{"$f":"$D104*($E$103/5.678)*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D104*($E$103/5.678)*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - FOOTINGS & SLABS","SUB-SLAB INSULATION"]
["BASEMENT FLOORING",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"HARDWOOD FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Hardwood flooring - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K107-L107","v":0},{"$f":"IF(H107=1,I107,\"\")","v":""},{"$f":"$F107*AVERAGE(K108:K110)","v":0},{"$f":"$F107*AVERAGE(L108:L110)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(119,'Master sheet'!$AL$1:$AL$441,0))","v":"Hardwood flooring / Typical Eastern Canadian, solid, pre-finished /  / 3-12\" x 3/4\" prefinished"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K108-L108","v":0},{"$f":"IF(H108=1,I108,\"\")","v":""},{"$f":"$D108*$F108*VLOOKUP($C108,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D108*$F108*VLOOKUP($C108,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(118,'Master sheet'!$AL$1:$AL$441,0))","v":"Hardwood flooring / mafi / Natural Hardwood Planks / 3/4\", 3 ply laminated solid, oil pre-finished"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K109-L109","v":0},{"$f":"IF(H109=1,I109,\"\")","v":""},{"$f":"$D109*$F109*VLOOKUP($C109,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D109*$F109*VLOOKUP($C109,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(117,'Master sheet'!$AL$1:$AL$441,0))","v":"Hardwood flooring / Action Floor Systems /  / 25/32\" x 3-1/4\" FSC certified"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K110-L110","v":0},{"$f":"IF(H110=1,I110,\"\")","v":""},{"$f":"$D110*$F110*VLOOKUP($C110,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D110*$F110*VLOOKUP($C110,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,"LINOLEUM FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(134,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Gerflor  / DLW Linoleum Acousticplus / 4.0 mm sheet style linoleum"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K112-L112","v":0},{"$f":"IF(H112=1,I112,\"\")","v":""},{"$f":"$D112*$F112*VLOOKUP($C112,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D112*$F112*VLOOKUP($C112,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,"Linoleum flooring - AVERAGE 2.5 mm",{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$F113*AVERAGE(K114:K116)","v":0},{"$f":"$F113*AVERAGE(L114:L116)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(132,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Forbo / Marmoleum / 2.5 mm sheet style linoleum"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D114*$F114*VLOOKUP($C114,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D114*$F114*VLOOKUP($C114,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(133,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Forbo / Marmoleum Striato / 2.5 mm sheet style linoleum"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D115*$F115*VLOOKUP($C115,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D115*$F115*VLOOKUP($C115,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(373,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Gerflor  / DLW Linoleum Compact / 2.5 mm sheet style linoleum"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D116*$F116*VLOOKUP($C116,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D116*$F116*VLOOKUP($C116,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(381,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Mannington / Legato Flooring / liquid applied"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D117*$F117*VLOOKUP($C117,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D117*$F117*VLOOKUP($C117,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,"TILE FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Tile flooring - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K119-L119","v":0},{"$f":"IF(H119=1,I119,\"\")","v":""},{"$f":"$F119*AVERAGE(K120:K124)","v":0},{"$f":"$F119*AVERAGE(L120:L124)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(41,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Tile Council of North America /  / Industry average. Includes porcelain, pressed, mosaic and quarry tile"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D120*$F120*VLOOKUP($C120,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D120*$F120*VLOOKUP($C120,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(40,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / StonePeak / Porcelain / Porcelain, standard grade"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D121*$F121*VLOOKUP($C121,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D121*$F121*VLOOKUP($C121,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(39,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Crossville / Porcelain / Standard grade"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D122*$F122*VLOOKUP($C122,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D122*$F122*VLOOKUP($C122,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(382,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Fireclay Tile / Ceramic - recycled content / Standard and Second grade"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D123*$F123*VLOOKUP($C123,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D123*$F123*VLOOKUP($C123,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(383,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / American Wonder Porcelain / Procelain - recycled content / Standard and Second grade"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D124*$F124*VLOOKUP($C124,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D124*$F124*VLOOKUP($C124,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,"VINYL FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Vinyl flooring - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K126-L126","v":0},{"$f":"IF(H126=1,I126,\"\")","v":""},{"$f":"$F126*AVERAGE(K127:K132)","v":0},{"$f":"$F126*AVERAGE(L127:L132)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(218,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Resilient Floor Covering Institute / Includes tile products from Armstrong, Congoleum, Tarkett / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D127*$F127*VLOOKUP($C127,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D127*$F127*VLOOKUP($C127,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(217,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Gerflor / Creation 70 CLIC / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D128*$F128*VLOOKUP($C128,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D128*$F128*VLOOKUP($C128,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(216,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Altro / Altro Lavencia Plus / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D129*$F129*VLOOKUP($C129,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D129*$F129*VLOOKUP($C129,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(215,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Altro / Altro Lavencia Click / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D130*$F130*VLOOKUP($C130,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D130*$F130*VLOOKUP($C130,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(372,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Shaw - Patcraft / Luxury Vinyl Tile / 2 - 5 mm "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D131*$F131*VLOOKUP($C131,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D131*$F131*VLOOKUP($C131,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(379,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Mannington / Luxury Vinyl Tile / 2.5 mm Tile and Plank"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,0,"",{"$f":"$D132*$F132*VLOOKUP($C132,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D132*$F132*VLOOKUP($C132,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,"LAMINATE FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(125,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminate flooring / Novalis / LVT / "},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K134-L134","v":0},{"$f":"IF(H134=1,I134,\"\")","v":""},{"$f":"$D134*$F134*VLOOKUP($C134,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D134*$F134*VLOOKUP($C134,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C134,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C134,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,"CORK FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(82,'Master sheet'!$AL$1:$AL$441,0))","v":"Cork flooring / European Resilient Flooring Manufacturers' Institute / Includes: Altro, Amorim, Amtico, Artigo, Aspecta, BeauFlor, Dickson, Mflor, Forbo, Gerflor, IVC, Nora, Polyflor, Tarkett, Kahrs, Windmoller / Cork floor tiles"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K136-L136","v":0},{"$f":"IF(H136=1,I136,\"\")","v":""},{"$f":"$D136*$F136*VLOOKUP($C136,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D136*$F136*VLOOKUP($C136,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(81,'Master sheet'!$AL$1:$AL$441,0))","v":"Cork flooring / Amorim / Revestimentos S.A. / Cork floating floor planks"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K137-L137","v":0},{"$f":"IF(H137=1,I137,\"\")","v":""},{"$f":"$D137*$F137*VLOOKUP($C137,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D137*$F137*VLOOKUP($C137,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,"CARPET",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(25,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet /  /  / Average from 150 samples in the EC3 database"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K139-L139","v":0},{"$f":"IF(H139=1,I139,\"\")","v":""},{"$f":"$D139*$F139*VLOOKUP($C139,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D139*$F139*VLOOKUP($C139,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Multi-EPD average from EC3 Tool"},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(29,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet / Interface / Cquest BioX / 1.5 mm Modular tile carpet"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K140-L140","v":0},{"$f":"IF(H140=1,I140,\"\")","v":""},{"$f":"$D140*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D140*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(378,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet / J+J Flooring / Standard Back / all Broadloom styles"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K141-L141","v":0},{"$f":"IF(H141=1,I141,\"\")","v":""},{"$f":"$D141*$F141*VLOOKUP($C141,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D141*$F141*VLOOKUP($C141,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[null,"FLOORING - VARIOUS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(18,'Master sheet'!$AL$1:$AL$441,0))","v":"BioBased Tile / Armstrong / BioBased Tile / Non-PVC with BioStride polyester binder, Striations BBT and Migrations BBT"},{"$f":"'USER INPUT SHEET'!$C$30","v":0},{"$f":"'USER INPUT SHEET'!$E$30","v":"m2"},1,null,null,{"$f":"K143-L143","v":0},{"$f":"IF(H143=1,I143,\"\")","v":""},{"$f":"$D143*$F143*VLOOKUP($C143,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D143*$F143*VLOOKUP($C143,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - FOOTINGS & SLABS","BASEMENT FLOORING"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Foundation Walls","index":9,"n_rows":203,"n_cols":16,"rows_kept":203,"cut":false,"hidden":false,"merged":[[71,1,71,2],[79,1,79,2],[80,0,86,1],[87,1,87,2],[88,0,94,1],[72,0,78,1],[101,0,107,1],[132,0,136,1],[95,0,95,2],[124,0,124,2],[125,1,125,2],[126,0,129,0],[130,0,130,2],[131,1,131,2],[96,0,99,1],[100,1,100,2],[108,1,108,2],[109,0,115,1],[116,1,116,2],[117,0,123,1],[142,1,142,2],[147,1,147,2],[149,0,151,1],[152,1,152,2],[137,0,137,2],[138,1,138,2],[139,0,141,1],[161,1,161,2],[154,0,160,1],[163,0,165,1],[166,1,166,2],[167,0,169,1],[190,1,190,2],[170,1,170,2],[172,0,174,1],[175,1,175,2],[176,0,177,1],[178,0,178,2],[179,1,179,2],[181,0,185,1],[186,1,186,2],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[0,0,0,2],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,0,3,1],[2,2,3,2],[2,5,3,5],[2,6,3,6],[0,3,0,11],[4,0,4,2],[29,0,29,2],[30,1,30,2],[38,0,38,2],[39,0,39,1],[31,0,37,1],[5,1,5,2],[6,0,12,1],[13,1,13,2],[14,0,20,1],[21,1,21,2],[22,0,28,1],[69,0,69,2],[70,0,70,1],[53,0,55,1],[56,1,56,2],[58,0,62,1],[63,1,63,2],[64,0,64,1],[65,1,65,2],[66,0,68,1],[45,1,45,2],[51,1,51,2],[40,0,40,2],[41,1,41,2],[43,0,44,1],[47,0,50,1]]}
["SECTION 2 ➜ COMPONENT MATERIALS FOR",null,null,"FOUNDATION - WALLS"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR FOUNDATION WALLS"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["CONCRETE WALLS",null,null,"THICKNESS:",null,"in","=",{"$f":"IF(F5=\"mm\",E5/1000,E5*2.54/100)","v":0},"m"]
[null,"CONCRETE – 25 MPa or less",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C6,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C6,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K7-L7","v":0},{"$f":"IF(H7=1,I7,\"\")","v":""},{"$f":"$D7*$H$5*$F7*VLOOKUP($C7,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D8*$H$5*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D9*$H$5*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D10*$H$5*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D11*$H$5*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K12-L12","v":0},{"$f":"IF(H12=1,I12,\"\")","v":""},{"$f":"$D12*$H$5*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D13*$H$5*$F13*VLOOKUP($C13,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K15-L15","v":0},{"$f":"IF(H15=1,I15,\"\")","v":""},{"$f":"$D15*$H$5*$F15*VLOOKUP($C15,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D16*$H$5*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D17*$H$5*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D18*$H$5*$F18*VLOOKUP($C18,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D19*$H$5*$F19*VLOOKUP($C19,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K20-L20","v":0},{"$f":"IF(H20=1,I20,\"\")","v":""},{"$f":"$D20*$H$5*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D21*$H$5*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,"CONCRETE – 31-35 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K23-L23","v":0},{"$f":"IF(H23=1,I23,\"\")","v":""},{"$f":"$D23*$H$5*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D24*$H$5*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D25*$H$5*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D26*$H$5*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D27*$H$5*$F27*VLOOKUP($C27,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K28-L28","v":0},{"$f":"IF(H28=1,I28,\"\")","v":""},{"$f":"$D28*$H$5*$F28*VLOOKUP($C28,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D29*$H$5*$F29*VLOOKUP($C29,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","CONCRETE FOUNDATION WALLS"]
["MASONRY UNIT WALLS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CONCRETE MASONRY UNITS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["If concrete grout and/or fill are being used for the CMU wall, be sure to add the volume of concrete separately.",null,"CMU Walls 8\" Hollow, No Grout - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K32-L32","v":0},{"$f":"IF(H32=1,I32,\"\")","v":""},{"$f":"$F32*AVERAGE(K33:K38)","v":0},{"$f":"$F32*AVERAGE(L33:L38)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(48,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Canadian Concrete Masonry Producers Assn / 8\" Normal weight blocks / 390 x 190 x 190 mm"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(47,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Angelus Block Co. / 8\" Normal weight blocks / 8 x 8 x 16 Precision"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FOUNDATION - WALLS","CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(49,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Permacon / 8\" Normal weight blocks / NW STD 20CM GLPW"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - WALLS","CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(46,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Canadian Concrete Masonry Producers Assn / 8\" Light weight blocks / 390 x 190 x 190 mm"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(44,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Angelus Block Co. / 8\" Light weight blocks / 9 x 8 x 16 Precision"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D37*$F37*VLOOKUP($C37,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D37*$F37*VLOOKUP($C37,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - WALLS","CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(45,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Brampton Brick / 8\" Carbon Cure Lightweight blocks / Carbon Cure 15 MPa"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D38*$F38*VLOOKUP($C38,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D38*$F38*VLOOKUP($C38,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FOUNDATION - WALLS","CMU FOUNDATION WALLS"]
["TREATED WOOD FOUNDATION",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(268,'Master sheet'!$AL$1:$AL$441,0))","v":"TREATED WOOD FOUNDATION - 2x8 framing @ 16\" OC, 3/4\" plywood sheathing"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K40-L40","v":0},{"$f":"IF(H40=1,I40,\"\")","v":""},{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","TREATED WOOD FOUNDATION"]
["CONTINUOUS INSULATION (Exterior and/or Interior)",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"EPS FOAM",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"EPS foam board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K43-L43","v":0},{"$f":"IF(H43=1,I43,\"\")","v":""},{"$f":"$F43*AVERAGE(K44:K45)","v":0},{"$f":"$F43*AVERAGE(L44:L45)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(94,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,{"$f":"IF(H44=1,I44,\"\")","v":""},{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,13,FALSE)*($E$42/5.678)","v":0},{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,27,FALSE)*($E$42/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(96,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board with graphite / BASF / Neopor / R 4.7/inch, Type II, 15 psi (Type 2, 110 kPa)"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,13,FALSE)*($E$42/5.678)","v":0},{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,27,FALSE)*($E$42/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,"XPS FOAM",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"XPS foam board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K47-L47","v":0},{"$f":"IF(H47=1,I47,\"\")","v":""},{"$f":"$F47*AVERAGE(K48:K50)","v":0},{"$f":"$F47*AVERAGE(L48:L50)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(258,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Owens Corning / Foamular NGX 250  / R 5/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K48-L48","v":0},{"$f":"IF(H48=1,I48,\"\")","v":""},{"$f":"$D48*$F48*VLOOKUP($C48,'Master sheet'!$A:$AJ,13,FALSE)*($E$46/5.678)","v":0},{"$f":"$D48*$F48*VLOOKUP($C48,'Master sheet'!$A:$AJ,27,FALSE)*($E$46/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(401,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Soprema / SOPRA-XPS / R 5.0/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K49-L49","v":0},{"$f":"IF(H49=1,I49,\"\")","v":""},{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,13,FALSE)*($E$46/5.678)","v":0},{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,27,FALSE)*($E$46/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(400,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / DuPont / Reduced GWP Grey Styrofoam™ (same as ST-100) / R 5.0/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K50-L50","v":0},{"$f":"IF(H50=1,I50,\"\")","v":""},{"$f":"$D50*$F50*VLOOKUP($C50,'Master sheet'!$A:$AJ,13,FALSE)*($E$46/5.678)","v":0},{"$f":"$D50*$F50*VLOOKUP($C50,'Master sheet'!$A:$AJ,27,FALSE)*($E$46/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(399,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) XPS foam board / DuPont / Styrofoam (Grey, Reduced GWP) / R 5.6/inch"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},"This is archived and can be deleted (BSUP)","FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,"MINERAL WOOL BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Mineral wool board - light density – AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K53-L53","v":0},{"$f":"IF(H53=1,I53,\"\")","v":""},{"$f":"$F53*AVERAGE(K54:K56)","v":0},{"$f":"$F53*AVERAGE(L54:L56)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(151,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board - light density / NAIMA / R 3.7/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D54*$F54*VLOOKUP($C54,'Master sheet'!$A:$AJ,13,FALSE)*($E$52/5.678)","v":0},{"$f":"$D54*$F54*VLOOKUP($C54,'Master sheet'!$A:$AJ,27,FALSE)*($E$52/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(150,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board / Rockwool / Rockboard 60 / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K55-L55","v":0},{"$f":"IF(H55=1,I55,\"\")","v":""},{"$f":"$D55*$F55*VLOOKUP($C55,'Master sheet'!$A:$AJ,13,FALSE)*($E$52/5.678)","v":0},{"$f":"$D55*$F55*VLOOKUP($C55,'Master sheet'!$A:$AJ,27,FALSE)*($E$52/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(407,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board  / Rockwool / Comfortboard 80 / R 4.2/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K56-L56","v":0},"",{"$f":"$D56*$F56*VLOOKUP($C56,'Master sheet'!$A:$AJ,13,FALSE)*($E$52/5.678)","v":0},{"$f":"$D56*$F56*VLOOKUP($C56,'Master sheet'!$A:$AJ,27,FALSE)*($E$52/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,"WOOD FIBER BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,"Wood fiber board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K58-L58","v":0},{"$f":"IF(H58=1,I58,\"\")","v":""},{"$f":"$F58*AVERAGE(K59:K63)","v":0},{"$f":"$F58*AVERAGE(L59:L63)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(242,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) Wood fiber board / AWC/CWC / Includes: Georgia Pacific, Louisville, BPC, Temple-Inland, Blue Ridge, Int'l Bildrite / R 2.7/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},"This is archived and can be deleted (BSUP)","FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(243,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / GUTEX / Multi-Therm / R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D60*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,13,FALSE)*($E$57/5.678)","v":0},{"$f":"$D60*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,27,FALSE)*($E$57/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(244,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Pavatex / Pavatherm / R 3.4/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D61*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,13,FALSE)*($E$57/5.678)","v":0},{"$f":"$D61*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,27,FALSE)*($E$57/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(245,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Steico / Special Dry / R 3.6/inch, 40, 120, 140, 160, 180, 200 mm"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,{"$f":"IF(H62=1,I62,\"\")","v":""},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,13,FALSE)*($E$57/5.678)","v":0},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,27,FALSE)*($E$57/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(397,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / North American Fiberboard Association / Includes: MSL, Blue Ridge Fiberboard Inc. / R 2.7/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D63*$F63*VLOOKUP($C63,'Master sheet'!$A:$AJ,13,FALSE)*($E$57/5.678)","v":0},{"$f":"$D63*$F63*VLOOKUP($C63,'Master sheet'!$A:$AJ,27,FALSE)*($E$57/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,"CORK BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(80,'Master sheet'!$AL$1:$AL$441,0))","v":"Cork board insulation / Amorim / Isolamentos / R4/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K65-L65","v":0},"",{"$f":"$D65*$F65*VLOOKUP($C65,'Master sheet'!$A:$AJ,13,FALSE)*($E$64/5.678)","v":0},{"$f":"$D65*$F65*VLOOKUP($C65,'Master sheet'!$A:$AJ,27,FALSE)*($E$64/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,"SPRAY FOAM - CLOSED CELL",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(183,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K67-L67","v":0},{"$f":"IF(H67=1,I67,\"\")","v":""},{"$f":"$D67*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,13,FALSE)*($E$66/5.678)","v":0},{"$f":"$D67*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,27,FALSE)*($E$66/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(184,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K68-L68","v":0},{"$f":"IF(H68=1,I68,\"\")","v":""},{"$f":"$D68*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,13,FALSE)*($E$66/5.678)","v":0},{"$f":"$D68*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,27,FALSE)*($E$66/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(410,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K69-L69","v":0},{"$f":"IF(H69=1,I69,\"\")","v":""},{"$f":"$D69*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,13,FALSE)*($E$66/5.678)","v":0},{"$f":"$D69*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,27,FALSE)*($E$66/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FOUNDATION - WALLS","FOUNDATION WALL CONTINUOUS INSULATION"]
["INSULATED CONCRETE FORMS (ICF) - EPS FOAM",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Step 1: Select ICF size",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(259,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS FOAM ICF R-23, 2 Sheets of 2.75\" @ R4/in., 15M rebar (6\" CONCRETE CORE must be added separately)"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},"m2",1,null,null,{"$f":"K71-L71","v":0},{"$f":"IF(H71=1,I71,\"\")","v":""},{"$f":"$D71*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D71*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,"CONCRETE – 25 MPa or less",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Step 2: Select concrete fill option.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D73*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D74*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D75*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D76*$F76*VLOOKUP($C76,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D77*$F77*VLOOKUP($C77,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K78-L78","v":0},{"$f":"IF(H78=1,I78,\"\")","v":""},{"$f":"$D78*$F78*VLOOKUP($C78,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D79*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K81-L81","v":0},{"$f":"IF(H81=1,I81,\"\")","v":""},{"$f":"$D81*$F81*VLOOKUP($C81,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D82*$F82*VLOOKUP($C82,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D83*$F83*VLOOKUP($C83,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D84*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D85*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D86*$F86*VLOOKUP($C86,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D87*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,"CONCRETE – 31-35 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K89-L89","v":0},{"$f":"IF(H89=1,I89,\"\")","v":""},{"$f":"$D89*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D90*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D91*$F91*VLOOKUP($C91,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D92*$F92*VLOOKUP($C92,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D93*$F93*VLOOKUP($C93,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D94*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D95*$F95*VLOOKUP($C95,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - EPS FOAM"]
["INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Step 1: Select ICF size",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(264,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 12\" R-22 with MINERAL WOOL INSERTS, (3 in. @ R4.2/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K97-L97","v":0},{"$f":"IF(H97=1,I97,\"\")","v":""},{"$f":"$D97*$F97*VLOOKUP($C97,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D97*$F97*VLOOKUP($C97,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(265,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 14\" R-28 with MINERAL WOOL INSERTS (5 in. @ R4.2/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,{"$f":"IF(H98=1,I98,\"\")","v":""},{"$f":"$D98*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D98*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(266,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 12\" R-21 with CORK BOARD INSERTS (3 in. @ R4/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,{"$f":"IF(H99=1,I99,\"\")","v":""},{"$f":"$D99*$F99*VLOOKUP($C99,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D99*$F99*VLOOKUP($C99,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(267,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 14\" R-27 with CORK BOARD INSERTS (5 in. @ R4/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,{"$f":"IF(H100=1,I100,\"\")","v":""},{"$f":"$D100*$F100*VLOOKUP($C100,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D100*$F100*VLOOKUP($C100,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,"CONCRETE – 25 MPa or less"]
["Step 2: Select concrete fill option for the ICF wall system. The quantity of concrete fill adapts to the form size selected.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,{"$f":"IF(H102=1,I102,\"\")","v":""},{"$f":"$D102*$F102*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C102,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D103*$F103*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C103,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D104*$F104*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C104,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D105*$F105*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C105,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D106*$F106*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C106,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K107-L107","v":0},{"$f":"IF(H107=1,I107,\"\")","v":""},{"$f":"$D107*$F107*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C107,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D108*$F108*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C108,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K110-L110","v":0},{"$f":"IF(H110=1,I110,\"\")","v":""},{"$f":"$D110*$F110*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C110,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D111*$F111*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C111,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D112*$F112*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C112,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D113*$F113*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C113,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D114*$F114*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C114,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D115*$F115*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C115,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D116*$F116*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C116,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,"CONCRETE – 31-35 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K118-L118","v":0},{"$f":"IF(H118=1,I118,\"\")","v":""},{"$f":"$D118*$F118*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C118,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D119*$F119*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C119,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D120*$F120*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C120,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D121*$F121*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C121,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D122*$F122*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C122,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D123*$F123*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C123,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D124*$F124*IF($H$97=1,0.105,IF($H$98=1,0.098,IF($H$99=1,0.105,IF($H$100=1,0.098,0))))*VLOOKUP($C124,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL ICF - WOOD CHIP/CEMENT"]
["INTERIOR FRAMING - WOOD",null,null,"FRAMING SPACING:",null,"in",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"WOOD FRAME CONSTRUCTION",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K127-L127","v":0},{"$f":"IF(H127=1,I127,\"\")","v":""},{"$f":"$D127*$F127*IF($E$125=16,0.25,0.22)*VLOOKUP($C127,'Master sheet'!$A:$AJ,13,FALSE)*0.0889","v":0},{"$f":"$F127*IF($E$125=16,$D127*0.25,$D127*0.22)*VLOOKUP($C127,'Master sheet'!$A:$AJ,27,FALSE)*0.0889","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL FRAMING - WOOD "]
[null,"2x6",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K128-L128","v":0},"",{"$f":"$D128*$F128*IF($E$125=16,0.25,0.22)*VLOOKUP($C128,'Master sheet'!$A:$AJ,13,FALSE)*0.1397","v":0},{"$f":"$F128*IF($E$125=16,$D128*0.25,$D128*0.22)*VLOOKUP($C128,'Master sheet'!$A:$AJ,27,FALSE)*0.1397","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL FRAMING - WOOD "]
[null,"2x8",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K129-L129","v":0},"",{"$f":"$D129*$F129*IF($E$125=16,0.25,0.22)*VLOOKUP($C129,'Master sheet'!$A:$AJ,13,FALSE)*0.18415","v":0},{"$f":"$F129*IF($E$125=16,$D129*0.25,$D129*0.22)*VLOOKUP($C129,'Master sheet'!$A:$AJ,27,FALSE)*0.18415","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL FRAMING - WOOD "]
[null,"Double 2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K130-L130","v":0},"",{"$f":"$D130*$F130*IF($E$125=16,0.25,0.22)*VLOOKUP($C130,'Master sheet'!$A:$AJ,13,FALSE)*(2*0.0889)","v":0},{"$f":"$F130*IF($E$125=16,$D130*0.25,$D130*0.22)*VLOOKUP($C130,'Master sheet'!$A:$AJ,27,FALSE)*(2*0.0889)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL FRAMING - WOOD "]
["INTERIOR FRAMING - STEEL",null,null,"FRAMING SPACING:",null,"in",null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"STEEL FRAMING, 2x4",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Use % to adjust if heavier gauge steel studs will be used. Framing factor based on 10' wall.",null,"Steel Framing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K133-L133","v":0},{"$f":"IF(H133=1,I133,\"\")","v":""},{"$f":"$F133*AVERAGE(K134:K137)","v":0},{"$f":"$F133*AVERAGE(L134:L137)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL FRAMING - STEEL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(209,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / Steel Recycling Institute /  / 362-S-125-18, 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K134-L134","v":0},"",{"$f":"$D134*$F134*IF($E$131=16,3.13,2.31)*VLOOKUP($C134,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D134*$F134*IF($E$131=16,3.13,2.31)*VLOOKUP($C134,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C134,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C134,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL FRAMING - STEEL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(207,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / MBA Building Supplies /  / 362-S-125-18, 20EQ gauge, ProSTUD, ProTRAK"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K135-L135","v":0},"",{"$f":"$D135*$F135*IF($E$131=16,3.13,2.31)*VLOOKUP($C135,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D135*$F135*IF($E$131=16,3.13,2.31)*VLOOKUP($C135,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL FRAMING - STEEL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(208,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / Scafco /  / 362VS125-18, 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K136-L136","v":0},"",{"$f":"$D136*$F136*IF($E$131=16,3.13,2.31)*VLOOKUP($C136,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D136*$F136*IF($E$131=16,3.13,2.31)*VLOOKUP($C136,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL FRAMING - STEEL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(205,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / ClarkDietrich /  / 362-S-125-18, 20EQ gauge, \"2x4\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K137-L137","v":0},"",{"$f":"$D137*$F137*IF($E$131=16,3.13,2.31)*VLOOKUP($C137,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D137*$F137*IF($E$131=16,3.13,2.31)*VLOOKUP($C137,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL FRAMING - STEEL"]
["CAVITY INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"SPRAY FOAM - CLOSED CELL",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(183,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K140-L140","v":0},{"$f":"IF(H140=1,I140,\"\")","v":""},{"$f":"$D140*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,13,FALSE)*($E$139/5.678)","v":0},{"$f":"$D140*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,27,FALSE)*($E$139/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(184,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K141-L141","v":0},{"$f":"IF(H141=1,I141,\"\")","v":""},{"$f":"$D141*$F141*VLOOKUP($C141,'Master sheet'!$A:$AJ,13,FALSE)*($E$139/5.678)","v":0},{"$f":"$D141*$F141*VLOOKUP($C141,'Master sheet'!$A:$AJ,27,FALSE)*($E$139/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(410,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K142-L142","v":0},{"$f":"IF(H142=1,I142,\"\")","v":""},{"$f":"$D142*$F142*VLOOKUP($C142,'Master sheet'!$A:$AJ,13,FALSE)*($E$139/5.678)","v":0},{"$f":"$D142*$F142*VLOOKUP($C142,'Master sheet'!$A:$AJ,27,FALSE)*($E$139/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,"FIBERGLASS BATT",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FOUNDATION WALL INSULATION"]
[null,null,"Fiberglass batt - Foundation Wall Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K144-L144","v":0},{"$f":"IF(H144=1,I144,\"\")","v":""},{"$f":"$F144*AVERAGE(K145:K147)","v":0},{"$f":"$F144*AVERAGE(L145:L147)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C144,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C144,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(104,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Owens Corning / EcoTouch Pink batt and roll / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K145-L145","v":0},"",{"$f":"$D145*($E$143/5.678)*$F145*VLOOKUP($C145,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D145*($E$143/5.678)*$F145*VLOOKUP($C145,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C145,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C145,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(103,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Knauf / EcoBatt / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K146-L146","v":0},"",{"$f":"$D146*($E$143/5.678)*$F146*VLOOKUP($C146,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D146*($E$143/5.678)*$F146*VLOOKUP($C146,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C146,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C146,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(102,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / CertainTeed / Sustainable Insulation / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K147-L147","v":0},"",{"$f":"$D147*($E$143/5.678)*$F147*VLOOKUP($C147,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D147*($E$143/5.678)*$F147*VLOOKUP($C147,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C147,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C147,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,"CELLULOSE INSULATION",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C148,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C148,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FOUNDATION WALL INSULATION"]
[null,null,"Cellulose - Foundation Wall Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K149-L149","v":0},{"$f":"IF(H149=1,I149,\"\")","v":""},{"$f":"$F149*AVERAGE(K150:K152)","v":0},{"$f":"$F149*AVERAGE(L150:L152)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C149,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C149,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(33,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - dense pack /  / R 3.7/inch / Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K150-L150","v":0},{"$f":"IF(H150=1,I150,\"\")","v":""},{"$f":"$D150*($E$148/5.678)*$F150*VLOOKUP($C150,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D150*($E$148/5.678)*$F150*VLOOKUP($C150,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C150,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C150,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(32,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - batt / CMS / R 3.6/inch / EcoCell"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K151-L151","v":0},"",{"$f":"$D151*($E$148/5.678)*$F151*VLOOKUP($C151,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D151*($E$148/5.678)*$F151*VLOOKUP($C151,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C151,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C151,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(35,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - spray applied / R 3.75/inch / International Cellulose Corp. / K-13, ThermoCon"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K152-L152","v":0},"",{"$f":"$D152*($E$148/5.678)*$F152*VLOOKUP($C152,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D152*($E$148/5.678)*$F152*VLOOKUP($C152,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C152,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C152,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,"MINERAL WOOL BATT",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C153,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C153,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FOUNDATION WALL INSULATION"]
[null,null,"Mineral wool batt - Foundation Wall Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K154-L154","v":0},{"$f":"IF(H154=1,I154,\"\")","v":""},{"$f":"$F154*AVERAGE(K155:K161)","v":0},{"$f":"$F154*AVERAGE(L155:L161)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C154,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C154,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(147,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Owens Corning / Thermafiber UltraBatt / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D155*($E$153/5.678)*$F155*VLOOKUP($C155,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D155*($E$153/5.678)*$F155*VLOOKUP($C155,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C155,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C155,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(148,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / Safe'n'Sound, ComfortBatt / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,{"$f":"IF(H156=1,I156,\"\")","v":""},{"$f":"$D156*($E$153/5.678)*$F156*VLOOKUP($C156,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D156*($E$153/5.678)*$F156*VLOOKUP($C156,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C156,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C156,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(402,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R14 / R 4.0/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D157*($E$153/5.678)*$F157*VLOOKUP($C157,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D157*($E$153/5.678)*$F157*VLOOKUP($C157,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C157,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C157,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(403,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R15 / R 4.3/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D158*($E$153/5.678)*$F158*VLOOKUP($C158,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D158*($E$153/5.678)*$F158*VLOOKUP($C158,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C158,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C158,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(404,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R22 / R 4.0/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D159*($E$153/5.678)*$F159*VLOOKUP($C159,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D159*($E$153/5.678)*$F159*VLOOKUP($C159,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C159,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C159,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(405,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 / R 4.4/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D160*($E$153/5.678)*$F160*VLOOKUP($C160,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D160*($E$153/5.678)*$F160*VLOOKUP($C160,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C160,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C160,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(406,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 SS / R 4.0/inch, 6\" Steel Studs"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D161*($E$153/5.678)*$F161*VLOOKUP($C161,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D161*($E$153/5.678)*$F161*VLOOKUP($C161,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C161,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C161,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,"WOOD FIBER BATT",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C162,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C162,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FOUNDATION WALL INSULATION"]
[null,null,"Wood fiber batt - Foundation Wall Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K163-L163","v":0},{"$f":"IF(H163=1,I163,\"\")","v":""},{"$f":"$F163*AVERAGE(K164:K166)","v":0},{"$f":"$F163*AVERAGE(L164:L166)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C163,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C163,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(239,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / GUTEX / ThermoFlex / R 4/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K164-L164","v":0},"",{"$f":"$D164*($E$162/5.678)*$F164*VLOOKUP($C164,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D164*($E$162/5.678)*$F164*VLOOKUP($C164,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C164,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C164,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(241,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Steico / SteicoFlex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K165-L165","v":0},"",{"$f":"$D165*($E$162/5.678)*$F165*VLOOKUP($C165,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D165*($E$162/5.678)*$F165*VLOOKUP($C165,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C165,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C165,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(240,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Pavatex / Pavaflex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K166-L166","v":0},"",{"$f":"$D166*($E$162/5.678)*$F166*VLOOKUP($C166,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D166*($E$162/5.678)*$F166*VLOOKUP($C166,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C166,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C166,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,"OTHER NATURAL FIBER INSULATIONS",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C167,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C167,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(254,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool batt / Havelock Wool /  / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K168-L168","v":0},"",{"$f":"$D168*($E$167/5.678)*$F168*VLOOKUP($C168,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D168*($E$167/5.678)*$F168*VLOOKUP($C168,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C168,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C168,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(255,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool loose fill / Havelock Wool /  / R 4.4/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K169-L169","v":0},"",{"$f":"$D169*($E$167/5.678)*$F169*VLOOKUP($C169,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D169*($E$167/5.678)*$F169*VLOOKUP($C169,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C169,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C169,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(121,'Master sheet'!$AL$1:$AL$441,0))","v":"Hemp fiber batt / NaturFibre / Hemp Wool / R 3.7/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K170-L170","v":0},"",{"$f":"$D170*($E$167/5.678)*$F170*VLOOKUP($C170,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D170*($E$167/5.678)*$F170*VLOOKUP($C170,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C170,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C170,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA"},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,"HEMPCRETE INSULATION",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C171,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C171,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FOUNDATION WALL INSULATION"]
[null,null,"Hempcrete - Foundation Wall Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K172-L172","v":0},{"$f":"IF(H172=1,I172,\"\")","v":""},{"$f":"$F172*AVERAGE(K173:K175)","v":0},{"$f":"$F172*AVERAGE(L173:L175)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C172,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C172,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(124,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / USA / R 2.1/inch, Avg. mix using NHL & PHL"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K173-L173","v":0},"",{"$f":"$D173*($E$171/5.678)*$F173*VLOOKUP($C173,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D173*($E$171/5.678)*$F173*VLOOKUP($C173,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C173,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C173,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2020"},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(123,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / Europe / R 2.1/inch, Avg. of 9 mixes"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K174-L174","v":0},"",{"$f":"$D174*($E$171/5.678)*$F174*VLOOKUP($C174,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D174*($E$171/5.678)*$F174*VLOOKUP($C174,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C174,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C174,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2017"},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(122,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / IsoHemp / Europe / R 2.1/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K175-L175","v":0},"",{"$f":"$D175*($E$171/5.678)*$F175*VLOOKUP($C175,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D175*($E$171/5.678)*$F175*VLOOKUP($C175,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C175,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C175,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA"},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,"HIGH R-VALUE INSULATION",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C176,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C176,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(214,'Master sheet'!$AL$1:$AL$441,0))","v":"Vacuum Insulated Panel / Porextherm / Vacupor / R 30/inch"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K177-L177","v":0},{"$f":"IF(H177=1,I177,\"\")","v":""},{"$f":"$D177*($E$176/5.678)*$F177*VLOOKUP($C177,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D177*($E$176/5.678)*$F177*VLOOKUP($C177,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C177,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C177,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(3,'Master sheet'!$AL$1:$AL$441,0))","v":"Aerogel blanket / Aspen Aerogels /  / R9.6/inch, White/Grey blanket"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K178-L178","v":0},"",{"$f":"$D178*($E$176/5.678)*$F178*VLOOKUP($C178,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D178*($E$176/5.678)*$F178*VLOOKUP($C178,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C178,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C178,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FOUNDATION - WALLS","FOUNDATION WALL INSULATION"]
["INTERIOR WALL CLADDING",null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C179,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C179,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"DRYWALL 1/2\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C180,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C180,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Drywall 1/2\" - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K181-L181","v":0},{"$f":"IF(H181=1,I181,\"\")","v":""},{"$f":"$F181*AVERAGE(K182:K186)","v":0},{"$f":"$F181*AVERAGE(L182:L186)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C181,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C181,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(87,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / Easi-Lite / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D182*$F182*VLOOKUP($C182,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D182*$F182*VLOOKUP($C182,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C182,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C182,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(86,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / AirRenew / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D183*$F183*VLOOKUP($C183,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D183*$F183*VLOOKUP($C183,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C183,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C183,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(88,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / M2Tech moisture resistant / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D184*$F184*VLOOKUP($C184,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D184*$F184*VLOOKUP($C184,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C184,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C184,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(89,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / Pabco / QuietRock / QuietRock 1/2\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,{"$f":"IF(H185=1,I185,\"\")","v":""},{"$f":"$D185*$F185*VLOOKUP($C185,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D185*$F185*VLOOKUP($C185,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C185,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C185,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(376,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / National Gypsum / Gold Bond XP Gypsum Board  / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D186*$F186*VLOOKUP($C186,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D186*$F186*VLOOKUP($C186,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C186,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C186,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,"DRYWALL 5/8\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C187,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C187,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(90,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K188-L188","v":0},"",{"$f":"$D188*$F188*VLOOKUP($C188,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D188*$F188*VLOOKUP($C188,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C188,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C188,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(91,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" / USG / EcoSmart Firecode / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K189-L189","v":0},"",{"$f":"$D189*$F189*VLOOKUP($C189,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D189*$F189*VLOOKUP($C189,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C189,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C189,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(377,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" Type X / National Gypsum / Gold Bond XP Fire-Shield Gypsum Board  / 5/8'' type X"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K190-L190","v":0},{"$f":"IF(H190=1,I190,\"\")","v":""},{"$f":"$D190*$F190*VLOOKUP($C190,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D190*$F190*VLOOKUP($C190,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C190,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C190,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,"OTHER CLADDING MATERIALS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C191,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C191,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(146,'Master sheet'!$AL$1:$AL$441,0))","v":"MgO board 1/2\" / North American MgO / MagTech Ultra / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,{"$f":"K192-L192","v":0},{"$f":"IF(H192=1,I192,\"\")","v":""},{"$f":"$D192*$F192*VLOOKUP($C192,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D192*$F192*VLOOKUP($C192,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C192,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C192,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,"3/4\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D193*$F193*VLOOKUP($C193,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D193*$F193*VLOOKUP($C193,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C193,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C193,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(31,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D194*$F194*VLOOKUP($C194,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D194*$F194*VLOOKUP($C194,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C194,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C194,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(17,'Master sheet'!$AL$1:$AL$441,0))","v":"Bamboo plywood / Smith & Fong / Plyboo / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D195*$F195*VLOOKUP($C195,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D195*$F195*VLOOKUP($C195,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C195,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C195,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D196*$F196*VLOOKUP($C196,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D196*$F196*VLOOKUP($C196,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C196,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C196,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(253,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood wool boards / Armstrong / Tectum / 2\" (50.8 mm)"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D197*$F197*VLOOKUP($C197,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D197*$F197*VLOOKUP($C197,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C197,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C197,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(129,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime Plaster / Mapei / MapeWall Muratura / 3/4\" Natural Hydraulic Lime (NHL)"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D198*$F198*VLOOKUP($C198,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D198*$F198*VLOOKUP($C198,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C198,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C198,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(130,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime/Cork Plaster / Diasen / Diathonite Evolution / Exterior plaster cladding, 3/4\""},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D199*$F199*VLOOKUP($C199,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D199*$F199*VLOOKUP($C199,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C199,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C199,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(42,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay plaster / Site mixed /  / 15 mm"},{"$f":"'USER INPUT SHEET'!$C$29","v":0},{"$f":"'USER INPUT SHEET'!$E$29","v":"m2"},1,null,null,0,"",{"$f":"$D200*$F200*VLOOKUP($C200,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D200*$F200*VLOOKUP($C200,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C200,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C200,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2014"},null,"FOUNDATION - WALLS","INTERIOR FOUNDATION WALL CLADDING"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Structural Elements","index":10,"n_rows":21,"n_cols":16,"rows_kept":21,"cut":false,"hidden":false,"merged":[[0,0,0,2],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[2,0,3,1],[2,2,3,2],[2,5,3,5],[2,6,3,6],[0,3,0,11],[15,0,17,1],[4,0,4,3],[5,1,5,2],[13,0,13,2],[14,1,14,2],[6,0,12,1]]}
["SECTION 3 ➜ COMPONENT MATERIALS FOR",null,null,"STRUCTURAL ELEMENTS"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR HEAVY STRUCTURE ELEMENTS"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["HEAVY TIMBER FRAMING"]
[null,"MASS TIMBER"]
["Use % function if multiple types of mass timber will be used.",null,"Heavy Timber Framing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$38","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,{"$f":"K7-L7","v":0},{"$f":"IF(H7=1,I7,\"\")","v":""},{"$f":"F7*AVERAGE(K$8:K$13)","v":0},{"$f":"F7*AVERAGE(L$8:L$13)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"STRUCTURAL ELEMENTS","MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$38","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,0,"",{"$f":"$D8*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D8*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"STRUCTURAL ELEMENTS","MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(126,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminated strand lumber (LSL) / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$38","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,0,"",{"$f":"$D9*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D9*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"STRUCTURAL ELEMENTS","MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(127,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminated veneer lumber (LVL) / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$38","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,0,"",{"$f":"$D10*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D10*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"STRUCTURAL ELEMENTS","MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(113,'Master sheet'!$AL$1:$AL$441,0))","v":"Glued laminated timber / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$38","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,0,"",{"$f":"$D11*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D11*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"STRUCTURAL ELEMENTS","MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(114,'Master sheet'!$AL$1:$AL$441,0))","v":"Glued laminated timber / Structurlam / Glulam Plus / 3-1/2\" (90mm) thick"},{"$f":"'USER INPUT SHEET'!$C$38","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,{"$f":"K12-L12","v":0},{"$f":"IF(H12=1,I12,\"\")","v":""},{"$f":"$D12*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D12*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"STRUCTURAL ELEMENTS","MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(409,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminated veneer lumber / Roseburg Forest Products / RigidLam LVL / "},{"$f":"'USER INPUT SHEET'!$C$38","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,0,"",{"$f":"$D13*$F13*VLOOKUP($C13,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D13*$F13*VLOOKUP($C13,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"STRUCTURAL ELEMENTS","MASS TIMBER"]
["HEAVY STEEL COMPONENTS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"STEEL POSTS & BEAMS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Select beam section from drop-down menu and input linear metres for each component type, as values do not come from User Input Sheet.",null,"Steel Beam W Section – AVERAGE",null,"m",1,null,null,{"$f":"K16-L16","v":0},{"$f":"IF(H16=1,I16,\"\")","v":""},{"$f":"$D16*$F16*'Master sheet'!$K$204*30","v":0},0,null,null,"STRUCTURAL ELEMENTS","HEAVY STEEL COMPONENTS"]
[null,null,null,null,"m",1,null,null,{"$f":"K17-L17","v":{"$error":"#N/A"}},{"$f":"IF(H17=1,I17,\"\")","v":""},{"$f":"$D17*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D17*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"STRUCTURAL ELEMENTS","HEAVY STEEL COMPONENTS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(199,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel post / Generic /  / 3.5 x 0.216\" (89 x 5.5 mm), Sched 40 STD"},null,"m",1,null,null,{"$f":"K18-L18","v":0},{"$f":"IF(H18=1,I18,\"\")","v":""},{"$f":"$D18*$F18*VLOOKUP($C18,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D18*$F18*VLOOKUP($C18,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"STRUCTURAL ELEMENTS","HEAVY STEEL COMPONENTS"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Ext. Walls","index":11,"n_rows":154,"n_cols":16,"rows_kept":154,"cut":false,"hidden":false,"merged":[[82,1,82,2],[90,1,90,2],[83,0,89,1],[92,0,94,1],[95,1,95,2],[111,1,111,2],[97,0,100,1],[101,1,101,2],[102,0,106,1],[107,1,107,2],[110,0,110,1],[149,0,150,1],[21,0,21,2],[22,1,22,2],[24,0,26,1],[114,1,114,2],[116,0,118,1],[119,0,119,2],[120,1,120,2],[122,0,123,1],[124,1,124,2],[126,0,130,1],[131,1,131,2],[137,1,137,2],[139,0,142,1],[143,1,143,2],[145,0,147,1],[2,8,3,8],[2,9,3,9],[2,10,3,10],[0,0,0,2],[0,3,0,12],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,0,3,1],[2,2,3,2],[71,1,71,2],[76,1,76,2],[67,1,67,2],[64,0,66,1],[2,7,3,7],[2,5,3,5],[2,6,3,6],[12,0,17,1],[53,0,53,2],[54,1,54,2],[18,0,18,2],[4,0,4,2],[5,1,5,2],[10,0,10,2],[11,1,11,2],[19,0,20,0],[27,0,27,2],[28,1,28,2],[148,0,148,2],[36,0,36,2],[37,1,37,2],[38,0,44,1],[45,1,45,2],[30,0,35,1],[46,0,52,1],[60,0,62,1],[68,0,69,1],[55,0,58,1],[59,1,59,2],[63,1,63,2],[78,0,81,1],[70,0,70,2]]}
["SECTION 4 ➜ COMPONENT MATERIALS FOR",null,null,"EXTERIOR WALLS"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR EXTERIOR WALLS"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["WOOD FRAME WALLS",null,null,"FRAMING SPACING:",null,"in. o/c"]
[null,"WOOD FRAME CONSTRUCTION"]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K7-L7","v":0},{"$f":"IF(H7=1,I7,\"\")","v":""},{"$f":"$F7*IF($E$5=16,$D7*0.25,$D7*0.22)*VLOOKUP($C7,'Master sheet'!$A:$AJ,13,FALSE)*0.0889","v":0},{"$f":"$F7*IF($E$5=16,$D7*0.25,$D7*0.22)*VLOOKUP($C7,'Master sheet'!$A:$AJ,27,FALSE)*0.0889","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","WOOD FRAME WALLS"]
[null,"2x6",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K8-L8","v":0},"",{"$f":"$F8*IF($E$5=16,$D8*0.25,$D8*0.22)*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)*0.1397","v":0},{"$f":"$F8*IF($E$5=16,$D8*0.25,$D8*0.22)*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)*0.1397","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","WOOD FRAME WALLS"]
[null,"2x8",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K9-L9","v":0},"",{"$f":"$F9*IF($E$5=16,$D9*0.25,$D9*0.22)*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)*0.18415","v":0},{"$f":"$F9*IF($E$5=16,$D9*0.25,$D9*0.22)*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)*0.18415","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","WOOD FRAME WALLS"]
[null,"Double 2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K10-L10","v":0},"",{"$f":"$F10*IF($E$5=16,$D10*0.25,$D10*0.22)*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)*(2*0.0889)","v":0},{"$f":"$F10*IF($E$5=16,$D10*0.25,$D10*0.22)*VLOOKUP($C10,'Master sheet'!$A:$AJ,27,FALSE)*(2*0.0889)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","WOOD FRAME WALLS"]
["STEEL FRAME WALLS",null,null,"FRAMING SPACING:",null,"in. o/c",null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"STEEL FRAMING, 2x6",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Use % function to adjust for other gauges of steel studs based on steel mass per unit length ratio.",null,"Steel Framing - Load bearing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K13-L13","v":0},{"$f":"IF(H13=1,I13,\"\")","v":""},{"$f":"F13*AVERAGE(K14:K18)","v":0},{"$f":"F13*AVERAGE(L14:L18)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(201,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / MarinoWARE / Structural stud and track / 600-S-137-54, 16 gauge, \"2x6\""},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D14*$F14*IF($E$11=16,3.79,2.97)*VLOOKUP($C14,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D14*$F14*IF($E$11=16,3.79,2.97)*VLOOKUP($C14,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(204,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / Steel Recycling Institute /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D15*$F15*IF($E$11=16,3.79,2.97)*VLOOKUP($C15,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D15*$F15*IF($E$11=16,3.79,2.97)*VLOOKUP($C15,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(202,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / MBA Building Supplies /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D16*$F16*IF($E$11=16,3.79,2.97)*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D16*$F16*IF($E$11=16,3.79,2.97)*VLOOKUP($C16,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(203,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / Scafco /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D17*$F17*IF($E$11=16,3.79,2.97)*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D17*$F17*IF($E$11=16,3.79,2.97)*VLOOKUP($C17,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(200,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing  / ClarkDietrich /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D18*$F18*IF($E$11=16,3.79,2.97)*VLOOKUP($C18,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D18*$F18*IF($E$11=16,3.79,2.97)*VLOOKUP($C18,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STEEL FRAME WALLS"]
["WOOD I-BEAM (TJI) FRAMING",null,null,"FRAMING SPACING:",null,"in. o/c",null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Does not include any other framing members. To include these, use Wood Frame Construction section above to enter % of wall that is lumber.","9-1/2\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K20-L20","v":0},"",{"$f":"$D20*$F20*IF($E$19=16,2.4606,1.6404)*VLOOKUP($C20,'Master sheet'!$A:$AJ,13,FALSE)*0.926","v":0},{"$f":"$D20*$F20*IF($E$19=16,2.4606,1.6404)*VLOOKUP($C20,'Master sheet'!$A:$AJ,27,FALSE)*0.926","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","WOOD I-BEAM (TJI) FRAMED WALLS"]
[null,"11-7/8\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K21-L21","v":0},"",{"$f":"$D21*$F21*IF($E$19=16,2.4606,1.6404)*VLOOKUP($C21,'Master sheet'!$A:$AJ,13,FALSE)*1.029","v":0},{"$f":"$D21*$F21*IF($E$19=16,2.4606,1.6404)*VLOOKUP($C21,'Master sheet'!$A:$AJ,27,FALSE)*1.029","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","WOOD I-BEAM (TJI) FRAMED WALLS"]
["CROSS LAMINATED TIMBER WALLS - 3-1/2\" (90mm)",null,null,null,null,null,null,null,null,{"$f":"IF(H22=1,I22,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CROSS LAMINATED TIMBER",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Cross Laminated Timber - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K24-L24","v":0},{"$f":"IF(H24=1,I24,\"\")","v":""},{"$f":"F24*AVERAGE(K25:K27)","v":0},{"$f":"F24*AVERAGE(L25:L27)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CROSS LAMINATED TIMBER WALLS - 3-1/2\" (90mm)"]
["Use % function to adjust for other thicknesses of CLT panel.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(83,'Master sheet'!$AL$1:$AL$441,0))","v":"Cross Laminated Timber / Nordic / X-Lam / 3-1/2\" (90mm) thick"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K25-L25","v":0},{"$f":"IF(H25=1,I25,\"\")","v":""},{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CROSS LAMINATED TIMBER WALLS - 3-1/2\" (90mm)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(84,'Master sheet'!$AL$1:$AL$441,0))","v":"Cross Laminated Timber / Structurlam / CrossLam / 3-1/2\" (90mm) thick"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K26-L26","v":0},{"$f":"IF(H26=1,I26,\"\")","v":""},{"$f":"$D26*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D26*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CROSS LAMINATED TIMBER WALLS - 3-1/2\" (90mm)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(85,'Master sheet'!$AL$1:$AL$441,0))","v":"Dowel Laminated Timber / StructureCraft / DowelLam / 3-1/2\" (90mm) thick"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K27-L27","v":0},{"$f":"IF(H27=1,I27,\"\")","v":""},{"$f":"$D27*$F27*VLOOKUP($C27,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D27*$F27*VLOOKUP($C27,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CROSS LAMINATED TIMBER WALLS - 3-1/2\" (90mm)"]
["CONCRETE MASONRY UNIT WALLS",null,null,null,null,null,null,null,null,{"$f":"IF(H28=1,I28,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CMU 8\" – HOLLOW, NO GROUT",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"CMU 8\" – hollow, no grout - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K30-L30","v":0},{"$f":"IF(H30=1,I30,\"\")","v":""},{"$f":"F30*AVERAGE(K31:K36)","v":0},{"$f":"F30*AVERAGE(L31:L36)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","MASONRY WALLS"]
["Use % function to adjust for other thicknesses of CMU. If filled, enter fill volume in CONCRETE FILL for CMU WALLS below",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(48,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Canadian Concrete Masonry Producers Assn / 8\" Normal weight blocks / 390 x 190 x 190 mm"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K31-L31","v":0},"",{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","MASONRY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(47,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Angelus Block Co. / 8\" Normal weight blocks / 8 x 8 x 16 Precision"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","MASONRY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(49,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Permacon / 8\" Normal weight blocks / NW STD 20CM GLPW"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","MASONRY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(46,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Canadian Concrete Masonry Producers Assn / 8\" Light weight blocks / 390 x 190 x 190 mm"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","MASONRY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(44,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Angelus Block Co. / 8\" Light weight blocks / 9 x 8 x 16 Precision"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","MASONRY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(45,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Brampton Brick / 8\" Carbon Cure Lightweight blocks / Carbon Cure 15 MPa"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","MASONRY WALLS"]
["CONCRETE FILL for CMU WALLS",null,null,"CONCRETE VOLUME",null,"m3"]
[null,"CONCRETE – 25 MPa or less",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Calculate the total concrete fill volume required for the CMU Wall area entered above.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"$E$37","v":0},"m3",1,null,null,{"$f":"K39-L39","v":0},{"$f":"IF(H39=1,I39,\"\")","v":""},{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D41*$F41*VLOOKUP($C41,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D42*$F42*VLOOKUP($C42,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,{"$f":"K44-L44","v":0},{"$f":"IF(H44=1,I44,\"\")","v":""},{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},0,"m3",1,null,null,{"$error":"#N/A"},"",{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Calculate the total concrete fill volume required for the CMU Wall area entered above.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"$E$37","v":0},"m3",1,null,null,{"$f":"K47-L47","v":0},{"$f":"IF(H47=1,I47,\"\")","v":""},{"$f":"$D47*$F47*VLOOKUP($C47,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D48*$F48*VLOOKUP($C48,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D50*$F50*VLOOKUP($C50,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D51*$F51*VLOOKUP($C51,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,{"$f":"K52-L52","v":0},{"$f":"IF(H52=1,I52,\"\")","v":""},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},0,"m3",1,null,null,{"$error":"#N/A"},"",{"$f":"$D53*$F53*VLOOKUP($C53,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CMU WALL CONCRETE FILL"]
["STRUCTURAL SHEATHING",null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"ORIENTED STRAND BOARD",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(154,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K56-L56","v":0},"",{"$f":"$D56*$F56*VLOOKUP($C56,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D56*$F56*VLOOKUP($C56,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(155,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K57-L57","v":0},{"$f":"IF(H57=1,I57,\"\")","v":""},{"$f":"$D57*$F57*VLOOKUP($C57,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D57*$F57*VLOOKUP($C57,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(157,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / Huber  / ZIP System / 7/16\" Sheathing, protective barrier and tape"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K58-L58","v":0},{"$f":"IF(H58=1,I58,\"\")","v":""},{"$f":"$D58*$F58*VLOOKUP($C58,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D58*$F58*VLOOKUP($C58,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(156,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / Huber  / AdvanTech / 1/2\" Sheathing"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K59-L59","v":0},{"$f":"IF(H59=1,I59,\"\")","v":""},{"$f":"$D59*$F59*VLOOKUP($C59,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D59*$F59*VLOOKUP($C59,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,"PLYWOOD",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K61-L61","v":0},{"$f":"IF(H61=1,I61,\"\")","v":""},{"$f":"$D61*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D61*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(160,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K62-L62","v":0},{"$f":"IF(H62=1,I62,\"\")","v":""},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(161,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 3/4\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K63-L63","v":0},{"$f":"IF(H63=1,I63,\"\")","v":""},{"$f":"$D63*$F63*VLOOKUP($C63,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D63*$F63*VLOOKUP($C63,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,"GYPSUM STRUCTURAL SHEATHING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(115,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K65-L65","v":0},{"$f":"IF(H65=1,I65,\"\")","v":""},{"$f":"$D65*$F65*VLOOKUP($C65,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D65*$F65*VLOOKUP($C65,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(116,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / USG / Securock ExoAir 430 / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K66-L66","v":0},{"$f":"IF(H66=1,I66,\"\")","v":""},{"$f":"$D66*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D66*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(418,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / CertainTeed / GlasRoc Sheathing gypsum board / 5/8\" "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D67*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D67*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,"CEMENT BOARD",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(36,'Master sheet'!$AL$1:$AL$441,0))","v":"Cement board 1/2\" / USG / Durock (132) / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D69*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D69*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(37,'Master sheet'!$AL$1:$AL$441,0))","v":"Cement board 1/2\" / USG / Durock (133) / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D70*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D70*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","STRUCTURAL SHEATHING"]
["CAVITY INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"FIBERGLASS BATT",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiberglass batt - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K73-L73","v":0},{"$f":"IF(H73=1,I73,\"\")","v":""},{"$f":"F73*AVERAGE(K74:K76)","v":0},{"$f":"F73*AVERAGE(L74:L76)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(104,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Owens Corning / EcoTouch Pink batt and roll / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K74-L74","v":0},"",{"$f":"$D74*($E$72/5.678)*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D74*($E$72/5.678)*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(102,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / CertainTeed / Sustainable Insulation / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D75*($E$72/5.678)*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D75*($E$72/5.678)*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(103,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Knauf / EcoBatt / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D76*($E$72/5.678)*$F76*VLOOKUP($C76,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D76*($E$72/5.678)*$F76*VLOOKUP($C76,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,"FIBERGLASS BLOWN-IN",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiberglass loose fill - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K78-L78","v":0},{"$f":"IF(H78=1,I78,\"\")","v":""},{"$f":"F78*AVERAGE(K79:K82)","v":0},{"$f":"F78*AVERAGE(L79:L82)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(107,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Owens Corning / AttiCat, ProCat, ProPink / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K79-L79","v":0},"",{"$f":"$D79*($E$77/5.678)*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D79*($E$77/5.678)*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(105,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / CertainTeed / InsulSafe, Optima, TruComfort / R 2.6/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D80*($E$77/5.678)*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D80*($E$77/5.678)*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(106,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Knauf / Jet Stream ULTRA / R 2.2/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K81-L81","v":0},{"$f":"IF(H81=1,I81,\"\")","v":""},{"$f":"$D81*($E$77/5.678)*$F81*VLOOKUP($C81,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D81*($E$77/5.678)*$F81*VLOOKUP($C81,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(374,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Johns Manville / Climate Pro, Attic Protector, JM Spider PLUS (Canada) / R 2.8/inch, Formaldehyde-free"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D82*($E$77/5.678)*$F82*VLOOKUP($C82,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D82*($E$77/5.678)*$F82*VLOOKUP($C82,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,"MINERAL WOOL BATT",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(147,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Owens Corning / Thermafiber UltraBatt / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D84*($E$83/5.678)*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D84*($E$83/5.678)*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(148,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / Safe'n'Sound, ComfortBatt / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K85-L85","v":0},{"$f":"IF(H85=1,I85,\"\")","v":""},{"$f":"$D85*($E$83/5.678)*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D85*($E$83/5.678)*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(402,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R14 / R 4.0/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D86*($E$83/5.678)*$F86*VLOOKUP($C86,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D86*($E$83/5.678)*$F86*VLOOKUP($C86,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(403,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R15 / R 4.3/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D87*($E$83/5.678)*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D87*($E$83/5.678)*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(404,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R22 / R 4.0/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D88*($E$83/5.678)*$F88*VLOOKUP($C88,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D88*($E$83/5.678)*$F88*VLOOKUP($C88,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(405,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 / R 4.4/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D89*($E$83/5.678)*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D89*($E$83/5.678)*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(406,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 SS / R 4.0/inch, 6\" Steel Studs"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D90*($E$83/5.678)*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D90*($E$83/5.678)*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,"CELLULOSE INSULATION",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Cellulose - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K92-L92","v":0},{"$f":"IF(H92=1,I92,\"\")","v":""},{"$f":"F92*AVERAGE(K93:K95)","v":0},{"$f":"F92*AVERAGE(L93:L95)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(33,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - dense pack /  / R 3.7/inch / Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K93-L93","v":0},{"$f":"IF(H93=1,I93,\"\")","v":""},{"$f":"$D93*($E$91/5.678)*$F93*VLOOKUP($C93,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D93*($E$91/5.678)*$F93*VLOOKUP($C93,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(32,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - batt / CMS / R 3.6/inch / EcoCell"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D94*($E$91/5.678)*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D94*($E$91/5.678)*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(35,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - spray applied / R 3.75/inch / International Cellulose Corp. / K-13, ThermoCon"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D95*($E$91/5.678)*$F95*VLOOKUP($C95,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D95*($E$91/5.678)*$F95*VLOOKUP($C95,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,"WOOD FIBER BATT",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Wood fiber batt - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K97-L97","v":0},{"$f":"IF(H97=1,I97,\"\")","v":""},{"$f":"F97*AVERAGE(K98:K101)","v":0},{"$f":"F97*AVERAGE(L98:L101)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(240,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Pavatex / Pavaflex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D98*($E$96/5.678)*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D98*($E$96/5.678)*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(239,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / GUTEX / ThermoFlex / R 4/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D99*($E$96/5.678)*$F99*VLOOKUP($C99,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D99*($E$96/5.678)*$F99*VLOOKUP($C99,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(241,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Steico / SteicoFlex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D100*($E$96/5.678)*$F100*VLOOKUP($C100,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D100*($E$96/5.678)*$F100*VLOOKUP($C100,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(238,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber - loose fill / GUTEX / ThermoFiber / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D101*($E$96/5.678)*$F101*VLOOKUP($C101,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D101*($E$96/5.678)*$F101*VLOOKUP($C101,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,"OTHER NATURAL FIBER INSULATION",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(254,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool batt / Havelock Wool /  / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K103-L103","v":0},{"$f":"IF(H103=1,I103,\"\")","v":""},{"$f":"$D103*($E$102/5.678)*$F103*VLOOKUP($C103,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D103*($E$102/5.678)*$F103*VLOOKUP($C103,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(255,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool loose fill / Havelock Wool /  / R 4.4/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K104-L104","v":0},{"$f":"IF(H104=1,I104,\"\")","v":""},{"$f":"$D104*($E$102/5.678)*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D104*($E$102/5.678)*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(121,'Master sheet'!$AL$1:$AL$441,0))","v":"Hemp fiber batt / NaturFibre / Hemp Wool / R 3.7/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K105-L105","v":0},{"$f":"IF(H105=1,I105,\"\")","v":""},{"$f":"$D105*($E$102/5.678)*$F105*VLOOKUP($C105,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D105*($E$102/5.678)*$F105*VLOOKUP($C105,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(210,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale /  / Wheat & rye straw / R 3.3/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K106-L106","v":0},{"$f":"IF(H106=1,I106,\"\")","v":""},{"$f":"$D106*($E$102/5.678)*$F106*VLOOKUP($C106,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D106*($E$102/5.678)*$F106*VLOOKUP($C106,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(412,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale / SNaB (UK) / Wheat & barley straw / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K107-L107","v":0},{"$f":"IF(H107=1,I107,\"\")","v":""},{"$f":"$D107*($E$102/5.678)*$F107*VLOOKUP($C107,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D107*($E$102/5.678)*$F107*VLOOKUP($C107,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,"SPRAY FOAM, CLOSED CELL",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(183,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K109-L109","v":0},{"$f":"IF(H109=1,I109,\"\")","v":""},{"$f":"$D109*($E$108/5.678)*$F109*VLOOKUP($C109,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D109*($E$108/5.678)*$F109*VLOOKUP($C109,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(184,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K110-L110","v":0},{"$f":"IF(H110=1,I110,\"\")","v":""},{"$f":"$D110*($E$108/5.678)*$F110*VLOOKUP($C110,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D110*($E$108/5.678)*$F110*VLOOKUP($C110,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(410,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K111-L111","v":0},{"$f":"IF(H111=1,I111,\"\")","v":""},{"$f":"$D111*($E$108/5.678)*$F111*VLOOKUP($C111,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D111*($E$108/5.678)*$F111*VLOOKUP($C111,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,"SPRAY FOAM, OPEN CELL",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(187,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell (HFC) / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K113-L113","v":0},{"$f":"IF(H113=1,I113,\"\")","v":""},{"$f":"$D113*($E$112/5.678)*$F113*VLOOKUP($C113,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D113*($E$112/5.678)*$F113*VLOOKUP($C113,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(188,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell - HFO gas / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K114-L114","v":0},{"$f":"IF(H114=1,I114,\"\")","v":""},{"$f":"$D114*($E$112/5.678)*$F114*VLOOKUP($C114,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D114*($E$112/5.678)*$F114*VLOOKUP($C114,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,"HEMPCRETE",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Hempcrete - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K116-L116","v":0},{"$f":"IF(H116=1,I116,\"\")","v":""},{"$f":"F116*AVERAGE(K117:K119)","v":0},{"$f":"F116*AVERAGE(L117:L119)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(124,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / USA / R 2.1/inch, Avg. mix using NHL & PHL"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D117*($E$115/5.678)*$F117*VLOOKUP($C117,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D117*($E$115/5.678)*$F117*VLOOKUP($C117,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2020"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(123,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / Europe / R 2.1/inch, Avg. of 9 mixes"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D118*($E$115/5.678)*$F118*VLOOKUP($C118,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D118*($E$115/5.678)*$F118*VLOOKUP($C118,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2017"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(122,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / IsoHemp / Europe / R 2.1/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D119*($E$115/5.678)*$F119*VLOOKUP($C119,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D119*($E$115/5.678)*$F119*VLOOKUP($C119,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CAVITY INSULATION"]
["CONTINUOUS INSULATION (EXT. or INT.)",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"EPS FOAM BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"EPS foam board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K122-L122","v":0},{"$f":"IF(H122=1,I122,\"\")","v":""},{"$f":"F122*AVERAGE(K123:K124)","v":0},{"$f":"F122*AVERAGE(L123:L124)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(94,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K123-L123","v":0},"",{"$f":"$D123*($E$121/5.678)*$F123*VLOOKUP($C123,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D123*($E$121/5.678)*$F123*VLOOKUP($C123,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(96,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board with graphite / BASF / Neopor / R 4.7/inch, Type II, 15 psi (Type 2, 110 kPa)"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D124*($E$121/5.678)*$F124*VLOOKUP($C124,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D124*($E$121/5.678)*$F124*VLOOKUP($C124,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,"WOOD FIBER BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Wood fiber board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K126-L126","v":0},{"$f":"IF(H126=1,I126,\"\")","v":""},{"$f":"F126*AVERAGE(K127:K131)","v":0},{"$f":"F126*AVERAGE(L127:L131)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(242,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) Wood fiber board / AWC/CWC / Includes: Georgia Pacific, Louisville, BPC, Temple-Inland, Blue Ridge, Int'l Bildrite / R 2.7/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},"This is archived and can be deleted (BSUP)","EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(243,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / GUTEX / Multi-Therm / R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D128*($E$125/5.678)*$F128*VLOOKUP($C128,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D128*($E$125/5.678)*$F128*VLOOKUP($C128,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(244,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Pavatex / Pavatherm / R 3.4/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D129*($E$125/5.678)*$F129*VLOOKUP($C129,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D129*($E$125/5.678)*$F129*VLOOKUP($C129,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(245,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Steico / Special Dry / R 3.6/inch, 40, 120, 140, 160, 180, 200 mm"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K130-L130","v":0},{"$f":"IF(H130=1,I130,\"\")","v":""},{"$f":"$D130*($E$125/5.678)*$F130*VLOOKUP($C130,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D130*($E$125/5.678)*$F130*VLOOKUP($C130,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(397,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / North American Fiberboard Association / Includes: MSL, Blue Ridge Fiberboard Inc. / R 2.7/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D131*($E$125/5.678)*$F131*VLOOKUP($C131,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D131*($E$125/5.678)*$F131*VLOOKUP($C131,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,"XPS FOAM BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"XPS foam board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K133-L133","v":0},{"$f":"IF(H133=1,I133,\"\")","v":""},{"$f":"F133*AVERAGE(K134:K136)","v":0},{"$f":"F133*AVERAGE(L134:L136)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(258,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Owens Corning / Foamular NGX 250  / R 5/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K134-L134","v":0},{"$f":"IF(H134=1,I134,\"\")","v":""},{"$f":"$D134*($E$132/5.678)*$F134*VLOOKUP($C134,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D134*($E$132/5.678)*$F134*VLOOKUP($C134,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C134,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C134,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(401,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Soprema / SOPRA-XPS / R 5.0/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K135-L135","v":0},{"$f":"IF(H135=1,I135,\"\")","v":""},{"$f":"$D135*($E$132/5.678)*$F135*VLOOKUP($C135,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D135*($E$132/5.678)*$F135*VLOOKUP($C135,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(400,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / DuPont / Reduced GWP Grey Styrofoam™ (same as ST-100) / R 5.0/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K136-L136","v":0},{"$f":"IF(H136=1,I136,\"\")","v":""},{"$f":"$D136*($E$132/5.678)*$F136*VLOOKUP($C136,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D136*($E$132/5.678)*$F136*VLOOKUP($C136,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(399,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) XPS foam board / DuPont / Styrofoam (Grey, Reduced GWP) / R 5.6/inch"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},"This is archived and can be deleted (BSUP)","EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,"POLYISOCYANURATE FOAM BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Polyisocyanurate - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K139-L139","v":0},{"$f":"IF(H139=1,I139,\"\")","v":""},{"$f":"F139*AVERAGE(K140:K143)","v":0},{"$f":"F139*AVERAGE(L140:L143)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(166,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / Dow Chemical Company / Tuff-R, Super Tuff-R, Thermax / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D140*($E$138/5.678)*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D140*($E$138/5.678)*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(167,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / Hunter / Polysio Wall insulation boards / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D141*($E$138/5.678)*$F141*VLOOKUP($C141,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D141*($E$138/5.678)*$F141*VLOOKUP($C141,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(408,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / DuPont / Thermax / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K142-L142","v":0},{"$f":"IF(H142=1,I142,\"\")","v":""},{"$f":"$D142*($E$138/5.678)*$F142*VLOOKUP($C142,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D142*($E$138/5.678)*$F142*VLOOKUP($C142,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(411,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / PIMA / Includes: Atlas, Firestone, GAF, Johns Manville, Rmax, Carlisle, Iko, Soprema / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D143*($E$138/5.678)*$F143*VLOOKUP($C143,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D143*($E$138/5.678)*$F143*VLOOKUP($C143,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,"MINERAL WOOL BOARD",null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C144,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C144,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Mineral wool board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K145-L145","v":0},{"$f":"IF(H145=1,I145,\"\")","v":""},{"$f":"F145*AVERAGE(K146:K148)","v":0},{"$f":"F145*AVERAGE(L146:L148)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C145,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C145,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(149,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board - heavy density / NAIMA / R 4.2/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D146*($E$144/5.678)*$F146*VLOOKUP($C146,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D146*($E$144/5.678)*$F146*VLOOKUP($C146,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C146,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C146,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(150,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board / Rockwool / Rockboard 60 / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K147-L147","v":0},{"$f":"IF(H147=1,I147,\"\")","v":""},{"$f":"$D147*($E$144/5.678)*$F147*VLOOKUP($C147,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D147*($E$144/5.678)*$F147*VLOOKUP($C147,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C147,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C147,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(407,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board  / Rockwool / Comfortboard 80 / R 4.2/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D148*($E$144/5.678)*$F148*VLOOKUP($C148,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D148*($E$144/5.678)*$F148*VLOOKUP($C148,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C148,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C148,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","CONTINUOUS INSULATION (EXT. or INT.)"]
["HIGH R-VALUE INSULATIONS",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,{"$f":"IF(H149=1,I149,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(VLOOKUP($C149,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C149,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(3,'Master sheet'!$AL$1:$AL$441,0))","v":"Aerogel blanket / Aspen Aerogels /  / R9.6/inch, White/Grey blanket"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K150-L150","v":0},"",{"$f":"$D150*($E$149/5.678)*$F150*VLOOKUP($C150,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D150*($E$149/5.678)*$F150*VLOOKUP($C150,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C150,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C150,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","HIGH R-VALUE INSULATION MATERIALS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(214,'Master sheet'!$AL$1:$AL$441,0))","v":"Vacuum Insulated Panel / Porextherm / Vacupor / R 30/inch"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K151-L151","v":0},"",{"$f":"$D151*($E$149/5.678)*$F151*VLOOKUP($C151,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D151*($E$149/5.678)*$F151*VLOOKUP($C151,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C151,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C151,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"EXTERIOR WALLS - STRUCTURE & INSULATION","HIGH R-VALUE INSULATION MATERIALS"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Ext. Wall Systems","index":12,"n_rows":71,"n_cols":16,"rows_kept":71,"cut":false,"hidden":false,"merged":[[59,0,59,5],[60,1,60,2],[14,1,14,2],[15,0,21,1],[22,1,22,2],[23,0,29,1],[52,0,58,1],[43,1,43,2],[35,1,35,2],[51,1,51,2],[44,0,50,1],[36,0,42,1],[2,2,3,2],[7,0,13,1],[4,0,4,2],[5,0,5,1],[30,0,30,5],[6,1,6,2],[2,6,3,6],[2,0,3,1],[63,1,63,2],[61,0,61,1],[0,3,0,11],[31,0,34,1],[0,0,0,2],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[2,5,3,5]]}
["SECTION 5 ➜ COMPONENT MATERIALS FOR",null,null,"EXTERIOR WALL SYSTEMS"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR EXTERIOR WALL SYSTEMS"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
["Step 1: Select ICF size",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(259,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS FOAM ICF R-23, 2 Sheets of 2.75\" @ R4/in., 15M rebar (6\" CONCRETE CORE must be added separately)"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K6-L6","v":0},{"$f":"IF(H6=1,I6,\"\")","v":""},{"$f":"$D6*$F6*VLOOKUP($C6,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D6*$F6*VLOOKUP($C6,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C6,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C6,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,"CONCRETE – 25 MPa or less"]
["Step 2: Select concrete fill option.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,{"$f":"IF(H8=1,I8,\"\")","v":""},{"$f":"$D8*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D8*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D9*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D9*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D10*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D10*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D11*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D11*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D12*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D12*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K13-L13","v":0},{"$f":"IF(H13=1,I13,\"\")","v":""},{"$f":"$D13*$F13*VLOOKUP($C13,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D13*$F13*VLOOKUP($C13,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D14*$F14*VLOOKUP($C14,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":{"$error":"#N/A"}},{"$f":"$D14*$F14*VLOOKUP($C14,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K16-L16","v":0},{"$f":"IF(H16=1,I16,\"\")","v":""},{"$f":"$D16*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D16*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D17*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D17*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D18*$F18*VLOOKUP($C18,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D18*$F18*VLOOKUP($C18,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D19*$F19*VLOOKUP($C19,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D19*$F19*VLOOKUP($C19,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":{"$error":"#N/A"}},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,"CONCRETE – 31-35 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K24-L24","v":0},{"$f":"IF(H24=1,I24,\"\")","v":""},{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D26*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D26*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D27*$F27*VLOOKUP($C27,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D27*$F27*VLOOKUP($C27,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D28*$F28*VLOOKUP($C28,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D28*$F28*VLOOKUP($C28,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D29*$F29*VLOOKUP($C29,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D29*$F29*VLOOKUP($C29,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D30*$F30*VLOOKUP($C30,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":{"$error":"#N/A"}},{"$f":"$D30*$F30*VLOOKUP($C30,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
["INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Step 1: Select ICF size and insulation",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(264,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 12\" R-22 with MINERAL WOOL INSERTS, (3 in. @ R4.2/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K32-L32","v":0},{"$f":"IF(H32=1,I32,\"\")","v":""},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(265,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 14\" R-28 with MINERAL WOOL INSERTS (5 in. @ R4.2/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(266,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 12\" R-21 with CORK BOARD INSERTS (3 in. @ R4/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(267,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 14\" R-27 with CORK BOARD INSERTS (5 in. @ R4/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K35-L35","v":0},{"$f":"IF(H35=1,I35,\"\")","v":""},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,"CONCRETE – 25 MPa or less"]
["Step 2: Select concrete fill option for the ICF wall system. The quantity of concrete adapts to the ICF selected.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,{"$f":"IF(H37=1,I37,\"\")","v":""},{"$f":"$D37*$F37*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C37,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D38*$F38*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C38,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D39*$F39*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C39,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D40*$F40*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C40,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D41*$F41*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C41,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K42-L42","v":0},{"$f":"IF(H42=1,I42,\"\")","v":""},{"$f":"$D42*$F42*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C42,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K43-L43","v":{"$error":"#N/A"}},"",{"$f":"$D43*$F43*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C43,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALL SYSTEMS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K45-L45","v":0},{"$f":"IF(H45=1,I45,\"\")","v":""},{"$f":"$D45*$F45*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C45,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D46*$F46*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C46,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D47*$F47*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C47,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D48*$F48*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C48,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D49*$F49*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C49,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D50*$F50*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C50,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D51*$F51*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C51,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,"CONCRETE – 31-35 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K53-L53","v":0},{"$f":"IF(H53=1,I53,\"\")","v":""},{"$f":"$D53*$F53*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C53,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D54*$F54*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C54,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D55*$F55*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C55,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D56*$F56*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C56,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D57*$F57*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C57,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D58*$F58*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C58,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D59*$F59*IF($H$32=1,0.105,IF($H$33=1,0.098,IF($H$34=1,0.105,IF($H$35=1,0.098,0))))*VLOOKUP($C59,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT"]
["PREFABRICATED PANELS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"WOOD FRAME & STRAW PANELS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(269,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD FRAME with STRAW BALE INFILL - 14\" R-46, Double 2x4 @ 30\" o/c"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K62-L62","v":0},{"$f":"IF(H62=1,I62,\"\")","v":""},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"EXTERIOR WALL SYSTEMS","PREFABRICATED PANELS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(387,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Panels / Ecocoon / Standard and Brace Panels / 40cm R16, panel only"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K63-L63","v":0},{"$f":"IF(H63=1,I63,\"\")","v":""},{"$f":"$D63*$F63*VLOOKUP($C63,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D63*$F63*VLOOKUP($C63,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALL SYSTEMS","PREFABRICATED PANELS"]
[null,"SIP PANELS - OSB & EPS FOAM",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(260,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R23 6.5\" - EPS 5.5\" @ R4/in. core, 2 sheets 1/2\" OSB"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K65-L65","v":0},{"$f":"IF(H65=1,I65,\"\")","v":""},{"$f":"$D65*$F65*VLOOKUP($C65,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D65*$F65*VLOOKUP($C65,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALL SYSTEMS","PREFABRICATED PANELS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(261,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R30 8.25\" - EPS 7.25\" @ R4/in. core, 2 sheets 1/2\" OSB"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K66-L66","v":0},{"$f":"IF(H66=1,I66,\"\")","v":""},{"$f":"$D66*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D66*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALL SYSTEMS","PREFABRICATED PANELS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(262,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R38 10.5\" - EPS 9.5\" @ R4/in. core, 2 sheets 1/2\" OSB"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K67-L67","v":0},{"$f":"IF(H67=1,I67,\"\")","v":""},{"$f":"$D67*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D67*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALL SYSTEMS","PREFABRICATED PANELS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(263,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R48 12-7/8\" - EPS 11.875\" @ R4/in. core, 2 sheets 1/2\" OSB"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K68-L68","v":0},{"$f":"IF(H68=1,I68,\"\")","v":""},{"$f":"$D68*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D68*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALL SYSTEMS","PREFABRICATED PANELS"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Party Walls","index":13,"n_rows":234,"n_cols":16,"rows_kept":234,"cut":false,"hidden":false,"merged":[[177,1,177,2],[185,1,185,2],[186,0,192,1],[193,1,193,2],[194,0,200,1],[13,1,13,2],[2,9,3,9],[2,10,3,10],[2,11,3,11],[135,1,135,2],[15,0,19,1],[39,0,45,1],[47,0,53,1],[67,1,67,2],[68,0,74,1],[75,1,75,2],[77,0,79,1],[80,1,80,2],[94,0,94,1],[116,1,116,2],[124,0,127,1],[0,0,0,2],[0,3,0,12],[1,0,1,12],[2,0,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[142,1,142,2],[146,1,146,2],[46,1,46,2],[2,8,3,8],[82,0,85,1],[122,1,122,2],[55,0,55,2],[56,1,56,2],[61,1,61,2],[63,0,66,1],[6,0,6,2],[7,1,7,2],[12,0,12,2],[20,1,20,2],[21,0,26,1],[143,0,145,1],[202,0,205,1],[99,1,99,2],[101,0,103,1],[134,0,134,2],[137,0,141,1],[168,0,170,1],[171,1,171,2],[167,1,167,2],[172,0,173,1],[175,0,175,2],[104,0,104,2],[163,1,163,2],[147,0,156,1],[157,0,157,2],[159,0,162,1],[176,0,176,1],[164,0,166,1],[158,1,158,2],[178,0,184,1],[201,0,201,5],[86,1,86,2],[87,0,91,1],[92,1,92,2],[93,0,93,1],[95,0,95,1],[96,1,96,2],[128,1,128,2],[130,0,132,1],[105,1,105,2],[107,0,108,1],[109,1,109,2],[111,0,115,1],[28,0,28,2],[29,1,29,2],[31,0,36,1],[37,0,37,2],[38,1,38,2],[223,0,229,1],[207,0,213,1],[206,1,206,2],[214,1,214,2],[215,0,221,1],[222,1,222,2]]}
["SECTION 6 ➜ COMPONENT MATERIALS FOR",null,null,"PARTY WALLS"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR PARTY WALLS"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["Note: only include half the thickness of total party wall materials using either the percentage or R-value fields. (The other half belongs to the adjacent building.) "]
["PARTY WALL FRAMING"]
["WOOD FRAME WALLS",null,null,"FRAMING SPACING:",null,"in"]
[null,"WOOD FRAME CONSTRUCTION"]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K9-L9","v":0},{"$f":"IF(H9=1,I9,\"\")","v":""},{"$f":"$F9*IF($E$7=16,$D9*0.25,$D9*0.22)*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)*0.0889","v":0},{"$f":"$F9*IF($E$7=16,$D9*0.25,$D9*0.22)*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)*0.0889","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,"2x6",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K10-L10","v":0},"",{"$f":"$F10*IF($E$7=16,$D10*0.25,$D10*0.22)*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)*0.1397","v":0},{"$f":"$F10*IF($E$7=16,$D10*0.25,$D10*0.22)*VLOOKUP($C10,'Master sheet'!$A:$AJ,27,FALSE)*0.1397","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,"2x8",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K11-L11","v":0},"",{"$f":"$F11*IF($E$7=16,$D11*0.25,$D11*0.22)*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)*0.18415","v":0},{"$f":"$F11*IF($E$7=16,$D11*0.25,$D11*0.22)*VLOOKUP($C11,'Master sheet'!$A:$AJ,27,FALSE)*0.18415","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,"Double 2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K12-L12","v":0},"",{"$f":"$F12*IF($E$7=16,$D12*0.25,$D12*0.22)*VLOOKUP($C12,'Master sheet'!$A:$AJ,13,FALSE)*(2*0.0889)","v":0},{"$f":"$F12*IF($E$7=16,$D12*0.25,$D12*0.22)*VLOOKUP($C12,'Master sheet'!$A:$AJ,27,FALSE)*(2*0.0889)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
["STEEL FRAME WALLS",null,null,"FRAMING SPACING:",null,"in",null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"STEEL FRAMING, 2x4",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Steel Framing - Interior Walls - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K15-L15","v":0},{"$f":"IF(H15=1,I15,\"\")","v":""},{"$f":"F15*AVERAGE(K16:K20)","v":0},{"$f":"F15*AVERAGE(L16:L20)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
["Use % function to adjust for different gauges of steel studs.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(206,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / MarinoWARE / Viper Stud Viper 20 / 362-S-125-18, 20EQ gauge, \"2x4\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D16*$F16*IF($E$13=16,3.13,2.31)*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D16*$F16*IF($E$13=16,3.13,2.31)*VLOOKUP($C16,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(209,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / Steel Recycling Institute /  / 362-S-125-18, 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D17*$F17*IF($E$13=16,3.13,2.31)*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D17*$F17*IF($E$13=16,3.13,2.31)*VLOOKUP($C17,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(207,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / MBA Building Supplies /  / 362-S-125-18, 20EQ gauge, ProSTUD, ProTRAK"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D18*$F18*IF($E$13=16,3.13,2.31)*VLOOKUP($C18,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D18*$F18*IF($E$13=16,3.13,2.31)*VLOOKUP($C18,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(208,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / Scafco /  / 362VS125-18, 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D19*$F19*IF($E$13=16,3.13,2.31)*VLOOKUP($C19,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D19*$F19*IF($E$13=16,3.13,2.31)*VLOOKUP($C19,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(205,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / ClarkDietrich /  / 362-S-125-18, 20EQ gauge, \"2x4\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D20*$F20*IF($E$13=16,3.13,2.31)*VLOOKUP($C20,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D20*$F20*IF($E$13=16,3.13,2.31)*VLOOKUP($C20,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,"STEEL FRAMING, 2x6",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Use % function to adjust for other gauges of steel studs.",null,"Steel Framing - Load bearing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K22-L22","v":0},{"$f":"IF(H22=1,I22,\"\")","v":""},{"$f":"F22*AVERAGE(K23:K27)","v":0},{"$f":"F22*AVERAGE(L23:L27)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(201,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / MarinoWARE / Structural stud and track / 600-S-137-54, 16 gauge, \"2x6\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D23*$F23*IF($E$13=16,3.13,2.31)*VLOOKUP($C23,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D23*$F23*IF($E$13=16,3.13,2.31)*VLOOKUP($C23,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(204,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / Steel Recycling Institute /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D24*$F24*IF($E$13=16,3.13,2.31)*VLOOKUP($C24,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D24*$F24*IF($E$13=16,3.13,2.31)*VLOOKUP($C24,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(202,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / MBA Building Supplies /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D25*$F25*IF($E$13=16,3.13,2.31)*VLOOKUP($C25,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D25*$F25*IF($E$13=16,3.13,2.31)*VLOOKUP($C25,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(203,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / Scafco /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D26*$F26*IF($E$13=16,3.13,2.31)*VLOOKUP($C26,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D26*$F26*IF($E$13=16,3.13,2.31)*VLOOKUP($C26,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(200,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing  / ClarkDietrich /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D27*$F27*IF($E$13=16,3.13,2.31)*VLOOKUP($C27,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D27*$F27*IF($E$13=16,3.13,2.31)*VLOOKUP($C27,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL FRAMING"]
["CONCRETE MASONRY UNIT PARTY WALLS"]
["CMU PARTY WALLS",null,null,null,null,null,null,null,null,{"$f":"IF(H29=1,I29,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CMU 8\" - HOLLOW, NO GROUT",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Concrete Masonry Units -  AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K31-L31","v":0},{"$f":"IF(H31=1,I31,\"\")","v":""},{"$f":"F31*AVERAGE(K32:K37)","v":0},{"$f":"F31*AVERAGE(L32:L37)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","CMU PARTY WALLS"]
["Use % function to adjust for other thicknesses of CMU.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(48,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Canadian Concrete Masonry Producers Assn / 8\" Normal weight blocks / 390 x 190 x 190 mm"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K32-L32","v":0},"",{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(47,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Angelus Block Co. / 8\" Normal weight blocks / 8 x 8 x 16 Precision"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(49,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Permacon / 8\" Normal weight blocks / NW STD 20CM GLPW"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(46,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Canadian Concrete Masonry Producers Assn / 8\" Light weight blocks / 390 x 190 x 190 mm"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(44,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Angelus Block Co. / 8\" Light weight blocks / 9 x 8 x 16 Precision"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(45,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Brampton Brick / 8\" Carbon Cure Lightweight blocks / Carbon Cure 15 MPa"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D37*$F37*VLOOKUP($C37,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D37*$F37*VLOOKUP($C37,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"PARTY WALLS","CMU PARTY WALLS"]
["CMU WALL CONCRETE FILL",null,null,"CONCRETE FILL VOLUME",null,"m3"]
[null,"CONCRETE – 25 MPa or less",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"$E$38","v":0},"m3",1,null,null,{"$f":"K40-L40","v":0},{"$f":"IF(H40=1,I40,\"\")","v":""},{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"$E$38","v":0},"m3",1,null,null,0,"",{"$f":"$D41*$F41*VLOOKUP($C41,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D42*$F42*VLOOKUP($C42,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,{"$f":"K45-L45","v":0},{"$f":"IF(H45=1,I45,\"\")","v":""},{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},0,"m3",1,null,null,{"$error":"#N/A"},"",{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"$E$38","v":0},"m3",1,null,null,{"$f":"K48-L48","v":0},{"$f":"IF(H48=1,I48,\"\")","v":""},{"$f":"$D48*$F48*VLOOKUP($C48,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D50*$F50*VLOOKUP($C50,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D51*$F51*VLOOKUP($C51,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,0,"",{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},0,"m3",1,null,null,{"$f":"K53-L53","v":0},{"$f":"IF(H53=1,I53,\"\")","v":""},{"$f":"$D53*$F53*VLOOKUP($C53,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","CMU PARTY WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},0,"m3",1,null,null,{"$error":"#N/A"},"",{"$f":"$D54*$F54*VLOOKUP($C54,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","CMU PARTY WALLS"]
["PARTY WALL INSULATION"]
["CAVITY INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,{"$f":"IF(H56=1,I56,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"FIBERGLASS BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiberglass batt - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K58-L58","v":0},{"$f":"IF(H58=1,I58,\"\")","v":""},{"$f":"F58*AVERAGE(K59:K61)","v":0},{"$f":"F58*AVERAGE(L59:L61)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(104,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Owens Corning / EcoTouch Pink batt and roll / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K59-L59","v":0},{"$f":"IF(H59=1,I59,\"\")","v":""},{"$f":"$D59*($E$57/5.678)*$F59*VLOOKUP($C59,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D59*($E$57/5.678)*$F59*VLOOKUP($C59,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(102,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / CertainTeed / Sustainable Insulation / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K60-L60","v":0},{"$f":"IF(H60=1,I60,\"\")","v":""},{"$f":"$D60*($E$57/5.678)*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D60*($E$57/5.678)*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(103,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Knauf / EcoBatt / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K61-L61","v":0},{"$f":"IF(H61=1,I61,\"\")","v":""},{"$f":"$D61*($E$57/5.678)*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D61*($E$57/5.678)*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"FIBERGLASS BLOWN-IN",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,"Fiberglass loose fill - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K63-L63","v":0},{"$f":"IF(H63=1,I63,\"\")","v":""},{"$f":"F63*AVERAGE(K64:K67)","v":0},{"$f":"F63*AVERAGE(L64:L67)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(107,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Owens Corning / AttiCat, ProCat, ProPink / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K64-L64","v":0},{"$f":"IF(H64=1,I64,\"\")","v":""},{"$f":"$D64*($E$62/5.678)*$F64*VLOOKUP($C64,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D64*($E$62/5.678)*$F64*VLOOKUP($C64,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(105,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / CertainTeed / InsulSafe, Optima, TruComfort / R 2.6/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K65-L65","v":0},{"$f":"IF(H65=1,I65,\"\")","v":""},{"$f":"$D65*($E$62/5.678)*$F65*VLOOKUP($C65,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D65*($E$62/5.678)*$F65*VLOOKUP($C65,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(106,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Knauf / Jet Stream ULTRA / R 2.2/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K66-L66","v":0},{"$f":"IF(H66=1,I66,\"\")","v":""},{"$f":"$D66*($E$62/5.678)*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D66*($E$62/5.678)*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(374,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Johns Manville / Climate Pro, Attic Protector, JM Spider PLUS (Canada) / R 2.8/inch, Formaldehyde-free"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K67-L67","v":0},{"$f":"IF(H67=1,I67,\"\")","v":""},{"$f":"$D67*($E$62/5.678)*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D67*($E$62/5.678)*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"MINERAL WOOL BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(147,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Owens Corning / Thermafiber UltraBatt / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K69-L69","v":0},{"$f":"IF(H69=1,I69,\"\")","v":""},{"$f":"$D69*($E$68/5.678)*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D69*($E$68/5.678)*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(148,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / Safe'n'Sound, ComfortBatt / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D70*($E$68/5.678)*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D70*($E$68/5.678)*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(402,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R14 / R 4.0/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D71*($E$68/5.678)*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D71*($E$68/5.678)*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(403,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R15 / R 4.3/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D72*($E$68/5.678)*$F72*VLOOKUP($C72,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D72*($E$68/5.678)*$F72*VLOOKUP($C72,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(404,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R22 / R 4.0/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D73*($E$68/5.678)*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D73*($E$68/5.678)*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(405,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 / R 4.4/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D74*($E$68/5.678)*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D74*($E$68/5.678)*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(406,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 SS / R 4.0/inch, 6\" Steel Studs"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D75*($E$68/5.678)*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D75*($E$68/5.678)*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"CELLULOSE INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,"Cellulose - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K77-L77","v":0},{"$f":"IF(H77=1,I77,\"\")","v":""},{"$f":"F77*AVERAGE(K78:K80)","v":0},{"$f":"F77*AVERAGE(L78:L80)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(33,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - dense pack /  / R 3.7/inch / Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K78-L78","v":0},{"$f":"IF(H78=1,I78,\"\")","v":""},{"$f":"$D78*($E$76/5.678)*$F78*VLOOKUP($C78,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D78*($E$76/5.678)*$F78*VLOOKUP($C78,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(32,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - batt / CMS / R 3.6/inch / EcoCell"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K79-L79","v":0},{"$f":"IF(H79=1,I79,\"\")","v":""},{"$f":"$D79*($E$76/5.678)*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D79*($E$76/5.678)*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(35,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - spray applied / R 3.75/inch / International Cellulose Corp. / K-13, ThermoCon"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K80-L80","v":0},{"$f":"IF(H80=1,I80,\"\")","v":""},{"$f":"$D80*($E$76/5.678)*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D80*($E$76/5.678)*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"WOOD FIBER BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,"Wood fiber batt - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K82-L82","v":0},{"$f":"IF(H82=1,I82,\"\")","v":""},{"$f":"F82*AVERAGE(K83:K86)","v":0},{"$f":"F82*AVERAGE(L83:L86)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(240,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Pavatex / Pavaflex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K83-L83","v":0},{"$f":"IF(H83=1,I83,\"\")","v":""},{"$f":"$D83*($E$81/5.678)*$F83*VLOOKUP($C83,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D83*($E$81/5.678)*$F83*VLOOKUP($C83,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(239,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / GUTEX / ThermoFlex / R 4/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K84-L84","v":0},{"$f":"IF(H84=1,I84,\"\")","v":""},{"$f":"$D84*($E$81/5.678)*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D84*($E$81/5.678)*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(241,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Steico / SteicoFlex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K85-L85","v":0},{"$f":"IF(H85=1,I85,\"\")","v":""},{"$f":"$D85*($E$81/5.678)*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D85*($E$81/5.678)*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(238,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber - loose fill / GUTEX / ThermoFiber / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K86-L86","v":0},{"$f":"IF(H86=1,I86,\"\")","v":""},{"$f":"$D86*($E$81/5.678)*$F86*VLOOKUP($C86,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D86*($E$81/5.678)*$F86*VLOOKUP($C86,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"OTHER NATURAL FIBER INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(254,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool batt / Havelock Wool /  / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K88-L88","v":0},{"$f":"IF(H88=1,I88,\"\")","v":""},{"$f":"$D88*($E$87/5.678)*$F88*VLOOKUP($C88,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D88*($E$87/5.678)*$F88*VLOOKUP($C88,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(255,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool loose fill / Havelock Wool /  / R 4.4/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K89-L89","v":0},{"$f":"IF(H89=1,I89,\"\")","v":""},{"$f":"$D89*($E$87/5.678)*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D89*($E$87/5.678)*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(121,'Master sheet'!$AL$1:$AL$441,0))","v":"Hemp fiber batt / NaturFibre / Hemp Wool / R 3.7/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K90-L90","v":0},{"$f":"IF(H90=1,I90,\"\")","v":""},{"$f":"$D90*($E$87/5.678)*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D90*($E$87/5.678)*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(210,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale /  / Wheat & rye straw / R 3.3/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K91-L91","v":0},{"$f":"IF(H91=1,I91,\"\")","v":""},{"$f":"$D91*($E$87/5.678)*$F91*VLOOKUP($C91,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D91*($E$87/5.678)*$F91*VLOOKUP($C91,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(412,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale / SNaB (UK) / Wheat & barley straw / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K92-L92","v":0},{"$f":"IF(H92=1,I92,\"\")","v":""},{"$f":"$D92*($E$87/5.678)*$F92*VLOOKUP($C92,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D92*($E$87/5.678)*$F92*VLOOKUP($C92,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"SPRAY FOAM, CLOSED CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(183,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K94-L94","v":0},{"$f":"IF(H94=1,I94,\"\")","v":""},{"$f":"$D94*($E$93/5.678)*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D94*($E$93/5.678)*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(184,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K95-L95","v":0},{"$f":"IF(H95=1,I95,\"\")","v":""},{"$f":"$D95*($E$93/5.678)*$F95*VLOOKUP($C95,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D95*($E$93/5.678)*$F95*VLOOKUP($C95,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(410,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K96-L96","v":0},{"$f":"IF(H96=1,I96,\"\")","v":""},{"$f":"$D96*($E$93/5.678)*$F96*VLOOKUP($C96,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D96*($E$93/5.678)*$F96*VLOOKUP($C96,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"SPRAY FOAM, OPEN CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(187,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell (HFC) / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K98-L98","v":0},{"$f":"IF(H98=1,I98,\"\")","v":""},{"$f":"$D98*($E$97/5.678)*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D98*($E$97/5.678)*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(188,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell - HFO gas / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K99-L99","v":0},{"$f":"IF(H99=1,I99,\"\")","v":""},{"$f":"$D99*($E$97/5.678)*$F99*VLOOKUP($C99,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D99*($E$97/5.678)*$F99*VLOOKUP($C99,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"HEMPCRETE",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,"Hempcrete - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K101-L101","v":0},{"$f":"IF(H101=1,I101,\"\")","v":""},{"$f":"F101*AVERAGE(K102:K104)","v":0},{"$f":"F101*AVERAGE(L102:L104)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(124,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / USA / R 2.1/inch, Avg. mix using NHL & PHL"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K102-L102","v":0},{"$f":"IF(H102=1,I102,\"\")","v":""},{"$f":"$D102*($E$100/5.678)*$F102*VLOOKUP($C102,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D102*($E$100/5.678)*$F102*VLOOKUP($C102,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2020"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(123,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / Europe / R 2.1/inch, Avg. of 9 mixes"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K103-L103","v":0},{"$f":"IF(H103=1,I103,\"\")","v":""},{"$f":"$D103*($E$100/5.678)*$F103*VLOOKUP($C103,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D103*($E$100/5.678)*$F103*VLOOKUP($C103,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2017"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(122,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / IsoHemp / Europe / R 2.1/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K104-L104","v":0},{"$f":"IF(H104=1,I104,\"\")","v":""},{"$f":"$D104*($E$100/5.678)*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D104*($E$100/5.678)*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA"},null,"PARTY WALLS","PARTY WALL INSULATION"]
["RIGID INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,{"$f":"IF(H105=1,I105,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"EPS FOAM BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"EPS foam board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K107-L107","v":0},{"$f":"IF(H107=1,I107,\"\")","v":""},{"$f":"F107*AVERAGE(K108:K109)","v":0},{"$f":"F107*AVERAGE(L108:L109)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(94,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K108-L108","v":0},"",{"$f":"$D108*($E$106/5.678)*$F108*VLOOKUP($C108,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D108*($E$106/5.678)*$F108*VLOOKUP($C108,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(96,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board with graphite / BASF / Neopor / R 4.7/inch, Type II, 15 psi (Type 2, 110 kPa)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D109*($E$106/5.678)*$F109*VLOOKUP($C109,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D109*($E$106/5.678)*$F109*VLOOKUP($C109,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"WOOD FIBER BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Wood fiber board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K111-L111","v":0},{"$f":"IF(H111=1,I111,\"\")","v":""},{"$f":"F111*AVERAGE(K112:K116)","v":0},{"$f":"F111*AVERAGE(L112:L116)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(242,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) Wood fiber board / AWC/CWC / Includes: Georgia Pacific, Louisville, BPC, Temple-Inland, Blue Ridge, Int'l Bildrite / R 2.7/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},"This is archived and can be deleted (BSUP)","PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(243,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / GUTEX / Multi-Therm / R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D113*($E$110/5.678)*$F113*VLOOKUP($C113,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D113*($E$110/5.678)*$F113*VLOOKUP($C113,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(244,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Pavatex / Pavatherm / R 3.4/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D114*($E$110/5.678)*$F114*VLOOKUP($C114,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D114*($E$110/5.678)*$F114*VLOOKUP($C114,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(245,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Steico / Special Dry / R 3.6/inch, 40, 120, 140, 160, 180, 200 mm"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K115-L115","v":0},{"$f":"IF(H115=1,I115,\"\")","v":""},{"$f":"$D115*($E$110/5.678)*$F115*VLOOKUP($C115,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D115*($E$110/5.678)*$F115*VLOOKUP($C115,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(397,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / North American Fiberboard Association / Includes: MSL, Blue Ridge Fiberboard Inc. / R 2.7/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D116*($E$110/5.678)*$F116*VLOOKUP($C116,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D116*($E$110/5.678)*$F116*VLOOKUP($C116,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"XPS FOAM BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"XPS foam board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K118-L118","v":0},{"$f":"IF(H118=1,I118,\"\")","v":""},{"$f":"F118*AVERAGE(K119:K121)","v":0},{"$f":"F118*AVERAGE(L119:L121)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(258,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Owens Corning / Foamular NGX 250  / R 5/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K119-L119","v":0},{"$f":"IF(H119=1,I119,\"\")","v":""},{"$f":"$D119*($E$117/5.678)*$F119*VLOOKUP($C119,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D119*($E$117/5.678)*$F119*VLOOKUP($C119,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(401,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Soprema / SOPRA-XPS / R 5.0/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K120-L120","v":0},{"$f":"IF(H120=1,I120,\"\")","v":""},{"$f":"$D120*($E$117/5.678)*$F120*VLOOKUP($C120,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D120*($E$117/5.678)*$F120*VLOOKUP($C120,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(400,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / DuPont / Reduced GWP Grey Styrofoam™ (same as ST-100) / R 5.0/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K121-L121","v":0},{"$f":"IF(H121=1,I121,\"\")","v":""},{"$f":"$D121*($E$117/5.678)*$F121*VLOOKUP($C121,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D121*($E$117/5.678)*$F121*VLOOKUP($C121,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(399,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) XPS foam board / DuPont / Styrofoam (Grey, Reduced GWP) / R 5.6/inch"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},"This is archived and can be deleted (BSUP)","PARTY WALLS","PARTY WALL INSULATION"]
[null,"POLYISOCYANURATE FOAM BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Polyisocyanurate - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K124-L124","v":0},{"$f":"IF(H124=1,I124,\"\")","v":""},{"$f":"F124*AVERAGE(K125:K128)","v":0},{"$f":"F124*AVERAGE(L125:L128)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(166,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / Dow Chemical Company / Tuff-R, Super Tuff-R, Thermax / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D125*($E$123/5.678)*$F125*VLOOKUP($C125,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D125*($E$123/5.678)*$F125*VLOOKUP($C125,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(167,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / Hunter / Polysio Wall insulation boards / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D126*($E$123/5.678)*$F126*VLOOKUP($C126,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D126*($E$123/5.678)*$F126*VLOOKUP($C126,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(408,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / DuPont / Thermax / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K127-L127","v":0},{"$f":"IF(H127=1,I127,\"\")","v":""},{"$f":"$D127*($E$123/5.678)*$F127*VLOOKUP($C127,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D127*($E$123/5.678)*$F127*VLOOKUP($C127,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(411,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / PIMA / Includes: Atlas, Firestone, GAF, Johns Manville, Rmax, Carlisle, Iko, Soprema / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D128*($E$123/5.678)*$F128*VLOOKUP($C128,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D128*($E$123/5.678)*$F128*VLOOKUP($C128,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,"MINERAL WOOL BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Mineral wool board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K130-L130","v":0},{"$f":"IF(H130=1,I130,\"\")","v":""},{"$f":"F130*AVERAGE(K131:K133)","v":0},{"$f":"F130*AVERAGE(L131:L133)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(149,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board - heavy density / NAIMA / R 4.2/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D131*($E$129/5.678)*$F131*VLOOKUP($C131,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D131*($E$129/5.678)*$F131*VLOOKUP($C131,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(150,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board / Rockwool / Rockboard 60 / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K132-L132","v":0},{"$f":"IF(H132=1,I132,\"\")","v":""},{"$f":"$D132*($E$129/5.678)*$F132*VLOOKUP($C132,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D132*($E$129/5.678)*$F132*VLOOKUP($C132,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(407,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board  / Rockwool / Comfortboard 80 / R 4.2/inch"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D133*($E$129/5.678)*$F133*VLOOKUP($C133,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D133*($E$129/5.678)*$F133*VLOOKUP($C133,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INSULATION"]
["PARTY WALL SHEETING"]
["INTERIOR CLADDING for PARTY WALLS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"DRYWALL 1/2\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Drywall 1/2\" Typical - Interior Cladding for Exterior Walls - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K137-L137","v":0},{"$f":"IF(H137=1,I137,\"\")","v":""},{"$f":"F137*AVERAGE(K138:K142)","v":0},{"$f":"F137*AVERAGE(L138:L142)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(87,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / Easi-Lite / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K138-L138","v":0},{"$f":"IF(H138=1,I138,\"\")","v":""},{"$f":"$D138*$F138*VLOOKUP($C138,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D138*$F138*VLOOKUP($C138,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(86,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / AirRenew / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D139*$F139*VLOOKUP($C139,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D139*$F139*VLOOKUP($C139,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(88,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / M2Tech moisture resistant / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D140*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D140*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(89,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / Pabco / QuietRock / QuietRock 1/2\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K141-L141","v":0},{"$f":"IF(H141=1,I141,\"\")","v":""},{"$f":"$D141*$F141*VLOOKUP($C141,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D141*$F141*VLOOKUP($C141,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(376,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / National Gypsum / Gold Bond XP Gypsum Board  / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D142*$F142*VLOOKUP($C142,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D142*$F142*VLOOKUP($C142,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,"DRYWALL 5/8\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(90,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D144*$F144*VLOOKUP($C144,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D144*$F144*VLOOKUP($C144,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C144,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C144,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(91,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" / USG / EcoSmart Firecode / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D145*$F145*VLOOKUP($C145,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D145*$F145*VLOOKUP($C145,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C145,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C145,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(377,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" Type X / National Gypsum / Gold Bond XP Fire-Shield Gypsum Board  / 5/8'' type X"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K146-L146","v":0},{"$f":"IF(H146=1,I146,\"\")","v":""},{"$f":"$D146*$F146*VLOOKUP($C146,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D146*$F146*VLOOKUP($C146,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C146,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C146,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,"OTHER CLADDING MATERIALS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C147,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C147,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(146,'Master sheet'!$AL$1:$AL$441,0))","v":"MgO board 1/2\" / North American MgO / MagTech Ultra / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K148-L148","v":0},{"$f":"IF(H148=1,I148,\"\")","v":""},{"$f":"$D148*$F148*VLOOKUP($C148,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D148*$F148*VLOOKUP($C148,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C148,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C148,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K149-L149","v":0},"",{"$f":"$D149*$F149*VLOOKUP($C149,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D149*$F149*VLOOKUP($C149,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C149,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C149,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(31,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D150*$F150*VLOOKUP($C150,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D150*$F150*VLOOKUP($C150,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C150,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C150,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(17,'Master sheet'!$AL$1:$AL$441,0))","v":"Bamboo plywood / Smith & Fong / Plyboo / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D151*$F151*VLOOKUP($C151,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D151*$F151*VLOOKUP($C151,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C151,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C151,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D152*$F152*VLOOKUP($C152,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D152*$F152*VLOOKUP($C152,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C152,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C152,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(253,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood wool boards / Armstrong / Tectum / 2\" (50.8 mm)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D153*$F153*VLOOKUP($C153,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D153*$F153*VLOOKUP($C153,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C153,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C153,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(129,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime Plaster / Mapei / MapeWall Muratura / 3/4\" Natural Hydraulic Lime (NHL)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D154*$F154*VLOOKUP($C154,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D154*$F154*VLOOKUP($C154,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C154,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C154,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(130,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime/Cork Plaster / Diasen / Diathonite Evolution / Exterior plaster cladding, 3/4\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D155*$F155*VLOOKUP($C155,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D155*$F155*VLOOKUP($C155,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C155,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C155,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(42,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay plaster / Site mixed /  / 15 mm"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D156*$F156*VLOOKUP($C156,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D156*$F156*VLOOKUP($C156,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C156,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C156,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2014"},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(41,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Tile Council of North America /  / Industry average. Includes porcelain, pressed, mosaic and quarry tile"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D157*$F157*VLOOKUP($C157,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D157*$F157*VLOOKUP($C157,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C157,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C157,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"PARTY WALLS","PARTY WALL INTERIOR CLADDING"]
["STRUCTURAL SHEATHING",null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C158,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C158,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"ORIENTED STRAND BOARD",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C159,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C159,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(154,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K160-L160","v":0},"",{"$f":"$D160*$F160*VLOOKUP($C160,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D160*$F160*VLOOKUP($C160,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C160,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C160,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(155,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K161-L161","v":0},{"$f":"IF(H161=1,I161,\"\")","v":""},{"$f":"$D161*$F161*VLOOKUP($C161,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D161*$F161*VLOOKUP($C161,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C161,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C161,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(157,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / Huber  / ZIP System / 7/16\" Sheathing, protective barrier and tape"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K162-L162","v":0},{"$f":"IF(H162=1,I162,\"\")","v":""},{"$f":"$D162*$F162*VLOOKUP($C162,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D162*$F162*VLOOKUP($C162,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C162,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C162,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(156,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / Huber  / AdvanTech / 1/2\" Sheathing"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K163-L163","v":0},{"$f":"IF(H163=1,I163,\"\")","v":""},{"$f":"$D163*$F163*VLOOKUP($C163,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D163*$F163*VLOOKUP($C163,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C163,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C163,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,"PLYWOOD",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C164,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C164,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K165-L165","v":0},{"$f":"IF(H165=1,I165,\"\")","v":""},{"$f":"$D165*$F165*VLOOKUP($C165,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D165*$F165*VLOOKUP($C165,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C165,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C165,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(160,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K166-L166","v":0},{"$f":"IF(H166=1,I166,\"\")","v":""},{"$f":"$D166*$F166*VLOOKUP($C166,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D166*$F166*VLOOKUP($C166,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C166,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C166,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(161,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 3/4\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K167-L167","v":0},{"$f":"IF(H167=1,I167,\"\")","v":""},{"$f":"$D167*$F167*VLOOKUP($C167,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D167*$F167*VLOOKUP($C167,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C167,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C167,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,"GYPSUM STRUCTURAL SHEATHING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C168,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C168,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(115,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D169*$F169*VLOOKUP($C169,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D169*$F169*VLOOKUP($C169,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C169,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C169,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(116,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / USG / Securock ExoAir 430 / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K170-L170","v":0},{"$f":"IF(H170=1,I170,\"\")","v":""},{"$f":"$D170*$F170*VLOOKUP($C170,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D170*$F170*VLOOKUP($C170,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C170,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C170,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(418,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / CertainTeed / GlasRoc Sheathing gypsum board / 5/8\" "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D171*$F171*VLOOKUP($C171,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D171*$F171*VLOOKUP($C171,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C171,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C171,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,"CEMENT BOARD",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C172,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C172,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(36,'Master sheet'!$AL$1:$AL$441,0))","v":"Cement board 1/2\" / USG / Durock (132) / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K173-L173","v":0},{"$f":"IF(H173=1,I173,\"\")","v":""},{"$f":"$D173*$F173*VLOOKUP($C173,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D173*$F173*VLOOKUP($C173,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C173,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C173,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(37,'Master sheet'!$AL$1:$AL$441,0))","v":"Cement board 1/2\" / USG / Durock (133) / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D174*$F174*VLOOKUP($C174,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D174*$F174*VLOOKUP($C174,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C174,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C174,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL SHEATHING"]
["PARTY WALL ICFs"]
["INSULATED CONCRETE FORMS (ICF) - EPS FOAM"]
["Step 1: Select ICF size",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(259,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS FOAM ICF R-23, 2 Sheets of 2.75\" @ R4/in., 15M rebar (6\" CONCRETE CORE must be added separately)"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K177-L177","v":0},{"$f":"IF(H177=1,I177,\"\")","v":""},{"$f":"$D177*$F177*VLOOKUP($C177,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D177*$F177*VLOOKUP($C177,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C177,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C177,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,"CONCRETE – 25 MPa or less"]
["Step 2: Select concrete fill option.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,{"$f":"IF(H179=1,I179,\"\")","v":""},{"$f":"$D179*$F179*VLOOKUP($C179,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D179*$F179*VLOOKUP($C179,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C179,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C179,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D180*$F180*VLOOKUP($C180,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D180*$F180*VLOOKUP($C180,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C180,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C180,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D181*$F181*VLOOKUP($C181,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D181*$F181*VLOOKUP($C181,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C181,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C181,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D182*$F182*VLOOKUP($C182,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D182*$F182*VLOOKUP($C182,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C182,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C182,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D183*$F183*VLOOKUP($C183,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D183*$F183*VLOOKUP($C183,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C183,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C183,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K184-L184","v":0},{"$f":"IF(H184=1,I184,\"\")","v":""},{"$f":"$D184*$F184*VLOOKUP($C184,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D184*$F184*VLOOKUP($C184,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C184,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C184,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D185*$F185*VLOOKUP($C185,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":{"$error":"#N/A"}},{"$f":"$D185*$F185*VLOOKUP($C185,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C185,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C185,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C186,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C186,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K187-L187","v":0},{"$f":"IF(H187=1,I187,\"\")","v":""},{"$f":"$D187*$F187*VLOOKUP($C187,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D187*$F187*VLOOKUP($C187,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C187,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C187,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D188*$F188*VLOOKUP($C188,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D188*$F188*VLOOKUP($C188,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C188,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C188,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D189*$F189*VLOOKUP($C189,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D189*$F189*VLOOKUP($C189,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C189,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C189,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D190*$F190*VLOOKUP($C190,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D190*$F190*VLOOKUP($C190,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C190,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C190,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D191*$F191*VLOOKUP($C191,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D191*$F191*VLOOKUP($C191,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C191,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C191,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D192*$F192*VLOOKUP($C192,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D192*$F192*VLOOKUP($C192,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C192,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C192,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D193*$F193*VLOOKUP($C193,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":{"$error":"#N/A"}},{"$f":"$D193*$F193*VLOOKUP($C193,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C193,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C193,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,"CONCRETE – 31-35 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C194,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C194,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K195-L195","v":0},{"$f":"IF(H195=1,I195,\"\")","v":""},{"$f":"$D195*$F195*VLOOKUP($C195,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D195*$F195*VLOOKUP($C195,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C195,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C195,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D196*$F196*VLOOKUP($C196,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D196*$F196*VLOOKUP($C196,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C196,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C196,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D197*$F197*VLOOKUP($C197,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D197*$F197*VLOOKUP($C197,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C197,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C197,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D198*$F198*VLOOKUP($C198,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D198*$F198*VLOOKUP($C198,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C198,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C198,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D199*$F199*VLOOKUP($C199,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D199*$F199*VLOOKUP($C199,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C199,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C199,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D200*$F200*VLOOKUP($C200,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":0},{"$f":"$D200*$F200*VLOOKUP($C200,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C200,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C200,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D201*$F201*VLOOKUP($C201,'Master sheet'!$A:$AJ,13,FALSE)*0.15875","v":{"$error":"#N/A"}},{"$f":"$D201*$F201*VLOOKUP($C201,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C201,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C201,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
["INSULATED CONCRETE FORMS (ICF) - WOOD CHIP/CEMENT",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C202,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C202,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Step 1: Select ICF size and insulation",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(264,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 12\" R-22 with MINERAL WOOL INSERTS, (3 in. @ R4.2/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K203-L203","v":0},{"$f":"IF(H203=1,I203,\"\")","v":""},{"$f":"$D203*$F203*VLOOKUP($C203,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D203*$F203*VLOOKUP($C203,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C203,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C203,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(265,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 14\" R-28 with MINERAL WOOL INSERTS (5 in. @ R4.2/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D204*$F204*VLOOKUP($C204,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D204*$F204*VLOOKUP($C204,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C204,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C204,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(266,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 12\" R-21 with CORK BOARD INSERTS (3 in. @ R4/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D205*$F205*VLOOKUP($C205,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D205*$F205*VLOOKUP($C205,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C205,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C205,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(267,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 14\" R-27 with CORK BOARD INSERTS (5 in. @ R4/in.), 15M REBAR"},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K206-L206","v":0},{"$f":"IF(H206=1,I206,\"\")","v":""},{"$f":"$D206*$F206*VLOOKUP($C206,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D206*$F206*VLOOKUP($C206,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C206,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C206,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA in Composite"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,"CONCRETE – 25 MPa or less"]
["Step 2: Select concrete fill option for the ICF wall system. The quantity of concrete adapts to the ICF selected.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,{"$f":"IF(H208=1,I208,\"\")","v":""},{"$f":"$D208*$F208*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C208,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D208*$F208*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C208,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C208,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C208,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D209*$F209*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C209,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D209*$F209*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C209,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C209,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C209,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D210*$F210*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C210,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D210*$F210*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C210,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C210,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C210,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D211*$F211*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C211,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D211*$F211*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C211,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C211,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C211,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D212*$F212*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C212,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D212*$F212*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C212,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C212,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C212,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K213-L213","v":0},{"$f":"IF(H213=1,I213,\"\")","v":""},{"$f":"$D213*$F213*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C213,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D213*$F213*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C213,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C213,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C213,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K214-L214","v":{"$error":"#N/A"}},"",{"$f":"$D214*$F214*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C214,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D214*$F214*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C214,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C214,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C214,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"PARTY WALLS","PARTY WALL ICFs"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C215,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C215,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K216-L216","v":0},{"$f":"IF(H216=1,I216,\"\")","v":""},{"$f":"$D216*$F216*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C216,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D216*$F216*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C216,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C216,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C216,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D217*$F217*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C217,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D217*$F217*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C217,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C217,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C217,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D218*$F218*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C218,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D218*$F218*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C218,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C218,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C218,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D219*$F219*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C219,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D219*$F219*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C219,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C219,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C219,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D220*$F220*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C220,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D220*$F220*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C220,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C220,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C220,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D221*$F221*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C221,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D221*$F221*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C221,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C221,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C221,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D222*$F222*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C222,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D222*$F222*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C222,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C222,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C222,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,"CONCRETE – 31-35 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C223,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C223,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$f":"K224-L224","v":0},{"$f":"IF(H224=1,I224,\"\")","v":""},{"$f":"$D224*$F224*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C224,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D224*$F224*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C224,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C224,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C224,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D225*$F225*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C225,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D225*$F225*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C225,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C225,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C225,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D226*$F226*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C226,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D226*$F226*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C226,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C226,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C226,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D227*$F227*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C227,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D227*$F227*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C227,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C227,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C227,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D228*$F228*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C228,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D228*$F228*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C228,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C228,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C228,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,0,"",{"$f":"$D229*$F229*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C229,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D229*$F229*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C229,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C229,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C229,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"31-35\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$39","v":0},{"$f":"'USER INPUT SHEET'!$E$39","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D230*$F230*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C230,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D230*$F230*IF($H$203=1,0.105,IF($H$204=1,0.098,IF($H$205=1,0.105,IF($H$206=1,0.098,0))))*VLOOKUP($C230,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C230,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C230,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FOUNDATION - WALLS","PARTY WALL ICFs"]
[]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Cladding","index":14,"n_rows":82,"n_cols":16,"rows_kept":82,"cut":false,"hidden":false,"merged":[[18,0,25,0],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[4,0,4,2],[5,1,5,2],[13,1,13,2],[16,1,16,2],[6,0,12,1],[14,0,15,0],[0,0,0,2],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,0,3,1],[2,2,3,2],[2,5,3,5],[2,6,3,6],[0,3,0,11],[26,1,26,2],[28,1,28,2],[27,0,27,1],[30,0,31,1],[32,1,32,2],[64,1,64,2],[68,1,68,2],[69,0,78,1],[40,1,40,2],[44,1,44,2],[59,0,63,1],[57,1,57,2],[49,1,49,2],[50,0,52,1],[65,0,67,1],[34,0,39,1],[42,0,43,1],[45,0,48,1],[53,0,53,2],[56,0,56,2]]}
["SECTION 7 ➜ COMPONENT MATERIALS FOR",null,null,"EXTERIOR WALLS - CLADDING"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR EXTERIOR WALLS CLADDING"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["EXTERIOR CLADDING"]
[null,"BRICK"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(23,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay, Generic Modular / Brick Industry Association / US-Canada Industry Average / 3-5/8\" x 2-3/4\" x 7-5/8\" incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K7-L7","v":0},{"$f":"IF(H7=1,I7,\"\")","v":""},{"$f":"$D7*$F7*VLOOKUP($C7,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D7*$F7*VLOOKUP($C7,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(19,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Calcium Silicate / Arriscraft / Contemporary Brick / 3-1/8\" x 3-1/2\" x any length, incl. mortar and ties"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D8*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D8*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(20,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Cement / MidWest / Architectural Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D9*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D9*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(21,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / Interstate / Avg Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D10*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D10*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(22,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / Interstate / Avg Thin Face Brick / 3-9/16\" x 5/8\" x 11-5/8\" (90 x 16 mm x 295) incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D11*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D11*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(388,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / SHAW / Slender - Thin Face Brick / 2 1/4\" x 1/2\" x 7-1/2\" (57 x 12.7 mm x 190) incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D12*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D12*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(389,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / SHAW / Avg Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D13*$F13*VLOOKUP($C13,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D13*$F13*VLOOKUP($C13,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"WOOD CLADDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"3/4\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(31,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K15-L15","v":0},{"$f":"IF(H15=1,I15,\"\")","v":""},{"$f":"$D15*$F15*VLOOKUP($C15,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D15*$F15*VLOOKUP($C15,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"3/4\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K16-L16","v":0},{"$f":"IF(H16=1,I16,\"\")","v":""},{"$f":"$D16*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D16*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"FIBER CEMENT",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiber Cement siding - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K18-L18","v":0},{"$f":"IF(H18=1,I18,\"\")","v":""},{"$f":"F18*AVERAGE(K19:K26)","v":0},{"$f":"F18*AVERAGE(L19:L26)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"5/16\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(101,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Cembrit / Solid & Express / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D19*$F19*VLOOKUP($C19,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D19*$F19*VLOOKUP($C19,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"5/16\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(100,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Cembrit / Patina / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(384,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Equitone / Pictura and Natura Pro / 8 mm (5/16\")"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(385,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Equitone / Tectiva / 8 mm (5/16\")"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(386,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Equitone / Natura, Textura and Materia / 8 mm (5/16\")"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K23-L23","v":0},{"$f":"IF(H23=1,I23,\"\")","v":""},{"$f":"$D23*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D23*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(417,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / James Hardie / HardiePanel® / 8 mm"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(419,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / James Hardie / Hardie VL Plank / 11 mm"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K25-L25","v":0},{"$f":"IF(H25=1,I25,\"\")","v":""},{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(420,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / James Hardie / HardiePlank / 8 mm"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D26*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D26*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"VINYL SIDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(219,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl Siding / Vinyl Siding Institute / Double 4.5\" products from: American Original, Associated Materials, CertainTeed, Novik, Ply Gem / 0.040\" Double 4.5\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K28-L28","v":0},{"$f":"IF(H28=1,I28,\"\")","v":""},{"$f":"$D28*$F28*VLOOKUP($C28,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D28*$F28*VLOOKUP($C28,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"POLYPROPYLENE SIDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Polypropylene siding - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K30-L30","v":0},{"$f":"IF(H30=1,I30,\"\")","v":""},{"$f":"F30*AVERAGE(K31:K32)","v":0},{"$f":"F30*AVERAGE(L31:L32)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(169,'Master sheet'!$AL$1:$AL$441,0))","v":"Polypropylene siding / Novik / NovikStone, NovikShake / Avg of 5 products"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K31-L31","v":0},{"$f":"IF(H31=1,I31,\"\")","v":""},{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(170,'Master sheet'!$AL$1:$AL$441,0))","v":"Polypropylene siding / Vinyl Siding Institute  /  / 0.085\" Single 7\" wood Shake appearance"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K32-L32","v":0},{"$f":"IF(H32=1,I32,\"\")","v":""},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"STEEL PANEL SIDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Steel Panel Siding - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K34-L34","v":0},{"$f":"IF(H34=1,I34,\"\")","v":""},{"$f":"F34*AVERAGE(K35:K40)","v":0},{"$f":"F34*AVERAGE(L35:L40)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(140,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / AEP Span / All products / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(141,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / ArcelorMittal / All products / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(142,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Canadian Sheet Steel Building Institute / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D37*$F37*VLOOKUP($C37,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D37*$F37*VLOOKUP($C37,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(143,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Metal Building Manufacturers Assn / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D38*$F38*VLOOKUP($C38,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D38*$F38*VLOOKUP($C38,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(144,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Metal Construction Assn. / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(145,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Petersen Aluminum Corp / PAC-CLAD / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"ALUMINUM PANEL SIDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Aluminum Panel Siding - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K42-L42","v":0},{"$f":"IF(H42=1,I42,\"\")","v":""},{"$f":"F42*AVERAGE(K43:K44)","v":0},{"$f":"F42*AVERAGE(L43:L44)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(138,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Aluminum / Metal Construction Assn. / 22 gauge / Includes: ATAS, DMI, Englert, Fabral,McElroy, Pac-Clad"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K43-L43","v":0},{"$f":"IF(H43=1,I43,\"\")","v":""},{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(139,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Aluminum / Petersen Aluminum Corp / Pac-Clad / 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K44-L44","v":0},{"$f":"IF(H44=1,I44,\"\")","v":""},{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"PLASTER FINISHES",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(129,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime Plaster / Mapei / MapeWall Muratura / 3/4\" Natural Hydraulic Lime (NHL)"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K46-L46","v":0},{"$f":"IF(H46=1,I46,\"\")","v":""},{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(130,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime/Cork Plaster / Diasen / Diathonite Evolution / Exterior plaster cladding, 3/4\""},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K47-L47","v":0},{"$f":"IF(H47=1,I47,\"\")","v":""},{"$f":"$D47*$F47*VLOOKUP($C47,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D47*$F47*VLOOKUP($C47,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(42,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay plaster / Site mixed /  / 15 mm"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K48-L48","v":0},{"$f":"IF(H48=1,I48,\"\")","v":""},{"$f":"$D48*$F48*VLOOKUP($C48,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D48*$F48*VLOOKUP($C48,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2014"},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(212,'Master sheet'!$AL$1:$AL$441,0))","v":"Acrylic Stucco Textured Finish / Sto / Stolit 1.0, Stolit 1.5, Stolit Freeform / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K49-L49","v":0},{"$f":"IF(H49=1,I49,\"\")","v":""},{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,"ENGINEERED WOOD SIDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(413,'Master sheet'!$AL$1:$AL$441,0))","v":"Engineered Wood Siding & Trim / LP / SmartSide / 0.315\" (8 mm)"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K51-L51","v":0},{"$f":"IF(H51=1,I51,\"\")","v":""},{"$f":"$D51*$F51*VLOOKUP($C51,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D51*$F51*VLOOKUP($C51,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(414,'Master sheet'!$AL$1:$AL$441,0))","v":"Engineered Wood Siding & Trim / LP / SmartSide / 0.375\" (9.5 mm)"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K52-L52","v":0},{"$f":"IF(H52=1,I52,\"\")","v":""},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(415,'Master sheet'!$AL$1:$AL$441,0))","v":"Engineered Wood Siding & Trim / LP / SmartSide / 0.530\" (13.5 mm)"},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K53-L53","v":0},{"$f":"IF(H53=1,I53,\"\")","v":""},{"$f":"$D53*$F53*VLOOKUP($C53,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D53*$F53*VLOOKUP($C53,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","EXTERIOR CLADDING"]
["STRAPPING for RAIN SCREEN",null,null,"STRAPPING SPACING:",null,"in",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"1x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K55-L55","v":0},{"$f":"IF(H55=1,I55,\"\")","v":""},{"$f":"$D55*$F55*IF($E$54=16,1/0.406,1/0.61)*VLOOKUP($C55,'Master sheet'!$A:$AJ,13,FALSE)*(0.0889*0.01905)","v":0},{"$f":"$D55*$F55*IF($E$54=16,1/0.406,1/0.61)*VLOOKUP($C55,'Master sheet'!$A:$AJ,27,FALSE)*(0.0889*0.01905)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","STRAPPING for RAIN SCREEN"]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$31","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K56-L56","v":0},{"$f":"IF(H56=1,I56,\"\")","v":""},{"$f":"$D56*$F56*IF($E$54=16,1/0.406,1/0.61)*VLOOKUP($C56,'Master sheet'!$A:$AJ,13,FALSE)*(0.0889*0.0381)","v":0},{"$f":"$D56*$F56*IF($E$54=16,1/0.406,1/0.61)*VLOOKUP($C56,'Master sheet'!$A:$AJ,27,FALSE)*(0.0889*0.0381)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","STRAPPING for RAIN SCREEN"]
["INTERIOR CLADDING for EXTERIOR WALLS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"DRYWALL 1/2\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Drywall 1/2\" Typical - Interior Cladding for Exterior Walls - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K59-L59","v":0},{"$f":"IF(H59=1,I59,\"\")","v":""},{"$f":"F59*AVERAGE(K60:K64)","v":0},{"$f":"F59*AVERAGE(L60:L64)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(87,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / Easi-Lite / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K60-L60","v":0},{"$f":"IF(H60=1,I60,\"\")","v":""},{"$f":"$D60*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D60*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(86,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / AirRenew / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D61*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D61*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(88,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / M2Tech moisture resistant / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(89,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / Pabco / QuietRock / QuietRock 1/2\""},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K63-L63","v":0},{"$f":"IF(H63=1,I63,\"\")","v":""},{"$f":"$D63*$F63*VLOOKUP($C63,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D63*$F63*VLOOKUP($C63,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(376,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / National Gypsum / Gold Bond XP Gypsum Board  / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D64*$F64*VLOOKUP($C64,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D64*$F64*VLOOKUP($C64,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,"DRYWALL 5/8\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(90,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D66*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D66*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(91,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" / USG / EcoSmart Firecode / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D67*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D67*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(377,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" Type X / National Gypsum / Gold Bond XP Fire-Shield Gypsum Board  / 5/8'' type X"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K68-L68","v":0},{"$f":"IF(H68=1,I68,\"\")","v":""},{"$f":"$D68*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D68*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,"OTHER CLADDING MATERIALS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(146,'Master sheet'!$AL$1:$AL$441,0))","v":"MgO board 1/2\" / North American MgO / MagTech Ultra / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K70-L70","v":0},{"$f":"IF(H70=1,I70,\"\")","v":""},{"$f":"$D70*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D70*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K71-L71","v":0},"",{"$f":"$D71*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D71*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(31,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D72*$F72*VLOOKUP($C72,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D72*$F72*VLOOKUP($C72,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(17,'Master sheet'!$AL$1:$AL$441,0))","v":"Bamboo plywood / Smith & Fong / Plyboo / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D73*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D73*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D74*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D74*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(253,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood wool boards / Armstrong / Tectum / 2\" (50.8 mm)"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D75*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D75*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(129,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime Plaster / Mapei / MapeWall Muratura / 3/4\" Natural Hydraulic Lime (NHL)"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D76*$F76*VLOOKUP($C76,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D76*$F76*VLOOKUP($C76,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(130,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime/Cork Plaster / Diasen / Diathonite Evolution / Exterior plaster cladding, 3/4\""},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D77*$F77*VLOOKUP($C77,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D77*$F77*VLOOKUP($C77,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(42,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay plaster / Site mixed /  / 15 mm"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D78*$F78*VLOOKUP($C78,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D78*$F78*VLOOKUP($C78,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2014"},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(41,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Tile Council of North America /  / Industry average. Includes porcelain, pressed, mosaic and quarry tile"},{"$f":"'USER INPUT SHEET'!$C$31+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D79*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D79*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"EXTERIOR WALLS - CLADDING","INTERIOR CLADDING for EXTERIOR WALLS"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Windows","index":15,"n_rows":25,"n_cols":16,"rows_kept":25,"cut":false,"hidden":false,"merged":[[0,0,0,2],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,0,3,1],[2,2,3,2],[2,5,3,5],[2,6,3,6],[0,3,0,11],[2,7,3,7],[2,8,3,8],[2,9,3,9],[4,0,4,2],[11,0,11,2],[18,0,18,2],[2,10,3,10],[19,0,21,1]]}
["SECTION 8 ➜ COMPONENT MATERIALS FOR",null,null,"WINDOWS"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR WINDOWS"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["DOUBLE PANE WINDOWS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(222,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Fiberglass frame /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,{"$f":"K6-L6","v":0},{"$f":"IF(H6=1,I6,\"\")","v":""},{"$f":"$D6*$F6*VLOOKUP($C6,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D6*$F6*VLOOKUP($C6,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C6,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C6,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"WINDOWS","DOUBLE PANE WINDOWS - GENERIC"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(224,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Vinyl frame /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,0,"",{"$f":"$D7*$F7*VLOOKUP($C7,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D7*$F7*VLOOKUP($C7,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"WINDOWS","DOUBLE PANE WINDOWS - GENERIC"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(225,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame /  / EU"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,0,"",{"$f":"$D8*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D8*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"WINDOWS","DOUBLE PANE WINDOWS - GENERIC"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(226,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,0,"",{"$f":"$D9*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D9*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"WINDOWS","DOUBLE PANE WINDOWS - GENERIC"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(227,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame, aluminum cladding /  / EU"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,0,"",{"$f":"$D10*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D10*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"WINDOWS","DOUBLE PANE WINDOWS - GENERIC"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(228,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame, aluminum cladding /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,{"$f":"K11-L11","v":0},{"$f":"IF(H11=1,I11,\"\")","v":""},{"$f":"$D11*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D11*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"WINDOWS","DOUBLE PANE WINDOWS - GENERIC"]
["TRIPLE PANE WINDOWS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(229,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Fiberglass frame /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,{"$f":"K13-L13","v":0},{"$f":"IF(H13=1,I13,\"\")","v":""},{"$f":"$D13*$F13*VLOOKUP($C13,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D13*$F13*VLOOKUP($C13,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"WINDOWS","TRIPLE PANE WINDOWS - GENERIC"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(230,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Vinyl frame /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,0,"",{"$f":"$D14*$F14*VLOOKUP($C14,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D14*$F14*VLOOKUP($C14,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"WINDOWS","TRIPLE PANE WINDOWS - GENERIC"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(231,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Wood frame /  / EU"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,0,"",{"$f":"$D15*$F15*VLOOKUP($C15,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D15*$F15*VLOOKUP($C15,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"WINDOWS","TRIPLE PANE WINDOWS - GENERIC"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(232,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Wood frame /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,0,"",{"$f":"$D16*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D16*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"WINDOWS","TRIPLE PANE WINDOWS - GENERIC"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(233,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Wood frame, aluminum cladding /  / EU"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,0,"",{"$f":"$D17*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D17*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"WINDOWS","TRIPLE PANE WINDOWS - GENERIC"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(234,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Wood frame, aluminum cladding /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,0,"",{"$f":"$D18*$F18*VLOOKUP($C18,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D18*$F18*VLOOKUP($C18,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"WINDOWS","TRIPLE PANE WINDOWS - GENERIC"]
["WINDOWS - SPECIFIC MANUFACTURERS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(375,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Andersen / E-series (Average Double-hung/Awning/Picture) / Wood frame, aluminum cladding"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,{"$f":"K20-L20","v":0},{"$f":"IF(H20=1,I20,\"\")","v":""},{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"WINDOWS","WINDOWS - SPECIFIC MANUFACTURERS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(416,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Inline Fiberglass / 300 Series Tilt and Turn, 300 Series Fixed, 325 Series Awning/Casement, 325 Series Fixed, and 400 Series / Fiberglass frame"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,0,"",{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"WINDOWS","WINDOWS - SPECIFIC MANUFACTURERS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(223,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Andersen / Fibrex / PVC & Wood composite / USA"},{"$f":"'USER INPUT SHEET'!$C$32","v":0},{"$f":"'USER INPUT SHEET'!$E$32","v":"m2"},1,null,null,{"$f":"K22-L22","v":0},{"$f":"IF(H22=1,I22,\"\")","v":""},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"WINDOWS","WINDOWS - SPECIFIC MANUFACTURERS"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Int. Walls","index":16,"n_rows":93,"n_cols":16,"rows_kept":93,"cut":false,"hidden":false,"merged":[[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[0,0,0,2],[0,3,0,12],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,0,3,1],[2,2,3,2],[2,5,3,5],[2,6,3,6],[4,0,4,2],[5,1,5,2],[6,0,8,0],[9,0,9,2],[10,1,10,2],[29,1,29,2],[12,0,16,1],[17,0,17,2],[18,1,18,2],[20,0,24,1],[25,1,25,2],[26,0,28,1],[40,0,40,2],[41,1,41,2],[46,1,46,2],[48,0,51,1],[52,1,52,2],[53,0,59,1],[60,1,60,2],[62,0,64,1],[65,1,65,2],[67,0,70,1],[81,1,81,2],[84,1,84,2],[86,0,88,1],[71,1,71,2],[72,0,76,1],[77,1,77,2],[78,0,78,1],[80,0,80,1],[79,0,79,1]]}
["SECTION 9 ➜ COMPONENT MATERIALS FOR",null,null,"INTERIOR WALLS"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR INTERIOR WALLS"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["WOOD FRAME CONSTRUCTION",null,null,"FRAMING SPACING:",null,"in"]
[null,"WOOD FRAME CONSTRUCTION"]
[null,"2x3",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K7-L7","v":0},{"$f":"IF(H7=1,I7,\"\")","v":""},{"$f":"$D7*$F7*IF($E$5=16,0.25,0.22)*VLOOKUP($C7,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*2.5)","v":0},{"$f":"$D7*$F7*IF($E$5=16,0.25,0.22)*VLOOKUP($C7,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*2.5)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL FRAMING"]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K8-L8","v":0},{"$f":"IF(H8=1,I8,\"\")","v":""},{"$f":"$D8*$F8*IF($E$5=16,0.25,0.22)*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*3.5)","v":0},{"$f":"$D8*$F8*IF($E$5=16,0.25,0.22)*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*3.5)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL FRAMING"]
[null,"2x6",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K9-L9","v":0},{"$f":"IF(H9=1,I9,\"\")","v":""},{"$f":"$D9*$F9*IF($E$5=16,0.25,0.22)*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*5.5)","v":0},{"$f":"$D9*$F9*IF($E$5=16,0.25,0.22)*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*5.5)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL FRAMING"]
["STEEL FRAME CONSTRUCTION",null,null,"FRAMING SPACING:",null,"in",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"STEEL FRAMING, 2x4",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Steel Framing - Interior Walls - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K12-L12","v":0},{"$f":"IF(H12=1,I12,\"\")","v":""},{"$f":"F12*AVERAGE(K13:K17)","v":0},{"$f":"F12*AVERAGE(L13:L17)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL FRAMING"]
["Use % function to adjust for different gauges of steel studs.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(206,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / MarinoWARE / Viper Stud Viper 20 / 362-S-125-18, 20EQ gauge, \"2x4\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D13*$F13*IF($E$10=16,3.13,2.31)*VLOOKUP($C13,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D13*$F13*IF($E$10=16,3.13,2.31)*VLOOKUP($C13,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(209,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / Steel Recycling Institute /  / 362-S-125-18, 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D14*$F14*IF($E$10=16,3.13,2.31)*VLOOKUP($C14,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D14*$F14*IF($E$10=16,3.13,2.31)*VLOOKUP($C14,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(207,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / MBA Building Supplies /  / 362-S-125-18, 20EQ gauge, ProSTUD, ProTRAK"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D15*$F15*IF($E$10=16,3.13,2.31)*VLOOKUP($C15,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D15*$F15*IF($E$10=16,3.13,2.31)*VLOOKUP($C15,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(208,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / Scafco /  / 362VS125-18, 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D16*$F16*IF($E$10=16,3.13,2.31)*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D16*$F16*IF($E$10=16,3.13,2.31)*VLOOKUP($C16,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(205,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / ClarkDietrich /  / 362-S-125-18, 20EQ gauge, \"2x4\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D17*$F17*IF($E$10=16,3.13,2.31)*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D17*$F17*IF($E$10=16,3.13,2.31)*VLOOKUP($C17,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL FRAMING"]
["INTERIOR WALL CLADDING",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"DRYWALL 1/2\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Drywall 1/2\" Typical - Interior Walls - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K20-L20","v":0},{"$f":"IF(H20=1,I20,\"\")","v":""},{"$f":"F20*AVERAGE(K21:K25)","v":0},{"$f":"F20*AVERAGE(L21:L25)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(87,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / Easi-Lite / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K21-L21","v":0},{"$f":"IF(H21=1,I21,\"\")","v":""},{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(86,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / AirRenew / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(88,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / M2Tech moisture resistant / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D23*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D23*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(89,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / Pabco / QuietRock / QuietRock 1/2\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K24-L24","v":0},{"$f":"IF(H24=1,I24,\"\")","v":""},{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(376,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / National Gypsum / Gold Bond XP Gypsum Board  / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,"DRYWALL 5/8\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(90,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D27*$F27*VLOOKUP($C27,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D27*$F27*VLOOKUP($C27,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(91,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" / USG / EcoSmart Firecode / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D28*$F28*VLOOKUP($C28,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D28*$F28*VLOOKUP($C28,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(377,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" Type X / National Gypsum / Gold Bond XP Fire-Shield Gypsum Board  / 5/8'' type X"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K29-L29","v":0},{"$f":"IF(H29=1,I29,\"\")","v":""},{"$f":"$D29*$F29*VLOOKUP($C29,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D29*$F29*VLOOKUP($C29,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,"OTHER CLADDING MATERIALS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(146,'Master sheet'!$AL$1:$AL$441,0))","v":"MgO board 1/2\" / North American MgO / MagTech Ultra / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,{"$f":"K31-L31","v":0},{"$f":"IF(H31=1,I31,\"\")","v":""},{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,"3/4\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,13,FALSE)*0.01905*2","v":0},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,27,FALSE)*0.01905*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(31,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D33*$F33*VLOOKUP($C33,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(17,'Master sheet'!$AL$1:$AL$441,0))","v":"Bamboo plywood / Smith & Fong / Plyboo / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(253,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood wool boards / Armstrong / Tectum / 2\" (50.8 mm)"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(129,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime Plaster / Mapei / MapeWall Muratura / 3/4\" Natural Hydraulic Lime (NHL)"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D37*$F37*VLOOKUP($C37,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D37*$F37*VLOOKUP($C37,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(130,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime/Cork Plaster / Diasen / Diathonite Evolution / Exterior plaster cladding, 3/4\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D38*$F38*VLOOKUP($C38,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D38*$F38*VLOOKUP($C38,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(42,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay plaster / Site mixed /  / 15 mm"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2014"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(41,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Tile Council of North America /  / Industry average. Includes porcelain, pressed, mosaic and quarry tile"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$33","v":"m2"},1,null,null,0,"",{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,13,FALSE)*2","v":0},{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL CLADDING"]
["CAVITY INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"FIBERGLASS BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiberglass batt - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K43-L43","v":0},{"$f":"IF(H43=1,I43,\"\")","v":""},{"$f":"F43*AVERAGE(K44:K46)","v":0},{"$f":"F43*AVERAGE(L44:L46)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(104,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Owens Corning / EcoTouch Pink batt and roll / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K44-L44","v":0},"",{"$f":"$D44*($E$42/5.678)*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D44*($E$42/5.678)*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(102,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / CertainTeed / Sustainable Insulation / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D45*($E$42/5.678)*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D45*($E$42/5.678)*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(103,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Knauf / EcoBatt / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D46*($E$42/5.678)*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D46*($E$42/5.678)*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,"FIBERGLASS BLOWN-IN",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,"Fiberglass loose fill - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K48-L48","v":0},{"$f":"IF(H48=1,I48,\"\")","v":""},{"$f":"F48*AVERAGE(K49:K52)","v":0},{"$f":"F48*AVERAGE(L49:L52)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(107,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Owens Corning / AttiCat, ProCat, ProPink / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D49*($E$47/5.678)*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D49*($E$47/5.678)*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(105,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / CertainTeed / InsulSafe, Optima, TruComfort / R 2.6/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D50*($E$47/5.678)*$F50*VLOOKUP($C50,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D50*($E$47/5.678)*$F50*VLOOKUP($C50,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(106,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Knauf / Jet Stream ULTRA / R 2.2/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K51-L51","v":0},{"$f":"IF(H51=1,I51,\"\")","v":""},{"$f":"$D51*($E$47/5.678)*$F51*VLOOKUP($C51,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D51*($E$47/5.678)*$F51*VLOOKUP($C51,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(374,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Johns Manville / Climate Pro, Attic Protector, JM Spider PLUS (Canada) / R 2.8/inch, Formaldehyde-free"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D52*($E$47/5.678)*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D52*($E$47/5.678)*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,"MINERAL WOOL BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(147,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Owens Corning / Thermafiber UltraBatt / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D54*($E$53/5.678)*$F54*VLOOKUP($C54,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D54*($E$53/5.678)*$F54*VLOOKUP($C54,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(148,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / Safe'n'Sound, ComfortBatt / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K55-L55","v":0},{"$f":"IF(H55=1,I55,\"\")","v":""},{"$f":"$D55*($E$53/5.678)*$F55*VLOOKUP($C55,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D55*($E$53/5.678)*$F55*VLOOKUP($C55,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(402,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R14 / R 4.0/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D56*($E$53/5.678)*$F56*VLOOKUP($C56,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D56*($E$53/5.678)*$F56*VLOOKUP($C56,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(403,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R15 / R 4.3/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D57*($E$53/5.678)*$F57*VLOOKUP($C57,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D57*($E$53/5.678)*$F57*VLOOKUP($C57,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(404,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R22 / R 4.0/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D58*($E$53/5.678)*$F58*VLOOKUP($C58,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D58*($E$53/5.678)*$F58*VLOOKUP($C58,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(405,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 / R 4.4/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D59*($E$53/5.678)*$F59*VLOOKUP($C59,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D59*($E$53/5.678)*$F59*VLOOKUP($C59,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(406,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 SS / R 4.0/inch, 6\" Steel Studs"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D60*($E$53/5.678)*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D60*($E$53/5.678)*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,"CELLULOSE INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,"Cellulose - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K62-L62","v":0},{"$f":"IF(H62=1,I62,\"\")","v":""},{"$f":"F62*AVERAGE(K63:K65)","v":0},{"$f":"F62*AVERAGE(L63:L65)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(33,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - dense pack /  / R 3.7/inch / Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K63-L63","v":0},{"$f":"IF(H63=1,I63,\"\")","v":""},{"$f":"$D63*($E$61/5.678)*$F63*VLOOKUP($C63,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D63*($E$61/5.678)*$F63*VLOOKUP($C63,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(32,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - batt / CMS / R 3.6/inch / EcoCell"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D64*($E$61/5.678)*$F64*VLOOKUP($C64,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D64*($E$61/5.678)*$F64*VLOOKUP($C64,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(35,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - spray applied / R 3.75/inch / International Cellulose Corp. / K-13, ThermoCon"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D65*($E$61/5.678)*$F65*VLOOKUP($C65,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D65*($E$61/5.678)*$F65*VLOOKUP($C65,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,"WOOD FIBER BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,"Wood fiber batt - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K67-L67","v":0},{"$f":"IF(H67=1,I67,\"\")","v":""},{"$f":"F67*AVERAGE(K68:K71)","v":0},{"$f":"F67*AVERAGE(L68:L71)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(240,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Pavatex / Pavaflex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D68*($E$66/5.678)*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D68*($E$66/5.678)*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(239,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / GUTEX / ThermoFlex / R 4/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D69*($E$66/5.678)*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D69*($E$66/5.678)*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(241,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Steico / SteicoFlex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D70*($E$66/5.678)*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D70*($E$66/5.678)*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(238,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber - loose fill / GUTEX / ThermoFiber / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D71*($E$66/5.678)*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D71*($E$66/5.678)*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,"OTHER NATURAL FIBER INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(254,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool batt / Havelock Wool /  / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K73-L73","v":0},{"$f":"IF(H73=1,I73,\"\")","v":""},{"$f":"$D73*($E$72/5.678)*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D73*($E$72/5.678)*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(255,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool loose fill / Havelock Wool /  / R 4.4/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K74-L74","v":0},{"$f":"IF(H74=1,I74,\"\")","v":""},{"$f":"$D74*($E$72/5.678)*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D74*($E$72/5.678)*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(121,'Master sheet'!$AL$1:$AL$441,0))","v":"Hemp fiber batt / NaturFibre / Hemp Wool / R 3.7/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K75-L75","v":0},{"$f":"IF(H75=1,I75,\"\")","v":""},{"$f":"$D75*($E$72/5.678)*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D75*($E$72/5.678)*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(210,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale /  / Wheat & rye straw / R 3.3/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K76-L76","v":0},{"$f":"IF(H76=1,I76,\"\")","v":""},{"$f":"$D76*($E$72/5.678)*$F76*VLOOKUP($C76,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D76*($E$72/5.678)*$F76*VLOOKUP($C76,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(412,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale / SNaB (UK) / Wheat & barley straw / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K77-L77","v":0},{"$f":"IF(H77=1,I77,\"\")","v":""},{"$f":"$D77*($E$72/5.678)*$F77*VLOOKUP($C77,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D77*($E$72/5.678)*$F77*VLOOKUP($C77,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,"SPRAY FOAM, CLOSED CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(183,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K79-L79","v":0},{"$f":"IF(H79=1,I79,\"\")","v":""},{"$f":"$D79*($E$78/5.678)*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D79*($E$78/5.678)*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(184,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K80-L80","v":0},{"$f":"IF(H80=1,I80,\"\")","v":""},{"$f":"$D80*($E$78/5.678)*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D80*($E$78/5.678)*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(410,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / "},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K81-L81","v":0},{"$f":"IF(H81=1,I81,\"\")","v":""},{"$f":"$D81*($E$78/5.678)*$F81*VLOOKUP($C81,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D81*($E$78/5.678)*$F81*VLOOKUP($C81,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,"SPRAY FOAM, OPEN CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(187,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell (HFC) / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K83-L83","v":0},{"$f":"IF(H83=1,I83,\"\")","v":""},{"$f":"$D83*($E$82/5.678)*$F83*VLOOKUP($C83,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D83*($E$82/5.678)*$F83*VLOOKUP($C83,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(188,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell - HFO gas / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K84-L84","v":0},{"$f":"IF(H84=1,I84,\"\")","v":""},{"$f":"$D84*($E$82/5.678)*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D84*($E$82/5.678)*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,"HEMPCRETE",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,"Hempcrete - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K86-L86","v":0},{"$f":"IF(H86=1,I86,\"\")","v":""},{"$f":"F86*AVERAGE(K87:K89)","v":0},{"$f":"F86*AVERAGE(L87:L89)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(124,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / USA / R 2.1/inch, Avg. mix using NHL & PHL"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D87*($E$85/5.678)*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D87*($E$85/5.678)*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2020"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(123,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / Europe / R 2.1/inch, Avg. of 9 mixes"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D88*($E$85/5.678)*$F88*VLOOKUP($C88,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D88*($E$85/5.678)*$F88*VLOOKUP($C88,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2017"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(122,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / IsoHemp / Europe / R 2.1/inch"},{"$f":"'USER INPUT SHEET'!$C$33","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D89*($E$85/5.678)*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D89*($E$85/5.678)*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA"},null,"INTERIOR WALLS - STRUCTURE & CLADDING","INTERIOR WALL INSULATION"]
[]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Floors","index":17,"n_rows":130,"n_cols":16,"rows_kept":130,"cut":false,"hidden":false,"merged":[[62,1,62,2],[2,10,3,10],[0,0,0,2],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,8,3,8],[2,5,3,5],[2,6,3,6],[0,3,0,11],[2,9,3,9],[2,7,3,7],[2,0,3,1],[2,2,3,2],[4,0,4,2],[18,0,18,2],[35,1,35,2],[25,0,25,2],[26,1,26,2],[28,0,30,1],[34,0,34,2],[31,0,31,2],[5,1,5,2],[9,1,9,2],[37,0,39,1],[32,1,32,2],[75,0,75,2],[40,1,40,2],[42,0,46,1],[47,1,47,2],[49,0,53,1],[54,1,54,2],[56,0,61,1],[13,1,13,2],[67,1,67,2],[68,0,70,1],[15,0,15,2],[16,1,16,2],[76,1,76,2],[78,0,80,1],[81,1,81,2],[63,0,63,1],[64,1,64,2],[71,1,71,2],[72,0,74,1],[65,0,66,1],[83,0,86,1],[111,1,111,2],[116,1,116,2],[123,1,123,2],[87,1,87,2],[89,0,95,1],[96,1,96,2],[97,0,97,1],[105,1,105,2],[99,0,99,1],[101,0,101,1],[102,1,102,2],[98,1,98,2],[100,0,100,1]]}
["SECTION 10 ➜ COMPONENT MATERIALS FOR",null,null,"FLOORS"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR FLOORS"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["WOOD FLOOR FRAMING",null,null,"FRAMING SPACING:",null,"in"]
[null,"WOOD LUMBER FRAMING"]
[null,"2X8",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K7-L7","v":0},{"$f":"IF(H7=1,I7,\"\")","v":""},{"$f":"$D7*$F7*IF($E$5=16,0.25,0.22)*VLOOKUP($C7,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*7.25)","v":0},{"$f":"$D7*$F7*IF($E$5=16,0.25,0.22)*VLOOKUP($C7,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*7.25)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","WOOD FLOOR FRAMING"]
[null,"2X10",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K8-L8","v":0},{"$f":"IF(H8=1,I8,\"\")","v":""},{"$f":"$D8*$F8*IF($E$5=16,0.25,0.22)*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*9.25)","v":0},{"$f":"$D8*$F8*IF($E$5=16,0.25,0.22)*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*9.25)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","WOOD FLOOR FRAMING"]
[null,"2X12",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K9-L9","v":0},{"$f":"IF(H9=1,I9,\"\")","v":""},{"$f":"$D9*$F9*IF($E$5=16,0.25,0.22)*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*11.25)","v":0},{"$f":"$D9*$F9*IF($E$5=16,0.25,0.22)*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*11.25)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","WOOD FLOOR FRAMING"]
[null,"WOOD I-JOIST FRAMING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"9-1/2\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K11-L11","v":0},{"$f":"IF(H11=1,I11,\"\")","v":""},{"$f":"$D11*$F11*IF($E$5=16,2.463,1.639)*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)*0.926","v":0},{"$f":"$D11*$F11*IF($E$5=16,2.463,1.639)*VLOOKUP($C11,'Master sheet'!$A:$AJ,27,FALSE)*0.926","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","WOOD FLOOR FRAMING"]
[null,"11-7/8\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K12-L12","v":0},{"$f":"IF(H12=1,I12,\"\")","v":""},{"$f":"$D12*$F12*IF($E$5=16,2.463,1.639)*VLOOKUP($C12,'Master sheet'!$A:$AJ,13,FALSE)*1.029","v":0},{"$f":"$D12*$F12*IF($E$5=16,2.463,1.639)*VLOOKUP($C12,'Master sheet'!$A:$AJ,27,FALSE)*1.029","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","WOOD FLOOR FRAMING"]
[null,"14\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K13-L13","v":0},{"$f":"IF(H13=1,I13,\"\")","v":""},{"$f":"$D13*$F13*IF($E$5=16,2.463,1.639)*VLOOKUP($C13,'Master sheet'!$A:$AJ,13,FALSE)*1.132","v":0},{"$f":"$D13*$F13*IF($E$5=16,2.463,1.639)*VLOOKUP($C13,'Master sheet'!$A:$AJ,27,FALSE)*1.132","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","WOOD FLOOR FRAMING"]
[null,"WOOD TRUSS FRAMING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(251,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood floor truss - prefabricated / Quebec Wood Export Bureau / Common (Warren, 45 deg) web pattern / Top chord bearing, variable depth"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K15-L15","v":0},{"$f":"IF(H15=1,I15,\"\")","v":""},{"$f":"$D15*$F15*IF($E$5=16,2.463,1.639)*VLOOKUP($C15,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D15*$F15*IF($E$5=16,2.463,1.639)*VLOOKUP($C15,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FLOORS - STRUCTURE & FLOORING","WOOD FLOOR FRAMING"]
["STEEL FLOOR FRAMING",null,null,"FRAMING SPACING:",null,"in",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"OPEN WEB STEEL JOIST",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(198,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel joist, open web / Steel Joist Institute /  / 12\" 12K3 joist"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K18-L18","v":0},{"$f":"IF(H18=1,I18,\"\")","v":""},{"$f":"$D18*$F18*IF($E$16=24,1.639,1.094)*VLOOKUP($C18,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D18*$F18*IF($E$16=24,1.639,1.094)*VLOOKUP($C18,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FLOORS - STRUCTURE & FLOORING","STEEL FLOOR FRAMING"]
["SUBFLOORING",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"5/8\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(155,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K20-L20","v":0},{"$f":"IF(H20=1,I20,\"\")","v":""},{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","SUBFLOORING"]
[null,"19/32\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(158,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB subflooring / Huber  / AdvanTech / 19/32\" Subflooring"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","SUBFLOORING"]
[null,"1/2\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","SUBFLOORING"]
[null,"5/8\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(160,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D23*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D23*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","SUBFLOORING"]
[null,"3/4\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(161,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 3/4\""},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","SUBFLOORING"]
[null,"5/8\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*5/8)","v":0},{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*5/8)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","SUBFLOORING"]
["CROSS-LAMINATED TIMBER",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CLT FLOOR SYSTEM",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"CLT Floor System – 3-1/2\" (90 mm) AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K28-L28","v":0},{"$f":"IF(H28=1,I28,\"\")","v":""},{"$f":"$F28*AVERAGE(K29:K31)","v":0},{"$f":"$F28*AVERAGE(L29:L31)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","CLT FLOOR SYSTEM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(83,'Master sheet'!$AL$1:$AL$441,0))","v":"Cross Laminated Timber / Nordic / X-Lam / 3-1/2\" (90mm) thick"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K29-L29","v":0},{"$f":"IF(H29=1,I29,\"\")","v":""},{"$f":"$D29*$F29*VLOOKUP($C29,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D29*$F29*VLOOKUP($C29,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","CLT FLOOR SYSTEM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(84,'Master sheet'!$AL$1:$AL$441,0))","v":"Cross Laminated Timber / Structurlam / CrossLam / 3-1/2\" (90mm) thick"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K30-L30","v":0},{"$f":"IF(H30=1,I30,\"\")","v":""},{"$f":"$D30*$F30*VLOOKUP($C30,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D30*$F30*VLOOKUP($C30,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","CLT FLOOR SYSTEM"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(85,'Master sheet'!$AL$1:$AL$441,0))","v":"Dowel Laminated Timber / StructureCraft / DowelLam / 3-1/2\" (90mm) thick"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K31-L31","v":0},{"$f":"IF(H31=1,I31,\"\")","v":""},{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","CLT FLOOR SYSTEM"]
["CLAY-BASED FLOOR SYSTEM",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"EARTHEN FLOOR",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(52,'Master sheet'!$AL$1:$AL$441,0))","v":"Earthen Floor / Site made /  / 3\" cob, 1\" clay plaster"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},"m2",1,null,null,{"$f":"K34-L34","v":0},{"$f":"IF(H34=1,I34,\"\")","v":""},{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D34*$F34*VLOOKUP($C34,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Adapted from peer-reviewed LCA, 2019"},null,"FLOORS - STRUCTURE & FLOORING","EARTHEN FLOOR"]
["FINISHED FLOORING",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"HARDWOOD 3/4\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Hardwood flooring - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K37-L37","v":0},{"$f":"IF(H37=1,I37,\"\")","v":""},{"$f":"$F37*AVERAGE(K38:K40)","v":0},{"$f":"$F37*AVERAGE(L38:L40)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(118,'Master sheet'!$AL$1:$AL$441,0))","v":"Hardwood flooring / mafi / Natural Hardwood Planks / 3/4\", 3 ply laminated solid, oil pre-finished"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K38-L38","v":0},{"$f":"IF(H38=1,I38,\"\")","v":""},{"$f":"$D38*$F38*VLOOKUP($C38,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D38*$F38*VLOOKUP($C38,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(119,'Master sheet'!$AL$1:$AL$441,0))","v":"Hardwood flooring / Typical Eastern Canadian, solid, pre-finished /  / 3-12\" x 3/4\" prefinished"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(117,'Master sheet'!$AL$1:$AL$441,0))","v":"Hardwood flooring / Action Floor Systems /  / 25/32\" x 3-1/4\" FSC certified"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,"LINOLEUM FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Linoleum flooring - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K42-L42","v":0},{"$f":"IF(H42=1,I42,\"\")","v":""},{"$f":"$F42*AVERAGE(K43:K45)","v":0},{"$f":"$F42*AVERAGE(L43:L45)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(132,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Forbo / Marmoleum / 2.5 mm sheet style linoleum"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(373,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Gerflor  / DLW Linoleum Compact / 2.5 mm sheet style linoleum"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(133,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Forbo / Marmoleum Striato / 2.5 mm sheet style linoleum"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(134,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Gerflor  / DLW Linoleum Acousticplus / 4.0 mm sheet style linoleum"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K46-L46","v":0},{"$f":"IF(H46=1,I46,\"\")","v":""},{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(381,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Mannington / Legato Flooring / liquid applied"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D47*$F47*VLOOKUP($C47,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D47*$F47*VLOOKUP($C47,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,"TILE FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Ceramic tile flooring - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K49-L49","v":0},{"$f":"IF(H49=1,I49,\"\")","v":""},{"$f":"$F49*AVERAGE(K50:K54)","v":0},{"$f":"$F49*AVERAGE(L50:L54)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(41,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Tile Council of North America /  / Industry average. Includes porcelain, pressed, mosaic and quarry tile"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D50*$F50*VLOOKUP($C50,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D50*$F50*VLOOKUP($C50,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(40,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / StonePeak / Porcelain / Porcelain, standard grade"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D51*$F51*VLOOKUP($C51,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D51*$F51*VLOOKUP($C51,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(39,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Crossville / Porcelain / Standard grade"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K52-L52","v":0},{"$f":"IF(H52=1,I52,\"\")","v":""},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(382,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Fireclay Tile / Ceramic - recycled content / Standard and Second grade"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D53*$F53*VLOOKUP($C53,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D53*$F53*VLOOKUP($C53,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(383,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / American Wonder Porcelain / Procelain - recycled content / Standard and Second grade"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D54*$F54*VLOOKUP($C54,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D54*$F54*VLOOKUP($C54,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,"VINYL FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Vinyl flooring - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K56-L56","v":0},{"$f":"IF(H56=1,I56,\"\")","v":""},{"$f":"$F56*AVERAGE(K57:K62)","v":0},{"$f":"$F56*AVERAGE(L57:L62)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(218,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Resilient Floor Covering Institute / Includes tile products from Armstrong, Congoleum, Tarkett / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D57*$F57*VLOOKUP($C57,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D57*$F57*VLOOKUP($C57,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(217,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Gerflor / Creation 70 CLIC / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D58*$F58*VLOOKUP($C58,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D58*$F58*VLOOKUP($C58,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(216,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Altro / Altro Lavencia Plus / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D59*$F59*VLOOKUP($C59,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D59*$F59*VLOOKUP($C59,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(215,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Altro / Altro Lavencia Click / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K60-L60","v":0},{"$f":"IF(H60=1,I60,\"\")","v":""},{"$f":"$D60*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D60*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(372,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Shaw - Patcraft / Luxury Vinyl Tile / 2 - 5 mm "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D61*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D61*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(379,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Mannington / Luxury Vinyl Tile / 2.5 mm Tile and Plank"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,"LAMINATE FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(125,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminate flooring / Novalis / LVT / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K64-L64","v":0},{"$f":"IF(H64=1,I64,\"\")","v":""},{"$f":"$D64*$F64*VLOOKUP($C64,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D64*$F64*VLOOKUP($C64,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,"CORK FLOORING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(82,'Master sheet'!$AL$1:$AL$441,0))","v":"Cork flooring / European Resilient Flooring Manufacturers' Institute / Includes: Altro, Amorim, Amtico, Artigo, Aspecta, BeauFlor, Dickson, Mflor, Forbo, Gerflor, IVC, Nora, Polyflor, Tarkett, Kahrs, Windmoller / Cork floor tiles"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K66-L66","v":0},{"$f":"IF(H66=1,I66,\"\")","v":""},{"$f":"$D66*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D66*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(81,'Master sheet'!$AL$1:$AL$441,0))","v":"Cork flooring / Amorim / Revestimentos S.A. / Cork floating floor planks"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K67-L67","v":0},{"$f":"IF(H67=1,I67,\"\")","v":""},{"$f":"$D67*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D67*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,"CARPET",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(25,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet /  /  / Average from 150 samples in the EC3 database"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K69-L69","v":0},{"$f":"IF(H69=1,I69,\"\")","v":""},{"$f":"$D69*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D69*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Multi-EPD average from EC3 Tool"},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(29,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet / Interface / Cquest BioX / 1.5 mm Modular tile carpet"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K70-L70","v":0},{"$f":"IF(H70=1,I70,\"\")","v":""},{"$f":"$D70*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D70*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(378,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet / J+J Flooring / Standard Back / all Broadloom styles"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K71-L71","v":0},{"$f":"IF(H71=1,I71,\"\")","v":""},{"$f":"$D71*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D71*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,"OTHER FLOORING OPTIONS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(18,'Master sheet'!$AL$1:$AL$441,0))","v":"BioBased Tile / Armstrong / BioBased Tile / Non-PVC with BioStride polyester binder, Striations BBT and Migrations BBT"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K73-L73","v":0},{"$f":"IF(H73=1,I73,\"\")","v":""},{"$f":"$D73*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D73*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(179,'Master sheet'!$AL$1:$AL$441,0))","v":"Rubber flooring / Resilient Floor Covering Institute / Includes tiles and rolls from American Biltrite, Armstrong, Burke, FLEXCO, Johnsonite, Mannington, Roppe, Tarkett / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K74-L74","v":0},{"$f":"IF(H74=1,I74,\"\")","v":""},{"$f":"$D74*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D74*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(42,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay plaster / Site mixed /  / 15 mm"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K75-L75","v":0},{"$f":"IF(H75=1,I75,\"\")","v":""},{"$f":"$D75*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D75*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2014"},null,"FLOORS - STRUCTURE & FLOORING","FINISHED FLOORING"]
["FLOOR CAVITY INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"FIBERGLASS BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiberglass batt - Floor Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K78-L78","v":0},{"$f":"IF(H78=1,I78,\"\")","v":""},{"$f":"F78*AVERAGE(K79:K81)","v":0},{"$f":"F78*AVERAGE(L79:L81)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(104,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Owens Corning / EcoTouch Pink batt and roll / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K79-L79","v":0},{"$f":"IF(H79=1,I79,\"\")","v":""},{"$f":"$D79*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,13,FALSE)*($E$77/5.678)","v":0},{"$f":"$D79*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,27,FALSE)*($E$77/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(102,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / CertainTeed / Sustainable Insulation / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D80*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,13,FALSE)*($E$77/5.678)","v":0},{"$f":"$D80*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,27,FALSE)*($E$77/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(103,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Knauf / EcoBatt / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K81-L81","v":0},{"$f":"IF(H81=1,I81,\"\")","v":""},{"$f":"$D81*$F81*VLOOKUP($C81,'Master sheet'!$A:$AJ,13,FALSE)*($E$77/5.678)","v":0},{"$f":"$D81*$F81*VLOOKUP($C81,'Master sheet'!$A:$AJ,27,FALSE)*($E$77/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,"FIBERGLASS LOOSE FILL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiberglass loose fill - Floor Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K83-L83","v":0},{"$f":"IF(H83=1,I83,\"\")","v":""},{"$f":"F83*AVERAGE(K84:K87)","v":0},{"$f":"F83*AVERAGE(L84:L87)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(107,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Owens Corning / AttiCat, ProCat, ProPink / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D84*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,13,FALSE)*($E$82/5.678)","v":0},{"$f":"$D84*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,27,FALSE)*($E$82/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(105,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / CertainTeed / InsulSafe, Optima, TruComfort / R 2.6/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D85*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,13,FALSE)*($E$82/5.678)","v":0},{"$f":"$D85*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,27,FALSE)*($E$82/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(106,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Knauf / Jet Stream ULTRA / R 2.2/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D86*$F86*VLOOKUP($C86,'Master sheet'!$A:$AJ,13,FALSE)*($E$82/5.678)","v":0},{"$f":"$D86*$F86*VLOOKUP($C86,'Master sheet'!$A:$AJ,27,FALSE)*($E$82/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(374,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Johns Manville / Climate Pro, Attic Protector, JM Spider PLUS (Canada) / R 2.8/inch, Formaldehyde-free"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K87-L87","v":0},{"$f":"IF(H87=1,I87,\"\")","v":""},{"$f":"$D87*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,13,FALSE)*($E$82/5.678)","v":0},{"$f":"$D87*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,27,FALSE)*($E$82/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,"MINERAL WOOL BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FLOOR CAVITY INSULATION"]
[null,null,"Mineral wool batt - Floor Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K89-L89","v":0},{"$f":"IF(H89=1,I89,\"\")","v":""},{"$f":"F89*AVERAGE(K90:K96)","v":0},{"$f":"F89*AVERAGE(L90:L96)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(147,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Owens Corning / Thermafiber UltraBatt / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D90*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,13,FALSE)*($E$88/5.678)","v":0},{"$f":"$D90*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,27,FALSE)*($E$88/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(148,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / Safe'n'Sound, ComfortBatt / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K91-L91","v":0},{"$f":"IF(H91=1,I91,\"\")","v":""},{"$f":"$D91*$F91*VLOOKUP($C91,'Master sheet'!$A:$AJ,13,FALSE)*($E$88/5.678)","v":0},{"$f":"$D91*$F91*VLOOKUP($C91,'Master sheet'!$A:$AJ,27,FALSE)*($E$88/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(402,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R14 / R 4.0/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D92*$F92*VLOOKUP($C92,'Master sheet'!$A:$AJ,13,FALSE)*($E$88/5.678)","v":0},{"$f":"$D92*$F92*VLOOKUP($C92,'Master sheet'!$A:$AJ,27,FALSE)*($E$88/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(403,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R15 / R 4.3/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D93*$F93*VLOOKUP($C93,'Master sheet'!$A:$AJ,13,FALSE)*($E$88/5.678)","v":0},{"$f":"$D93*$F93*VLOOKUP($C93,'Master sheet'!$A:$AJ,27,FALSE)*($E$88/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(404,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R22 / R 4.0/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D94*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,13,FALSE)*($E$88/5.678)","v":0},{"$f":"$D94*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,27,FALSE)*($E$88/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(405,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 / R 4.4/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D95*$F95*VLOOKUP($C95,'Master sheet'!$A:$AJ,13,FALSE)*($E$88/5.678)","v":0},{"$f":"$D95*$F95*VLOOKUP($C95,'Master sheet'!$A:$AJ,27,FALSE)*($E$88/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(406,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 SS / R 4.0/inch, 6\" Steel Studs"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D96*$F96*VLOOKUP($C96,'Master sheet'!$A:$AJ,13,FALSE)*($E$88/5.678)","v":0},{"$f":"$D96*$F96*VLOOKUP($C96,'Master sheet'!$A:$AJ,27,FALSE)*($E$88/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,"MINERAL WOOL LOOSE FILL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(152,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool loose fill / NAIMA / R 3/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K98-L98","v":0},{"$f":"IF(H98=1,I98,\"\")","v":""},{"$f":"$D98*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,13,FALSE)*($E$97/5.678)","v":0},{"$f":"$D98*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,27,FALSE)*($E$97/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,"SPRAY FOAM, CLOSED CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(183,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K100-L100","v":0},{"$f":"IF(H100=1,I100,\"\")","v":""},{"$f":"$D100*($E$99/5.678)*$F100*VLOOKUP($C100,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D100*($E$99/5.678)*$F100*VLOOKUP($C100,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(184,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K101-L101","v":0},{"$f":"IF(H101=1,I101,\"\")","v":""},{"$f":"$D101*($E$99/5.678)*$F101*VLOOKUP($C101,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D101*($E$99/5.678)*$F101*VLOOKUP($C101,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(410,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / "},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K102-L102","v":0},{"$f":"IF(H102=1,I102,\"\")","v":""},{"$f":"$D102*($E$99/5.678)*$F102*VLOOKUP($C102,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D102*($E$99/5.678)*$F102*VLOOKUP($C102,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,"SPRAY FOAM, OPEN CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(187,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell (HFC) / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K104-L104","v":0},{"$f":"IF(H104=1,I104,\"\")","v":""},{"$f":"$D104*($E$103/5.678)*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D104*($E$103/5.678)*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(188,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell - HFO gas / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K105-L105","v":0},{"$f":"IF(H105=1,I105,\"\")","v":""},{"$f":"$D105*($E$103/5.678)*$F105*VLOOKUP($C105,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D105*($E$103/5.678)*$F105*VLOOKUP($C105,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,"CELLULOSE INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FLOOR CAVITY INSULATION"]
[null,null,"Cellulose - Floor Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K107-L107","v":0},{"$f":"IF(H107=1,I107,\"\")","v":""},{"$f":"F107*AVERAGE(K108:K111)","v":0},{"$f":"F107*AVERAGE(L108:L111)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(32,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - batt / CMS / R 3.6/inch / EcoCell"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K108-L108","v":0},{"$f":"IF(H108=1,I108,\"\")","v":""},{"$f":"$D108*$F108*VLOOKUP($C108,'Master sheet'!$A:$AJ,13,FALSE)*($E$106/5.678)","v":0},{"$f":"$D108*$F108*VLOOKUP($C108,'Master sheet'!$A:$AJ,27,FALSE)*($E$106/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(33,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - dense pack /  / R 3.7/inch / Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D109*$F109*VLOOKUP($C109,'Master sheet'!$A:$AJ,13,FALSE)*($E$106/5.678)","v":0},{"$f":"$D109*$F109*VLOOKUP($C109,'Master sheet'!$A:$AJ,27,FALSE)*($E$106/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(34,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - loose fill /  / R 3.7/inch / Includes: AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D110*$F110*VLOOKUP($C110,'Master sheet'!$A:$AJ,13,FALSE)*($E$106/5.678)","v":0},{"$f":"$D110*$F110*VLOOKUP($C110,'Master sheet'!$A:$AJ,27,FALSE)*($E$106/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(35,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - spray applied / R 3.75/inch / International Cellulose Corp. / K-13, ThermoCon"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K111-L111","v":0},{"$f":"IF(H111=1,I111,\"\")","v":""},{"$f":"$D111*$F111*VLOOKUP($C111,'Master sheet'!$A:$AJ,13,FALSE)*($E$106/5.678)","v":0},{"$f":"$D111*$F111*VLOOKUP($C111,'Master sheet'!$A:$AJ,27,FALSE)*($E$106/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,"WOOD FIBER BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FLOOR CAVITY INSULATION"]
[null,null,"Wood fiber batt - Floor Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K113-L113","v":0},{"$f":"IF(H113=1,I113,\"\")","v":""},{"$f":"F113*AVERAGE(K114:K116)","v":0},{"$f":"F113*AVERAGE(L114:L116)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(239,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / GUTEX / ThermoFlex / R 4/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D114*$F114*VLOOKUP($C114,'Master sheet'!$A:$AJ,13,FALSE)*($E$112/5.678)","v":0},{"$f":"$D114*$F114*VLOOKUP($C114,'Master sheet'!$A:$AJ,27,FALSE)*($E$112/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(241,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Steico / SteicoFlex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D115*$F115*VLOOKUP($C115,'Master sheet'!$A:$AJ,13,FALSE)*($E$112/5.678)","v":0},{"$f":"$D115*$F115*VLOOKUP($C115,'Master sheet'!$A:$AJ,27,FALSE)*($E$112/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(240,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Pavatex / Pavaflex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D116*$F116*VLOOKUP($C116,'Master sheet'!$A:$AJ,13,FALSE)*($E$112/5.678)","v":0},{"$f":"$D116*$F116*VLOOKUP($C116,'Master sheet'!$A:$AJ,27,FALSE)*($E$112/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,"OTHER NATURAL FIBER INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(254,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool batt / Havelock Wool /  / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K118-L118","v":0},{"$f":"IF(H118=1,I118,\"\")","v":""},{"$f":"$D118*$F118*VLOOKUP($C118,'Master sheet'!$A:$AJ,13,FALSE)*($E$117/5.678)","v":0},{"$f":"$D118*$F118*VLOOKUP($C118,'Master sheet'!$A:$AJ,27,FALSE)*($E$117/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(255,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool loose fill / Havelock Wool /  / R 4.4/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D119*$F119*VLOOKUP($C119,'Master sheet'!$A:$AJ,13,FALSE)*($E$117/5.678)","v":0},{"$f":"$D119*$F119*VLOOKUP($C119,'Master sheet'!$A:$AJ,27,FALSE)*($E$117/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(121,'Master sheet'!$AL$1:$AL$441,0))","v":"Hemp fiber batt / NaturFibre / Hemp Wool / R 3.7/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D120*$F120*VLOOKUP($C120,'Master sheet'!$A:$AJ,13,FALSE)*($E$117/5.678)","v":0},{"$f":"$D120*$F120*VLOOKUP($C120,'Master sheet'!$A:$AJ,27,FALSE)*($E$117/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA"},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(238,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber - loose fill / GUTEX / ThermoFiber / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D121*$F121*VLOOKUP($C121,'Master sheet'!$A:$AJ,13,FALSE)*($E$117/5.678)","v":0},{"$f":"$D121*$F121*VLOOKUP($C121,'Master sheet'!$A:$AJ,27,FALSE)*($E$117/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(210,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale /  / Wheat & rye straw / R 3.3/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K122-L122","v":0},{"$f":"IF(H122=1,I122,\"\")","v":""},{"$f":"$D122*$F122*VLOOKUP($C122,'Master sheet'!$A:$AJ,13,FALSE)*($E$117/5.678)","v":0},{"$f":"$D122*$F122*VLOOKUP($C122,'Master sheet'!$A:$AJ,27,FALSE)*($E$117/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(412,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale / SNaB (UK) / Wheat & barley straw / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D123*$F123*VLOOKUP($C123,'Master sheet'!$A:$AJ,13,FALSE)*($E$117/5.678)","v":0},{"$f":"$D123*$F123*VLOOKUP($C123,'Master sheet'!$A:$AJ,27,FALSE)*($E$117/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"FLOORS","FLOOR CAVITY INSULATION"]
[null,"HEMPCRETE LOOSE FILL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"FLOOR CAVITY INSULATION"]
[null,null,"Hempcrete - Floor Insulation - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,{"$f":"K125-L125","v":0},{"$f":"IF(H125=1,I125,\"\")","v":""},{"$f":"F125*AVERAGE(K126:K127)","v":0},{"$f":"F125*AVERAGE(L126:L127)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(124,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / USA / R 2.1/inch, Avg. mix using NHL & PHL"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D126*$F126*VLOOKUP($C126,'Master sheet'!$A:$AJ,13,FALSE)*($E$124/5.678)","v":0},{"$f":"$D126*$F126*VLOOKUP($C126,'Master sheet'!$A:$AJ,27,FALSE)*($E$124/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2020"},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(123,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / Europe / R 2.1/inch, Avg. of 9 mixes"},{"$f":"'USER INPUT SHEET'!$C$34","v":0},{"$f":"'USER INPUT SHEET'!$E$34","v":"m2"},1,null,null,0,"",{"$f":"$D127*$F127*VLOOKUP($C127,'Master sheet'!$A:$AJ,13,FALSE)*($E$124/5.678)","v":0},{"$f":"$D127*$F127*VLOOKUP($C127,'Master sheet'!$A:$AJ,27,FALSE)*($E$124/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2017"},null,{"$f":"D$1","v":"FLOORS"},"FLOOR CAVITY INSULATION"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Ceilings","index":18,"n_rows":27,"n_cols":16,"rows_kept":27,"cut":false,"hidden":false,"merged":[[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[0,0,0,2],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,0,3,1],[2,2,3,2],[2,5,3,5],[2,6,3,6],[0,3,0,11],[17,1,17,2],[18,1,19,1],[21,1,23,1],[4,0,4,2],[5,1,5,2],[7,0,11,1],[12,1,12,2],[14,0,16,1]]}
["SECTION 11 ➜ COMPONENT MATERIALS FOR",null,null,"CEILINGS"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR CEILINGS"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0},null,"SECTION","CATEGORY"]
["CEILING FINISHES"]
[null,"DRYWALL 1/2\""]
[null,null,"Drywall 1/2\" - Ceilings - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,{"$f":"K7-L7","v":0},{"$f":"IF(H7=1,I7,\"\")","v":""},{"$f":"F7*AVERAGE(K8:K12)","v":0},{"$f":"F7*AVERAGE(L8:L12)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"$D$1","v":"CEILINGS"},"CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(87,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / Easi-Lite / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,{"$f":"K8-L8","v":0},{"$f":"IF(H8=1,I8,\"\")","v":""},{"$f":"$D8*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D8*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"CEILINGS","CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(86,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / AirRenew / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,0,"",{"$f":"$D9*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D9*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"CEILINGS","CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(88,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / M2Tech moisture resistant / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,0,"",{"$f":"$D10*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D10*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"CEILINGS","CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(89,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / Pabco / QuietRock / QuietRock 1/2\""},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,{"$f":"K11-L11","v":0},{"$f":"IF(H11=1,I11,\"\")","v":""},{"$f":"$D11*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D11*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"CEILINGS","CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(376,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / National Gypsum / Gold Bond XP Gypsum Board  / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,0,"",{"$f":"$D12*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D12*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"CEILINGS","CLADDING"]
[null,"DRYWALL 5/8\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Drywall 5/8\" - Ceilings - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,{"$f":"K14-L14","v":0},{"$f":"IF(H14=1,I14,\"\")","v":""},{"$f":"F14*AVERAGE(K15:K17)","v":0},{"$f":"F14*AVERAGE(L15:L17)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"$D$1","v":"CEILINGS"},"CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(90,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,0,"",{"$f":"$D15*$F15*VLOOKUP($C15,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D15*$F15*VLOOKUP($C15,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"$D$1","v":"CEILINGS"},"CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(91,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" / USG / EcoSmart Firecode / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,0,"",{"$f":"$D16*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D16*$F16*VLOOKUP($C16,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"$D$1","v":"CEILINGS"},"CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(377,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" Type X / National Gypsum / Gold Bond XP Fire-Shield Gypsum Board  / 5/8'' type X"},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,{"$f":"K17-L17","v":0},{"$f":"IF(H17=1,I17,\"\")","v":""},{"$f":"$D17*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D17*$F17*VLOOKUP($C17,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"$D$1","v":"CEILINGS"},"CLADDING"]
[null,"OTHER CEILING FINISHES",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(146,'Master sheet'!$AL$1:$AL$441,0))","v":"MgO board 1/2\" / North American MgO / MagTech Ultra / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,{"$f":"K19-L19","v":0},{"$f":"IF(H19=1,I19,\"\")","v":""},{"$f":"$D19*$F19*VLOOKUP($C19,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D19*$F19*VLOOKUP($C19,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"$D$1","v":"CEILINGS"},"CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(31,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards"},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,0,"",{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D20*$F20*VLOOKUP($C20,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"CEILINGS","CLADDING"]
[null,"3/4\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,0,"",{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"CEILINGS","CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(17,'Master sheet'!$AL$1:$AL$441,0))","v":"Bamboo plywood / Smith & Fong / Plyboo / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,0,"",{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"CEILINGS","CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,0,"",{"$f":"$D23*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D23*$F23*VLOOKUP($C23,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"CEILINGS","CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(253,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood wool boards / Armstrong / Tectum / 2\" (50.8 mm)"},{"$f":"'USER INPUT SHEET'!$C$35","v":0},{"$f":"'USER INPUT SHEET'!$E$35","v":"m2"},1,null,null,0,"",{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"CEILINGS","CLADDING"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Roof","index":19,"n_rows":158,"n_cols":16,"rows_kept":158,"cut":false,"hidden":false,"merged":[[4,0,4,2],[5,1,5,2],[148,0,148,2],[13,1,13,2],[14,0,17,0],[11,1,11,2],[18,0,18,2],[27,1,27,2],[20,0,21,1],[22,1,22,2],[23,0,25,1],[32,0,32,2],[12,0,12,1],[26,0,26,2],[28,0,31,1],[19,1,19,2],[149,1,149,2],[67,0,69,1],[70,1,70,2],[72,0,75,1],[76,1,76,2],[78,0,84,1],[85,1,85,2],[143,1,143,2],[145,0,147,1],[119,0,119,2],[120,1,120,2],[122,0,123,1],[124,1,124,2],[126,0,130,1],[89,0,89,1],[94,1,94,2],[0,0,0,2],[0,3,0,12],[1,0,1,12],[2,3,3,3],[2,4,3,4],[2,11,3,11],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[2,0,3,1],[2,2,3,2],[2,5,3,5],[2,6,3,6],[33,1,33,2],[65,1,65,2],[57,1,57,2],[59,0,61,1],[62,1,62,2],[63,0,63,1],[64,0,64,2],[40,0,45,1],[46,1,46,2],[53,1,53,2],[55,0,56,1],[37,0,37,2],[38,1,38,2],[34,0,36,0],[119,5,119,7],[64,5,64,7],[131,1,131,2],[137,1,137,2],[139,0,142,1],[116,1,116,2],[87,1,87,2],[88,0,88,1],[90,0,90,1],[91,1,91,2],[86,0,86,1],[100,1,100,2],[105,1,105,2],[112,1,112,2]]}
["SECTION 12 ➜ COMPONENT MATERIALS FOR",null,null,"ROOF"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR ROOF"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["WOOD FRAME ROOF",null,null,"FRAMING SPACING:",null,"in"]
[null,"WOOD FRAMING"]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K7-L7","v":0},{"$f":"IF(H7=1,I7,\"\")","v":""},{"$f":"$D7*$F7*IF($E$5=16,0.25,0.22)*VLOOKUP($C7,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*3.5)","v":0},{"$f":"$D7*$F7*IF($E$5=16,0.25,0.22)*VLOOKUP($C7,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*3.5)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"WOOD FRAME ROOF"]
[null,"2x6",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K8-L8","v":0},{"$f":"IF(H8=1,I8,\"\")","v":""},{"$f":"$D8*$F8*IF($E$5=16,0.25,0.22)*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*5.5)","v":0},{"$f":"$D8*$F8*IF($E$5=16,0.25,0.22)*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*5.5)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"WOOD FRAME ROOF"]
[null,"2x8",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K9-L9","v":0},{"$f":"IF(H9=1,I9,\"\")","v":""},{"$f":"$D9*$F9*IF($E$5=16,0.25,0.22)*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*7.25)","v":0},{"$f":"$D9*$F9*IF($E$5=16,0.25,0.22)*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*7.25)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"WOOD FRAME ROOF"]
[null,"2x10",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K10-L10","v":0},{"$f":"IF(H10=1,I10,\"\")","v":""},{"$f":"$D10*$F10*IF($E$5=16,0.25,0.22)*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*9.25)","v":0},{"$f":"$D10*$F10*IF($E$5=16,0.25,0.22)*VLOOKUP($C10,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*9.25)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"WOOD FRAME ROOF"]
[null,"2x12",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K11-L11","v":0},{"$f":"IF(H11=1,I11,\"\")","v":""},{"$f":"$D11*$F11*IF($E$5=16,0.25,0.22)*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*11.25)","v":0},{"$f":"$D11*$F11*IF($E$5=16,0.25,0.22)*VLOOKUP($C11,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*11.25)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"WOOD FRAME ROOF"]
[null,"WOOD TRUSS FRAMING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"WOOD FRAME ROOF"]
["Use percent function to adjust wood volume relative to described roof design",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(252,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood roof truss - prefabricated / Quebec Wood Export Bureau / Common (Double Howe) Gabrel Roof / 2x6 Chords, 2x4 Webs, 4:12 Pitch, 40 ft span, 20\" overhang"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K13-L13","v":0},{"$f":"IF(H13=1,I13,\"\")","v":""},{"$f":"$D13*$F13*IF($E$5=16,2.46, 1.64)*VLOOKUP($C13,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D13*$F13*IF($E$5=16,2.46, 1.64)*VLOOKUP($C13,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,{"$f":"D$1","v":"ROOF"},"WOOD FRAME ROOF"]
[null,"WOOD I-JOIST FRAMING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"WOOD FRAME ROOF"]
[null,"9-1/2\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D15*$F15*IF($E$5=16,2.46,1.64)*VLOOKUP($C15,'Master sheet'!$A:$AJ,13,FALSE)*0.926","v":0},{"$f":"$D15*$F15*IF($E$5=16,2.46,1.64)*VLOOKUP($C15,'Master sheet'!$A:$AJ,27,FALSE)*0.926","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"WOOD FRAME ROOF"]
[null,"11-7/8\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D16*$F16*IF($E$5=16,2.46,1.64)*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)*1.029","v":0},{"$f":"$D16*$F16*IF($E$5=16,2.46,1.64)*VLOOKUP($C16,'Master sheet'!$A:$AJ,27,FALSE)*1.029","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"WOOD FRAME ROOF"]
[null,"14\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D17*$F17*IF($E$5=16,2.46,1.64)*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)*1.132","v":0},{"$f":"$D17*$F17*IF($E$5=16,2.46,1.64)*VLOOKUP($C17,'Master sheet'!$A:$AJ,27,FALSE)*1.132","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"WOOD FRAME ROOF"]
[null,"16\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D18*$F18*IF($E$5=16,2.46,1.64)*VLOOKUP($C18,'Master sheet'!$A:$AJ,13,FALSE)*1.2","v":0},{"$f":"$D18*$F18*IF($E$5=16,2.46,1.64)*VLOOKUP($C18,'Master sheet'!$A:$AJ,27,FALSE)*1.2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"WOOD FRAME ROOF"]
["ROOF DECKING",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"WOOD SHEET PRODUCTS - 5/8\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(160,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K21-L21","v":0},{"$f":"IF(H21=1,I21,\"\")","v":""},{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D21*$F21*VLOOKUP($C21,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF DECKING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(155,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K22-L22","v":0},{"$f":"IF(H22=1,I22,\"\")","v":""},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D22*$F22*VLOOKUP($C22,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF DECKING"]
[null,"GYPSUM PANELS 1/2\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(115,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K24-L24","v":0},{"$f":"IF(H24=1,I24,\"\")","v":""},{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D24*$F24*VLOOKUP($C24,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,{"$f":"D$1","v":"ROOF"},"ROOF DECKING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(116,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / USG / Securock ExoAir 430 / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K25-L25","v":0},{"$f":"IF(H25=1,I25,\"\")","v":""},{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D25*$F25*VLOOKUP($C25,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF DECKING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(418,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / CertainTeed / GlasRoc Sheathing gypsum board / 5/8\" "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K26-L26","v":0},{"$f":"IF(H26=1,I26,\"\")","v":""},{"$f":"$D26*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D26*$F26*VLOOKUP($C26,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF DECKING"]
["ROOFING MEMBRANE",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"ROOFING MEMBRANE",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(92,'Master sheet'!$AL$1:$AL$441,0))","v":"EPDM Roofing Membrane / SPRI /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K29-L29","v":0},{"$f":"IF(H29=1,I29,\"\")","v":""},{"$f":"$D29*$F29*VLOOKUP($C29,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D29*$F29*VLOOKUP($C29,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,{"$f":"D$1","v":"ROOF"},"ROOFING MEMBRANE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(180,'Master sheet'!$AL$1:$AL$441,0))","v":"SBS Modified Bitumen Roofing / ARMA / Includes: CertainTeed, Firestone, GAF, Henry, IKO, Johns Mansville, Malarkey, Siplast, Soprema / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K30-L30","v":0},{"$f":"IF(H30=1,I30,\"\")","v":""},{"$f":"$D30*$F30*VLOOKUP($C30,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D30*$F30*VLOOKUP($C30,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,{"$f":"D$1","v":"ROOF"},"ROOFING MEMBRANE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(172,'Master sheet'!$AL$1:$AL$441,0))","v":"PVC Roofing Membrane / CIFA / Includes: Canadian General-Tower, Duro-Last, FiberTite / 48 mils"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K31-L31","v":0},{"$f":"IF(H31=1,I31,\"\")","v":""},{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D31*$F31*VLOOKUP($C31,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,{"$f":"D$1","v":"ROOF"},"ROOFING MEMBRANE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(213,'Master sheet'!$AL$1:$AL$441,0))","v":"TPO Roofing Membrane / Carlisle /  / 60 mils"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K32-L32","v":0},{"$f":"IF(H32=1,I32,\"\")","v":""},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,{"$f":"D$1","v":"ROOF"},"ROOFING MEMBRANE"]
["ROOF STRAPPING",null,null,"STRAPPING SPACING:",null,"in",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"WOOD STRAPPING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"1x3",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K35-L35","v":0},{"$f":"IF(H35=1,I35,\"\")","v":""},{"$f":"$D35*$F35*IF($E$33=16,2.5/16,2.5/24)*VLOOKUP($C35,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D35*$F35*IF($E$33=16,2.5/16,2.5/24)*VLOOKUP($C35,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF STRAPPING"]
[null,"1x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K36-L36","v":0},{"$f":"IF(H36=1,I36,\"\")","v":""},{"$f":"$D36*$F36*IF($E$33=16,3.5/16,3.5/24)*VLOOKUP($C36,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D36*$F36*IF($E$33=16,3.5/16,3.5/24)*VLOOKUP($C36,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF STRAPPING"]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K37-L37","v":0},{"$f":"IF(H37=1,I37,\"\")","v":""},{"$f":"$D37*$F37*IF($E$33=16,3.5/16,3.5/24)*VLOOKUP($C37,'Master sheet'!$A:$AJ,13,FALSE)*0.0381","v":0},{"$f":"$D37*$F37*IF($E$33=16,3.5/16,3.5/24)*VLOOKUP($C37,'Master sheet'!$A:$AJ,27,FALSE)*0.0381","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF STRAPPING"]
["ROOFING",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"ASPHALT SHINGLES",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Asphalt Shingles - Roofing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K40-L40","v":0},{"$f":"IF(H40=1,I40,\"\")","v":""},{"$f":"F40*AVERAGE(K41:K46)","v":0},{"$f":"F40*AVERAGE(L41:L46)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(12,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Includes: Atlas, BP, CertainTeed, GAF, IKO, Malarkey, Owens Corning, Pabco /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K41-L41","v":0},{"$f":"IF(H41=1,I41,\"\")","v":""},{"$f":"$D41*$F41*VLOOKUP($C41,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D41*$F41*VLOOKUP($C41,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"ROOF","ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(14,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Owens Corning / Duration / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D42*$F42*VLOOKUP($C42,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D42*$F42*VLOOKUP($C42,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(15,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Owens Corning / Oakridge / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K43-L43","v":0},{"$f":"IF(H43=1,I43,\"\")","v":""},{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(16,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Owens Corning / Supreme / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(13,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / GAF / Timberline / Timberline"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K45-L45","v":0},{"$f":"IF(H45=1,I45,\"\")","v":""},{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(380,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / GAF / Timberline Cool Series / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOFING"]
[null,"STEEL PANELS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Steel Panels - Roofing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K48-L48","v":0},{"$f":"IF(H48=1,I48,\"\")","v":""},{"$f":"F48*AVERAGE(K49:K53)","v":0},{"$f":"F48*AVERAGE(L49:L53)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(141,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / ArcelorMittal / All products / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"ROOF","ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(142,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Canadian Sheet Steel Building Institute / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D50*$F50*VLOOKUP($C50,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D50*$F50*VLOOKUP($C50,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"ROOF","ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(143,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Metal Building Manufacturers Assn / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D51*$F51*VLOOKUP($C51,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D51*$F51*VLOOKUP($C51,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"ROOF","ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(144,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Metal Construction Assn. / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K52-L52","v":0},{"$f":"IF(H52=1,I52,\"\")","v":""},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(145,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Petersen Aluminum Corp / PAC-CLAD / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K53-L53","v":0},{"$f":"IF(H53=1,I53,\"\")","v":""},{"$f":"$D53*$F53*VLOOKUP($C53,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D53*$F53*VLOOKUP($C53,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"ROOF","ROOFING"]
[null,"ALUMINUM PANELS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Aluminum l Panels - Roofing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K55-L55","v":0},{"$f":"IF(H55=1,I55,\"\")","v":""},{"$f":"F55*AVERAGE(K56:K57)","v":0},{"$f":"F55*AVERAGE(L56:L57)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(138,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Aluminum / Metal Construction Assn. / 22 gauge / Includes: ATAS, DMI, Englert, Fabral,McElroy, Pac-Clad"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D56*$F56*VLOOKUP($C56,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D56*$F56*VLOOKUP($C56,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(139,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Aluminum / Petersen Aluminum Corp / Pac-Clad / 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D57*$F57*VLOOKUP($C57,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D57*$F57*VLOOKUP($C57,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
[null,"FIBER CEMENT ROOFING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiber Cement roofing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K59-L59","v":0},{"$f":"IF(H59=1,I59,\"\")","v":""},{"$f":"F59*AVERAGE(K60:K62)","v":0},{"$f":"F59*AVERAGE(L60:L62)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(97,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement roofing / Cembrit / Corrugated sheets / 6.5 mm"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D60*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D60*$F60*VLOOKUP($C60,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(98,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement roofing / Cembrit / Slates / 4 mm"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D61*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D61*$F61*VLOOKUP($C61,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(99,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement roofing / Mahaphant / Fibre-Cement / 5 mm"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
[null,"OTHER ROOFING OPTIONS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C63,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(43,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay roof tiles / HISPALYT /  / "},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K64-L64","v":0},{"$f":"IF(H64=1,I64,\"\")","v":""},{"$f":"$D64*$F64*VLOOKUP($C64,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D64*$F64*VLOOKUP($C64,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C64,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,{"$f":"D$1","v":"ROOF"},"ROOFING"]
["ROOF CAVITY INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,"INSULATION PARALLEL TO:",null,null,"Ceiling surface",null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"FIBERGLASS BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiberglass batt - Roof Insulation - AVERAGE",{"$f":"IF(OR($I$65=\"Roof surface\",$I$65=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K67-L67","v":0},{"$f":"IF(H67=1,I67,\"\")","v":""},{"$f":"F67*AVERAGE(K68:K70)","v":0},{"$f":"F67*AVERAGE(L68:L70)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(104,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Owens Corning / EcoTouch Pink batt and roll / R 3.6/inch"},{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K68-L68","v":0},{"$f":"IF(H68=1,I68,\"\")","v":""},{"$f":"$D68*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,13,FALSE)*($E$66/5.678)","v":0},{"$f":"$D68*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,27,FALSE)*($E$66/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(102,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / CertainTeed / Sustainable Insulation / R 3.6/inch"},{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D69*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,13,FALSE)*($E$66/5.678)","v":0},{"$f":"$D69*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,27,FALSE)*($E$66/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(103,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Knauf / EcoBatt / R 3.6/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D70*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,13,FALSE)*($E$66/5.678)","v":0},{"$f":"$D70*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,27,FALSE)*($E$66/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,"FIBERGLASS LOOSE FILL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiberglass loose fill - Roof Insulation - AVERAGE",{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K72-L72","v":0},{"$f":"IF(H72=1,I72,\"\")","v":""},{"$f":"F72*AVERAGE(K73:K76)","v":0},{"$f":"F72*AVERAGE(L73:L76)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(107,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Owens Corning / AttiCat, ProCat, ProPink / R 2.8/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D73*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,13,FALSE)*($E$71/5.678)","v":0},{"$f":"$D73*$F73*VLOOKUP($C73,'Master sheet'!$A:$AJ,27,FALSE)*($E$71/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(105,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / CertainTeed / InsulSafe, Optima, TruComfort / R 2.6/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D74*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,13,FALSE)*($E$71/5.678)","v":0},{"$f":"$D74*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,27,FALSE)*($E$71/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(106,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Knauf / Jet Stream ULTRA / R 2.2/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K75-L75","v":0},{"$f":"IF(H75=1,I75,\"\")","v":""},{"$f":"$D75*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,13,FALSE)*($E$71/5.678)","v":0},{"$f":"$D75*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,27,FALSE)*($E$71/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(374,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Johns Manville / Climate Pro, Attic Protector, JM Spider PLUS (Canada) / R 2.8/inch, Formaldehyde-free"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D76*$F76*VLOOKUP($C76,'Master sheet'!$A:$AJ,13,FALSE)*($E$71/5.678)","v":0},{"$f":"$D76*$F76*VLOOKUP($C76,'Master sheet'!$A:$AJ,27,FALSE)*($E$71/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,"MINERAL WOOL BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Mineral wool batt - Roof Insulation - AVERAGE",{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K78-L78","v":0},{"$f":"IF(H78=1,I78,\"\")","v":""},{"$f":"F78*AVERAGE(K79:K85)","v":0},{"$f":"F78*AVERAGE(L79:L85)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(147,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Owens Corning / Thermafiber UltraBatt / R 4.3/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D79*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,13,FALSE)*($E$77/5.678)","v":0},{"$f":"$D79*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,27,FALSE)*($E$77/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(148,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / Safe'n'Sound, ComfortBatt / R 3.8/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K80-L80","v":0},{"$f":"IF(H80=1,I80,\"\")","v":""},{"$f":"$D80*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,13,FALSE)*($E$77/5.678)","v":0},{"$f":"$D80*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,27,FALSE)*($E$77/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(402,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R14 / R 4.0/inch, 3.5\""},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D81*$F81*VLOOKUP($C81,'Master sheet'!$A:$AJ,13,FALSE)*($E$77/5.678)","v":0},{"$f":"$D81*$F81*VLOOKUP($C81,'Master sheet'!$A:$AJ,27,FALSE)*($E$77/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(403,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R15 / R 4.3/inch, 3.5\""},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D82*$F82*VLOOKUP($C82,'Master sheet'!$A:$AJ,13,FALSE)*($E$77/5.678)","v":0},{"$f":"$D82*$F82*VLOOKUP($C82,'Master sheet'!$A:$AJ,27,FALSE)*($E$77/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(404,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R22 / R 4.0/inch, 5.5\""},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D83*$F83*VLOOKUP($C83,'Master sheet'!$A:$AJ,13,FALSE)*($E$77/5.678)","v":0},{"$f":"$D83*$F83*VLOOKUP($C83,'Master sheet'!$A:$AJ,27,FALSE)*($E$77/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(405,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 / R 4.4/inch, 5.5\""},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D84*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,13,FALSE)*($E$77/5.678)","v":0},{"$f":"$D84*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,27,FALSE)*($E$77/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(406,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 SS / R 4.0/inch, 6\" Steel Studs"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D85*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,13,FALSE)*($E$77/5.678)","v":0},{"$f":"$D85*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,27,FALSE)*($E$77/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOF INSULATION"]
[null,"MINERAL WOOL LOOSE FILL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(152,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool loose fill / NAIMA / R 3/inch"},{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K87-L87","v":0},{"$f":"IF(H87=1,I87,\"\")","v":""},{"$f":"$D87*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,13,FALSE)*($E$86/5.678)","v":0},{"$f":"$D87*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,27,FALSE)*($E$86/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,"SPRAY FOAM, CLOSED CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(183,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch"},{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K89-L89","v":0},{"$f":"IF(H89=1,I89,\"\")","v":""},{"$f":"$D89*($E$88/5.678)*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D89*($E$88/5.678)*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(184,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K90-L90","v":0},{"$f":"IF(H90=1,I90,\"\")","v":""},{"$f":"$D90*($E$88/5.678)*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D90*($E$88/5.678)*$F90*VLOOKUP($C90,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C90,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(410,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / "},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K91-L91","v":0},{"$f":"IF(H91=1,I91,\"\")","v":""},{"$f":"$D91*($E$88/5.678)*$F91*VLOOKUP($C91,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D91*($E$88/5.678)*$F91*VLOOKUP($C91,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C91,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,"SPRAY FOAM, OPEN CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C92,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(187,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell (HFC) / SPFA /  / R 4.1/inch"},{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K93-L93","v":0},{"$f":"IF(H93=1,I93,\"\")","v":""},{"$f":"$D93*($E$92/5.678)*$F93*VLOOKUP($C93,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D93*($E$92/5.678)*$F93*VLOOKUP($C93,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(188,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell - HFO gas / SPFA /  / R 4.1/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K94-L94","v":0},{"$f":"IF(H94=1,I94,\"\")","v":""},{"$f":"$D94*($E$92/5.678)*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D94*($E$92/5.678)*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,"CELLULOSE INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Cellulose - Roof Insulation - AVERAGE",{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K96-L96","v":0},{"$f":"IF(H96=1,I96,\"\")","v":""},{"$f":"F96*AVERAGE(K97:K100)","v":0},{"$f":"F96*AVERAGE(L97:L100)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(32,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - batt / CMS / R 3.6/inch / EcoCell"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K97-L97","v":0},{"$f":"IF(H97=1,I97,\"\")","v":""},{"$f":"$D97*$F97*VLOOKUP($C97,'Master sheet'!$A:$AJ,13,FALSE)*($E$95/5.678)","v":0},{"$f":"$D97*$F97*VLOOKUP($C97,'Master sheet'!$A:$AJ,27,FALSE)*($E$95/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(33,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - dense pack /  / R 3.7/inch / Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D98*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,13,FALSE)*($E$95/5.678)","v":0},{"$f":"$D98*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,27,FALSE)*($E$95/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(34,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - loose fill /  / R 3.7/inch / Includes: AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D99*$F99*VLOOKUP($C99,'Master sheet'!$A:$AJ,13,FALSE)*($E$95/5.678)","v":0},{"$f":"$D99*$F99*VLOOKUP($C99,'Master sheet'!$A:$AJ,27,FALSE)*($E$95/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(35,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - spray applied / R 3.75/inch / International Cellulose Corp. / K-13, ThermoCon"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K100-L100","v":0},{"$f":"IF(H100=1,I100,\"\")","v":""},{"$f":"$D100*$F100*VLOOKUP($C100,'Master sheet'!$A:$AJ,13,FALSE)*($E$95/5.678)","v":0},{"$f":"$D100*$F100*VLOOKUP($C100,'Master sheet'!$A:$AJ,27,FALSE)*($E$95/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,"WOOD FIBER BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Wood fiber batt - Roof Insulation - AVERAGE",{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K102-L102","v":0},{"$f":"IF(H102=1,I102,\"\")","v":""},{"$f":"F102*AVERAGE(K103:K105)","v":0},{"$f":"F102*AVERAGE(L103:L105)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C102,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(239,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / GUTEX / ThermoFlex / R 4/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D103*$F103*VLOOKUP($C103,'Master sheet'!$A:$AJ,13,FALSE)*($E$101/5.678)","v":0},{"$f":"$D103*$F103*VLOOKUP($C103,'Master sheet'!$A:$AJ,27,FALSE)*($E$101/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(241,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Steico / SteicoFlex / R 3.8/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D104*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,13,FALSE)*($E$101/5.678)","v":0},{"$f":"$D104*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,27,FALSE)*($E$101/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(240,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Pavatex / Pavaflex / R 3.8/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D105*$F105*VLOOKUP($C105,'Master sheet'!$A:$AJ,13,FALSE)*($E$101/5.678)","v":0},{"$f":"$D105*$F105*VLOOKUP($C105,'Master sheet'!$A:$AJ,27,FALSE)*($E$101/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C105,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,"OTHER NATURAL FIBER INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C106,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(254,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool batt / Havelock Wool /  / R 3.6/inch"},{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K107-L107","v":0},{"$f":"IF(H107=1,I107,\"\")","v":""},{"$f":"$D107*$F107*VLOOKUP($C107,'Master sheet'!$A:$AJ,13,FALSE)*($E$106/5.678)","v":0},{"$f":"$D107*$F107*VLOOKUP($C107,'Master sheet'!$A:$AJ,27,FALSE)*($E$106/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C107,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(255,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool loose fill / Havelock Wool /  / R 4.4/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D108*$F108*VLOOKUP($C108,'Master sheet'!$A:$AJ,13,FALSE)*($E$106/5.678)","v":0},{"$f":"$D108*$F108*VLOOKUP($C108,'Master sheet'!$A:$AJ,27,FALSE)*($E$106/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(121,'Master sheet'!$AL$1:$AL$441,0))","v":"Hemp fiber batt / NaturFibre / Hemp Wool / R 3.7/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D109*$F109*VLOOKUP($C109,'Master sheet'!$A:$AJ,13,FALSE)*($E$106/5.678)","v":0},{"$f":"$D109*$F109*VLOOKUP($C109,'Master sheet'!$A:$AJ,27,FALSE)*($E$106/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA"},null,"ROOF","ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(238,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber - loose fill / GUTEX / ThermoFiber / R 3.6/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D110*$F110*VLOOKUP($C110,'Master sheet'!$A:$AJ,13,FALSE)*($E$106/5.678)","v":0},{"$f":"$D110*$F110*VLOOKUP($C110,'Master sheet'!$A:$AJ,27,FALSE)*($E$106/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(210,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale /  / Wheat & rye straw / R 3.3/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K111-L111","v":0},{"$f":"IF(H111=1,I111,\"\")","v":""},{"$f":"$D111*$F111*VLOOKUP($C111,'Master sheet'!$A:$AJ,13,FALSE)*($E$106/5.678)","v":0},{"$f":"$D111*$F111*VLOOKUP($C111,'Master sheet'!$A:$AJ,27,FALSE)*($E$106/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"ROOF","ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(412,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale / SNaB (UK) / Wheat & barley straw / R 2.8/inch"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D112*$F112*VLOOKUP($C112,'Master sheet'!$A:$AJ,13,FALSE)*($E$106/5.678)","v":0},{"$f":"$D112*$F112*VLOOKUP($C112,'Master sheet'!$A:$AJ,27,FALSE)*($E$106/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","ROOF INSULATION"]
[null,"HEMPCRETE LOOSE FILL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Hempcrete - Roof Insulation - AVERAGE",{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K114-L114","v":0},{"$f":"IF(H114=1,I114,\"\")","v":""},{"$f":"F114*AVERAGE(K115:K116)","v":0},{"$f":"F114*AVERAGE(L115:L116)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(124,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / USA / R 2.1/inch, Avg. mix using NHL & PHL"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D115*$F115*VLOOKUP($C115,'Master sheet'!$A:$AJ,13,FALSE)*($E$113/5.678)","v":0},{"$f":"$D115*$F115*VLOOKUP($C115,'Master sheet'!$A:$AJ,27,FALSE)*($E$113/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2020"},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(123,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / Europe / R 2.1/inch, Avg. of 9 mixes"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D116*$F116*VLOOKUP($C116,'Master sheet'!$A:$AJ,13,FALSE)*($E$113/5.678)","v":0},{"$f":"$D116*$F116*VLOOKUP($C116,'Master sheet'!$A:$AJ,27,FALSE)*($E$113/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2017"},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,"HIGH R-VALUE INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(214,'Master sheet'!$AL$1:$AL$441,0))","v":"Vacuum Insulated Panel / Porextherm / Vacupor / R 30/inch"},{"$f":"$D$67","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K118-L118","v":0},{"$f":"IF(H118=1,I118,\"\")","v":""},{"$f":"$D118*$F118*VLOOKUP($C118,'Master sheet'!$A:$AJ,13,FALSE)*($E$117/5.678)","v":0},{"$f":"$D118*$F118*VLOOKUP($C118,'Master sheet'!$A:$AJ,27,FALSE)*($E$117/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(3,'Master sheet'!$AL$1:$AL$441,0))","v":"Aerogel blanket / Aspen Aerogels /  / R9.6/inch, White/Grey blanket"},0,{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K119-L119","v":0},{"$f":"IF(H119=1,I119,\"\")","v":""},{"$f":"$D119*$F119*VLOOKUP($C119,'Master sheet'!$A:$AJ,13,FALSE)*($E$117/5.678)","v":0},{"$f":"$D119*$F119*VLOOKUP($C119,'Master sheet'!$A:$AJ,27,FALSE)*($E$117/5.678)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,{"$f":"D$1","v":"ROOF"},"ROOF INSULATION"]
["RIGID ROOF INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,"INSULATION PARALLEL TO:",null,null,"Roof surface",{"$f":"IF(H120=1,I120,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"EPS FOAM BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"EPS foam board - AVERAGE",{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K122-L122","v":0},{"$f":"IF(H122=1,I122,\"\")","v":""},{"$f":"F122*AVERAGE(K123:K124)","v":0},{"$f":"F122*AVERAGE(L123:L124)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(94,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K123-L123","v":0},"",{"$f":"$D123*($E$121/5.678)*$F123*VLOOKUP($C123,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D123*($E$121/5.678)*$F123*VLOOKUP($C123,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,{"$f":"D$1","v":"ROOF"},"RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(96,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board with graphite / BASF / Neopor / R 4.7/inch, Type II, 15 psi (Type 2, 110 kPa)"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D124*($E$121/5.678)*$F124*VLOOKUP($C124,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D124*($E$121/5.678)*$F124*VLOOKUP($C124,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"RIGID ROOF INSULATION"]
[null,"WOOD FIBER BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Wood fiber board - AVERAGE",{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K126-L126","v":0},{"$f":"IF(H126=1,I126,\"\")","v":""},{"$f":"F126*AVERAGE(K127:K131)","v":0},{"$f":"F126*AVERAGE(L127:L131)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(242,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) Wood fiber board / AWC/CWC / Includes: Georgia Pacific, Louisville, BPC, Temple-Inland, Blue Ridge, Int'l Bildrite / R 2.7/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},"This is archived and can be deleted (BSUP)","ROOF","RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(243,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / GUTEX / Multi-Therm / R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D128*($E$125/5.678)*$F128*VLOOKUP($C128,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D128*($E$125/5.678)*$F128*VLOOKUP($C128,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(244,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Pavatex / Pavatherm / R 3.4/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D129*($E$125/5.678)*$F129*VLOOKUP($C129,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D129*($E$125/5.678)*$F129*VLOOKUP($C129,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"ROOF","RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(245,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Steico / Special Dry / R 3.6/inch, 40, 120, 140, 160, 180, 200 mm"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K130-L130","v":0},{"$f":"IF(H130=1,I130,\"\")","v":""},{"$f":"$D130*($E$125/5.678)*$F130*VLOOKUP($C130,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D130*($E$125/5.678)*$F130*VLOOKUP($C130,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"ROOF","RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(397,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / North American Fiberboard Association / Includes: MSL, Blue Ridge Fiberboard Inc. / R 2.7/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D131*($E$125/5.678)*$F131*VLOOKUP($C131,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D131*($E$125/5.678)*$F131*VLOOKUP($C131,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","RIGID ROOF INSULATION"]
[null,"XPS FOAM BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"XPS foam board - AVERAGE",{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K133-L133","v":0},{"$f":"IF(H133=1,I133,\"\")","v":""},{"$f":"F133*AVERAGE(K134:K136)","v":0},{"$f":"F133*AVERAGE(L134:L136)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(258,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Owens Corning / Foamular NGX 250  / R 5/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K134-L134","v":0},{"$f":"IF(H134=1,I134,\"\")","v":""},{"$f":"$D134*($E$132/5.678)*$F134*VLOOKUP($C134,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D134*($E$132/5.678)*$F134*VLOOKUP($C134,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C134,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C134,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"ROOF","RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(401,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Soprema / SOPRA-XPS / R 5.0/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K135-L135","v":0},{"$f":"IF(H135=1,I135,\"\")","v":""},{"$f":"$D135*($E$132/5.678)*$F135*VLOOKUP($C135,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D135*($E$132/5.678)*$F135*VLOOKUP($C135,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"ROOF","RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(400,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / DuPont / Reduced GWP Grey Styrofoam™ (same as ST-100) / R 5.0/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K136-L136","v":0},{"$f":"IF(H136=1,I136,\"\")","v":""},{"$f":"$D136*($E$132/5.678)*$F136*VLOOKUP($C136,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D136*($E$132/5.678)*$F136*VLOOKUP($C136,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"ROOF","RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(399,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) XPS foam board / DuPont / Styrofoam (Grey, Reduced GWP) / R 5.6/inch"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},"This is archived and can be deleted (BSUP)","ROOF","RIGID ROOF INSULATION"]
[null,"POLYISOCYANURATE FOAM BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Polyisocyanurate - AVERAGE",{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K139-L139","v":0},{"$f":"IF(H139=1,I139,\"\")","v":""},{"$f":"F139*AVERAGE(K140:K143)","v":0},{"$f":"F139*AVERAGE(L140:L143)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(166,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / Dow Chemical Company / Tuff-R, Super Tuff-R, Thermax / R 6.5/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D140*($E$138/5.678)*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D140*($E$138/5.678)*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"ROOF","RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(167,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / Hunter / Polysio Wall insulation boards / R 6.5/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D141*($E$138/5.678)*$F141*VLOOKUP($C141,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D141*($E$138/5.678)*$F141*VLOOKUP($C141,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(408,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / DuPont / Thermax / R 6.5/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K142-L142","v":0},{"$f":"IF(H142=1,I142,\"\")","v":""},{"$f":"$D142*($E$138/5.678)*$F142*VLOOKUP($C142,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D142*($E$138/5.678)*$F142*VLOOKUP($C142,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(411,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / PIMA / Includes: Atlas, Firestone, GAF, Johns Manville, Rmax, Carlisle, Iko, Soprema / R 6.5/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D143*($E$138/5.678)*$F143*VLOOKUP($C143,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D143*($E$138/5.678)*$F143*VLOOKUP($C143,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"ROOF","RIGID ROOF INSULATION"]
[null,"MINERAL WOOL BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C144,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C144,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Mineral wool board - AVERAGE",{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K145-L145","v":0},{"$f":"IF(H145=1,I145,\"\")","v":""},{"$f":"F145*AVERAGE(K146:K148)","v":0},{"$f":"F145*AVERAGE(L146:L148)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C145,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C145,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(149,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board - heavy density / NAIMA / R 4.2/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D146*($E$144/5.678)*$F146*VLOOKUP($C146,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D146*($E$144/5.678)*$F146*VLOOKUP($C146,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C146,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C146,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(150,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board / Rockwool / Rockboard 60 / R 4.3/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K147-L147","v":0},{"$f":"IF(H147=1,I147,\"\")","v":""},{"$f":"$D147*($E$144/5.678)*$F147*VLOOKUP($C147,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D147*($E$144/5.678)*$F147*VLOOKUP($C147,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C147,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C147,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"RIGID ROOF INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(407,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board  / Rockwool / Comfortboard 80 / R 4.2/inch"},{"$f":"IF(OR($I$120=\"Roof surface\",$I$120=\"Surface de toit\"), 'USER INPUT SHEET'!$C$36,'USER INPUT SHEET'!$C$37)","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D148*($E$144/5.678)*$F148*VLOOKUP($C148,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D148*($E$144/5.678)*$F148*VLOOKUP($C148,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C148,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C148,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"RIGID ROOF INSULATION"]
["INSULATED ROOFING PANELS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C149,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C149,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"SIP PANEL - EPS FOAM CORE with OSB",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C150,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C150,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"SIP panel - Roof - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K151-L151","v":0},{"$f":"IF(H151=1,I151,\"\")","v":""},{"$f":"F151*AVERAGE(K152:K155)","v":0},{"$f":"F151*AVERAGE(L152:L155)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C151,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C151,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"INSULATED ROOFING PANELS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(260,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R23 6.5\" - EPS 5.5\" @ R4/in. core, 2 sheets 1/2\" OSB"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K152-L152","v":0},{"$f":"IF(H152=1,I152,\"\")","v":""},{"$f":"$D152*$F152*VLOOKUP($C152,'Master sheet'!$A:$AJ,13,FALSE)*3.8746","v":0},{"$f":"$D152*$F152*VLOOKUP($C152,'Master sheet'!$A:$AJ,27,FALSE)*3.8746","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C152,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C152,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"INSULATED ROOFING PANELS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(261,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R30 8.25\" - EPS 7.25\" @ R4/in. core, 2 sheets 1/2\" OSB"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K153-L153","v":0},{"$f":"IF(H153=1,I153,\"\")","v":""},{"$f":"$D153*$F153*VLOOKUP($C153,'Master sheet'!$A:$AJ,13,FALSE)*5.1074","v":0},{"$f":"$D153*$F153*VLOOKUP($C153,'Master sheet'!$A:$AJ,27,FALSE)*5.1074","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C153,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C153,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"INSULATED ROOFING PANELS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(262,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R38 10.5\" - EPS 9.5\" @ R4/in. core, 2 sheets 1/2\" OSB"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K154-L154","v":0},{"$f":"IF(H154=1,I154,\"\")","v":""},{"$f":"$D154*$F154*VLOOKUP($C154,'Master sheet'!$A:$AJ,13,FALSE)*6.6925","v":0},{"$f":"$D154*$F154*VLOOKUP($C154,'Master sheet'!$A:$AJ,27,FALSE)*6.6925","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C154,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C154,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"INSULATED ROOFING PANELS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(263,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R48 12-7/8\" - EPS 11.875\" @ R4/in. core, 2 sheets 1/2\" OSB"},{"$f":"'USER INPUT SHEET'!$C$36","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K155-L155","v":0},{"$f":"IF(H155=1,I155,\"\")","v":""},{"$f":"$D155*$F155*VLOOKUP($C155,'Master sheet'!$A:$AJ,13,FALSE)*8.3656","v":0},{"$f":"$D155*$F155*VLOOKUP($C155,'Master sheet'!$A:$AJ,27,FALSE)*8.3656","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C155,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C155,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,{"$f":"D$1","v":"ROOF"},"INSULATED ROOFING PANELS"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Garage","index":20,"n_rows":450,"n_cols":16,"rows_kept":450,"cut":false,"hidden":false,"merged":[[323,1,323,2],[324,0,326,1],[49,0,49,2],[50,1,50,2],[51,0,58,1],[80,0,80,2],[81,1,81,2],[5,0,5,2],[6,1,6,2],[7,0,11,1],[32,0,32,2],[33,1,33,2],[34,0,40,1],[41,1,41,2],[42,0,48,1],[14,0,20,1],[21,1,21,2],[22,0,28,1],[29,0,29,2],[30,1,30,2],[12,0,12,2],[13,1,13,2],[65,0,71,1],[72,1,72,2],[0,3,0,12],[1,0,1,12],[2,0,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,9,3,9],[2,10,3,10],[2,11,3,11],[0,0,0,2],[73,0,79,1],[63,0,63,2],[64,1,64,2],[59,0,59,2],[60,1,60,2],[61,0,61,1],[141,1,141,2],[82,0,88,1],[90,0,90,3],[91,1,91,2],[99,0,99,2],[100,1,100,2],[92,0,98,1],[143,0,148,1],[140,0,140,2],[101,0,103,1],[132,1,132,2],[133,0,135,1],[136,1,136,2],[137,0,139,1],[111,0,111,2],[112,1,112,2],[113,0,118,1],[126,0,126,2],[105,0,105,2],[119,1,119,2],[127,1,127,2],[128,0,131,1],[106,1,106,2],[121,0,125,1],[190,1,190,2],[191,0,191,1],[176,0,179,1],[180,1,180,2],[181,0,185,1],[149,0,149,2],[150,1,150,2],[155,1,155,2],[157,0,160,1],[161,1,161,2],[162,0,168,1],[169,1,169,2],[171,0,173,1],[174,1,174,2],[188,0,188,1],[186,1,186,2],[187,0,187,1],[189,0,189,1],[319,0,322,1],[290,1,290,2],[292,0,299,0],[300,1,300,2],[301,0,301,1],[302,1,302,2],[304,0,305,1],[205,0,209,1],[210,1,210,2],[216,1,216,2],[218,0,221,1],[222,1,222,2],[224,0,226,1],[278,0,278,2],[267,0,267,1],[279,1,279,2],[280,0,286,1],[287,1,287,2],[288,0,289,0],[306,1,306,2],[308,0,313,1],[314,1,314,2],[316,0,317,1],[318,1,318,2],[342,1,342,2],[343,0,352,1],[354,0,354,2],[361,0,361,2],[366,0,366,2],[327,0,327,2],[330,0,330,2],[331,1,331,2],[333,0,337,1],[338,1,338,2],[339,0,341,1],[362,0,364,1],[406,0,408,1],[383,1,385,1],[387,0,387,2],[388,1,388,2],[394,1,394,2],[395,0,395,1],[396,1,396,2],[367,1,367,2],[369,0,373,1],[374,1,374,2],[379,1,379,2],[380,1,381,1],[376,0,378,1],[199,1,199,2],[201,0,202,1],[203,1,203,2],[440,1,440,2],[442,0,444,1],[445,1,445,2],[446,0,446,1],[420,0,420,2],[421,1,421,2],[423,0,428,1],[429,1,429,2],[436,1,436,2],[438,0,439,1],[409,0,409,2],[410,1,410,2],[411,0,414,1],[415,0,415,2],[416,1,416,2],[417,0,419,0],[397,0,400,0],[401,0,401,2],[402,1,402,2],[403,0,404,1],[405,1,405,2],[149,6,149,11],[192,0,192,1],[193,1,193,2],[195,0,197,1],[198,0,198,2],[272,1,272,2],[274,0,276,1],[198,6,198,10],[255,0,258,1],[259,1,259,2],[260,0,264,1],[265,1,265,2],[266,0,266,1],[268,0,268,1],[269,1,269,2],[228,0,228,2],[229,1,229,2],[234,1,234,2],[236,0,239,1],[240,1,240,2],[241,0,247,1],[248,1,248,2],[250,0,252,1],[253,1,253,2]]}
["SECTION 13 ➜ COMPONENT MATERIALS FOR",null,null,"GARAGE"]
["INSTRUCTIONS: (double-click)\nThe NET kgCO2e EMISSIONS column (Col. I) shows the global warming potential (GWP) of each material based on the information provided. \nYou must specify the R-VALUE, THICKNESS, FRAMING SPACING or any other required information in areas highlighted in YELLOW.\nEnter \"1\" in the SELECT column (Col. H) to add each material to your building. The net carbon emissions for the selected material will be highlighted in ORANGE. \nUse the percentage values cell (Col. G) if necessary to adjust the material quantity present in the building. \nThe carbon footprint of each selection will be added to the section SUBTOTAL (top of Col. M)  for this page, and for summary reporting."]
["CATEGORY",null,"MATERIAL","QUANTITY",null,"%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR GARAGE"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUM(J:J)","v":0}]
["GARAGE FOOTINGS & SLABS"]
["CRUSHED STONE BASE",null,null,"THICKNESS:",null,"in","=",{"$f":"IF(F6=\"mm\",E6/1000,E6*0.0254)","v":0},"m"]
[null,"AGGREGATE"]
["If you do not know the specific carbon footprint of your aggregate, chose the \"AVERAGE\" value",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(4,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate /  /  / Avg construction aggregate (gravel & sand)"},{"$f":"'USER INPUT SHEET'!$C$50","v":0},"m2",1,null,null,{"$f":"K8-L8","v":0},{"$f":"IF(H8=1,I8,\"\")","v":""},{"$f":"$D8*$H$6*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D8*$H$6*$F8*VLOOKUP($C8,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CRUSHED STONE BASE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(5,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Kangley Rock & Recycling /  / Avg construction aggregate (gravel & sand)"},{"$f":"'USER INPUT SHEET'!$C$50","v":0},"m2",1,null,null,{"$f":"K9-L9","v":0},{"$f":"IF(H9=1,I9,\"\")","v":""},{"$f":"$D9*$H$6*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D9*$H$6*$F9*VLOOKUP($C9,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CRUSHED STONE BASE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(6,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Martin Marietta /  / Avg construction aggregate (gravel & sand)"},{"$f":"'USER INPUT SHEET'!$C$50","v":0},"m2",1,null,null,{"$f":"K10-L10","v":0},{"$f":"IF(H10=1,I10,\"\")","v":""},{"$f":"$D10*$H$6*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D10*$H$6*$F10*VLOOKUP($C10,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CRUSHED STONE BASE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(7,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Polaris Mtls Corp. /  / Avg construction aggregate (gravel & sand)"},{"$f":"'USER INPUT SHEET'!$C$50","v":0},"m2",1,null,null,{"$f":"K11-L11","v":0},{"$f":"IF(H11=1,I11,\"\")","v":""},{"$f":"$D11*$H$6*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D11*$H$6*$F11*VLOOKUP($C11,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CRUSHED STONE BASE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(8,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Vulcan Mtls Co. /  / Avg construction aggregate (gravel & sand)"},{"$f":"'USER INPUT SHEET'!$C$50","v":0},"m2",1,null,null,{"$f":"K12-L12","v":0},{"$f":"IF(H12=1,I12,\"\")","v":""},{"$f":"$D12*$H$6*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D12*$H$6*$F12*VLOOKUP($C12,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE CRUSHED STONE BASE"]
["CONCRETE SLAB FLOOR",null,null,"THICKNESS:",null,"in","=",{"$f":"IF(F13=\"mm\",E13/1000,E13*0.0254)","v":0},"m",null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CONCRETE – 25 MPa or less",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,{"$f":"K15-L15","v":0},{"$f":"IF(H15=1,I15,\"\")","v":""},{"$f":"$D15*$F15*$H$13*VLOOKUP($C15,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D15*$F15*$H$13*VLOOKUP($C15,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,0,"",{"$f":"$D16*$F16*$H$13*VLOOKUP($C16,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D16*$F16*$H$13*VLOOKUP($C16,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,0,"",{"$f":"$D17*$F17*$H$13*VLOOKUP($C17,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D17*$F17*$H$13*VLOOKUP($C17,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,0,"",{"$f":"$D18*$F18*$H$13*VLOOKUP($C18,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D18*$F18*$H$13*VLOOKUP($C18,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,0,"",{"$f":"$D19*$F19*$H$13*VLOOKUP($C19,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D19*$F19*$H$13*VLOOKUP($C19,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,{"$f":"K20-L20","v":0},{"$f":"IF(H20=1,I20,\"\")","v":""},{"$f":"$D20*$F20*$H$13*VLOOKUP($C20,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D20*$F20*$H$13*VLOOKUP($C20,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D21*$F21*$H$13*VLOOKUP($C21,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D21*$F21*$H$13*VLOOKUP($C21,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C22,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE SLAB FLOOR"]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,{"$f":"K23-L23","v":0},{"$f":"IF(H23=1,I23,\"\")","v":""},{"$f":"$D23*$F23*$H$13*VLOOKUP($C23,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D23*$F23*$H$13*VLOOKUP($C23,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C23,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,0,"",{"$f":"$D24*$F24*$H$13*VLOOKUP($C24,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D24*$F24*$H$13*VLOOKUP($C24,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C24,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,0,"",{"$f":"$D25*$F25*$H$13*VLOOKUP($C25,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D25*$F25*$H$13*VLOOKUP($C25,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C25,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,0,"",{"$f":"$D26*$F26*$H$13*VLOOKUP($C26,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D26*$F26*$H$13*VLOOKUP($C26,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C26,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,0,"",{"$f":"$D27*$F27*$H$13*VLOOKUP($C27,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D27*$F27*$H$13*VLOOKUP($C27,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C27,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,{"$f":"K28-L28","v":0},{"$f":"IF(H28=1,I28,\"\")","v":""},{"$f":"$D28*$F28*$H$13*VLOOKUP($C28,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D28*$F28*$H$13*VLOOKUP($C28,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C28,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE SLAB FLOOR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$50","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D29*$F29*$H$13*VLOOKUP($C29,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D29*$F29*$H$13*VLOOKUP($C29,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C29,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE SLAB FLOOR"]
["SLAB REINFORCING MESH",null,null,"CUSTOM AREA:",null,"m2",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C30,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"WELDED WIRE MESH (WWM)",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C31,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(221,'Master sheet'!$AL$1:$AL$441,0))","v":"Welded wire mesh / Serfas /  / 6\" x 6\" x 6/6g / Norway"},{"$f":"IF(E30>0,E30,'USER INPUT SHEET'!$C$50)","v":0},{"$f":"'USER INPUT SHEET'!$E$50","v":"m2"},1,null,null,{"$f":"K32-L32","v":0},{"$f":"IF(H32=1,I32,\"\")","v":""},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D32*$F32*VLOOKUP($C32,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C32,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE SLAB WIRE MESH"]
["FOOTINGS, PIERS & PADS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C33,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CONCRETE – 25 MPa or less",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C34,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,{"$f":"K35-L35","v":0},{"$f":"IF(H35=1,I35,\"\")","v":""},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D35*$F35*VLOOKUP($C35,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C35,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,0,"",{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D36*$F36*VLOOKUP($C36,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C36,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,0,"",{"$f":"$D37*$F37*VLOOKUP($C37,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D37*$F37*VLOOKUP($C37,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C37,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,0,"",{"$f":"$D38*$F38*VLOOKUP($C38,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D38*$F38*VLOOKUP($C38,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C38,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,0,"",{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D39*$F39*VLOOKUP($C39,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C39,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,{"$f":"K40-L40","v":0},{"$f":"IF(H40=1,I40,\"\")","v":""},{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D40*$F40*VLOOKUP($C40,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C40,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D41*$F41*VLOOKUP($C41,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D41*$F41*VLOOKUP($C41,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C41,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C42,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE FOOTINGS & PADS"]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,{"$f":"K43-L43","v":0},{"$f":"IF(H43=1,I43,\"\")","v":""},{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D43*$F43*VLOOKUP($C43,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C43,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,0,"",{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D44*$F44*VLOOKUP($C44,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C44,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,0,"",{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D45*$F45*VLOOKUP($C45,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C45,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,0,"",{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D46*$F46*VLOOKUP($C46,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C46,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,0,"",{"$f":"$D47*$F47*VLOOKUP($C47,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D47*$F47*VLOOKUP($C47,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C47,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,{"$f":"K48-L48","v":0},{"$f":"IF(H48=1,I48,\"\")","v":""},{"$f":"$D48*$F48*VLOOKUP($C48,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D48*$F48*VLOOKUP($C48,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C48,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE FOOTINGS & PADS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!C$47","v":0},{"$f":"'USER INPUT SHEET'!E$47","v":"m3"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D49*$F49*VLOOKUP($C49,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C49,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE FOOTINGS & PADS"]
["REBAR",null,null,"CUSTOM LENGTH:",null,"m",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C50,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,"CONCRETE REINFORCING BAR",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C51,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
["Specify an overall rebar length.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(176,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Concrete Reinforcing Steel Institute /  / 10M"},{"$f":"IF(E$50>0,E$50,'USER INPUT SHEET'!$F$48)","v":0},{"$f":"$F$50","v":"m"},1,null,null,{"$f":"K52-L52","v":0},{"$f":"IF(H52=1,I52,\"\")","v":""},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D52*$F52*VLOOKUP($C52,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C52,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(177,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Concrete Reinforcing Steel Institute /  / 15M"},{"$f":"IF(E$50>0,E$50,'USER INPUT SHEET'!$F$48)","v":0},"m",1,null,null,0,"",{"$f":"$D53*$F53*VLOOKUP($C53,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D53*$F53*VLOOKUP($C53,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C53,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(390,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Nucor Corporation / Canadian sizes / 10M"},{"$f":"IF(E$50>0,E$50,'USER INPUT SHEET'!$F$48)","v":0},"m",1,null,null,0,"",{"$f":"$D54*$F54*VLOOKUP($C54,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D54*$F54*VLOOKUP($C54,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C54,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(391,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Nucor Corporation / Canadian sizes / 15M"},{"$f":"IF(E$50>0,E$50,'USER INPUT SHEET'!$F$48)","v":0},"m",1,null,null,0,"",{"$f":"$D55*$F55*VLOOKUP($C55,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D55*$F55*VLOOKUP($C55,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C55,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(392,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Nucor Corporation / Canadian sizes / 20M"},{"$f":"IF(E$50>0,E$50,'USER INPUT SHEET'!$F$48)","v":0},"m",1,null,null,0,"",{"$f":"$D56*$F56*VLOOKUP($C56,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D56*$F56*VLOOKUP($C56,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C56,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(393,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 10M"},{"$f":"IF(E$50>0,E$50,'USER INPUT SHEET'!$F$48)","v":0},"m",1,null,null,0,"",{"$f":"$D57*$F57*VLOOKUP($C57,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D57*$F57*VLOOKUP($C57,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C57,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(394,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 15M"},{"$f":"IF(E$50>0,E$50,'USER INPUT SHEET'!$F$48)","v":0},"m",1,null,null,0,"",{"$f":"$D58*$F58*VLOOKUP($C58,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D58*$F58*VLOOKUP($C58,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C58,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE REBAR"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(395,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 20M"},{"$f":"IF(E$50>0,E$50,'USER INPUT SHEET'!$F$48)","v":0},"m",1,null,null,0,"",{"$f":"$D59*$F59*VLOOKUP($C59,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D59*$F59*VLOOKUP($C59,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C59,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE REBAR"]
["HELICAL PIERS",null,null,"TOTAL LENGTH OF ALL PIERS:",null,"m",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C60,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,"HELICAL PIERS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C61,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
["Specify the total length of all piers. Use % to adjust for different sized piers",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(120,'Master sheet'!$AL$1:$AL$441,0))","v":"Helical pier / Generic /  / 3\" Nominal Pipe, 3.5 x 3/16\" (89 x 5.5 mm), 10\" Helix, Sched 40 STD Galvanized steel"},{"$f":"E$60","v":0},"m",1,null,null,{"$f":"K62-L62","v":0},{"$f":"IF(H62=1,I62,\"\")","v":""},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D62*$F62*VLOOKUP($C62,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C62,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE HELICAL PIERS"]
["GARAGE FOUNDATION WALLS"]
["CONCRETE FOUNDATION WALLS",null,null,"THICKNESS:",null,"in","=",{"$f":"IF(F64=\"mm\",E64/1000,E64*2.54/100)","v":0},"m",null,null,null,null,null,"GARAGE"]
[null,"CONCRETE – 25 MPa or less",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C65,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,{"$f":"K66-L66","v":0},{"$f":"IF(H66=1,I66,\"\")","v":""},{"$f":"$D66*$H$64*$F66*VLOOKUP($C66,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C66,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D67*$H$64*$F67*VLOOKUP($C67,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C67,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D68*$H$64*$F68*VLOOKUP($C68,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C68,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D69*$H$64*$F69*VLOOKUP($C69,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C69,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D70*$H$64*$F70*VLOOKUP($C70,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C70,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,{"$f":"K71-L71","v":0},{"$f":"IF(H71=1,I71,\"\")","v":""},{"$f":"$D71*$H$64*$F71*VLOOKUP($C71,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C71,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"0-25\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D72*$H$64*$F72*VLOOKUP($C72,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C72,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,"CONCRETE – 26-30 MPa",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C73,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CONCRETE WALLS"]
["Concrete mix specification makes a big difference in carbon footprint. The mix specifications here can be used to discuss low-carbon mix options with your supplier.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(1 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,{"$f":"K74-L74","v":0},{"$f":"IF(H74=1,I74,\"\")","v":""},{"$f":"$D74*$H$64*$F74*VLOOKUP($C74,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C74,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(2 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D75*$H$64*$F75*VLOOKUP($C75,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C75,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(3 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D76*$H$64*$F76*VLOOKUP($C76,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C76,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(4 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D77*$H$64*$F77*VLOOKUP($C77,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C77,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(5 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D78*$H$64*$F78*VLOOKUP($C78,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C78,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(6 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,{"$f":"K79-L79","v":0},{"$f":"IF(H79=1,I79,\"\")","v":""},{"$f":"$D79*$H$64*$F79*VLOOKUP($C79,'Master sheet'!$A:$AJ,13,FALSE)","v":0},0,{"$f":"IF(ISTEXT(VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C79,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CONCRETE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,(\"26-30\" = 'Master sheet'!$AM$1:$AM$441)*(7 = 'Master sheet'!$AN$1:$AN$441)*('Master sheet'!$AR$1:$AR$441),0))","v":{"$error":"#N/A"}},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,{"$error":"#N/A"},"",{"$f":"$D80*$H$64*$F80*VLOOKUP($C80,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},0,{"$f":"IF(ISTEXT(VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C80,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CONCRETE WALLS"]
["CMU FOUNDATION WALLS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C81,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CONCRETE MASONRY UNITS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C82,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["If concrete grout is being used in the CMU wall use the concrete wall area to specify the quantity of concrete fill being used in the CMUs.",null,"CMU Walls 8\" Hollow, no grout - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,{"$f":"K83-L83","v":0},{"$f":"IF(H83=1,I83,\"\")","v":""},{"$f":"$F83*AVERAGE(K84:K89)","v":0},{"$f":"$F83*AVERAGE(L84:L89)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C83,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(48,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Canadian Concrete Masonry Producers Assn / 8\" Normal weight blocks / 390 x 190 x 190 mm"},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D84*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D84*$F84*VLOOKUP($C84,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C84,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(47,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Angelus Block Co. / 8\" Normal weight blocks / 8 x 8 x 16 Precision"},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D85*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D85*$F85*VLOOKUP($C85,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C85,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(49,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Permacon / 8\" Normal weight blocks / NW STD 20CM GLPW"},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D86*$F86*VLOOKUP($C86,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D86*$F86*VLOOKUP($C86,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C86,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(46,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Canadian Concrete Masonry Producers Assn / 8\" Light weight blocks / 390 x 190 x 190 mm"},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D87*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D87*$F87*VLOOKUP($C87,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C87,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(44,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Angelus Block Co. / 8\" Light weight blocks / 9 x 8 x 16 Precision"},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D88*$F88*VLOOKUP($C88,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D88*$F88*VLOOKUP($C88,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C88,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE CMU FOUNDATION WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(45,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Brampton Brick / 8\" Carbon Cure Lightweight blocks / Carbon Cure 15 MPa"},{"$f":"'USER INPUT SHEET'!$C$49","v":0},{"$f":"'USER INPUT SHEET'!$E$49","v":"m2"},1,null,null,0,"",{"$f":"$D89*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D89*$F89*VLOOKUP($C89,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C89,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE CMU FOUNDATION WALLS"]
["GARAGE HEAVY STRUCTURAL ELEMENTS"]
["MASS TIMBER FRAMING"]
[null,"MASS TIMBER"]
["Use % function if multiple types of mass timber will be used.",null,"Heavy Timber Framing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$55","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,{"$f":"K93-L93","v":0},{"$f":"IF(H93=1,I93,\"\")","v":""},{"$f":"$F93*AVERAGE(K94:K99)","v":0},{"$f":"$F93*AVERAGE(L94:L99)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C93,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$55","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,0,"",{"$f":"$D94*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D94*$F94*VLOOKUP($C94,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C94,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(126,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminated strand lumber (LSL) / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$55","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,0,"",{"$f":"$D95*$F95*VLOOKUP($C95,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D95*$F95*VLOOKUP($C95,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C95,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(127,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminated veneer lumber (LVL) / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$55","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,0,"",{"$f":"$D96*$F96*VLOOKUP($C96,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D96*$F96*VLOOKUP($C96,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C96,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(113,'Master sheet'!$AL$1:$AL$441,0))","v":"Glued laminated timber / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$55","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,0,"",{"$f":"$D97*$F97*VLOOKUP($C97,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D97*$F97*VLOOKUP($C97,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C97,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(114,'Master sheet'!$AL$1:$AL$441,0))","v":"Glued laminated timber / Structurlam / Glulam Plus / 3-1/2\" (90mm) thick"},{"$f":"'USER INPUT SHEET'!$C$55","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,0,"",{"$f":"$D98*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D98*$F98*VLOOKUP($C98,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C98,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE MASS TIMBER"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(409,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminated veneer lumber / Roseburg Forest Products / RigidLam LVL / "},{"$f":"'USER INPUT SHEET'!$C$55","v":0},{"$f":"'USER INPUT SHEET'!$E$38","v":"m3"},1,null,null,{"$f":"K99-L99","v":0},{"$f":"IF(H99=1,I99,\"\")","v":""},{"$f":"$D99*$F99*VLOOKUP($C99,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D99*$F99*VLOOKUP($C99,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C99,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE MASS TIMBER"]
["HEAVY STEEL COMPONENTS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C100,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"STEEL POSTS & BEAMS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C101,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Choose steel beam section from drop-down menu and input linear metres for each component type, as values do not come from User Input Sheet.",null,"Steel Beam W Section – AVERAGE",null,"m",1,null,null,{"$f":"K102-L102","v":0},{"$f":"IF(H102=1,I102,\"\")","v":""},{"$f":"$D102*$F102*'Master sheet'!$K$204*30","v":0},0,null,null,"GARAGE","GARAGE HEAVY STEEL COMPONENTS"]
[null,null,null,null,"m",1,null,null,{"$f":"K103-L103","v":{"$error":"#N/A"}},{"$f":"IF(H103=1,I103,\"\")","v":""},{"$f":"$D103*$F103*VLOOKUP($C103,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$D103*$F103*VLOOKUP($C103,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C103,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE HEAVY STEEL COMPONENTS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(199,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel post / Generic /  / 3.5 x 0.216\" (89 x 5.5 mm), Sched 40 STD"},null,"m",1,null,null,{"$f":"K104-L104","v":0},{"$f":"IF(H104=1,I104,\"\")","v":""},{"$f":"$D104*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D104*$F104*VLOOKUP($C104,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C104,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE HEAVY STEEL COMPONENTS"]
["GARAGE EXTERIOR WALLS"]
["WOOD FRAME CONSTRUCTION",null,null,"FRAMING SPACING:",null,"in"]
[null,"WOOD FRAME CONSTRUCTION"]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K108-L108","v":0},{"$f":"IF(H108=1,I108,\"\")","v":""},{"$f":"$F108*IF($E$106=16,$D108*0.25,$D108*0.22)*VLOOKUP($C108,'Master sheet'!$A:$AJ,13,FALSE)*0.0889","v":0},{"$f":"$F108*IF($E$106=16,$D108*0.25,$D108*0.22)*VLOOKUP($C108,'Master sheet'!$A:$AJ,27,FALSE)*0.0889","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C108,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD FRAME WALLS"]
[null,"2x6",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K109-L109","v":0},"",{"$f":"$F109*IF($E$106=16,$D109*0.25,$D109*0.22)*VLOOKUP($C109,'Master sheet'!$A:$AJ,13,FALSE)*0.1397","v":0},{"$f":"$F109*IF($E$106=16,$D109*0.25,$D109*0.22)*VLOOKUP($C109,'Master sheet'!$A:$AJ,27,FALSE)*0.1397","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C109,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD FRAME WALLS"]
[null,"2x8",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K110-L110","v":0},"",{"$f":"$F110*IF($E$106=16,$D110*0.25,$D110*0.22)*VLOOKUP($C110,'Master sheet'!$A:$AJ,13,FALSE)*0.18415","v":0},{"$f":"$F110*IF($E$106=16,$D110*0.25,$D110*0.22)*VLOOKUP($C110,'Master sheet'!$A:$AJ,27,FALSE)*0.18415","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C110,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD FRAME WALLS"]
[null,"Double 2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K111-L111","v":0},"",{"$f":"$F111*IF($E$106=16,$D111*0.25,$D111*0.22)*VLOOKUP($C111,'Master sheet'!$A:$AJ,13,FALSE)*(2*0.0889)","v":0},{"$f":"$F111*IF($E$106=16,$D111*0.25,$D111*0.22)*VLOOKUP($C111,'Master sheet'!$A:$AJ,27,FALSE)*(2*0.0889)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C111,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD FRAME WALLS"]
["STEEL FRAME CONSTRUCTION",null,null,"FRAMING SPACING:",null,"in",null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C112,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"STEEL FRAMING, 2x6",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C113,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
["Use % function to adjust for other gauges of steel studs.",null,"Steel Framing - Load bearing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K114-L114","v":0},{"$f":"IF(H114=1,I114,\"\")","v":""},{"$f":"F114*AVERAGE(K115:K119)","v":0},{"$f":"F114*AVERAGE(L115:L119)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C114,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(201,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / MarinoWARE / Structural stud and track / 600-S-137-54, 16 gauge, \"2x6\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D115*$F115*IF($E$112=16,3.79,2.97)*VLOOKUP($C115,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D115*$F115*IF($E$112=16,3.79,2.97)*VLOOKUP($C115,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C115,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(204,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / Steel Recycling Institute /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D116*$F116*IF($E$112=16,3.79,2.97)*VLOOKUP($C116,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D116*$F116*IF($E$112=16,3.79,2.97)*VLOOKUP($C116,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C116,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(202,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / MBA Building Supplies /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D117*$F117*IF($E$112=16,3.79,2.97)*VLOOKUP($C117,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D117*$F117*IF($E$112=16,3.79,2.97)*VLOOKUP($C117,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C117,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(203,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / Scafco /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D118*$F118*IF($E$112=16,3.79,2.97)*VLOOKUP($C118,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D118*$F118*IF($E$112=16,3.79,2.97)*VLOOKUP($C118,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C118,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(200,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing  / ClarkDietrich /  / 600-S-137-54, 16 gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D119*$F119*IF($E$112=16,3.79,2.97)*VLOOKUP($C119,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D119*$F119*IF($E$112=16,3.79,2.97)*VLOOKUP($C119,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C119,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
[null,"STEEL FRAMING, 2x4",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C120,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Steel Framing - Interior Walls - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K121-L121","v":0},{"$f":"IF(H121=1,I121,\"\")","v":""},{"$f":"F121*AVERAGE(K122:K126)","v":0},{"$f":"F121*AVERAGE(L122:L126)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C121,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
["Use % function to adjust for different gauges of steel studs.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(206,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / MarinoWARE / Viper Stud Viper 20 / 362-S-125-18, 20EQ gauge, \"2x4\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D122*$F122*IF($E$112=16,3.13,2.31)*VLOOKUP($C122,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D122*$F122*IF($E$112=16,3.13,2.31)*VLOOKUP($C122,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C122,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(209,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / Steel Recycling Institute /  / 362-S-125-18, 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D123*$F123*IF($E$112=16,3.13,2.31)*VLOOKUP($C123,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D123*$F123*IF($E$112=16,3.13,2.31)*VLOOKUP($C123,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C123,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(207,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / MBA Building Supplies /  / 362-S-125-18, 20EQ gauge, ProSTUD, ProTRAK"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D124*$F124*IF($E$112=16,3.13,2.31)*VLOOKUP($C124,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D124*$F124*IF($E$112=16,3.13,2.31)*VLOOKUP($C124,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C124,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(208,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / Scafco /  / 362VS125-18, 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D125*$F125*IF($E$112=16,3.13,2.31)*VLOOKUP($C125,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D125*$F125*IF($E$112=16,3.13,2.31)*VLOOKUP($C125,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C125,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(205,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / ClarkDietrich /  / 362-S-125-18, 20EQ gauge, \"2x4\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D126*$F126*IF($E$112=16,3.13,2.31)*VLOOKUP($C126,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D126*$F126*IF($E$112=16,3.13,2.31)*VLOOKUP($C126,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C126,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE STEEL FRAME WALLS"]
["STRUCTURAL SHEATHING",null,null,null,null,null,null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C127,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"ORIENTED STRAND BOARD",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C128,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(154,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K129-L129","v":0},"",{"$f":"$D129*$F129*VLOOKUP($C129,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D129*$F129*VLOOKUP($C129,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C129,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(155,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K130-L130","v":0},{"$f":"IF(H130=1,I130,\"\")","v":""},{"$f":"$D130*$F130*VLOOKUP($C130,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D130*$F130*VLOOKUP($C130,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C130,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(157,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / Huber  / ZIP System / 7/16\" Sheathing, protective barrier and tape"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K131-L131","v":0},{"$f":"IF(H131=1,I131,\"\")","v":""},{"$f":"$D131*$F131*VLOOKUP($C131,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D131*$F131*VLOOKUP($C131,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C131,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(156,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / Huber  / AdvanTech / 1/2\" Sheathing"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K132-L132","v":0},{"$f":"IF(H132=1,I132,\"\")","v":""},{"$f":"$D132*$F132*VLOOKUP($C132,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D132*$F132*VLOOKUP($C132,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C132,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WALL SHEATHING"]
[null,"PLYWOOD",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C133,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K134-L134","v":0},{"$f":"IF(H134=1,I134,\"\")","v":""},{"$f":"$D134*$F134*VLOOKUP($C134,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D134*$F134*VLOOKUP($C134,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C134,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C134,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(160,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K135-L135","v":0},{"$f":"IF(H135=1,I135,\"\")","v":""},{"$f":"$D135*$F135*VLOOKUP($C135,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D135*$F135*VLOOKUP($C135,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C135,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(161,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 3/4\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K136-L136","v":0},{"$f":"IF(H136=1,I136,\"\")","v":""},{"$f":"$D136*$F136*VLOOKUP($C136,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D136*$F136*VLOOKUP($C136,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C136,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WALL SHEATHING"]
[null,"GYPSUM STRUCTURAL SHEATHING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C137,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,"GARAGE WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(115,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D138*$F138*VLOOKUP($C138,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D138*$F138*VLOOKUP($C138,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C138,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(116,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / USG / Securock ExoAir 430 / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K139-L139","v":0},{"$f":"IF(H139=1,I139,\"\")","v":""},{"$f":"$D139*$F139*VLOOKUP($C139,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D139*$F139*VLOOKUP($C139,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C139,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WALL SHEATHING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(418,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / CertainTeed / GlasRoc Sheathing gypsum board / 5/8\" "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D140*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D140*$F140*VLOOKUP($C140,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C140,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WALL SHEATHING"]
["CMU EXTERIOR WALLS",null,null,null,null,null,null,null,null,{"$f":"IF(H141=1,I141,\"\")","v":""},null,null,{"$f":"IF(ISTEXT(VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C141,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"CMU 8\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C142,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Concrete Masonry Units - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K143-L143","v":0},{"$f":"IF(H143=1,I143,\"\")","v":""},{"$f":"F143*AVERAGE(K144:K149)","v":0},{"$f":"F143*AVERAGE(L144:L149)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C143,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CMU EXTERIOR WALLS"]
["Use % function to adjust for other thicknesses of CMU.",null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(48,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Canadian Concrete Masonry Producers Assn / 8\" Normal weight blocks / 390 x 190 x 190 mm"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K144-L144","v":0},"",{"$f":"$D144*$F144*VLOOKUP($C144,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D144*$F144*VLOOKUP($C144,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C144,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C144,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CMU EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(47,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Angelus Block Co. / 8\" Normal weight blocks / 8 x 8 x 16 Precision"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D145*$F145*VLOOKUP($C145,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D145*$F145*VLOOKUP($C145,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C145,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C145,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE CMU EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(49,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Permacon / 8\" Normal weight blocks / NW STD 20CM GLPW"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D146*$F146*VLOOKUP($C146,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D146*$F146*VLOOKUP($C146,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C146,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C146,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE CMU EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(46,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Canadian Concrete Masonry Producers Assn / 8\" Light weight blocks / 390 x 190 x 190 mm"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D147*$F147*VLOOKUP($C147,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D147*$F147*VLOOKUP($C147,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C147,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C147,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CMU EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(44,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Angelus Block Co. / 8\" Light weight blocks / 9 x 8 x 16 Precision"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D148*$F148*VLOOKUP($C148,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D148*$F148*VLOOKUP($C148,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C148,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C148,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE CMU EXTERIOR WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(45,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Brampton Brick / 8\" Carbon Cure Lightweight blocks / Carbon Cure 15 MPa"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D149*$F149*VLOOKUP($C149,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D149*$F149*VLOOKUP($C149,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C149,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C149,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE CMU EXTERIOR WALLS"]
["EXTERIOR GARAGE WALL CAVITY INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,"(Excludes attachment wall area, specified separately in section below)",null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C150,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C150,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"FIBERGLASS BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C151,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C151,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiberglass batt - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K152-L152","v":0},{"$f":"IF(H152=1,I152,\"\")","v":""},{"$f":"F152*AVERAGE(K153:K155)","v":0},{"$f":"F152*AVERAGE(L153:L155)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C152,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C152,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(104,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Owens Corning / EcoTouch Pink batt and roll / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K153-L153","v":0},{"$f":"IF(H153=1,I153,\"\")","v":""},{"$f":"$D153*($E$151/5.678)*$F153*VLOOKUP($C153,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D153*($E$151/5.678)*$F153*VLOOKUP($C153,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C153,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C153,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(102,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / CertainTeed / Sustainable Insulation / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D154*($E$151/5.678)*$F154*VLOOKUP($C154,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D154*($E$151/5.678)*$F154*VLOOKUP($C154,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C154,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C154,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(103,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Knauf / EcoBatt / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D155*($E$151/5.678)*$F155*VLOOKUP($C155,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D155*($E$151/5.678)*$F155*VLOOKUP($C155,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C155,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C155,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"FIBERGLASS BLOWN-IN",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C156,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C156,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,"Fiberglass loose fill - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K157-L157","v":0},{"$f":"IF(H157=1,I157,\"\")","v":""},{"$f":"F157*AVERAGE(K158:K161)","v":0},{"$f":"F157*AVERAGE(L158:L161)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C157,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C157,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(107,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Owens Corning / AttiCat, ProCat, ProPink / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D158*($E$156/5.678)*$F158*VLOOKUP($C158,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D158*($E$156/5.678)*$F158*VLOOKUP($C158,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C158,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C158,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(105,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / CertainTeed / InsulSafe, Optima, TruComfort / R 2.6/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D159*($E$156/5.678)*$F159*VLOOKUP($C159,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D159*($E$156/5.678)*$F159*VLOOKUP($C159,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C159,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C159,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(106,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Knauf / Jet Stream ULTRA / R 2.2/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K160-L160","v":0},{"$f":"IF(H160=1,I160,\"\")","v":""},{"$f":"$D160*($E$156/5.678)*$F160*VLOOKUP($C160,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D160*($E$156/5.678)*$F160*VLOOKUP($C160,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C160,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C160,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(374,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Johns Manville / Climate Pro, Attic Protector, JM Spider PLUS (Canada) / R 2.8/inch, Formaldehyde-free"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D161*($E$156/5.678)*$F161*VLOOKUP($C161,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D161*($E$156/5.678)*$F161*VLOOKUP($C161,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C161,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C161,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"MINERAL WOOL BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C162,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C162,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(147,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Owens Corning / Thermafiber UltraBatt / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D163*($E$162/5.678)*$F163*VLOOKUP($C163,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D163*($E$162/5.678)*$F163*VLOOKUP($C163,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C163,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C163,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(148,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / Safe'n'Sound, ComfortBatt / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K164-L164","v":0},{"$f":"IF(H164=1,I164,\"\")","v":""},{"$f":"$D164*($E$162/5.678)*$F164*VLOOKUP($C164,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D164*($E$162/5.678)*$F164*VLOOKUP($C164,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C164,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C164,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(402,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R14 / R 4.0/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D165*($E$162/5.678)*$F165*VLOOKUP($C165,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D165*($E$162/5.678)*$F165*VLOOKUP($C165,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C165,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C165,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(403,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R15 / R 4.3/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D166*($E$162/5.678)*$F166*VLOOKUP($C166,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D166*($E$162/5.678)*$F166*VLOOKUP($C166,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C166,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C166,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(404,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R22 / R 4.0/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D167*($E$162/5.678)*$F167*VLOOKUP($C167,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D167*($E$162/5.678)*$F167*VLOOKUP($C167,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C167,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C167,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(405,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 / R 4.4/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D168*($E$162/5.678)*$F168*VLOOKUP($C168,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D168*($E$162/5.678)*$F168*VLOOKUP($C168,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C168,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C168,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(406,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 SS / R 4.0/inch, 6\" Steel Studs"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D169*($E$162/5.678)*$F169*VLOOKUP($C169,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D169*($E$162/5.678)*$F169*VLOOKUP($C169,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C169,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C169,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"CELLULOSE INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C170,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C170,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,"Cellulose - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K171-L171","v":0},{"$f":"IF(H171=1,I171,\"\")","v":""},{"$f":"F171*AVERAGE(K172:K174)","v":0},{"$f":"F171*AVERAGE(L172:L174)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C171,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C171,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(33,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - dense pack /  / R 3.7/inch / Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K172-L172","v":0},{"$f":"IF(H172=1,I172,\"\")","v":""},{"$f":"$D172*($E$170/5.678)*$F172*VLOOKUP($C172,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D172*($E$170/5.678)*$F172*VLOOKUP($C172,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C172,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C172,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(32,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - batt / CMS / R 3.6/inch / EcoCell"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D173*($E$170/5.678)*$F173*VLOOKUP($C173,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D173*($E$170/5.678)*$F173*VLOOKUP($C173,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C173,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C173,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(35,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - spray applied / R 3.75/inch / International Cellulose Corp. / K-13, ThermoCon"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D174*($E$170/5.678)*$F174*VLOOKUP($C174,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D174*($E$170/5.678)*$F174*VLOOKUP($C174,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C174,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C174,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"WOOD FIBER BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C175,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C175,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,"Wood fiber batt - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K176-L176","v":0},{"$f":"IF(H176=1,I176,\"\")","v":""},{"$f":"F176*AVERAGE(K177:K180)","v":0},{"$f":"F176*AVERAGE(L177:L180)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C176,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C176,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(240,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Pavatex / Pavaflex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D177*($E$175/5.678)*$F177*VLOOKUP($C177,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D177*($E$175/5.678)*$F177*VLOOKUP($C177,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C177,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C177,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(239,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / GUTEX / ThermoFlex / R 4/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D178*($E$175/5.678)*$F178*VLOOKUP($C178,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D178*($E$175/5.678)*$F178*VLOOKUP($C178,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C178,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C178,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(241,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Steico / SteicoFlex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D179*($E$175/5.678)*$F179*VLOOKUP($C179,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D179*($E$175/5.678)*$F179*VLOOKUP($C179,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C179,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C179,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(238,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber - loose fill / GUTEX / ThermoFiber / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D180*($E$175/5.678)*$F180*VLOOKUP($C180,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D180*($E$175/5.678)*$F180*VLOOKUP($C180,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C180,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C180,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"OTHER NATURAL FIBER INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C181,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C181,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(254,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool batt / Havelock Wool /  / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K182-L182","v":0},{"$f":"IF(H182=1,I182,\"\")","v":""},{"$f":"$D182*($E$181/5.678)*$F182*VLOOKUP($C182,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D182*($E$181/5.678)*$F182*VLOOKUP($C182,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C182,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C182,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(255,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool loose fill / Havelock Wool /  / R 4.4/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K183-L183","v":0},{"$f":"IF(H183=1,I183,\"\")","v":""},{"$f":"$D183*($E$181/5.678)*$F183*VLOOKUP($C183,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D183*($E$181/5.678)*$F183*VLOOKUP($C183,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C183,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C183,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(121,'Master sheet'!$AL$1:$AL$441,0))","v":"Hemp fiber batt / NaturFibre / Hemp Wool / R 3.7/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K184-L184","v":0},{"$f":"IF(H184=1,I184,\"\")","v":""},{"$f":"$D184*($E$181/5.678)*$F184*VLOOKUP($C184,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D184*($E$181/5.678)*$F184*VLOOKUP($C184,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C184,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C184,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(210,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale /  / Wheat & rye straw / R 3.3/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K185-L185","v":0},{"$f":"IF(H185=1,I185,\"\")","v":""},{"$f":"$D185*($E$181/5.678)*$F185*VLOOKUP($C185,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D185*($E$181/5.678)*$F185*VLOOKUP($C185,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C185,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C185,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(412,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale / SNaB (UK) / Wheat & barley straw / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K186-L186","v":0},{"$f":"IF(H186=1,I186,\"\")","v":""},{"$f":"$D186*($E$181/5.678)*$F186*VLOOKUP($C186,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D186*($E$181/5.678)*$F186*VLOOKUP($C186,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C186,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C186,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"SPRAY FOAM, CLOSED CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C187,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C187,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(183,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K188-L188","v":0},{"$f":"IF(H188=1,I188,\"\")","v":""},{"$f":"$D188*($E$187/5.678)*$F188*VLOOKUP($C188,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D188*($E$187/5.678)*$F188*VLOOKUP($C188,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C188,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C188,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(184,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K189-L189","v":0},{"$f":"IF(H189=1,I189,\"\")","v":""},{"$f":"$D189*($E$187/5.678)*$F189*VLOOKUP($C189,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D189*($E$187/5.678)*$F189*VLOOKUP($C189,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C189,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C189,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(410,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K190-L190","v":0},{"$f":"IF(H190=1,I190,\"\")","v":""},{"$f":"$D190*($E$187/5.678)*$F190*VLOOKUP($C190,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D190*($E$187/5.678)*$F190*VLOOKUP($C190,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C190,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C190,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"SPRAY FOAM, OPEN CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C191,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C191,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(187,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell (HFC) / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K192-L192","v":0},{"$f":"IF(H192=1,I192,\"\")","v":""},{"$f":"$D192*($E$191/5.678)*$F192*VLOOKUP($C192,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D192*($E$191/5.678)*$F192*VLOOKUP($C192,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C192,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C192,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(188,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell - HFO gas / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K193-L193","v":0},{"$f":"IF(H193=1,I193,\"\")","v":""},{"$f":"$D193*($E$191/5.678)*$F193*VLOOKUP($C193,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D193*($E$191/5.678)*$F193*VLOOKUP($C193,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C193,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C193,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"HEMPCRETE",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C194,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C194,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,"Hempcrete - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K195-L195","v":0},{"$f":"IF(H195=1,I195,\"\")","v":""},{"$f":"F195*AVERAGE(K196:K198)","v":0},{"$f":"F195*AVERAGE(L196:L198)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C195,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C195,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(124,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / USA / R 2.1/inch, Avg. mix using NHL & PHL"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D196*($E$194/5.678)*$F196*VLOOKUP($C196,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D196*($E$194/5.678)*$F196*VLOOKUP($C196,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C196,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C196,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2020"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(123,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / Europe / R 2.1/inch, Avg. of 9 mixes"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D197*($E$194/5.678)*$F197*VLOOKUP($C197,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D197*($E$194/5.678)*$F197*VLOOKUP($C197,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C197,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C197,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2017"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(122,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / IsoHemp / Europe / R 2.1/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D198*($E$194/5.678)*$F198*VLOOKUP($C198,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D198*($E$194/5.678)*$F198*VLOOKUP($C198,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C198,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C198,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
["EXTERIOR GARAGE WALL RIGID INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,"(Excludes attachment wall area)",null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C199,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C199,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"EPS FOAM BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C200,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C200,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"EPS foam board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K201-L201","v":0},{"$f":"IF(H201=1,I201,\"\")","v":""},{"$f":"F201*AVERAGE(K202:K203)","v":0},{"$f":"F201*AVERAGE(L202:L203)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C201,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C201,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(94,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K202-L202","v":0},"",{"$f":"$D202*($E$200/5.678)*$F202*VLOOKUP($C202,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D202*($E$200/5.678)*$F202*VLOOKUP($C202,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C202,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C202,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(96,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board with graphite / BASF / Neopor / R 4.7/inch, Type II, 15 psi (Type 2, 110 kPa)"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D203*($E$200/5.678)*$F203*VLOOKUP($C203,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D203*($E$200/5.678)*$F203*VLOOKUP($C203,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C203,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C203,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"WOOD FIBER BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C204,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C204,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,"Wood fiber board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K205-L205","v":0},{"$f":"IF(H205=1,I205,\"\")","v":""},{"$f":"F205*AVERAGE(K206:K210)","v":0},{"$f":"F205*AVERAGE(L206:L210)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C205,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C205,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(242,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) Wood fiber board / AWC/CWC / Includes: Georgia Pacific, Louisville, BPC, Temple-Inland, Blue Ridge, Int'l Bildrite / R 2.7/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C206,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C206,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},"This is archived and can be deleted (BSUP)","GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(243,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / GUTEX / Multi-Therm / R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D207*($E$204/5.678)*$F207*VLOOKUP($C207,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D207*($E$204/5.678)*$F207*VLOOKUP($C207,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C207,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C207,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(244,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Pavatex / Pavatherm / R 3.4/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D208*($E$204/5.678)*$F208*VLOOKUP($C208,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D208*($E$204/5.678)*$F208*VLOOKUP($C208,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C208,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C208,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(245,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Steico / Special Dry / R 3.6/inch, 40, 120, 140, 160, 180, 200 mm"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K209-L209","v":0},{"$f":"IF(H209=1,I209,\"\")","v":""},{"$f":"$D209*($E$204/5.678)*$F209*VLOOKUP($C209,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D209*($E$204/5.678)*$F209*VLOOKUP($C209,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C209,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C209,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(397,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / North American Fiberboard Association / Includes: MSL, Blue Ridge Fiberboard Inc. / R 2.7/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D210*($E$204/5.678)*$F210*VLOOKUP($C210,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D210*($E$204/5.678)*$F210*VLOOKUP($C210,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C210,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C210,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"XPS FOAM BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C211,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C211,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,"XPS foam board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K212-L212","v":0},{"$f":"IF(H212=1,I212,\"\")","v":""},{"$f":"F212*AVERAGE(K213:K215)","v":0},{"$f":"F212*AVERAGE(L213:L215)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C212,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C212,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(258,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Owens Corning / Foamular NGX 250  / R 5/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K213-L213","v":0},{"$f":"IF(H213=1,I213,\"\")","v":""},{"$f":"$D213*($E$211/5.678)*$F213*VLOOKUP($C213,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D213*($E$211/5.678)*$F213*VLOOKUP($C213,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C213,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C213,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(401,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Soprema / SOPRA-XPS / R 5.0/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K214-L214","v":0},{"$f":"IF(H214=1,I214,\"\")","v":""},{"$f":"$D214*($E$211/5.678)*$F214*VLOOKUP($C214,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D214*($E$211/5.678)*$F214*VLOOKUP($C214,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C214,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C214,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(400,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / DuPont / Reduced GWP Grey Styrofoam™ (same as ST-100) / R 5.0/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K215-L215","v":0},{"$f":"IF(H215=1,I215,\"\")","v":""},{"$f":"$D215*($E$211/5.678)*$F215*VLOOKUP($C215,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D215*($E$211/5.678)*$F215*VLOOKUP($C215,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C215,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C215,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(399,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) XPS foam board / DuPont / Styrofoam (Grey, Reduced GWP) / R 5.6/inch"},null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C216,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C216,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},"This is archived and can be deleted (BSUP)","GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"POLYISOCYANURATE FOAM BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C217,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C217,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,"Polyisocyanurate - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K218-L218","v":0},{"$f":"IF(H218=1,I218,\"\")","v":""},{"$f":"F218*AVERAGE(K219:K222)","v":0},{"$f":"F218*AVERAGE(L219:L222)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C218,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C218,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(166,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / Dow Chemical Company / Tuff-R, Super Tuff-R, Thermax / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D219*($E$217/5.678)*$F219*VLOOKUP($C219,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D219*($E$217/5.678)*$F219*VLOOKUP($C219,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C219,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C219,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(167,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / Hunter / Polysio Wall insulation boards / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D220*($E$217/5.678)*$F220*VLOOKUP($C220,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D220*($E$217/5.678)*$F220*VLOOKUP($C220,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C220,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C220,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(408,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / DuPont / Thermax / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K221-L221","v":0},{"$f":"IF(H221=1,I221,\"\")","v":""},{"$f":"$D221*($E$217/5.678)*$F221*VLOOKUP($C221,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D221*($E$217/5.678)*$F221*VLOOKUP($C221,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C221,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C221,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(411,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / PIMA / Includes: Atlas, Firestone, GAF, Johns Manville, Rmax, Carlisle, Iko, Soprema / R 6.5/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D222*($E$217/5.678)*$F222*VLOOKUP($C222,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D222*($E$217/5.678)*$F222*VLOOKUP($C222,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C222,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C222,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,"MINERAL WOOL BOARD",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C223,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C223,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Mineral wool board - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K224-L224","v":0},{"$f":"IF(H224=1,I224,\"\")","v":""},{"$f":"F224*AVERAGE(K225:K227)","v":0},{"$f":"F224*AVERAGE(L225:L227)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C224,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C224,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(149,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board - heavy density / NAIMA / R 4.2/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D225*($E$223/5.678)*$F225*VLOOKUP($C225,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D225*($E$223/5.678)*$F225*VLOOKUP($C225,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C225,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C225,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(150,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board / Rockwool / Rockboard 60 / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K226-L226","v":0},{"$f":"IF(H226=1,I226,\"\")","v":""},{"$f":"$D226*($E$223/5.678)*$F226*VLOOKUP($C226,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D226*($E$223/5.678)*$F226*VLOOKUP($C226,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C226,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C226,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(407,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board  / Rockwool / Comfortboard 80 / R 4.2/inch"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D227*($E$223/5.678)*$F227*VLOOKUP($C227,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D227*($E$223/5.678)*$F227*VLOOKUP($C227,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C227,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C227,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","EXTERIOR GARAGE WALL INSULATION"]
["GARAGE ATTACHMENT WALL INSULATION"]
["GARAGE ATTACHMENT WALL CAVITY INSULATION",null,null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,null,null,"",null,null,{"$f":"IF(ISTEXT(VLOOKUP($C229,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C229,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"FIBERGLASS BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C230,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C230,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,"Fiberglass batt - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K231-L231","v":0},{"$f":"IF(H231=1,I231,\"\")","v":""},{"$f":"F231*AVERAGE(K232:K234)","v":0},{"$f":"F231*AVERAGE(L232:L234)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C231,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C231,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(104,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Owens Corning / EcoTouch Pink batt and roll / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K232-L232","v":0},{"$f":"IF(H232=1,I232,\"\")","v":""},{"$f":"$D232*($E$230/5.678)*$F232*VLOOKUP($C232,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D232*($E$230/5.678)*$F232*VLOOKUP($C232,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C232,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C232,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(102,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / CertainTeed / Sustainable Insulation / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D233*($E$230/5.678)*$F233*VLOOKUP($C233,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D233*($E$230/5.678)*$F233*VLOOKUP($C233,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C233,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C233,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(103,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Knauf / EcoBatt / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D234*($E$230/5.678)*$F234*VLOOKUP($C234,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D234*($E$230/5.678)*$F234*VLOOKUP($C234,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C234,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C234,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,"FIBERGLASS BLOWN-IN",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C235,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C235,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,"Fiberglass loose fill - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K236-L236","v":0},{"$f":"IF(H236=1,I236,\"\")","v":""},{"$f":"F236*AVERAGE(K237:K240)","v":0},{"$f":"F236*AVERAGE(L237:L240)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C236,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C236,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(107,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Owens Corning / AttiCat, ProCat, ProPink / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K237-L237","v":0},{"$f":"IF(H237=1,I237,\"\")","v":""},{"$f":"$D237*($E$235/5.678)*$F237*VLOOKUP($C237,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D237*($E$235/5.678)*$F237*VLOOKUP($C237,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C237,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C237,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(105,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / CertainTeed / InsulSafe, Optima, TruComfort / R 2.6/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D238*($E$235/5.678)*$F238*VLOOKUP($C238,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D238*($E$235/5.678)*$F238*VLOOKUP($C238,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C238,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C238,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(106,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Knauf / Jet Stream ULTRA / R 2.2/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K239-L239","v":0},{"$f":"IF(H239=1,I239,\"\")","v":""},{"$f":"$D239*($E$235/5.678)*$F239*VLOOKUP($C239,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D239*($E$235/5.678)*$F239*VLOOKUP($C239,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C239,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C239,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(374,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Johns Manville / Climate Pro, Attic Protector, JM Spider PLUS (Canada) / R 2.8/inch, Formaldehyde-free"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D240*($E$235/5.678)*$F240*VLOOKUP($C240,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D240*($E$235/5.678)*$F240*VLOOKUP($C240,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C240,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C240,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,"MINERAL WOOL BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C241,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C241,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(147,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Owens Corning / Thermafiber UltraBatt / R 4.3/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K242-L242","v":0},{"$f":"IF(H242=1,I242,\"\")","v":""},{"$f":"$D242*($E$241/5.678)*$F242*VLOOKUP($C242,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D242*($E$241/5.678)*$F242*VLOOKUP($C242,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C242,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C242,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(148,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / Safe'n'Sound, ComfortBatt / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K243-L243","v":0},{"$f":"IF(H243=1,I243,\"\")","v":""},{"$f":"$D243*($E$241/5.678)*$F243*VLOOKUP($C243,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D243*($E$241/5.678)*$F243*VLOOKUP($C243,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C243,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C243,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(402,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R14 / R 4.0/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D244*($E$241/5.678)*$F244*VLOOKUP($C244,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D244*($E$241/5.678)*$F244*VLOOKUP($C244,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C244,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C244,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(403,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R15 / R 4.3/inch, 3.5\""},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D245*($E$241/5.678)*$F245*VLOOKUP($C245,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D245*($E$241/5.678)*$F245*VLOOKUP($C245,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C245,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C245,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(404,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R22 / R 4.0/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D246*($E$241/5.678)*$F246*VLOOKUP($C246,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D246*($E$241/5.678)*$F246*VLOOKUP($C246,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C246,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C246,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(405,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 / R 4.4/inch, 5.5\""},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D247*($E$241/5.678)*$F247*VLOOKUP($C247,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D247*($E$241/5.678)*$F247*VLOOKUP($C247,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C247,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C247,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(406,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 SS / R 4.0/inch, 6\" Steel Studs"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D248*($E$241/5.678)*$F248*VLOOKUP($C248,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D248*($E$241/5.678)*$F248*VLOOKUP($C248,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C248,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C248,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,"CELLULOSE INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C249,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C249,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,"Cellulose - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K250-L250","v":0},{"$f":"IF(H250=1,I250,\"\")","v":""},{"$f":"F250*AVERAGE(K251:K253)","v":0},{"$f":"F250*AVERAGE(L251:L253)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C250,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C250,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(33,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - dense pack /  / R 3.7/inch / Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K251-L251","v":0},{"$f":"IF(H251=1,I251,\"\")","v":""},{"$f":"$D251*($E$249/5.678)*$F251*VLOOKUP($C251,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D251*($E$249/5.678)*$F251*VLOOKUP($C251,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C251,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C251,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(32,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - batt / CMS / R 3.6/inch / EcoCell"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D252*($E$249/5.678)*$F252*VLOOKUP($C252,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D252*($E$249/5.678)*$F252*VLOOKUP($C252,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C252,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C252,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(35,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - spray applied / R 3.75/inch / International Cellulose Corp. / K-13, ThermoCon"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D253*($E$249/5.678)*$F253*VLOOKUP($C253,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D253*($E$249/5.678)*$F253*VLOOKUP($C253,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C253,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C253,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,"WOOD FIBER BATT",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C254,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C254,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,"Wood fiber batt - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K255-L255","v":0},{"$f":"IF(H255=1,I255,\"\")","v":""},{"$f":"F255*AVERAGE(K256:K259)","v":0},{"$f":"F255*AVERAGE(L256:L259)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C255,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C255,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(240,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Pavatex / Pavaflex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K256-L256","v":0},{"$f":"IF(H256=1,I256,\"\")","v":""},{"$f":"$D256*($E$254/5.678)*$F256*VLOOKUP($C256,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D256*($E$254/5.678)*$F256*VLOOKUP($C256,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C256,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C256,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(239,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / GUTEX / ThermoFlex / R 4/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D257*($E$254/5.678)*$F257*VLOOKUP($C257,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D257*($E$254/5.678)*$F257*VLOOKUP($C257,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C257,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C257,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(241,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Steico / SteicoFlex / R 3.8/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D258*($E$254/5.678)*$F258*VLOOKUP($C258,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D258*($E$254/5.678)*$F258*VLOOKUP($C258,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C258,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C258,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(238,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber - loose fill / GUTEX / ThermoFiber / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D259*($E$254/5.678)*$F259*VLOOKUP($C259,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D259*($E$254/5.678)*$F259*VLOOKUP($C259,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C259,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C259,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,"OTHER NATURAL FIBER INSULATION",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C260,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C260,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(254,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool batt / Havelock Wool /  / R 3.6/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K261-L261","v":0},{"$f":"IF(H261=1,I261,\"\")","v":""},{"$f":"$D261*($E$260/5.678)*$F261*VLOOKUP($C261,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D261*($E$260/5.678)*$F261*VLOOKUP($C261,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C261,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C261,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(255,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool loose fill / Havelock Wool /  / R 4.4/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K262-L262","v":0},{"$f":"IF(H262=1,I262,\"\")","v":""},{"$f":"$D262*($E$260/5.678)*$F262*VLOOKUP($C262,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D262*($E$260/5.678)*$F262*VLOOKUP($C262,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C262,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C262,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(121,'Master sheet'!$AL$1:$AL$441,0))","v":"Hemp fiber batt / NaturFibre / Hemp Wool / R 3.7/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K263-L263","v":0},{"$f":"IF(H263=1,I263,\"\")","v":""},{"$f":"$D263*($E$260/5.678)*$F263*VLOOKUP($C263,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D263*($E$260/5.678)*$F263*VLOOKUP($C263,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C263,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C263,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA"},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(210,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale /  / Wheat & rye straw / R 3.3/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K264-L264","v":0},{"$f":"IF(H264=1,I264,\"\")","v":""},{"$f":"$D264*($E$260/5.678)*$F264*VLOOKUP($C264,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D264*($E$260/5.678)*$F264*VLOOKUP($C264,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C264,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C264,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(412,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale / SNaB (UK) / Wheat & barley straw / R 2.8/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K265-L265","v":0},{"$f":"IF(H265=1,I265,\"\")","v":""},{"$f":"$D265*($E$260/5.678)*$F265*VLOOKUP($C265,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D265*($E$260/5.678)*$F265*VLOOKUP($C265,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C265,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C265,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,"SPRAY FOAM, CLOSED CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C266,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C266,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(183,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K267-L267","v":0},{"$f":"IF(H267=1,I267,\"\")","v":""},{"$f":"$D267*($E$266/5.678)*$F267*VLOOKUP($C267,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D267*($E$266/5.678)*$F267*VLOOKUP($C267,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C267,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C267,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(184,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K268-L268","v":0},{"$f":"IF(H268=1,I268,\"\")","v":""},{"$f":"$D268*($E$266/5.678)*$F268*VLOOKUP($C268,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D268*($E$266/5.678)*$F268*VLOOKUP($C268,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C268,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C268,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(410,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / "},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K269-L269","v":0},{"$f":"IF(H269=1,I269,\"\")","v":""},{"$f":"$D269*($E$266/5.678)*$F269*VLOOKUP($C269,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D269*($E$266/5.678)*$F269*VLOOKUP($C269,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C269,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C269,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,"SPRAY FOAM, OPEN CELL",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C270,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C270,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(187,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell (HFC) / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K271-L271","v":0},{"$f":"IF(H271=1,I271,\"\")","v":""},{"$f":"$D271*($E$270/5.678)*$F271*VLOOKUP($C271,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D271*($E$270/5.678)*$F271*VLOOKUP($C271,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C271,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C271,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"A1-B1"},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(188,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell - HFO gas / SPFA /  / R 4.1/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K272-L272","v":0},{"$f":"IF(H272=1,I272,\"\")","v":""},{"$f":"$D272*($E$270/5.678)*$F272*VLOOKUP($C272,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D272*($E$270/5.678)*$F272*VLOOKUP($C272,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C272,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C272,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,"HEMPCRETE",null,"R-VALUE:",null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C273,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C273,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,"Hempcrete - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K274-L274","v":0},{"$f":"IF(H274=1,I274,\"\")","v":""},{"$f":"F274*AVERAGE(K275:K277)","v":0},{"$f":"F274*AVERAGE(L275:L277)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C274,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C274,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(124,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / USA / R 2.1/inch, Avg. mix using NHL & PHL"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,{"$f":"K275-L275","v":0},{"$f":"IF(H275=1,I275,\"\")","v":""},{"$f":"$D275*($E$273/5.678)*$F275*VLOOKUP($C275,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D275*($E$273/5.678)*$F275*VLOOKUP($C275,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C275,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C275,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2020"},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(123,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / Europe / R 2.1/inch, Avg. of 9 mixes"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D276*($E$273/5.678)*$F276*VLOOKUP($C276,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D276*($E$273/5.678)*$F276*VLOOKUP($C276,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C276,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C276,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2017"},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(122,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / IsoHemp / Europe / R 2.1/inch"},{"$f":"'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$31","v":"m2"},1,null,null,0,"",{"$f":"$D277*($E$273/5.678)*$F277*VLOOKUP($C277,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D277*($E$273/5.678)*$F277*VLOOKUP($C277,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C277,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C277,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"LCA"},null,"GARAGE","GARAGE ATTACHMENT WALL INSULATION"]
["GARAGE CLADDING"]
["EXTERIOR CLADDING"]
[null,"BRICK"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(23,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay, Generic Modular / Brick Industry Association / US-Canada Industry Average / 3-5/8\" x 2-3/4\" x 7-5/8\" incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K281-L281","v":0},{"$f":"IF(H281=1,I281,\"\")","v":""},{"$f":"$D281*$F281*VLOOKUP($C281,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D281*$F281*VLOOKUP($C281,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C281,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C281,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(19,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Calcium Silicate / Arriscraft / Contemporary Brick / 3-1/8\" x 3-1/2\" x any length, incl. mortar and ties"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D282*$F282*VLOOKUP($C282,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D282*$F282*VLOOKUP($C282,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C282,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C282,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(20,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Cement / MidWest / Architectural Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D283*$F283*VLOOKUP($C283,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D283*$F283*VLOOKUP($C283,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C283,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C283,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(21,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / Interstate / Avg Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D284*$F284*VLOOKUP($C284,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D284*$F284*VLOOKUP($C284,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C284,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C284,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(22,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / Interstate / Avg Thin Face Brick / 3-9/16\" x 5/8\" x 11-5/8\" (90 x 16 mm x 295) incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D285*$F285*VLOOKUP($C285,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D285*$F285*VLOOKUP($C285,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C285,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C285,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(388,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / SHAW / Slender - Thin Face Brick / 2 1/4\" x 1/2\" x 7-1/2\" (57 x 12.7 mm x 190) incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D286*$F286*VLOOKUP($C286,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D286*$F286*VLOOKUP($C286,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C286,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C286,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(389,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / SHAW / Avg Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D287*$F287*VLOOKUP($C287,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D287*$F287*VLOOKUP($C287,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C287,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C287,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"WOOD CLADDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C288,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C288,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,"3/4\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(31,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K289-L289","v":0},{"$f":"IF(H289=1,I289,\"\")","v":""},{"$f":"$D289*$F289*VLOOKUP($C289,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D289*$F289*VLOOKUP($C289,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C289,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C289,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"3/4\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K290-L290","v":0},{"$f":"IF(H290=1,I290,\"\")","v":""},{"$f":"$D290*$F290*VLOOKUP($C290,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D290*$F290*VLOOKUP($C290,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C290,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C290,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"FIBER CEMENT",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C291,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C291,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,null,"Fiber Cement siding - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K292-L292","v":0},{"$f":"IF(H292=1,I292,\"\")","v":""},{"$f":"F292*AVERAGE(K293:K300)","v":0},{"$f":"F292*AVERAGE(L293:L300)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C292,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C292,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"5/16\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(101,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Cembrit / Solid & Express / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D293*$F293*VLOOKUP($C293,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D293*$F293*VLOOKUP($C293,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C293,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C293,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"5/16\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(100,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Cembrit / Patina / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D294*$F294*VLOOKUP($C294,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D294*$F294*VLOOKUP($C294,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C294,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C294,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(384,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Equitone / Pictura and Natura Pro / 8 mm (5/16\")"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D295*$F295*VLOOKUP($C295,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D295*$F295*VLOOKUP($C295,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C295,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C295,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(385,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Equitone / Tectiva / 8 mm (5/16\")"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D296*$F296*VLOOKUP($C296,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D296*$F296*VLOOKUP($C296,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C296,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C296,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(386,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Equitone / Natura, Textura and Materia / 8 mm (5/16\")"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K297-L297","v":0},{"$f":"IF(H297=1,I297,\"\")","v":""},{"$f":"$D297*$F297*VLOOKUP($C297,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D297*$F297*VLOOKUP($C297,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C297,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C297,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(417,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / James Hardie / HardiePanel® / 8 mm"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D298*$F298*VLOOKUP($C298,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D298*$F298*VLOOKUP($C298,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C298,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C298,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(419,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / James Hardie / Hardie VL Plank / 11 mm"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D299*$F299*VLOOKUP($C299,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D299*$F299*VLOOKUP($C299,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C299,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C299,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(420,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / James Hardie / HardiePlank / 8 mm"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D300*$F300*VLOOKUP($C300,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D300*$F300*VLOOKUP($C300,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C300,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C300,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"VINYL SIDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C301,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C301,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(219,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl Siding / Vinyl Siding Institute / Double 4.5\" products from: American Original, Associated Materials, CertainTeed, Novik, Ply Gem / 0.040\" Double 4.5\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K302-L302","v":0},{"$f":"IF(H302=1,I302,\"\")","v":""},{"$f":"$D302*$F302*VLOOKUP($C302,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D302*$F302*VLOOKUP($C302,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C302,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C302,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"POLYPROPYLENE SIDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C303,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C303,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,"Polypropylene siding - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K304-L304","v":0},{"$f":"IF(H304=1,I304,\"\")","v":""},{"$f":"F304*AVERAGE(K305:K306)","v":0},{"$f":"F304*AVERAGE(L305:L306)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C304,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C304,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(169,'Master sheet'!$AL$1:$AL$441,0))","v":"Polypropylene siding / Novik / NovikStone, NovikShake / Avg of 5 products"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K305-L305","v":0},{"$f":"IF(H305=1,I305,\"\")","v":""},{"$f":"$D305*$F305*VLOOKUP($C305,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D305*$F305*VLOOKUP($C305,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C305,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C305,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(170,'Master sheet'!$AL$1:$AL$441,0))","v":"Polypropylene siding / Vinyl Siding Institute  /  / 0.085\" Single 7\" wood Shake appearance"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K306-L306","v":0},{"$f":"IF(H306=1,I306,\"\")","v":""},{"$f":"$D306*$F306*VLOOKUP($C306,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D306*$F306*VLOOKUP($C306,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C306,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C306,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"STEEL PANEL SIDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C307,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C307,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,"Steel Panel Siding - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K308-L308","v":0},{"$f":"IF(H308=1,I308,\"\")","v":""},{"$f":"F308*AVERAGE(K309:K314)","v":0},{"$f":"F308*AVERAGE(L309:L314)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C308,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C308,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(140,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / AEP Span / All products / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D309*$F309*VLOOKUP($C309,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D309*$F309*VLOOKUP($C309,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C309,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C309,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(141,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / ArcelorMittal / All products / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D310*$F310*VLOOKUP($C310,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D310*$F310*VLOOKUP($C310,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C310,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C310,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(142,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Canadian Sheet Steel Building Institute / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D311*$F311*VLOOKUP($C311,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D311*$F311*VLOOKUP($C311,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C311,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C311,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(143,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Metal Building Manufacturers Assn / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D312*$F312*VLOOKUP($C312,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D312*$F312*VLOOKUP($C312,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C312,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C312,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(144,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Metal Construction Assn. / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D313*$F313*VLOOKUP($C313,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D313*$F313*VLOOKUP($C313,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C313,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C313,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(145,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Petersen Aluminum Corp / PAC-CLAD / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D314*$F314*VLOOKUP($C314,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D314*$F314*VLOOKUP($C314,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C314,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C314,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"ALUMINUM PANEL SIDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C315,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C315,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,"Aluminum Panel Siding - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K316-L316","v":0},{"$f":"IF(H316=1,I316,\"\")","v":""},{"$f":"F316*AVERAGE(K317:K318)","v":0},{"$f":"F316*AVERAGE(L317:L318)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C316,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C316,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(138,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Aluminum / Metal Construction Assn. / 22 gauge / Includes: ATAS, DMI, Englert, Fabral,McElroy, Pac-Clad"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K317-L317","v":0},{"$f":"IF(H317=1,I317,\"\")","v":""},{"$f":"$D317*$F317*VLOOKUP($C317,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D317*$F317*VLOOKUP($C317,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C317,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C317,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(139,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Aluminum / Petersen Aluminum Corp / Pac-Clad / 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K318-L318","v":0},{"$f":"IF(H318=1,I318,\"\")","v":""},{"$f":"$D318*$F318*VLOOKUP($C318,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D318*$F318*VLOOKUP($C318,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C318,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C318,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"PLASTER FINISHES",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C319,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C319,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(129,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime Plaster / Mapei / MapeWall Muratura / 3/4\" Natural Hydraulic Lime (NHL)"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K320-L320","v":0},{"$f":"IF(H320=1,I320,\"\")","v":""},{"$f":"$D320*$F320*VLOOKUP($C320,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D320*$F320*VLOOKUP($C320,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C320,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C320,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(130,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime/Cork Plaster / Diasen / Diathonite Evolution / Exterior plaster cladding, 3/4\""},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K321-L321","v":0},{"$f":"IF(H321=1,I321,\"\")","v":""},{"$f":"$D321*$F321*VLOOKUP($C321,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D321*$F321*VLOOKUP($C321,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C321,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C321,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(42,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay plaster / Site mixed /  / 15 mm"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K322-L322","v":0},{"$f":"IF(H322=1,I322,\"\")","v":""},{"$f":"$D322*$F322*VLOOKUP($C322,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D322*$F322*VLOOKUP($C322,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C322,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C322,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2014"},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(212,'Master sheet'!$AL$1:$AL$441,0))","v":"Acrylic Stucco Textured Finish / Sto / Stolit 1.0, Stolit 1.5, Stolit Freeform / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K323-L323","v":0},{"$f":"IF(H323=1,I323,\"\")","v":""},{"$f":"$D323*$F323*VLOOKUP($C323,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D323*$F323*VLOOKUP($C323,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C323,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C323,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,"ENGINEERED WOOD SIDING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C324,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C324,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(413,'Master sheet'!$AL$1:$AL$441,0))","v":"Engineered Wood Siding & Trim / LP / SmartSide / 0.315\" (8 mm)"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K325-L325","v":0},{"$f":"IF(H325=1,I325,\"\")","v":""},{"$f":"$D325*$F325*VLOOKUP($C325,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D325*$F325*VLOOKUP($C325,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C325,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C325,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(414,'Master sheet'!$AL$1:$AL$441,0))","v":"Engineered Wood Siding & Trim / LP / SmartSide / 0.375\" (9.5 mm)"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K326-L326","v":0},{"$f":"IF(H326=1,I326,\"\")","v":""},{"$f":"$D326*$F326*VLOOKUP($C326,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D326*$F326*VLOOKUP($C326,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C326,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C326,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(415,'Master sheet'!$AL$1:$AL$441,0))","v":"Engineered Wood Siding & Trim / LP / SmartSide / 0.530\" (13.5 mm)"},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K327-L327","v":0},{"$f":"IF(H327=1,I327,\"\")","v":""},{"$f":"$D327*$F327*VLOOKUP($C327,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D327*$F327*VLOOKUP($C327,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C327,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C327,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE EXTERIOR CLADDING"]
["STRAPPING for RAIN SCREEN",null,null,"STRAPPING SPACING:",null,"in",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C328,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C328,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,"1x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K329-L329","v":0},{"$f":"IF(H329=1,I329,\"\")","v":""},{"$f":"$D329*$F329*IF($E$328=16,1/0.406,1/0.61)*VLOOKUP($C329,'Master sheet'!$A:$AJ,13,FALSE)*(0.0889*0.01905)","v":0},{"$f":"$D329*$F329*IF($E$328=16,1/0.406,1/0.61)*VLOOKUP($C329,'Master sheet'!$A:$AJ,27,FALSE)*(0.0889*0.01905)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C329,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C329,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE STRAPPING for RAIN SCREEN"]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$51","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K330-L330","v":0},{"$f":"IF(H330=1,I330,\"\")","v":""},{"$f":"$D330*$F330*IF($E$328=16,1/0.406,1/0.61)*VLOOKUP($C330,'Master sheet'!$A:$AJ,13,FALSE)*(0.0889*0.0381)","v":0},{"$f":"$D330*$F330*IF($E$328=16,1/0.406,1/0.61)*VLOOKUP($C330,'Master sheet'!$A:$AJ,27,FALSE)*(0.0889*0.0381)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C330,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C330,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE STRAPPING for RAIN SCREEN"]
["INTERIOR CLADDING of GARAGE WALLS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C331,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C331,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,"DRYWALL 1/2\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C332,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C332,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,null,"Drywall 1/2\" Typical - Interior Cladding for Exterior Walls - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K333-L333","v":0},{"$f":"IF(H333=1,I333,\"\")","v":""},{"$f":"F333*AVERAGE(K334:K338)","v":0},{"$f":"F333*AVERAGE(L334:L338)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C333,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C333,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(87,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / Easi-Lite / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K334-L334","v":0},{"$f":"IF(H334=1,I334,\"\")","v":""},{"$f":"$D334*$F334*VLOOKUP($C334,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D334*$F334*VLOOKUP($C334,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C334,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C334,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(86,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / AirRenew / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D335*$F335*VLOOKUP($C335,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D335*$F335*VLOOKUP($C335,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C335,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C335,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(88,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / M2Tech moisture resistant / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D336*$F336*VLOOKUP($C336,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D336*$F336*VLOOKUP($C336,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C336,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C336,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(89,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / Pabco / QuietRock / QuietRock 1/2\""},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K337-L337","v":0},{"$f":"IF(H337=1,I337,\"\")","v":""},{"$f":"$D337*$F337*VLOOKUP($C337,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D337*$F337*VLOOKUP($C337,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C337,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C337,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(376,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / National Gypsum / Gold Bond XP Gypsum Board  / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D338*$F338*VLOOKUP($C338,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D338*$F338*VLOOKUP($C338,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C338,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C338,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,"DRYWALL 5/8\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C339,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C339,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(90,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D340*$F340*VLOOKUP($C340,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D340*$F340*VLOOKUP($C340,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C340,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C340,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(91,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" / USG / EcoSmart Firecode / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D341*$F341*VLOOKUP($C341,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D341*$F341*VLOOKUP($C341,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C341,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C341,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(377,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" Type X / National Gypsum / Gold Bond XP Fire-Shield Gypsum Board  / 5/8'' type X"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K342-L342","v":0},{"$f":"IF(H342=1,I342,\"\")","v":""},{"$f":"$D342*$F342*VLOOKUP($C342,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D342*$F342*VLOOKUP($C342,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C342,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C342,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,"OTHER CLADDING MATERIALS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C343,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C343,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(146,'Master sheet'!$AL$1:$AL$441,0))","v":"MgO board 1/2\" / North American MgO / MagTech Ultra / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K344-L344","v":0},{"$f":"IF(H344=1,I344,\"\")","v":""},{"$f":"$D344*$F344*VLOOKUP($C344,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D344*$F344*VLOOKUP($C344,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C344,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C344,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,{"$f":"K345-L345","v":0},"",{"$f":"$D345*$F345*VLOOKUP($C345,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D345*$F345*VLOOKUP($C345,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C345,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C345,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(31,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D346*$F346*VLOOKUP($C346,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D346*$F346*VLOOKUP($C346,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C346,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C346,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(17,'Master sheet'!$AL$1:$AL$441,0))","v":"Bamboo plywood / Smith & Fong / Plyboo / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D347*$F347*VLOOKUP($C347,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D347*$F347*VLOOKUP($C347,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C347,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C347,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D348*$F348*VLOOKUP($C348,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D348*$F348*VLOOKUP($C348,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C348,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C348,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(253,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood wool boards / Armstrong / Tectum / 2\" (50.8 mm)"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D349*$F349*VLOOKUP($C349,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D349*$F349*VLOOKUP($C349,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C349,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C349,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(129,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime Plaster / Mapei / MapeWall Muratura / 3/4\" Natural Hydraulic Lime (NHL)"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D350*$F350*VLOOKUP($C350,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D350*$F350*VLOOKUP($C350,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C350,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C350,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(130,'Master sheet'!$AL$1:$AL$441,0))","v":"Lime/Cork Plaster / Diasen / Diathonite Evolution / Exterior plaster cladding, 3/4\""},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D351*$F351*VLOOKUP($C351,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D351*$F351*VLOOKUP($C351,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C351,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C351,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(42,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay plaster / Site mixed /  / 15 mm"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D352*$F352*VLOOKUP($C352,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D352*$F352*VLOOKUP($C352,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C352,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C352,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Peer-reviewed LCA, 2014"},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(41,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Tile Council of North America /  / Industry average. Includes porcelain, pressed, mosaic and quarry tile"},{"$f":"'USER INPUT SHEET'!$C$51+'USER INPUT SHEET'!$C$46","v":0},{"$f":"'USER INPUT SHEET'!$E$51","v":"m2"},1,null,null,0,"",{"$f":"$D353*$F353*VLOOKUP($C353,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D353*$F353*VLOOKUP($C353,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C353,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C353,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","INTERIOR CLADDING of GARAGE WALLS"]
["GARAGE WINDOWS"]
["DOUBLE PANE WINDOWS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(222,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Fiberglass frame /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$52","v":0},{"$f":"'USER INPUT SHEET'!$E$52","v":"m2"},1,null,null,{"$f":"K356-L356","v":0},{"$f":"IF(H356=1,I356,\"\")","v":""},{"$f":"$D356*$F356*VLOOKUP($C356,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D356*$F356*VLOOKUP($C356,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C356,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C356,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"GARAGE","GARAGE WINDOWS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(224,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Vinyl frame /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$52","v":0},{"$f":"'USER INPUT SHEET'!$E$52","v":"m2"},1,null,null,0,"",{"$f":"$D357*$F357*VLOOKUP($C357,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D357*$F357*VLOOKUP($C357,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C357,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C357,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"GARAGE","GARAGE WINDOWS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(225,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame /  / EU"},{"$f":"'USER INPUT SHEET'!$C$52","v":0},{"$f":"'USER INPUT SHEET'!$E$52","v":"m2"},1,null,null,0,"",{"$f":"$D358*$F358*VLOOKUP($C358,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D358*$F358*VLOOKUP($C358,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C358,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C358,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WINDOWS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(226,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$52","v":0},{"$f":"'USER INPUT SHEET'!$E$52","v":"m2"},1,null,null,0,"",{"$f":"$D359*$F359*VLOOKUP($C359,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D359*$F359*VLOOKUP($C359,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C359,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C359,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"GARAGE","GARAGE WINDOWS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(227,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame, aluminum cladding /  / EU"},{"$f":"'USER INPUT SHEET'!$C$52","v":0},{"$f":"'USER INPUT SHEET'!$E$52","v":"m2"},1,null,null,0,"",{"$f":"$D360*$F360*VLOOKUP($C360,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D360*$F360*VLOOKUP($C360,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C360,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C360,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"GARAGE","GARAGE WINDOWS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(228,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame, aluminum cladding /  / USA & CAN"},{"$f":"'USER INPUT SHEET'!$C$52","v":0},{"$f":"'USER INPUT SHEET'!$E$52","v":"m2"},1,null,null,{"$f":"K361-L361","v":0},{"$f":"IF(H361=1,I361,\"\")","v":""},{"$f":"$D361*$F361*VLOOKUP($C361,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D361*$F361*VLOOKUP($C361,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C361,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C361,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"BfCA Study (Tally)"},null,"GARAGE","GARAGE WINDOWS"]
["WINDOWS - SPECIFIC MANUFACTURERS",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C362,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C362,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(375,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Andersen / E-series (Average Double-hung/Awning/Picture) / Wood frame, aluminum cladding"},{"$f":"'USER INPUT SHEET'!$C$52","v":0},{"$f":"'USER INPUT SHEET'!$E$52","v":"m2"},1,null,null,{"$f":"K363-L363","v":0},{"$f":"IF(H363=1,I363,\"\")","v":""},{"$f":"$D363*$F363*VLOOKUP($C363,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D363*$F363*VLOOKUP($C363,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C363,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C363,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WINDOWS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(416,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Inline Fiberglass / 300 Series Tilt and Turn, 300 Series Fixed, 325 Series Awning/Casement, 325 Series Fixed, and 400 Series / Fiberglass frame"},{"$f":"'USER INPUT SHEET'!$C$52","v":0},{"$f":"'USER INPUT SHEET'!$E$52","v":"m2"},1,null,null,0,"",{"$f":"$D364*$F364*VLOOKUP($C364,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D364*$F364*VLOOKUP($C364,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C364,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C364,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WINDOWS"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(223,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Andersen / Fibrex / PVC & Wood composite / USA"},{"$f":"'USER INPUT SHEET'!$C$52","v":0},{"$f":"'USER INPUT SHEET'!$E$52","v":"m2"},1,null,null,{"$f":"K365-L365","v":0},{"$f":"IF(H365=1,I365,\"\")","v":""},{"$f":"$D365*$F365*VLOOKUP($C365,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D365*$F365*VLOOKUP($C365,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C365,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C365,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE WINDOWS"]
["GARAGE CEILING"]
["GARAGE CEILING CLADDING",null,null,null,null,null,null,null,null,null,null,null,null,null,"GARAGE"]
[null,"DRYWALL 1/2\"",null,null,null,null,null,null,null,null,null,null,null,null,"GARAGE"]
[null,null,"Drywall 1/2\" - Ceilings - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,{"$f":"K369-L369","v":0},{"$f":"IF(H369=1,I369,\"\")","v":""},{"$f":"F369*AVERAGE(K370:K374)","v":0},{"$f":"F369*AVERAGE(L370:L374)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C369,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C369,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(87,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / Easi-Lite / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,{"$f":"K370-L370","v":0},{"$f":"IF(H370=1,I370,\"\")","v":""},{"$f":"$D370*$F370*VLOOKUP($C370,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D370*$F370*VLOOKUP($C370,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C370,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C370,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(86,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / AirRenew / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,0,"",{"$f":"$D371*$F371*VLOOKUP($C371,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D371*$F371*VLOOKUP($C371,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C371,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C371,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(88,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / M2Tech moisture resistant / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,0,"",{"$f":"$D372*$F372*VLOOKUP($C372,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D372*$F372*VLOOKUP($C372,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C372,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C372,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(89,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / Pabco / QuietRock / QuietRock 1/2\""},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,{"$f":"K373-L373","v":0},{"$f":"IF(H373=1,I373,\"\")","v":""},{"$f":"$D373*$F373*VLOOKUP($C373,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D373*$F373*VLOOKUP($C373,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C373,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C373,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(376,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / National Gypsum / Gold Bond XP Gypsum Board  / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,0,"",{"$f":"$D374*$F374*VLOOKUP($C374,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D374*$F374*VLOOKUP($C374,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C374,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C374,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,"DRYWALL 5/8\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C375,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C375,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,null,"Drywall 5/8\" - Ceilings - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,{"$f":"K376-L376","v":0},{"$f":"IF(H376=1,I376,\"\")","v":""},{"$f":"F376*AVERAGE(K377:K379)","v":0},{"$f":"F376*AVERAGE(L377:L379)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C376,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C376,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(90,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,0,"",{"$f":"$D377*$F377*VLOOKUP($C377,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D377*$F377*VLOOKUP($C377,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C377,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C377,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(91,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" / USG / EcoSmart Firecode / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,0,"",{"$f":"$D378*$F378*VLOOKUP($C378,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D378*$F378*VLOOKUP($C378,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C378,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C378,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(377,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" Type X / National Gypsum / Gold Bond XP Fire-Shield Gypsum Board  / 5/8'' type X"},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,{"$f":"K379-L379","v":0},{"$f":"IF(H379=1,I379,\"\")","v":""},{"$f":"$D379*$F379*VLOOKUP($C379,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D379*$F379*VLOOKUP($C379,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C379,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C379,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,"OTHER CEILING FINISHES",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C380,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C380,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(146,'Master sheet'!$AL$1:$AL$441,0))","v":"MgO board 1/2\" / North American MgO / MagTech Ultra / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,{"$f":"K381-L381","v":0},{"$f":"IF(H381=1,I381,\"\")","v":""},{"$f":"$D381*$F381*VLOOKUP($C381,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D381*$F381*VLOOKUP($C381,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C381,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C381,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(31,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards"},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,0,"",{"$f":"$D382*$F382*VLOOKUP($C382,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D382*$F382*VLOOKUP($C382,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C382,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C382,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,"3/4\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,0,"",{"$f":"$D383*$F383*VLOOKUP($C383,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D383*$F383*VLOOKUP($C383,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C383,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C383,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(17,'Master sheet'!$AL$1:$AL$441,0))","v":"Bamboo plywood / Smith & Fong / Plyboo / 1/2\" (12.7 mm)"},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,0,"",{"$f":"$D384*$F384*VLOOKUP($C384,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D384*$F384*VLOOKUP($C384,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C384,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C384,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,0,"",{"$f":"$D385*$F385*VLOOKUP($C385,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D385*$F385*VLOOKUP($C385,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C385,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C385,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE CEILING CLADDING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(253,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood wool boards / Armstrong / Tectum / 2\" (50.8 mm)"},{"$f":"'USER INPUT SHEET'!$C$53","v":0},{"$f":"'USER INPUT SHEET'!$E$53","v":"m2"},1,null,null,0,"",{"$f":"$D386*$F386*VLOOKUP($C386,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D386*$F386*VLOOKUP($C386,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C386,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C386,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE CEILING CLADDING"]
["GARAGE ROOF"]
["WOOD FRAME CONSTRUCTION",null,null,"FRAMING SPACING:",null,"in",null,null,null,null,null,null,null,null,"GARAGE"]
[null,"WOOD FRAMING",null,null,null,null,null,null,null,null,null,null,null,null,"GARAGE"]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K390-L390","v":0},{"$f":"IF(H390=1,I390,\"\")","v":""},{"$f":"$D390*$F390*IF($E$388=16,0.25,0.22)*VLOOKUP($C390,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*3.5)","v":0},{"$f":"$D390*$F390*IF($E$388=16,0.25,0.22)*VLOOKUP($C390,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*3.5)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C390,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C390,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,"2x6",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K391-L391","v":0},{"$f":"IF(H391=1,I391,\"\")","v":""},{"$f":"$D391*$F391*IF($E$388=16,0.25,0.22)*VLOOKUP($C391,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*5.5)","v":0},{"$f":"$D391*$F391*IF($E$388=16,0.25,0.22)*VLOOKUP($C391,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*5.5)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C391,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C391,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,"2x8",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K392-L392","v":0},{"$f":"IF(H392=1,I392,\"\")","v":""},{"$f":"$D392*$F392*IF($E$388=16,0.25,0.22)*VLOOKUP($C392,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*7.25)","v":0},{"$f":"$D392*$F392*IF($E$388=16,0.25,0.22)*VLOOKUP($C392,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*7.25)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C392,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C392,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,"2x10",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K393-L393","v":0},{"$f":"IF(H393=1,I393,\"\")","v":""},{"$f":"$D393*$F393*IF($E$388=16,0.25,0.22)*VLOOKUP($C393,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*9.25)","v":0},{"$f":"$D393*$F393*IF($E$388=16,0.25,0.22)*VLOOKUP($C393,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*9.25)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C393,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C393,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,"2x12",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K394-L394","v":0},{"$f":"IF(H394=1,I394,\"\")","v":""},{"$f":"$D394*$F394*IF($E$388=16,0.25,0.22)*VLOOKUP($C394,'Master sheet'!$A:$AJ,13,FALSE)*(0.0254*11.25)","v":0},{"$f":"$D394*$F394*IF($E$388=16,0.25,0.22)*VLOOKUP($C394,'Master sheet'!$A:$AJ,27,FALSE)*(0.0254*11.25)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C394,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C394,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,"WOOD TRUSS FRAMING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C395,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C395,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(252,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood roof truss - prefabricated / Quebec Wood Export Bureau / Common (Double Howe) Gabrel Roof / 2x6 Chords, 2x4 Webs, 4:12 Pitch, 40 ft span, 20\" overhang"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K396-L396","v":0},{"$f":"IF(H396=1,I396,\"\")","v":""},{"$f":"$D396*$F396*IF($E$5=16,2.46, 1.64)*VLOOKUP($C396,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D396*$F396*IF($E$5=16,2.46, 1.64)*VLOOKUP($C396,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C396,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C396,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,"WOOD I-JOIST FRAMING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C397,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C397,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,"9-1/2\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D398*$F398*IF($E$5=16,2.46,1.64)*VLOOKUP($C398,'Master sheet'!$A:$AJ,13,FALSE)*0.926","v":0},{"$f":"$D398*$F398*IF($E$5=16,2.46,1.64)*VLOOKUP($C398,'Master sheet'!$A:$AJ,27,FALSE)*0.926","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C398,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C398,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,"11-7/8\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D399*$F399*IF($E$5=16,2.46,1.64)*VLOOKUP($C399,'Master sheet'!$A:$AJ,13,FALSE)*1.029","v":0},{"$f":"$D399*$F399*IF($E$5=16,2.46,1.64)*VLOOKUP($C399,'Master sheet'!$A:$AJ,27,FALSE)*1.029","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C399,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C399,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,"14\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D400*$F400*IF($E$5=16,2.46,1.64)*VLOOKUP($C400,'Master sheet'!$A:$AJ,13,FALSE)*1.132","v":0},{"$f":"$D400*$F400*IF($E$5=16,2.46,1.64)*VLOOKUP($C400,'Master sheet'!$A:$AJ,27,FALSE)*1.132","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C400,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C400,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
[null,"16\"",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D401*$F401*IF($E$5=16,2.46,1.64)*VLOOKUP($C401,'Master sheet'!$A:$AJ,13,FALSE)*1.2","v":0},{"$f":"$D401*$F401*IF($E$5=16,2.46,1.64)*VLOOKUP($C401,'Master sheet'!$A:$AJ,27,FALSE)*1.2","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C401,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C401,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE WOOD ROOF FRAMING"]
["ROOF DECKING",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C402,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C402,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"WOOD SHEET PRODUCTS - 5/8\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C403,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C403,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(160,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K404-L404","v":0},{"$f":"IF(H404=1,I404,\"\")","v":""},{"$f":"$D404*$F404*VLOOKUP($C404,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D404*$F404*VLOOKUP($C404,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C404,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C404,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOF DECKING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(155,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 5/8\""},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K405-L405","v":0},{"$f":"IF(H405=1,I405,\"\")","v":""},{"$f":"$D405*$F405*VLOOKUP($C405,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D405*$F405*VLOOKUP($C405,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C405,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C405,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOF DECKING"]
[null,"GYPSUM PANELS 1/2\"",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C406,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C406,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(115,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K407-L407","v":0},{"$f":"IF(H407=1,I407,\"\")","v":""},{"$f":"$D407*$F407*VLOOKUP($C407,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D407*$F407*VLOOKUP($C407,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C407,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C407,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE ROOF DECKING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(116,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / USG / Securock ExoAir 430 / 1/2\""},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K408-L408","v":0},{"$f":"IF(H408=1,I408,\"\")","v":""},{"$f":"$D408*$F408*VLOOKUP($C408,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D408*$F408*VLOOKUP($C408,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C408,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C408,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOF DECKING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(418,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / CertainTeed / GlasRoc Sheathing gypsum board / 5/8\" "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K409-L409","v":0},{"$f":"IF(H409=1,I409,\"\")","v":""},{"$f":"$D409*$F409*VLOOKUP($C409,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D409*$F409*VLOOKUP($C409,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C409,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C409,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOF DECKING"]
["ROOFING MEMBRANE",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C410,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C410,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"ROOFING MEMBRANE",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C411,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C411,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(92,'Master sheet'!$AL$1:$AL$441,0))","v":"EPDM Roofing Membrane / SPRI /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K412-L412","v":0},{"$f":"IF(H412=1,I412,\"\")","v":""},{"$f":"$D412*$F412*VLOOKUP($C412,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D412*$F412*VLOOKUP($C412,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C412,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C412,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE ROOFING MEMBRANE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(180,'Master sheet'!$AL$1:$AL$441,0))","v":"SBS Modified Bitumen Roofing / ARMA / Includes: CertainTeed, Firestone, GAF, Henry, IKO, Johns Mansville, Malarkey, Siplast, Soprema / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K413-L413","v":0},{"$f":"IF(H413=1,I413,\"\")","v":""},{"$f":"$D413*$F413*VLOOKUP($C413,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D413*$F413*VLOOKUP($C413,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C413,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C413,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE ROOFING MEMBRANE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(172,'Master sheet'!$AL$1:$AL$441,0))","v":"PVC Roofing Membrane / CIFA / Includes: Canadian General-Tower, Duro-Last, FiberTite / 48 mils"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K414-L414","v":0},{"$f":"IF(H414=1,I414,\"\")","v":""},{"$f":"$D414*$F414*VLOOKUP($C414,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D414*$F414*VLOOKUP($C414,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C414,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C414,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"GARAGE","GARAGE ROOFING MEMBRANE"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(213,'Master sheet'!$AL$1:$AL$441,0))","v":"TPO Roofing Membrane / Carlisle /  / 60 mils"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K415-L415","v":0},{"$f":"IF(H415=1,I415,\"\")","v":""},{"$f":"$D415*$F415*VLOOKUP($C415,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D415*$F415*VLOOKUP($C415,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C415,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C415,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE ROOFING MEMBRANE"]
["ROOF STRAPPING",null,null,"STRAPPING SPACING:",null,"in",null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C416,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C416,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,"WOOD STRAPPING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C417,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C417,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,"1x3",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K418-L418","v":0},{"$f":"IF(H418=1,I418,\"\")","v":""},{"$f":"$D418*$F418*IF($E$416=16,2.5/16,2.5/24)*VLOOKUP($C418,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D418*$F418*IF($E$416=16,2.5/16,2.5/24)*VLOOKUP($C418,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C418,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C418,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOF STRAPPING"]
[null,"1x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K419-L419","v":0},{"$f":"IF(H419=1,I419,\"\")","v":""},{"$f":"$D419*$F419*IF($E$416=16,3.5/16,3.5/24)*VLOOKUP($C419,'Master sheet'!$A:$AJ,13,FALSE)*0.01905","v":0},{"$f":"$D419*$F419*IF($E$416=16,3.5/16,3.5/24)*VLOOKUP($C419,'Master sheet'!$A:$AJ,27,FALSE)*0.01905","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C419,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C419,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOF STRAPPING"]
[null,"2x4",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K420-L420","v":0},{"$f":"IF(H420=1,I420,\"\")","v":""},{"$f":"$D420*$F420*IF($E$416=16,3.5/16,3.5/24)*VLOOKUP($C420,'Master sheet'!$A:$AJ,13,FALSE)*0.0381","v":0},{"$f":"$D420*$F420*IF($E$416=16,3.5/16,3.5/24)*VLOOKUP($C420,'Master sheet'!$A:$AJ,27,FALSE)*0.0381","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C420,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C420,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOF STRAPPING"]
["ROOFING",null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C421,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C421,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,"ASPHALT SHINGLES",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C422,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C422,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE"]
[null,null,"Asphalt Shingles - Roofing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K423-L423","v":0},{"$f":"IF(H423=1,I423,\"\")","v":""},{"$f":"F423*AVERAGE(K424:K429)","v":0},{"$f":"F423*AVERAGE(L424:L429)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C423,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C423,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(12,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Includes: Atlas, BP, CertainTeed, GAF, IKO, Malarkey, Owens Corning, Pabco /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K424-L424","v":0},{"$f":"IF(H424=1,I424,\"\")","v":""},{"$f":"$D424*$F424*VLOOKUP($C424,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D424*$F424*VLOOKUP($C424,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C424,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C424,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(14,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Owens Corning / Duration / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D425*$F425*VLOOKUP($C425,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D425*$F425*VLOOKUP($C425,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C425,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C425,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(15,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Owens Corning / Oakridge / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K426-L426","v":0},{"$f":"IF(H426=1,I426,\"\")","v":""},{"$f":"$D426*$F426*VLOOKUP($C426,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D426*$F426*VLOOKUP($C426,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C426,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C426,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(16,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Owens Corning / Supreme / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D427*$F427*VLOOKUP($C427,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D427*$F427*VLOOKUP($C427,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C427,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C427,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(13,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / GAF / Timberline / Timberline"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K428-L428","v":0},{"$f":"IF(H428=1,I428,\"\")","v":""},{"$f":"$D428*$F428*VLOOKUP($C428,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D428*$F428*VLOOKUP($C428,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C428,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C428,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(380,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / GAF / Timberline Cool Series / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D429*$F429*VLOOKUP($C429,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D429*$F429*VLOOKUP($C429,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C429,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C429,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,"STEEL PANELS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C430,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C430,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,"Steel Panels - Roofing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K431-L431","v":0},{"$f":"IF(H431=1,I431,\"\")","v":""},{"$f":"F431*AVERAGE(K432:K436)","v":0},{"$f":"F431*AVERAGE(L432:L436)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C431,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C431,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(141,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / ArcelorMittal / All products / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D432*$F432*VLOOKUP($C432,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D432*$F432*VLOOKUP($C432,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C432,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C432,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(142,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Canadian Sheet Steel Building Institute / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D433*$F433*VLOOKUP($C433,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D433*$F433*VLOOKUP($C433,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C433,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C433,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(143,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Metal Building Manufacturers Assn / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D434*$F434*VLOOKUP($C434,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D434*$F434*VLOOKUP($C434,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C434,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C434,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(144,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Metal Construction Assn. / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K435-L435","v":0},{"$f":"IF(H435=1,I435,\"\")","v":""},{"$f":"$D435*$F435*VLOOKUP($C435,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D435*$F435*VLOOKUP($C435,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C435,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C435,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(145,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Petersen Aluminum Corp / PAC-CLAD / 24 gauge"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K436-L436","v":0},{"$f":"IF(H436=1,I436,\"\")","v":""},{"$f":"$D436*$F436*VLOOKUP($C436,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D436*$F436*VLOOKUP($C436,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C436,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C436,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE ROOFING"]
[null,"ALUMINUM PANELS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C437,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C437,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,"Aluminum l Panels - Roofing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K438-L438","v":0},{"$f":"IF(H438=1,I438,\"\")","v":""},{"$f":"F438*AVERAGE(K439:K440)","v":0},{"$f":"F438*AVERAGE(L439:L440)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C438,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C438,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(138,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Aluminum / Metal Construction Assn. / 22 gauge / Includes: ATAS, DMI, Englert, Fabral,McElroy, Pac-Clad"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D439*$F439*VLOOKUP($C439,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D439*$F439*VLOOKUP($C439,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C439,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C439,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(139,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Aluminum / Petersen Aluminum Corp / Pac-Clad / 20EQ gauge"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D440*$F440*VLOOKUP($C440,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D440*$F440*VLOOKUP($C440,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C440,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C440,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2020"},null,"GARAGE","GARAGE ROOFING"]
[null,"FIBER CEMENT ROOFING",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C441,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C441,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,"Fiber Cement roofing - AVERAGE",{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K442-L442","v":0},{"$f":"IF(H442=1,I442,\"\")","v":""},{"$f":"F442*AVERAGE(K443:K445)","v":0},{"$f":"F442*AVERAGE(L443:L445)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C442,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C442,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(97,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement roofing / Cembrit / Corrugated sheets / 6.5 mm"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D443*$F443*VLOOKUP($C443,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D443*$F443*VLOOKUP($C443,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C443,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C443,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(98,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement roofing / Cembrit / Slates / 4 mm"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D444*$F444*VLOOKUP($C444,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D444*$F444*VLOOKUP($C444,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C444,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C444,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2021"},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(99,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement roofing / Mahaphant / Fibre-Cement / 5 mm"},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,0,"",{"$f":"$D445*$F445*VLOOKUP($C445,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D445*$F445*VLOOKUP($C445,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C445,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C445,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2019"},null,"GARAGE","GARAGE ROOFING"]
[null,"OTHER ROOFING OPTIONS",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($C446,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C446,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"GARAGE","GARAGE ROOFING"]
[null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(43,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay roof tiles / HISPALYT /  / "},{"$f":"'USER INPUT SHEET'!$C$54","v":0},{"$f":"'USER INPUT SHEET'!$E$36","v":"m2"},1,null,null,{"$f":"K447-L447","v":0},{"$f":"IF(H447=1,I447,\"\")","v":""},{"$f":"$D447*$F447*VLOOKUP($C447,'Master sheet'!$A:$AJ,13,FALSE)","v":0},{"$f":"$D447*$F447*VLOOKUP($C447,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"IF(ISTEXT(VLOOKUP($C447,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($C447,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":"Expired 2022"},null,"GARAGE","GARAGE ROOFING"]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"User-Defined","index":21,"n_rows":31,"n_cols":20,"rows_kept":31,"cut":false,"hidden":false,"merged":[[27,1,27,4],[2,10,3,10],[2,11,3,11],[2,12,3,12],[5,2,5,3],[26,1,26,2],[7,1,7,2],[8,1,8,2],[10,1,10,2],[14,1,14,2],[15,1,15,2],[12,1,12,2],[16,1,16,2],[11,1,11,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[1,13,1,14],[0,4,0,12],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[1,1,1,4],[1,5,1,12],[2,9,3,9],[0,0,0,3],[2,0,3,2],[4,0,4,3],[21,0,21,3],[9,2,9,3],[13,2,13,3],[17,2,17,3],[6,1,6,2]]}
["SECTION 14 ➜ COMPONENT MATERIALS FOR",null,null,null,"USER-DEFINED MATERIALS"]
[null,"INSTRUCTIONS FOR USING AN EXISTING DATABASE MATERIAL:         << double-click >>\n- Select material from LIGHT YELLOW DROPDOWN CELL (column C) matching the units of measurement for the material (volume, area, length, or R-value & area)\n- Enter all required inputs into DARK YELLOW cells for that row, including '1' in select column.\n- If adding insulation, enter its total R-VALUE (I-P units) in column B & surface area in column D.  \n\n",null,null,null,"INSTRUCTIONS FOR ADDING A MATERIAL NOT IN THE DATABASE: \n(user must know all required information)\nIn a row with CUSTOM as the category, ENTER CUSTOM DATA into all DARK YELLOW fields (CATEGORY, MATERIAL, QUANITY, UNIT, %, kgCO2e EMISSIONS, kgCO2e STORAGE). \n- Only use A1-A3 values from EPDs.\n- Changing the category name does not move the entry to another building section total.",null,null,null,null,null,null,null,"Caution: Any user-defined options that have not been validated and approved will reduce the reliability of results. "]
["CATEGORY",null,null,"MATERIAL","QUANTITY","UNIT","%",null,"SELECT","NET kgCO2e EMISSIONS","SELECTED MATERIAL kgCO2e CONTENT","kgCO2e EMISSIONS","kgCO2 STORAGE","kgCO2e SUBTOTAL FOR USER-DEFINED MATERIALS"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"SUMIF(A:A,\"\",K:K)","v":0}]
["EXISTING DATABASE MATERIALS"]
[null,null,"MATERIALS BY VOLUME",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($D6,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D6,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,null,null,null,"Material Index"]
[null,"VOLUME",null,null,null,"m3",1,null,null,{"$f":"L7-M7","v":{"$error":"#N/A"}},{"$f":"IF(I7=1,J7,\"\")","v":""},{"$f":"$E7*$G7*VLOOKUP($D7,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$E7*$G7*VLOOKUP($D7,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D7,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D7,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A7)>0, $A7,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D7,'Dropdown Lists'!$E$2:$E$143,0), \"\") & \",\" & CELL(\"col\", 'Dropdown Lists'!$E$2)","v":",5"},",5"]
[null,"VOLUME",null,null,null,"m3",1,null,null,{"$error":"#N/A"},"",{"$f":"$E8*$G8*VLOOKUP($D8,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$E8*$G8*VLOOKUP($D8,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D8,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D8,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A8)>0, $A8,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D8,'Dropdown Lists'!$E$2:$E$143,0), \"\") & \",\" & CELL(\"col\", 'Dropdown Lists'!$E$2)","v":",5"},",5"]
[null,"VOLUME",null,null,null,"m3",1,null,null,{"$error":"#N/A"},"",{"$f":"$E9*$G9*VLOOKUP($D9,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$E9*$G9*VLOOKUP($D9,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D9,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D9,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A9)>0, $A9,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D9,'Dropdown Lists'!$E$2:$E$143,0), \"\") & \",\" & CELL(\"col\", 'Dropdown Lists'!$E$2)","v":",5"},",5"]
[null,null,"MATERIALS BY AREA",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($D10,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D10,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"AREA",null,null,null,"m2",1,null,null,{"$error":"#N/A"},"",{"$f":"$E11*$G11*VLOOKUP($D11,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$E11*$G11*VLOOKUP($D11,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D11,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D11,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A11)>0, $A11,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D11,'Dropdown Lists'!$F$2:$F$156,0), \"\")& \",\" & CELL(\"col\", 'Dropdown Lists'!$F$2)","v":",6"},",6"]
[null,"AREA",null,null,null,"m2",1,null,null,{"$error":"#N/A"},"",{"$f":"$E12*$G12*VLOOKUP($D12,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$E12*$G12*VLOOKUP($D12,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D12,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D12,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A12)>0, $A12,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D12,'Dropdown Lists'!$F$2:$F$156,0), \"\")& \",\" & CELL(\"col\", 'Dropdown Lists'!$F$2)","v":",6"},",6"]
[null,"AREA",null,null,null,"m2",1,null,null,{"$error":"#N/A"},"",{"$f":"$E13*$G13*VLOOKUP($D13,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$E13*$G13*VLOOKUP($D13,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D13,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D13,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A13)>0, $A13,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D13,'Dropdown Lists'!$F$2:$F$156,0), \"\")& \",\" & CELL(\"col\", 'Dropdown Lists'!$F$2)","v":",6"},",6"]
[null,null,"MATERIALS BY LENGTH",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($D14,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D14,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,"LENGTH",null,null,null,"m",1,null,null,{"$error":"#N/A"},"",{"$f":"$E15*$G15*VLOOKUP($D15,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$E15*$G15*VLOOKUP($D15,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D15,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D15,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A15)>0, $A15,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D15,'Dropdown Lists'!$G$2:$G$36,0), \"\")& \",\" & CELL(\"col\", 'Dropdown Lists'!$G$2)","v":",7"},",7"]
[null,"LENGTH",null,null,null,"m",1,null,null,{"$error":"#N/A"},"",{"$f":"$E16*$G16*VLOOKUP($D16,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$E16*$G16*VLOOKUP($D16,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D16,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D16,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A16)>0, $A16,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D16,'Dropdown Lists'!$G$2:$G$36,0), \"\")& \",\" & CELL(\"col\", 'Dropdown Lists'!$G$2)","v":",7"},",7"]
[null,"LENGTH",null,null,null,"m",1,null,null,{"$error":"#N/A"},"",{"$f":"$E17*$G17*VLOOKUP($D17,'Master sheet'!$A:$AJ,13,FALSE)","v":{"$error":"#N/A"}},{"$f":"$E17*$G17*VLOOKUP($D17,'Master sheet'!$A:$AJ,27,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D17,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D17,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A17)>0, $A17,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D17,'Dropdown Lists'!$G$2:$G$36,0), \"\")& \",\" & CELL(\"col\", 'Dropdown Lists'!$G$2)","v":",7"},",7"]
[null,null,"MATERIALS BY AREA & R-VALUE",null,null,null,null,null,null,null,null,null,null,{"$f":"IF(ISTEXT(VLOOKUP($D18,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D18,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""}]
[null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,"m2",1,null,null,{"$error":"#N/A"},"",{"$f":"$E19*$G19*VLOOKUP($D19,'Master sheet'!$A:$AJ,13,FALSE)*$C19/5.678","v":{"$error":"#N/A"}},{"$f":"$E19*$G19*VLOOKUP($D19,'Master sheet'!$A:$AJ,27,FALSE)*$C19/5.678","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D19,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D19,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A19)>0, $A19,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D19,'Dropdown Lists'!$H$2:$H$75,0), \"\")& \",\" & CELL(\"col\", 'Dropdown Lists'!$H$2)","v":",8"},",8"]
[null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,"m2",1,null,null,{"$error":"#N/A"},"",{"$f":"$E20*$G20*VLOOKUP($D20,'Master sheet'!$A:$AJ,13,FALSE)*$C20/5.678","v":{"$error":"#N/A"}},{"$f":"$E20*$G20*VLOOKUP($D20,'Master sheet'!$A:$AJ,27,FALSE)*$C20/5.678","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D20,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D20,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A20)>0, $A20,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D20,'Dropdown Lists'!$H$2:$H$75,0), \"\")& \",\" & CELL(\"col\", 'Dropdown Lists'!$H$2)","v":",8"},",8"]
[null,{"$f":"IF(LOWER(Setting!rng_language)=\"english\",\"R-VALUE:\",\"VALEUR R :\")","v":"R-VALUE:"},null,null,null,"m2",1,null,null,{"$error":"#N/A"},"",{"$f":"$E21*$G21*VLOOKUP($D21,'Master sheet'!$A:$AJ,13,FALSE)*$C21/5.678","v":{"$error":"#N/A"}},{"$f":"$E21*$G21*VLOOKUP($D21,'Master sheet'!$A:$AJ,27,FALSE)*$C21/5.678","v":{"$error":"#N/A"}},{"$f":"IF(ISTEXT(VLOOKUP($D21,'Master sheet'!$A:$AP,42,FALSE)),VLOOKUP($D21,'Master sheet'!$A:$AP,42,FALSE),\"\")","v":""},null,"USER-DEFINED",{"$f":"IF(LEN($A21)>0, $A21,$A$5)","v":"EXISTING DATABASE MATERIALS"},null,{"$f":"_xlfn.IFNA(MATCH(D21,'Dropdown Lists'!$H$2:$H$75,0), \"\")& \",\" & CELL(\"col\", 'Dropdown Lists'!$H$2)","v":",8"},",8"]
["CUSTOM USER-DEFINED MATERIALS"]
[null,"User-Defined",null,null,null,null,1,null,null,0,{"$f":"IF(I23=1,J23,\"\")","v":""},null,null,null,null,"USER-DEFINED",{"$f":"B23","v":"User-Defined"}]
[null,"User-Defined",null,null,null,null,1,null,null,0,{"$f":"IF(I24=1,J24,\"\")","v":""},null,null,null,null,"USER-DEFINED",{"$f":"B24","v":"User-Defined"}]
[null,"User-Defined",null,null,null,null,1,null,null,0,{"$f":"IF(I25=1,J25,\"\")","v":""},null,null,null,null,"USER-DEFINED","User-Defined"]
[null,"User-Defined",null,null,null,null,1,null,null,0,{"$f":"IF(I26=1,J26,\"\")","v":""},null,null,null,null,"USER-DEFINED","User-Defined"]
[null,"User-Defined",null,null,null,null,1,null,null,0,{"$f":"IF(I27=1,J27,\"\")","v":""},null,null,null,null,"USER-DEFINED","User-Defined"]
[null,"Note: User-Defined materials will be listed separately in summary reports."]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"REVIEW","index":22,"n_rows":200,"n_cols":8,"rows_kept":200,"cut":false,"hidden":false,"merged":[[0,0,0,1]]}
["SECTION 12 ➜ REVIEW",null,"SELECTED MATERIALS",{"$f":"SUM($D$3:$D$499)","v":0},{"$f":"SUM($E$3:$E$499)","v":0},{"$f":"SUM($F$3:$F$499)","v":0}]
["SECTION","CATEGORY","MATERIAL","NET CARBON FOOTPRINT \n[kg CO2e]","CARBON EMISSIONS \n[kg CO2e]","CARBON STORAGE\n[kg CO2e]"]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B3=\"\",\"END\",B3),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B3)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C3)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},{"$f":"IFERROR(E3-F3,\"\")","v":""},{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E3)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F3)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""},null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B4=\"\",\"END\",B4),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B4)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C4)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},{"$f":"IFERROR(E4-F4,\"\")","v":""},{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E4)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F4)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""},null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B5=\"\",\"END\",B5),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B5)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C5)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E5)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F5)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B6=\"\",\"END\",B6),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B6)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C6)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E6)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F6)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B7=\"\",\"END\",B7),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B7)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C7)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E7)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F7)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B8=\"\",\"END\",B8),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B8)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C8)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E8)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F8)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B9=\"\",\"END\",B9),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B9)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C9)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E9)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F9)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B10=\"\",\"END\",B10),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B10)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C10)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E10)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F10)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B11=\"\",\"END\",B11),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B11)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C11)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E11)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F11)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B12=\"\",\"END\",B12),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B12)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C12)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E12)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F12)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B13=\"\",\"END\",B13),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B13)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C13)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E13)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F13)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B14=\"\",\"END\",B14),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B14)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C14)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E14)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F14)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B15=\"\",\"END\",B15),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B15)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C15)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E15)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F15)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B16=\"\",\"END\",B16),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B16)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C16)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E16)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F16)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B17=\"\",\"END\",B17),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B17)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C17)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E17)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F17)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B18=\"\",\"END\",B18),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B18)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C18)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E18)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F18)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B19=\"\",\"END\",B19),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B19)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C19)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E19)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F19)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B20=\"\",\"END\",B20),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B20)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C20)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E20)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F20)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B21=\"\",\"END\",B21),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B21)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C21)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E21)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F21)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B22=\"\",\"END\",B22),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B22)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C22)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E22)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F22)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B23=\"\",\"END\",B23),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B23)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C23)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E23)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F23)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B24=\"\",\"END\",B24),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B24)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C24)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E24)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F24)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B25=\"\",\"END\",B25),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B25)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C25)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E25)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F25)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B26=\"\",\"END\",B26),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B26)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C26)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E26)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F26)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B27=\"\",\"END\",B27),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B27)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C27)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E27)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F27)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B28=\"\",\"END\",B28),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B28)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C28)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E28)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F28)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B29=\"\",\"END\",B29),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B29)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C29)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E29)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F29)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B30=\"\",\"END\",B30),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B30)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C30)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E30)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F30)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B31=\"\",\"END\",B31),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B31)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C31)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E31)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F31)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B32=\"\",\"END\",B32),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B32)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C32)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E32)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F32)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B33=\"\",\"END\",B33),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B33)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C33)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E33)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F33)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B34=\"\",\"END\",B34),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B34)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C34)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E34)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F34)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B35=\"\",\"END\",B35),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B35)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C35)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E35)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F35)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B36=\"\",\"END\",B36),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B36)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C36)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E36)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F36)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B37=\"\",\"END\",B37),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B37)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C37)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E37)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F37)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B38=\"\",\"END\",B38),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B38)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C38)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E38)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F38)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B39=\"\",\"END\",B39),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B39)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C39)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E39)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F39)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B40=\"\",\"END\",B40),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B40)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C40)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E40)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F40)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B41=\"\",\"END\",B41),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B41)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C41)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E41)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F41)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B42=\"\",\"END\",B42),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B42)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C42)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E42)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F42)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B43=\"\",\"END\",B43),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B43)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C43)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E43)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F43)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B44=\"\",\"END\",B44),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B44)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C44)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E44)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F44)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B45=\"\",\"END\",B45),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B45)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C45)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E45)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F45)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B46=\"\",\"END\",B46),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B46)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C46)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E46)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F46)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B47=\"\",\"END\",B47),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B47)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C47)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E47)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F47)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B48=\"\",\"END\",B48),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B48)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C48)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E48)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F48)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B49=\"\",\"END\",B49),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B49)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C49)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E49)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F49)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B50=\"\",\"END\",B50),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B50)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C50)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E50)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F50)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B51=\"\",\"END\",B51),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B51)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C51)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E51)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F51)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B52=\"\",\"END\",B52),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B52)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C52)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E52)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F52)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B53=\"\",\"END\",B53),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B53)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C53)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E53)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F53)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B54=\"\",\"END\",B54),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B54)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C54)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E54)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F54)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B55=\"\",\"END\",B55),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B55)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C55)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E55)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F55)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B56=\"\",\"END\",B56),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B56)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C56)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E56)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F56)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B57=\"\",\"END\",B57),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B57)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C57)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E57)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F57)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B58=\"\",\"END\",B58),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B58)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C58)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E58)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F58)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B59=\"\",\"END\",B59),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B59)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C59)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E59)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F59)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B60=\"\",\"END\",B60),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B60)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C60)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E60)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F60)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B61=\"\",\"END\",B61),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B61)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C61)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E61)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F61)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B62=\"\",\"END\",B62),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B62)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C62)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E62)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F62)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B63=\"\",\"END\",B63),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B63)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C63)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E63)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F63)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B64=\"\",\"END\",B64),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B64)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C64)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E64)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F64)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B65=\"\",\"END\",B65),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B65)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C65)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E65)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F65)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B66=\"\",\"END\",B66),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B66)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C66)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E66)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F66)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B67=\"\",\"END\",B67),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B67)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C67)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E67)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F67)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B68=\"\",\"END\",B68),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B68)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C68)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},{"$f":"IFERROR(E68-F68,\"\")","v":""},{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E68)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F68)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B69=\"\",\"END\",B69),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B69)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C69)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E69)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F69)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B70=\"\",\"END\",B70),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B70)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C70)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E70)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F70)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B71=\"\",\"END\",B71),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B71)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C71)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E71)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F71)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B72=\"\",\"END\",B72),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B72)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C72)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E72)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F72)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B73=\"\",\"END\",B73),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B73)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C73)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E73)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F73)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B74=\"\",\"END\",B74),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B74)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C74)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E74)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F74)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B75=\"\",\"END\",B75),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B75)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C75)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E75)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F75)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B76=\"\",\"END\",B76),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B76)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C76)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E76)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F76)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B77=\"\",\"END\",B77),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B77)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C77)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E77)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F77)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B78=\"\",\"END\",B78),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B78)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C78)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E78)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F78)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B79=\"\",\"END\",B79),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B79)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C79)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E79)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F79)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B80=\"\",\"END\",B80),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B80)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C80)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E80)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F80)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B81=\"\",\"END\",B81),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B81)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C81)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E81)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F81)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B82=\"\",\"END\",B82),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B82)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C82)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E82)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F82)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B83=\"\",\"END\",B83),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B83)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C83)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E83)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F83)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B84=\"\",\"END\",B84),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B84)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C84)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E84)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F84)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B85=\"\",\"END\",B85),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B85)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C85)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E85)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F85)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B86=\"\",\"END\",B86),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B86)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C86)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E86)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F86)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B87=\"\",\"END\",B87),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B87)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C87)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E87)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F87)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B88=\"\",\"END\",B88),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B88)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C88)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E88)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F88)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B89=\"\",\"END\",B89),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B89)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C89)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E89)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F89)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B90=\"\",\"END\",B90),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B90)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C90)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E90)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F90)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B91=\"\",\"END\",B91),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B91)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C91)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E91)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F91)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B92=\"\",\"END\",B92),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B92)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C92)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E92)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F92)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B93=\"\",\"END\",B93),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B93)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C93)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E93)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F93)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B94=\"\",\"END\",B94),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B94)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C94)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E94)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F94)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B95=\"\",\"END\",B95),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B95)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C95)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E95)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F95)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B96=\"\",\"END\",B96),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B96)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C96)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E96)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F96)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B97=\"\",\"END\",B97),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B97)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C97)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E97)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F97)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B98=\"\",\"END\",B98),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B98)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C98)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E98)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F98)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B99=\"\",\"END\",B99),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B99)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C99)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E99)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F99)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B100=\"\",\"END\",B100),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B100)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C100)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E100)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F100)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B101=\"\",\"END\",B101),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B101)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C101)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E101)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F101)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B102=\"\",\"END\",B102),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B102)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C102)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E102)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F102)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B103=\"\",\"END\",B103),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B103)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C103)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E103)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F103)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B104=\"\",\"END\",B104),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B104)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C104)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E104)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F104)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B105=\"\",\"END\",B105),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B105)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C105)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E105)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F105)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B106=\"\",\"END\",B106),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B106)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C106)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E106)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F106)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B107=\"\",\"END\",B107),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B107)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C107)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E107)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F107)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B108=\"\",\"END\",B108),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B108)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C108)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E108)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F108)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B109=\"\",\"END\",B109),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B109)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C109)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E109)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F109)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B110=\"\",\"END\",B110),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B110)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C110)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E110)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F110)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B111=\"\",\"END\",B111),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B111)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C111)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E111)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F111)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B112=\"\",\"END\",B112),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B112)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C112)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E112)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F112)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B113=\"\",\"END\",B113),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B113)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C113)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E113)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F113)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B114=\"\",\"END\",B114),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B114)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C114)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E114)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F114)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B115=\"\",\"END\",B115),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B115)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C115)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E115)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F115)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B116=\"\",\"END\",B116),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B116)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C116)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E116)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F116)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B117=\"\",\"END\",B117),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B117)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C117)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E117)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F117)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B118=\"\",\"END\",B118),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B118)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C118)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E118)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F118)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B119=\"\",\"END\",B119),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B119)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C119)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E119)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F119)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B120=\"\",\"END\",B120),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B120)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C120)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E120)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F120)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B121=\"\",\"END\",B121),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B121)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C121)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E121)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F121)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B122=\"\",\"END\",B122),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B122)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C122)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E122)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F122)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B123=\"\",\"END\",B123),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B123)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C123)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E123)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F123)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B124=\"\",\"END\",B124),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B124)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C124)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E124)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F124)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B125=\"\",\"END\",B125),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B125)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C125)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E125)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F125)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B126=\"\",\"END\",B126),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B126)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C126)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E126)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F126)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B127=\"\",\"END\",B127),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B127)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C127)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E127)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F127)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B128=\"\",\"END\",B128),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B128)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C128)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E128)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F128)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B129=\"\",\"END\",B129),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B129)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C129)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E129)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F129)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B130=\"\",\"END\",B130),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B130)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C130)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E130)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F130)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B131=\"\",\"END\",B131),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B131)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C131)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E131)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F131)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B132=\"\",\"END\",B132),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B132)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C132)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},{"$f":"IFERROR(E132-F132,\"\")","v":""},{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E132)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F132)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B133=\"\",\"END\",B133),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B133)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C133)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E133)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F133)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B134=\"\",\"END\",B134),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B134)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C134)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E134)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F134)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B135=\"\",\"END\",B135),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B135)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C135)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E135)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F135)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B136=\"\",\"END\",B136),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B136)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C136)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E136)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F136)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B137=\"\",\"END\",B137),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B137)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C137)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E137)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F137)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B138=\"\",\"END\",B138),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B138)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C138)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E138)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F138)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B139=\"\",\"END\",B139),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B139)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C139)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E139)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F139)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B140=\"\",\"END\",B140),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B140)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C140)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E140)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F140)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B141=\"\",\"END\",B141),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B141)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C141)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E141)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F141)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B142=\"\",\"END\",B142),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B142)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C142)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E142)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F142)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B143=\"\",\"END\",B143),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B143)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C143)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E143)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F143)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B144=\"\",\"END\",B144),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B144)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C144)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E144)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F144)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B145=\"\",\"END\",B145),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B145)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C145)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E145)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F145)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B146=\"\",\"END\",B146),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B146)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C146)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E146)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F146)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B147=\"\",\"END\",B147),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B147)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C147)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E147)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F147)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B148=\"\",\"END\",B148),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B148)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C148)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E148)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F148)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B149=\"\",\"END\",B149),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B149)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C149)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E149)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F149)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B150=\"\",\"END\",B150),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B150)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C150)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E150)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F150)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B151=\"\",\"END\",B151),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B151)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C151)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E151)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F151)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B152=\"\",\"END\",B152),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B152)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C152)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E152)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F152)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B153=\"\",\"END\",B153),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B153)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C153)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E153)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F153)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B154=\"\",\"END\",B154),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B154)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C154)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E154)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F154)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B155=\"\",\"END\",B155),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B155)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C155)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E155)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F155)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B156=\"\",\"END\",B156),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B156)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C156)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E156)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F156)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B157=\"\",\"END\",B157),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B157)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C157)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E157)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F157)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B158=\"\",\"END\",B158),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B158)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C158)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E158)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F158)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B159=\"\",\"END\",B159),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B159)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C159)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E159)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F159)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B160=\"\",\"END\",B160),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B160)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C160)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E160)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F160)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B161=\"\",\"END\",B161),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B161)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C161)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E161)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F161)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B162=\"\",\"END\",B162),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B162)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C162)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E162)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F162)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B163=\"\",\"END\",B163),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B163)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C163)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E163)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F163)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B164=\"\",\"END\",B164),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B164)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C164)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E164)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F164)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B165=\"\",\"END\",B165),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B165)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C165)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E165)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F165)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B166=\"\",\"END\",B166),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B166)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C166)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E166)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F166)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B167=\"\",\"END\",B167),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B167)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C167)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E167)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F167)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B168=\"\",\"END\",B168),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B168)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C168)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E168)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F168)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B169=\"\",\"END\",B169),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B169)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C169)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E169)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F169)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B170=\"\",\"END\",B170),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B170)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C170)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E170)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F170)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B171=\"\",\"END\",B171),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B171)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C171)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E171)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F171)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B172=\"\",\"END\",B172),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B172)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C172)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E172)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F172)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B173=\"\",\"END\",B173),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B173)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C173)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E173)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F173)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B174=\"\",\"END\",B174),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B174)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C174)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E174)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F174)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B175=\"\",\"END\",B175),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B175)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C175)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E175)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F175)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B176=\"\",\"END\",B176),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B176)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C176)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E176)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F176)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B177=\"\",\"END\",B177),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B177)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C177)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E177)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F177)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B178=\"\",\"END\",B178),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B178)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C178)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E178)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F178)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B179=\"\",\"END\",B179),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B179)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C179)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E179)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F179)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B180=\"\",\"END\",B180),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B180)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C180)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E180)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F180)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B181=\"\",\"END\",B181),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B181)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C181)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E181)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F181)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B182=\"\",\"END\",B182),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B182)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C182)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E182)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F182)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B183=\"\",\"END\",B183),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B183)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C183)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E183)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F183)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B184=\"\",\"END\",B184),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B184)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C184)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E184)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F184)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B185=\"\",\"END\",B185),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B185)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C185)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E185)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F185)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B186=\"\",\"END\",B186),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B186)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C186)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E186)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F186)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B187=\"\",\"END\",B187),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B187)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C187)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E187)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F187)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B188=\"\",\"END\",B188),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B188)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C188)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E188)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F188)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B189=\"\",\"END\",B189),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B189)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C189)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E189)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F189)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B190=\"\",\"END\",B190),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B190)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C190)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E190)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F190)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B191=\"\",\"END\",B191),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B191)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C191)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E191)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F191)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B192=\"\",\"END\",B192),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B192)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C192)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E192)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F192)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B193=\"\",\"END\",B193),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B193)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C193)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E193)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F193)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B194=\"\",\"END\",B194),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B194)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C194)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E194)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F194)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B195=\"\",\"END\",B195),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B195)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C195)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},"",{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E195)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F195)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B196=\"\",\"END\",B196),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B196)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C196)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},{"$f":"IFERROR(E196-F196,\"\")","v":""},{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E196)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F196)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B197=\"\",\"END\",B197),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B197)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C197)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},{"$f":"IFERROR(E197-F197,\"\")","v":""},{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E197)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F197)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B198=\"\",\"END\",B198),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B198)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C198)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},{"$f":"IFERROR(E198-F198,\"\")","v":""},{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E198)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F198)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B199=\"\",\"END\",B199),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B199)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C199)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},{"$f":"IFERROR(E199-F199,\"\")","v":""},{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E199)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F199)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]
[{"$f":"IFERROR(INDEX(Data!A$3:A$620,MATCH(IF(B200=\"\",\"END\",B200),Data!$B$3:$B$620,0)),\"\")","v":""},{"$f":"INDEX(Data!B$3:B$620,MATCH(SMALL(IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,ROWS(B$3:B200)),IFERROR(SEARCH(,Data!B$3:B$620),10^9)+ROW(Data!B$3:B$620)/1000,0))","v":""},{"$f":"INDEX(Data!C$3:C$620,MATCH(SMALL(IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,ROWS(C$3:C200)),IFERROR(SEARCH(,Data!C$3:C$620),10^9)+ROW(Data!C$3:C$620)/1000,0))","v":""},{"$f":"IFERROR(E200-F200,\"\")","v":""},{"$f":"INDEX(Data!E$3:E$620,MATCH(SMALL(IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,ROWS(E$3:E200)),IFERROR(SEARCH(,Data!E$3:E$620),10^9)+ROW(Data!E$3:E$620)/1000,0))","v":""},{"$f":"INDEX(Data!F$3:F$620,MATCH(SMALL(IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,ROWS(F$3:F200)),IFERROR(SEARCH(,Data!F$3:F$620),10^9)+ROW(Data!F$3:F$620)/1000,0))","v":""}]

{"sheet":"RESULTS","index":23,"n_rows":70,"n_cols":9,"rows_kept":70,"cut":false,"hidden":false,"merged":[[68,2,68,8],[69,2,69,8],[1,7,1,9],[8,4,8,5],[12,7,13,7],[12,8,13,8],[10,7,10,8],[10,4,10,5],[12,4,13,4],[12,5,13,5],[54,5,54,8],[54,3,54,4],[67,1,67,8],[31,2,31,7],[28,1,28,8],[55,5,55,7],[61,5,61,7],[62,5,62,7],[63,5,63,7],[64,5,64,7],[16,1,16,9],[56,5,56,7],[57,5,57,7],[58,5,58,7],[59,5,59,7],[60,5,60,7],[8,6,8,9],[9,10,10,10],[2,10,2,11],[4,11,5,11],[7,11,8,11],[9,11,10,11],[4,4,4,5],[5,4,5,5],[6,4,6,5],[7,4,7,5],[4,6,4,9],[5,6,5,9],[6,6,6,9],[7,6,7,9]]}
[]
["Material Carbon Emissions Estimator (MCE2)",null,null,null,null,null,null,"Project Carbon Emissions Estimates"]
[null,"PROJECT SUMMARY"]
[]
[null,null,null,null,"Project:"]
[null,null,null,null,"Evaluator:"]
[null,null,null,null,"Location:"]
[null,null,null,null,"Home description:"]
[null,null,null,null,"Building Size:"]
[]
[null,null,null,null,"Material Emissions",null,null,"Operational Emissions"]
[null,null,null,null,"tonnes CO2e","kg CO2e / m2",null,"tonnes CO2e / yr","t CO2e / 30 yrs"]
[null,null,null,null,{"$f":"'USER INPUT SHEET'!M21","v":0},{"$f":"'USER INPUT SHEET'!N21","v":0},null,{"$f":"'USER INPUT SHEET'!M16","v":0},{"$f":"'USER INPUT SHEET'!N16","v":0}]
[]
[]
[null,"Project Notes"]
[null,"Home is aiming to achieve XYZ level of performance…"]
[null,"PROJECT EMISSIONS TIMELINE"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Chart information"]
[null,"Note: In grids with low carbon intensities, MCE2 users should consider energy efficiency measures to reduce overall loads on local and regional grids. \nThe Cumulative Carbon Emissions chart offers a simplified view of the climate impact of materials manufacturing and building operations for the initial 30 years. This chart should be used as a directional guidepost for where to focus carbon reduction efforts, rather than as a predictive model for future emissions. There are several unknowns which may cause deviations from this model, some of which are described below. \n\nNotes on simplifying assumptions\n- Only the cradle-to-gate new construction material carbon emissions are modeled. Realistically, there would be some fluctuations in material carbon due to renovations, maintenance, material decomposition, etc. \n- The operational carbon emissions, the grey line, is shown to increase at the same annual rate. This too, in reality, will vary from year to year and especially as the building ages. \n- GHG emissions associated with fuels and electricity generation (by province or territory) are unchanging values. These values should be reasonably expected to change over time."]
[]
[]
[]
[]
[null,"Project Carbon Emissions Results"]
[null,"EMISSIONS BY ELEMENT OF THE HOME"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"TOP 10 MOST IMPACTFUL MATERIALS"]
[]
[null,"Rank","kg CO2e","Section",null,"Material"]
[null,1,{"$f":"Data!$J3","v":{"$error":"#NUM!"}},{"$f":"Data!K3","v":{"$error":"#NUM!"}},null,{"$f":"Data!M3","v":{"$error":"#NUM!"}}]
[null,2,{"$f":"Data!$J4","v":{"$error":"#NUM!"}},{"$f":"Data!K4","v":{"$error":"#NUM!"}},null,{"$f":"Data!M4","v":{"$error":"#NUM!"}}]
[null,3,{"$f":"Data!$J5","v":{"$error":"#NUM!"}},{"$f":"Data!K5","v":{"$error":"#NUM!"}},null,{"$f":"Data!M5","v":{"$error":"#NUM!"}}]
[null,4,{"$f":"Data!$J6","v":{"$error":"#NUM!"}},{"$f":"Data!K6","v":{"$error":"#NUM!"}},null,{"$f":"Data!M6","v":{"$error":"#NUM!"}}]
[null,5,{"$f":"Data!$J7","v":{"$error":"#NUM!"}},{"$f":"Data!K7","v":{"$error":"#NUM!"}},null,{"$f":"Data!M7","v":{"$error":"#NUM!"}}]
[null,6,{"$f":"Data!$J8","v":{"$error":"#NUM!"}},{"$f":"Data!K8","v":{"$error":"#NUM!"}},null,{"$f":"Data!M8","v":{"$error":"#NUM!"}}]
[null,7,{"$f":"Data!$J9","v":{"$error":"#NUM!"}},{"$f":"Data!K9","v":{"$error":"#NUM!"}},null,{"$f":"Data!M9","v":{"$error":"#NUM!"}}]
[null,8,{"$f":"Data!$J10","v":{"$error":"#NUM!"}},{"$f":"Data!K10","v":{"$error":"#NUM!"}},null,{"$f":"Data!M10","v":{"$error":"#NUM!"}}]
[null,9,{"$f":"Data!$J11","v":{"$error":"#NUM!"}},{"$f":"Data!K11","v":{"$error":"#NUM!"}},null,{"$f":"Data!M11","v":{"$error":"#NUM!"}}]
[null,10,{"$f":"Data!$J12","v":{"$error":"#NUM!"}},{"$f":"Data!K12","v":{"$error":"#NUM!"}},null,{"$f":"Data!M12","v":{"$error":"#NUM!"}}]
[null,"RECOMMENDATIONS"]
[]
[null,"User or embodied carbon advisor to provide recommendations here…"]
[null,null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"SCENARIOS","index":24,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[[2,2,6,2],[2,3,2,7],[3,3,3,7],[4,3,4,7],[5,3,5,7],[6,3,6,7]]}
[]
[null,null,"Project Carbon Emissions Scenarios"]
[null,null,"How to use this TAB:","1. Users can save scenarios to this page in order to compare results generated in the calculator."]
[null,null,null,"2. All data associated with the saved scenarios can be re-populated across the spreadsheet."]
[null,null,null,"3. To populate a scenario in the estimator, users can select the scenario by clicking on the green button labeled \"Reset Calculator\" on the left."]
[null,null,null,"4. Users can establish custom scenarios and apply these to different homes by loading a new geometry in the USER INPUT SHEET and clicking on the blue button on the left labeled \"Recalculate all Scenarios\"."]
[null,null,null,"5 . This will calculate new values associated with the updated geometry for each saved scenario below."]
[]
[null,null,"Name of Scenario Here","Name of Scenario Here","Name of Scenario Here","Name of Scenario Here","Name of Scenario Here","Name of Scenario Here"]
[null,"Notes","Type notes here","Type notes here","Type notes here","Type notes here","Type notes here"]
[null,"MCE Total (tonnes CO2e)"]
[null,"Embodied Carbon per m2 (kg CO2e / m2)"]
[null,"Footings & Slabs (kg CO2e)"]
[null,"Foundation Walls (kg CO2e)"]
[null,"Structural Elements (kg CO2e)"]
[null,"Ext. Walls (kg CO2e / m2)"]
[null,"Ext. Wall Systems (kg CO2e)"]
[null,"Party Walls (kg CO2e)"]
[null,"Cladding (kg CO2e)"]
[null,"Windows (kg CO2e)"]
[null,"Int. Walls (kg CO2e)"]
[null,"Floors (kg CO2e)"]
[null,"Ceilings (kg CO2e)"]
[null,"Roof (kg CO2e)"]
[null,"Garage (kg CO2e)"]
[null,"User-Defined (kg CO2e)"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Scenarios-DB","index":25,"n_rows":2910,"n_cols":4,"rows_kept":2910,"cut":false,"hidden":true,"merged":[]}
[null,"Sheet Names","Rows","Columns"]
[]
[null,"Footings & Slabs",5,5]
[null,"Footings & Slabs",5,6]
[null,"Footings & Slabs",7,6]
[null,"Footings & Slabs",7,8]
[null,"Footings & Slabs",8,6]
[null,"Footings & Slabs",8,8]
[null,"Footings & Slabs",9,6]
[null,"Footings & Slabs",9,8]
[null,"Footings & Slabs",10,6]
[null,"Footings & Slabs",10,8]
[null,"Footings & Slabs",11,6]
[null,"Footings & Slabs",11,8]
[null,"Footings & Slabs",14,6]
[null,"Footings & Slabs",14,8]
[null,"Footings & Slabs",15,6]
[null,"Footings & Slabs",15,8]
[null,"Footings & Slabs",16,6]
[null,"Footings & Slabs",16,8]
[null,"Footings & Slabs",17,6]
[null,"Footings & Slabs",17,8]
[null,"Footings & Slabs",18,6]
[null,"Footings & Slabs",18,8]
[null,"Footings & Slabs",19,6]
[null,"Footings & Slabs",19,8]
[null,"Footings & Slabs",20,6]
[null,"Footings & Slabs",20,8]
[null,"Footings & Slabs",22,6]
[null,"Footings & Slabs",22,8]
[null,"Footings & Slabs",23,6]
[null,"Footings & Slabs",23,8]
[null,"Footings & Slabs",24,6]
[null,"Footings & Slabs",24,8]
[null,"Footings & Slabs",25,6]
[null,"Footings & Slabs",25,8]
[null,"Footings & Slabs",26,6]
[null,"Footings & Slabs",26,8]
[null,"Footings & Slabs",27,6]
[null,"Footings & Slabs",27,8]
[null,"Footings & Slabs",28,6]
[null,"Footings & Slabs",28,8]
[null,"Footings & Slabs",30,6]
[null,"Footings & Slabs",30,8]
[null,"Footings & Slabs",31,6]
[null,"Footings & Slabs",31,8]
[null,"Footings & Slabs",32,6]
[null,"Footings & Slabs",32,8]
[null,"Footings & Slabs",33,6]
[null,"Footings & Slabs",33,8]
[null,"Footings & Slabs",34,6]
[null,"Footings & Slabs",34,8]
[null,"Footings & Slabs",35,6]
[null,"Footings & Slabs",35,8]
[null,"Footings & Slabs",36,6]
[null,"Footings & Slabs",36,8]
[null,"Footings & Slabs",37,5]
[null,"Footings & Slabs",39,6]
[null,"Footings & Slabs",39,8]
[null,"Footings & Slabs",40,6]
[null,"Footings & Slabs",40,8]
[null,"Footings & Slabs",41,6]
[null,"Footings & Slabs",41,8]
[null,"Footings & Slabs",42,6]
[null,"Footings & Slabs",42,8]
[null,"Footings & Slabs",43,6]
[null,"Footings & Slabs",43,8]
[null,"Footings & Slabs",44,6]
[null,"Footings & Slabs",44,8]
[null,"Footings & Slabs",45,6]
[null,"Footings & Slabs",45,8]
[null,"Footings & Slabs",46,6]
[null,"Footings & Slabs",46,8]
[null,"Footings & Slabs",47,5]
[null,"Footings & Slabs",49,6]
[null,"Footings & Slabs",49,8]
[null,"Footings & Slabs",50,5]
[null,"Footings & Slabs",52,6]
[null,"Footings & Slabs",52,8]
[null,"Footings & Slabs",53,5]
[null,"Footings & Slabs",53,6]
[null,"Footings & Slabs",55,6]
[null,"Footings & Slabs",55,8]
[null,"Footings & Slabs",56,6]
[null,"Footings & Slabs",56,8]
[null,"Footings & Slabs",57,6]
[null,"Footings & Slabs",57,8]
[null,"Footings & Slabs",58,6]
[null,"Footings & Slabs",58,8]
[null,"Footings & Slabs",59,6]
[null,"Footings & Slabs",59,8]
[null,"Footings & Slabs",60,6]
[null,"Footings & Slabs",60,8]
[null,"Footings & Slabs",61,6]
[null,"Footings & Slabs",61,8]
[null,"Footings & Slabs",63,6]
[null,"Footings & Slabs",63,8]
[null,"Footings & Slabs",64,6]
[null,"Footings & Slabs",64,8]
[null,"Footings & Slabs",65,6]
[null,"Footings & Slabs",65,8]
[null,"Footings & Slabs",66,6]
[null,"Footings & Slabs",66,8]
[null,"Footings & Slabs",67,6]
[null,"Footings & Slabs",67,8]
[null,"Footings & Slabs",68,6]
[null,"Footings & Slabs",68,8]
[null,"Footings & Slabs",69,6]
[null,"Footings & Slabs",69,8]
[null,"Footings & Slabs",71,6]
[null,"Footings & Slabs",71,8]
[null,"Footings & Slabs",72,6]
[null,"Footings & Slabs",72,8]
[null,"Footings & Slabs",73,6]
[null,"Footings & Slabs",73,8]
[null,"Footings & Slabs",74,6]
[null,"Footings & Slabs",74,8]
[null,"Footings & Slabs",75,6]
[null,"Footings & Slabs",75,8]
[null,"Footings & Slabs",76,6]
[null,"Footings & Slabs",76,8]
[null,"Footings & Slabs",77,6]
[null,"Footings & Slabs",77,8]
[null,"Footings & Slabs",80,6]
[null,"Footings & Slabs",80,8]
[null,"Footings & Slabs",81,5]
[null,"Footings & Slabs",82,5]
[null,"Footings & Slabs",83,6]
[null,"Footings & Slabs",83,8]
[null,"Footings & Slabs",84,6]
[null,"Footings & Slabs",84,8]
[null,"Footings & Slabs",85,6]
[null,"Footings & Slabs",85,8]
[null,"Footings & Slabs",86,5]
[null,"Footings & Slabs",87,6]
[null,"Footings & Slabs",87,8]
[null,"Footings & Slabs",88,6]
[null,"Footings & Slabs",88,8]
[null,"Footings & Slabs",89,6]
[null,"Footings & Slabs",89,8]
[null,"Footings & Slabs",90,6]
[null,"Footings & Slabs",90,8]
[null,"Footings & Slabs",91,6]
[null,"Footings & Slabs",91,8]
[null,"Footings & Slabs",92,5]
[null,"Footings & Slabs",93,6]
[null,"Footings & Slabs",93,8]
[null,"Footings & Slabs",94,5]
[null,"Footings & Slabs",95,6]
[null,"Footings & Slabs",95,8]
[null,"Footings & Slabs",96,6]
[null,"Footings & Slabs",96,8]
[null,"Footings & Slabs",97,6]
[null,"Footings & Slabs",97,8]
[null,"Footings & Slabs",98,6]
[null,"Footings & Slabs",98,8]
[null,"Footings & Slabs",99,5]
[null,"Footings & Slabs",100,6]
[null,"Footings & Slabs",100,8]
[null,"Footings & Slabs",101,6]
[null,"Footings & Slabs",101,8]
[null,"Footings & Slabs",102,6]
[null,"Footings & Slabs",102,8]
[null,"Footings & Slabs",103,5]
[null,"Footings & Slabs",104,6]
[null,"Footings & Slabs",104,8]
[null,"Footings & Slabs",107,6]
[null,"Footings & Slabs",107,8]
[null,"Footings & Slabs",108,6]
[null,"Footings & Slabs",108,8]
[null,"Footings & Slabs",109,6]
[null,"Footings & Slabs",109,8]
[null,"Footings & Slabs",110,6]
[null,"Footings & Slabs",110,8]
[null,"Footings & Slabs",112,6]
[null,"Footings & Slabs",112,8]
[null,"Footings & Slabs",113,6]
[null,"Footings & Slabs",113,8]
[null,"Footings & Slabs",114,6]
[null,"Footings & Slabs",114,8]
[null,"Footings & Slabs",115,6]
[null,"Footings & Slabs",115,8]
[null,"Footings & Slabs",116,6]
[null,"Footings & Slabs",116,8]
[null,"Footings & Slabs",117,6]
[null,"Footings & Slabs",117,8]
[null,"Footings & Slabs",119,6]
[null,"Footings & Slabs",119,8]
[null,"Footings & Slabs",120,6]
[null,"Footings & Slabs",120,8]
[null,"Footings & Slabs",121,6]
[null,"Footings & Slabs",121,8]
[null,"Footings & Slabs",122,6]
[null,"Footings & Slabs",122,8]
[null,"Footings & Slabs",123,6]
[null,"Footings & Slabs",123,8]
[null,"Footings & Slabs",124,6]
[null,"Footings & Slabs",124,8]
[null,"Footings & Slabs",126,6]
[null,"Footings & Slabs",126,8]
[null,"Footings & Slabs",127,6]
[null,"Footings & Slabs",127,8]
[null,"Footings & Slabs",128,6]
[null,"Footings & Slabs",128,8]
[null,"Footings & Slabs",129,6]
[null,"Footings & Slabs",129,8]
[null,"Footings & Slabs",130,6]
[null,"Footings & Slabs",130,8]
[null,"Footings & Slabs",131,6]
[null,"Footings & Slabs",131,8]
[null,"Footings & Slabs",132,6]
[null,"Footings & Slabs",132,8]
[null,"Footings & Slabs",134,6]
[null,"Footings & Slabs",134,8]
[null,"Footings & Slabs",136,6]
[null,"Footings & Slabs",136,8]
[null,"Footings & Slabs",137,6]
[null,"Footings & Slabs",137,8]
[null,"Footings & Slabs",139,6]
[null,"Footings & Slabs",139,8]
[null,"Footings & Slabs",140,6]
[null,"Footings & Slabs",140,8]
[null,"Footings & Slabs",141,6]
[null,"Footings & Slabs",141,8]
[null,"Footings & Slabs",143,6]
[null,"Footings & Slabs",143,8]
[null,"Foundation Walls",5,5]
[null,"Foundation Walls",5,6]
[null,"Foundation Walls",7,6]
[null,"Foundation Walls",7,8]
[null,"Foundation Walls",8,6]
[null,"Foundation Walls",8,8]
[null,"Foundation Walls",9,6]
[null,"Foundation Walls",9,8]
[null,"Foundation Walls",10,6]
[null,"Foundation Walls",10,8]
[null,"Foundation Walls",11,6]
[null,"Foundation Walls",11,8]
[null,"Foundation Walls",12,6]
[null,"Foundation Walls",12,8]
[null,"Foundation Walls",13,6]
[null,"Foundation Walls",13,8]
[null,"Foundation Walls",15,6]
[null,"Foundation Walls",15,8]
[null,"Foundation Walls",16,6]
[null,"Foundation Walls",16,8]
[null,"Foundation Walls",17,6]
[null,"Foundation Walls",17,8]
[null,"Foundation Walls",18,6]
[null,"Foundation Walls",18,8]
[null,"Foundation Walls",19,6]
[null,"Foundation Walls",19,8]
[null,"Foundation Walls",20,6]
[null,"Foundation Walls",20,8]
[null,"Foundation Walls",21,6]
[null,"Foundation Walls",21,8]
[null,"Foundation Walls",23,6]
[null,"Foundation Walls",23,8]
[null,"Foundation Walls",24,6]
[null,"Foundation Walls",24,8]
[null,"Foundation Walls",25,6]
[null,"Foundation Walls",25,8]
[null,"Foundation Walls",26,6]
[null,"Foundation Walls",26,8]
[null,"Foundation Walls",27,6]
[null,"Foundation Walls",27,8]
[null,"Foundation Walls",28,6]
[null,"Foundation Walls",28,8]
[null,"Foundation Walls",29,6]
[null,"Foundation Walls",29,8]
[null,"Foundation Walls",32,6]
[null,"Foundation Walls",32,8]
[null,"Foundation Walls",33,6]
[null,"Foundation Walls",33,8]
[null,"Foundation Walls",34,6]
[null,"Foundation Walls",34,8]
[null,"Foundation Walls",35,6]
[null,"Foundation Walls",35,8]
[null,"Foundation Walls",36,6]
[null,"Foundation Walls",36,8]
[null,"Foundation Walls",37,6]
[null,"Foundation Walls",37,8]
[null,"Foundation Walls",38,6]
[null,"Foundation Walls",38,8]
[null,"Foundation Walls",40,6]
[null,"Foundation Walls",40,8]
[null,"Foundation Walls",41,5]
[null,"Foundation Walls",42,5]
[null,"Foundation Walls",43,6]
[null,"Foundation Walls",43,8]
[null,"Foundation Walls",44,6]
[null,"Foundation Walls",44,8]
[null,"Foundation Walls",45,6]
[null,"Foundation Walls",45,8]
[null,"Foundation Walls",46,5]
[null,"Foundation Walls",47,6]
[null,"Foundation Walls",47,8]
[null,"Foundation Walls",48,6]
[null,"Foundation Walls",48,8]
[null,"Foundation Walls",49,6]
[null,"Foundation Walls",49,8]
[null,"Foundation Walls",50,6]
[null,"Foundation Walls",50,8]
[null,"Foundation Walls",51,6]
[null,"Foundation Walls",51,8]
[null,"Foundation Walls",52,5]
[null,"Foundation Walls",53,6]
[null,"Foundation Walls",53,8]
[null,"Foundation Walls",54,6]
[null,"Foundation Walls",54,8]
[null,"Foundation Walls",55,6]
[null,"Foundation Walls",55,8]
[null,"Foundation Walls",56,6]
[null,"Foundation Walls",56,8]
[null,"Foundation Walls",57,5]
[null,"Foundation Walls",58,6]
[null,"Foundation Walls",58,8]
[null,"Foundation Walls",59,6]
[null,"Foundation Walls",59,8]
[null,"Foundation Walls",60,6]
[null,"Foundation Walls",60,8]
[null,"Foundation Walls",61,6]
[null,"Foundation Walls",61,8]
[null,"Foundation Walls",62,6]
[null,"Foundation Walls",62,8]
[null,"Foundation Walls",63,6]
[null,"Foundation Walls",63,8]
[null,"Foundation Walls",64,5]
[null,"Foundation Walls",65,6]
[null,"Foundation Walls",65,8]
[null,"Foundation Walls",66,5]
[null,"Foundation Walls",67,6]
[null,"Foundation Walls",67,8]
[null,"Foundation Walls",68,6]
[null,"Foundation Walls",68,8]
[null,"Foundation Walls",69,6]
[null,"Foundation Walls",69,8]
[null,"Foundation Walls",71,6]
[null,"Foundation Walls",71,8]
[null,"Foundation Walls",73,6]
[null,"Foundation Walls",73,8]
[null,"Foundation Walls",74,6]
[null,"Foundation Walls",74,8]
[null,"Foundation Walls",75,6]
[null,"Foundation Walls",75,8]
[null,"Foundation Walls",76,6]
[null,"Foundation Walls",76,8]
[null,"Foundation Walls",77,6]
[null,"Foundation Walls",77,8]
[null,"Foundation Walls",78,6]
[null,"Foundation Walls",78,8]
[null,"Foundation Walls",79,6]
[null,"Foundation Walls",79,8]
[null,"Foundation Walls",81,6]
[null,"Foundation Walls",81,8]
[null,"Foundation Walls",82,6]
[null,"Foundation Walls",82,8]
[null,"Foundation Walls",83,6]
[null,"Foundation Walls",83,8]
[null,"Foundation Walls",84,6]
[null,"Foundation Walls",84,8]
[null,"Foundation Walls",85,6]
[null,"Foundation Walls",85,8]
[null,"Foundation Walls",86,6]
[null,"Foundation Walls",86,8]
[null,"Foundation Walls",87,6]
[null,"Foundation Walls",87,8]
[null,"Foundation Walls",89,6]
[null,"Foundation Walls",89,8]
[null,"Foundation Walls",90,6]
[null,"Foundation Walls",90,8]
[null,"Foundation Walls",91,6]
[null,"Foundation Walls",91,8]
[null,"Foundation Walls",92,6]
[null,"Foundation Walls",92,8]
[null,"Foundation Walls",93,6]
[null,"Foundation Walls",93,8]
[null,"Foundation Walls",94,6]
[null,"Foundation Walls",94,8]
[null,"Foundation Walls",95,6]
[null,"Foundation Walls",95,8]
[null,"Foundation Walls",97,6]
[null,"Foundation Walls",97,8]
[null,"Foundation Walls",98,6]
[null,"Foundation Walls",98,8]
[null,"Foundation Walls",99,6]
[null,"Foundation Walls",99,8]
[null,"Foundation Walls",100,6]
[null,"Foundation Walls",100,8]
[null,"Foundation Walls",102,6]
[null,"Foundation Walls",102,8]
[null,"Foundation Walls",103,6]
[null,"Foundation Walls",103,8]
[null,"Foundation Walls",104,6]
[null,"Foundation Walls",104,8]
[null,"Foundation Walls",105,6]
[null,"Foundation Walls",105,8]
[null,"Foundation Walls",106,6]
[null,"Foundation Walls",106,8]
[null,"Foundation Walls",107,6]
[null,"Foundation Walls",107,8]
[null,"Foundation Walls",108,6]
[null,"Foundation Walls",108,8]
[null,"Foundation Walls",110,6]
[null,"Foundation Walls",110,8]
[null,"Foundation Walls",111,6]
[null,"Foundation Walls",111,8]
[null,"Foundation Walls",112,6]
[null,"Foundation Walls",112,8]
[null,"Foundation Walls",113,6]
[null,"Foundation Walls",113,8]
[null,"Foundation Walls",114,6]
[null,"Foundation Walls",114,8]
[null,"Foundation Walls",115,6]
[null,"Foundation Walls",115,8]
[null,"Foundation Walls",116,6]
[null,"Foundation Walls",116,8]
[null,"Foundation Walls",118,6]
[null,"Foundation Walls",118,8]
[null,"Foundation Walls",119,6]
[null,"Foundation Walls",119,8]
[null,"Foundation Walls",120,6]
[null,"Foundation Walls",120,8]
[null,"Foundation Walls",121,6]
[null,"Foundation Walls",121,8]
[null,"Foundation Walls",122,6]
[null,"Foundation Walls",122,8]
[null,"Foundation Walls",123,6]
[null,"Foundation Walls",123,8]
[null,"Foundation Walls",124,6]
[null,"Foundation Walls",124,8]
[null,"Foundation Walls",125,5]
[null,"Foundation Walls",127,6]
[null,"Foundation Walls",127,8]
[null,"Foundation Walls",128,6]
[null,"Foundation Walls",128,8]
[null,"Foundation Walls",129,6]
[null,"Foundation Walls",129,8]
[null,"Foundation Walls",130,6]
[null,"Foundation Walls",130,8]
[null,"Foundation Walls",131,5]
[null,"Foundation Walls",133,6]
[null,"Foundation Walls",133,8]
[null,"Foundation Walls",134,6]
[null,"Foundation Walls",134,8]
[null,"Foundation Walls",135,6]
[null,"Foundation Walls",135,8]
[null,"Foundation Walls",136,6]
[null,"Foundation Walls",136,8]
[null,"Foundation Walls",137,6]
[null,"Foundation Walls",137,8]
[null,"Foundation Walls",138,5]
[null,"Foundation Walls",139,5]
[null,"Foundation Walls",140,6]
[null,"Foundation Walls",140,8]
[null,"Foundation Walls",141,6]
[null,"Foundation Walls",141,8]
[null,"Foundation Walls",142,6]
[null,"Foundation Walls",142,8]
[null,"Foundation Walls",143,5]
[null,"Foundation Walls",144,6]
[null,"Foundation Walls",144,8]
[null,"Foundation Walls",145,6]
[null,"Foundation Walls",145,8]
[null,"Foundation Walls",146,6]
[null,"Foundation Walls",146,8]
[null,"Foundation Walls",147,6]
[null,"Foundation Walls",147,8]
[null,"Foundation Walls",148,5]
[null,"Foundation Walls",149,6]
[null,"Foundation Walls",149,8]
[null,"Foundation Walls",150,6]
[null,"Foundation Walls",150,8]
[null,"Foundation Walls",151,6]
[null,"Foundation Walls",151,8]
[null,"Foundation Walls",152,6]
[null,"Foundation Walls",152,8]
[null,"Foundation Walls",153,5]
[null,"Foundation Walls",154,6]
[null,"Foundation Walls",154,8]
[null,"Foundation Walls",155,6]
[null,"Foundation Walls",155,8]
[null,"Foundation Walls",156,6]
[null,"Foundation Walls",156,8]
[null,"Foundation Walls",157,6]
[null,"Foundation Walls",157,8]
[null,"Foundation Walls",158,6]
[null,"Foundation Walls",158,8]
[null,"Foundation Walls",159,6]
[null,"Foundation Walls",159,8]
[null,"Foundation Walls",160,6]
[null,"Foundation Walls",160,8]
[null,"Foundation Walls",161,6]
[null,"Foundation Walls",161,8]
[null,"Foundation Walls",162,5]
[null,"Foundation Walls",163,6]
[null,"Foundation Walls",163,8]
[null,"Foundation Walls",164,6]
[null,"Foundation Walls",164,8]
[null,"Foundation Walls",165,6]
[null,"Foundation Walls",165,8]
[null,"Foundation Walls",166,6]
[null,"Foundation Walls",166,8]
[null,"Foundation Walls",167,5]
[null,"Foundation Walls",168,6]
[null,"Foundation Walls",168,8]
[null,"Foundation Walls",169,6]
[null,"Foundation Walls",169,8]
[null,"Foundation Walls",170,6]
[null,"Foundation Walls",170,8]
[null,"Foundation Walls",171,5]
[null,"Foundation Walls",172,6]
[null,"Foundation Walls",172,8]
[null,"Foundation Walls",173,6]
[null,"Foundation Walls",173,8]
[null,"Foundation Walls",174,6]
[null,"Foundation Walls",174,8]
[null,"Foundation Walls",175,6]
[null,"Foundation Walls",175,8]
[null,"Foundation Walls",176,5]
[null,"Foundation Walls",177,6]
[null,"Foundation Walls",177,8]
[null,"Foundation Walls",178,6]
[null,"Foundation Walls",178,8]
[null,"Foundation Walls",181,6]
[null,"Foundation Walls",181,8]
[null,"Foundation Walls",182,6]
[null,"Foundation Walls",182,8]
[null,"Foundation Walls",183,6]
[null,"Foundation Walls",183,8]
[null,"Foundation Walls",184,6]
[null,"Foundation Walls",184,8]
[null,"Foundation Walls",185,6]
[null,"Foundation Walls",185,8]
[null,"Foundation Walls",186,6]
[null,"Foundation Walls",186,8]
[null,"Foundation Walls",188,6]
[null,"Foundation Walls",188,8]
[null,"Foundation Walls",189,6]
[null,"Foundation Walls",189,8]
[null,"Foundation Walls",190,6]
[null,"Foundation Walls",190,8]
[null,"Foundation Walls",192,6]
[null,"Foundation Walls",192,8]
[null,"Foundation Walls",193,6]
[null,"Foundation Walls",193,8]
[null,"Foundation Walls",194,6]
[null,"Foundation Walls",194,8]
[null,"Foundation Walls",195,6]
[null,"Foundation Walls",195,8]
[null,"Foundation Walls",196,6]
[null,"Foundation Walls",196,8]
[null,"Foundation Walls",197,6]
[null,"Foundation Walls",197,8]
[null,"Foundation Walls",198,6]
[null,"Foundation Walls",198,8]
[null,"Foundation Walls",199,6]
[null,"Foundation Walls",199,8]
[null,"Foundation Walls",200,6]
[null,"Foundation Walls",200,8]
[null,"Structural Elements",7,6]
[null,"Structural Elements",7,8]
[null,"Structural Elements",8,6]
[null,"Structural Elements",8,8]
[null,"Structural Elements",9,6]
[null,"Structural Elements",9,8]
[null,"Structural Elements",10,6]
[null,"Structural Elements",10,8]
[null,"Structural Elements",11,6]
[null,"Structural Elements",11,8]
[null,"Structural Elements",12,6]
[null,"Structural Elements",12,8]
[null,"Structural Elements",13,6]
[null,"Structural Elements",13,8]
[null,"Structural Elements",16,4]
[null,"Structural Elements",16,6]
[null,"Structural Elements",16,8]
[null,"Structural Elements",17,3]
[null,"Structural Elements",17,4]
[null,"Structural Elements",17,6]
[null,"Structural Elements",17,8]
[null,"Structural Elements",18,4]
[null,"Structural Elements",18,6]
[null,"Structural Elements",18,8]
[null,"Ext. Walls",5,5]
[null,"Ext. Walls",7,6]
[null,"Ext. Walls",7,8]
[null,"Ext. Walls",8,6]
[null,"Ext. Walls",8,8]
[null,"Ext. Walls",9,6]
[null,"Ext. Walls",9,8]
[null,"Ext. Walls",10,6]
[null,"Ext. Walls",10,8]
[null,"Ext. Walls",11,5]
[null,"Ext. Walls",13,6]
[null,"Ext. Walls",13,8]
[null,"Ext. Walls",14,6]
[null,"Ext. Walls",14,8]
[null,"Ext. Walls",15,6]
[null,"Ext. Walls",15,8]
[null,"Ext. Walls",16,6]
[null,"Ext. Walls",16,8]
[null,"Ext. Walls",17,6]
[null,"Ext. Walls",17,8]
[null,"Ext. Walls",18,6]
[null,"Ext. Walls",18,8]
[null,"Ext. Walls",19,5]
[null,"Ext. Walls",20,6]
[null,"Ext. Walls",20,8]
[null,"Ext. Walls",21,6]
[null,"Ext. Walls",21,8]
[null,"Ext. Walls",24,6]
[null,"Ext. Walls",24,8]
[null,"Ext. Walls",25,6]
[null,"Ext. Walls",25,8]
[null,"Ext. Walls",26,6]
[null,"Ext. Walls",26,8]
[null,"Ext. Walls",27,6]
[null,"Ext. Walls",27,8]
[null,"Ext. Walls",30,6]
[null,"Ext. Walls",30,8]
[null,"Ext. Walls",31,6]
[null,"Ext. Walls",31,8]
[null,"Ext. Walls",32,6]
[null,"Ext. Walls",32,8]
[null,"Ext. Walls",33,6]
[null,"Ext. Walls",33,8]
[null,"Ext. Walls",34,6]
[null,"Ext. Walls",34,8]
[null,"Ext. Walls",35,6]
[null,"Ext. Walls",35,8]
[null,"Ext. Walls",36,6]
[null,"Ext. Walls",36,8]
[null,"Ext. Walls",37,5]
[null,"Ext. Walls",39,6]
[null,"Ext. Walls",39,8]
[null,"Ext. Walls",40,6]
[null,"Ext. Walls",40,8]
[null,"Ext. Walls",41,6]
[null,"Ext. Walls",41,8]
[null,"Ext. Walls",42,6]
[null,"Ext. Walls",42,8]
[null,"Ext. Walls",43,6]
[null,"Ext. Walls",43,8]
[null,"Ext. Walls",44,6]
[null,"Ext. Walls",44,8]
[null,"Ext. Walls",45,6]
[null,"Ext. Walls",45,8]
[null,"Ext. Walls",47,6]
[null,"Ext. Walls",47,8]
[null,"Ext. Walls",48,6]
[null,"Ext. Walls",48,8]
[null,"Ext. Walls",49,6]
[null,"Ext. Walls",49,8]
[null,"Ext. Walls",50,6]
[null,"Ext. Walls",50,8]
[null,"Ext. Walls",51,6]
[null,"Ext. Walls",51,8]
[null,"Ext. Walls",52,6]
[null,"Ext. Walls",52,8]
[null,"Ext. Walls",53,6]
[null,"Ext. Walls",53,8]
[null,"Ext. Walls",56,6]
[null,"Ext. Walls",56,8]
[null,"Ext. Walls",57,6]
[null,"Ext. Walls",57,8]
[null,"Ext. Walls",58,6]
[null,"Ext. Walls",58,8]
[null,"Ext. Walls",59,6]
[null,"Ext. Walls",59,8]
[null,"Ext. Walls",61,6]
[null,"Ext. Walls",61,8]
[null,"Ext. Walls",62,6]
[null,"Ext. Walls",62,8]
[null,"Ext. Walls",63,6]
[null,"Ext. Walls",63,8]
[null,"Ext. Walls",65,6]
[null,"Ext. Walls",65,8]
[null,"Ext. Walls",66,6]
[null,"Ext. Walls",66,8]
[null,"Ext. Walls",67,6]
[null,"Ext. Walls",67,8]
[null,"Ext. Walls",69,6]
[null,"Ext. Walls",69,8]
[null,"Ext. Walls",70,6]
[null,"Ext. Walls",70,8]
[null,"Ext. Walls",71,5]
[null,"Ext. Walls",72,5]
[null,"Ext. Walls",73,6]
[null,"Ext. Walls",73,8]
[null,"Ext. Walls",74,6]
[null,"Ext. Walls",74,8]
[null,"Ext. Walls",75,6]
[null,"Ext. Walls",75,8]
[null,"Ext. Walls",76,6]
[null,"Ext. Walls",76,8]
[null,"Ext. Walls",77,5]
[null,"Ext. Walls",78,6]
[null,"Ext. Walls",78,8]
[null,"Ext. Walls",79,6]
[null,"Ext. Walls",79,8]
[null,"Ext. Walls",80,6]
[null,"Ext. Walls",80,8]
[null,"Ext. Walls",81,6]
[null,"Ext. Walls",81,8]
[null,"Ext. Walls",82,6]
[null,"Ext. Walls",82,8]
[null,"Ext. Walls",83,5]
[null,"Ext. Walls",84,6]
[null,"Ext. Walls",84,8]
[null,"Ext. Walls",85,6]
[null,"Ext. Walls",85,8]
[null,"Ext. Walls",86,6]
[null,"Ext. Walls",86,8]
[null,"Ext. Walls",87,6]
[null,"Ext. Walls",87,8]
[null,"Ext. Walls",88,6]
[null,"Ext. Walls",88,8]
[null,"Ext. Walls",89,6]
[null,"Ext. Walls",89,8]
[null,"Ext. Walls",90,6]
[null,"Ext. Walls",90,8]
[null,"Ext. Walls",91,5]
[null,"Ext. Walls",92,6]
[null,"Ext. Walls",92,8]
[null,"Ext. Walls",93,6]
[null,"Ext. Walls",93,8]
[null,"Ext. Walls",94,6]
[null,"Ext. Walls",94,8]
[null,"Ext. Walls",95,6]
[null,"Ext. Walls",95,8]
[null,"Ext. Walls",96,5]
[null,"Ext. Walls",97,6]
[null,"Ext. Walls",97,8]
[null,"Ext. Walls",98,6]
[null,"Ext. Walls",98,8]
[null,"Ext. Walls",99,6]
[null,"Ext. Walls",99,8]
[null,"Ext. Walls",100,6]
[null,"Ext. Walls",100,8]
[null,"Ext. Walls",101,6]
[null,"Ext. Walls",101,8]
[null,"Ext. Walls",102,5]
[null,"Ext. Walls",103,6]
[null,"Ext. Walls",103,8]
[null,"Ext. Walls",104,6]
[null,"Ext. Walls",104,8]
[null,"Ext. Walls",105,6]
[null,"Ext. Walls",105,8]
[null,"Ext. Walls",106,6]
[null,"Ext. Walls",106,8]
[null,"Ext. Walls",107,6]
[null,"Ext. Walls",107,8]
[null,"Ext. Walls",108,5]
[null,"Ext. Walls",109,6]
[null,"Ext. Walls",109,8]
[null,"Ext. Walls",110,6]
[null,"Ext. Walls",110,8]
[null,"Ext. Walls",111,6]
[null,"Ext. Walls",111,8]
[null,"Ext. Walls",112,5]
[null,"Ext. Walls",113,6]
[null,"Ext. Walls",113,8]
[null,"Ext. Walls",114,6]
[null,"Ext. Walls",114,8]
[null,"Ext. Walls",115,5]
[null,"Ext. Walls",116,6]
[null,"Ext. Walls",116,8]
[null,"Ext. Walls",117,6]
[null,"Ext. Walls",117,8]
[null,"Ext. Walls",118,6]
[null,"Ext. Walls",118,8]
[null,"Ext. Walls",119,6]
[null,"Ext. Walls",119,8]
[null,"Ext. Walls",120,5]
[null,"Ext. Walls",121,5]
[null,"Ext. Walls",122,6]
[null,"Ext. Walls",122,8]
[null,"Ext. Walls",123,6]
[null,"Ext. Walls",123,8]
[null,"Ext. Walls",124,6]
[null,"Ext. Walls",124,8]
[null,"Ext. Walls",125,5]
[null,"Ext. Walls",126,6]
[null,"Ext. Walls",126,8]
[null,"Ext. Walls",127,6]
[null,"Ext. Walls",127,8]
[null,"Ext. Walls",128,6]
[null,"Ext. Walls",128,8]
[null,"Ext. Walls",129,6]
[null,"Ext. Walls",129,8]
[null,"Ext. Walls",130,6]
[null,"Ext. Walls",130,8]
[null,"Ext. Walls",131,6]
[null,"Ext. Walls",131,8]
[null,"Ext. Walls",132,5]
[null,"Ext. Walls",133,6]
[null,"Ext. Walls",133,8]
[null,"Ext. Walls",134,6]
[null,"Ext. Walls",134,8]
[null,"Ext. Walls",135,6]
[null,"Ext. Walls",135,8]
[null,"Ext. Walls",136,6]
[null,"Ext. Walls",136,8]
[null,"Ext. Walls",137,6]
[null,"Ext. Walls",137,8]
[null,"Ext. Walls",138,5]
[null,"Ext. Walls",139,6]
[null,"Ext. Walls",139,8]
[null,"Ext. Walls",140,6]
[null,"Ext. Walls",140,8]
[null,"Ext. Walls",141,6]
[null,"Ext. Walls",141,8]
[null,"Ext. Walls",142,6]
[null,"Ext. Walls",142,8]
[null,"Ext. Walls",143,6]
[null,"Ext. Walls",143,8]
[null,"Ext. Walls",144,5]
[null,"Ext. Walls",145,6]
[null,"Ext. Walls",145,8]
[null,"Ext. Walls",146,6]
[null,"Ext. Walls",146,8]
[null,"Ext. Walls",147,6]
[null,"Ext. Walls",147,8]
[null,"Ext. Walls",148,6]
[null,"Ext. Walls",148,8]
[null,"Ext. Walls",149,5]
[null,"Ext. Walls",150,6]
[null,"Ext. Walls",150,8]
[null,"Ext. Walls",151,6]
[null,"Ext. Walls",151,8]
[null,"Ext. Wall Systems",6,6]
[null,"Ext. Wall Systems",6,8]
[null,"Ext. Wall Systems",8,6]
[null,"Ext. Wall Systems",8,8]
[null,"Ext. Wall Systems",9,6]
[null,"Ext. Wall Systems",9,8]
[null,"Ext. Wall Systems",10,6]
[null,"Ext. Wall Systems",10,8]
[null,"Ext. Wall Systems",11,6]
[null,"Ext. Wall Systems",11,8]
[null,"Ext. Wall Systems",12,6]
[null,"Ext. Wall Systems",12,8]
[null,"Ext. Wall Systems",13,6]
[null,"Ext. Wall Systems",13,8]
[null,"Ext. Wall Systems",14,6]
[null,"Ext. Wall Systems",14,8]
[null,"Ext. Wall Systems",16,6]
[null,"Ext. Wall Systems",16,8]
[null,"Ext. Wall Systems",17,6]
[null,"Ext. Wall Systems",17,8]
[null,"Ext. Wall Systems",18,6]
[null,"Ext. Wall Systems",18,8]
[null,"Ext. Wall Systems",19,6]
[null,"Ext. Wall Systems",19,8]
[null,"Ext. Wall Systems",20,6]
[null,"Ext. Wall Systems",20,8]
[null,"Ext. Wall Systems",21,6]
[null,"Ext. Wall Systems",21,8]
[null,"Ext. Wall Systems",22,6]
[null,"Ext. Wall Systems",22,8]
[null,"Ext. Wall Systems",24,6]
[null,"Ext. Wall Systems",24,8]
[null,"Ext. Wall Systems",25,6]
[null,"Ext. Wall Systems",25,8]
[null,"Ext. Wall Systems",26,6]
[null,"Ext. Wall Systems",26,8]
[null,"Ext. Wall Systems",27,6]
[null,"Ext. Wall Systems",27,8]
[null,"Ext. Wall Systems",28,6]
[null,"Ext. Wall Systems",28,8]
[null,"Ext. Wall Systems",29,6]
[null,"Ext. Wall Systems",29,8]
[null,"Ext. Wall Systems",30,6]
[null,"Ext. Wall Systems",30,8]
[null,"Ext. Wall Systems",32,6]
[null,"Ext. Wall Systems",32,8]
[null,"Ext. Wall Systems",33,6]
[null,"Ext. Wall Systems",33,8]
[null,"Ext. Wall Systems",34,6]
[null,"Ext. Wall Systems",34,8]
[null,"Ext. Wall Systems",35,6]
[null,"Ext. Wall Systems",35,8]
[null,"Ext. Wall Systems",37,6]
[null,"Ext. Wall Systems",37,8]
[null,"Ext. Wall Systems",38,6]
[null,"Ext. Wall Systems",38,8]
[null,"Ext. Wall Systems",39,6]
[null,"Ext. Wall Systems",39,8]
[null,"Ext. Wall Systems",40,6]
[null,"Ext. Wall Systems",40,8]
[null,"Ext. Wall Systems",41,6]
[null,"Ext. Wall Systems",41,8]
[null,"Ext. Wall Systems",42,6]
[null,"Ext. Wall Systems",42,8]
[null,"Ext. Wall Systems",43,6]
[null,"Ext. Wall Systems",43,8]
[null,"Ext. Wall Systems",45,6]
[null,"Ext. Wall Systems",45,8]
[null,"Ext. Wall Systems",46,6]
[null,"Ext. Wall Systems",46,8]
[null,"Ext. Wall Systems",47,6]
[null,"Ext. Wall Systems",47,8]
[null,"Ext. Wall Systems",48,6]
[null,"Ext. Wall Systems",48,8]
[null,"Ext. Wall Systems",49,6]
[null,"Ext. Wall Systems",49,8]
[null,"Ext. Wall Systems",50,6]
[null,"Ext. Wall Systems",50,8]
[null,"Ext. Wall Systems",51,6]
[null,"Ext. Wall Systems",51,8]
[null,"Ext. Wall Systems",53,6]
[null,"Ext. Wall Systems",53,8]
[null,"Ext. Wall Systems",54,6]
[null,"Ext. Wall Systems",54,8]
[null,"Ext. Wall Systems",55,6]
[null,"Ext. Wall Systems",55,8]
[null,"Ext. Wall Systems",56,6]
[null,"Ext. Wall Systems",56,8]
[null,"Ext. Wall Systems",57,6]
[null,"Ext. Wall Systems",57,8]
[null,"Ext. Wall Systems",58,6]
[null,"Ext. Wall Systems",58,8]
[null,"Ext. Wall Systems",59,6]
[null,"Ext. Wall Systems",59,8]
[null,"Ext. Wall Systems",62,6]
[null,"Ext. Wall Systems",62,8]
[null,"Ext. Wall Systems",63,6]
[null,"Ext. Wall Systems",63,8]
[null,"Ext. Wall Systems",65,6]
[null,"Ext. Wall Systems",65,8]
[null,"Ext. Wall Systems",66,6]
[null,"Ext. Wall Systems",66,8]
[null,"Ext. Wall Systems",67,6]
[null,"Ext. Wall Systems",67,8]
[null,"Ext. Wall Systems",68,6]
[null,"Ext. Wall Systems",68,8]
[null,"Party Walls",7,5]
[null,"Party Walls",9,6]
[null,"Party Walls",9,8]
[null,"Party Walls",10,6]
[null,"Party Walls",10,8]
[null,"Party Walls",11,6]
[null,"Party Walls",11,8]
[null,"Party Walls",12,6]
[null,"Party Walls",12,8]
[null,"Party Walls",13,5]
[null,"Party Walls",15,6]
[null,"Party Walls",15,8]
[null,"Party Walls",16,6]
[null,"Party Walls",16,8]
[null,"Party Walls",17,6]
[null,"Party Walls",17,8]
[null,"Party Walls",18,6]
[null,"Party Walls",18,8]
[null,"Party Walls",19,6]
[null,"Party Walls",19,8]
[null,"Party Walls",20,6]
[null,"Party Walls",20,8]
[null,"Party Walls",22,6]
[null,"Party Walls",22,8]
[null,"Party Walls",23,6]
[null,"Party Walls",23,8]
[null,"Party Walls",24,6]
[null,"Party Walls",24,8]
[null,"Party Walls",25,6]
[null,"Party Walls",25,8]
[null,"Party Walls",26,6]
[null,"Party Walls",26,8]
[null,"Party Walls",27,6]
[null,"Party Walls",27,8]
[null,"Party Walls",31,6]
[null,"Party Walls",31,8]
[null,"Party Walls",32,6]
[null,"Party Walls",32,8]
[null,"Party Walls",33,6]
[null,"Party Walls",33,8]
[null,"Party Walls",34,6]
[null,"Party Walls",34,8]
[null,"Party Walls",35,6]
[null,"Party Walls",35,8]
[null,"Party Walls",36,6]
[null,"Party Walls",36,8]
[null,"Party Walls",37,6]
[null,"Party Walls",37,8]
[null,"Party Walls",38,5]
[null,"Party Walls",40,6]
[null,"Party Walls",40,8]
[null,"Party Walls",41,6]
[null,"Party Walls",41,8]
[null,"Party Walls",42,6]
[null,"Party Walls",42,8]
[null,"Party Walls",43,6]
[null,"Party Walls",43,8]
[null,"Party Walls",44,6]
[null,"Party Walls",44,8]
[null,"Party Walls",45,6]
[null,"Party Walls",45,8]
[null,"Party Walls",46,6]
[null,"Party Walls",46,8]
[null,"Party Walls",48,6]
[null,"Party Walls",48,8]
[null,"Party Walls",49,6]
[null,"Party Walls",49,8]
[null,"Party Walls",50,6]
[null,"Party Walls",50,8]
[null,"Party Walls",51,6]
[null,"Party Walls",51,8]
[null,"Party Walls",52,6]
[null,"Party Walls",52,8]
[null,"Party Walls",53,6]
[null,"Party Walls",53,8]
[null,"Party Walls",54,6]
[null,"Party Walls",54,8]
[null,"Party Walls",56,5]
[null,"Party Walls",57,5]
[null,"Party Walls",58,6]
[null,"Party Walls",58,8]
[null,"Party Walls",59,6]
[null,"Party Walls",59,8]
[null,"Party Walls",60,6]
[null,"Party Walls",60,8]
[null,"Party Walls",61,6]
[null,"Party Walls",61,8]
[null,"Party Walls",62,5]
[null,"Party Walls",63,6]
[null,"Party Walls",63,8]
[null,"Party Walls",64,6]
[null,"Party Walls",64,8]
[null,"Party Walls",65,6]
[null,"Party Walls",65,8]
[null,"Party Walls",66,6]
[null,"Party Walls",66,8]
[null,"Party Walls",67,6]
[null,"Party Walls",67,8]
[null,"Party Walls",68,5]
[null,"Party Walls",69,6]
[null,"Party Walls",69,8]
[null,"Party Walls",70,6]
[null,"Party Walls",70,8]
[null,"Party Walls",71,6]
[null,"Party Walls",71,8]
[null,"Party Walls",72,6]
[null,"Party Walls",72,8]
[null,"Party Walls",73,6]
[null,"Party Walls",73,8]
[null,"Party Walls",74,6]
[null,"Party Walls",74,8]
[null,"Party Walls",75,6]
[null,"Party Walls",75,8]
[null,"Party Walls",76,5]
[null,"Party Walls",77,6]
[null,"Party Walls",77,8]
[null,"Party Walls",78,6]
[null,"Party Walls",78,8]
[null,"Party Walls",79,6]
[null,"Party Walls",79,8]
[null,"Party Walls",80,6]
[null,"Party Walls",80,8]
[null,"Party Walls",81,5]
[null,"Party Walls",82,6]
[null,"Party Walls",82,8]
[null,"Party Walls",83,6]
[null,"Party Walls",83,8]
[null,"Party Walls",84,6]
[null,"Party Walls",84,8]
[null,"Party Walls",85,6]
[null,"Party Walls",85,8]
[null,"Party Walls",86,6]
[null,"Party Walls",86,8]
[null,"Party Walls",87,5]
[null,"Party Walls",88,6]
[null,"Party Walls",88,8]
[null,"Party Walls",89,6]
[null,"Party Walls",89,8]
[null,"Party Walls",90,6]
[null,"Party Walls",90,8]
[null,"Party Walls",91,6]
[null,"Party Walls",91,8]
[null,"Party Walls",92,6]
[null,"Party Walls",92,8]
[null,"Party Walls",93,5]
[null,"Party Walls",94,6]
[null,"Party Walls",94,8]
[null,"Party Walls",95,6]
[null,"Party Walls",95,8]
[null,"Party Walls",96,6]
[null,"Party Walls",96,8]
[null,"Party Walls",97,5]
[null,"Party Walls",98,6]
[null,"Party Walls",98,8]
[null,"Party Walls",99,6]
[null,"Party Walls",99,8]
[null,"Party Walls",100,5]
[null,"Party Walls",101,6]
[null,"Party Walls",101,8]
[null,"Party Walls",102,6]
[null,"Party Walls",102,8]
[null,"Party Walls",103,6]
[null,"Party Walls",103,8]
[null,"Party Walls",104,6]
[null,"Party Walls",104,8]
[null,"Party Walls",105,5]
[null,"Party Walls",106,5]
[null,"Party Walls",107,6]
[null,"Party Walls",107,8]
[null,"Party Walls",108,6]
[null,"Party Walls",108,8]
[null,"Party Walls",109,6]
[null,"Party Walls",109,8]
[null,"Party Walls",110,5]
[null,"Party Walls",111,6]
[null,"Party Walls",111,8]
[null,"Party Walls",112,6]
[null,"Party Walls",112,8]
[null,"Party Walls",113,6]
[null,"Party Walls",113,8]
[null,"Party Walls",114,6]
[null,"Party Walls",114,8]
[null,"Party Walls",115,6]
[null,"Party Walls",115,8]
[null,"Party Walls",116,6]
[null,"Party Walls",116,8]
[null,"Party Walls",117,5]
[null,"Party Walls",118,6]
[null,"Party Walls",118,8]
[null,"Party Walls",119,6]
[null,"Party Walls",119,8]
[null,"Party Walls",120,6]
[null,"Party Walls",120,8]
[null,"Party Walls",121,6]
[null,"Party Walls",121,8]
[null,"Party Walls",122,6]
[null,"Party Walls",122,8]
[null,"Party Walls",123,5]
[null,"Party Walls",124,6]
[null,"Party Walls",124,8]
[null,"Party Walls",125,6]
[null,"Party Walls",125,8]
[null,"Party Walls",126,6]
[null,"Party Walls",126,8]
[null,"Party Walls",127,6]
[null,"Party Walls",127,8]
[null,"Party Walls",128,6]
[null,"Party Walls",128,8]
[null,"Party Walls",129,5]
[null,"Party Walls",130,6]
[null,"Party Walls",130,8]
[null,"Party Walls",131,6]
[null,"Party Walls",131,8]
[null,"Party Walls",132,6]
[null,"Party Walls",132,8]
[null,"Party Walls",133,6]
[null,"Party Walls",133,8]
[null,"Party Walls",137,6]
[null,"Party Walls",137,8]
[null,"Party Walls",138,6]
[null,"Party Walls",138,8]
[null,"Party Walls",139,6]
[null,"Party Walls",139,8]
[null,"Party Walls",140,6]
[null,"Party Walls",140,8]
[null,"Party Walls",141,6]
[null,"Party Walls",141,8]
[null,"Party Walls",142,6]
[null,"Party Walls",142,8]
[null,"Party Walls",144,6]
[null,"Party Walls",144,8]
[null,"Party Walls",145,6]
[null,"Party Walls",145,8]
[null,"Party Walls",146,6]
[null,"Party Walls",146,8]
[null,"Party Walls",148,6]
[null,"Party Walls",148,8]
[null,"Party Walls",149,6]
[null,"Party Walls",149,8]
[null,"Party Walls",150,6]
[null,"Party Walls",150,8]
[null,"Party Walls",151,6]
[null,"Party Walls",151,8]
[null,"Party Walls",152,6]
[null,"Party Walls",152,8]
[null,"Party Walls",153,6]
[null,"Party Walls",153,8]
[null,"Party Walls",154,6]
[null,"Party Walls",154,8]
[null,"Party Walls",155,6]
[null,"Party Walls",155,8]
[null,"Party Walls",156,6]
[null,"Party Walls",156,8]
[null,"Party Walls",157,6]
[null,"Party Walls",157,8]
[null,"Party Walls",160,6]
[null,"Party Walls",160,8]
[null,"Party Walls",161,6]
[null,"Party Walls",161,8]
[null,"Party Walls",162,6]
[null,"Party Walls",162,8]
[null,"Party Walls",163,6]
[null,"Party Walls",163,8]
[null,"Party Walls",165,6]
[null,"Party Walls",165,8]
[null,"Party Walls",166,6]
[null,"Party Walls",166,8]
[null,"Party Walls",167,6]
[null,"Party Walls",167,8]
[null,"Party Walls",169,6]
[null,"Party Walls",169,8]
[null,"Party Walls",170,6]
[null,"Party Walls",170,8]
[null,"Party Walls",171,6]
[null,"Party Walls",171,8]
[null,"Party Walls",173,6]
[null,"Party Walls",173,8]
[null,"Party Walls",174,6]
[null,"Party Walls",174,8]
[null,"Party Walls",177,6]
[null,"Party Walls",177,8]
[null,"Party Walls",179,6]
[null,"Party Walls",179,8]
[null,"Party Walls",180,6]
[null,"Party Walls",180,8]
[null,"Party Walls",181,6]
[null,"Party Walls",181,8]
[null,"Party Walls",182,6]
[null,"Party Walls",182,8]
[null,"Party Walls",183,6]
[null,"Party Walls",183,8]
[null,"Party Walls",184,6]
[null,"Party Walls",184,8]
[null,"Party Walls",185,6]
[null,"Party Walls",185,8]
[null,"Party Walls",187,6]
[null,"Party Walls",187,8]
[null,"Party Walls",188,6]
[null,"Party Walls",188,8]
[null,"Party Walls",189,6]
[null,"Party Walls",189,8]
[null,"Party Walls",190,6]
[null,"Party Walls",190,8]
[null,"Party Walls",191,6]
[null,"Party Walls",191,8]
[null,"Party Walls",192,6]
[null,"Party Walls",192,8]
[null,"Party Walls",193,6]
[null,"Party Walls",193,8]
[null,"Party Walls",195,6]
[null,"Party Walls",195,8]
[null,"Party Walls",196,6]
[null,"Party Walls",196,8]
[null,"Party Walls",197,6]
[null,"Party Walls",197,8]
[null,"Party Walls",198,6]
[null,"Party Walls",198,8]
[null,"Party Walls",199,6]
[null,"Party Walls",199,8]
[null,"Party Walls",200,6]
[null,"Party Walls",200,8]
[null,"Party Walls",201,6]
[null,"Party Walls",201,8]
[null,"Party Walls",203,6]
[null,"Party Walls",203,8]
[null,"Party Walls",204,6]
[null,"Party Walls",204,8]
[null,"Party Walls",205,6]
[null,"Party Walls",205,8]
[null,"Party Walls",206,6]
[null,"Party Walls",206,8]
[null,"Party Walls",208,6]
[null,"Party Walls",208,8]
[null,"Party Walls",209,6]
[null,"Party Walls",209,8]
[null,"Party Walls",210,6]
[null,"Party Walls",210,8]
[null,"Party Walls",211,6]
[null,"Party Walls",211,8]
[null,"Party Walls",212,6]
[null,"Party Walls",212,8]
[null,"Party Walls",213,6]
[null,"Party Walls",213,8]
[null,"Party Walls",214,6]
[null,"Party Walls",214,8]
[null,"Party Walls",216,6]
[null,"Party Walls",216,8]
[null,"Party Walls",217,6]
[null,"Party Walls",217,8]
[null,"Party Walls",218,6]
[null,"Party Walls",218,8]
[null,"Party Walls",219,6]
[null,"Party Walls",219,8]
[null,"Party Walls",220,6]
[null,"Party Walls",220,8]
[null,"Party Walls",221,6]
[null,"Party Walls",221,8]
[null,"Party Walls",222,6]
[null,"Party Walls",222,8]
[null,"Party Walls",224,6]
[null,"Party Walls",224,8]
[null,"Party Walls",225,6]
[null,"Party Walls",225,8]
[null,"Party Walls",226,6]
[null,"Party Walls",226,8]
[null,"Party Walls",227,6]
[null,"Party Walls",227,8]
[null,"Party Walls",228,6]
[null,"Party Walls",228,8]
[null,"Party Walls",229,6]
[null,"Party Walls",229,8]
[null,"Party Walls",230,6]
[null,"Party Walls",230,8]
[null,"Cladding",7,6]
[null,"Cladding",7,8]
[null,"Cladding",8,6]
[null,"Cladding",8,8]
[null,"Cladding",9,6]
[null,"Cladding",9,8]
[null,"Cladding",10,6]
[null,"Cladding",10,8]
[null,"Cladding",11,6]
[null,"Cladding",11,8]
[null,"Cladding",12,6]
[null,"Cladding",12,8]
[null,"Cladding",13,6]
[null,"Cladding",13,8]
[null,"Cladding",15,6]
[null,"Cladding",15,8]
[null,"Cladding",16,6]
[null,"Cladding",16,8]
[null,"Cladding",18,6]
[null,"Cladding",18,8]
[null,"Cladding",19,6]
[null,"Cladding",19,8]
[null,"Cladding",20,6]
[null,"Cladding",20,8]
[null,"Cladding",21,6]
[null,"Cladding",21,8]
[null,"Cladding",22,6]
[null,"Cladding",22,8]
[null,"Cladding",23,6]
[null,"Cladding",23,8]
[null,"Cladding",24,6]
[null,"Cladding",24,8]
[null,"Cladding",25,6]
[null,"Cladding",25,8]
[null,"Cladding",26,6]
[null,"Cladding",26,8]
[null,"Cladding",28,6]
[null,"Cladding",28,8]
[null,"Cladding",30,6]
[null,"Cladding",30,8]
[null,"Cladding",31,6]
[null,"Cladding",31,8]
[null,"Cladding",32,6]
[null,"Cladding",32,8]
[null,"Cladding",34,6]
[null,"Cladding",34,8]
[null,"Cladding",35,6]
[null,"Cladding",35,8]
[null,"Cladding",36,6]
[null,"Cladding",36,8]
[null,"Cladding",37,6]
[null,"Cladding",37,8]
[null,"Cladding",38,6]
[null,"Cladding",38,8]
[null,"Cladding",39,6]
[null,"Cladding",39,8]
[null,"Cladding",40,6]
[null,"Cladding",40,8]
[null,"Cladding",42,6]
[null,"Cladding",42,8]
[null,"Cladding",43,6]
[null,"Cladding",43,8]
[null,"Cladding",44,6]
[null,"Cladding",44,8]
[null,"Cladding",46,6]
[null,"Cladding",46,8]
[null,"Cladding",47,6]
[null,"Cladding",47,8]
[null,"Cladding",48,6]
[null,"Cladding",48,8]
[null,"Cladding",49,6]
[null,"Cladding",49,8]
[null,"Cladding",51,6]
[null,"Cladding",51,8]
[null,"Cladding",52,6]
[null,"Cladding",52,8]
[null,"Cladding",53,6]
[null,"Cladding",53,8]
[null,"Cladding",54,5]
[null,"Cladding",55,6]
[null,"Cladding",55,8]
[null,"Cladding",56,6]
[null,"Cladding",56,8]
[null,"Cladding",59,6]
[null,"Cladding",59,8]
[null,"Cladding",60,6]
[null,"Cladding",60,8]
[null,"Cladding",61,6]
[null,"Cladding",61,8]
[null,"Cladding",62,6]
[null,"Cladding",62,8]
[null,"Cladding",63,6]
[null,"Cladding",63,8]
[null,"Cladding",64,6]
[null,"Cladding",64,8]
[null,"Cladding",66,6]
[null,"Cladding",66,8]
[null,"Cladding",67,6]
[null,"Cladding",67,8]
[null,"Cladding",68,6]
[null,"Cladding",68,8]
[null,"Cladding",70,6]
[null,"Cladding",70,8]
[null,"Cladding",71,6]
[null,"Cladding",71,8]
[null,"Cladding",72,6]
[null,"Cladding",72,8]
[null,"Cladding",73,6]
[null,"Cladding",73,8]
[null,"Cladding",74,6]
[null,"Cladding",74,8]
[null,"Cladding",75,6]
[null,"Cladding",75,8]
[null,"Cladding",76,6]
[null,"Cladding",76,8]
[null,"Cladding",77,6]
[null,"Cladding",77,8]
[null,"Cladding",78,6]
[null,"Cladding",78,8]
[null,"Cladding",79,6]
[null,"Cladding",79,8]
[null,"Windows",6,6]
[null,"Windows",6,8]
[null,"Windows",7,6]
[null,"Windows",7,8]
[null,"Windows",8,6]
[null,"Windows",8,8]
[null,"Windows",9,6]
[null,"Windows",9,8]
[null,"Windows",10,6]
[null,"Windows",10,8]
[null,"Windows",11,6]
[null,"Windows",11,8]
[null,"Windows",13,6]
[null,"Windows",13,8]
[null,"Windows",14,6]
[null,"Windows",14,8]
[null,"Windows",15,6]
[null,"Windows",15,8]
[null,"Windows",16,6]
[null,"Windows",16,8]
[null,"Windows",17,6]
[null,"Windows",17,8]
[null,"Windows",18,6]
[null,"Windows",18,8]
[null,"Windows",20,6]
[null,"Windows",20,8]
[null,"Windows",21,6]
[null,"Windows",21,8]
[null,"Windows",22,6]
[null,"Windows",22,8]
[null,"Int. Walls",5,5]
[null,"Int. Walls",7,6]
[null,"Int. Walls",7,8]
[null,"Int. Walls",8,6]
[null,"Int. Walls",8,8]
[null,"Int. Walls",9,6]
[null,"Int. Walls",9,8]
[null,"Int. Walls",10,5]
[null,"Int. Walls",12,6]
[null,"Int. Walls",12,8]
[null,"Int. Walls",13,6]
[null,"Int. Walls",13,8]
[null,"Int. Walls",14,6]
[null,"Int. Walls",14,8]
[null,"Int. Walls",15,6]
[null,"Int. Walls",15,8]
[null,"Int. Walls",16,6]
[null,"Int. Walls",16,8]
[null,"Int. Walls",17,6]
[null,"Int. Walls",17,8]
[null,"Int. Walls",20,6]
[null,"Int. Walls",20,8]
[null,"Int. Walls",21,6]
[null,"Int. Walls",21,8]
[null,"Int. Walls",22,6]
[null,"Int. Walls",22,8]
[null,"Int. Walls",23,6]
[null,"Int. Walls",23,8]
[null,"Int. Walls",24,6]
[null,"Int. Walls",24,8]
[null,"Int. Walls",25,6]
[null,"Int. Walls",25,8]
[null,"Int. Walls",27,6]
[null,"Int. Walls",27,8]
[null,"Int. Walls",28,6]
[null,"Int. Walls",28,8]
[null,"Int. Walls",29,6]
[null,"Int. Walls",29,8]
[null,"Int. Walls",31,6]
[null,"Int. Walls",31,8]
[null,"Int. Walls",32,6]
[null,"Int. Walls",32,8]
[null,"Int. Walls",33,6]
[null,"Int. Walls",33,8]
[null,"Int. Walls",34,6]
[null,"Int. Walls",34,8]
[null,"Int. Walls",35,6]
[null,"Int. Walls",35,8]
[null,"Int. Walls",36,6]
[null,"Int. Walls",36,8]
[null,"Int. Walls",37,6]
[null,"Int. Walls",37,8]
[null,"Int. Walls",38,6]
[null,"Int. Walls",38,8]
[null,"Int. Walls",39,6]
[null,"Int. Walls",39,8]
[null,"Int. Walls",40,6]
[null,"Int. Walls",40,8]
[null,"Int. Walls",41,5]
[null,"Int. Walls",42,5]
[null,"Int. Walls",43,6]
[null,"Int. Walls",43,8]
[null,"Int. Walls",44,6]
[null,"Int. Walls",44,8]
[null,"Int. Walls",45,6]
[null,"Int. Walls",45,8]
[null,"Int. Walls",46,6]
[null,"Int. Walls",46,8]
[null,"Int. Walls",47,5]
[null,"Int. Walls",48,6]
[null,"Int. Walls",48,8]
[null,"Int. Walls",49,6]
[null,"Int. Walls",49,8]
[null,"Int. Walls",50,6]
[null,"Int. Walls",50,8]
[null,"Int. Walls",51,6]
[null,"Int. Walls",51,8]
[null,"Int. Walls",52,6]
[null,"Int. Walls",52,8]
[null,"Int. Walls",53,5]
[null,"Int. Walls",54,6]
[null,"Int. Walls",54,8]
[null,"Int. Walls",55,6]
[null,"Int. Walls",55,8]
[null,"Int. Walls",56,6]
[null,"Int. Walls",56,8]
[null,"Int. Walls",57,6]
[null,"Int. Walls",57,8]
[null,"Int. Walls",58,6]
[null,"Int. Walls",58,8]
[null,"Int. Walls",59,6]
[null,"Int. Walls",59,8]
[null,"Int. Walls",60,6]
[null,"Int. Walls",60,8]
[null,"Int. Walls",61,5]
[null,"Int. Walls",62,6]
[null,"Int. Walls",62,8]
[null,"Int. Walls",63,6]
[null,"Int. Walls",63,8]
[null,"Int. Walls",64,6]
[null,"Int. Walls",64,8]
[null,"Int. Walls",65,6]
[null,"Int. Walls",65,8]
[null,"Int. Walls",66,5]
[null,"Int. Walls",67,6]
[null,"Int. Walls",67,8]
[null,"Int. Walls",68,6]
[null,"Int. Walls",68,8]
[null,"Int. Walls",69,6]
[null,"Int. Walls",69,8]
[null,"Int. Walls",70,6]
[null,"Int. Walls",70,8]
[null,"Int. Walls",71,6]
[null,"Int. Walls",71,8]
[null,"Int. Walls",72,5]
[null,"Int. Walls",73,6]
[null,"Int. Walls",73,8]
[null,"Int. Walls",74,6]
[null,"Int. Walls",74,8]
[null,"Int. Walls",75,6]
[null,"Int. Walls",75,8]
[null,"Int. Walls",76,6]
[null,"Int. Walls",76,8]
[null,"Int. Walls",77,6]
[null,"Int. Walls",77,8]
[null,"Int. Walls",78,5]
[null,"Int. Walls",79,6]
[null,"Int. Walls",79,8]
[null,"Int. Walls",80,6]
[null,"Int. Walls",80,8]
[null,"Int. Walls",81,6]
[null,"Int. Walls",81,8]
[null,"Int. Walls",82,5]
[null,"Int. Walls",83,6]
[null,"Int. Walls",83,8]
[null,"Int. Walls",84,6]
[null,"Int. Walls",84,8]
[null,"Int. Walls",85,5]
[null,"Int. Walls",86,6]
[null,"Int. Walls",86,8]
[null,"Int. Walls",87,6]
[null,"Int. Walls",87,8]
[null,"Int. Walls",88,6]
[null,"Int. Walls",88,8]
[null,"Int. Walls",89,6]
[null,"Int. Walls",89,8]
[null,"Floors",5,5]
[null,"Floors",7,6]
[null,"Floors",7,8]
[null,"Floors",8,6]
[null,"Floors",8,8]
[null,"Floors",9,6]
[null,"Floors",9,8]
[null,"Floors",11,6]
[null,"Floors",11,8]
[null,"Floors",12,6]
[null,"Floors",12,8]
[null,"Floors",13,6]
[null,"Floors",13,8]
[null,"Floors",15,6]
[null,"Floors",15,8]
[null,"Floors",16,5]
[null,"Floors",18,6]
[null,"Floors",18,8]
[null,"Floors",20,6]
[null,"Floors",20,8]
[null,"Floors",21,6]
[null,"Floors",21,8]
[null,"Floors",22,6]
[null,"Floors",22,8]
[null,"Floors",23,6]
[null,"Floors",23,8]
[null,"Floors",24,6]
[null,"Floors",24,8]
[null,"Floors",25,6]
[null,"Floors",25,8]
[null,"Floors",28,6]
[null,"Floors",28,8]
[null,"Floors",29,6]
[null,"Floors",29,8]
[null,"Floors",30,6]
[null,"Floors",30,8]
[null,"Floors",31,6]
[null,"Floors",31,8]
[null,"Floors",34,6]
[null,"Floors",34,8]
[null,"Floors",37,6]
[null,"Floors",37,8]
[null,"Floors",38,6]
[null,"Floors",38,8]
[null,"Floors",39,6]
[null,"Floors",39,8]
[null,"Floors",40,6]
[null,"Floors",40,8]
[null,"Floors",42,6]
[null,"Floors",42,8]
[null,"Floors",43,6]
[null,"Floors",43,8]
[null,"Floors",44,6]
[null,"Floors",44,8]
[null,"Floors",45,6]
[null,"Floors",45,8]
[null,"Floors",46,6]
[null,"Floors",46,8]
[null,"Floors",47,6]
[null,"Floors",47,8]
[null,"Floors",49,6]
[null,"Floors",49,8]
[null,"Floors",50,6]
[null,"Floors",50,8]
[null,"Floors",51,6]
[null,"Floors",51,8]
[null,"Floors",52,6]
[null,"Floors",52,8]
[null,"Floors",53,6]
[null,"Floors",53,8]
[null,"Floors",54,6]
[null,"Floors",54,8]
[null,"Floors",56,6]
[null,"Floors",56,8]
[null,"Floors",57,6]
[null,"Floors",57,8]
[null,"Floors",58,6]
[null,"Floors",58,8]
[null,"Floors",59,6]
[null,"Floors",59,8]
[null,"Floors",60,6]
[null,"Floors",60,8]
[null,"Floors",61,6]
[null,"Floors",61,8]
[null,"Floors",62,6]
[null,"Floors",62,8]
[null,"Floors",64,6]
[null,"Floors",64,8]
[null,"Floors",66,6]
[null,"Floors",66,8]
[null,"Floors",67,6]
[null,"Floors",67,8]
[null,"Floors",69,6]
[null,"Floors",69,8]
[null,"Floors",70,6]
[null,"Floors",70,8]
[null,"Floors",71,6]
[null,"Floors",71,8]
[null,"Floors",73,6]
[null,"Floors",73,8]
[null,"Floors",74,6]
[null,"Floors",74,8]
[null,"Floors",75,6]
[null,"Floors",75,8]
[null,"Floors",76,5]
[null,"Floors",77,5]
[null,"Floors",78,6]
[null,"Floors",78,8]
[null,"Floors",79,6]
[null,"Floors",79,8]
[null,"Floors",80,6]
[null,"Floors",80,8]
[null,"Floors",81,6]
[null,"Floors",81,8]
[null,"Floors",82,5]
[null,"Floors",83,6]
[null,"Floors",83,8]
[null,"Floors",84,6]
[null,"Floors",84,8]
[null,"Floors",85,6]
[null,"Floors",85,8]
[null,"Floors",86,6]
[null,"Floors",86,8]
[null,"Floors",87,6]
[null,"Floors",87,8]
[null,"Floors",88,5]
[null,"Floors",89,6]
[null,"Floors",89,8]
[null,"Floors",90,6]
[null,"Floors",90,8]
[null,"Floors",91,6]
[null,"Floors",91,8]
[null,"Floors",92,6]
[null,"Floors",92,8]
[null,"Floors",93,6]
[null,"Floors",93,8]
[null,"Floors",94,6]
[null,"Floors",94,8]
[null,"Floors",95,6]
[null,"Floors",95,8]
[null,"Floors",96,6]
[null,"Floors",96,8]
[null,"Floors",97,5]
[null,"Floors",98,6]
[null,"Floors",98,8]
[null,"Floors",99,5]
[null,"Floors",100,6]
[null,"Floors",100,8]
[null,"Floors",101,6]
[null,"Floors",101,8]
[null,"Floors",102,6]
[null,"Floors",102,8]
[null,"Floors",103,5]
[null,"Floors",104,6]
[null,"Floors",104,8]
[null,"Floors",105,6]
[null,"Floors",105,8]
[null,"Floors",106,5]
[null,"Floors",107,6]
[null,"Floors",107,8]
[null,"Floors",108,6]
[null,"Floors",108,8]
[null,"Floors",109,6]
[null,"Floors",109,8]
[null,"Floors",110,6]
[null,"Floors",110,8]
[null,"Floors",111,6]
[null,"Floors",111,8]
[null,"Floors",112,5]
[null,"Floors",113,6]
[null,"Floors",113,8]
[null,"Floors",114,6]
[null,"Floors",114,8]
[null,"Floors",115,6]
[null,"Floors",115,8]
[null,"Floors",116,6]
[null,"Floors",116,8]
[null,"Floors",117,5]
[null,"Floors",118,6]
[null,"Floors",118,8]
[null,"Floors",119,6]
[null,"Floors",119,8]
[null,"Floors",120,6]
[null,"Floors",120,8]
[null,"Floors",121,6]
[null,"Floors",121,8]
[null,"Floors",122,6]
[null,"Floors",122,8]
[null,"Floors",123,6]
[null,"Floors",123,8]
[null,"Floors",124,5]
[null,"Floors",125,6]
[null,"Floors",125,8]
[null,"Floors",126,6]
[null,"Floors",126,8]
[null,"Floors",127,6]
[null,"Floors",127,8]
[null,"Ceilings",7,6]
[null,"Ceilings",7,8]
[null,"Ceilings",8,6]
[null,"Ceilings",8,8]
[null,"Ceilings",9,6]
[null,"Ceilings",9,8]
[null,"Ceilings",10,6]
[null,"Ceilings",10,8]
[null,"Ceilings",11,6]
[null,"Ceilings",11,8]
[null,"Ceilings",12,6]
[null,"Ceilings",12,8]
[null,"Ceilings",14,6]
[null,"Ceilings",14,8]
[null,"Ceilings",15,6]
[null,"Ceilings",15,8]
[null,"Ceilings",16,6]
[null,"Ceilings",16,8]
[null,"Ceilings",17,6]
[null,"Ceilings",17,8]
[null,"Ceilings",19,6]
[null,"Ceilings",19,8]
[null,"Ceilings",20,6]
[null,"Ceilings",20,8]
[null,"Ceilings",21,6]
[null,"Ceilings",21,8]
[null,"Ceilings",22,6]
[null,"Ceilings",22,8]
[null,"Ceilings",23,6]
[null,"Ceilings",23,8]
[null,"Ceilings",24,6]
[null,"Ceilings",24,8]
[null,"Roof",5,5]
[null,"Roof",7,6]
[null,"Roof",7,8]
[null,"Roof",8,6]
[null,"Roof",8,8]
[null,"Roof",9,6]
[null,"Roof",9,8]
[null,"Roof",10,6]
[null,"Roof",10,8]
[null,"Roof",11,6]
[null,"Roof",11,8]
[null,"Roof",13,6]
[null,"Roof",13,8]
[null,"Roof",15,6]
[null,"Roof",15,8]
[null,"Roof",16,6]
[null,"Roof",16,8]
[null,"Roof",17,6]
[null,"Roof",17,8]
[null,"Roof",18,6]
[null,"Roof",18,8]
[null,"Roof",21,6]
[null,"Roof",21,8]
[null,"Roof",22,6]
[null,"Roof",22,8]
[null,"Roof",24,6]
[null,"Roof",24,8]
[null,"Roof",25,6]
[null,"Roof",25,8]
[null,"Roof",26,6]
[null,"Roof",26,8]
[null,"Roof",29,6]
[null,"Roof",29,8]
[null,"Roof",30,6]
[null,"Roof",30,8]
[null,"Roof",31,6]
[null,"Roof",31,8]
[null,"Roof",32,6]
[null,"Roof",32,8]
[null,"Roof",33,5]
[null,"Roof",35,6]
[null,"Roof",35,8]
[null,"Roof",36,6]
[null,"Roof",36,8]
[null,"Roof",37,6]
[null,"Roof",37,8]
[null,"Roof",40,6]
[null,"Roof",40,8]
[null,"Roof",41,6]
[null,"Roof",41,8]
[null,"Roof",42,6]
[null,"Roof",42,8]
[null,"Roof",43,6]
[null,"Roof",43,8]
[null,"Roof",44,6]
[null,"Roof",44,8]
[null,"Roof",45,6]
[null,"Roof",45,8]
[null,"Roof",46,6]
[null,"Roof",46,8]
[null,"Roof",48,6]
[null,"Roof",48,8]
[null,"Roof",49,6]
[null,"Roof",49,8]
[null,"Roof",50,6]
[null,"Roof",50,8]
[null,"Roof",51,6]
[null,"Roof",51,8]
[null,"Roof",52,6]
[null,"Roof",52,8]
[null,"Roof",53,6]
[null,"Roof",53,8]
[null,"Roof",55,6]
[null,"Roof",55,8]
[null,"Roof",56,6]
[null,"Roof",56,8]
[null,"Roof",57,6]
[null,"Roof",57,8]
[null,"Roof",59,6]
[null,"Roof",59,8]
[null,"Roof",60,6]
[null,"Roof",60,8]
[null,"Roof",61,6]
[null,"Roof",61,8]
[null,"Roof",62,6]
[null,"Roof",62,8]
[null,"Roof",64,6]
[null,"Roof",64,8]
[null,"Roof",65,5]
[null,"Roof",65,9]
[null,"Roof",66,5]
[null,"Roof",67,6]
[null,"Roof",67,8]
[null,"Roof",68,6]
[null,"Roof",68,8]
[null,"Roof",69,6]
[null,"Roof",69,8]
[null,"Roof",70,6]
[null,"Roof",70,8]
[null,"Roof",71,5]
[null,"Roof",72,6]
[null,"Roof",72,8]
[null,"Roof",73,6]
[null,"Roof",73,8]
[null,"Roof",74,6]
[null,"Roof",74,8]
[null,"Roof",75,6]
[null,"Roof",75,8]
[null,"Roof",76,6]
[null,"Roof",76,8]
[null,"Roof",77,5]
[null,"Roof",78,6]
[null,"Roof",78,8]
[null,"Roof",79,6]
[null,"Roof",79,8]
[null,"Roof",80,6]
[null,"Roof",80,8]
[null,"Roof",81,6]
[null,"Roof",81,8]
[null,"Roof",82,6]
[null,"Roof",82,8]
[null,"Roof",83,6]
[null,"Roof",83,8]
[null,"Roof",84,6]
[null,"Roof",84,8]
[null,"Roof",85,6]
[null,"Roof",85,8]
[null,"Roof",86,5]
[null,"Roof",87,6]
[null,"Roof",87,8]
[null,"Roof",88,5]
[null,"Roof",89,6]
[null,"Roof",89,8]
[null,"Roof",90,6]
[null,"Roof",90,8]
[null,"Roof",91,6]
[null,"Roof",91,8]
[null,"Roof",92,5]
[null,"Roof",93,6]
[null,"Roof",93,8]
[null,"Roof",94,6]
[null,"Roof",94,8]
[null,"Roof",95,5]
[null,"Roof",96,6]
[null,"Roof",96,8]
[null,"Roof",97,6]
[null,"Roof",97,8]
[null,"Roof",98,6]
[null,"Roof",98,8]
[null,"Roof",99,6]
[null,"Roof",99,8]
[null,"Roof",100,6]
[null,"Roof",100,8]
[null,"Roof",101,5]
[null,"Roof",102,6]
[null,"Roof",102,8]
[null,"Roof",103,6]
[null,"Roof",103,8]
[null,"Roof",104,6]
[null,"Roof",104,8]
[null,"Roof",105,6]
[null,"Roof",105,8]
[null,"Roof",106,5]
[null,"Roof",107,6]
[null,"Roof",107,8]
[null,"Roof",108,6]
[null,"Roof",108,8]
[null,"Roof",109,6]
[null,"Roof",109,8]
[null,"Roof",110,6]
[null,"Roof",110,8]
[null,"Roof",111,6]
[null,"Roof",111,8]
[null,"Roof",112,6]
[null,"Roof",112,8]
[null,"Roof",113,5]
[null,"Roof",114,6]
[null,"Roof",114,8]
[null,"Roof",115,6]
[null,"Roof",115,8]
[null,"Roof",116,6]
[null,"Roof",116,8]
[null,"Roof",117,5]
[null,"Roof",118,6]
[null,"Roof",118,8]
[null,"Roof",119,6]
[null,"Roof",119,8]
[null,"Roof",120,5]
[null,"Roof",120,9]
[null,"Roof",121,5]
[null,"Roof",122,6]
[null,"Roof",122,8]
[null,"Roof",123,6]
[null,"Roof",123,8]
[null,"Roof",124,6]
[null,"Roof",124,8]
[null,"Roof",125,5]
[null,"Roof",126,6]
[null,"Roof",126,8]
[null,"Roof",127,6]
[null,"Roof",127,8]
[null,"Roof",128,6]
[null,"Roof",128,8]
[null,"Roof",129,6]
[null,"Roof",129,8]
[null,"Roof",130,6]
[null,"Roof",130,8]
[null,"Roof",131,6]
[null,"Roof",131,8]
[null,"Roof",132,5]
[null,"Roof",133,6]
[null,"Roof",133,8]
[null,"Roof",134,6]
[null,"Roof",134,8]
[null,"Roof",135,6]
[null,"Roof",135,8]
[null,"Roof",136,6]
[null,"Roof",136,8]
[null,"Roof",137,6]
[null,"Roof",137,8]
[null,"Roof",138,5]
[null,"Roof",139,6]
[null,"Roof",139,8]
[null,"Roof",140,6]
[null,"Roof",140,8]
[null,"Roof",141,6]
[null,"Roof",141,8]
[null,"Roof",142,6]
[null,"Roof",142,8]
[null,"Roof",143,6]
[null,"Roof",143,8]
[null,"Roof",144,5]
[null,"Roof",145,6]
[null,"Roof",145,8]
[null,"Roof",146,6]
[null,"Roof",146,8]
[null,"Roof",147,6]
[null,"Roof",147,8]
[null,"Roof",148,6]
[null,"Roof",148,8]
[null,"Roof",151,6]
[null,"Roof",151,8]
[null,"Roof",152,6]
[null,"Roof",152,8]
[null,"Roof",153,6]
[null,"Roof",153,8]
[null,"Roof",154,6]
[null,"Roof",154,8]
[null,"Roof",155,6]
[null,"Roof",155,8]
[null,"Garage",6,5]
[null,"Garage",6,6]
[null,"Garage",8,6]
[null,"Garage",8,8]
[null,"Garage",9,6]
[null,"Garage",9,8]
[null,"Garage",10,6]
[null,"Garage",10,8]
[null,"Garage",11,6]
[null,"Garage",11,8]
[null,"Garage",12,6]
[null,"Garage",12,8]
[null,"Garage",13,5]
[null,"Garage",13,6]
[null,"Garage",15,6]
[null,"Garage",15,8]
[null,"Garage",16,6]
[null,"Garage",16,8]
[null,"Garage",17,6]
[null,"Garage",17,8]
[null,"Garage",18,6]
[null,"Garage",18,8]
[null,"Garage",19,6]
[null,"Garage",19,8]
[null,"Garage",20,6]
[null,"Garage",20,8]
[null,"Garage",21,6]
[null,"Garage",21,8]
[null,"Garage",23,6]
[null,"Garage",23,8]
[null,"Garage",24,6]
[null,"Garage",24,8]
[null,"Garage",25,6]
[null,"Garage",25,8]
[null,"Garage",26,6]
[null,"Garage",26,8]
[null,"Garage",27,6]
[null,"Garage",27,8]
[null,"Garage",28,6]
[null,"Garage",28,8]
[null,"Garage",29,6]
[null,"Garage",29,8]
[null,"Garage",30,5]
[null,"Garage",32,6]
[null,"Garage",32,8]
[null,"Garage",35,6]
[null,"Garage",35,8]
[null,"Garage",36,6]
[null,"Garage",36,8]
[null,"Garage",37,6]
[null,"Garage",37,8]
[null,"Garage",38,6]
[null,"Garage",38,8]
[null,"Garage",39,6]
[null,"Garage",39,8]
[null,"Garage",40,6]
[null,"Garage",40,8]
[null,"Garage",41,6]
[null,"Garage",41,8]
[null,"Garage",43,6]
[null,"Garage",43,8]
[null,"Garage",44,6]
[null,"Garage",44,8]
[null,"Garage",45,6]
[null,"Garage",45,8]
[null,"Garage",46,6]
[null,"Garage",46,8]
[null,"Garage",47,6]
[null,"Garage",47,8]
[null,"Garage",48,6]
[null,"Garage",48,8]
[null,"Garage",49,6]
[null,"Garage",49,8]
[null,"Garage",50,5]
[null,"Garage",52,6]
[null,"Garage",52,8]
[null,"Garage",53,6]
[null,"Garage",53,8]
[null,"Garage",54,6]
[null,"Garage",54,8]
[null,"Garage",55,6]
[null,"Garage",55,8]
[null,"Garage",56,6]
[null,"Garage",56,8]
[null,"Garage",57,6]
[null,"Garage",57,8]
[null,"Garage",58,6]
[null,"Garage",58,8]
[null,"Garage",59,6]
[null,"Garage",59,8]
[null,"Garage",60,5]
[null,"Garage",62,6]
[null,"Garage",62,8]
[null,"Garage",64,5]
[null,"Garage",64,6]
[null,"Garage",66,6]
[null,"Garage",66,8]
[null,"Garage",67,6]
[null,"Garage",67,8]
[null,"Garage",68,6]
[null,"Garage",68,8]
[null,"Garage",69,6]
[null,"Garage",69,8]
[null,"Garage",70,6]
[null,"Garage",70,8]
[null,"Garage",71,6]
[null,"Garage",71,8]
[null,"Garage",72,6]
[null,"Garage",72,8]
[null,"Garage",74,6]
[null,"Garage",74,8]
[null,"Garage",75,6]
[null,"Garage",75,8]
[null,"Garage",76,6]
[null,"Garage",76,8]
[null,"Garage",77,6]
[null,"Garage",77,8]
[null,"Garage",78,6]
[null,"Garage",78,8]
[null,"Garage",79,6]
[null,"Garage",79,8]
[null,"Garage",80,6]
[null,"Garage",80,8]
[null,"Garage",83,6]
[null,"Garage",83,8]
[null,"Garage",84,6]
[null,"Garage",84,8]
[null,"Garage",85,6]
[null,"Garage",85,8]
[null,"Garage",86,6]
[null,"Garage",86,8]
[null,"Garage",87,6]
[null,"Garage",87,8]
[null,"Garage",88,6]
[null,"Garage",88,8]
[null,"Garage",89,6]
[null,"Garage",89,8]
[null,"Garage",93,6]
[null,"Garage",93,8]
[null,"Garage",94,6]
[null,"Garage",94,8]
[null,"Garage",95,6]
[null,"Garage",95,8]
[null,"Garage",96,6]
[null,"Garage",96,8]
[null,"Garage",97,6]
[null,"Garage",97,8]
[null,"Garage",98,6]
[null,"Garage",98,8]
[null,"Garage",99,6]
[null,"Garage",99,8]
[null,"Garage",102,4]
[null,"Garage",102,6]
[null,"Garage",102,8]
[null,"Garage",103,3]
[null,"Garage",103,4]
[null,"Garage",103,6]
[null,"Garage",103,8]
[null,"Garage",104,4]
[null,"Garage",104,6]
[null,"Garage",104,8]
[null,"Garage",106,5]
[null,"Garage",108,6]
[null,"Garage",108,8]
[null,"Garage",109,6]
[null,"Garage",109,8]
[null,"Garage",110,6]
[null,"Garage",110,8]
[null,"Garage",111,6]
[null,"Garage",111,8]
[null,"Garage",112,5]
[null,"Garage",114,6]
[null,"Garage",114,8]
[null,"Garage",115,6]
[null,"Garage",115,8]
[null,"Garage",116,6]
[null,"Garage",116,8]
[null,"Garage",117,6]
[null,"Garage",117,8]
[null,"Garage",118,6]
[null,"Garage",118,8]
[null,"Garage",119,6]
[null,"Garage",119,8]
[null,"Garage",121,6]
[null,"Garage",121,8]
[null,"Garage",122,6]
[null,"Garage",122,8]
[null,"Garage",123,6]
[null,"Garage",123,8]
[null,"Garage",124,6]
[null,"Garage",124,8]
[null,"Garage",125,6]
[null,"Garage",125,8]
[null,"Garage",126,6]
[null,"Garage",126,8]
[null,"Garage",129,6]
[null,"Garage",129,8]
[null,"Garage",130,6]
[null,"Garage",130,8]
[null,"Garage",131,6]
[null,"Garage",131,8]
[null,"Garage",132,6]
[null,"Garage",132,8]
[null,"Garage",134,6]
[null,"Garage",134,8]
[null,"Garage",135,6]
[null,"Garage",135,8]
[null,"Garage",136,6]
[null,"Garage",136,8]
[null,"Garage",138,6]
[null,"Garage",138,8]
[null,"Garage",139,6]
[null,"Garage",139,8]
[null,"Garage",140,6]
[null,"Garage",140,8]
[null,"Garage",143,6]
[null,"Garage",143,8]
[null,"Garage",144,6]
[null,"Garage",144,8]
[null,"Garage",145,6]
[null,"Garage",145,8]
[null,"Garage",146,6]
[null,"Garage",146,8]
[null,"Garage",147,6]
[null,"Garage",147,8]
[null,"Garage",148,6]
[null,"Garage",148,8]
[null,"Garage",149,6]
[null,"Garage",149,8]
[null,"Garage",150,5]
[null,"Garage",151,5]
[null,"Garage",152,6]
[null,"Garage",152,8]
[null,"Garage",153,6]
[null,"Garage",153,8]
[null,"Garage",154,6]
[null,"Garage",154,8]
[null,"Garage",155,6]
[null,"Garage",155,8]
[null,"Garage",156,5]
[null,"Garage",157,6]
[null,"Garage",157,8]
[null,"Garage",158,6]
[null,"Garage",158,8]
[null,"Garage",159,6]
[null,"Garage",159,8]
[null,"Garage",160,6]
[null,"Garage",160,8]
[null,"Garage",161,6]
[null,"Garage",161,8]
[null,"Garage",162,5]
[null,"Garage",163,6]
[null,"Garage",163,8]
[null,"Garage",164,6]
[null,"Garage",164,8]
[null,"Garage",165,6]
[null,"Garage",165,8]
[null,"Garage",166,6]
[null,"Garage",166,8]
[null,"Garage",167,6]
[null,"Garage",167,8]
[null,"Garage",168,6]
[null,"Garage",168,8]
[null,"Garage",169,6]
[null,"Garage",169,8]
[null,"Garage",170,5]
[null,"Garage",171,6]
[null,"Garage",171,8]
[null,"Garage",172,6]
[null,"Garage",172,8]
[null,"Garage",173,6]
[null,"Garage",173,8]
[null,"Garage",174,6]
[null,"Garage",174,8]
[null,"Garage",175,5]
[null,"Garage",176,6]
[null,"Garage",176,8]
[null,"Garage",177,6]
[null,"Garage",177,8]
[null,"Garage",178,6]
[null,"Garage",178,8]
[null,"Garage",179,6]
[null,"Garage",179,8]
[null,"Garage",180,6]
[null,"Garage",180,8]
[null,"Garage",181,5]
[null,"Garage",182,6]
[null,"Garage",182,8]
[null,"Garage",183,6]
[null,"Garage",183,8]
[null,"Garage",184,6]
[null,"Garage",184,8]
[null,"Garage",185,6]
[null,"Garage",185,8]
[null,"Garage",186,6]
[null,"Garage",186,8]
[null,"Garage",187,5]
[null,"Garage",188,6]
[null,"Garage",188,8]
[null,"Garage",189,6]
[null,"Garage",189,8]
[null,"Garage",190,6]
[null,"Garage",190,8]
[null,"Garage",191,5]
[null,"Garage",192,6]
[null,"Garage",192,8]
[null,"Garage",193,6]
[null,"Garage",193,8]
[null,"Garage",194,5]
[null,"Garage",195,6]
[null,"Garage",195,8]
[null,"Garage",196,6]
[null,"Garage",196,8]
[null,"Garage",197,6]
[null,"Garage",197,8]
[null,"Garage",198,6]
[null,"Garage",198,8]
[null,"Garage",199,5]
[null,"Garage",200,5]
[null,"Garage",201,6]
[null,"Garage",201,8]
[null,"Garage",202,6]
[null,"Garage",202,8]
[null,"Garage",203,6]
[null,"Garage",203,8]
[null,"Garage",204,5]
[null,"Garage",205,6]
[null,"Garage",205,8]
[null,"Garage",206,6]
[null,"Garage",206,8]
[null,"Garage",207,6]
[null,"Garage",207,8]
[null,"Garage",208,6]
[null,"Garage",208,8]
[null,"Garage",209,6]
[null,"Garage",209,8]
[null,"Garage",210,6]
[null,"Garage",210,8]
[null,"Garage",211,5]
[null,"Garage",212,6]
[null,"Garage",212,8]
[null,"Garage",213,6]
[null,"Garage",213,8]
[null,"Garage",214,6]
[null,"Garage",214,8]
[null,"Garage",215,6]
[null,"Garage",215,8]
[null,"Garage",216,6]
[null,"Garage",216,8]
[null,"Garage",217,5]
[null,"Garage",218,6]
[null,"Garage",218,8]
[null,"Garage",219,6]
[null,"Garage",219,8]
[null,"Garage",220,6]
[null,"Garage",220,8]
[null,"Garage",221,6]
[null,"Garage",221,8]
[null,"Garage",222,6]
[null,"Garage",222,8]
[null,"Garage",223,5]
[null,"Garage",224,6]
[null,"Garage",224,8]
[null,"Garage",225,6]
[null,"Garage",225,8]
[null,"Garage",226,6]
[null,"Garage",226,8]
[null,"Garage",227,6]
[null,"Garage",227,8]
[null,"Garage",229,5]
[null,"Garage",230,5]
[null,"Garage",231,6]
[null,"Garage",231,8]
[null,"Garage",232,6]
[null,"Garage",232,8]
[null,"Garage",233,6]
[null,"Garage",233,8]
[null,"Garage",234,6]
[null,"Garage",234,8]
[null,"Garage",235,5]
[null,"Garage",236,6]
[null,"Garage",236,8]
[null,"Garage",237,6]
[null,"Garage",237,8]
[null,"Garage",238,6]
[null,"Garage",238,8]
[null,"Garage",239,6]
[null,"Garage",239,8]
[null,"Garage",240,6]
[null,"Garage",240,8]
[null,"Garage",241,5]
[null,"Garage",242,6]
[null,"Garage",242,8]
[null,"Garage",243,6]
[null,"Garage",243,8]
[null,"Garage",244,6]
[null,"Garage",244,8]
[null,"Garage",245,6]
[null,"Garage",245,8]
[null,"Garage",246,6]
[null,"Garage",246,8]
[null,"Garage",247,6]
[null,"Garage",247,8]
[null,"Garage",248,6]
[null,"Garage",248,8]
[null,"Garage",249,5]
[null,"Garage",250,6]
[null,"Garage",250,8]
[null,"Garage",251,6]
[null,"Garage",251,8]
[null,"Garage",252,6]
[null,"Garage",252,8]
[null,"Garage",253,6]
[null,"Garage",253,8]
[null,"Garage",254,5]
[null,"Garage",255,6]
[null,"Garage",255,8]
[null,"Garage",256,6]
[null,"Garage",256,8]
[null,"Garage",257,6]
[null,"Garage",257,8]
[null,"Garage",258,6]
[null,"Garage",258,8]
[null,"Garage",259,6]
[null,"Garage",259,8]
[null,"Garage",260,5]
[null,"Garage",261,6]
[null,"Garage",261,8]
[null,"Garage",262,6]
[null,"Garage",262,8]
[null,"Garage",263,6]
[null,"Garage",263,8]
[null,"Garage",264,6]
[null,"Garage",264,8]
[null,"Garage",265,6]
[null,"Garage",265,8]
[null,"Garage",266,5]
[null,"Garage",267,6]
[null,"Garage",267,8]
[null,"Garage",268,6]
[null,"Garage",268,8]
[null,"Garage",269,6]
[null,"Garage",269,8]
[null,"Garage",270,5]
[null,"Garage",271,6]
[null,"Garage",271,8]
[null,"Garage",272,6]
[null,"Garage",272,8]
[null,"Garage",273,5]
[null,"Garage",274,6]
[null,"Garage",274,8]
[null,"Garage",275,6]
[null,"Garage",275,8]
[null,"Garage",276,6]
[null,"Garage",276,8]
[null,"Garage",277,6]
[null,"Garage",277,8]
[null,"Garage",281,6]
[null,"Garage",281,8]
[null,"Garage",282,6]
[null,"Garage",282,8]
[null,"Garage",283,6]
[null,"Garage",283,8]
[null,"Garage",284,6]
[null,"Garage",284,8]
[null,"Garage",285,6]
[null,"Garage",285,8]
[null,"Garage",286,6]
[null,"Garage",286,8]
[null,"Garage",287,6]
[null,"Garage",287,8]
[null,"Garage",289,6]
[null,"Garage",289,8]
[null,"Garage",290,6]
[null,"Garage",290,8]
[null,"Garage",292,6]
[null,"Garage",292,8]
[null,"Garage",293,6]
[null,"Garage",293,8]
[null,"Garage",294,6]
[null,"Garage",294,8]
[null,"Garage",295,6]
[null,"Garage",295,8]
[null,"Garage",296,6]
[null,"Garage",296,8]
[null,"Garage",297,6]
[null,"Garage",297,8]
[null,"Garage",298,6]
[null,"Garage",298,8]
[null,"Garage",299,6]
[null,"Garage",299,8]
[null,"Garage",300,6]
[null,"Garage",300,8]
[null,"Garage",302,6]
[null,"Garage",302,8]
[null,"Garage",304,6]
[null,"Garage",304,8]
[null,"Garage",305,6]
[null,"Garage",305,8]
[null,"Garage",306,6]
[null,"Garage",306,8]
[null,"Garage",308,6]
[null,"Garage",308,8]
[null,"Garage",309,6]
[null,"Garage",309,8]
[null,"Garage",310,6]
[null,"Garage",310,8]
[null,"Garage",311,6]
[null,"Garage",311,8]
[null,"Garage",312,6]
[null,"Garage",312,8]
[null,"Garage",313,6]
[null,"Garage",313,8]
[null,"Garage",314,6]
[null,"Garage",314,8]
[null,"Garage",316,6]
[null,"Garage",316,8]
[null,"Garage",317,6]
[null,"Garage",317,8]
[null,"Garage",318,6]
[null,"Garage",318,8]
[null,"Garage",320,6]
[null,"Garage",320,8]
[null,"Garage",321,6]
[null,"Garage",321,8]
[null,"Garage",322,6]
[null,"Garage",322,8]
[null,"Garage",323,6]
[null,"Garage",323,8]
[null,"Garage",325,6]
[null,"Garage",325,8]
[null,"Garage",326,6]
[null,"Garage",326,8]
[null,"Garage",327,6]
[null,"Garage",327,8]
[null,"Garage",328,5]
[null,"Garage",329,6]
[null,"Garage",329,8]
[null,"Garage",330,6]
[null,"Garage",330,8]
[null,"Garage",333,6]
[null,"Garage",333,8]
[null,"Garage",334,6]
[null,"Garage",334,8]
[null,"Garage",335,6]
[null,"Garage",335,8]
[null,"Garage",336,6]
[null,"Garage",336,8]
[null,"Garage",337,6]
[null,"Garage",337,8]
[null,"Garage",338,6]
[null,"Garage",338,8]
[null,"Garage",340,6]
[null,"Garage",340,8]
[null,"Garage",341,6]
[null,"Garage",341,8]
[null,"Garage",342,6]
[null,"Garage",342,8]
[null,"Garage",344,6]
[null,"Garage",344,8]
[null,"Garage",345,6]
[null,"Garage",345,8]
[null,"Garage",346,6]
[null,"Garage",346,8]
[null,"Garage",347,6]
[null,"Garage",347,8]
[null,"Garage",348,6]
[null,"Garage",348,8]
[null,"Garage",349,6]
[null,"Garage",349,8]
[null,"Garage",350,6]
[null,"Garage",350,8]
[null,"Garage",351,6]
[null,"Garage",351,8]
[null,"Garage",352,6]
[null,"Garage",352,8]
[null,"Garage",353,6]
[null,"Garage",353,8]
[null,"Garage",356,6]
[null,"Garage",356,8]
[null,"Garage",357,6]
[null,"Garage",357,8]
[null,"Garage",358,6]
[null,"Garage",358,8]
[null,"Garage",359,6]
[null,"Garage",359,8]
[null,"Garage",360,6]
[null,"Garage",360,8]
[null,"Garage",361,6]
[null,"Garage",361,8]
[null,"Garage",363,6]
[null,"Garage",363,8]
[null,"Garage",364,6]
[null,"Garage",364,8]
[null,"Garage",365,6]
[null,"Garage",365,8]
[null,"Garage",369,6]
[null,"Garage",369,8]
[null,"Garage",370,6]
[null,"Garage",370,8]
[null,"Garage",371,6]
[null,"Garage",371,8]
[null,"Garage",372,6]
[null,"Garage",372,8]
[null,"Garage",373,6]
[null,"Garage",373,8]
[null,"Garage",374,6]
[null,"Garage",374,8]
[null,"Garage",376,6]
[null,"Garage",376,8]
[null,"Garage",377,6]
[null,"Garage",377,8]
[null,"Garage",378,6]
[null,"Garage",378,8]
[null,"Garage",379,6]
[null,"Garage",379,8]
[null,"Garage",381,6]
[null,"Garage",381,8]
[null,"Garage",382,6]
[null,"Garage",382,8]
[null,"Garage",383,6]
[null,"Garage",383,8]
[null,"Garage",384,6]
[null,"Garage",384,8]
[null,"Garage",385,6]
[null,"Garage",385,8]
[null,"Garage",386,6]
[null,"Garage",386,8]
[null,"Garage",388,5]
[null,"Garage",390,6]
[null,"Garage",390,8]
[null,"Garage",391,6]
[null,"Garage",391,8]
[null,"Garage",392,6]
[null,"Garage",392,8]
[null,"Garage",393,6]
[null,"Garage",393,8]
[null,"Garage",394,6]
[null,"Garage",394,8]
[null,"Garage",396,6]
[null,"Garage",396,8]
[null,"Garage",398,6]
[null,"Garage",398,8]
[null,"Garage",399,6]
[null,"Garage",399,8]
[null,"Garage",400,6]
[null,"Garage",400,8]
[null,"Garage",401,6]
[null,"Garage",401,8]
[null,"Garage",404,6]
[null,"Garage",404,8]
[null,"Garage",405,6]
[null,"Garage",405,8]
[null,"Garage",407,6]
[null,"Garage",407,8]
[null,"Garage",408,6]
[null,"Garage",408,8]
[null,"Garage",409,6]
[null,"Garage",409,8]
[null,"Garage",412,6]
[null,"Garage",412,8]
[null,"Garage",413,6]
[null,"Garage",413,8]
[null,"Garage",414,6]
[null,"Garage",414,8]
[null,"Garage",415,6]
[null,"Garage",415,8]
[null,"Garage",416,5]
[null,"Garage",418,6]
[null,"Garage",418,8]
[null,"Garage",419,6]
[null,"Garage",419,8]
[null,"Garage",420,6]
[null,"Garage",420,8]
[null,"Garage",423,6]
[null,"Garage",423,8]
[null,"Garage",424,6]
[null,"Garage",424,8]
[null,"Garage",425,6]
[null,"Garage",425,8]
[null,"Garage",426,6]
[null,"Garage",426,8]
[null,"Garage",427,6]
[null,"Garage",427,8]
[null,"Garage",428,6]
[null,"Garage",428,8]
[null,"Garage",429,6]
[null,"Garage",429,8]
[null,"Garage",431,6]
[null,"Garage",431,8]
[null,"Garage",432,6]
[null,"Garage",432,8]
[null,"Garage",433,6]
[null,"Garage",433,8]
[null,"Garage",434,6]
[null,"Garage",434,8]
[null,"Garage",435,6]
[null,"Garage",435,8]
[null,"Garage",436,6]
[null,"Garage",436,8]
[null,"Garage",438,6]
[null,"Garage",438,8]
[null,"Garage",439,6]
[null,"Garage",439,8]
[null,"Garage",440,6]
[null,"Garage",440,8]
[null,"Garage",442,6]
[null,"Garage",442,8]
[null,"Garage",443,6]
[null,"Garage",443,8]
[null,"Garage",444,6]
[null,"Garage",444,8]
[null,"Garage",445,6]
[null,"Garage",445,8]
[null,"Garage",447,6]
[null,"Garage",447,8]
[null,"User-Defined",7,1]
[null,"User-Defined",7,4]
[null,"User-Defined",7,5]
[null,"User-Defined",7,7]
[null,"User-Defined",7,9]
[null,"User-Defined",8,1]
[null,"User-Defined",8,4]
[null,"User-Defined",8,5]
[null,"User-Defined",8,7]
[null,"User-Defined",8,9]
[null,"User-Defined",9,1]
[null,"User-Defined",9,4]
[null,"User-Defined",9,5]
[null,"User-Defined",9,7]
[null,"User-Defined",9,9]
[null,"User-Defined",11,1]
[null,"User-Defined",11,4]
[null,"User-Defined",11,5]
[null,"User-Defined",11,7]
[null,"User-Defined",11,9]
[null,"User-Defined",12,1]
[null,"User-Defined",12,4]
[null,"User-Defined",12,5]
[null,"User-Defined",12,7]
[null,"User-Defined",12,9]
[null,"User-Defined",13,1]
[null,"User-Defined",13,4]
[null,"User-Defined",13,5]
[null,"User-Defined",13,7]
[null,"User-Defined",13,9]
[null,"User-Defined",15,1]
[null,"User-Defined",15,4]
[null,"User-Defined",15,5]
[null,"User-Defined",15,7]
[null,"User-Defined",15,9]
[null,"User-Defined",16,1]
[null,"User-Defined",16,4]
[null,"User-Defined",16,5]
[null,"User-Defined",16,7]
[null,"User-Defined",16,9]
[null,"User-Defined",17,1]
[null,"User-Defined",17,4]
[null,"User-Defined",17,5]
[null,"User-Defined",17,7]
[null,"User-Defined",17,9]
[null,"User-Defined",19,1]
[null,"User-Defined",19,3]
[null,"User-Defined",19,4]
[null,"User-Defined",19,5]
[null,"User-Defined",19,7]
[null,"User-Defined",19,9]
[null,"User-Defined",20,1]
[null,"User-Defined",20,3]
[null,"User-Defined",20,4]
[null,"User-Defined",20,5]
[null,"User-Defined",20,7]
[null,"User-Defined",20,9]
[null,"User-Defined",21,1]
[null,"User-Defined",21,3]
[null,"User-Defined",21,4]
[null,"User-Defined",21,5]
[null,"User-Defined",21,7]
[null,"User-Defined",21,9]
[null,"User-Defined",23,2]
[null,"User-Defined",23,3]
[null,"User-Defined",23,4]
[null,"User-Defined",23,5]
[null,"User-Defined",23,6]
[null,"User-Defined",23,7]
[null,"User-Defined",23,9]
[null,"User-Defined",23,12]
[null,"User-Defined",23,13]
[null,"User-Defined",24,2]
[null,"User-Defined",24,3]
[null,"User-Defined",24,4]
[null,"User-Defined",24,5]
[null,"User-Defined",24,6]
[null,"User-Defined",24,7]
[null,"User-Defined",24,9]
[null,"User-Defined",24,12]
[null,"User-Defined",24,13]
[null,"User-Defined",25,2]
[null,"User-Defined",25,3]
[null,"User-Defined",25,4]
[null,"User-Defined",25,5]
[null,"User-Defined",25,6]
[null,"User-Defined",25,7]
[null,"User-Defined",25,9]
[null,"User-Defined",25,12]
[null,"User-Defined",25,13]
[null,"User-Defined",26,2]
[null,"User-Defined",26,3]
[null,"User-Defined",26,4]
[null,"User-Defined",26,5]
[null,"User-Defined",26,6]
[null,"User-Defined",26,7]
[null,"User-Defined",26,9]
[null,"User-Defined",26,12]
[null,"User-Defined",26,13]
[null,"User-Defined",27,2]
[null,"User-Defined",27,3]
[null,"User-Defined",27,4]
[null,"User-Defined",27,5]
[null,"User-Defined",27,6]
[null,"User-Defined",27,7]
[null,"User-Defined",27,9]
[null,"User-Defined",27,12]
[null,"User-Defined",27,13]

{"sheet":"Glossary","index":26,"n_rows":56,"n_cols":4,"rows_kept":56,"cut":false,"hidden":false,"merged":[[0,14,0,15],[0,16,0,17],[1,16,1,17],[1,1,1,3]]}
[]
[null,"GLOSSARY OF TERMS\nNovember 2023"]
[]
[null,"Abbreviated Term","Full Term","Description"]
[]
[null,"Assemblies","Building envelope assemblies","Assembly of building materials to form a wall, floor or roof unit. Can be prefabricated or site-built. May or may not include vapor, air, and water barriers."]
[null,"BfCA","Builders for Climate Action","A non-profit division of the Endeavour Centre and the developers of this tool."]
[null,"Carbon Storage or CO2e Storage","Biogenic carbon dioxide equivalent storage","The amount of uptake of the element carbon (C) from the atmosphere during a biological process, such as photosynthesis. Each mole of carbon (molar mass = 12) can be equated to one mole of carbon dioxide (molar mass = 44) removed from the atmosphere for the purpose of carbon accounting. Thus 1 carbon element contained in biomass represents 44/12, (approximately 3.67) molecules of biogenic CO2 sequestered from the atmosphere. The transformation of biomass (and its embodied “biogenic” carbon) into products represents in effect a removal of CO2, via its continued storage in the product over a period of time. These are counted as negative emissions."]
[null,"CLT","Cross-Laminated Timber"]
[null,"CMU","Concrete Masonry Unit"]
[null,"CO2e Emissions or \"Carbon\"","Carbon dioxide equivalent emissions","\"Carbon\", shorthand for carbon dioxide equivalent emissions, is the standard for measuring GWP attributed to a person, object, process or system with defined boundaries. In general, the term \"carbon\" may reference material carbon emissions, operational carbon emissions, or the sum of both. The unit is kilograms of CO2 equivalent by total mass or mass per unit (e.g. kg CO2e/m2). For any amount of any greenhouse gas in the atmosphere, it is the amount of CO2 which would warm the Earth as much as the amount of that particular gas. The GWP for CO2 is 1, since it is the baseline reference. For example, the GWP20 of HFC-23 gas is 12,000 kg CO2e, meaning 1 kg of HFC-23 in the atmosphere for 20 years has the same GWP as 12,000 kg of carbon dioxide gas. In this calculator the cradle-to-gate carbon attributed to the building or project is reported as a total and by unit floor area."]
[null,"Cob",null,"A traditional building material composed of clay-based soil, sand, and chopped straw. Cob walls are a vapour-open, monolithic, structural assembly, usually plastered on both sides with clay or lime plaster."]
[null,"Cradle-to-Gate","EPD phases A1-A3","Essentially the manufacturing phase, the cradle-to-gate lifecycle phases of a product or material include resource extraction/collection, transportation of materials to be processed, processing/manufacturing and packaging."]
[null,"CRMCA","Canadian Ready-Mixed Concrete Association"]
[null,"DLT","Dowel Laminated Timber"]
[null,"EC3","Embodied Carbon in Construction Calculator","An online carbon calculator tool from Building Transparency, developed by C-Change Labs. EC3 is used for counting and comparing embodied carbon of building materials with available EPDs."]
[null,"Energy Consumption","Operational energy consumption","The quantity of energy consumed annually (kW·h/yr) to operate the building over a given time period, usually a year. Operational energy typically includes, but is not limited to, heating, cooling, refrigeration, hot water, ventilation lighting, mechanical equipment and electronics. Often non-electric energy consumption is expressed as a mass or volume of fuel (e.g. wood, natural gas, propane, etc.) required to provide the energy consumed in that period."]
[null,"EPD","Environmental Product Declaration","A transparent, independently verified delaration that quantifies the environmental impacts of the life cycle of a product to enable comparisons between products fulfilling the same function. The EPD methodology is based on the Life Cycle Assessment (LCA) tool that follows International Organization for Standardization (ISO) standards and product category rules (PCRs). This calculator uses the GWP values for phases A1-A3 from EPDs unless otherwise specified."]
[null,"FA","Fly Ash","A byproduct of coal-fired power production. It is used as a Supplementary Cementitious Material (SCM) to replace cement content in concrete production."]
[null,"FSC","Forest Stewardship Council","FSC is an international non-profit, multistakeholder organization that has developed rigorous procedures and global standards for voluntary forest certification systems established for forests and forest products."]
[null,"GHG","Greenhouse Gas (Emissions)","Gases responsible for radiative forcing that traps heat in the atmosphere causing increased global temperatures. Units: kg CO2e"]
[null,"GLT or Glulam","Glue Laminated Timber"]
[null,"GU","General Use cement type"]
[null,"GWP","Global Warming Potential","The impact of GHGs attributed to a material, process or system measured in units of kg of CO2e. (See Carbon dioxide equivalent)"]
[null,"Hempcrete",null,"A building material made with lime (CaO), water and hemp hurd. Hempcrete performs as a vapour-open, insulative-dominant material, with thermal mass properties. Performance and properties change with density and binder formulations. It can be used as infill insulation in walls, floors and roofs, or pre-formed into panels or blocks."]
[null,"HFC","Hydroflurocarbons"]
[null,"HFO","Hydrofluoroolefins"]
[null,"ICE","Inventory of Carbon and Energy","Database of embodied energy and carbon of building materials from the University of Bath (UK), Sustainable Energy Research Team. (https://www.bath.ac.uk/teams/sustainable-energy-research-team/)"]
[null,"ICF","Insulated Concrete Forms"]
[null,"ISO","International Organization for Standardization","An international standard-setting body composed of representatives from various national standards organizations"]
[null,"kW·h","Kilowatt-hours","A metric system unit – power (kJ/s) multiplied by time (hours)  – used to measure electrical energy consumption."]
[null,"LCA","Life Cycle Assessment","Also known as life-cycle analysis, it is a methodology for assessing environmental impacts associated with all the stages of the life-cycle of a product, process, or service. For instance, in the case of a manufactured product, environmental impacts are assessed from raw material extraction and processing (cradle), through the product's manufacturing (gate), distribution and use, and recycling or final disposal of the materials (grave)."]
[null,"LSL","Laminated Strand Lumber"]
[null,"LVL","Laminated Veneer Lumber"]
[null,"MCE","Material Carbon Emissions","MCE is sometimes referred to informally as embodied carbon.  MCEs differ from embodied carbon in that MCEs include the emissions only from the product manufacturing stages (A1 to A3) of the building lifecycle (with a few exceptions), while embodied carbon includes all phases of the lifecycle except B6 (operational emissions) and B7 (operational water use).  This Materials Carbon Emissions Estimator calculates estimated MCEs"]
[null,"MgO","Magnesium Oxide"]
[null,"MPa","Megapascals"]
[null,"N. Gas","Natural Gas"]
[null,"NZC","Net Zero Carbon","For embodied carbon, NZC means a parity has been reached of embodied carbon emissions (+) and biogenic carbon storage (-), resulting in a net zero balance of CO2e exchange with the atmosphere. For operational carbon, NZC means any carbon emissions from generating offsite energy consumed annually by the building are offset with carbon credits. Typically a NZ operating carbon building design will prioritize reducing energy consumption and produce on-site energy generation to meet all demand. Definitions and criteria will vary from these descriptions between certification systems and sources."]
[null,"Off-gassing","VOC evaporation","Volatile organic compounds (VOCs) evaporate from some building materials over time, releasing them into the indoor and/or outdoor environment, potentially causing indoor air quality and climate concerns. Off-gassing also refers to the gases that release from some insulation types which use high GHG blowing-agents that leak from the cells during use."]
[null,"Operational Carbon","Operational carbon emissions","Also known as operating carbon, carbon emissions, or simply emissions or carbon, terms that may implicitly exclude embodied carbon. Operation carbon is the mass quantity of CO2e emitted to generate (and sometimes transport) the operational energy consumed in the operation of the building. (see Energy Consumption)"]
[null,"PSL","Parallel Strand Lumber"]
[null,"RSI","Thermal Resistance per area in SI units","A measure per unit area of resistance to heat flow through a material or assembly of materials in metric/SI units (m2·K/W or m2·°C/W)."]
[null,"R-Value","Thermal Resistance in U.S./imperial units","A measure per unit area of resistance to heat flow through a material or assembly of materials in I-P units (ft2·°F·h/BTU) in the U.S. and Canada, where I-P stands for Inches and Pounds. R-Value is often communicated as R-value per inch of material thickness, or R per inch. "]
[null,"SL","Slag","A glass-like byproduct of smelting or refining ore. It is used as a Supplementary Cementitious Material (SCM) to replace cement content in concrete production."]
[null,"SPF","Spruce, Pine, Fir ","A group of similar tree species predominantly used for softwood lumber products in various regions of North America, particularly in the East of the continent."]
[null,"SPFA","Spray Polyurethane Foam Association"]
[null,"t","tonne or metric tonne","One metric tonne, abbrebiated to 't', is a unit equivalent to 1000 kg. This is distinct from US Tons, Short Tons, etc."]
[null,"W Section","Structural steel wide flange I-beam","W-sections form a category of steel beam section profiles with a wide flanged I shape."]
[]
[null,"Cradle-to-grave","EPD phases A, B, and C","Includes the full life cycle from extraction of raw materials from the Earth (the cradle, phase A1 – raw material supply) to the end of the end-of-life process (the grave, phase C4 – disposal).  Does not include phase D – benefits and loads beyond the lifecycle (e.g. recycling).  "]
[null,"EC","Embodied Carbon","The lifecycle carbon emissions of the building materials.  Includes emissions from all lifecycle phases of the building except for B6 (operational emissions) and B7 (operational water use)."]
[]
[]
[null,"© His Majesty the King in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Glossaire","index":27,"n_rows":55,"n_cols":4,"rows_kept":55,"cut":false,"hidden":true,"merged":[[0,14,0,15],[0,16,0,17],[1,1,1,3],[1,16,1,17]]}
[]
[null,"GLOSSAIRE\nNovembre 2023"]
[]
[null,"Sigle ou abréviation","Terme en entier","Description"]
[null,"ACV","Analyse du cycle de vie","Également connu sous le nom d’analyse du cycle de vie, il s’agit d’une méthodologie permettant d’évaluer les impacts environnementaux associés à toutes les étapes du cycle de vie d’un produit, d’un processus ou d’un service. Par exemple, dans le cas d’un produit manufacturé, les impacts environnementaux sont évalués depuis l’extraction et le traitement des matières premières (berceau), en passant par la fabrication du produit (porte), la distribution et l’utilisation, et le recyclage ou l’élimination des matériaux (tombe)."]
[null,"AMPP","Association de la mousse de polyuréthane pulvérisée"]
[null,"ANBP","Association nationale du béton prémélangé"]
[null,"BCP","Bois à copeaux parallèles"]
[null,"BfCA","Builders for Climate Action","Une division à but non lucratif de l’Endeavour Centre et des développeurs de cet outil."]
[null,"BLC","Bois lamellé-croisé"]
[null,"BLC","Bois lamellé-collé"]
[null,"BLCG","Bois lamellé-collé à goujon"]
[null,"BLCL","Bois de longs copeaux lamellés "]
[null,"BPS","Bois en placage stratifié"]
[null,"Brique de chanvre",null,"Un matériau de construction fait de chaux (CaO), d’eau et de chanvre. La brique de chanvre se comporte comme un matériau ouvert à la vapeur, à dominante isolante, avec des propriétés de masse thermique. Les performances et les propriétés changent en fonction de la densité et de la formulation des liants. Il peut être utilisé comme isolant de remplissage dans les murs, les planchers et les toits, ou préformé en panneaux ou en blocs."]
[null,"Carbone intrinsèque","Phases A1-A3 de la DEP","Essentiellement la phase de production, de l’extraction des matières premières à la fabrication, d’un produit ou d’un matériau comprennent l’extraction/collecte des ressources, le transport des matériaux à traiter, la transformation/fabrication et le conditionnement."]
[null,"Carbone opérationnel","Émissions de carbone opérationnel","Également connu sous le nom d’émissions de carbone ou simplement d’émissions ou de carbone, des termes qui peuvent implicitement exclure le carbone incorporé. Le carbone d’exploitation est la quantité massique de CO2 émise pour générer (et parfois transporter) l’énergie d’exploitation consommée pour le fonctionnement du bâtiment. (voir la consommation d’énergie)"]
[null,"CBI","Coffrage à béton isolé"]
[null,"CCIC","Calculateur de carbone incorporé dans la construction","Un outil de calcul du carbone en ligne de Building Transparency, développé par C-Change Labs. Le CCIC est utilisé pour compter et comparer le carbone incorporé des matériaux de construction avec les DEP disponibles."]
[null,"CNZ","Carbone net zéro","Pour le carbone incorporé, NZC signifie qu’une parité a été atteinte entre les émissions de carbone incorporé (+) et le stockage de carbone biogénique (– ), ce qui se traduit par un solde net nul d’échange de CO2 avec l’atmosphère. Pour le carbone opérationnel, le CNZ signifie que toute émission de carbone provenant de la production d’énergie hors site consommée annuellement par le bâtiment est compensée par des crédits carbone. En général, la conception d’un bâtiment carboneutre donne la priorité à la réduction de la consommation d’énergie et à la production d’énergie sur place pour répondre à toute la demande. Les définitions et les critères varieront de ces descriptions entre les systèmes et les sources de certification."]
[null,"Consommation d’énergie","La consommation d’énergie opérationnelle","La quantité d’énergie consommée annuellement (kW-h/an) pour faire fonctionner le bâtiment sur une période donnée, généralement un an. L’énergie opérationnelle comprend généralement, mais pas exclusivement, le chauffage, le refroidissement, la réfrigération, l’eau chaude, la ventilation, l’éclairage, les équipements mécaniques et l’électronique. Souvent, la consommation d’énergie non électrique est exprimée en masse ou en volume de combustible (par exemple, bois, gaz naturel, propane, etc.) nécessaire pour fournir l’énergie consommée pendant cette période."]
[null,"CTU","Type de ciment tout usage"]
[null,"CV","Cendres volantes","Un sous-produit de la production d’électricité à partir du charbon. Il est utilisé comme matériau cimentaire supplémentaire (MCS) pour remplacer le ciment dans la production de béton."]
[null,"Dégagement gazeux","Évaporation de COV","Les composés organiques volatils (COV) s’évaporent de certains matériaux de construction au fil du temps, les libérant dans l’environnement intérieur et/ou extérieur, ce qui peut poser des problèmes de qualité de l’air intérieur et de climat. Le dégagement gazeux fait également référence aux gaz qui se dégagent de certains types d’isolation utilisant des agents gonflants à forte teneur en GES et qui s’échappent des cellules pendant l’utilisation."]
[null,"DEP","Déclaration environnementale de produit","Une déclaration transparente, vérifiée de manière indépendante, qui quantifie les impacts environnementaux du cycle de vie d’un produit afin de permettre des comparaisons entre des produits remplissant la même fonction. La méthodologie EPD est basée sur l’outil d’analyse du cycle de vie (ACV) qui suit les normes de l’Organisation internationale de normalisation (ISO) et les règles des catégories de produits (RCP; ce calculateur utilise les valeurs de PRP pour les phases A1-A3 des DEP, sauf indication contraire."]
[null,"ECM","Émissions de carbone des matériaux","Les émissions de carbone des matériaux (ECM) sont parfois appelé de manière informelle le carbone intrinsèque.  Les ECM diffèrent du carbone intrinsèque en ce sens que les ECM ne comprennent les émissions que des étapes de fabrication du produit (A1 à A3) du cycle de vie du bâtiment (à quelques exceptions près), tandis que le carbone intrinsèque comprend toutes les phases du cycle de vie, à l'exception de B6 (émissions opérationnelles) et B7 (utilisation opérationnelle de l'eau).  Cet estimateur d'émissions de carbone des matériaux calcule les EMC estimés"]
[null,"EMB","Élément de maçonnerie en béton"]
[null,"Émissions de CO2e ou de « carbone »","Émissions d’équivalent dioxyde de carbone","« Carbone », abréviation d’émissions équivalentes de dioxyde de carbone, est la norme de mesure du PRP attribué à une personne, un objet, un processus ou un système aux limites définies. En général, le terme « carbone » peut faire référence aux émissions de carbone matérielles, aux émissions de carbone opérationnelles, ou à la somme des deux. L’unité est le kilogramme d’équivalent CO2 par masse totale ou masse par unité (par exemple, kg CO2 e/m2). Pour toute quantité de gaz à effet de serre dans l’atmosphère, c’est la quantité de CO2 qui réchaufferait la Terre autant que la quantité de ce gaz particulier. Le PRP du CO2 est de 1, puisqu’il s’agit de la référence de base. Par exemple, le PRP20 du gaz HFC-23 est de 12 000 kg CO2e, ce qui signifie que 1 kg de HFC-23 dans l’atmosphère pendant 20 ans a le même PRGPque 12 000 kg de gaz carbonique. Dans ce calculateur, le carbone du berceau à la porte attribué au bâtiment ou au projet est indiqué en tant que total et par unité de surface."]
[null,"Ensemble","L’ensemble de l’enveloppe du bâtiment","Plusieurs matériaux de construction utilisés ensemble pour former une paroi, un plancher ou un toit. Peut être préfabriqué ou construit sur place. Peut ou non inclure des barrières de vapeur, d’air ou d’eau."]
[null,"EPS","Épicéa, pin, sapin ","Un groupe d’espèces d’arbres similaires utilisées principalement pour les produits de bois d’œuvre résineux dans diverses régions d’Amérique du Nord, en particulier dans l’Est du continent."]
[null,"FSC","Forest Stewardship Council","Le FSC est une organisation internationale à but non lucratif et multipartite qui a développé des procédures rigoureuses et des normes mondiales pour les systèmes de certification forestière volontaire établis pour les forêts et les produits forestiers."]
[null,"GES","Gaz à effet de serre (émissions)","Gaz responsables du forçage radiatif qui piège la chaleur dans l’atmosphère et provoque une augmentation des températures mondiales. Unités : kg de CO2e"]
[null,"GN","Gaz naturel"]
[null,"HFC","Hydroflurocarbones"]
[null,"HFO","Hydrofluoroléfine"]
[null,"ICE","Inventaire du carbone et de l’énergie","Base de données sur l’énergie intrinsèque et le carbone des matériaux de construction de l’équipe de recherche sur l’énergie durable de l’université de Bath (Royaume-Uni). (https://www.bath.ac.uk/teams/sustainable-energy-research-team/)"]
[null,"ISO","Organisation internationale de normalisation","Organisme international de normalisation composé de représentants de divers organismes nationaux de normalisation."]
[null,"kW·h","Kilowattheure","Unité du système métrique – puissance (kJ/s) multipliée par le temps (heures) – utilisée pour mesurer la consommation d’énergie électrique."]
[null,"MF","Mâchefer","Un sous-produit semblable à du verre provenant de la fonte ou de l’affinage du minerai. Il est utilisé comme matériau cimentaire supplémentaire (MCS) pour remplacer le ciment dans la production de béton."]
[null,"MPa","Megapascals"]
[null,"OM","Oxyde de magnésium"]
[null,"PRP","Potentiel de réchauffement de la planète","L’impact des GES attribué à un matériau, un processus ou un système, mesuré en unités de kg de CO2e. (Voir Équivalent en dioxyde de carbone)"]
[null,"RTS","Résistance thermique par surface en unités SI.","Mesure par unité de surface de la résistance au flux de chaleur à travers un matériau ou un assemblage de matériaux en unités métriques/SI (m2·K/W ou m2·°C/W)."]
[null,"Section W","Poutre en I à ailes larges en acier de construction","Les profilés W forment une catégorie de profilés de poutre en acier avec une forme en I à large rebord."]
[null,"Stockage de carbone ou stockage de CO2e ","Stockage d’équivalent dioxyde de carbone biogénique","La quantité d’absorption de l’élément carbone (C) de l’atmosphère au cours d’un processus biologique, tel que la photosynthèse. Chaque mole de carbone (masse molaire = 12) peut être assimilée à une mole de dioxyde de carbone (masse molaire = 44) retirée de l’atmosphère aux fins de la comptabilisation du carbone. Ainsi, un élément de carbone contenu dans la biomasse représente 44/12, (environ 3,67) molécules de CO2 biogénique séquestré de l’atmosphère. La transformation de la biomasse (et de son carbone « biogénique » incorporé) en produits représente en fait une élimination du CO2, par le biais de son stockage continu dans le produit pendant un certain temps. Ces émissions sont comptabilisées comme des émissions négatives."]
[null,"t","tonne ou tonne métrique","Une tonne métrique équivaut à 1000 kg. Il s’agit d’une différence par rapport aux tonnes américaines, aux tonnes courtes, etc."]
[null,"Torchis",null,"Un matériau de construction traditionnel composé de terre argileuse, de sable et de paille hachée. Les murs en torchis sont un assemblage structurel monolithique ouvert à la vapeur, généralement enduit sur les deux faces d’un plâtre d’argile ou de chaux."]
[null,"Valeur R","Résistance thermique en unités étasunienne/impériales","Mesure par unité de surface de la résistance au flux de chaleur à travers un matériau ou un assemblage de matériaux en unités I-P (pi2– °F-h/BTU) aux États-Unis et au Canada, où I-P signifie Pouce (inches) et Livre (pound). La valeur R est souvent communiquée comme valeur R par pouce d’épaisseur du matériau, ou R par pouce. "]
[]
[null,"du berceau à la tombe","Phases A, B et C de la DEP","Comprend le cycle de vie complet depuis l'extraction des matières premières de la Terre (le berceau, phase A1 - approvisionnement en matières premières) jusqu'à la fin du processus de fin de vie (la tombe, phase C4 - élimination).  Ne comprend pas la phase D - avantages et charges au-delà du cycle de vie (par exemple, le recyclage).  "]
[null,"CI","Carbone intrinsèque","Les émissions de carbone du cycle de vie des matériaux de construction.  Comprend les émissions de toutes les phases du cycle de vie du bâtiment, à l'exception de B6 (émissions opérationnelles) et B7 (utilisation opérationnelle de l'eau)."]
[]
[]
[null,"© His Majesty the king in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Energy GHG","index":28,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[[18,2,18,8],[19,0,19,1]]}
[null,null,"Province","GHG Factor Electricity","GHG Factor Natural Gas","GHG Factor Oil","GHG Factor Propane","GHG Factor Wood"]
[null,null,"Newfoundland and Labrador",3.4E-5,1.9123549999999999E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Prince Edward Island",2.7599999999999999E-4,1.9123549999999999E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Nova Scotia",7.3999999999999999E-4,1.9123549999999999E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"New Brunswick",2.7599999999999999E-4,1.9123549999999999E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Quebec",1.6199999999999999E-6,1.898355E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Ontario",3.4E-5,1.8993549999999999E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Manitoba",2.6599999999999999E-6,1.8973550000000001E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Saskatchewan",7.5199999999999996E-4,1.8403550000000001E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Alberta",8.0199999999999998E-4,1.939355E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"British Columbia",1.1579999999999998E-5,1.937355E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Yukon",5.3600000000000002E-5,1.9123549999999999E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Northwest Territories",2.32E-4,1.9123549999999999E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Nunavut",7.8200000000000003E-4,1.9123549999999999E-3,2.7554380000000002E-3,1.547859E-3,3.5826E-4]
[null,null,"Override Province"]
[null,null,"Override Value"]
[null,null,"Information Source"]
[]
[null,null,"GHG Calculations Results"]
["Fuel consumption from h2k file",null,"Province","Electricity","Natural Gas","Oil","Propane","Wood","Total"]
["Electricity_kWh",{"$f":"'USER INPUT SHEET'!M9","v":0},"Newfoundland and Labrador",{"$f":"($B$21-$B$32*277.77777778)*IF(D$15=C21,D$16,D2)","v":0},{"$f":"$B$22*IF(E$15=$C21,E$16,E2)","v":0},{"$f":"$B$23*F2","v":0},{"$f":"$B$24*G2","v":0},{"$f":"$B$25*H2","v":0},{"$f":"SUM(D21:H21)","v":0}]
["Natural Gas_m3",{"$f":"'USER INPUT SHEET'!N9","v":0},"Prince Edward Island",0,0,{"$f":"$B$23*F3","v":0},{"$f":"$B$24*G3","v":0},{"$f":"$B$25*H3","v":0},0]
["Oil_Litres",{"$f":"'USER INPUT SHEET'!N12","v":0},"Nova Scotia",0,0,0,0,0,0]
["Propane_Litres",{"$f":"'USER INPUT SHEET'!M12","v":0},"New Brunswick",0,0,0,0,0,0]
["Wood_Kg",{"$f":"'USER INPUT SHEET'!O12","v":0},"Quebec",0,0,0,0,0,0]
[null,null,"Ontario",{"$f":"($B$21-$B$32*277.77777778)*IF(D$15=C26,D$16,D7)","v":0},0,0,0,0,0]
[null,null,"Manitoba",{"$f":"($B$21-$B$32*277.77777778)*IF(D$15=C27,D$16,D8)","v":0},{"$f":"$B$22*IF(E$15=$C27,E$16,E8)","v":0},0,0,0,0]
[null,null,"Saskatchewan",0,0,0,0,0,0]
[null,null,"Alberta",0,0,0,0,0,0]
[null,null,"British Columbia",0,0,0,0,0,0]
[null,null,"Yukon",0,0,0,0,0,0]
["Renewables_GJ",null,"Northwest Territories",0,0,0,0,0,0]
[null,null,"Nunavut",0,0,0,0,0,0]
[]
[]
[]
[null,"© His Majesty the king in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Element Properties","index":29,"n_rows":1283,"n_cols":11,"rows_kept":1283,"cut":false,"hidden":true,"merged":[[1,3,1,4],[1,5,1,6]]}
["About this sheet"]
[null,null,null,"English version",null,"French version"]
["Sheet code","Type","Address","Width","Height","Width","Height","French sheet name","For Search - EN","For Search - FR","© His Majesty the king in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
["USER INPUT SHEET","Button","Rounded Rectangle 16||Rectangle: Rounded Corners 16",353.0625,37.861649999999997,345,52.687399999999997,"FICHE D’ENTRÉE UTILISATEUR",{"$f":"A4&C4","v":"USER INPUT SHEETRounded Rectangle 16||Rectangle: Rounded Corners 16"},{"$f":"H4&C4","v":"FICHE D’ENTRÉE UTILISATEURRounded Rectangle 16||Rectangle: Rounded Corners 16"},"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]
["USER INPUT SHEET","Button","Rounded Rectangle 15||Rectangle: Rounded Corners 15",296.37049999999999,37.861649999999997,296.37049999999999,52.687399999999997,"FICHE D’ENTRÉE UTILISATEUR",{"$f":"A5&C5","v":"USER INPUT SHEETRounded Rectangle 15||Rectangle: Rounded Corners 15"},{"$f":"H5&C5","v":"FICHE D’ENTRÉE UTILISATEURRounded Rectangle 15||Rectangle: Rounded Corners 15"}]
["USER INPUT SHEET","Range","$B$16",32.78,20.25,34,20.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$B$16","FICHE D’ENTRÉE UTILISATEUR$B$16"]
["USER INPUT SHEET","Range","$B$17",32.78,23.25,34,23.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$B$17","FICHE D’ENTRÉE UTILISATEUR$B$17"]
["USER INPUT SHEET","Range","$B$18",32.78,20.25,34,20.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$B$18","FICHE D’ENTRÉE UTILISATEUR$B$18"]
["USER INPUT SHEET","Range","$E$25",3.56,38.75,5.33,38.75,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$E$25","FICHE D’ENTRÉE UTILISATEUR$E$25"]
["USER INPUT SHEET","Range","$F$42",11,35,11,53.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$F$42","FICHE D’ENTRÉE UTILISATEUR$F$42"]
["USER INPUT SHEET","Range","$G$42",1.56,35,1.56,53.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$G$42","FICHE D’ENTRÉE UTILISATEUR$G$42"]
["USER INPUT SHEET","Range","$H$42",10.44,35,10.44,53.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$H$42","FICHE D’ENTRÉE UTILISATEUR$H$42"]
["USER INPUT SHEET","Range","$I$42",1.44,35,1.44,53.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$I$42","FICHE D’ENTRÉE UTILISATEUR$I$42"]
["USER INPUT SHEET","Range","$J$42",9.44,35,9.44,53.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$J$42","FICHE D’ENTRÉE UTILISATEUR$J$42"]
["USER INPUT SHEET","Range","$K$42",12.89,35,12.89,53.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$K$42","FICHE D’ENTRÉE UTILISATEUR$K$42"]
["USER INPUT SHEET","Range","$M$45",17,8.1,18,8.1,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$M$45","FICHE D’ENTRÉE UTILISATEUR$M$45"]
["USER INPUT SHEET","Range","$N$45",17,8.1,18,8.1,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$N$45","FICHE D’ENTRÉE UTILISATEUR$N$45"]
["USER INPUT SHEET","Range","$O$45",14.67,8.1,14.67,8.1,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$O$45","FICHE D’ENTRÉE UTILISATEUR$O$45"]
["USER INPUT SHEET","Range","$M$46",17,44.5,{"$f":"$F$16","v":18},47,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$M$46","FICHE D’ENTRÉE UTILISATEUR$M$46"]
["USER INPUT SHEET","Range","$M$47",17,34,{"$f":"$F$16","v":18},54.75,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$M$47","FICHE D’ENTRÉE UTILISATEUR$M$47"]
["USER INPUT SHEET","Range","$N$47",17,34,{"$f":"$F$17","v":18},54.75,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$N$47","FICHE D’ENTRÉE UTILISATEUR$N$47"]
["USER INPUT SHEET","Range","$O$47",14.67,34,14.67,54.75,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$O$47","FICHE D’ENTRÉE UTILISATEUR$O$47"]
["USER INPUT SHEET","Range","$M$51",17,47.25,{"$f":"$F$16","v":18},53.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$M$51","FICHE D’ENTRÉE UTILISATEUR$M$51"]
["USER INPUT SHEET","Range","$N$51",17,47.25,{"$f":"$F$17","v":18},53.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$N$51","FICHE D’ENTRÉE UTILISATEUR$N$51"]
["USER INPUT SHEET","Range","$O$51",14.67,47.25,14.67,53.25,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$O$51","FICHE D’ENTRÉE UTILISATEUR$O$51"]
["USER INPUT SHEET","Range","$M$55",17,35,{"$f":"$F$16","v":18},47,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$M$55","FICHE D’ENTRÉE UTILISATEUR$M$55"]
["USER INPUT SHEET","Range","$S$37",6.91,54.8,7.18,54.8,"FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET$S$37","FICHE D’ENTRÉE UTILISATEUR$S$37"]
["Footings & Slabs","Range","$D$1",18.89,54.75,18.89,83.25,"Semelles et dalles","Footings & Slabs$D$1","Semelles et dalles$D$1"]
["Footings & Slabs","Range","$C$7",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$7","Semelles et dalles$C$7"]
["Footings & Slabs","Range","$C$8",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$8","Semelles et dalles$C$8"]
["Footings & Slabs","Range","$C$9",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$9","Semelles et dalles$C$9"]
["Footings & Slabs","Range","$C$10",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$10","Semelles et dalles$C$10"]
["Footings & Slabs","Range","$C$11",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$11","Semelles et dalles$C$11"]
["Footings & Slabs","Range","$C$14",56.78,"two_lines",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$14","Semelles et dalles$C$14"]
["Footings & Slabs","Range","$C$15",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$15","Semelles et dalles$C$15"]
["Footings & Slabs","Range","$C$16",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$16","Semelles et dalles$C$16"]
["Footings & Slabs","Range","$C$17",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$17","Semelles et dalles$C$17"]
["Footings & Slabs","Range","$C$18",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$18","Semelles et dalles$C$18"]
["Footings & Slabs","Range","$C$19",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$19","Semelles et dalles$C$19"]
["Footings & Slabs","Range","$C$20",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$20","Semelles et dalles$C$20"]
["Footings & Slabs","Range","$C$22",56.78,"two_lines",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$22","Semelles et dalles$C$22"]
["Footings & Slabs","Range","$C$23",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$23","Semelles et dalles$C$23"]
["Footings & Slabs","Range","$C$24",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$24","Semelles et dalles$C$24"]
["Footings & Slabs","Range","$C$25",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$25","Semelles et dalles$C$25"]
["Footings & Slabs","Range","$C$26",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$26","Semelles et dalles$C$26"]
["Footings & Slabs","Range","$C$27",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$27","Semelles et dalles$C$27"]
["Footings & Slabs","Range","$C$28",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$28","Semelles et dalles$C$28"]
["Footings & Slabs","Range","$C$30",56.78,"two_lines",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$30","Semelles et dalles$C$30"]
["Footings & Slabs","Range","$C$31",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$31","Semelles et dalles$C$31"]
["Footings & Slabs","Range","$C$32",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$32","Semelles et dalles$C$32"]
["Footings & Slabs","Range","$C$33",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$33","Semelles et dalles$C$33"]
["Footings & Slabs","Range","$C$34",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$34","Semelles et dalles$C$34"]
["Footings & Slabs","Range","$C$35",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$35","Semelles et dalles$C$35"]
["Footings & Slabs","Range","$C$36",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$36","Semelles et dalles$C$36"]
["Footings & Slabs","Range","$C$39",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$39","Semelles et dalles$C$39"]
["Footings & Slabs","Range","$C$40",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$40","Semelles et dalles$C$40"]
["Footings & Slabs","Range","$C$41",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$41","Semelles et dalles$C$41"]
["Footings & Slabs","Range","$C$42",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$42","Semelles et dalles$C$42"]
["Footings & Slabs","Range","$C$43",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$43","Semelles et dalles$C$43"]
["Footings & Slabs","Range","$C$44",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$44","Semelles et dalles$C$44"]
["Footings & Slabs","Range","$C$45",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$45","Semelles et dalles$C$45"]
["Footings & Slabs","Range","$C$46",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$46","Semelles et dalles$C$46"]
["Footings & Slabs","Range","$C$50",56.78,23.25,46.44,73,"Semelles et dalles","Footings & Slabs$C$50","Semelles et dalles$C$50"]
["Footings & Slabs","Range","$C$52",56.78,84.75,46.44,105,"Semelles et dalles","Footings & Slabs$C$52","Semelles et dalles$C$52"]
["Footings & Slabs","Range","$C$55",56.78,"two_lines",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$55","Semelles et dalles$C$55"]
["Footings & Slabs","Range","$C$56",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$56","Semelles et dalles$C$56"]
["Footings & Slabs","Range","$C$57",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$57","Semelles et dalles$C$57"]
["Footings & Slabs","Range","$C$58",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$58","Semelles et dalles$C$58"]
["Footings & Slabs","Range","$C$59",56.78,"one_line",46.44,"two_lines","Semelles et dalles",{"$f":"A69&C69","v":"Footings & Slabs$C$59"},{"$f":"H69&C69","v":"Semelles et dalles$C$59"}]
["Footings & Slabs","Range","$C$60",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$60","Semelles et dalles$C$60"]
["Footings & Slabs","Range","$C$61",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$61","Semelles et dalles$C$61"]
["Footings & Slabs","Range","$C$63",56.78,"two_lines",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$63","Semelles et dalles$C$63"]
["Footings & Slabs","Range","$C$64",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$64","Semelles et dalles$C$64"]
["Footings & Slabs","Range","$C$65",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$65","Semelles et dalles$C$65"]
["Footings & Slabs","Range","$C$66",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$66","Semelles et dalles$C$66"]
["Footings & Slabs","Range","$C$67",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$67","Semelles et dalles$C$67"]
["Footings & Slabs","Range","$C$68",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$68","Semelles et dalles$C$68"]
["Footings & Slabs","Range","$C$69",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$69","Semelles et dalles$C$69"]
["Footings & Slabs","Range","$C$71",56.78,"two_lines",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$71","Semelles et dalles$C$71"]
["Footings & Slabs","Range","$C$72",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$72","Semelles et dalles$C$72"]
["Footings & Slabs","Range","$C$73",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$73","Semelles et dalles$C$73"]
["Footings & Slabs","Range","$C$74",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$74","Semelles et dalles$C$74"]
["Footings & Slabs","Range","$C$75",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$75","Semelles et dalles$C$75"]
["Footings & Slabs","Range","$C$76",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$76","Semelles et dalles$C$76"]
["Footings & Slabs","Range","$C$77",56.78,"one_line",46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$77","Semelles et dalles$C$77"]
["Footings & Slabs","Range","$C$80",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$80","Semelles et dalles$C$80"]
["Footings & Slabs","Range","$C$84",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$84","Semelles et dalles$C$84"]
["Footings & Slabs","Range","$C$85",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$85","Semelles et dalles$C$85"]
["Footings & Slabs","Range","$C$88",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$88","Semelles et dalles$C$88"]
["Footings & Slabs","Range","$C$89",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$89","Semelles et dalles$C$89"]
["Footings & Slabs","Range","$C$90",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$90","Semelles et dalles$C$90"]
["Footings & Slabs","Range","$C$91",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$91","Semelles et dalles$C$91"]
["Footings & Slabs","Range","$C$93",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$93","Semelles et dalles$C$93"]
["Footings & Slabs","Range","$C$96",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$96","Semelles et dalles$C$96"]
["Footings & Slabs","Range","$C$97",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$97","Semelles et dalles$C$97"]
["Footings & Slabs","Range","$C$98",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$98","Semelles et dalles$C$98"]
["Footings & Slabs","Range","$C$101",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$101","Semelles et dalles$C$101"]
["Footings & Slabs","Range","$C$102",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$102","Semelles et dalles$C$102"]
["Footings & Slabs","Range","$C$104",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$104","Semelles et dalles$C$104"]
["Footings & Slabs","Range","$C$108",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$108","Semelles et dalles$C$108"]
["Footings & Slabs","Range","$C$109",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$109","Semelles et dalles$C$109"]
["Footings & Slabs","Range","$C$110",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$110","Semelles et dalles$C$110"]
["Footings & Slabs","Range","$C$112",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$112","Semelles et dalles$C$112"]
["Footings & Slabs","Range","$C$114",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$114","Semelles et dalles$C$114"]
["Footings & Slabs","Range","$C$115",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$115","Semelles et dalles$C$115"]
["Footings & Slabs","Range","$C$116",56.78,31.5,46.44,"three_lines","Semelles et dalles","Footings & Slabs$C$116","Semelles et dalles$C$116"]
["Footings & Slabs","Range","$C$117",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$117","Semelles et dalles$C$117"]
["Footings & Slabs","Range","$C$120",56.78,31.5,46.44,"four_lines","Semelles et dalles","Footings & Slabs$C$120","Semelles et dalles$C$120"]
["Footings & Slabs","Range","$C$121",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$121","Semelles et dalles$C$121"]
["Footings & Slabs","Range","$C$122",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$122","Semelles et dalles$C$122"]
["Footings & Slabs","Range","$C$123",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$123","Semelles et dalles$C$123"]
["Footings & Slabs","Range","$C$124",56.78,23.25,46.44,"three_lines","Semelles et dalles","Footings & Slabs$C$124","Semelles et dalles$C$124"]
["Footings & Slabs","Range","$C$127",56.78,31.5,46.44,"three_lines","Semelles et dalles","Footings & Slabs$C$127","Semelles et dalles$C$127"]
["Footings & Slabs","Range","$C$128",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$128","Semelles et dalles$C$128"]
["Footings & Slabs","Range","$C$129",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$129","Semelles et dalles$C$129"]
["Footings & Slabs","Range","$C$130",56.78,29.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$130","Semelles et dalles$C$130"]
["Footings & Slabs","Range","$C$131",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$131","Semelles et dalles$C$131"]
["Footings & Slabs","Range","$C$132",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$132","Semelles et dalles$C$132"]
["Footings & Slabs","Range","$C$136",56.78,63,46.44,"five_lines","Semelles et dalles","Footings & Slabs$C$136","Semelles et dalles$C$136"]
["Footings & Slabs","Range","$C$137",56.78,31.5,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$137","Semelles et dalles$C$137"]
["Footings & Slabs","Range","$C$139",56.78,23.25,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$139","Semelles et dalles$C$139"]
["Footings & Slabs","Range","$C$140",56.78,30.75,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$140","Semelles et dalles$C$140"]
["Footings & Slabs","Range","$C$141",56.78,30.75,46.44,"two_lines","Semelles et dalles","Footings & Slabs$C$141","Semelles et dalles$C$141"]
["Footings & Slabs","Range","$C$143",56.78,31.5,46.44,"three_lines","Semelles et dalles","Footings & Slabs$C$143","Semelles et dalles$C$143"]
["Foundation Walls","Range","$C$7",54.89,"two_lines",46.44,"two_lines","Murs de fondation","Foundation Walls$C$7","Murs de fondation$C$7"]
["Foundation Walls","Range","$C$8",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$8","Murs de fondation$C$8"]
["Foundation Walls","Range","$C$9",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$9","Murs de fondation$C$9"]
["Foundation Walls","Range","$C$10",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$10","Murs de fondation$C$10"]
["Foundation Walls","Range","$C$11",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$11","Murs de fondation$C$11"]
["Foundation Walls","Range","$C$12",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$12","Murs de fondation$C$12"]
["Foundation Walls","Range","$C$13",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$13","Murs de fondation$C$13"]
["Foundation Walls","Range","$C$15",54.89,"two_lines",46.44,"two_lines","Murs de fondation","Foundation Walls$C$15","Murs de fondation$C$15"]
["Foundation Walls","Range","$C$16",54.89,"one_line",46.44,"two_lines","Murs de fondation",{"$f":"A133&C133","v":"Foundation Walls$C$16"},{"$f":"H133&C133","v":"Murs de fondation$C$16"}]
["Foundation Walls","Range","$C$17",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$17","Murs de fondation$C$17"]
["Foundation Walls","Range","$C$18",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$18","Murs de fondation$C$18"]
["Foundation Walls","Range","$C$19",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$19","Murs de fondation$C$19"]
["Foundation Walls","Range","$C$20",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$20","Murs de fondation$C$20"]
["Foundation Walls","Range","$C$21",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$21","Murs de fondation$C$21"]
["Foundation Walls","Range","$C$23",54.89,"two_lines",46.44,"two_lines","Murs de fondation","Foundation Walls$C$23","Murs de fondation$C$23"]
["Foundation Walls","Range","$C$24",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$24","Murs de fondation$C$24"]
["Foundation Walls","Range","$C$25",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$25","Murs de fondation$C$25"]
["Foundation Walls","Range","$C$26",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$26","Murs de fondation$C$26"]
["Foundation Walls","Range","$C$27",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$27","Murs de fondation$C$27"]
["Foundation Walls","Range","$C$28",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$28","Murs de fondation$C$28"]
["Foundation Walls","Range","$C$29",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$29","Murs de fondation$C$29"]
["Foundation Walls","Range","$C$33",54.89,31.5,46.44,"three_lines","Murs de fondation","Foundation Walls$C$33","Murs de fondation$C$33"]
["Foundation Walls","Range","$C$34",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$34","Murs de fondation$C$34"]
["Foundation Walls","Range","$C$35",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$35","Murs de fondation$C$35"]
["Foundation Walls","Range","$C$36",54.89,31.5,46.44,"three_lines","Murs de fondation","Foundation Walls$C$36","Murs de fondation$C$36"]
["Foundation Walls","Range","$C$37",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$37","Murs de fondation$C$37"]
["Foundation Walls","Range","$C$38",54.89,31.5,46.44,"three_lines","Murs de fondation","Foundation Walls$C$38","Murs de fondation$C$38"]
["Foundation Walls","Range","$C$40",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$40","Murs de fondation$C$40"]
["Foundation Walls","Range","$C$44",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$44","Murs de fondation$C$44"]
["Foundation Walls","Range","$C$45",54.89,31.5,46.44,"three_lines","Murs de fondation","Foundation Walls$C$45","Murs de fondation$C$45"]
["Foundation Walls","Range","$C$47",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$47","Murs de fondation$C$47"]
["Foundation Walls","Range","$C$48",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$48","Murs de fondation$C$48"]
["Foundation Walls","Range","$C$49",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$49","Murs de fondation$C$49"]
["Foundation Walls","Range","$C$50",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$50","Murs de fondation$C$50"]
["Foundation Walls","Range","$C$51",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$51","Murs de fondation$C$51"]
["Foundation Walls","Range","$C$53",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$53","Murs de fondation$C$53"]
["Foundation Walls","Range","$C$54",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$54","Murs de fondation$C$54"]
["Foundation Walls","Range","$C$55",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$55","Murs de fondation$C$55"]
["Foundation Walls","Range","$C$56",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$56","Murs de fondation$C$56"]
["Foundation Walls","Range","$C$59",54.89,47.25,46.44,"three_lines","Murs de fondation","Foundation Walls$C$59","Murs de fondation$C$59"]
["Foundation Walls","Range","$C$60",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$60","Murs de fondation$C$60"]
["Foundation Walls","Range","$C$61",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$61","Murs de fondation$C$61"]
["Foundation Walls","Range","$C$62",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$62","Murs de fondation$C$62"]
["Foundation Walls","Range","$C$63",54.89,31.5,46.44,"four_lines","Murs de fondation","Foundation Walls$C$63","Murs de fondation$C$63"]
["Foundation Walls","Range","$C$65",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$65","Murs de fondation$C$65"]
["Foundation Walls","Range","$C$67",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$67","Murs de fondation$C$67"]
["Foundation Walls","Range","$C$68",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$68","Murs de fondation$C$68"]
["Foundation Walls","Range","$C$69",54.89,23.25,46.44,"three_lines","Murs de fondation","Foundation Walls$C$69","Murs de fondation$C$69"]
["Foundation Walls","Range","$C$70",54.89,23.25,46.44,60,"Murs de fondation","Foundation Walls$C$70","Murs de fondation$C$70"]
["Foundation Walls","Range","$C$71",54.89,23.25,46.44,"three_lines","Murs de fondation","Foundation Walls$C$71","Murs de fondation$C$71"]
["Foundation Walls","Range","$C$73",54.89,"two_lines",46.44,"two_lines","Murs de fondation","Foundation Walls$C$73","Murs de fondation$C$73"]
["Foundation Walls","Range","$C$74",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$74","Murs de fondation$C$74"]
["Foundation Walls","Range","$C$75",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$75","Murs de fondation$C$75"]
["Foundation Walls","Range","$C$76",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$76","Murs de fondation$C$76"]
["Foundation Walls","Range","$C$77",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$77","Murs de fondation$C$77"]
["Foundation Walls","Range","$C$78",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$78","Murs de fondation$C$78"]
["Foundation Walls","Range","$C$79",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$79","Murs de fondation$C$79"]
["Foundation Walls","Range","$C$81",54.89,"two_lines",46.44,"two_lines","Murs de fondation","Foundation Walls$C$81","Murs de fondation$C$81"]
["Foundation Walls","Range","$C$82",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$82","Murs de fondation$C$82"]
["Foundation Walls","Range","$C$83",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$83","Murs de fondation$C$83"]
["Foundation Walls","Range","$C$84",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$84","Murs de fondation$C$84"]
["Foundation Walls","Range","$C$85",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$85","Murs de fondation$C$85"]
["Foundation Walls","Range","$C$86",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$86","Murs de fondation$C$86"]
["Foundation Walls","Range","$C$87",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$87","Murs de fondation$C$87"]
["Foundation Walls","Range","$C$89",54.89,"two_lines",46.44,"two_lines","Murs de fondation","Foundation Walls$C$89","Murs de fondation$C$89"]
["Foundation Walls","Range","$C$90",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$90","Murs de fondation$C$90"]
["Foundation Walls","Range","$C$91",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$91","Murs de fondation$C$91"]
["Foundation Walls","Range","$C$92",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$92","Murs de fondation$C$92"]
["Foundation Walls","Range","$C$93",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$93","Murs de fondation$C$93"]
["Foundation Walls","Range","$C$94",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$94","Murs de fondation$C$94"]
["Foundation Walls","Range","$C$95",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$95","Murs de fondation$C$95"]
["Foundation Walls","Range","$C$97",54.89,31.5,46.44,"three_lines","Murs de fondation","Foundation Walls$C$97","Murs de fondation$C$97"]
["Foundation Walls","Range","$C$98",54.89,31.5,46.44,"three_lines","Murs de fondation",{"$f":"A197&C197","v":"Foundation Walls$C$98"},{"$f":"H197&C197","v":"Murs de fondation$C$98"}]
["Foundation Walls","Range","$C$99",54.89,31.5,46.44,"three_lines","Murs de fondation","Foundation Walls$C$99","Murs de fondation$C$99"]
["Foundation Walls","Range","$C$100",54.89,32.25,46.44,"three_lines","Murs de fondation","Foundation Walls$C$100","Murs de fondation$C$100"]
["Foundation Walls","Range","$C$102",54.89,"two_lines",46.44,"two_lines","Murs de fondation","Foundation Walls$C$102","Murs de fondation$C$102"]
["Foundation Walls","Range","$C$103",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$103","Murs de fondation$C$103"]
["Foundation Walls","Range","$C$104",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$104","Murs de fondation$C$104"]
["Foundation Walls","Range","$C$105",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$105","Murs de fondation$C$105"]
["Foundation Walls","Range","$C$106",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$106","Murs de fondation$C$106"]
["Foundation Walls","Range","$C$107",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$107","Murs de fondation$C$107"]
["Foundation Walls","Range","$C$108",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$108","Murs de fondation$C$108"]
["Foundation Walls","Range","$C$110",54.89,"two_lines",46.44,"two_lines","Murs de fondation","Foundation Walls$C$110","Murs de fondation$C$110"]
["Foundation Walls","Range","$C$111",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$111","Murs de fondation$C$111"]
["Foundation Walls","Range","$C$112",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$112","Murs de fondation$C$112"]
["Foundation Walls","Range","$C$113",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$113","Murs de fondation$C$113"]
["Foundation Walls","Range","$C$114",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$114","Murs de fondation$C$114"]
["Foundation Walls","Range","$C$115",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$115","Murs de fondation$C$115"]
["Foundation Walls","Range","$C$116",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$116","Murs de fondation$C$116"]
["Foundation Walls","Range","$C$118",54.89,"two_lines",46.44,"two_lines","Murs de fondation","Foundation Walls$C$118","Murs de fondation$C$118"]
["Foundation Walls","Range","$C$119",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$119","Murs de fondation$C$119"]
["Foundation Walls","Range","$C$120",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$120","Murs de fondation$C$120"]
["Foundation Walls","Range","$C$121",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$121","Murs de fondation$C$121"]
["Foundation Walls","Range","$C$122",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$122","Murs de fondation$C$122"]
["Foundation Walls","Range","$C$123",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$123","Murs de fondation$C$123"]
["Foundation Walls","Range","$C$124",54.89,"one_line",46.44,"two_lines","Murs de fondation","Foundation Walls$C$124","Murs de fondation$C$124"]
["Foundation Walls","Range","$C$127",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$127","Murs de fondation$C$127"]
["Foundation Walls","Range","$C$128",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$128","Murs de fondation$C$128"]
["Foundation Walls","Range","$C$129",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$129","Murs de fondation$C$129"]
["Foundation Walls","Range","$C$130",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$130","Murs de fondation$C$130"]
["Foundation Walls","Range","$C$134",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$134","Murs de fondation$C$134"]
["Foundation Walls","Range","$C$135",54.89,31.5,46.44,"three_lines","Murs de fondation","Foundation Walls$C$135","Murs de fondation$C$135"]
["Foundation Walls","Range","$C$136",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$136","Murs de fondation$C$136"]
["Foundation Walls","Range","$C$137",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$137","Murs de fondation$C$137"]
["Foundation Walls","Range","$C$140",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$140","Murs de fondation$C$140"]
["Foundation Walls","Range","$C$141",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$141","Murs de fondation$C$141"]
["Foundation Walls","Range","$C$142",54.89,31.5,46.44,"three_lines","Murs de fondation","Foundation Walls$C$142","Murs de fondation$C$142"]
["Foundation Walls","Range","$C$144",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$144","Murs de fondation$C$144"]
["Foundation Walls","Range","$C$145",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$145","Murs de fondation$C$145"]
["Foundation Walls","Range","$C$146",54.89,23.25,46.44,"one_line","Murs de fondation","Foundation Walls$C$146","Murs de fondation$C$146"]
["Foundation Walls","Range","$C$147",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$147","Murs de fondation$C$147"]
["Foundation Walls","Range","$C$149",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$149","Murs de fondation$C$149"]
["Foundation Walls","Range","$C$150",54.89,47.25,46.44,"four_lines","Murs de fondation","Foundation Walls$C$150","Murs de fondation$C$150"]
["Foundation Walls","Range","$C$152",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$152","Murs de fondation$C$152"]
["Foundation Walls","Range","$C$154",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$154","Murs de fondation$C$154"]
["Foundation Walls","Range","$C$155",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$155","Murs de fondation$C$155"]
["Foundation Walls","Range","$C$156",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$156","Murs de fondation$C$156"]
["Foundation Walls","Range","$C$157",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$157","Murs de fondation$C$157"]
["Foundation Walls","Range","$C$158",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$158","Murs de fondation$C$158"]
["Foundation Walls","Range","$C$159",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$159","Murs de fondation$C$159"]
["Foundation Walls","Range","$C$160",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$160","Murs de fondation$C$160"]
["Foundation Walls","Range","$C$161",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$161","Murs de fondation$C$161"]
["Foundation Walls","Range","$C$163",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$163","Murs de fondation$C$163"]
["Foundation Walls","Range","$C$170",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$170","Murs de fondation$C$170"]
["Foundation Walls","Range","$C$172",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$172","Murs de fondation$C$172"]
["Foundation Walls","Range","$C$173",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$173","Murs de fondation$C$173"]
["Foundation Walls","Range","$C$174",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$174","Murs de fondation$C$174"]
["Foundation Walls","Range","$C$175",54.89,23.25,46.44,"one_line","Murs de fondation","Foundation Walls$C$175","Murs de fondation$C$175"]
["Foundation Walls","Range","$C$177",54.89,30.75,46.44,"two_lines","Murs de fondation","Foundation Walls$C$177","Murs de fondation$C$177"]
["Foundation Walls","Range","$C$178",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$178","Murs de fondation$C$178"]
["Foundation Walls","Range","$C$182",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$182","Murs de fondation$C$182"]
["Foundation Walls","Range","$C$183",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$183","Murs de fondation$C$183"]
["Foundation Walls","Range","$C$184",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$184","Murs de fondation$C$184"]
["Foundation Walls","Range","$C$185",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$185","Murs de fondation$C$185"]
["Foundation Walls","Range","$C$186",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$186","Murs de fondation$C$186"]
["Foundation Walls","Range","$C$188",54.89,47.25,46.44,"three_lines","Murs de fondation","Foundation Walls$C$188","Murs de fondation$C$188"]
["Foundation Walls","Range","$C$189",54.89,23.25,46.44,"two_lines","Murs de fondation",{"$f":"A261&C261","v":"Foundation Walls$C$189"},{"$f":"H261&C261","v":"Murs de fondation$C$189"}]
["Foundation Walls","Range","$C$190",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$190","Murs de fondation$C$190"]
["Foundation Walls","Range","$C$192",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$192","Murs de fondation$C$192"]
["Foundation Walls","Range","$C$193",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$193","Murs de fondation$C$193"]
["Foundation Walls","Range","$C$194",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$194","Murs de fondation$C$194"]
["Foundation Walls","Range","$C$195",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$195","Murs de fondation$C$195"]
["Foundation Walls","Range","$C$196",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$196","Murs de fondation$C$196"]
["Foundation Walls","Range","$C$197",54.89,23.25,46.44,"two_lines","Murs de fondation","Foundation Walls$C$197","Murs de fondation$C$197"]
["Foundation Walls","Range","$C$198",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$198","Murs de fondation$C$198"]
["Foundation Walls","Range","$C$199",54.89,31.5,46.44,"two_lines","Murs de fondation","Foundation Walls$C$199","Murs de fondation$C$199"]
["Foundation Walls","Range","$C$200",54.89,23.25,46.44,"one_line","Murs de fondation","Foundation Walls$C$200","Murs de fondation$C$200"]
["Structural Elements","Range","$M$3",27.89,60,27.89,77,"Éléments structuraux","Structural Elements$M$3","Éléments structuraux$M$3"]
["Structural Elements","Range","$C$7",54.89,23.25,46.44,"one_line","Éléments structuraux","Structural Elements$C$7","Éléments structuraux$C$7"]
["Structural Elements","Range","$C$8",54.89,31.5,46.44,"two_lines","Éléments structuraux","Structural Elements$C$8","Éléments structuraux$C$8"]
["Structural Elements","Range","$C$9",54.89,31.5,46.44,"two_lines","Éléments structuraux","Structural Elements$C$9","Éléments structuraux$C$9"]
["Structural Elements","Range","$C$10",54.89,31.5,46.44,"two_lines","Éléments structuraux","Structural Elements$C$10","Éléments structuraux$C$10"]
["Structural Elements","Range","$C$11",54.89,31.5,46.44,"two_lines","Éléments structuraux","Structural Elements$C$11","Éléments structuraux$C$11"]
["Structural Elements","Range","$C$12",54.89,31.5,46.44,"two_lines","Éléments structuraux","Structural Elements$C$12","Éléments structuraux$C$12"]
["Structural Elements","Range","$C$13",54.89,31.5,46.44,"two_lines","Éléments structuraux","Structural Elements$C$13","Éléments structuraux$C$13"]
["Ext. Walls","Range","$C$7",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$7","Murs ext.$C$7"]
["Ext. Walls","Range","$C$8",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$8","Murs ext.$C$8"]
["Ext. Walls","Range","$C$9",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$9","Murs ext.$C$9"]
["Ext. Walls","Range","$C$10",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$10","Murs ext.$C$10"]
["Ext. Walls","Range","$C$14",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$14","Murs ext.$C$14"]
["Ext. Walls","Range","$C$15",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$15","Murs ext.$C$15"]
["Ext. Walls","Range","$C$16",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$16","Murs ext.$C$16"]
["Ext. Walls","Range","$C$17",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$17","Murs ext.$C$17"]
["Ext. Walls","Range","$C$18",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$18","Murs ext.$C$18"]
["Ext. Walls","Range","$C$20",54.89,31.5,46.44,140,"Murs ext.","Ext. Walls$C$20","Murs ext.$C$20"]
["Ext. Walls","Range","$C$21",54.89,31.5,46.44,140,"Murs ext.","Ext. Walls$C$21","Murs ext.$C$21"]
["Ext. Walls","Range","$C$25",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$25","Murs ext.$C$25"]
["Ext. Walls","Range","$C$26",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$26","Murs ext.$C$26"]
["Ext. Walls","Range","$C$27",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$27","Murs ext.$C$27"]
["Ext. Walls","Range","$C$31",54.89,31.5,46.44,"three_lines","Murs ext.","Ext. Walls$C$31","Murs ext.$C$31"]
["Ext. Walls","Range","$C$33",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$33","Murs ext.$C$33"]
["Ext. Walls","Range","$C$32",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$32","Murs ext.$C$32"]
["Ext. Walls","Range","$C$34",54.89,31.5,46.44,"three_lines","Murs ext.","Ext. Walls$C$34","Murs ext.$C$34"]
["Ext. Walls","Range","$C$35",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$35","Murs ext.$C$35"]
["Ext. Walls","Range","$C$36",54.89,31.5,46.44,"three_lines","Murs ext.","Ext. Walls$C$36","Murs ext.$C$36"]
["Ext. Walls","Range","$C$37",54.89,31.5,46.44,60,"Murs ext.","Ext. Walls$C$37","Murs ext.$C$37"]
["Ext. Walls","Range","$C$39",54.89,"two_lines",46.44,"two_lines","Murs ext.","Ext. Walls$C$39","Murs ext.$C$39"]
["Ext. Walls","Range","$C$40",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$40","Murs ext.$C$40"]
["Ext. Walls","Range","$C$41",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$41","Murs ext.$C$41"]
["Ext. Walls","Range","$C$42",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$42","Murs ext.$C$42"]
["Ext. Walls","Range","$C$43",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$43","Murs ext.$C$43"]
["Ext. Walls","Range","$C$44",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$44","Murs ext.$C$44"]
["Ext. Walls","Range","$C$45",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$45","Murs ext.$C$45"]
["Ext. Walls","Range","$C$47",54.89,"two_lines",46.44,"two_lines","Murs ext.","Ext. Walls$C$47","Murs ext.$C$47"]
["Ext. Walls","Range","$C$48",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$48","Murs ext.$C$48"]
["Ext. Walls","Range","$C$49",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$49","Murs ext.$C$49"]
["Ext. Walls","Range","$C$50",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$50","Murs ext.$C$50"]
["Ext. Walls","Range","$C$51",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$51","Murs ext.$C$51"]
["Ext. Walls","Range","$C$52",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$52","Murs ext.$C$52"]
["Ext. Walls","Range","$C$53",54.89,"one_line",46.44,"two_lines","Murs ext.","Ext. Walls$C$53","Murs ext.$C$53"]
["Ext. Walls","Range","$C$56",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$56","Murs ext.$C$56"]
["Ext. Walls","Range","$C$57",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$57","Murs ext.$C$57"]
["Ext. Walls","Range","$C$58",54.89,31.5,46.44,"three_lines","Murs ext.","Ext. Walls$C$58","Murs ext.$C$58"]
["Ext. Walls","Range","$C$59",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$59","Murs ext.$C$59"]
["Ext. Walls","Range","$C$61",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$61","Murs ext.$C$61"]
["Ext. Walls","Range","$C$62",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$62","Murs ext.$C$62"]
["Ext. Walls","Range","$C$63",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$63","Murs ext.$C$63"]
["Ext. Walls","Range","$C$65",54.89,47.25,46.44,"three_lines","Murs ext.","Ext. Walls$C$65","Murs ext.$C$65"]
["Ext. Walls","Range","$C$66",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$66","Murs ext.$C$66"]
["Ext. Walls","Range","$C$67",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$67","Murs ext.$C$67"]
["Ext. Walls","Range","$C$69",54.89,23.25,46.44,"two_lines","Murs ext.",{"$f":"A325&C325","v":"Ext. Walls$C$69"},{"$f":"H325&C325","v":"Murs ext.$C$69"}]
["Ext. Walls","Range","$C$70",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$70","Murs ext.$C$70"]
["Ext. Walls","Range","$C$74",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$74","Murs ext.$C$74"]
["Ext. Walls","Range","$C$75",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$75","Murs ext.$C$75"]
["Ext. Walls","Range","$C$76",54.89,23.25,46.44,"one_line","Murs ext.","Ext. Walls$C$76","Murs ext.$C$76"]
["Ext. Walls","Range","$C$79",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$79","Murs ext.$C$79"]
["Ext. Walls","Range","$C$80",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$80","Murs ext.$C$80"]
["Ext. Walls","Range","$C$81",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$81","Murs ext.$C$81"]
["Ext. Walls","Range","$C$82",54.89,23.25,46.44,"three_lines","Murs ext.","Ext. Walls$C$82","Murs ext.$C$82"]
["Ext. Walls","Range","$C$84",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$84","Murs ext.$C$84"]
["Ext. Walls","Range","$C$85",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$85","Murs ext.$C$85"]
["Ext. Walls","Range","$C$86",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$86","Murs ext.$C$86"]
["Ext. Walls","Range","$C$87",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$87","Murs ext.$C$87"]
["Ext. Walls","Range","$C$88",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$88","Murs ext.$C$88"]
["Ext. Walls","Range","$C$89",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$89","Murs ext.$C$89"]
["Ext. Walls","Range","$C$90",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$90","Murs ext.$C$90"]
["Ext. Walls","Range","$C$93",54.89,47.25,46.44,"four_lines","Murs ext.","Ext. Walls$C$93","Murs ext.$C$93"]
["Ext. Walls","Range","$C$94",54.89,23.25,46.44,"one_line","Murs ext.","Ext. Walls$C$94","Murs ext.$C$94"]
["Ext. Walls","Range","$C$95",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$95","Murs ext.$C$95"]
["Ext. Walls","Range","$C$98",54.89,23.25,46.44,"one_line","Murs ext.","Ext. Walls$C$98","Murs ext.$C$98"]
["Ext. Walls","Range","$C$99",54.89,23.25,46.44,"one_line","Murs ext.","Ext. Walls$C$99","Murs ext.$C$99"]
["Ext. Walls","Range","$C$100",54.89,23.25,46.44,"one_line","Murs ext.","Ext. Walls$C$100","Murs ext.$C$100"]
["Ext. Walls","Range","$C$101",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$101","Murs ext.$C$101"]
["Ext. Walls","Range","$C$103",54.89,23.25,46.44,"one_line","Murs ext.","Ext. Walls$C$103","Murs ext.$C$103"]
["Ext. Walls","Range","$C$104",54.89,23.25,46.44,"one_line","Murs ext.","Ext. Walls$C$104","Murs ext.$C$104"]
["Ext. Walls","Range","$C$105",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$105","Murs ext.$C$105"]
["Ext. Walls","Range","$C$106",54.89,23.25,46.44,"one_line","Murs ext.","Ext. Walls$C$106","Murs ext.$C$106"]
["Ext. Walls","Range","$C$107",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$107","Murs ext.$C$107"]
["Ext. Walls","Range","$C$109",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$109","Murs ext.$C$109"]
["Ext. Walls","Range","$C$110",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$110","Murs ext.$C$110"]
["Ext. Walls","Range","$C$111",54.89,31.5,46.44,"three_lines","Murs ext.","Ext. Walls$C$111","Murs ext.$C$111"]
["Ext. Walls","Range","$C$113",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$113","Murs ext.$C$113"]
["Ext. Walls","Range","$C$114",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$114","Murs ext.$C$114"]
["Ext. Walls","Range","$C$117",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$117","Murs ext.$C$117"]
["Ext. Walls","Range","$C$118",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$118","Murs ext.$C$118"]
["Ext. Walls","Range","$C$119",54.89,23.25,46.44,"one_line","Murs ext.","Ext. Walls$C$119","Murs ext.$C$119"]
["Ext. Walls","Range","$C$123",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$123","Murs ext.$C$123"]
["Ext. Walls","Range","$C$124",54.89,31.5,46.44,"three_lines","Murs ext.","Ext. Walls$C$124","Murs ext.$C$124"]
["Ext. Walls","Range","$C$127",54.89,47.25,46.44,"three_lines","Murs ext.","Ext. Walls$C$127","Murs ext.$C$127"]
["Ext. Walls","Range","$C$128",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$128","Murs ext.$C$128"]
["Ext. Walls","Range","$C$129",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$129","Murs ext.$C$129"]
["Ext. Walls","Range","$C$130",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$130","Murs ext.$C$130"]
["Ext. Walls","Range","$C$131",54.89,31.5,46.44,"four_lines","Murs ext.","Ext. Walls$C$131","Murs ext.$C$131"]
["Ext. Walls","Range","$C$134",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$134","Murs ext.$C$134"]
["Ext. Walls","Range","$C$135",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$135","Murs ext.$C$135"]
["Ext. Walls","Range","$C$136",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$136","Murs ext.$C$136"]
["Ext. Walls","Range","$C$137",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$137","Murs ext.$C$137"]
["Ext. Walls","Range","$C$140",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$140","Murs ext.$C$140"]
["Ext. Walls","Range","$C$141",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$141","Murs ext.$C$141"]
["Ext. Walls","Range","$C$142",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$142","Murs ext.$C$142"]
["Ext. Walls","Range","$C$143",54.89,31.5,46.44,"three_lines","Murs ext.","Ext. Walls$C$143","Murs ext.$C$143"]
["Ext. Walls","Range","$C$146",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$146","Murs ext.$C$146"]
["Ext. Walls","Range","$C$147",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$147","Murs ext.$C$147"]
["Ext. Walls","Range","$C$148",54.89,23.25,46.44,"two_lines","Murs ext.","Ext. Walls$C$148","Murs ext.$C$148"]
["Ext. Walls","Range","$C$150",54.89,31.5,46.44,"two_lines","Murs ext.","Ext. Walls$C$150","Murs ext.$C$150"]
["Ext. Walls","Range","$C$151",54.89,30.75,46.44,"two_lines","Murs ext.","Ext. Walls$C$151","Murs ext.$C$151"]
["Ext. Wall Systems","Range","$C$6",54.89,59.25,54.89,"three_lines","Systèmes de murs ext.","Ext. Wall Systems$C$6","Systèmes de murs ext.$C$6"]
["Ext. Wall Systems","Range","$C$8",54.89,"two_lines",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$8","Systèmes de murs ext.$C$8"]
["Ext. Wall Systems","Range","$C$9",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$9","Systèmes de murs ext.$C$9"]
["Ext. Wall Systems","Range","$C$10",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$10","Systèmes de murs ext.$C$10"]
["Ext. Wall Systems","Range","$C$11",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$11","Systèmes de murs ext.$C$11"]
["Ext. Wall Systems","Range","$C$12",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$12","Systèmes de murs ext.$C$12"]
["Ext. Wall Systems","Range","$C$13",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$13","Systèmes de murs ext.$C$13"]
["Ext. Wall Systems","Range","$C$14",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$14","Systèmes de murs ext.$C$14"]
["Ext. Wall Systems","Range","$C$16",54.89,"two_lines",54.89,"two_lines","Systèmes de murs ext.",{"$f":"A389&C389","v":"Ext. Wall Systems$C$16"},{"$f":"H389&C389","v":"Systèmes de murs ext.$C$16"}]
["Ext. Wall Systems","Range","$C$17",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$17","Systèmes de murs ext.$C$17"]
["Ext. Wall Systems","Range","$C$18",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$18","Systèmes de murs ext.$C$18"]
["Ext. Wall Systems","Range","$C$19",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$19","Systèmes de murs ext.$C$19"]
["Ext. Wall Systems","Range","$C$20",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$20","Systèmes de murs ext.$C$20"]
["Ext. Wall Systems","Range","$C$21",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$21","Systèmes de murs ext.$C$21"]
["Ext. Wall Systems","Range","$C$22",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$22","Systèmes de murs ext.$C$22"]
["Ext. Wall Systems","Range","$C$24",54.89,"two_lines",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$24","Systèmes de murs ext.$C$24"]
["Ext. Wall Systems","Range","$C$25",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$25","Systèmes de murs ext.$C$25"]
["Ext. Wall Systems","Range","$C$26",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$26","Systèmes de murs ext.$C$26"]
["Ext. Wall Systems","Range","$C$27",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$27","Systèmes de murs ext.$C$27"]
["Ext. Wall Systems","Range","$C$28",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$28","Systèmes de murs ext.$C$28"]
["Ext. Wall Systems","Range","$C$29",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$29","Systèmes de murs ext.$C$29"]
["Ext. Wall Systems","Range","$C$30",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$30","Systèmes de murs ext.$C$30"]
["Ext. Wall Systems","Range","$C$32",54.89,31.5,54.89,"three_lines","Systèmes de murs ext.","Ext. Wall Systems$C$32","Systèmes de murs ext.$C$32"]
["Ext. Wall Systems","Range","$C$33",54.89,31.5,54.89,"three_lines","Systèmes de murs ext.","Ext. Wall Systems$C$33","Systèmes de murs ext.$C$33"]
["Ext. Wall Systems","Range","$C$34",54.89,31.5,54.89,"three_lines","Systèmes de murs ext.","Ext. Wall Systems$C$34","Systèmes de murs ext.$C$34"]
["Ext. Wall Systems","Range","$C$35",54.89,32.25,54.89,"three_lines","Systèmes de murs ext.","Ext. Wall Systems$C$35","Systèmes de murs ext.$C$35"]
["Ext. Wall Systems","Range","$C$37",54.89,"two_lines",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$37","Systèmes de murs ext.$C$37"]
["Ext. Wall Systems","Range","$C$38",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$38","Systèmes de murs ext.$C$38"]
["Ext. Wall Systems","Range","$C$39",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$39","Systèmes de murs ext.$C$39"]
["Ext. Wall Systems","Range","$C$40",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$40","Systèmes de murs ext.$C$40"]
["Ext. Wall Systems","Range","$C$41",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$41","Systèmes de murs ext.$C$41"]
["Ext. Wall Systems","Range","$C$42",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$42","Systèmes de murs ext.$C$42"]
["Ext. Wall Systems","Range","$C$43",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$43","Systèmes de murs ext.$C$43"]
["Ext. Wall Systems","Range","$C$45",54.89,"two_lines",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$45","Systèmes de murs ext.$C$45"]
["Ext. Wall Systems","Range","$C$46",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$46","Systèmes de murs ext.$C$46"]
["Ext. Wall Systems","Range","$C$47",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$47","Systèmes de murs ext.$C$47"]
["Ext. Wall Systems","Range","$C$48",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$48","Systèmes de murs ext.$C$48"]
["Ext. Wall Systems","Range","$C$49",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$49","Systèmes de murs ext.$C$49"]
["Ext. Wall Systems","Range","$C$50",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$50","Systèmes de murs ext.$C$50"]
["Ext. Wall Systems","Range","$C$51",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$51","Systèmes de murs ext.$C$51"]
["Ext. Wall Systems","Range","$C$53",54.89,"two_lines",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$53","Systèmes de murs ext.$C$53"]
["Ext. Wall Systems","Range","$C$54",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$54","Systèmes de murs ext.$C$54"]
["Ext. Wall Systems","Range","$C$55",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$55","Systèmes de murs ext.$C$55"]
["Ext. Wall Systems","Range","$C$56",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$56","Systèmes de murs ext.$C$56"]
["Ext. Wall Systems","Range","$C$57",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$57","Systèmes de murs ext.$C$57"]
["Ext. Wall Systems","Range","$C$58",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$58","Systèmes de murs ext.$C$58"]
["Ext. Wall Systems","Range","$C$59",54.89,"one_line",54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$59","Systèmes de murs ext.$C$59"]
["Ext. Wall Systems","Range","$C$62",54.89,31.5,54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$62","Systèmes de murs ext.$C$62"]
["Ext. Wall Systems","Range","$C$63",54.89,31.5,54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$63","Systèmes de murs ext.$C$63"]
["Ext. Wall Systems","Range","$C$65",54.89,31.5,54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$65","Systèmes de murs ext.$C$65"]
["Ext. Wall Systems","Range","$C$66",54.89,31.5,54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$66","Systèmes de murs ext.$C$66"]
["Ext. Wall Systems","Range","$C$67",54.89,31.5,54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$67","Systèmes de murs ext.$C$67"]
["Ext. Wall Systems","Range","$C$68",54.89,31.5,54.89,"two_lines","Systèmes de murs ext.","Ext. Wall Systems$C$68","Systèmes de murs ext.$C$68"]
["Party Walls","Range","$C$9",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$9","Murs mitoyens$C$9"]
["Party Walls","Range","$C$10",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$10","Murs mitoyens$C$10"]
["Party Walls","Range","$C$11",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$11","Murs mitoyens$C$11"]
["Party Walls","Range","$C$12",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$12","Murs mitoyens$C$12"]
["Party Walls","Range","$C$16",54.89,31.5,46.44,"three_lines","Murs mitoyens","Party Walls$C$16","Murs mitoyens$C$16"]
["Party Walls","Range","$C$17",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$17","Murs mitoyens$C$17"]
["Party Walls","Range","$C$18",54.89,31.5,46.44,"three_lines","Murs mitoyens","Party Walls$C$18","Murs mitoyens$C$18"]
["Party Walls","Range","$C$19",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$19","Murs mitoyens$C$19"]
["Party Walls","Range","$C$20",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$20","Murs mitoyens$C$20"]
["Party Walls","Range","$C$23",54.89,31.75,46.44,"two_lines","Murs mitoyens","Party Walls$C$23","Murs mitoyens$C$23"]
["Party Walls","Range","$C$24",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$24","Murs mitoyens$C$24"]
["Party Walls","Range","$C$25",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$25","Murs mitoyens$C$25"]
["Party Walls","Range","$C$26",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$26","Murs mitoyens$C$26"]
["Party Walls","Range","$C$27",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$27","Murs mitoyens$C$27"]
["Party Walls","Range","$C$32",54.89,31.5,46.44,"three_lines","Murs mitoyens","Party Walls$C$32","Murs mitoyens$C$32"]
["Party Walls","Range","$C$33",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$33","Murs mitoyens$C$33"]
["Party Walls","Range","$C$34",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$34","Murs mitoyens$C$34"]
["Party Walls","Range","$C$35",54.89,31.5,46.44,"three_lines","Murs mitoyens","Party Walls$C$35","Murs mitoyens$C$35"]
["Party Walls","Range","$C$36",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$36","Murs mitoyens$C$36"]
["Party Walls","Range","$C$37",54.89,31.5,46.44,"three_lines","Murs mitoyens",{"$f":"A453&C453","v":"Party Walls$C$37"},{"$f":"H453&C453","v":"Murs mitoyens$C$37"}]
["Party Walls","Range","$C$40",54.89,"two_lines",46.44,"two_lines","Murs mitoyens","Party Walls$C$40","Murs mitoyens$C$40"]
["Party Walls","Range","$C$41",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$41","Murs mitoyens$C$41"]
["Party Walls","Range","$C$42",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$42","Murs mitoyens$C$42"]
["Party Walls","Range","$C$43",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$43","Murs mitoyens$C$43"]
["Party Walls","Range","$C$44",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$44","Murs mitoyens$C$44"]
["Party Walls","Range","$C$45",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$45","Murs mitoyens$C$45"]
["Party Walls","Range","$C$46",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$46","Murs mitoyens$C$46"]
["Party Walls","Range","$C$48",54.89,"two_lines",46.44,"two_lines","Murs mitoyens","Party Walls$C$48","Murs mitoyens$C$48"]
["Party Walls","Range","$C$49",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$49","Murs mitoyens$C$49"]
["Party Walls","Range","$C$50",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$50","Murs mitoyens$C$50"]
["Party Walls","Range","$C$51",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$51","Murs mitoyens$C$51"]
["Party Walls","Range","$C$52",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$52","Murs mitoyens$C$52"]
["Party Walls","Range","$C$53",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$53","Murs mitoyens$C$53"]
["Party Walls","Range","$C$54",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$54","Murs mitoyens$C$54"]
["Party Walls","Range","$C$59",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$59","Murs mitoyens$C$59"]
["Party Walls","Range","$C$60",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$60","Murs mitoyens$C$60"]
["Party Walls","Range","$C$61",54.89,23.25,46.44,"one_line","Murs mitoyens","Party Walls$C$61","Murs mitoyens$C$61"]
["Party Walls","Range","$C$64",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$64","Murs mitoyens$C$64"]
["Party Walls","Range","$C$65",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$65","Murs mitoyens$C$65"]
["Party Walls","Range","$C$66",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$66","Murs mitoyens$C$66"]
["Party Walls","Range","$C$67",54.89,23.25,46.44,"three_lines","Murs mitoyens","Party Walls$C$67","Murs mitoyens$C$67"]
["Party Walls","Range","$C$69",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$69","Murs mitoyens$C$69"]
["Party Walls","Range","$C$70",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$70","Murs mitoyens$C$70"]
["Party Walls","Range","$C$71",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$71","Murs mitoyens$C$71"]
["Party Walls","Range","$C$72",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$72","Murs mitoyens$C$72"]
["Party Walls","Range","$C$73",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$73","Murs mitoyens$C$73"]
["Party Walls","Range","$C$74",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$74","Murs mitoyens$C$74"]
["Party Walls","Range","$C$75",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$75","Murs mitoyens$C$75"]
["Party Walls","Range","$C$78",54.89,47.25,46.44,"four_lines","Murs mitoyens","Party Walls$C$78","Murs mitoyens$C$78"]
["Party Walls","Range","$C$79",54.89,23.25,46.44,"one_line","Murs mitoyens","Party Walls$C$79","Murs mitoyens$C$79"]
["Party Walls","Range","$C$80",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$80","Murs mitoyens$C$80"]
["Party Walls","Range","$C$83",54.89,23.25,46.44,"one_line","Murs mitoyens","Party Walls$C$83","Murs mitoyens$C$83"]
["Party Walls","Range","$C$84",54.89,23.25,46.44,"one_line","Murs mitoyens","Party Walls$C$84","Murs mitoyens$C$84"]
["Party Walls","Range","$C$85",54.89,23.25,46.44,"one_line","Murs mitoyens","Party Walls$C$85","Murs mitoyens$C$85"]
["Party Walls","Range","$C$86",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$86","Murs mitoyens$C$86"]
["Party Walls","Range","$C$88",54.89,23.25,46.44,"one_line","Murs mitoyens","Party Walls$C$88","Murs mitoyens$C$88"]
["Party Walls","Range","$C$89",54.89,23.25,46.44,"one_line","Murs mitoyens","Party Walls$C$89","Murs mitoyens$C$89"]
["Party Walls","Range","$C$90",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$90","Murs mitoyens$C$90"]
["Party Walls","Range","$C$91",54.89,23.25,46.44,"one_line","Murs mitoyens","Party Walls$C$91","Murs mitoyens$C$91"]
["Party Walls","Range","$C$92",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$92","Murs mitoyens$C$92"]
["Party Walls","Range","$C$94",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$94","Murs mitoyens$C$94"]
["Party Walls","Range","$C$95",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$95","Murs mitoyens$C$95"]
["Party Walls","Range","$C$96",54.89,31.5,46.44,"three_lines","Murs mitoyens","Party Walls$C$96","Murs mitoyens$C$96"]
["Party Walls","Range","$C$98",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$98","Murs mitoyens$C$98"]
["Party Walls","Range","$C$99",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$99","Murs mitoyens$C$99"]
["Party Walls","Range","$C$102",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$102","Murs mitoyens$C$102"]
["Party Walls","Range","$C$103",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$103","Murs mitoyens$C$103"]
["Party Walls","Range","$C$104",54.89,23.25,46.44,"one_line","Murs mitoyens","Party Walls$C$104","Murs mitoyens$C$104"]
["Party Walls","Range","$C$108",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$108","Murs mitoyens$C$108"]
["Party Walls","Range","$C$109",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$109","Murs mitoyens$C$109"]
["Party Walls","Range","$C$112",54.89,47.25,46.44,"three_lines","Murs mitoyens","Party Walls$C$112","Murs mitoyens$C$112"]
["Party Walls","Range","$C$113",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$113","Murs mitoyens$C$113"]
["Party Walls","Range","$C$114",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$114","Murs mitoyens$C$114"]
["Party Walls","Range","$C$115",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$115","Murs mitoyens$C$115"]
["Party Walls","Range","$C$116",54.89,31.5,46.44,"four_lines","Murs mitoyens","Party Walls$C$116","Murs mitoyens$C$116"]
["Party Walls","Range","$C$118",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$118","Murs mitoyens$C$118"]
["Party Walls","Range","$C$119",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$119","Murs mitoyens$C$119"]
["Party Walls","Range","$C$120",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$120","Murs mitoyens$C$120"]
["Party Walls","Range","$C$121",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$121","Murs mitoyens$C$121"]
["Party Walls","Range","$C$122",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$122","Murs mitoyens$C$122"]
["Party Walls","Range","$C$125",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$125","Murs mitoyens$C$125"]
["Party Walls","Range","$C$126",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$126","Murs mitoyens$C$126"]
["Party Walls","Range","$C$127",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$127","Murs mitoyens$C$127"]
["Party Walls","Range","$C$128",54.89,31.5,46.44,"three_lines","Murs mitoyens",{"$f":"A517&C517","v":"Party Walls$C$128"},{"$f":"H517&C517","v":"Murs mitoyens$C$128"}]
["Party Walls","Range","$C$131",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$131","Murs mitoyens$C$131"]
["Party Walls","Range","$C$132",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$132","Murs mitoyens$C$132"]
["Party Walls","Range","$C$133",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$133","Murs mitoyens$C$133"]
["Party Walls","Range","$C$135",54.89,23.25,46.44,60,"Murs mitoyens","Party Walls$C$135","Murs mitoyens$C$135"]
["Party Walls","Range","$C$137",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$137","Murs mitoyens$C$137"]
["Party Walls","Range","$C$138",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$138","Murs mitoyens$C$138"]
["Party Walls","Range","$C$139",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$139","Murs mitoyens$C$139"]
["Party Walls","Range","$C$140",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$140","Murs mitoyens$C$140"]
["Party Walls","Range","$C$141",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$141","Murs mitoyens$C$141"]
["Party Walls","Range","$C$142",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$142","Murs mitoyens$C$142"]
["Party Walls","Range","$C$144",54.89,47.25,46.44,"three_lines","Murs mitoyens","Party Walls$C$144","Murs mitoyens$C$144"]
["Party Walls","Range","$C$145",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$145","Murs mitoyens$C$145"]
["Party Walls","Range","$C$146",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$146","Murs mitoyens$C$146"]
["Party Walls","Range","$C$148",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$148","Murs mitoyens$C$148"]
["Party Walls","Range","$C$149",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$149","Murs mitoyens$C$149"]
["Party Walls","Range","$C$150",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$150","Murs mitoyens$C$150"]
["Party Walls","Range","$C$151",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$151","Murs mitoyens$C$151"]
["Party Walls","Range","$C$152",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$152","Murs mitoyens$C$152"]
["Party Walls","Range","$C$153",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$153","Murs mitoyens$C$153"]
["Party Walls","Range","$C$154",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$154","Murs mitoyens$C$154"]
["Party Walls","Range","$C$155",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$155","Murs mitoyens$C$155"]
["Party Walls","Range","$C$156",54.89,23.25,46.44,"one_line","Murs mitoyens","Party Walls$C$156","Murs mitoyens$C$156"]
["Party Walls","Range","$C$157",54.89,31.5,46.44,"four_lines","Murs mitoyens","Party Walls$C$157","Murs mitoyens$C$157"]
["Party Walls","Range","$C$160",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$160","Murs mitoyens$C$160"]
["Party Walls","Range","$C$161",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$161","Murs mitoyens$C$161"]
["Party Walls","Range","$C$162",54.89,31.5,46.44,"three_lines","Murs mitoyens","Party Walls$C$162","Murs mitoyens$C$162"]
["Party Walls","Range","$C$163",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$163","Murs mitoyens$C$163"]
["Party Walls","Range","$C$165",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$165","Murs mitoyens$C$165"]
["Party Walls","Range","$C$166",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$166","Murs mitoyens$C$166"]
["Party Walls","Range","$C$167",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$167","Murs mitoyens$C$167"]
["Party Walls","Range","$C$169",54.89,47.25,46.44,"three_lines","Murs mitoyens","Party Walls$C$169","Murs mitoyens$C$169"]
["Party Walls","Range","$C$170",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$170","Murs mitoyens$C$170"]
["Party Walls","Range","$C$171",54.89,23.25,46.44,"two_lines","Murs mitoyens","Party Walls$C$171","Murs mitoyens$C$171"]
["Party Walls","Range","$C$173",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$173","Murs mitoyens$C$173"]
["Party Walls","Range","$C$174",54.89,31.5,46.44,"two_lines","Murs mitoyens","Party Walls$C$174","Murs mitoyens$C$174"]
["Party Walls","Range","$C$176",54.89,31.5,46.44,60,"Murs mitoyens","Party Walls$C$176","Murs mitoyens$C$176"]
["Party Walls","Range","$C$177",54.89,32.25,46.44,"three_lines","Murs mitoyens","Party Walls$C$177","Murs mitoyens$C$177"]
["Party Walls","Range","$C$179",54.89,"two_lines",46.44,"two_lines","Murs mitoyens","Party Walls$C$179","Murs mitoyens$C$179"]
["Party Walls","Range","$C$180",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$180","Murs mitoyens$C$180"]
["Party Walls","Range","$C$181",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$181","Murs mitoyens$C$181"]
["Party Walls","Range","$C$182",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$182","Murs mitoyens$C$182"]
["Party Walls","Range","$C$183",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$183","Murs mitoyens$C$183"]
["Party Walls","Range","$C$184",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$184","Murs mitoyens$C$184"]
["Party Walls","Range","$C$185",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$185","Murs mitoyens$C$185"]
["Party Walls","Range","$C$187",54.89,"two_lines",46.44,"two_lines","Murs mitoyens","Party Walls$C$187","Murs mitoyens$C$187"]
["Party Walls","Range","$C$188",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$188","Murs mitoyens$C$188"]
["Party Walls","Range","$C$189",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$189","Murs mitoyens$C$189"]
["Party Walls","Range","$C$190",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$190","Murs mitoyens$C$190"]
["Party Walls","Range","$C$191",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$191","Murs mitoyens$C$191"]
["Party Walls","Range","$C$192",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$192","Murs mitoyens$C$192"]
["Party Walls","Range","$C$193",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$193","Murs mitoyens$C$193"]
["Party Walls","Range","$C$195",54.89,"two_lines",46.44,"two_lines","Murs mitoyens","Party Walls$C$195","Murs mitoyens$C$195"]
["Party Walls","Range","$C$196",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$196","Murs mitoyens$C$196"]
["Party Walls","Range","$C$197",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$197","Murs mitoyens$C$197"]
["Party Walls","Range","$C$198",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$198","Murs mitoyens$C$198"]
["Party Walls","Range","$C$199",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$199","Murs mitoyens$C$199"]
["Party Walls","Range","$C$200",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$200","Murs mitoyens$C$200"]
["Party Walls","Range","$C$201",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$201","Murs mitoyens$C$201"]
["Party Walls","Range","$C$203",54.89,31.5,46.44,"three_lines","Murs mitoyens","Party Walls$C$203","Murs mitoyens$C$203"]
["Party Walls","Range","$C$204",54.89,31.5,46.44,"three_lines","Murs mitoyens","Party Walls$C$204","Murs mitoyens$C$204"]
["Party Walls","Range","$C$205",54.89,31.5,46.44,"three_lines","Murs mitoyens","Party Walls$C$205","Murs mitoyens$C$205"]
["Party Walls","Range","$C$206",54.89,32.25,46.44,"three_lines","Murs mitoyens","Party Walls$C$206","Murs mitoyens$C$206"]
["Party Walls","Range","$C$208",54.89,"two_lines",46.44,"two_lines","Murs mitoyens","Party Walls$C$208","Murs mitoyens$C$208"]
["Party Walls","Range","$C$209",54.89,"one_line",46.44,"two_lines","Murs mitoyens",{"$f":"A581&C581","v":"Party Walls$C$209"},{"$f":"H581&C581","v":"Murs mitoyens$C$209"}]
["Party Walls","Range","$C$210",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$210","Murs mitoyens$C$210"]
["Party Walls","Range","$C$211",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$211","Murs mitoyens$C$211"]
["Party Walls","Range","$C$212",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$212","Murs mitoyens$C$212"]
["Party Walls","Range","$C$213",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$213","Murs mitoyens$C$213"]
["Party Walls","Range","$C$214",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$214","Murs mitoyens$C$214"]
["Party Walls","Range","$C$216",54.89,"two_lines",46.44,"two_lines","Murs mitoyens","Party Walls$C$216","Murs mitoyens$C$216"]
["Party Walls","Range","$C$217",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$217","Murs mitoyens$C$217"]
["Party Walls","Range","$C$218",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$218","Murs mitoyens$C$218"]
["Party Walls","Range","$C$219",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$219","Murs mitoyens$C$219"]
["Party Walls","Range","$C$220",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$220","Murs mitoyens$C$220"]
["Party Walls","Range","$C$221",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$221","Murs mitoyens$C$221"]
["Party Walls","Range","$C$222",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$222","Murs mitoyens$C$222"]
["Party Walls","Range","$C$224",54.89,"two_lines",46.44,"two_lines","Murs mitoyens","Party Walls$C$224","Murs mitoyens$C$224"]
["Party Walls","Range","$C$225",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$225","Murs mitoyens$C$225"]
["Party Walls","Range","$C$226",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$226","Murs mitoyens$C$226"]
["Party Walls","Range","$C$227",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$227","Murs mitoyens$C$227"]
["Party Walls","Range","$C$228",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$228","Murs mitoyens$C$228"]
["Party Walls","Range","$C$229",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$229","Murs mitoyens$C$229"]
["Party Walls","Range","$C$230",54.89,"one_line",46.44,"two_lines","Murs mitoyens","Party Walls$C$230","Murs mitoyens$C$230"]
["Cladding","Range","$C$7",54.89,47.25,54.89,"three_lines","Bardage","Cladding$C$7","Bardage$C$7"]
["Cladding","Range","$C$8",54.89,31.5,54.89,"three_lines","Bardage","Cladding$C$8","Bardage$C$8"]
["Cladding","Range","$C$9",54.89,31.5,54.89,"four_lines","Bardage","Cladding$C$9","Bardage$C$9"]
["Cladding","Range","$C$10",54.89,31.5,54.89,"four_lines","Bardage","Cladding$C$10","Bardage$C$10"]
["Cladding","Range","$C$11",54.89,31.5,54.89,"three_lines","Bardage","Cladding$C$11","Bardage$C$11"]
["Cladding","Range","$C$12",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$12","Bardage$C$12"]
["Cladding","Range","$C$13",54.89,31.5,54.89,"four_lines","Bardage","Cladding$C$13","Bardage$C$13"]
["Cladding","Range","$C$15",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$15","Bardage$C$15"]
["Cladding","Range","$C$16",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$16","Bardage$C$16"]
["Cladding","Range","$C$19",54.89,23.25,54.89,"one_line","Bardage","Cladding$C$19","Bardage$C$19"]
["Cladding","Range","$C$20",54.89,23.25,54.89,"one_line","Bardage","Cladding$C$20","Bardage$C$20"]
["Cladding","Range","$C$21",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$21","Bardage$C$21"]
["Cladding","Range","$C$22",54.89,23.25,54.89,"one_line","Bardage","Cladding$C$22","Bardage$C$22"]
["Cladding","Range","$C$23",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$23","Bardage$C$23"]
["Cladding","Range","$C$24",54.89,23.25,54.89,"one_line","Bardage","Cladding$C$24","Bardage$C$24"]
["Cladding","Range","$C$25",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$25","Bardage$C$25"]
["Cladding","Range","$C$26",54.89,23.25,54.89,"one_line","Bardage","Cladding$C$26","Bardage$C$26"]
["Cladding","Range","$C$28",54.89,23.25,54.89,"three_lines","Bardage","Cladding$C$28","Bardage$C$28"]
["Cladding","Range","$C$31",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$31","Bardage$C$31"]
["Cladding","Range","$C$32",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$32","Bardage$C$32"]
["Cladding","Range","$C$35",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$35","Bardage$C$35"]
["Cladding","Range","$C$36",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$36","Bardage$C$36"]
["Cladding","Range","$C$37",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$37","Bardage$C$37"]
["Cladding","Range","$C$38",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$38","Bardage$C$38"]
["Cladding","Range","$C$39",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$39","Bardage$C$39"]
["Cladding","Range","$C$40",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$40","Bardage$C$40"]
["Cladding","Range","$C$43",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$43","Bardage$C$43"]
["Cladding","Range","$C$44",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$44","Bardage$C$44"]
["Cladding","Range","$C$46",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$46","Bardage$C$46"]
["Cladding","Range","$C$47",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$47","Bardage$C$47"]
["Cladding","Range","$C$48",54.89,23.25,54.89,"one_line","Bardage","Cladding$C$48","Bardage$C$48"]
["Cladding","Range","$C$49",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$49","Bardage$C$49"]
["Cladding","Range","$C$51",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$51","Bardage$C$51"]
["Cladding","Range","$C$52",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$52","Bardage$C$52"]
["Cladding","Range","$C$53",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$53","Bardage$C$53"]
["Cladding","Range","$C$55",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$55","Bardage$C$55"]
["Cladding","Range","$C$56",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$56","Bardage$C$56"]
["Cladding","Range","$C$59",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$59","Bardage$C$59"]
["Cladding","Range","$C$60",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$60","Bardage$C$60"]
["Cladding","Range","$C$61",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$61","Bardage$C$61"]
["Cladding","Range","$C$62",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$62","Bardage$C$62"]
["Cladding","Range","$C$63",54.89,23.25,54.89,"one_line","Bardage","Cladding$C$63","Bardage$C$63"]
["Cladding","Range","$C$64",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$64","Bardage$C$64"]
["Cladding","Range","$C$66",54.89,47.25,54.89,"three_lines","Bardage","Cladding$C$66","Bardage$C$66"]
["Cladding","Range","$C$67",54.89,23.25,54.89,"one_line","Bardage",{"$f":"A645&C645","v":"Cladding$C$67"},{"$f":"H645&C645","v":"Bardage$C$67"}]
["Cladding","Range","$C$68",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$68","Bardage$C$68"]
["Cladding","Range","$C$70",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$70","Bardage$C$70"]
["Cladding","Range","$C$71",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$71","Bardage$C$71"]
["Cladding","Range","$C$72",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$72","Bardage$C$72"]
["Cladding","Range","$C$73",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$73","Bardage$C$73"]
["Cladding","Range","$C$74",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$74","Bardage$C$74"]
["Cladding","Range","$C$75",54.89,23.25,54.89,"two_lines","Bardage","Cladding$C$75","Bardage$C$75"]
["Cladding","Range","$C$76",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$76","Bardage$C$76"]
["Cladding","Range","$C$77",54.89,31.5,54.89,"two_lines","Bardage","Cladding$C$77","Bardage$C$77"]
["Cladding","Range","$C$78",54.89,23.25,54.89,"one_line","Bardage","Cladding$C$78","Bardage$C$78"]
["Cladding","Range","$C$79",54.89,31.5,54.89,"three_lines","Bardage","Cladding$C$79","Bardage$C$79"]
["Windows","Range","$C$6",54.89,23.25,54.89,"two_lines","Fenêtres","Windows$C$6","Fenêtres$C$6"]
["Windows","Range","$C$7",54.89,23.25,54.89,"two_lines","Fenêtres","Windows$C$7","Fenêtres$C$7"]
["Windows","Range","$C$8",54.89,23.25,54.89,"one_line","Fenêtres","Windows$C$8","Fenêtres$C$8"]
["Windows","Range","$C$9",54.89,23.25,54.89,"two_lines","Fenêtres","Windows$C$9","Fenêtres$C$9"]
["Windows","Range","$C$10",54.89,23.25,54.89,"two_lines","Fenêtres","Windows$C$10","Fenêtres$C$10"]
["Windows","Range","$C$11",54.89,31.5,54.89,"two_lines","Fenêtres","Windows$C$11","Fenêtres$C$11"]
["Windows","Range","$C$13",54.89,23.25,54.89,"two_lines","Fenêtres","Windows$C$13","Fenêtres$C$13"]
["Windows","Range","$C$14",54.89,23.25,54.89,"two_lines","Fenêtres","Windows$C$14","Fenêtres$C$14"]
["Windows","Range","$C$15",54.89,23.25,54.89,"one_line","Fenêtres","Windows$C$15","Fenêtres$C$15"]
["Windows","Range","$C$16",54.89,23.25,54.89,"two_lines","Fenêtres","Windows$C$16","Fenêtres$C$16"]
["Windows","Range","$C$17",54.89,23.25,54.89,"two_lines","Fenêtres","Windows$C$17","Fenêtres$C$17"]
["Windows","Range","$C$18",54.89,31.5,54.89,"two_lines","Fenêtres","Windows$C$18","Fenêtres$C$18"]
["Windows","Range","$C$20",54.89,31.5,54.89,"three_lines","Fenêtres","Windows$C$20","Fenêtres$C$20"]
["Windows","Range","$C$21",54.89,31.5,54.89,"three_lines","Fenêtres","Windows$C$21","Fenêtres$C$21"]
["Windows","Range","$C$22",54.89,31.5,54.89,"two_lines","Fenêtres","Windows$C$22","Fenêtres$C$22"]
["Int. Walls","Range","$C$7",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$7","Murs int.$C$7"]
["Int. Walls","Range","$C$8",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$8","Murs int.$C$8"]
["Int. Walls","Range","$C$9",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$9","Murs int.$C$9"]
["Int. Walls","Range","$C$13",54.89,31.5,46.44,"three_lines","Murs int.","Int. Walls$C$13","Murs int.$C$13"]
["Int. Walls","Range","$C$14",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$14","Murs int.$C$14"]
["Int. Walls","Range","$C$15",54.89,31.5,46.44,"three_lines","Murs int.","Int. Walls$C$15","Murs int.$C$15"]
["Int. Walls","Range","$C$16",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$16","Murs int.$C$16"]
["Int. Walls","Range","$C$17",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$17","Murs int.$C$17"]
["Int. Walls","Range","$C$20",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$20","Murs int.$C$20"]
["Int. Walls","Range","$C$21",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$21","Murs int.$C$21"]
["Int. Walls","Range","$C$22",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$22","Murs int.$C$22"]
["Int. Walls","Range","$C$23",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$23","Murs int.$C$23"]
["Int. Walls","Range","$C$24",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$24","Murs int.$C$24"]
["Int. Walls","Range","$C$25",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$25","Murs int.$C$25"]
["Int. Walls","Range","$C$27",54.89,47.25,46.44,"three_lines","Murs int.","Int. Walls$C$27","Murs int.$C$27"]
["Int. Walls","Range","$C$28",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$28","Murs int.$C$28"]
["Int. Walls","Range","$C$29",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$29","Murs int.$C$29"]
["Int. Walls","Range","$C$31",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$31","Murs int.$C$31"]
["Int. Walls","Range","$C$32",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$32","Murs int.$C$32"]
["Int. Walls","Range","$C$33",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$33","Murs int.$C$33"]
["Int. Walls","Range","$C$34",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$34","Murs int.$C$34"]
["Int. Walls","Range","$C$35",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$35","Murs int.$C$35"]
["Int. Walls","Range","$C$36",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$36","Murs int.$C$36"]
["Int. Walls","Range","$C$37",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$37","Murs int.$C$37"]
["Int. Walls","Range","$C$38",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$38","Murs int.$C$38"]
["Int. Walls","Range","$C$39",54.89,23.25,46.44,"one_line","Murs int.","Int. Walls$C$39","Murs int.$C$39"]
["Int. Walls","Range","$C$40",54.89,31.5,46.44,"four_lines","Murs int.","Int. Walls$C$40","Murs int.$C$40"]
["Int. Walls","Range","$C$44",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$44","Murs int.$C$44"]
["Int. Walls","Range","$C$45",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$45","Murs int.$C$45"]
["Int. Walls","Range","$C$46",54.89,23.25,46.44,"one_line","Murs int.","Int. Walls$C$46","Murs int.$C$46"]
["Int. Walls","Range","$C$49",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$49","Murs int.$C$49"]
["Int. Walls","Range","$C$50",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$50","Murs int.$C$50"]
["Int. Walls","Range","$C$51",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$51","Murs int.$C$51"]
["Int. Walls","Range","$C$52",54.89,23.25,46.44,"three_lines","Murs int.","Int. Walls$C$52","Murs int.$C$52"]
["Int. Walls","Range","$C$54",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$54","Murs int.$C$54"]
["Int. Walls","Range","$C$55",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$55","Murs int.$C$55"]
["Int. Walls","Range","$C$56",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$56","Murs int.$C$56"]
["Int. Walls","Range","$C$57",54.89,31.5,46.44,"two_lines","Murs int.",{"$f":"A709&C709","v":"Int. Walls$C$57"},{"$f":"H709&C709","v":"Murs int.$C$57"}]
["Int. Walls","Range","$C$58",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$58","Murs int.$C$58"]
["Int. Walls","Range","$C$59",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$59","Murs int.$C$59"]
["Int. Walls","Range","$C$60",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$60","Murs int.$C$60"]
["Int. Walls","Range","$C$63",54.89,47.25,46.44,"four_lines","Murs int.","Int. Walls$C$63","Murs int.$C$63"]
["Int. Walls","Range","$C$64",54.89,23.25,46.44,"one_line","Murs int.","Int. Walls$C$64","Murs int.$C$64"]
["Int. Walls","Range","$C$65",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$65","Murs int.$C$65"]
["Int. Walls","Range","$C$68",54.89,23.25,46.44,"one_line","Murs int.","Int. Walls$C$68","Murs int.$C$68"]
["Int. Walls","Range","$C$69",54.89,23.25,46.44,"one_line","Murs int.","Int. Walls$C$69","Murs int.$C$69"]
["Int. Walls","Range","$C$70",54.89,23.25,46.44,"one_line","Murs int.","Int. Walls$C$70","Murs int.$C$70"]
["Int. Walls","Range","$C$71",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$71","Murs int.$C$71"]
["Int. Walls","Range","$C$73",54.89,23.25,46.44,"one_line","Murs int.","Int. Walls$C$73","Murs int.$C$73"]
["Int. Walls","Range","$C$74",54.89,23.25,46.44,"one_line","Murs int.","Int. Walls$C$74","Murs int.$C$74"]
["Int. Walls","Range","$C$75",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$75","Murs int.$C$75"]
["Int. Walls","Range","$C$76",54.89,23.25,46.44,"one_line","Murs int.","Int. Walls$C$76","Murs int.$C$76"]
["Int. Walls","Range","$C$77",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$77","Murs int.$C$77"]
["Int. Walls","Range","$C$79",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$79","Murs int.$C$79"]
["Int. Walls","Range","$C$80",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$80","Murs int.$C$80"]
["Int. Walls","Range","$C$81",54.89,31.5,46.44,"three_lines","Murs int.","Int. Walls$C$81","Murs int.$C$81"]
["Int. Walls","Range","$C$83",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$83","Murs int.$C$83"]
["Int. Walls","Range","$C$84",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$84","Murs int.$C$84"]
["Int. Walls","Range","$C$87",54.89,31.5,46.44,"two_lines","Murs int.","Int. Walls$C$87","Murs int.$C$87"]
["Int. Walls","Range","$C$88",54.89,23.25,46.44,"two_lines","Murs int.","Int. Walls$C$88","Murs int.$C$88"]
["Int. Walls","Range","$C$89",54.89,23.25,46.44,"one_line","Murs int.","Int. Walls$C$89","Murs int.$C$89"]
["Floors","Range","$C$7",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$7","Planchers$C$7"]
["Floors","Range","$C$8",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$8","Planchers$C$8"]
["Floors","Range","$C$9",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$9","Planchers$C$9"]
["Floors","Range","$C$11",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$11","Planchers$C$11"]
["Floors","Range","$C$12",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$12","Planchers$C$12"]
["Floors","Range","$C$13",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$13","Planchers$C$13"]
["Floors","Range","$C$15",54.89,47.25,46.44,"four_lines","Planchers","Floors$C$15","Planchers$C$15"]
["Floors","Range","$C$18",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$18","Planchers$C$18"]
["Floors","Range","$C$20",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$20","Planchers$C$20"]
["Floors","Range","$C$21",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$21","Planchers$C$21"]
["Floors","Range","$C$22",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$22","Planchers$C$22"]
["Floors","Range","$C$23",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$23","Planchers$C$23"]
["Floors","Range","$C$24",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$24","Planchers$C$24"]
["Floors","Range","$C$25",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$25","Planchers$C$25"]
["Floors","Range","$C$28",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$28","Planchers$C$28"]
["Floors","Range","$C$29",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$29","Planchers$C$29"]
["Floors","Range","$C$30",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$30","Planchers$C$30"]
["Floors","Range","$C$31",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$31","Planchers$C$31"]
["Floors","Range","$C$34",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$34","Planchers$C$34"]
["Floors","Range","$C$38",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$38","Planchers$C$38"]
["Floors","Range","$C$39",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$39","Planchers$C$39"]
["Floors","Range","$C$40",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$40","Planchers$C$40"]
["Floors","Range","$C$43",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$43","Planchers$C$43"]
["Floors","Range","$C$44",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$44","Planchers$C$44"]
["Floors","Range","$C$45",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$45","Planchers$C$45"]
["Floors","Range","$C$46",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$46","Planchers$C$46"]
["Floors","Range","$C$47",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$47","Planchers$C$47"]
["Floors","Range","$C$49",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$49","Planchers$C$49"]
["Floors","Range","$C$50",54.89,31.5,46.44,"four_lines","Planchers","Floors$C$50","Planchers$C$50"]
["Floors","Range","$C$51",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$51","Planchers$C$51"]
["Floors","Range","$C$52",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$52","Planchers$C$52"]
["Floors","Range","$C$53",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$53","Planchers$C$53"]
["Floors","Range","$C$54",54.89,23.25,46.44,"three_lines","Planchers","Floors$C$54","Planchers$C$54"]
["Floors","Range","$C$57",54.89,31.5,46.44,"three_lines","Planchers","Floors$C$57","Planchers$C$57"]
["Floors","Range","$C$58",54.89,31.75,46.44,"two_lines","Planchers","Floors$C$58","Planchers$C$58"]
["Floors","Range","$C$59",54.89,30.25,46.44,"two_lines","Planchers","Floors$C$59","Planchers$C$59"]
["Floors","Range","$C$60",54.89,33.75,46.44,"two_lines","Planchers","Floors$C$60","Planchers$C$60"]
["Floors","Range","$C$61",54.89,63,46.44,"two_lines","Planchers","Floors$C$61","Planchers$C$61"]
["Floors","Range","$C$62",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$62","Planchers$C$62"]
["Floors","Range","$C$64",54.89,23.25,46.44,"one_line","Planchers","Floors$C$64","Planchers$C$64"]
["Floors","Range","$C$66",54.89,63,46.44,"five_lines","Planchers",{"$f":"A773&C773","v":"Floors$C$66"},{"$f":"H773&C773","v":"Planchers$C$66"}]
["Floors","Range","$C$67",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$67","Planchers$C$67"]
["Floors","Range","$C$69",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$69","Planchers$C$69"]
["Floors","Range","$C$70",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$70","Planchers$C$70"]
["Floors","Range","$C$71",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$71","Planchers$C$71"]
["Floors","Range","$C$73",54.89,31.5,46.44,"three_lines","Planchers","Floors$C$73","Planchers$C$73"]
["Floors","Range","$C$74",54.89,47.25,46.44,"five_lines","Planchers","Floors$C$74","Planchers$C$74"]
["Floors","Range","$C$75",54.89,23.25,46.44,"one_line","Planchers","Floors$C$75","Planchers$C$75"]
["Floors","Range","$C$78",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$78","Planchers$C$78"]
["Floors","Range","$C$79",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$79","Planchers$C$79"]
["Floors","Range","$C$80",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$80","Planchers$C$80"]
["Floors","Range","$C$81",54.89,23.25,46.44,"one_line","Planchers","Floors$C$81","Planchers$C$81"]
["Floors","Range","$C$83",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$83","Planchers$C$83"]
["Floors","Range","$C$84",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$84","Planchers$C$84"]
["Floors","Range","$C$85",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$85","Planchers$C$85"]
["Floors","Range","$C$86",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$86","Planchers$C$86"]
["Floors","Range","$C$87",54.89,23.25,46.44,"three_lines","Planchers","Floors$C$87","Planchers$C$87"]
["Floors","Range","$C$89",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$89","Planchers$C$89"]
["Floors","Range","$C$90",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$90","Planchers$C$90"]
["Floors","Range","$C$91",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$91","Planchers$C$91"]
["Floors","Range","$C$92",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$92","Planchers$C$92"]
["Floors","Range","$C$93",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$93","Planchers$C$93"]
["Floors","Range","$C$94",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$94","Planchers$C$94"]
["Floors","Range","$C$95",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$95","Planchers$C$95"]
["Floors","Range","$C$96",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$96","Planchers$C$96"]
["Floors","Range","$C$98",54.89,23.25,46.44,"one_line","Planchers","Floors$C$98","Planchers$C$98"]
["Floors","Range","$C$100",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$100","Planchers$C$100"]
["Floors","Range","$C$101",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$101","Planchers$C$101"]
["Floors","Range","$C$102",54.89,31.5,46.44,"three_lines","Planchers","Floors$C$102","Planchers$C$102"]
["Floors","Range","$C$104",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$104","Planchers$C$104"]
["Floors","Range","$C$105",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$105","Planchers$C$105"]
["Floors","Range","$C$108",54.89,23.25,46.44,"one_line","Planchers","Floors$C$108","Planchers$C$108"]
["Floors","Range","$C$109",54.89,47.25,46.44,"four_lines","Planchers","Floors$C$109","Planchers$C$109"]
["Floors","Range","$C$110",54.89,47.25,46.44,"four_lines","Planchers","Floors$C$110","Planchers$C$110"]
["Floors","Range","$C$111",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$111","Planchers$C$111"]
["Floors","Range","$C$113",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$113","Planchers$C$113"]
["Floors","Range","$C$114",54.89,23.25,46.44,"one_line","Planchers","Floors$C$114","Planchers$C$114"]
["Floors","Range","$C$115",54.89,23.25,46.44,"one_line","Planchers","Floors$C$115","Planchers$C$115"]
["Floors","Range","$C$116",54.89,23.25,46.44,"one_line","Planchers","Floors$C$116","Planchers$C$116"]
["Floors","Range","$C$118",54.89,23.25,46.44,"one_line","Planchers","Floors$C$118","Planchers$C$118"]
["Floors","Range","$C$119",54.89,23.25,46.44,"one_line","Planchers","Floors$C$119","Planchers$C$119"]
["Floors","Range","$C$120",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$120","Planchers$C$120"]
["Floors","Range","$C$121",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$121","Planchers$C$121"]
["Floors","Range","$C$122",54.89,23.25,46.44,"one_line","Planchers","Floors$C$122","Planchers$C$122"]
["Floors","Range","$C$123",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$123","Planchers$C$123"]
["Floors","Range","$C$125",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$125","Planchers$C$125"]
["Floors","Range","$C$126",54.89,31.5,46.44,"two_lines","Planchers","Floors$C$126","Planchers$C$126"]
["Floors","Range","$C$127",54.89,23.25,46.44,"two_lines","Planchers","Floors$C$127","Planchers$C$127"]
["Ceilings","Range","$C$8",54.89,23.25,54.89,"two_lines","Plafonds","Ceilings$C$8","Plafonds$C$8"]
["Ceilings","Range","$C$9",54.89,23.25,54.89,"two_lines","Plafonds","Ceilings$C$9","Plafonds$C$9"]
["Ceilings","Range","$C$10",54.89,31.5,54.89,"two_lines","Plafonds","Ceilings$C$10","Plafonds$C$10"]
["Ceilings","Range","$C$11",54.89,23.25,54.89,"one_line","Plafonds","Ceilings$C$11","Plafonds$C$11"]
["Ceilings","Range","$C$12",54.89,31.5,54.89,"two_lines","Plafonds","Ceilings$C$12","Plafonds$C$12"]
["Ceilings","Range","$C$15",54.89,47.25,54.89,"three_lines","Plafonds","Ceilings$C$15","Plafonds$C$15"]
["Ceilings","Range","$C$16",54.89,23.25,54.89,"one_line","Plafonds","Ceilings$C$16","Plafonds$C$16"]
["Ceilings","Range","$C$17",54.89,47.25,54.89,"two_lines","Plafonds","Ceilings$C$17","Plafonds$C$17"]
["Ceilings","Range","$C$19",54.89,23.25,54.89,"two_lines","Plafonds","Ceilings$C$19","Plafonds$C$19"]
["Ceilings","Range","$C$20",54.89,31.5,54.89,"two_lines","Plafonds","Ceilings$C$20","Plafonds$C$20"]
["Ceilings","Range","$C$21",54.89,31.5,54.89,"two_lines","Plafonds","Ceilings$C$21","Plafonds$C$21"]
["Ceilings","Range","$C$22",54.89,23.25,54.89,"two_lines","Plafonds","Ceilings$C$22","Plafonds$C$22"]
["Ceilings","Range","$C$23",54.89,31.5,54.89,"two_lines","Plafonds","Ceilings$C$23","Plafonds$C$23"]
["Ceilings","Range","$C$24",54.89,23.25,54.89,"two_lines","Plafonds","Ceilings$C$24","Plafonds$C$24"]
["Roof","Range","$C$7",54.89,31.5,46.44,"two_lines","Toit","Roof$C$7","Toit$C$7"]
["Roof","Range","$C$8",54.89,31.5,46.44,"two_lines","Toit","Roof$C$8","Toit$C$8"]
["Roof","Range","$C$9",54.89,31.5,46.44,"two_lines","Toit",{"$f":"A837&C837","v":"Roof$C$9"},{"$f":"H837&C837","v":"Toit$C$9"}]
["Roof","Range","$C$10",54.89,31.5,46.44,"two_lines","Toit","Roof$C$10","Toit$C$10"]
["Roof","Range","$C$11",54.89,31.5,46.44,"two_lines","Toit","Roof$C$11","Toit$C$11"]
["Roof","Range","$C$13",54.89,74.25,46.44,85,"Toit","Roof$C$13","Toit$C$13"]
["Roof","Range","$C$15",54.89,31.5,46.44,"two_lines","Toit","Roof$C$15","Toit$C$15"]
["Roof","Range","$C$16",54.89,31.5,46.44,"two_lines","Toit","Roof$C$16","Toit$C$16"]
["Roof","Range","$C$17",54.89,31.5,46.44,"two_lines","Toit","Roof$C$17","Toit$C$17"]
["Roof","Range","$C$18",54.89,31.5,46.44,"two_lines","Toit","Roof$C$18","Toit$C$18"]
["Roof","Range","$C$21",54.89,31.5,46.44,"two_lines","Toit","Roof$C$21","Toit$C$21"]
["Roof","Range","$C$22",54.89,31.5,46.44,"two_lines","Toit","Roof$C$22","Toit$C$22"]
["Roof","Range","$C$24",54.89,47.25,46.44,"three_lines","Toit","Roof$C$24","Toit$C$24"]
["Roof","Range","$C$25",54.89,23.25,46.44,"two_lines","Toit","Roof$C$25","Toit$C$25"]
["Roof","Range","$C$26",54.89,23.25,46.44,"two_lines","Toit","Roof$C$26","Toit$C$26"]
["Roof","Range","$C$29",54.89,23.25,46.44,"one_line","Toit","Roof$C$29","Toit$C$29"]
["Roof","Range","$C$30",54.89,47.25,46.44,"three_lines","Toit","Roof$C$30","Toit$C$30"]
["Roof","Range","$C$31",54.89,31.5,46.44,"three_lines","Toit","Roof$C$31","Toit$C$31"]
["Roof","Range","$C$32",54.89,23.25,46.44,"one_line","Toit","Roof$C$32","Toit$C$32"]
["Roof","Range","$C$35",54.89,31.5,46.44,"two_lines","Toit","Roof$C$35","Toit$C$35"]
["Roof","Range","$C$36",54.89,31.5,46.44,"two_lines","Toit","Roof$C$36","Toit$C$36"]
["Roof","Range","$C$37",54.89,31.5,46.44,"two_lines","Toit","Roof$C$37","Toit$C$37"]
["Roof","Range","$C$41",54.89,31.5,46.44,"three_lines","Toit","Roof$C$41","Toit$C$41"]
["Roof","Range","$C$42",54.89,23.25,46.44,"one_line","Toit","Roof$C$42","Toit$C$42"]
["Roof","Range","$C$43",54.89,23.25,46.44,"one_line","Toit","Roof$C$43","Toit$C$43"]
["Roof","Range","$C$44",54.89,23.25,46.44,"one_line","Toit","Roof$C$44","Toit$C$44"]
["Roof","Range","$C$45",54.89,23.25,46.44,"one_line","Toit","Roof$C$45","Toit$C$45"]
["Roof","Range","$C$46",54.89,23.25,46.44,"two_lines","Toit","Roof$C$46","Toit$C$46"]
["Roof","Range","$C$49",54.89,23.25,46.44,"two_lines","Toit","Roof$C$49","Toit$C$49"]
["Roof","Range","$C$50",54.89,31.5,46.44,"two_lines","Toit","Roof$C$50","Toit$C$50"]
["Roof","Range","$C$51",54.89,31.5,46.44,"two_lines","Toit","Roof$C$51","Toit$C$51"]
["Roof","Range","$C$52",54.89,23.25,46.44,"two_lines","Toit","Roof$C$52","Toit$C$52"]
["Roof","Range","$C$53",54.89,31.5,46.44,"two_lines","Toit","Roof$C$53","Toit$C$53"]
["Roof","Range","$C$56",54.89,31.5,46.44,"three_lines","Toit","Roof$C$56","Toit$C$56"]
["Roof","Range","$C$57",54.89,31.5,46.44,"two_lines","Toit","Roof$C$57","Toit$C$57"]
["Roof","Range","$C$60",54.89,23.25,46.44,"two_lines","Toit","Roof$C$60","Toit$C$60"]
["Roof","Range","$C$61",54.89,23.25,46.44,"one_line","Toit","Roof$C$61","Toit$C$61"]
["Roof","Range","$C$62",54.89,23.25,46.44,"two_lines","Toit","Roof$C$62","Toit$C$62"]
["Roof","Range","$C$64",54.89,23.25,46.44,"one_line","Toit","Roof$C$64","Toit$C$64"]
["Roof","Range","$C$68",54.89,31.5,46.44,"two_lines","Toit","Roof$C$68","Toit$C$68"]
["Roof","Range","$C$69",54.89,31.5,46.44,"two_lines","Toit","Roof$C$69","Toit$C$69"]
["Roof","Range","$C$70",54.89,23.25,46.44,"one_line","Toit","Roof$C$70","Toit$C$70"]
["Roof","Range","$C$73",54.89,31.5,46.44,"two_lines","Toit","Roof$C$73","Toit$C$73"]
["Roof","Range","$C$74",54.89,31.5,46.44,"two_lines","Toit","Roof$C$74","Toit$C$74"]
["Roof","Range","$C$75",54.89,23.25,46.44,"two_lines","Toit","Roof$C$75","Toit$C$75"]
["Roof","Range","$C$76",54.89,23.25,46.44,"three_lines","Toit","Roof$C$76","Toit$C$76"]
["Roof","Range","$C$79",54.89,23.25,46.44,"two_lines","Toit","Roof$C$79","Toit$C$79"]
["Roof","Range","$C$80",54.89,31.5,46.44,"two_lines","Toit","Roof$C$80","Toit$C$80"]
["Roof","Range","$C$81",54.89,31.5,46.44,"two_lines","Toit","Roof$C$81","Toit$C$81"]
["Roof","Range","$C$82",54.89,31.5,46.44,"two_lines","Toit","Roof$C$82","Toit$C$82"]
["Roof","Range","$C$83",54.89,31.5,46.44,"two_lines","Toit","Roof$C$83","Toit$C$83"]
["Roof","Range","$C$84",54.89,31.5,46.44,"two_lines","Toit","Roof$C$84","Toit$C$84"]
["Roof","Range","$C$85",54.89,31.5,46.44,"two_lines","Toit","Roof$C$85","Toit$C$85"]
["Roof","Range","$C$87",54.89,23.25,46.44,"one_line","Toit","Roof$C$87","Toit$C$87"]
["Roof","Range","$C$89",54.89,31.5,46.44,"two_lines","Toit","Roof$C$89","Toit$C$89"]
["Roof","Range","$C$90",54.89,31.5,46.44,"two_lines","Toit","Roof$C$90","Toit$C$90"]
["Roof","Range","$C$91",54.89,31.5,46.44,"three_lines","Toit","Roof$C$91","Toit$C$91"]
["Roof","Range","$C$93",54.89,31.5,46.44,"two_lines","Toit","Roof$C$93","Toit$C$93"]
["Roof","Range","$C$94",54.89,31.5,46.44,"two_lines","Toit","Roof$C$94","Toit$C$94"]
["Roof","Range","$C$97",54.89,23.25,46.44,"one_line","Toit","Roof$C$97","Toit$C$97"]
["Roof","Range","$C$98",54.89,47.25,46.44,"four_lines","Toit","Roof$C$98","Toit$C$98"]
["Roof","Range","$C$99",54.89,47.25,46.44,"four_lines","Toit","Roof$C$99","Toit$C$99"]
["Roof","Range","$C$100",54.89,31.5,46.44,"two_lines","Toit","Roof$C$100","Toit$C$100"]
["Roof","Range","$C$103",54.89,23.25,46.44,"one_line","Toit","Roof$C$103","Toit$C$103"]
["Roof","Range","$C$104",54.89,23.25,46.44,"one_line","Toit","Roof$C$104","Toit$C$104"]
["Roof","Range","$C$105",54.89,23.25,46.44,"one_line","Toit","Roof$C$105","Toit$C$105"]
["Roof","Range","$C$107",54.89,23.25,46.44,"one_line","Toit",{"$f":"A901&C901","v":"Roof$C$107"},{"$f":"H901&C901","v":"Toit$C$107"}]
["Roof","Range","$C$108",54.89,23.25,46.44,"one_line","Toit","Roof$C$108","Toit$C$108"]
["Roof","Range","$C$109",54.89,23.25,46.44,"two_lines","Toit","Roof$C$109","Toit$C$109"]
["Roof","Range","$C$110",54.89,23.25,46.44,"two_lines","Toit","Roof$C$110","Toit$C$110"]
["Roof","Range","$C$111",54.89,23.25,46.44,"one_line","Toit","Roof$C$111","Toit$C$111"]
["Roof","Range","$C$112",54.89,23.25,46.44,"two_lines","Toit","Roof$C$112","Toit$C$112"]
["Roof","Range","$C$115",54.89,31.5,46.44,"two_lines","Toit","Roof$C$115","Toit$C$115"]
["Roof","Range","$C$116",54.89,23.25,46.44,"two_lines","Toit","Roof$C$116","Toit$C$116"]
["Roof","Range","$C$118",54.89,36,46.44,"two_lines","Toit","Roof$C$118","Toit$C$118"]
["Roof","Range","$C$119",54.89,36,46.44,"two_lines","Toit","Roof$C$119","Toit$C$119"]
["Roof","Range","$C$120",54.89,36,46.44,60,"Toit","Roof$C$120","Toit$C$120"]
["Roof","Range","$C$123",54.89,31.5,46.44,"two_lines","Toit","Roof$C$123","Toit$C$123"]
["Roof","Range","$C$124",54.89,31.5,46.44,"two_lines","Toit","Roof$C$124","Toit$C$124"]
["Roof","Range","$C$127",54.89,47.25,46.44,"three_lines","Toit","Roof$C$127","Toit$C$127"]
["Roof","Range","$C$128",54.89,31.5,46.44,"two_lines","Toit","Roof$C$128","Toit$C$128"]
["Roof","Range","$C$129",54.89,23.25,46.44,"two_lines","Toit","Roof$C$129","Toit$C$129"]
["Roof","Range","$C$130",54.89,31.5,46.44,"two_lines","Toit","Roof$C$130","Toit$C$130"]
["Roof","Range","$C$131",54.89,31.5,46.44,"four_lines","Toit","Roof$C$131","Toit$C$131"]
["Roof","Range","$C$133",54.89,23.25,46.44,"two_lines","Toit","Roof$C$133","Toit$C$133"]
["Roof","Range","$C$134",54.89,31.5,46.44,"two_lines","Toit","Roof$C$134","Toit$C$134"]
["Roof","Range","$C$135",54.89,23.25,46.44,"two_lines","Toit","Roof$C$135","Toit$C$135"]
["Roof","Range","$C$136",54.89,31.5,46.44,"two_lines","Toit","Roof$C$136","Toit$C$136"]
["Roof","Range","$C$137",54.89,31.5,46.44,"two_lines","Toit","Roof$C$137","Toit$C$137"]
["Roof","Range","$C$140",54.89,31.5,46.44,"two_lines","Toit","Roof$C$140","Toit$C$140"]
["Roof","Range","$C$141",54.89,23.25,46.44,"two_lines","Toit","Roof$C$141","Toit$C$141"]
["Roof","Range","$C$142",54.89,31.5,46.44,"two_lines","Toit","Roof$C$142","Toit$C$142"]
["Roof","Range","$C$143",54.89,31.5,46.44,"three_lines","Toit","Roof$C$143","Toit$C$143"]
["Roof","Range","$C$146",54.89,23.25,46.44,"two_lines","Toit","Roof$C$146","Toit$C$146"]
["Roof","Range","$C$147",54.89,23.25,46.44,"two_lines","Toit","Roof$C$147","Toit$C$147"]
["Roof","Range","$C$148",54.89,23.25,46.44,"two_lines","Toit","Roof$C$148","Toit$C$148"]
["Roof","Range","$C$150",54.89,23.25,46.44,46,"Toit","Roof$C$150","Toit$C$150"]
["Roof","Range","$C$152",54.89,33.75,46.44,"two_lines","Toit","Roof$C$152","Toit$C$152"]
["Roof","Range","$C$153",54.89,33.75,46.44,"two_lines","Toit","Roof$C$153","Toit$C$153"]
["Roof","Range","$C$154",54.89,33.75,46.44,"two_lines","Toit","Roof$C$154","Toit$C$154"]
["Roof","Range","$C$155",54.89,33.75,46.44,"three_lines","Toit","Roof$C$155","Toit$C$155"]
["Garage","Range","$C$8",54.89,23.25,46.22,"two_lines","Garage","Garage$C$8","Garage$C$8"]
["Garage","Range","$C$9",54.89,31.5,46.22,"two_lines","Garage","Garage$C$9","Garage$C$9"]
["Garage","Range","$C$10",54.89,31.5,46.22,"two_lines","Garage","Garage$C$10","Garage$C$10"]
["Garage","Range","$C$11",54.89,31.5,46.22,"two_lines","Garage","Garage$C$11","Garage$C$11"]
["Garage","Range","$C$12",54.89,31.5,46.22,"two_lines","Garage","Garage$C$12","Garage$C$12"]
["Garage","Range","$C$15",54.89,"two_lines",46.22,"two_lines","Garage","Garage$C$15","Garage$C$15"]
["Garage","Range","$C$16",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$16","Garage$C$16"]
["Garage","Range","$C$17",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$17","Garage$C$17"]
["Garage","Range","$C$18",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$18","Garage$C$18"]
["Garage","Range","$C$19",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$19","Garage$C$19"]
["Garage","Range","$C$20",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$20","Garage$C$20"]
["Garage","Range","$C$21",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$21","Garage$C$21"]
["Garage","Range","$C$23",54.89,"two_lines",46.22,"two_lines","Garage","Garage$C$23","Garage$C$23"]
["Garage","Range","$C$24",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$24","Garage$C$24"]
["Garage","Range","$C$25",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$25","Garage$C$25"]
["Garage","Range","$C$26",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$26","Garage$C$26"]
["Garage","Range","$C$27",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$27","Garage$C$27"]
["Garage","Range","$C$28",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$28","Garage$C$28"]
["Garage","Range","$C$29",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$29","Garage$C$29"]
["Garage","Range","$C$32",54.89,23.25,46.22,"one_line","Garage","Garage$C$32","Garage$C$32"]
["Garage","Range","$C$35",54.89,"two_lines",46.22,"two_lines","Garage","Garage$C$35","Garage$C$35"]
["Garage","Range","$C$36",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$36","Garage$C$36"]
["Garage","Range","$C$37",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$37","Garage$C$37"]
["Garage","Range","$C$38",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$38","Garage$C$38"]
["Garage","Range","$C$39",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$39","Garage$C$39"]
["Garage","Range","$C$40",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$40","Garage$C$40"]
["Garage","Range","$C$41",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$41","Garage$C$41"]
["Garage","Range","$C$43",54.89,"two_lines",46.22,"two_lines","Garage","Garage$C$43","Garage$C$43"]
["Garage","Range","$C$44",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$44","Garage$C$44"]
["Garage","Range","$C$45",54.89,"one_line",46.22,"two_lines","Garage",{"$f":"A965&C965","v":"Garage$C$45"},{"$f":"H965&C965","v":"Garage$C$45"}]
["Garage","Range","$C$46",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$46","Garage$C$46"]
["Garage","Range","$C$47",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$47","Garage$C$47"]
["Garage","Range","$C$48",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$48","Garage$C$48"]
["Garage","Range","$C$49",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$49","Garage$C$49"]
["Garage","Range","$C$48",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$48","Garage$C$48"]
["Garage","Range","$C$49",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$49","Garage$C$49"]
["Garage","Range","$C$52",54.89,23.25,46.22,"two_lines","Garage","Garage$C$52","Garage$C$52"]
["Garage","Range","$C$53",54.89,23.25,46.22,"two_lines","Garage","Garage$C$53","Garage$C$53"]
["Garage","Range","$C$54",54.89,23.25,46.22,"two_lines","Garage","Garage$C$54","Garage$C$54"]
["Garage","Range","$C$55",54.89,23.25,46.22,"two_lines","Garage","Garage$C$55","Garage$C$55"]
["Garage","Range","$C$56",54.89,23.25,46.22,"two_lines","Garage","Garage$C$56","Garage$C$56"]
["Garage","Range","$C$57",54.89,23.25,46.22,"two_lines","Garage","Garage$C$57","Garage$C$57"]
["Garage","Range","$C$60",54.89,23.25,46.22,73,"Garage","Garage$C$60","Garage$C$60"]
["Garage","Range","$C$62",54.89,82.5,46.22,98.25,"Garage","Garage$C$62","Garage$C$62"]
["Garage","Range","$C$66",54.89,"two_lines",46.22,"two_lines","Garage","Garage$C$66","Garage$C$66"]
["Garage","Range","$C$67",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$67","Garage$C$67"]
["Garage","Range","$C$68",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$68","Garage$C$68"]
["Garage","Range","$C$69",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$69","Garage$C$69"]
["Garage","Range","$C$70",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$70","Garage$C$70"]
["Garage","Range","$C$71",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$71","Garage$C$71"]
["Garage","Range","$C$72",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$72","Garage$C$72"]
["Garage","Range","$C$74",54.89,"two_lines",46.22,"two_lines","Garage","Garage$C$74","Garage$C$74"]
["Garage","Range","$C$75",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$75","Garage$C$75"]
["Garage","Range","$C$76",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$76","Garage$C$76"]
["Garage","Range","$C$77",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$77","Garage$C$77"]
["Garage","Range","$C$78",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$78","Garage$C$78"]
["Garage","Range","$C$79",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$79","Garage$C$79"]
["Garage","Range","$C$80",54.89,"one_line",46.22,"two_lines","Garage","Garage$C$80","Garage$C$80"]
["Garage","Range","$C$84",54.89,31.5,46.22,"three_lines","Garage","Garage$C$84","Garage$C$84"]
["Garage","Range","$C$85",54.89,31.5,46.22,"two_lines","Garage","Garage$C$85","Garage$C$85"]
["Garage","Range","$C$86",54.89,31.5,46.22,"two_lines","Garage","Garage$C$86","Garage$C$86"]
["Garage","Range","$C$87",54.89,31.5,46.22,"three_lines","Garage","Garage$C$87","Garage$C$87"]
["Garage","Range","$C$88",54.89,31.5,46.22,"two_lines","Garage","Garage$C$88","Garage$C$88"]
["Garage","Range","$C$89",54.89,31.5,46.22,"three_lines","Garage","Garage$C$89","Garage$C$89"]
["Garage","Range","$C$94",54.89,31.5,46.22,"two_lines","Garage","Garage$C$94","Garage$C$94"]
["Garage","Range","$C$95",54.89,31.5,46.22,"two_lines","Garage","Garage$C$95","Garage$C$95"]
["Garage","Range","$C$96",54.89,31.5,46.22,"two_lines","Garage","Garage$C$96","Garage$C$96"]
["Garage","Range","$C$97",54.89,31.5,46.22,"two_lines","Garage","Garage$C$97","Garage$C$97"]
["Garage","Range","$C$98",54.89,31.5,46.22,"two_lines","Garage","Garage$C$98","Garage$C$98"]
["Garage","Range","$C$99",54.89,31.5,46.22,"two_lines","Garage","Garage$C$99","Garage$C$99"]
["Garage","Range","$C$102",54.89,84.75,46.22,50,"Garage","Garage$C$102","Garage$C$102"]
["Garage","Range","$C$103",54.89,84.75,46.22,50,"Garage","Garage$C$103","Garage$C$103"]
["Garage","Range","$C$104",54.89,84.75,46.22,50,"Garage","Garage$C$104","Garage$C$104"]
["Garage","Range","$C$108",54.89,31.5,46.22,"two_lines","Garage","Garage$C$108","Garage$C$108"]
["Garage","Range","$C$109",54.89,31.5,46.22,"two_lines","Garage","Garage$C$109","Garage$C$109"]
["Garage","Range","$C$110",54.89,31.5,46.22,"two_lines","Garage","Garage$C$110","Garage$C$110"]
["Garage","Range","$C$111",54.89,31.5,46.22,"two_lines","Garage","Garage$C$111","Garage$C$111"]
["Garage","Range","$C$115",54.89,31.75,46.22,"two_lines","Garage","Garage$C$115","Garage$C$115"]
["Garage","Range","$C$116",54.89,31.5,46.22,"two_lines","Garage","Garage$C$116","Garage$C$116"]
["Garage","Range","$C$117",54.89,31.5,46.22,"two_lines","Garage","Garage$C$117","Garage$C$117"]
["Garage","Range","$C$118",54.89,23.25,46.22,"two_lines","Garage","Garage$C$118","Garage$C$118"]
["Garage","Range","$C$119",54.89,31.5,46.22,"two_lines","Garage","Garage$C$119","Garage$C$119"]
["Garage","Range","$C$122",54.89,31.5,46.22,"three_lines","Garage","Garage$C$122","Garage$C$122"]
["Garage","Range","$C$123",54.89,31.5,46.22,"two_lines","Garage","Garage$C$123","Garage$C$123"]
["Garage","Range","$C$124",54.89,31.5,46.22,"three_lines","Garage","Garage$C$124","Garage$C$124"]
["Garage","Range","$C$125",54.89,31.5,46.22,"two_lines","Garage","Garage$C$125","Garage$C$125"]
["Garage","Range","$C$126",54.89,31.5,46.22,"two_lines","Garage","Garage$C$126","Garage$C$126"]
["Garage","Range","$C$129",54.89,31.5,46.22,"two_lines","Garage","Garage$C$129","Garage$C$129"]
["Garage","Range","$C$130",54.89,31.5,46.22,"two_lines","Garage","Garage$C$130","Garage$C$130"]
["Garage","Range","$C$131",54.89,42.75,46.22,"three_lines","Garage","Garage$C$131","Garage$C$131"]
["Garage","Range","$C$132",54.89,23.25,46.22,"two_lines","Garage","Garage$C$132","Garage$C$132"]
["Garage","Range","$C$134",54.89,31.5,46.22,"two_lines","Garage","Garage$C$134","Garage$C$134"]
["Garage","Range","$C$135",54.89,31.5,46.22,"two_lines","Garage","Garage$C$135","Garage$C$135"]
["Garage","Range","$C$136",54.89,31.5,46.22,"two_lines","Garage",{"$f":"A1029&C1029","v":"Garage$C$136"},{"$f":"H1029&C1029","v":"Garage$C$136"}]
["Garage","Range","$C$138",54.89,47,46.22,"three_lines","Garage","Garage$C$138","Garage$C$138"]
["Garage","Range","$C$139",54.89,23.25,46.22,"two_lines","Garage","Garage$C$139","Garage$C$139"]
["Garage","Range","$C$140",54.89,23.25,46.22,"two_lines","Garage","Garage$C$140","Garage$C$140"]
["Garage","Range","$C$143",54.89,23.25,46.22,"two_lines","Garage","Garage$C$143","Garage$C$143"]
["Garage","Range","$C$144",54.89,31.5,46.22,"three_lines","Garage","Garage$C$144","Garage$C$144"]
["Garage","Range","$C$145",54.89,31.5,46.22,"two_lines","Garage","Garage$C$145","Garage$C$145"]
["Garage","Range","$C$146",54.89,31.5,46.22,"two_lines","Garage","Garage$C$146","Garage$C$146"]
["Garage","Range","$C$147",54.89,31.5,46.22,"three_lines","Garage","Garage$C$147","Garage$C$147"]
["Garage","Range","$C$148",54.89,31.5,46.22,"two_lines","Garage","Garage$C$148","Garage$C$148"]
["Garage","Range","$C$149",54.89,31.5,46.22,"three_lines","Garage","Garage$C$149","Garage$C$149"]
["Garage","Range","$C$153",54.89,31.5,46.22,"two_lines","Garage","Garage$C$153","Garage$C$153"]
["Garage","Range","$C$154",54.89,31.5,46.22,"two_lines","Garage","Garage$C$154","Garage$C$154"]
["Garage","Range","$C$155",54.89,23.25,46.22,"one_line","Garage","Garage$C$155","Garage$C$155"]
["Garage","Range","$C$158",54.89,31.5,46.22,"two_lines","Garage","Garage$C$158","Garage$C$158"]
["Garage","Range","$C$159",54.89,31.5,46.22,"two_lines","Garage","Garage$C$159","Garage$C$159"]
["Garage","Range","$C$160",54.89,23.25,46.22,"two_lines","Garage","Garage$C$160","Garage$C$160"]
["Garage","Range","$C$161",54.89,23.25,46.22,"three_lines","Garage","Garage$C$161","Garage$C$161"]
["Garage","Range","$C$163",54.89,31.5,46.22,"two_lines","Garage","Garage$C$163","Garage$C$163"]
["Garage","Range","$C$164",54.89,31.5,46.22,"two_lines","Garage","Garage$C$164","Garage$C$164"]
["Garage","Range","$C$165",54.89,31.5,46.22,"two_lines","Garage","Garage$C$165","Garage$C$165"]
["Garage","Range","$C$166",54.89,31.5,46.22,"two_lines","Garage","Garage$C$166","Garage$C$166"]
["Garage","Range","$C$167",54.89,31.5,46.22,"two_lines","Garage","Garage$C$167","Garage$C$167"]
["Garage","Range","$C$168",54.89,31.5,46.22,"two_lines","Garage","Garage$C$168","Garage$C$168"]
["Garage","Range","$C$169",54.89,31.5,46.22,"two_lines","Garage","Garage$C$169","Garage$C$169"]
["Garage","Range","$C$172",54.89,47.25,46.22,"four_lines","Garage","Garage$C$172","Garage$C$172"]
["Garage","Range","$C$173",54.89,23.25,46.22,"one_line","Garage","Garage$C$173","Garage$C$173"]
["Garage","Range","$C$174",54.89,31.5,46.22,"two_lines","Garage","Garage$C$174","Garage$C$174"]
["Garage","Range","$C$177",54.89,23.25,46.22,"one_line","Garage","Garage$C$177","Garage$C$177"]
["Garage","Range","$C$178",54.89,23.25,46.22,"one_line","Garage","Garage$C$178","Garage$C$178"]
["Garage","Range","$C$179",54.89,23.25,46.22,"one_line","Garage","Garage$C$179","Garage$C$179"]
["Garage","Range","$C$180",54.89,23.25,46.22,"two_lines","Garage","Garage$C$180","Garage$C$180"]
["Garage","Range","$C$182",54.89,23.25,46.22,"one_line","Garage","Garage$C$182","Garage$C$182"]
["Garage","Range","$C$183",54.89,23.25,46.22,"one_line","Garage","Garage$C$183","Garage$C$183"]
["Garage","Range","$C$184",54.89,23.25,46.22,"two_lines","Garage","Garage$C$184","Garage$C$184"]
["Garage","Range","$C$185",54.89,23.25,46.22,"one_line","Garage","Garage$C$185","Garage$C$185"]
["Garage","Range","$C$186",54.89,23.25,46.22,"two_lines","Garage","Garage$C$186","Garage$C$186"]
["Garage","Range","$C$188",54.89,31.5,46.22,"two_lines","Garage","Garage$C$188","Garage$C$188"]
["Garage","Range","$C$189",54.89,31.5,46.22,"two_lines","Garage","Garage$C$189","Garage$C$189"]
["Garage","Range","$C$190",54.89,31.5,46.22,"three_lines","Garage","Garage$C$190","Garage$C$190"]
["Garage","Range","$C$192",54.89,31.5,46.22,"two_lines","Garage","Garage$C$192","Garage$C$192"]
["Garage","Range","$C$193",54.89,31.5,46.22,"two_lines","Garage","Garage$C$193","Garage$C$193"]
["Garage","Range","$C$196",54.89,31.5,46.22,"two_lines","Garage","Garage$C$196","Garage$C$196"]
["Garage","Range","$C$197",54.89,23.25,46.22,"two_lines","Garage","Garage$C$197","Garage$C$197"]
["Garage","Range","$C$198",54.89,23.25,46.22,"one_line","Garage","Garage$C$198","Garage$C$198"]
["Garage","Range","$C$202",54.89,31.5,46.22,"two_lines","Garage","Garage$C$202","Garage$C$202"]
["Garage","Range","$C$203",54.89,31.5,46.22,"two_lines","Garage","Garage$C$203","Garage$C$203"]
["Garage","Range","$C$206",54.89,47.25,46.22,"three_lines","Garage","Garage$C$206","Garage$C$206"]
["Garage","Range","$C$207",54.89,31.5,46.22,"two_lines","Garage","Garage$C$207","Garage$C$207"]
["Garage","Range","$C$208",54.89,23.25,46.22,"two_lines","Garage","Garage$C$208","Garage$C$208"]
["Garage","Range","$C$209",54.89,31.5,46.22,"two_lines","Garage","Garage$C$209","Garage$C$209"]
["Garage","Range","$C$210",54.89,31.5,46.22,"four_lines","Garage","Garage$C$210","Garage$C$210"]
["Garage","Range","$C$212",54.89,23.25,46.22,"two_lines","Garage","Garage$C$212","Garage$C$212"]
["Garage","Range","$C$213",54.89,31.5,46.22,"two_lines","Garage","Garage$C$213","Garage$C$213"]
["Garage","Range","$C$214",54.89,23.25,46.22,"two_lines","Garage","Garage$C$214","Garage$C$214"]
["Garage","Range","$C$215",54.89,31.5,46.22,"two_lines","Garage","Garage$C$215","Garage$C$215"]
["Garage","Range","$C$216",54.89,31.5,46.22,"two_lines","Garage","Garage$C$216","Garage$C$216"]
["Garage","Range","$C$219",54.89,31.5,46.22,"two_lines","Garage","Garage$C$219","Garage$C$219"]
["Garage","Range","$C$220",54.89,23.25,46.22,"two_lines","Garage","Garage$C$220","Garage$C$220"]
["Garage","Range","$C$221",54.89,31.5,46.22,"two_lines","Garage","Garage$C$221","Garage$C$221"]
["Garage","Range","$C$222",54.89,31.5,46.22,"three_lines","Garage","Garage$C$222","Garage$C$222"]
["Garage","Range","$C$225",54.89,23.25,46.22,"two_lines","Garage","Garage$C$225","Garage$C$225"]
["Garage","Range","$C$226",54.89,23.25,46.22,"two_lines","Garage","Garage$C$226","Garage$C$226"]
["Garage","Range","$C$227",54.89,23.25,46.22,"two_lines","Garage","Garage$C$227","Garage$C$227"]
["Garage","Range","$C$232",54.89,31.5,46.22,"two_lines","Garage",{"$f":"A1093&C1093","v":"Garage$C$232"},{"$f":"H1093&C1093","v":"Garage$C$232"}]
["Garage","Range","$C$233",54.89,31.5,46.22,"two_lines","Garage","Garage$C$233","Garage$C$233"]
["Garage","Range","$C$234",54.89,23.25,46.22,"one_line","Garage","Garage$C$234","Garage$C$234"]
["Garage","Range","$C$237",54.89,31.5,46.22,"two_lines","Garage","Garage$C$237","Garage$C$237"]
["Garage","Range","$C$238",54.89,31.5,46.22,"two_lines","Garage","Garage$C$238","Garage$C$238"]
["Garage","Range","$C$239",54.89,23.25,46.22,"two_lines","Garage","Garage$C$239","Garage$C$239"]
["Garage","Range","$C$240",54.89,23.25,46.22,"three_lines","Garage","Garage$C$240","Garage$C$240"]
["Garage","Range","$C$242",54.89,31.5,46.22,"two_lines","Garage","Garage$C$242","Garage$C$242"]
["Garage","Range","$C$243",54.89,31.5,46.22,"two_lines","Garage","Garage$C$243","Garage$C$243"]
["Garage","Range","$C$244",54.89,31.5,46.22,"two_lines","Garage","Garage$C$244","Garage$C$244"]
["Garage","Range","$C$245",54.89,31.5,46.22,"two_lines","Garage","Garage$C$245","Garage$C$245"]
["Garage","Range","$C$246",54.89,31.5,46.22,"two_lines","Garage","Garage$C$246","Garage$C$246"]
["Garage","Range","$C$247",54.89,31.5,46.22,"two_lines","Garage","Garage$C$247","Garage$C$247"]
["Garage","Range","$C$248",54.89,31.5,46.22,"two_lines","Garage","Garage$C$248","Garage$C$248"]
["Garage","Range","$C$251",54.89,47.25,46.22,"four_lines","Garage","Garage$C$251","Garage$C$251"]
["Garage","Range","$C$252",54.89,23.25,46.22,"one_line","Garage","Garage$C$252","Garage$C$252"]
["Garage","Range","$C$253",54.89,31.5,46.22,"two_lines","Garage","Garage$C$253","Garage$C$253"]
["Garage","Range","$C$256",54.89,23.25,46.22,"one_line","Garage","Garage$C$256","Garage$C$256"]
["Garage","Range","$C$257",54.89,23.25,46.22,"one_line","Garage","Garage$C$257","Garage$C$257"]
["Garage","Range","$C$258",54.89,23.25,46.22,"one_line","Garage","Garage$C$258","Garage$C$258"]
["Garage","Range","$C$259",54.89,23.25,46.22,"two_lines","Garage","Garage$C$259","Garage$C$259"]
["Garage","Range","$C$261",54.89,23.25,46.22,"one_line","Garage","Garage$C$261","Garage$C$261"]
["Garage","Range","$C$262",54.89,23.25,46.22,"one_line","Garage","Garage$C$262","Garage$C$262"]
["Garage","Range","$C$263",54.89,23.25,46.22,"two_lines","Garage","Garage$C$263","Garage$C$263"]
["Garage","Range","$C$264",54.89,23.25,46.22,"one_line","Garage","Garage$C$264","Garage$C$264"]
["Garage","Range","$C$265",54.89,23.25,46.22,"two_lines","Garage","Garage$C$265","Garage$C$265"]
["Garage","Range","$C$267",54.89,31.5,46.22,"two_lines","Garage","Garage$C$267","Garage$C$267"]
["Garage","Range","$C$268",54.89,31.5,46.22,"two_lines","Garage","Garage$C$268","Garage$C$268"]
["Garage","Range","$C$269",54.89,31.5,46.22,"three_lines","Garage","Garage$C$269","Garage$C$269"]
["Garage","Range","$C$271",54.89,31.5,46.22,"two_lines","Garage","Garage$C$271","Garage$C$271"]
["Garage","Range","$C$272",54.89,31.5,46.22,"two_lines","Garage","Garage$C$272","Garage$C$272"]
["Garage","Range","$C$275",54.89,31.5,46.22,"two_lines","Garage","Garage$C$275","Garage$C$275"]
["Garage","Range","$C$276",54.89,23.25,46.22,"two_lines","Garage","Garage$C$276","Garage$C$276"]
["Garage","Range","$C$277",54.89,23.25,46.22,"one_line","Garage","Garage$C$277","Garage$C$277"]
["Garage","Range","$C$281",54.89,47.25,46.22,"four_lines","Garage","Garage$C$281","Garage$C$281"]
["Garage","Range","$C$282",54.89,31.5,46.22,"three_lines","Garage","Garage$C$282","Garage$C$282"]
["Garage","Range","$C$283",54.89,31.5,46.22,"four_lines","Garage","Garage$C$283","Garage$C$283"]
["Garage","Range","$C$284",54.89,31.5,46.22,"four_lines","Garage","Garage$C$284","Garage$C$284"]
["Garage","Range","$C$285",54.89,31.5,46.22,"three_lines","Garage","Garage$C$285","Garage$C$285"]
["Garage","Range","$C$286",54.89,31.5,46.22,"three_lines","Garage","Garage$C$286","Garage$C$286"]
["Garage","Range","$C$287",54.89,31.5,46.22,"four_lines","Garage","Garage$C$287","Garage$C$287"]
["Garage","Range","$C$289",54.89,31.5,46.22,"two_lines","Garage","Garage$C$289","Garage$C$289"]
["Garage","Range","$C$290",54.89,31.5,46.22,"two_lines","Garage","Garage$C$290","Garage$C$290"]
["Garage","Range","$C$293",54.89,23.25,46.22,"one_line","Garage","Garage$C$293","Garage$C$293"]
["Garage","Range","$C$294",54.89,23.25,46.22,"one_line","Garage","Garage$C$294","Garage$C$294"]
["Garage","Range","$C$295",54.89,23.25,46.22,"two_lines","Garage","Garage$C$295","Garage$C$295"]
["Garage","Range","$C$296",54.89,23.25,46.22,"two_lines","Garage","Garage$C$296","Garage$C$296"]
["Garage","Range","$C$297",54.89,23.25,46.22,"two_lines","Garage","Garage$C$297","Garage$C$297"]
["Garage","Range","$C$298",54.89,23.25,46.22,"two_lines","Garage","Garage$C$298","Garage$C$298"]
["Garage","Range","$C$299",54.89,23.25,46.22,"two_lines","Garage","Garage$C$299","Garage$C$299"]
["Garage","Range","$C$300",54.89,23.25,46.22,"two_lines","Garage","Garage$C$300","Garage$C$300"]
["Garage","Range","$C$302",54.89,23.25,46.22,"four_lines","Garage","Garage$C$302","Garage$C$302"]
["Garage","Range","$C$305",54.89,31.5,46.22,"two_lines","Garage","Garage$C$305","Garage$C$305"]
["Garage","Range","$C$306",54.89,31.5,46.22,"two_lines","Garage","Garage$C$306","Garage$C$306"]
["Garage","Range","$C$309",54.89,23.25,46.22,"two_lines","Garage","Garage$C$309","Garage$C$309"]
["Garage","Range","$C$310",54.89,23.25,46.22,"two_lines","Garage","Garage$C$310","Garage$C$310"]
["Garage","Range","$C$311",54.89,31.5,46.22,"two_lines","Garage","Garage$C$311","Garage$C$311"]
["Garage","Range","$C$312",54.89,31.5,46.22,"two_lines","Garage","Garage$C$312","Garage$C$312"]
["Garage","Range","$C$313",54.89,23.25,46.22,"two_lines","Garage","Garage$C$313","Garage$C$313"]
["Garage","Range","$C$314",54.89,31.5,46.22,"two_lines","Garage","Garage$C$314","Garage$C$314"]
["Garage","Range","$C$317",54.89,31.5,46.22,"three_lines","Garage","Garage$C$317","Garage$C$317"]
["Garage","Range","$C$318",54.89,31.5,46.22,"two_lines","Garage","Garage$C$318","Garage$C$318"]
["Garage","Range","$C$320",54.89,31.5,46.22,"two_lines","Garage","Garage$C$320","Garage$C$320"]
["Garage","Range","$C$321",54.89,31.5,46.22,"two_lines","Garage","Garage$C$321","Garage$C$321"]
["Garage","Range","$C$322",54.89,23.25,46.22,"one_line","Garage",{"$f":"A1157&C1157","v":"Garage$C$322"},{"$f":"H1157&C1157","v":"Garage$C$322"}]
["Garage","Range","$C$323",54.89,31.5,46.22,"two_lines","Garage","Garage$C$323","Garage$C$323"]
["Garage","Range","$C$325",54.89,31.5,46.22,"two_lines","Garage","Garage$C$325","Garage$C$325"]
["Garage","Range","$C$326",54.89,31.5,46.22,"two_lines","Garage","Garage$C$326","Garage$C$326"]
["Garage","Range","$C$327",54.89,31.5,46.22,"two_lines","Garage","Garage$C$327","Garage$C$327"]
["Garage","Range","$C$329",54.89,31.5,46.22,"two_lines","Garage","Garage$C$329","Garage$C$329"]
["Garage","Range","$C$330",54.89,31.5,46.22,"two_lines","Garage","Garage$C$330","Garage$C$330"]
["Garage","Range","$C$331",54.89,31.5,46.22,50,"Garage","Garage$C$331","Garage$C$331"]
["Garage","Range","$C$333",54.89,31.5,46.22,"two_lines","Garage","Garage$C$333","Garage$C$333"]
["Garage","Range","$C$334",54.89,23.25,46.22,"two_lines","Garage","Garage$C$334","Garage$C$334"]
["Garage","Range","$C$335",54.89,23.25,46.22,"two_lines","Garage","Garage$C$335","Garage$C$335"]
["Garage","Range","$C$336",54.89,31.5,46.22,"two_lines","Garage","Garage$C$336","Garage$C$336"]
["Garage","Range","$C$337",54.89,23.25,46.22,"two_lines","Garage","Garage$C$337","Garage$C$337"]
["Garage","Range","$C$338",54.89,23.25,46.22,"two_lines","Garage","Garage$C$338","Garage$C$338"]
["Garage","Range","$C$340",54.89,47.25,46.22,"three_lines","Garage","Garage$C$340","Garage$C$340"]
["Garage","Range","$C$341",54.89,23.25,46.22,"two_lines","Garage","Garage$C$341","Garage$C$341"]
["Garage","Range","$C$342",54.89,23.25,46.22,"two_lines","Garage","Garage$C$342","Garage$C$342"]
["Garage","Range","$C$344",54.89,23.25,46.22,"two_lines","Garage","Garage$C$344","Garage$C$344"]
["Garage","Range","$C$345",54.89,31.5,46.22,"two_lines","Garage","Garage$C$345","Garage$C$345"]
["Garage","Range","$C$346",54.89,31.5,46.22,"two_lines","Garage","Garage$C$346","Garage$C$346"]
["Garage","Range","$C$347",54.89,23.25,46.22,"two_lines","Garage","Garage$C$347","Garage$C$347"]
["Garage","Range","$C$348",54.89,31.5,46.22,"two_lines","Garage","Garage$C$348","Garage$C$348"]
["Garage","Range","$C$349",54.89,23.25,46.22,"two_lines","Garage","Garage$C$349","Garage$C$349"]
["Garage","Range","$C$350",54.89,31.5,46.22,"two_lines","Garage","Garage$C$350","Garage$C$350"]
["Garage","Range","$C$351",54.89,31.5,46.22,"two_lines","Garage","Garage$C$351","Garage$C$351"]
["Garage","Range","$C$352",54.89,23.25,46.22,"one_line","Garage","Garage$C$352","Garage$C$352"]
["Garage","Range","$C$353",54.89,31.5,46.22,"four_lines","Garage","Garage$C$353","Garage$C$353"]
["Garage","Range","$C$356",54.89,23.25,46.22,"two_lines","Garage","Garage$C$356","Garage$C$356"]
["Garage","Range","$C$357",54.89,23.25,46.22,"two_lines","Garage","Garage$C$357","Garage$C$357"]
["Garage","Range","$C$358",54.89,23.25,46.22,"two_lines","Garage","Garage$C$358","Garage$C$358"]
["Garage","Range","$C$359",54.89,23.25,46.22,"two_lines","Garage","Garage$C$359","Garage$C$359"]
["Garage","Range","$C$360",54.89,23.25,46.22,"two_lines","Garage","Garage$C$360","Garage$C$360"]
["Garage","Range","$C$361",54.89,31.5,46.22,"two_lines","Garage","Garage$C$361","Garage$C$361"]
["Garage","Range","$C$363",54.89,31.5,46.22,"two_lines","Garage","Garage$C$363","Garage$C$363"]
["Garage","Range","$C$364",54.89,31.5,46.22,"four_lines","Garage","Garage$C$364","Garage$C$364"]
["Garage","Range","$C$365",54.89,31.5,46.22,"two_lines","Garage","Garage$C$365","Garage$C$365"]
["Garage","Range","$C$370",54.89,23.25,46.22,"two_lines","Garage","Garage$C$370","Garage$C$370"]
["Garage","Range","$C$371",54.89,23.25,46.22,"two_lines","Garage","Garage$C$371","Garage$C$371"]
["Garage","Range","$C$372",54.89,31.5,46.22,"two_lines","Garage","Garage$C$372","Garage$C$372"]
["Garage","Range","$C$373",54.89,23.25,46.22,"two_lines","Garage","Garage$C$373","Garage$C$373"]
["Garage","Range","$C$374",54.89,23.25,46.22,"two_lines","Garage","Garage$C$374","Garage$C$374"]
["Garage","Range","$C$377",54.89,47.25,46.22,"three_lines","Garage","Garage$C$377","Garage$C$377"]
["Garage","Range","$C$378",54.89,23.25,46.22,"two_lines","Garage","Garage$C$378","Garage$C$378"]
["Garage","Range","$C$379",54.89,23.25,46.22,"two_lines","Garage","Garage$C$379","Garage$C$379"]
["Garage","Range","$C$381",54.89,31.5,46.22,"two_lines","Garage","Garage$C$381","Garage$C$381"]
["Garage","Range","$C$382",54.89,31.5,46.22,"two_lines","Garage","Garage$C$382","Garage$C$382"]
["Garage","Range","$C$383",54.89,23.25,46.22,"two_lines","Garage","Garage$C$383","Garage$C$383"]
["Garage","Range","$C$384",54.89,31.5,46.22,"two_lines","Garage","Garage$C$384","Garage$C$384"]
["Garage","Range","$C$385",54.89,23.25,46.22,"two_lines","Garage","Garage$C$385","Garage$C$385"]
["Garage","Range","$C$386",54.89,23.25,46.22,"two_lines","Garage","Garage$C$386","Garage$C$386"]
["Garage","Range","$C$390",54.89,31.5,46.22,"two_lines","Garage","Garage$C$390","Garage$C$390"]
["Garage","Range","$C$391",54.89,31.5,46.22,"two_lines","Garage","Garage$C$391","Garage$C$391"]
["Garage","Range","$C$392",54.89,31.5,46.22,"two_lines","Garage","Garage$C$392","Garage$C$392"]
["Garage","Range","$C$393",54.89,31.75,46.22,"two_lines","Garage","Garage$C$393","Garage$C$393"]
["Garage","Range","$C$394",54.89,31.5,46.22,"two_lines","Garage","Garage$C$394","Garage$C$394"]
["Garage","Range","$C$396",54.89,47.25,46.22,"four_lines","Garage","Garage$C$396","Garage$C$396"]
["Garage","Range","$C$398",54.89,31.5,46.22,"two_lines","Garage","Garage$C$398","Garage$C$398"]
["Garage","Range","$C$399",54.89,31.5,46.22,"two_lines","Garage","Garage$C$399","Garage$C$399"]
["Garage","Range","$C$400",54.89,31.5,46.22,"two_lines","Garage","Garage$C$400","Garage$C$400"]
["Garage","Range","$C$401",54.89,31.5,46.22,"two_lines","Garage","Garage$C$401","Garage$C$401"]
["Garage","Range","$C$404",54.89,31.5,46.22,"two_lines","Garage","Garage$C$404","Garage$C$404"]
["Garage","Range","$C$405",54.89,31.5,46.22,"two_lines","Garage","Garage$C$405","Garage$C$405"]
["Garage","Range","$C$407",54.89,47.25,46.22,"three_lines","Garage","Garage$C$407","Garage$C$407"]
["Garage","Range","$C$408",54.89,23.25,46.22,"two_lines","Garage","Garage$C$408","Garage$C$408"]
["Garage","Range","$C$409",54.89,23.25,46.22,"two_lines","Garage",{"$f":"A1221&C1221","v":"Garage$C$409"},{"$f":"H1221&C1221","v":"Garage$C$409"}]
["Garage","Range","$C$412",54.89,23.25,46.22,"one_line","Garage","Garage$C$412","Garage$C$412"]
["Garage","Range","$C$413",54.89,47.25,46.22,"three_lines","Garage","Garage$C$413","Garage$C$413"]
["Garage","Range","$C$414",54.89,31.5,46.22,"three_lines","Garage","Garage$C$414","Garage$C$414"]
["Garage","Range","$C$415",54.89,23.25,46.22,"one_line","Garage","Garage$C$415","Garage$C$415"]
["Garage","Range","$C$418",54.89,31.5,46.22,"two_lines","Garage","Garage$C$418","Garage$C$418"]
["Garage","Range","$C$419",54.89,31.5,46.22,"two_lines","Garage","Garage$C$419","Garage$C$419"]
["Garage","Range","$C$420",54.89,31.5,46.22,"two_lines","Garage","Garage$C$420","Garage$C$420"]
["Garage","Range","$C$424",54.89,31.5,46.22,"three_lines","Garage","Garage$C$424","Garage$C$424"]
["Garage","Range","$C$425",54.89,23.25,46.22,"one_line","Garage","Garage$C$425","Garage$C$425"]
["Garage","Range","$C$426",54.89,23.25,46.22,"one_line","Garage","Garage$C$426","Garage$C$426"]
["Garage","Range","$C$427",54.89,23.25,46.22,"one_line","Garage","Garage$C$427","Garage$C$427"]
["Garage","Range","$C$428",54.89,23.25,46.22,"one_line","Garage","Garage$C$428","Garage$C$428"]
["Garage","Range","$C$429",54.89,23.25,46.22,"two_lines","Garage","Garage$C$429","Garage$C$429"]
["Garage","Range","$C$432",54.89,23.25,46.22,"two_lines","Garage","Garage$C$432","Garage$C$432"]
["Garage","Range","$C$433",54.89,31.5,46.22,"two_lines","Garage","Garage$C$433","Garage$C$433"]
["Garage","Range","$C$434",54.89,31.5,46.22,"two_lines","Garage","Garage$C$434","Garage$C$434"]
["Garage","Range","$C$435",54.89,23.25,46.22,"two_lines","Garage","Garage$C$435","Garage$C$435"]
["Garage","Range","$C$436",54.89,31.5,46.22,"two_lines","Garage","Garage$C$436","Garage$C$436"]
["Garage","Range","$C$439",54.89,31.5,46.22,"three_lines","Garage","Garage$C$439","Garage$C$439"]
["Garage","Range","$C$440",54.89,31.5,46.22,"two_lines","Garage","Garage$C$440","Garage$C$440"]
["Garage","Range","$C$443",54.89,23.25,46.22,"two_lines","Garage","Garage$C$443","Garage$C$443"]
["Garage","Range","$C$444",54.89,23.25,46.22,"one_line","Garage","Garage$C$444","Garage$C$444"]
["Garage","Range","$C$445",54.89,23.25,46.22,"two_lines","Garage","Garage$C$445","Garage$C$445"]
["Garage","Range","$C$447",54.89,23.25,46.22,"one_line","Garage","Garage$C$447","Garage$C$447"]
["User-Defined","Range","$B$1",9,54.75,12.22,75,"Défini par l’utilisateur","User-Defined$B$1","Défini par l’utilisateur$B$1"]
["User-Defined","Range","$N$3",9,54.75,28,73,"Défini par l’utilisateur","User-Defined$N$3","Défini par l’utilisateur$N$3"]
["User-Defined","Range","$B$23",9,23.75,12.22,23.75,"Défini par l’utilisateur","User-Defined$B$23","Défini par l’utilisateur$B$23"]
["REVIEW","Range","$C$1",65.78,79.5,62.56,72,"REVOIR","REVIEW$C$1","REVOIR$C$1"]
["RESULTS","Font","$A$2",16,null,12,null,"RÉSULTATS","RESULTS$A$2","RÉSULTATS$A$2"]
["RESULTS","Range","$E$11",7.56,15.5,7.56,25,"RÉSULTATS","RESULTS$E$11","RÉSULTATS$E$11"]
["RESULTS","Range","$B$68",5.73,159,5.73,154.80000000000001,"RÉSULTATS",{"$f":"A1252&C1252","v":"RESULTS$B$68"},{"$f":"H1252&C1252","v":"RÉSULTATS$B$68"}]
["SCENARIOS","Range","$D$5",23.22,15,23.22,34,"SCÉNARIOS","SCENARIOS$D$5","SCÉNARIOS$D$5"]
["SCENARIOS","Range","$E$5",23.22,15,23.22,34,"SCÉNARIOS","SCENARIOS$E$5","SCÉNARIOS$E$5"]
["SCENARIOS","Range","$F$5",23.22,15,23.22,34,"SCÉNARIOS","SCENARIOS$F$5","SCÉNARIOS$F$5"]
["SCENARIOS","Range","$G$5",23.22,15,23.22,34,"SCÉNARIOS","SCENARIOS$G$5","SCÉNARIOS$G$5"]
["SCENARIOS","Range","$H$5",23.22,15,23.22,34,"SCÉNARIOS","SCENARIOS$H$5","SCÉNARIOS$H$5"]
["SCENARIOS","Range","$B$13",15.67,27,15.67,31,"SCÉNARIOS","SCENARIOS$B$13","SCÉNARIOS$B$13"]
["SCENARIOS","Range","$B$14",15.67,27,15.67,31,"SCÉNARIOS","SCENARIOS$B$14","SCÉNARIOS$B$14"]
["SCENARIOS","Range","$B$15",15.67,27,15.67,41,"SCÉNARIOS","SCENARIOS$B$15","SCÉNARIOS$B$15"]
["SCENARIOS","Range","$B$16",15.67,27,15.67,31,"SCÉNARIOS","SCENARIOS$B$16","SCÉNARIOS$B$16"]
["SCENARIOS","Range","$B$17",15.67,27,15.67,41,"SCÉNARIOS","SCENARIOS$B$17","SCÉNARIOS$B$17"]
["SCENARIOS","Range","$B$18",15.67,30.75,15.67,31,"SCÉNARIOS","SCENARIOS$B$18","SCÉNARIOS$B$18"]
["SCENARIOS","Range","$B$19",15.67,15,15.67,31,"SCÉNARIOS","SCENARIOS$B$19","SCÉNARIOS$B$19"]
["SCENARIOS","Range","$B$20",15.67,15,15.67,31,"SCÉNARIOS","SCENARIOS$B$20","SCÉNARIOS$B$20"]
["SCENARIOS","Range","$B$21",15.67,15,15.67,25.5,"SCÉNARIOS","SCENARIOS$B$21","SCÉNARIOS$B$21"]
["SCENARIOS","Range","$B$22",15.67,15,15.67,31,"SCÉNARIOS","SCENARIOS$B$22","SCÉNARIOS$B$22"]
["SCENARIOS","Range","$B$23",15.67,15,15.67,31,"SCÉNARIOS","SCENARIOS$B$23","SCÉNARIOS$B$23"]
["SCENARIOS","Range","$B$26",15.67,29.25,15.67,44,"SCÉNARIOS","SCENARIOS$B$26","SCÉNARIOS$B$26"]
["Footings & Slabs","Button","Rounded Rectangle 2||Rectangle: Rounded Corners 2",189.375,37.674169999999997,170.81,57.18,null,"Footings & SlabsRounded Rectangle 2||Rectangle: Rounded Corners 2","Rounded Rectangle 2||Rectangle: Rounded Corners 2"]
["Foundation Walls","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"Foundation WallsRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Structural Elements","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"Structural ElementsRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Ext. Walls","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"Ext. WallsRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Ext. Wall Systems","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"Ext. Wall SystemsRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Party Walls","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"Party WallsRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Cladding","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"CladdingRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Windows","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"WindowsRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Int. Walls","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"Int. WallsRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Floors","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"FloorsRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Ceilings","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"CeilingsRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Roof","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"RoofRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["Garage","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"GarageRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]
["User-Defined","Button","Rounded Rectangle 1||Rectangle: Rounded Corners 1",189.375,37.674169999999997,234.5625,37.674169999999997,null,"User-DefinedRounded Rectangle 1||Rectangle: Rounded Corners 1","Rounded Rectangle 1||Rectangle: Rounded Corners 1"]

{"sheet":"Master sheet","index":30,"n_rows":441,"n_cols":54,"rows_kept":441,"cut":false,"hidden":true,"merged":[]}
["Product","Material","Company (EPD Commissioner)","Brand","Spec's","CSI #","Category","Notes","Country of Mfr","NRCan","Stated EPD kgCO2e / unit","EPD units kgCO2e per","Common Emissions kgCO2e/unit","Units: kgCO2e per","EPD #","Verifying agency","Exp. Year","Density","Units","Addn'l factors","Units","R-value/inch","Thermal Cond. (k) for RSI","Units","Biogenic carbon factor","% Carbon content (kgC/kg)","Biogenic Storage kgCO2/unit","Units: kgCO2e per","WWF Storage Factor kgCO2/kgC","Carbon content kgC/unit","Units","Biogenic CO2 kg - full C value","Height (m)","Length (m)","Width (m)","Unit Volume (m3)","Units/m2","Product ID","MPa","Product ID per MPa & Province","-","EPD Note","Biogenic Storage Adjustment Factor","Province Match","Province 1","Province 1 - French","Province 2","Province 2 - French","Province 3","Province 3 - French","Province 4","Province 4 - French","Province 5","Province 5 - French"]
[{"$f":"B2&\" / \"&C2&\" / \"&D2&\" / \"&E2","v":"ACQ wood treatment /  /  / "},"ACQ wood treatment",null,null,null,null,null,null,"USA & CAN",null,174,"1000 BF",{"$f":"(K2/T2)","v":0.8029533917858791},"m2 surface area","Bolin & Smith, 2011, LCA Assessment of ACQ-treated lumber, Journal of Cleaner Production",null,"",null,null,216.7,"m2 surface area/1000 BF",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1,null,null,null,"Peer-reviewed LCA, 2011",0.9,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS2:$BB2,0))","v":false}]
[{"$f":"B3&\" / \"&C3&\" / \"&D3&\" / \"&E3","v":"Adobe block /  / 8\" block wall / Avg of site made and factory made (Cyprus)"},"Adobe block",null,"8\" block wall","Avg of site made and factory made (Cyprus)",null,null,"Avg of site made and factory made","Cyprus",null,6.6449999999999999E-3,"kg",{"$f":"(T3*K3)","v":2.0254538114999998},"m2 at 8 \" block","Christoforou et al LCA, 2016, Journal of Cleaner Production",null,"",1500,"kg/m3",{"$f":"24.22*12.585","v":304.80869999999999},"24.22 blocks/m2 * 12.585 kg/block",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2,null,null,null,"Peer-reviewed LCA, 2016",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS3:$BB3,0))","v":false}]
["Aerogel blanket / Aspen Aerogels /  / R9.6/inch, White/Grey blanket","Aerogel blanket","Aspen Aerogels",null,"R9.6/inch, White/Grey blanket",null,null,null,"USA",null,12.3,"1m2 @ 10 mm",{"$f":"(K4/0.01*W4)","v":18.45},"m2-RSI1","S-P-00725 ","Renuables",2020,150,"kg/m3",null,null,{"$f":"1/W4*0.0254*5.678","v":9.614746666666667},1.4999999999999999E-2,"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,3,null,null,null,{"$f":"IF(LEN(Q4)=4,IF(Q4<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q4),\"\"),\"\")","v":"Expired 2020"},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS4:$BB4,0))","v":false}]
[{"$f":"B5&\" / \"&C5&\" / \"&D5&\" / \"&E5","v":"Aggregate /  /  / Avg construction aggregate (gravel & sand)"},"Aggregate",null,null,"Avg construction aggregate (gravel & sand)",null,null,null,"USA",null,9.52,"MT",{"$f":"((K5*R5)/1000)","v":16.012640000000001},"m2 at 0.0254 m (1\")","NRMCAEPD: 10020 ","Athena",2023,1682,"kg/m3",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,4,null,null,null,{"$f":"IF(LEN(Q5)=4,IF(Q5<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q5),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS5:$BB5,0))","v":false}]
[{"$f":"B6&\" / \"&C6&\" / \"&D6&\" / \"&E6","v":"Aggregate / Kangley Rock & Recycling /  / Avg construction aggregate (gravel & sand)"},"Aggregate","Kangley Rock & Recycling",null,"Avg construction aggregate (gravel & sand)",null,null,null,"USA",null,5.07,"MT",8.5277399999999997,"m2 at 0.0254 m (1\")","EPD-079","ASTM",2023,1682,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS6:$BB6,0))","v":false}]
[{"$f":"B7&\" / \"&C7&\" / \"&D7&\" / \"&E7","v":"Aggregate / Martin Marietta /  / Avg construction aggregate (gravel & sand)"},"Aggregate","Martin Marietta",null,"Avg construction aggregate (gravel & sand)",null,null,null,"USA",null,2.57,"MT",4.3227399999999996,"m2 at 0.0254 m (1\")","EPD-063","ASTM",2022,1682,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,6,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS7:$BB7,0))","v":false}]
[{"$f":"B8&\" / \"&C8&\" / \"&D8&\" / \"&E8","v":"Aggregate / Polaris Mtls Corp. /  / Avg construction aggregate (gravel & sand)"},"Aggregate","Polaris Mtls Corp.",null,"Avg construction aggregate (gravel & sand)",null,null,null,"CAN",null,1.58,"MT",2.6575600000000001,"m2 at 0.0254 m (1\")","EPD-059 ","ASTM",2022,1682,"kg/m3",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,7,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS8:$BB8,0))","v":false}]
[{"$f":"B9&\" / \"&C9&\" / \"&D9&\" / \"&E9","v":"Aggregate / Vulcan Mtls Co. /  / Avg construction aggregate (gravel & sand)"},"Aggregate","Vulcan Mtls Co.",null,"Avg construction aggregate (gravel & sand)",null,null,null,"USA",null,5.7,"MT",{"$f":"((K9*R9)/1000)","v":9.5873999999999988},"m2 at 0.0254 m (1\")","No number","Climate Earth",2021,1682,"kg/m3",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,8,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS9:$BB9,0))","v":false}]
["Air barrier / Dupont / Tyvek Fluid Applied Weather Barrier System - All components / 25 Perms","Air barrier","Dupont","Tyvek Fluid Applied Weather Barrier System - All components","25 Perms",null,null,null,"USA",null,3.5,"m2",{"$f":"(3.5)","v":3.5},"m2","4787059050.101.1 ","UL Env.",2022,0.89900000000000002,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,9,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS10:$BB10,0))","v":false}]
["Air barrier / Dupont / Tyvek HomeWrap / 54 Perms","Air barrier","Dupont","Tyvek HomeWrap","54 Perms",null,null,null,"USA",null,0.49,"m2",{"$f":"(0.49)","v":0.49},"m2","4787059050.102.1 ","UL Env.",2022,0.11,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,10,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS11:$BB11,0))","v":false}]
["Air barrier / GCP / Perm-a-Barrier VPL liquid applied permeable barrier / 15 Perms, 40 mils thickness","Air barrier","GCP","Perm-a-Barrier VPL liquid applied permeable barrier","15 Perms, 40 mils thickness",null,null,null,"USA",null,3.8,"m2",{"$f":"(3.8)","v":3.8},"m2","EPD-074","ASTM",2022,2.4169999999999998,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,1.016E-3,null,null,null,null,11,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS12:$BB12,0))","v":false}]
["Asphalt Shingles / Includes: Atlas, BP, CertainTeed, GAF, IKO, Malarkey, Owens Corning, Pabco /  / ","Asphalt Shingles","Includes: Atlas, BP, CertainTeed, GAF, IKO, Malarkey, Owens Corning, Pabco",null,null,null,null,"Incl. underlayment","USA & CAN",null,5.0999999999999996,"m2",{"$f":"(5.1)","v":5.0999999999999996},"m2","4787168709.101.1 ","UL Env.",2021,12.7,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,12,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS13:$BB13,0))","v":false}]
["Asphalt Shingles / GAF / Timberline / Timberline","Asphalt Shingles","GAF","Timberline","Timberline",null,null,"Installed","USA",null,3.88,"m2",{"$f":"(3.88)","v":3.88},"m2","EPD10397 ","NSF",2025,9.83,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,13,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS14:$BB14,0))","v":false}]
["Asphalt Shingles / Owens Corning / Duration / ","Asphalt Shingles","Owens Corning","Duration",null,null,null,null,"USA",null,3.49,"m2",{"$f":"(3.49)","v":3.49},"m2","4789400789.101.1 ","UL Env.",2025,10.119999999999999,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,14,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS15:$BB15,0))","v":false}]
["Asphalt Shingles / Owens Corning / Oakridge / ","Asphalt Shingles","Owens Corning","Oakridge",null,null,null,null,"USA",null,3.21,"m2",{"$f":"(3.21)","v":3.21},"m2","4789400789.101.3","UL Env.",2025,9.93,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS16:$BB16,0))","v":false}]
["Asphalt Shingles / Owens Corning / Supreme / ","Asphalt Shingles","Owens Corning","Supreme",null,null,null,null,"USA",null,2.75,"m2",{"$f":"(2.75)","v":2.75},"m2","4789400789.101.2","UL Env.",2025,9.26,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS17:$BB17,0))","v":false}]
["Bamboo plywood / Smith & Fong / Plyboo / 1/2\" (12.7 mm)","Bamboo plywood","Smith & Fong","Plyboo","1/2\" (12.7 mm)",null,null,null,"China",null,3.6,"kg",{"$f":"(T18*K18)","v":31.546800000000001},"m2 at 0.0127 m (1/2\")","EPD-072","ASTM",2022,690,"kg/m3",{"$f":"R18*0.0127","v":8.7629999999999999},"kg/m2 at 0.0127 m",null,null,null,0.98,0.47199999999999998,{"$f":"(44/12*AD18)*rng_biogenic_storage","v":13.376263824},"m2 at 0.0127 m",1.7,{"$f":"T18*Y18*Z18","v":4.05341328},null,null,null,null,null,null,null,17,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS18:$BB18,0))","v":false}]
["BioBased Tile / Armstrong / BioBased Tile / Non-PVC with BioStride polyester binder, Striations BBT and Migrations BBT","BioBased Tile","Armstrong","BioBased Tile","Non-PVC with BioStride polyester binder, Striations BBT and Migrations BBT",null,null,null,"USA",null,4.55,"m2",{"$f":"(4.55)","v":4.55},"m2","EPD-003","ASTM",2024,7.03,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,3.1749999999999999E-3,null,null,null,null,18,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS19:$BB19,0))","v":false}]
["Brick, Calcium Silicate / Arriscraft / Contemporary Brick / 3-1/8\" x 3-1/2\" x any length, incl. mortar and ties","Brick, Calcium Silicate","Arriscraft","Contemporary Brick","3-1/8\" x 3-1/2\" x any length, incl. mortar and ties",null,null,"EPD included mortar and ties","CAN",null,280,"9.29m2",{"$f":"(K20/9.29)","v":30.139935414424116},"m2","EPD-055","ASTM",2021,2082,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,7.9000000000000001E-2,0.254,0.09,null,null,19,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS20:$BB20,0))","v":false}]
["Brick, Cement / MidWest / Architectural Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar","Brick, Cement","MidWest","Architectural Face Brick","3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar",null,null,null,"USA",null,419,"m3",{"$f":"((0.83*K21+0.17*R21)*AI21)","v":36.201999999999998},"m2","EPD10051","NSF",2020,269,"kgCO2/m3 mortar",null,"83% brick, 17% mortar",null,null,null,null,null,null,null,null,null,null,null,7.0000000000000007E-2,0.19367500000000001,9.1999999999999998E-2,{"$f":"AG21*AH21*AI21","v":1.247267E-3},null,20,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS21:$BB21,0))","v":false}]
["Brick, Clay / Interstate / Avg Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar","Brick, Clay","Interstate","Avg Face Brick","3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar",null,null,"Avg of 10 colors & 2 kilns","USA",null,566.85,"m3",{"$f":"((0.83*K22+0.17*R22)*AI22)","v":47.491826000000003},"m2","EPD-131","ASTM",2025,269,"kgCO2/m3 mortar",null,"83% brick, 17% mortar",null,null,null,null,null,null,null,null,null,null,null,7.0000000000000007E-2,0.19367500000000001,9.1999999999999998E-2,{"$f":"AG22*AH22*AI22","v":1.247267E-3},null,21,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS22:$BB22,0))","v":false}]
["Brick, Clay / Interstate / Avg Thin Face Brick / 3-9/16\" x 5/8\" x 11-5/8\" (90 x 16 mm x 295) incl. 3/8\" mortar","Brick, Clay","Interstate","Avg Thin Face Brick","3-9/16\" x 5/8\" x 11-5/8\" (90 x 16 mm x 295) incl. 3/8\" mortar",null,null,"Avg of 10 colors & 2 kilns","USA",null,755.85,"m3",{"$f":"((0.87*K23+0.13*R23)*AI23+0.01*R23)","v":13.770952000000001},"m2","EPD-132","ASTM",2025,269,"kgCO2/m3 mortar",null,"87% brick, 13% mortar, plus 100% surface mortar @ 10mm",null,null,null,null,null,null,null,null,null,null,null,0.09,0.29527500000000001,1.6E-2,{"$f":"AG23*AH23*AI23","v":4.2519600000000003E-4},null,22,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS23:$BB23,0))","v":false}]
["Brick, Clay, Generic Modular / Brick Industry Association / US-Canada Industry Average / 3-5/8\" x 2-3/4\" x 7-5/8\" incl. 3/8\" mortar","Brick, Clay, Generic Modular","Brick Industry Association","US-Canada Industry Average","3-5/8\" x 2-3/4\" x 7-5/8\" incl. 3/8\" mortar",null,null,null,"USA & CAN",null,503,"m3 of brick",{"$f":"((0.83*K24+0.17*R24)*AI24)","v":47.248439999999995},"m2","EPD10447","PRé Consultants",2025,269,"kgCO2/m3 mortar",null,"83% brick, 17% mortar",null,null,null,null,null,null,null,null,null,null,null,7.0000000000000007E-2,0.20300000000000001,0.10199999999999999,{"$f":"AG24*AH24*AI24","v":1.4494200000000001E-3},null,23,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS24:$BB24,0))","v":false}]
["Brick, Clay / Brick Industry Association / US-Canada Industrywide Average / ","Brick, Clay","Brick Industry Association","US-Canada Industrywide Average",null,null,null,"Use outer dimensions of brick, ignore voids","USA & CAN",null,503,"m3 of brick",{"$f":"(503)","v":503},"m3","EPD10447","PRé Consultants",2025,2120,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,24,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS25:$BB25,0))","v":false}]
[{"$f":"B26&\" / \"&C26&\" / \"&D26&\" / \"&E26","v":"Carpet /  /  / Average from 150 samples in the EC3 database"},"Carpet",null,null,"Average from 150 samples in the EC3 database",null,null,null,"USA & CAN",null,13.3,"m2",{"$f":"(13.3)","v":13.3},"m2","EC3",null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,null,null,null,"Multi-EPD average from EC3 Tool",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS26:$BB26,0))","v":false}]
[{"$f":"B27&\" / \"&C27&\" / \"&D27&\" / \"&E27","v":"Carpet /  / Achievable from EC3 / Achievable from 150 samples in the EC3 database"},"Carpet",null,"Achievable from EC3","Achievable from 150 samples in the EC3 database",null,null,null,"USA & CAN",null,8.3000000000000007,"m2",{"$f":"(8.3)","v":8.3000000000000007},"m2","EC3",null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,26,null,null,null,"Multi-EPD average from EC3 Tool",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS27:$BB27,0))","v":false}]
[{"$f":"B28&\" / \"&C28&\" / \"&D28&\" / \"&E28","v":"Carpet /  / Conservative from EC3 / Conservative from 150 samples in the EC3 database"},"Carpet",null,"Conservative from EC3","Conservative from 150 samples in the EC3 database",null,null,null,"USA & CAN",null,17.399999999999999,"m2",{"$f":"(17.4)","v":17.399999999999999},"m2","EC3",null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,27,null,null,null,"Multi-EPD average from EC3 Tool",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS28:$BB28,0))","v":false}]
[{"$f":"B29&\" / \"&C29&\" / \"&D29&\" / \"&E29","v":"Carpet / Interface / GLASBAC®RE, Nylon / Modular tile carpet (closed loop recycling)"},"Carpet","Interface","GLASBAC®RE, Nylon","Modular tile carpet (closed loop recycling)",null,null,null,"USA",null,4.4000000000000004,"m2",{"$f":"(4.4)","v":4.4000000000000004},"m2","4787521006.104.1","UL Env.",2021,4.13,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,28,null,null,null,{"$f":"IF(LEN(Q29)=4,IF(Q29<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q29),\"\"),\"\")","v":"Expired 2021"},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS29:$BB29,0))","v":false}]
[{"$f":"B30&\" / \"&C30&\" / \"&D30&\" / \"&E30","v":"Carpet / Interface / Cquest BioX / 1.5 mm Modular tile carpet"},"Carpet","Interface","Cquest BioX","1.5 mm Modular tile carpet",null,null,null,"USA",null,-0.25600000000000001,"m2",{"$f":"(AA30-0.256)","v":4.0910000000000002},"m2","4788873607.102.1","UL Env.",2025,2.8,"kg/m2",null,null,null,null,null,null,null,{"$f":"(4.83)*rng_biogenic_storage","v":4.3470000000000004},"m2",null,null,null,null,null,null,null,null,null,29,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS30:$BB30,0))","v":false}]
["Cedar Shingles/shakes /  /  / 3/4\" coverage","Cedar Shingles/shakes",null,null,"3/4\" coverage",null,null,"Wood biogenic carbon storage set to zero",null,null,213.52,"1000 BF",{"$f":"((K31*AG31)/T31)","v":1.723540677966102},"m2 at 0.01905 m (3/4\")","2016-06-01","FPInnovations",2021,209,"kg/m3",2.36,"m3/1000 BF",{"$f":"R31*0.01905","v":3.9814500000000002},"kg/m2 at 0.01905 (3/4\")",null,1,0.5,null,"m2 at 3/4\"",0.82499999999999996,{"$f":"V31*Y31*Z31","v":1.9907250000000001},"kgC/m2",null,1.9050000000000001E-2,null,null,null,null,30,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS31:$BB31,0))","v":false}]
["Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards","Cedar Siding","Western Red Cedar Lumber Assn",null,"1 x 6 Boards",null,null,null,"CAN",null,213.52,"1000 BF",{"$f":"((K32*AG32)/T32)","v":1.723540677966102},"m2 at 0.01905 m (3/4\")","2016-06-01","FPInnovations",2021,209,"kg/m3",2.36,"m3/1000 BF",{"$f":"R32*0.01905","v":3.9814500000000002},"kg/m2 at 0.01905 (3/4\")",null,1,0.5,null,"m2 at 0.01905 m (3/4\")",1.26,{"$f":"V32*Y32*Z32","v":1.9907250000000001},"kgC/m2",null,1.9050000000000001E-2,null,null,null,null,31,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS32:$BB32,0))","v":false}]
[{"$f":"B33&\" / \"&C33&\" / \"&E33&\" / \"&D33","v":"Cellulose - batt / CMS / R 3.6/inch / EcoCell"},"Cellulose - batt","CMS","EcoCell","R 3.6/inch",null,null,null,"USA",null,0.48699999999999999,"m2 RSI 1",{"$f":"(0.487)","v":0.48699999999999999},"m2 RSI 1","CIM – 20191223 – 003","Sustainable Minds",2024,40,"kg/m3",1.6,"kg/m2 at RSI1",3.6,null,null,0.86,0.5,{"$f":"(AD33*44/12)*rng_biogenic_storage","v":2.2704000000000004},"m2 RSI 1",1.84,{"$f":"T33*Y33*Z33","v":0.68800000000000006},null,null,null,null,null,null,null,32,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS33:$BB33,0))","v":false}]
[{"$f":"B34&\" / \"&C34&\" / \"&E34&\" / \"&D34","v":"Cellulose - dense pack /  / R 3.7/inch / Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},"Cellulose - dense pack",null,"Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool","R 3.7/inch",null,null,null,"USA & CAN",null,0.48699999999999999,"m2 RSI 1",{"$f":"(K34*T34/T35)","v":0.97399999999999998},"m2 RSI 1","CIM – 20191223 – 002","Sustainable Minds",2024,56,"kg/m3",2.1840000000000002,"kg/m2 at RSI1",3.7,null,null,0.86,0.5,{"$f":"(AD34*44/12)*rng_biogenic_storage","v":3.0990960000000003},"m2 RSI 1",1.84,{"$f":"T34*Y34*Z34","v":0.93912000000000007},null,null,null,null,null,null,null,33,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS34:$BB34,0))","v":false}]
[{"$f":"B35&\" / \"&C35&\" / \"&E35&\" / \"&D35","v":"Cellulose - loose fill /  / R 3.7/inch / Includes: AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},"Cellulose - loose fill",null,"Includes: AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool","R 3.7/inch",null,null,"0.04 m at RSI 1 avg of 12 companies","USA & CAN",null,0.48699999999999999,"m2 RSI 1",{"$f":"(0.487)","v":0.48699999999999999},"m2 RSI 1","CIM – 20191223 – 001 ","Sustainable Minds",2024,28,"kg/m3",1.0920000000000001,"kg/m2 at RSI1",3.7,null,null,0.86,0.5,{"$f":"(AD35*44/12)*rng_biogenic_storage","v":1.5495480000000001},"m2 RSI 1",1.84,{"$f":"T35*Y35*Z35","v":0.46956000000000003},null,null,null,null,null,null,null,34,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS35:$BB35,0))","v":false}]
[{"$f":"B36&\" / \"&E36&\" / \"&C36&\" / \"&D36","v":"Cellulose - spray applied / R 3.75/inch / International Cellulose Corp. / K-13, ThermoCon"},"Cellulose - spray applied","International Cellulose Corp.","K-13, ThermoCon","R 3.75/inch",null,null,"0.0384 m at RSI 1",null,null,0.32500000000000001,"m2 RSI 1",{"$f":"(0.325)","v":0.32500000000000001},"m2 RSI 1","ICC – 20200122– 001","Sustainable Minds",2025,54.5,"kg/m3",2.0710000000000002,"kg/m2 at RSI1",3.75,null,null,0.71,0.5,{"$f":"(AD36*44/12)*rng_biogenic_storage","v":2.4261765},"m2 RSI 1",1.84,{"$f":"T36*Y36*Z36","v":0.735205},null,null,null,null,null,null,null,35,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS36:$BB36,0))","v":false}]
["Cement board 1/2\" / USG / Durock (132) / 1/2\" (12.7 mm)","Cement board 1/2\"","USG","Durock (132)","1/2\" (12.7 mm)",null,null,null,"USA",null,912,"92.9m2",{"$f":"(K37/92.9)","v":9.817007534983853},"m2","EPD-132","ASTM",2025,921,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,36,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS37:$BB37,0))","v":false}]
["Cement board 1/2\" / USG / Durock (133) / 1/2\" (12.7 mm)","Cement board 1/2\"","USG","Durock (133)","1/2\" (12.7 mm)",null,null,null,"USA",null,841,"92.9m2",{"$f":"(K38/92.9)","v":9.0527448869752423},"m2","EPD-133","ASTM",2025,921,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,37,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS38:$BB38,0))","v":false}]
["Cement mortar, tile / Tile Council of North America /  / Industry average. Includes dry-set, modified dry-set and improved modified dry-set cement mortar","Cement mortar, tile","Tile Council of North America",null,"Industry average. Includes dry-set, modified dry-set and improved modified dry-set cement mortar",null,null,null,"USA & CAN",null,0.51900000000000002,"m2",{"$f":"(0.519)","v":0.51900000000000002},"m2","4787109018.102.1 ","UL Env.",2021,4.07,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,38,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS39:$BB39,0))","v":false}]
["Ceramic tile / Crossville / Porcelain / Standard grade","Ceramic tile","Crossville","Porcelain","Standard grade",null,null,null,"USA",null,23.9,"m2",{"$f":"(23.9)","v":23.9},"m2","4788863727.101.1 ","UL Env.",2024,24.41,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,39,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS40:$BB40,0))","v":false}]
["Ceramic tile / StonePeak / Porcelain / Porcelain, standard grade","Ceramic tile","StonePeak","Porcelain","Porcelain, standard grade",null,null,null,"USA",null,16.22,"m2",{"$f":"(16.22)","v":16.22},"m2","4786822856.101.1 ","UL Env.",2020,22,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,8.5000000000000006E-3,null,null,null,null,40,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS41:$BB41,0))","v":false}]
["Ceramic tile / Tile Council of North America /  / Industry average. Includes porcelain, pressed, mosaic and quarry tile","Ceramic tile","Tile Council of North America",null,"Industry average. Includes porcelain, pressed, mosaic and quarry tile",null,null,null,"USA & CAN",null,13.14,"m2",{"$f":"(13.14)","v":13.14},"m2","4786483078.101.1 ","UL Env.",2020,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,41,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS42:$BB42,0))","v":false}]
["Clay plaster / Site mixed /  / 15 mm","Clay plaster","Site mixed",null,"15 mm",null,null,null,"EU",null,0.88,"m2 at 15mm",{"$f":"(0.88)","v":0.88},"m2 at 15mm","Melia et al LCA, 2014",null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,42,null,null,null,"Peer-reviewed LCA, 2014",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS43:$BB43,0))","v":false}]
["Clay roof tiles / HISPALYT /  / ","Clay roof tiles","HISPALYT",null,null,null,null,null,"EU",null,3.55,"m2",{"$f":"(3.55)","v":3.55},"m2","008-001","GlobalEPD",2022,56,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,43,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS44:$BB44,0))","v":false}]
["CMU - Light weight / Angelus Block Co. / 8\" Light weight blocks / 9 x 8 x 16 Precision","CMU - Light weight","Angelus Block Co.","8\" Light weight blocks","9 x 8 x 16 Precision",null,null,"Avg of 2000, 2800 & 3750 psi","USA",null,214.25,"m3",{"$f":"(K45*T45/R45)","v":19.487945205479452},"m2 at 8\" block thickness","EPD-011","ASTM",2021,1825,"kg/m3",166,"kg/m2 of wall",null,null,null,null,null,null,null,null,null,null,null,0.19,0.39,0.19,null,null,44,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS45:$BB45,0))","v":false}]
["CMU - Light weight / Brampton Brick / 8\" Carbon Cure Lightweight blocks / Carbon Cure 15 MPa","CMU - Light weight","Brampton Brick","8\" Carbon Cure Lightweight blocks","Carbon Cure 15 MPa",null,null,null,"CAN",null,387.9,"m3",35.282958904109584,"m2 at 8\" block thickness",null,"CarbonCure",2020,1825,"kg/m3",166,"kg/m2 of wall",null,null,null,null,null,null,null,null,null,null,null,0.19,0.39,0.19,null,null,45,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS46:$BB46,0))","v":false}]
["CMU - Light weight / Canadian Concrete Masonry Producers Assn / 8\" Light weight blocks / 390 x 190 x 190 mm","CMU - Light weight","Canadian Concrete Masonry Producers Assn","8\" Light weight blocks","390 x 190 x 190 mm",null,null,"Avg of East and West region","CAN",null,195.24,"m3",18.814926620843398,"m2 at 8\" block thickness","EPD 338","ASTM",2027,1722.56,"kg/m3",166,"kg/m2 of wall",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,46,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS47:$BB47,0))","v":false}]
["(ARCHIVED 2023) CMU - Light weight / Canadian Concrete Masonry Producers Assn / 8\" Light weight blocks / 391 x 190 x 190 mm","(ARCHIVED 2023) CMU - Light weight","Canadian Concrete Masonry Producers Assn","8\" Light weight blocks","391 x 190 x 190 mm",null,null,null,"CAN",null,270,"m3",24.55890410958904,"m2 at 8\" block thickness","EPD-043","ASTM",2022,1825,"kg/m3",166,"kg/m2 of wall",null,null,null,null,null,null,null,null,null,null,null,0.19,0.39,0.19,null,null,"46_Archived",null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS48:$BB48,0))","v":false}]
["CMU - Normal weight / Angelus Block Co. / 8\" Normal weight blocks / 8 x 8 x 16 Precision","CMU - Normal weight","Angelus Block Co.","8\" Normal weight blocks","8 x 8 x 16 Precision",null,null,"Avg of 2000, 2800 & 3750 psi","USA",null,194.67,"m3",16.525320000000001,"m2 at 8\" block thickness","EPD-010","ASTM",2020,2250,"kg/m3",191,"kg/m2 of wall",null,null,null,null,null,null,null,null,null,null,null,0.19,0.39,0.19,null,null,47,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS49:$BB49,0))","v":false}]
["CMU - Normal weight / Canadian Concrete Masonry Producers Assn / 8\" Normal weight blocks / 390 x 190 x 190 mm","CMU - Normal weight","Canadian Concrete Masonry Producers Assn","8\" Normal weight blocks","390 x 190 x 190 mm",null,null,"Avg of East and West region","CAN",null,228.51,"m3",19.965878316559927,"m2 at 8\" block thickness","EPD 338","ASTM",2027,2186,"kg/m3",191,"kg/m2 of wall",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,48,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS50:$BB50,0))","v":false}]
["(ARCHIVED 2023) CMU - Normal weight / Canadian Concrete Masonry Producers Assn / 8\" Normal weight blocks / 390 x 190 x 190 mm","(ARCHIVED 2023) CMU - Normal weight","Canadian Concrete Masonry Producers Assn","8\" Normal weight blocks","390 x 190 x 190 mm",null,null,null,"CAN",null,260,"m3",22.071111111111112,"m2 at 8\" block thickness","EPD-042","ASTM",2021,2250,"kg/m3",191,"kg/m2 of wall",null,null,null,null,null,null,null,null,null,null,null,0.19,0.39,0.19,null,null,"48_Archived",null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS51:$BB51,0))","v":false}]
["CMU - Normal weight / Permacon / 8\" Normal weight blocks / NW STD 20CM GLPW","CMU - Normal weight","Permacon","8\" Normal weight blocks","NW STD 20CM GLPW",null,null,null,"CAN",null,209,"m3",17.741777777777777,"m2 at 8\" block thickness","7135-8939","CSA",2021,2250,"kg/m3",191,"kg/m2 of wall",null,null,null,null,null,null,null,null,null,null,null,0.19,0.39,0.19,null,null,49,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS52:$BB52,0))","v":false}]
["CMU - Rammed earth / Watershed Materials / Watershed Block / ","CMU - Rammed earth","Watershed Materials","Watershed Block",null,null,null,"4% cement ","USA",null,1.284,"block",{"$f":"(K53*T53)","v":15.549239999999999},"m2 at 8\" block thickness","LCA Dahmen & Kim, UBC",null,"",2100,"kg/m3",12.11,"blocks/m2",null,null,null,null,null,null,null,null,null,null,null,0.19,0.39,0.19,null,null,50,null,null,null,"Peer-reviewed LCA",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS53:$BB53,0))","v":false}]
["CMU - Rammed earth / Watershed Materials / Watershed ZeroBlock / ","CMU - Rammed earth","Watershed Materials","Watershed ZeroBlock",null,null,null,"0% cement","USA",null,0.98199999999999998,"block",{"$f":"(K54*T54)","v":11.892019999999999},"m2 at 8\" block thickness","LCA Dahmen & Kim, UBC",null,"",2100,"kg/m3",12.11,"blocks/m2",null,null,null,null,null,null,null,null,null,null,null,0.19,0.39,0.19,null,null,51,null,null,null,"Peer-reviewed LCA",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS54:$BB54,0))","v":false}]
[{"$f":"B55&\" / \"&C55&\" / \"&D55&\" / \"&E55","v":"Earthen Floor / Site made /  / 3\" cob, 1\" clay plaster"},"Earthen Floor","Site made",null,"3\" cob, 1\" clay plaster",null,null,"Adapted by Erik Bowden from cob wall LCA study data","USA",null,3.45,"m2",{"$f":"(K55)","v":3.45},"m2","Ben-Alon et al LCA, 2019",null,"",168.2,"kg/m2",1.8,"kg straw/m2",null,null,null,1,0.47,{"$f":"(T55*Z55*44/12)*rng_biogenic_storage","v":2.7917999999999998},null,null,null,null,null,1,1,0.10199999999999999,null,null,52,null,null,null,"Adapted from peer-reviewed LCA, 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS55:$BB55,0))","v":false}]
["Cob wall / Site mixed /  / 18\" (457 mm) avg. thickness","Cob wall","Site mixed",null,"18\" (457 mm) avg. thickness",null,null,null,"USA",null,13.2,"m2",{"$f":"(13.12)","v":13.12},"m2 at 457 mm","Ben-Alon et al LCA, 2019",null,"",1222,"kg/m3",10.1,"kg straw/m2",null,null,null,1,0.47,{"$f":"(T56*Z56*44/12)*rng_biogenic_storage","v":15.665099999999999},null,null,null,null,null,1,1,0.45700000000000002,null,null,53,null,null,null,"Peer-reviewed LCA, 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS56:$BB56,0))","v":false}]
["Compressed earth block / Factory made / Stabilized with 6.5% NHL / 31.5 x 6 x 2.75 \" (300 x 150 x 70 mm)","Compressed earth block","Factory made","Stabilized with 6.5% NHL","31.5 x 6 x 2.75 \" (300 x 150 x 70 mm)",null,null,null,"EU",null,0.38800000000000001,"block",{"$f":"(K57*T57)","v":8.6222222222222218},"m2 at 6\" block","Fernandes et al LCA, 2019",null,"",1900,"kg/m3",{"$f":"1/0.045","v":22.222222222222221},"blocks/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,54,null,null,null,"Peer-reviewed LCA, 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS57:$BB57,0))","v":false}]
["Compressed straw board / Stramit / 60 mm board / R 3.9/inch","Compressed straw board","Stramit","60 mm board","R 3.9/inch",null,null,null,"EU",null,0.59,"m2",{"$f":"(K58)","v":0.59},{"$f":"L58","v":"m2"},"Stramit LCA, 2019",null,"",23,"kg/m2 at 60mm",1.4,"kgCO2/kg storage",3.9,null,null,1,0.47,{"$f":"(38.5)*rng_biogenic_storage","v":34.65},"m2 at 60mm",null,null,null,null,null,null,null,null,null,55,null,null,null,"Peer-reviewed LCA, 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS58:$BB58,0))","v":false}]
[{"$f":"B59&\" / \"&C59&\" / \"&D59&\" / \"&E59","v":"Concrete / Butler Concrete / Avg of 19 different 25 Mpa mixes / "},"Concrete","Butler Concrete","Avg of 19 different 25 Mpa mixes",null,null,null,null,"CAN",null,189,"m3",{"$f":"(189)","v":189},"m3","07/26/2020","ASTM",2025,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,56,"0-25",null,null,{"$f":"IF(LEN(Q59)=4,IF(Q59<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q59),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS59:$BB59,0))","v":false}]
["Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / ","Concrete - 0-25 MPa, Industry Average Benchmark","CRMCA","Can. Avg.",null,null,null,"Mix #3","CAN","2021-02-04",304.52,"m3",{"$f":"(K60)","v":304.52},"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,57,"0-25",1,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS60:$BB60,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / ","Concrete - 0-25 MPa, 0-14% FA/SL, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #1 with and #2 without air","CAN","2021-02-04",{"$f":"AVERAGE(327.33,313.45)","v":320.39},"m3",320.39,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,58,"0-25",2,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS61:$BB61,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / ","Concrete - 0-25 MPa, 15-29% Fly Ash, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #4 with and #6 without air","CAN","2021-02-04",{"$f":"AVERAGE(295.2,283.03)","v":289.11500000000001},"m3",289.11500000000001,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,59,"0-25",3,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS62:$BB62,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / ","Concrete - 0-25 MPa, 30-40% Fly Ash, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #8 with and #10 without air","CAN","2021-02-04",{"$f":"AVERAGE(260.47,250.14)","v":255.30500000000001},"m3",255.30500000000001,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60,"0-25",4,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS63:$BB63,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / ","Concrete - 0-25 MPa, 25-34% Slag, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #12 with and #14 without air","CAN","2021-02-04",{"$f":"AVERAGE(267.59,256.89)","v":262.24},"m3",262.24,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,61,"0-25",5,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS64:$BB64,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / ","Concrete - 0-25 MPa, 35-50% Slag, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #16 with and #18 without air","CAN","2021-02-04",{"$f":"AVERAGE(243.7,234.27)","v":238.98500000000001},"m3",238.98500000000001,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62,"0-25",6,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS65:$BB65,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / ","Concrete - 26-30 MPa, Canadian Benchmark Average","CRMCA","Can. Avg.",null,null,null,"Mix #22","CAN","2021-02-04",349.68,"m3",349.68,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,63,"26-30",1,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS66:$BB66,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / ","Concrete - 26-30 MPa, 0-14% FA/SL, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #20 with and #21 without air","CAN","2021-02-04",{"$f":"AVERAGE(376.48,344.12)","v":360.3},"m3",360.3,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,64,"26-30",2,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS67:$BB67,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / ","Concrete - 26-30 MPa, 15-29% Fly Ash, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #23 with and #25 without air","CAN","2021-02-04",{"$f":"AVERAGE(338.73,310.24)","v":324.48500000000001},"m3",324.48500000000001,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,65,"26-30",3,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS68:$BB68,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / ","Concrete - 26-30 MPa, 30-40% Fly Ash, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #27 with and #29 without air","CAN","2021-02-04",{"$f":"AVERAGE(297.92, 273.61)","v":285.76499999999999},"m3",285.76499999999999,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,66,"26-30",4,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS69:$BB69,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / ","Concrete - 26-30 MPa, 25-34% Slag, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #31 with and #33 without air","CAN","2021-02-04",{"$f":"AVERAGE(306.29, 281.13)","v":293.71000000000004},"m3",293.71000000000004,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,67,"26-30",5,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS70:$BB70,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / ","Concrete - 26-30 MPa, 35-50% Slag, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #35 with and #37 without air","CAN","2021-02-04",{"$f":"AVERAGE(278.22, 255.94)","v":267.08000000000004},"m3",267.08000000000004,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,68,"26-30",6,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS71:$BB71,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / ","Concrete - 31-35 MPa, Canadian Benchmark Average","CRMCA","Can. Avg.",null,null,null,"Mix #41","CAN","2021-02-04",417.05,"m3",417.05,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,69,"31-35",1,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS72:$BB72,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / ","Concrete - 31-35 MPa, 0-14% FA/SL, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #39 with and #40 without air","CAN","2021-02-04",{"$f":"AVERAGE(449.79, 386.61)","v":418.20000000000005},"m3",418.20000000000005,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,70,"31-35",2,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS73:$BB73,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / ","Concrete - 31-35 MPa, 15-29% Fly Ash, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #42 with and #44 without air","CAN","2021-02-04",{"$f":"AVERAGE(403.68, 347.87)","v":375.77499999999998},"m3",375.77499999999998,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,71,"31-35",3,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS74:$BB74,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / ","Concrete - 31-35 MPa, 30-40% Fly Ash, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #46 with and #48 without air","CAN","2021-02-04",{"$f":"AVERAGE(353.84, 305.99)","v":329.91499999999996},"m3",329.91499999999996,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,72,"31-35",4,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS75:$BB75,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / ","Concrete - 31-35 MPa, 25-34% Slag, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #50 with and #52 without air","CAN","2021-02-04",{"$f":"AVERAGE(364.06, 314.59)","v":339.32499999999999},"m3",339.32499999999999,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,73,"31-35",5,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS76:$BB76,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / ","Concrete - 31-35 MPa, 35-50% Slag, GU","CRMCA","Can. Avg.",null,null,null,"Avg of #54 with and #56 without air","CAN","2021-02-04",{"$f":"AVERAGE(329.77, 285.78)","v":307.77499999999998},"m3",307.77499999999998,"m3",10092,"NSF",2022,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,74,"31-35",6,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS77:$BB77,0))","v":true},"Yukon","Yukon","Northwest Territories","Territoires du Nord-Ouest","Nunavut","Nunavut","Canada"]
["Concrete - 20 MPa, Standard mix / NRMCA / US Avg / ","Concrete - 20 MPa, Standard mix","NRMCA","US Avg",null,null,null,"3000-00-FA/SL","USA","2021-02-04",345.5,"m3",345.5,"m3","EPD10294","NSF",2024,2305,"kg/m3",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,75,"0-25",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS78:$BB78,0))","v":false}]
["Concrete - 20 MPa, 20-30% Fly Ash / NRMCA / US Avg / ","Concrete - 20 MPa, 20-30% Fly Ash","NRMCA","US Avg",null,null,null,"3000-20-FA","USA","2021-02-04",297.10000000000002,"m3",297.10000000000002,"m3","EPD10295","NSF",2024,2305,"kg/m3",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,76,"0-25",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS79:$BB79,0))","v":false}]
["Concrete - 20 MPa, 30-40% FA/SL / NRMCA / US Avg / ","Concrete - 20 MPa, 30-40% FA/SL","NRMCA","US Avg",null,null,null,"3000-30-FA/SL","USA","2021-02-04",{"$f":"AVERAGE(270.97,267.26)","v":269.11500000000001},"m3",269.11500000000001,"m3","EPD10296","NSF",2024,2305,"kg/m3",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,77,"0-25",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS80:$BB80,0))","v":false}]
["Concrete - 20 MPa, 40-50% FA/SL mix / NRMCA / US Avg / ","Concrete - 20 MPa, 40-50% FA/SL mix","NRMCA","US Avg",null,null,null,"3000-40-FA/SL","USA","2021-02-04",242.3,"m3",242.3,"m3","EPD10297","NSF",2024,2305,"kg/m3",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,78,"0-25",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS81:$BB81,0))","v":false}]
["Concrete - 20 MPa, >50% SCM mix / NRMCA / US Avg / ","Concrete - 20 MPa, >50% SCM mix","NRMCA","US Avg",null,null,null,"3000-50-FA/SL","USA","2021-02-04",214.8,"m3",214.8,"m3","EPD10298","NSF",2024,2305,"kg/m3",null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,79,"0-25",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS82:$BB82,0))","v":false}]
[{"$f":"B83&\" / \"&C83&\" / \"&D83&\" / \"&E83","v":"Cork board insulation / Amorim / Isolamentos / R4/inch"},"Cork board insulation","Amorim","Isolamentos","R4/inch",null,null,null,"EU",null,-198,"m3",{"$f":"((K83*W83)--(R83*W83*Z83*44/12))","v":2.9758666666666684},"m2 RSI 1","DAP 002:2016","DAP Habitat",2021,115,"kg/m3",null,null,null,0.04,"W/(mK)",1,0.64600000000000002,{"$f":"(AF83*W83)*rng_biogenic_storage","v":9.806280000000001},"kg CO2e/m2-RSI1",null,null,null,{"$f":"R83*Y83*Z83*44/12","v":272.3966666666667},null,null,null,null,null,80,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS83:$BB83,0))","v":false}]
["Cork flooring / Amorim / Revestimentos S.A. / Cork floating floor planks","Cork flooring","Amorim","Revestimentos S.A.","Cork floating floor planks",null,null,null,"EU",null,9.34,"m2",{"$f":"(9.34)","v":9.34},"m2","EPD-AMO-20150057-IAA1-EN ","IBU",2021,8.4,"kg/m2",null,null,null,null,null,0.31,0.55000000000000004,{"$f":"(AF84)*rng_biogenic_storage","v":4.7262600000000008},"m2",null,null,null,{"$f":"R84*Y84*Z84*44/12","v":5.2514000000000003},6.0000000000000001E-3,1.2250000000000001,0.14499999999999999,null,null,81,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS84:$BB84,0))","v":false}]
["Cork flooring / European Resilient Flooring Manufacturers' Institute / Includes: Altro, Amorim, Amtico, Artigo, Aspecta, BeauFlor, Dickson, Mflor, Forbo, Gerflor, IVC, Nora, Polyflor, Tarkett, Kahrs, Windmoller / Cork floor tiles","Cork flooring","European Resilient Flooring Manufacturers' Institute","Includes: Altro, Amorim, Amtico, Artigo, Aspecta, BeauFlor, Dickson, Mflor, Forbo, Gerflor, IVC, Nora, Polyflor, Tarkett, Kahrs, Windmoller","Cork floor tiles",null,null,null,"EU",null,-2.74,"m2",{"$f":"(K85--R85*Y85*Z85*3.67)","v":0.77219000000000015},"m2","EPD-ERF-20180184-CCI1-EN ","IBU",2024,2,"kg/m2",null,null,null,null,null,0.87,0.55000000000000004,{"$f":"(AF85)*rng_biogenic_storage","v":3.1581000000000006},"m2",null,null,null,{"$f":"R85*Y85*Z85*44/12","v":3.5090000000000003},4.0000000000000001E-3,null,null,null,null,82,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS85:$BB85,0))","v":false}]
["Cross Laminated Timber / Nordic / X-Lam / 3-1/2\" (90mm) thick","Cross Laminated Timber","Nordic","X-Lam","3-1/2\" (90mm) thick",null,null,"Wood biogenic carbon storage set to zero","CAN",null,121.89,"m3",{"$f":"(K86*T86)","v":10.9701},"m2 at 3-1/2\" thickness","August, 2018","FPInnovations",2023,410.46,"kg/m3",0.09,"m thickness",null,null,null,0.98899999999999999,0.5,null,"m2 at 3-1/2\" thickness",0.82499999999999996,{"$f":"R86*T86*Y86*Z86","v":18.267522299999996},null,null,null,null,null,null,null,83,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS86:$BB86,0))","v":false}]
["Cross Laminated Timber / Structurlam / CrossLam / 3-1/2\" (90mm) thick","Cross Laminated Timber","Structurlam","CrossLam","3-1/2\" (90mm) thick",null,null,"Wood biogenic carbon storage set to zero","CAN",null,124.02,"m3",{"$f":"(K87*T87)","v":11.161799999999999},"m2 at 3-1/2\" thickness","EPD124 ","ASTM",2025,481,"kg/m3",0.09,"m thickness",null,null,null,0.995,0.5,null,"m2 at 3-1/2\" thickness",0.82499999999999996,{"$f":"R87*T87*Y87*Z87","v":21.536774999999999},null,null,null,null,null,null,null,84,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS87:$BB87,0))","v":false}]
["Dowel Laminated Timber / StructureCraft / DowelLam / 3-1/2\" (90mm) thick","Dowel Laminated Timber","StructureCraft","DowelLam","3-1/2\" (90mm) thick",null,null,"Wood biogenic carbon storage set to zero","CAN",null,121.4,"m3",{"$f":"(K88*T88)","v":10.926},"m2 at 3-1/2\" thickness","EPD157 ","ASTM",2025,449,"kg/m3",0.09,"m thickness",null,null,null,0.99860000000000004,0.5,null,"m2 at 3-1/2\" thickness",0.82499999999999996,{"$f":"R88*T88*Y88*Z88","v":20.176712999999999},null,null,null,null,null,null,null,85,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS88:$BB88,0))","v":false}]
["Drywall 1/2\" / CertainTeed / AirRenew / 1/2\" (12.7 mm)","Drywall 1/2\"","CertainTeed","AirRenew","1/2\" (12.7 mm)",null,null,null,"USA",null,138,"92.9m2",{"$f":"(K89/92.9)","v":1.4854682454251882},"m2","4786663719.107.0","UL Env.",2022,7.3,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,86,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS89:$BB89,0))","v":false}]
["Drywall 1/2\" / CertainTeed / Easi-Lite / 1/2\" (12.7 mm)","Drywall 1/2\"","CertainTeed","Easi-Lite","1/2\" (12.7 mm)",null,null,null,"CAN",null,142,"92.9m2",1.5285252960172226,"m2","4786663719.111.1","ASTM",2020,6.35,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,87,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS90:$BB90,0))","v":false}]
["Drywall 1/2\" / CertainTeed / M2Tech moisture resistant / 1/2\" (12.7 mm)","Drywall 1/2\"","CertainTeed","M2Tech moisture resistant","1/2\" (12.7 mm)",null,null,null,"CAN",null,174,"92.9m2",1.8729817007534983,"m2","4786663719.114.1","UL Env.",2022,7.8,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,88,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS91:$BB91,0))","v":false}]
["Drywall 1/2\" / Pabco / QuietRock / QuietRock 1/2\"","Drywall 1/2\"","Pabco","QuietRock","QuietRock 1/2\"",null,null,null,"USA",null,451,"92.9m2",4.8546824542518836,"m2","EPD-156","ASTM",2025,10.3,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,89,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS92:$BB92,0))","v":false}]
["Drywall 5/8\" /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 5/8\"","Drywall 5/8\"",null,"Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC","5/8\"",null,null,null,"USA & CAN",null,277,"92.9m2",2.981700753498385,"m2","EPD 10270 ","NSF",2025,10.67,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,90,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS93:$BB93,0))","v":false}]
["Drywall 5/8\" / USG / EcoSmart Firecode / 5/8\"","Drywall 5/8\"","USG","EcoSmart Firecode","5/8\"",null,null,null,null,null,193,"92.9m2",2.077502691065662,"m2","4787352797.107.1 ","UL Env.",2023,8.3000000000000007,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,91,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS94:$BB94,0))","v":false}]
["EPDM Roofing Membrane / SPRI /  / ","EPDM Roofing Membrane","SPRI",null,null,null,null,"60 mils, Non-reinforced single ply","USA",null,6.69,"m2",{"$f":"(6.69)","v":6.69},"m2","4786842353.103.1 ","UL Env.",2022,2.0699999999999998,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,92,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS95:$BB95,0))","v":false}]
[{"$f":"B96&\" / \"&C96&\" / \"&D96&\" / \"&E96","v":"EPS foam board / EPS Industry Alliance /  / R 4.6/inch, Type IX, 25 psi (Type 3, 140 kPa)"},"EPS foam board","EPS Industry Alliance",null,"R 4.6/inch, Type IX, 25 psi (Type 3, 140 kPa)",null,null,null,"USA & CAN",null,4.7699999999999996,"m2 RSI 1",{"$f":"(4.77)","v":4.7699999999999996},"m2 RSI 1","4787238561.101.2","UL Env.",2022,48,"kg/m3",null,null,4.5999999999999996,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,93,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS96:$BB96,0))","v":false}]
[{"$f":"B97&\" / \"&C97&\" / \"&D97&\" / \"&E97","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},"EPS foam board","EPS Industry Alliance",null,"R 4/inch, Type II, 15 psi (Type 2, 110 kPa)",null,null,null,"USA & CAN",null,3.77,"m2 RSI 1",{"$f":"(3.77)","v":3.77},"m2 RSI 1","4787238561.101.1 ","UL Env.",2022,21.6,"kg/m3",null,null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,94,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS97:$BB97,0))","v":false}]
[{"$f":"B98&\" / \"&C98&\" / \"&D98&\" / \"&E98","v":"EPS foam board with graphite / BASF / Neopor / R 4.7/inch, Type IX"},"EPS foam board with graphite","BASF","Neopor","R 4.7/inch, Type IX",null,null,null,"USA & CAN",null,3.42,"m2 RSI 1",{"$f":"(3.42)","v":3.42},"m2 RSI 1","EPD10328","NSF",2026,28.8,"kg/m3",null,null,4.7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS98:$BB98,0))","v":false}]
[{"$f":"B99&\" / \"&C99&\" / \"&D99&\" / \"&E99","v":"EPS foam board with graphite / BASF / Neopor / R 4.7/inch, Type II, 15 psi (Type 2, 110 kPa)"},"EPS foam board with graphite","BASF","Neopor","R 4.7/inch, Type II, 15 psi (Type 2, 110 kPa)",null,null,null,"USA & CAN",null,2.76,"m2 RSI 1",{"$f":"(2.76)","v":2.76},"m2 RSI 1","EPD10327","NSF",2025,21.6,"kg/m3",null,null,4.7,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,96,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS99:$BB99,0))","v":false}]
["Fiber Cement roofing / Cembrit / Corrugated sheets / 6.5 mm","Fiber Cement roofing","Cembrit","Corrugated sheets","6.5 mm",null,null,null,"EU",null,0.80400000000000005,"kg",{"$f":"(K100*R100)","v":8.3093400000000006},"m2 at 6.5 mm","EPD-CEM-20160114-IAD1-EN ","IBU",2021,{"$f":"1590*0.0065","v":10.334999999999999},"kg/m2",null,null,null,null,null,0.04,0.5,{"$f":"(AC100*AD100)*rng_biogenic_storage","v":0.34229520000000002},"m2",1.84,{"$f":"R100*Y100*Z100","v":0.20669999999999999},null,null,null,null,null,null,null,97,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS100:$BB100,0))","v":false}]
["Fiber Cement roofing / Cembrit / Slates / 4 mm","Fiber Cement roofing","Cembrit","Slates","4 mm",null,null,null,"EU",null,0.94599999999999995,"kg",{"$f":"(K101*R101)","v":7.0004},"m2 at 4 mm","EPD-CEM-20160113-IAD1-EN ","IBU",2021,{"$f":"1850*0.004","v":7.4},"kg/m2",null,null,null,null,null,3.5000000000000003E-2,0.5,{"$f":"(AC101*AD101)*rng_biogenic_storage","v":0.21445200000000006},"m2",1.84,{"$f":"R101*Y101*Z101","v":0.12950000000000003},null,null,null,null,null,null,null,98,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS101:$BB101,0))","v":false}]
["Fiber Cement roofing / Mahaphant / Fibre-Cement / 5 mm","Fiber Cement roofing","Mahaphant","Fibre-Cement","5 mm",null,null,null,"EU",null,0.87,"kg",{"$f":"(K102*R102)","v":6.4815000000000005},"m2 at 5 mm","EPD-MET-20140068-IAC1-EN ","IBU",2019,{"$f":"1490*0.005","v":7.45},"kg/m2",null,null,null,null,null,0.03,0.5,{"$f":"(AC102*AD102)*rng_biogenic_storage","v":0.18505800000000003},"m2",1.84,{"$f":"R102*Y102*Z102","v":0.11175},null,null,null,null,null,null,null,99,null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS102:$BB102,0))","v":false}]
["Fiber Cement siding / Cembrit / Patina / ","Fiber Cement siding","Cembrit","Patina",null,null,null,null,"EU",null,790,"T",{"$f":"((K103*R103)/1000*AG103)","v":11.186399999999999},"m2 at 8 mm (5/16\")","MD-18011-EN","epddanmark",2023,1770,"kg/m3",{"$f":"R103*0.008","v":14.16},"kg/m2 at 8mm",null,null,null,9.5000000000000001E-2,0.5,{"$f":"(AC103*AD103)*rng_biogenic_storage","v":1.1138256},"m2",1.84,{"$f":"T103*Y103*Z103","v":0.67259999999999998},null,null,8.0000000000000002E-3,3.05,1.25,null,null,100,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS103:$BB103,0))","v":false}]
["Fiber Cement siding / Cembrit / Solid & Express / ","Fiber Cement siding","Cembrit","Solid & Express",null,null,null,null,"EU",null,1790,"T",{"$f":"((K104*R104)/1000*AG104)","v":25.346400000000003},"m2 at 8 mm (5/16\")","MD-18011-EN","epddanmark",2023,1770,"kg/m3",{"$f":"R104*0.008","v":14.16},"kg/m2 at 8mm",null,null,null,9.5000000000000001E-2,0.5,{"$f":"(AC104*AD104)*rng_biogenic_storage","v":1.1138256},"m2",1.84,{"$f":"T104*Y104*Z104","v":0.67259999999999998},null,null,8.0000000000000002E-3,2.5,1.25,null,null,101,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS104:$BB104,0))","v":false}]
["Fiberglass batt / CertainTeed / Sustainable Insulation / R 3.6/inch","Fiberglass batt","CertainTeed","Sustainable Insulation","R 3.6/inch",null,null,null,"USA",null,0.94,"m2 RSI 1",{"$f":"(0.94)","v":0.94},"m2 RSI 1","4788647002.101.1 ","UL Env.",2024,0.48799999999999999,"kg/m2 at RSI 1",null,null,3.64,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,102,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS105:$BB105,0))","v":false}]
["Fiberglass batt / Knauf / EcoBatt / R 3.6/inch","Fiberglass batt","Knauf","EcoBatt","R 3.6/inch",null,null,null,"USA",null,0.61,"m2 RSI 1",{"$f":"(0.61)","v":0.61},"m2 RSI 1","KNA-12032018-001","Sustainable Minds",2023,null,null,null,null,3.64,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,103,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS106:$BB106,0))","v":false}]
["Fiberglass batt / Owens Corning / EcoTouch Pink batt and roll / R 3.6/inch","Fiberglass batt","Owens Corning","EcoTouch Pink batt and roll","R 3.6/inch",null,null,null,"USA & CAN",null,0.46400000000000002,"m2 RSI 1",{"$f":"(0.464)","v":0.46400000000000002},"m2 RSI 1","4788548937.101.1","UL Env.",2023,null,null,null,null,3.64,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS107:$BB107,0))","v":false}]
["Fiberglass loose fill / CertainTeed / InsulSafe, Optima, TruComfort / R 2.6/inch","Fiberglass loose fill","CertainTeed","InsulSafe, Optima, TruComfort","R 2.6/inch",null,null,null,"USA",null,1.29,"m2 RSI 1",{"$f":"(1.29)","v":1.29},"m2 RSI 1","4788647002.102.1 ","UL Env.",2024,0.57399999999999995,"kg/m2 at RSI 1",null,null,2.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,105,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS108:$BB108,0))","v":false}]
["Fiberglass loose fill / Knauf / Jet Stream ULTRA / R 2.2/inch","Fiberglass loose fill","Knauf","Jet Stream ULTRA","R 2.2/inch",null,null,null,"USA",null,0.73,"m2 RSI 1",{"$f":"(0.73)","v":0.73},"m2 RSI 1","KNA-12032018-003","Sustainable Minds",2023,28.8,"kg/m3",null,null,2.2000000000000002,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,106,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS109:$BB109,0))","v":false}]
["Fiberglass loose fill / Owens Corning / AttiCat, ProCat, ProPink / R 2.8/inch","Fiberglass loose fill","Owens Corning","AttiCat, ProCat, ProPink","R 2.8/inch",null,null,null,"USA & CAN",null,0.98299999999999998,"m2 RSI 1",{"$f":"(0.983)","v":0.98299999999999998},"m2 RSI 1","4788548937.101.1","UL Env.",2023,null,null,null,null,2.84,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,107,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS110:$BB110,0))","v":false}]
["Foam glass aggregate / Glasopor AS /  / R 1.7/inch, 10-60 mm","Foam glass aggregate","Glasopor AS",null,"R 1.7/inch, 10-60 mm",null,null,null,"EU",null,6.96,"m3",{"$f":"(K111*W111)","v":0.61943999999999999},"m2 RSI1","NEPD-1243-396-EN","Norwegian EPD Foundation",2022,180,"kg/m3",null,null,null,8.8999999999999996E-2,"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,108,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS111:$BB111,0))","v":false}]
["Foam glass aggregate / Hasopor /  / R 1.7/inch, 10-60 mm","Foam glass aggregate","Hasopor",null,"R 1.7/inch, 10-60 mm",null,null,null,"EU",null,7.77,"m3",{"$f":"(K112*W112)","v":0.62159999999999993},"m2 RSI1","S-P-01088 ","EPD International AB",2022,180,"kg/m3",null,null,null,0.08,"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,109,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS112:$BB112,0))","v":false}]
["Foam glass aggregate / Misapor / Glavel / R 1.7/inch, 10-60 mm","Foam glass aggregate","Misapor","Glavel","R 1.7/inch, 10-60 mm",null,null,null,"EU",null,15.2,"m3",{"$f":"(K113*W113)","v":1.2464},"m2 RSI1","EPD-MIS-20150019-IAA2-DE ","IBU",2020,130,"kg/m3",null,null,null,8.2000000000000003E-2,"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,110,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS113:$BB113,0))","v":false}]
["Foam glass board / Pittsburgh Corning Europe / Foamglas T4 / R3.7/inch","Foam glass board","Pittsburgh Corning Europe","Foamglas T4","R3.7/inch",null,null,null,"EU",null,1.32,"kg",{"$f":"(K114*R114*W114)","v":6.2238000000000007},"m2 RSI1","EPD-PCE-2013256-IBA2-DE ","IBU",2020,115,"kg/m3",null,null,null,4.1000000000000002E-2,"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,111,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS114:$BB114,0))","v":false}]
["Foam glass board / Pittsburgh Corning Europe / Foamglas W+F, Foamglas T3 / R4/inch","Foam glass board","Pittsburgh Corning Europe","Foamglas W+F, Foamglas T3","R4/inch",null,null,null,"EU",null,1.26,"kg",{"$f":"(K115*R115*W115)","v":4.7880000000000003},"m2 RSI1","EPD-PCE-20150042-IBA1-DE ","IBU",2020,100,"kg/m3",null,null,null,3.7999999999999999E-2,"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,112,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS115:$BB115,0))","v":false}]
["Glued laminated timber / American Wood Council & Canadian Wood Council /  / ","Glued laminated timber","American Wood Council & Canadian Wood Council",null,null,null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,137.19,"m3",{"$f":"(137.19)","v":137.19},"m3","4788424634.104.1 ","UL Env.",2025,548,"kg/m3",null,null,null,null,null,0.98899999999999999,0.5,null,"m3",0.82499999999999996,{"$f":"R116*Y116*Z116","v":270.98599999999999},null,null,null,null,null,null,null,113,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS116:$BB116,0))","v":false}]
["Glued laminated timber / Structurlam / Glulam Plus / 3-1/2\" (90mm) thick","Glued laminated timber","Structurlam","Glulam Plus","3-1/2\" (90mm) thick",null,null,"Wood biogenic carbon storage set to zero","CAN",null,115.32,"m3",{"$f":"(115.32)","v":115.32},"m3","EPD125 ","ASTM",2025,544,"kg/m3",null,null,null,null,null,0.997,0.5,null,"m3",0.82499999999999996,{"$f":"R117*Y117*Z117","v":271.18400000000003},null,null,null,null,null,null,null,114,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS117:$BB117,0))","v":false}]
["Gypsum panels - glass mat /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 1/2\"","Gypsum panels - glass mat",null,"Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC","1/2\"",null,null,null,"USA & CAN",null,358,"92.9m2",{"$f":"(K118/92.9)","v":3.8536060279870825},"m2","EPD-038","ASTM",2021,2.0299999999999998,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS118:$BB118,0))","v":false}]
["Gypsum panels - glass mat / USG / Securock ExoAir 430 / 1/2\"","Gypsum panels - glass mat","USG","Securock ExoAir 430","1/2\"",null,null,null,"USA",null,568,"92.9m2",{"$f":"(K119/92.9)","v":6.1141011840688906},"m2","4787352797.110.1 ","UL Env.",2024,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,116,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS119:$BB119,0))","v":false}]
["Hardwood flooring / Action Floor Systems /  / 25/32\" x 3-1/4\" FSC certified","Hardwood flooring","Action Floor Systems",null,"25/32\" x 3-1/4\" FSC certified",null,null,"Wood biogenic carbon storage set to zero","USA",null,11.8,"m2",{"$f":"(11.8)","v":11.8},"m2","SCS-EPD-04591","SCS Global",2022,13.91,"kg/m2",null,null,null,null,null,0.98,0.5,null,"m2 at product thickness",null,null,null,null,1.9844000000000001E-2,null,null,null,null,117,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS120:$BB120,0))","v":false}]
["Hardwood flooring / mafi / Natural Hardwood Planks / 3/4\", 3 ply laminated solid, oil pre-finished","Hardwood flooring","mafi","Natural Hardwood Planks","3/4\", 3 ply laminated solid, oil pre-finished",null,null,"Wood biogenic carbon storage set to zero","EU",null,-8.09,"m2",{"$f":"(K121--R121*Y121*Z121*44/12)","v":13.985643333333336},"m2","4789456400.101.1","UL Env.",2025,12.287000000000001,"kg/m2 at 3/4\"",null,null,null,null,null,0.98,0.5,null,"m2 at product thickness",null,null,null,null,1.9E-2,null,null,null,null,118,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS121:$BB121,0))","v":false}]
["Hardwood flooring / Typical Eastern Canadian, solid, pre-finished /  / 3-12\" x 3/4\" prefinished","Hardwood flooring","Typical Eastern Canadian, solid, pre-finished",null,"3-12\" x 3/4\" prefinished",null,null,"Wood biogenic carbon storage set to zero","CAN",null,-2.29,"kg/m2",{"$f":"(K122--R122*Y122*Z122*44/12)","v":17.408249999999999},"m2",null,"FPInnovations",2019,11.02,"kg/m2 at 3/4\"",null,null,null,null,null,0.97499999999999998,0.5,null,"m2 at product thickness",null,null,null,{"$f":"R122*Y122*Z122*3.67","v":19.716157499999998},1.9E-2,null,8.3000000000000004E-2,null,null,119,null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS122:$BB122,0))","v":false}]
[{"$f":"B123&\" / \"&C123&\" / \"&D123&\" / \"&E123","v":"Helical pier / Generic /  / 3\" Nominal Pipe, 3.5 x 3/16\" (89 x 5.5 mm), 10\" Helix, Sched 40 STD Galvanized steel"},"Helical pier","Generic",null,"3\" Nominal Pipe, 3.5 x 3/16\" (89 x 5.5 mm), 10\" Helix, Sched 40 STD Galvanized steel",null,null,null,null,null,1.48,"kg",{"$f":"(T123*K123)","v":17.623840000000001},"m of pier length","11345278.101.1","UL Env.",2021,7800,"kg/m3",{"$f":"11.284+0.624","v":11.908000000000001},"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,null,null,null,{"$f":"IF(LEN(Q123)=4,IF(Q123<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q123),\"\"),\"\")","v":"Expired 2021"},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS123:$BB123,0))","v":false}]
["Hemp fiber batt / NaturFibre / Hemp Wool / R 3.7/inch","Hemp fiber batt","NaturFibre","Hemp Wool","R 3.7/inch",null,null,null,"USA & CAN",null,{"$f":"4.54-8.82","v":-4.28},"m2 @ 0.2m",{"$f":"(4.54/0.2*W124)","v":0.90800000000000003},"m2 RSI","Zampori et al. LCA",null,"",30,"kg/m3",6,"kg/m2 at 0.2m",3.69,0.04,"W/(mK)","Biocarbon from EPD",null,{"$f":"(1.9+0.633)*rng_biogenic_storage","v":2.2797000000000001},"m2 RSI",null,null,null,null,null,null,0.2,null,null,121,null,null,null,"Peer-reviewed LCA",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS124:$BB124,0))","v":false}]
["Hempcrete / IsoHemp / Europe / R 2.1/inch","Hempcrete","IsoHemp","Europe","R 2.1/inch",null,null,null,"EU",null,-96.3,"m3",{"$f":"(K125*W125--AA125)","v":4.5422729999999998},"m2 RSI 1","April, 2018","Uliege",2023,300,"kg/m3",{"$f":"R125*W125","v":22.8},"kg/m2 at RSI1",2.13,7.5999999999999998E-2,"W/(mK)",0.35,0.45,{"$f":"(T125*Y125*Z125*3.67)*rng_biogenic_storage","v":11.861072999999999},"m2-RSI1",null,null,null,null,null,null,null,null,null,122,null,null,null,"LCA",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS125:$BB125,0))","v":false}]
["Hempcrete / Site mixed / Europe / R 2.1/inch, Avg. of 9 mixes","Hempcrete","Site mixed","Europe","R 2.1/inch, Avg. of 9 mixes",null,null,null,"EU",null,13.1,"m2 RSI 1",{"$f":"(13.1)","v":13.1},"m2 RSI 1","Arrigoni et al, 2017, LCA",null,"",300,"kg/m3",{"$f":"R126*W126","v":22.8},"kg/m2 at RSI1",2.13,7.5999999999999998E-2,"W/(mK)",0.35,0.45,{"$f":"(20.35)*rng_biogenic_storage","v":18.315000000000001},"m2-RSI1",null,null,null,null,null,null,null,null,null,123,null,null,null,"Peer-reviewed LCA, 2017",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS126:$BB126,0))","v":false}]
["Hempcrete / Site mixed / USA / R 2.1/inch, Avg. mix using NHL & PHL","Hempcrete","Site mixed","USA","R 2.1/inch, Avg. mix using NHL & PHL",null,null,null,"USA",null,-4.32,"m2 RSI 1",{"$f":"(K127--AA127)","v":7.541072999999999},"m2 RSI 1","Arehart et al, 2020 LCA",null,"",300,"kg/m3",{"$f":"R127*W127","v":22.8},"kg/m2 at RSI1",2.13,7.5999999999999998E-2,"W/(mK)",0.35,0.45,{"$f":"(T127*Y127*Z127*3.67)*rng_biogenic_storage","v":11.861072999999999},"m2-RSI1",null,null,null,null,null,null,null,null,null,124,null,null,null,"Peer-reviewed LCA, 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS127:$BB127,0))","v":false}]
["Laminate flooring / Novalis / LVT / ","Laminate flooring","Novalis","LVT",null,null,null,"Wood biogenic carbon storage set to zero","USA",null,27.1,"m2",{"$f":"(27.1)","v":27.1},"m2","4786462817.102.1","UL Env.",2019,5.26,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,4.1000000000000003E-3,null,null,null,null,125,null,null,null,{"$f":"IF(LEN(Q128)=4,IF(Q128<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q128),\"\"),\"\")","v":"Expired 2019"},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS128:$BB128,0))","v":false}]
["(ARCHIVED 2023) Laminated strand lumber / American Wood Council & Canadian Wood Council /  / ","(ARCHIVED 2023) Laminated strand lumber","American Wood Council & Canadian Wood Council",null,null,null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,310.27999999999997,"m3",{"$f":"(310.28)","v":310.27999999999997},"m3","4787193543.101.1 ","UL Env.",2021,570.22,"kg/m3",null,null,null,null,null,0.93500000000000005,0.5,null,"m3",0.82499999999999996,{"$f":"R129*Y129*Z129","v":266.57785000000001},null,null,null,null,null,null,null,"126_Archived",null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS129:$BB129,0))","v":false}]
["Laminated strand lumber (LSL) / American Wood Council & Canadian Wood Council /  / ","Laminated strand lumber (LSL)","American Wood Council & Canadian Wood Council",null,null,null,null,"No biogenic carbon credited","US & CA",null,274.89999999999998,"m3",274.89999999999998,"m3","4789710952.101.1","UL Environment",2026,null,null,null,null,null,null,null,0.93500000000000005,0.5,null,"m3",0.82499999999999996,266.57785000000001,null,null,null,null,null,null,null,126,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS130:$BB130,0))","v":false}]
["Laminated veneer lumber (LVL) / American Wood Council & Canadian Wood Council /  / ","Laminated veneer lumber (LVL)","American Wood Council & Canadian Wood Council",null,null,null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,361.45,"m3",{"$f":"(361.45)","v":361.45},"m3","4788424634.105.1 ","UL Env.",2025,548,"kg/m3",null,null,null,null,null,0.95599999999999996,0.5,null,"m3",0.82499999999999996,{"$f":"R131*Y131*Z131","v":261.94400000000002},null,null,null,null,null,null,null,127,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS131:$BB131,0))","v":false}]
["Laminated veneer lumber (LVL) / RedBuilt / RedLam / ","Laminated veneer lumber (LVL)","RedBuilt","RedLam",null,null,null,"Wood biogenic carbon storage set to zero","USA",null,360,"m3",{"$f":"(360)","v":360},"m3","SCS-EPD-04128","SCS Global",2021,593,"kg/m3",null,null,null,null,null,0.97,0.5,null,"m3",0.82499999999999996,{"$f":"R132*Y132*Z132","v":287.60500000000002},null,null,null,null,null,null,null,128,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS132:$BB132,0))","v":false}]
["Lime Plaster / Mapei / MapeWall Muratura / 3/4\" Natural Hydraulic Lime (NHL)","Lime Plaster","Mapei","MapeWall Muratura","3/4\" Natural Hydraulic Lime (NHL)",null,null,"Aggregate included","EU",null,0.40200000000000002,"kg",{"$f":"(K133*R133*AG133)","v":9.5726250000000022},"m2 at 0.01905 m (3/4\")","EPD-FEI-20160017-IBG1-EN ","IBU",2021,1250,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,1.9050000000000001E-2,null,null,null,null,129,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS133:$BB133,0))","v":false}]
["Lime/Cork Plaster / Diasen / Diathonite Evolution / Exterior plaster cladding, 3/4\"","Lime/Cork Plaster","Diasen","Diathonite Evolution","Exterior plaster cladding, 3/4\"",null,null,null,"EU",null,0.51900000000000002,"kg",{"$f":"(R134*AG134*K134)","v":3.5593020000000002},"m2 at 0.01905 m (3/4\")","S-P-00838","Rina Services/Environdec",2022,360,"kg/m3",{"$f":"R134*0.01905","v":6.8580000000000005},"kg/m2 at 0.01905 (3/4\")",null,null,null,0.45,0.55000000000000004,null,"kg",null,null,null,null,1.9050000000000001E-2,null,null,null,null,130,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS134:$BB134,0))","v":false}]
[{"$f":"B135&\" / \"&C135&\" / \"&D135&\" / \"&E135","v":"Linoleum flooring / Armstrong / Sheet style / 2.5 mm sheet style linoleum"},"Linoleum flooring","Armstrong","Sheet style","2.5 mm sheet style linoleum",null,null,null,"USA",null,4.34,"m2",{"$f":"(4.34)","v":4.34},"m2","EPD-0002","ASTM",2019,2.88,"kg/m2",null,null,null,null,null,0.72,0.4,{"$f":"3.04*rng_biogenic_storage","v":2.7360000000000002},null,null,null,null,null,2.5000000000000001E-3,null,null,null,null,131,null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS135:$BB135,0))","v":false}]
[{"$f":"B136&\" / \"&C136&\" / \"&D136&\" / \"&E136","v":"Linoleum flooring / Forbo / Marmoleum / 2.5 mm sheet style linoleum"},"Linoleum flooring","Forbo","Marmoleum","2.5 mm sheet style linoleum",null,null,null,"USA",null,1.29,"m2",{"$f":"(K136--AA136)","v":5.0340000000000007},"m2","12CA64879.101.1 ","UL Env.",2023,3,"kg/m2",null,null,null,null,null,null,0.378,{"$f":"4.16*rng_biogenic_storage","v":3.7440000000000002},null,null,1.1349,null,4.1612999999999998,2.5000000000000001E-3,null,null,null,null,132,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS136:$BB136,0))","v":false}]
[{"$f":"B137&\" / \"&C137&\" / \"&D137&\" / \"&E137","v":"Linoleum flooring / Forbo / Marmoleum Striato / 2.5 mm sheet style linoleum"},"Linoleum flooring","Forbo","Marmoleum Striato","2.5 mm sheet style linoleum",null,null,null,"USA",null,-0.26800000000000002,"m2",{"$f":"(K137--AA137)","v":4.016},"m2","4789275679.141.1 ","UL Env.",2025,3,"kg/m2",null,null,null,null,null,null,0.433,{"$f":"4.76*rng_biogenic_storage","v":4.2839999999999998},null,null,1.2978000000000001,null,4.7586000000000004,2.5000000000000001E-3,null,null,null,null,133,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS137:$BB137,0))","v":false}]
[{"$f":"B138&\" / \"&C138&\" / \"&D138&\" / \"&E138","v":"Linoleum flooring / Gerflor  / DLW Linoleum Acousticplus / 4.0 mm sheet style linoleum"},"Linoleum flooring","Gerflor ","DLW Linoleum Acousticplus","4.0 mm sheet style linoleum",null,null,null,"US","2022-12-21",2.9169999999999998,"m²",7.7679999999999998,"m²","4788756650.101.1 ","UL Environment",2025,3.5,"kg/m2",null,null,null,null,null,null,0.42,{"$f":"AF138*rng_biogenic_storage","v":6.2910000000000004},null,null,1.47,null,6.99,null,null,4.0000000000000001E-3,null,null,134,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS138:$BB138,0))","v":false}]
[{"$f":"B139&\" / \"&C139&\" / \"&D139&\" / \"&E139","v":"(ARCHIVED 2023) Linoleum flooring / Gerflor / DLW Linoleum / 4.0 mm sheet style linoleum"},"(ARCHIVED 2023) Linoleum flooring","Gerflor","DLW Linoleum","4.0 mm sheet style linoleum",null,null,null,"USA",null,2.9169999999999998,"m2",{"$f":"(2.917)","v":2.9169999999999998},"m2","4788756650.101.1 ","UL Env.",2024,3.5,"kg/m2",null,null,null,null,null,0.68,0.4,{"$f":"(R139*Y139*Z139*3.67)*rng_biogenic_storage","v":3.1444560000000004},null,null,null,null,null,4.0000000000000001E-3,null,null,null,null,"134_Archived",null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS139:$BB139,0))","v":false}]
["Liquid linoleum flooring / Duracryl Corques / Liquid Lino / 2.0 mm liquid applied","Liquid linoleum flooring","Duracryl Corques","Liquid Lino","2.0 mm liquid applied",null,null,null,"EU",null,3.98,"m2",{"$f":"(3.98)","v":3.98},"m2","EPD-NIBE-20181206-3522 ","NIBE Research",2021,1.8,"kg/m2",null,null,null,null,null,0.88,0.4,{"$f":"(R140*Y140*Z140*3.67)*rng_biogenic_storage","v":2.0927808000000003},null,null,null,null,null,2E-3,null,null,null,null,135,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS140:$BB140,0))","v":false}]
["Masonry cement / Portland Cement Association / Includes Argos, Buzzi, CalPortland, Capitol Aggregates, Cemex, Essroc, LafargeHolcim, Monarch, St. Mary's, Titan / ","Masonry cement","Portland Cement Association","Includes Argos, Buzzi, CalPortland, Capitol Aggregates, Cemex, Essroc, LafargeHolcim, Monarch, St. Mary's, Titan",null,null,null,null,"USA & CAN",null,0.69199999999999995,"kg",{"$f":"(K141)","v":0.69199999999999995},"kg","EPD 034 ","ASTM","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,136,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS141:$BB141,0))","v":false}]
["Masonry Mortar Mix / 1 part Masonry cement / 3 parts avg sand / ","Masonry Mortar Mix","1 part Masonry cement","3 parts avg sand",null,null,null,null,null,null,null,null,{"$f":"(R142*M141+T142*K5/1000)","v":268.63920000000002},"m3","EPD 034 ","ASTM","",{"$f":"0.25*1500","v":375},"kg/m3 masonry cement",{"$f":"0.75*1280","v":960},"kg/m3 sand",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,137,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS142:$BB142,0))","v":false}]
[{"$f":"B143&\" / \"&C143&\" / \"&E143&\" / \"&D143","v":"Metal Panels - Aluminum / Metal Construction Assn. / 22 gauge / Includes: ATAS, DMI, Englert, Fabral,McElroy, Pac-Clad"},"Metal Panels - Aluminum","Metal Construction Assn.","Includes: ATAS, DMI, Englert, Fabral,McElroy, Pac-Clad","22 gauge",null,null,null,"USA",null,1860,"100m2",{"$f":"(K143/100)","v":18.600000000000001},"m2","4789289084.103.2","UL Env.",2026,2720,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,6.4000000000000005E-4,null,null,null,null,138,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS143:$BB143,0))","v":false}]
["Metal Panels - Aluminum / Petersen Aluminum Corp / Pac-Clad / 20EQ gauge","Metal Panels - Aluminum","Petersen Aluminum Corp","Pac-Clad","20EQ gauge",null,null,null,"USA",null,1900.45,"92.9m2",{"$f":"(K144/92.9)","v":20.456942949407964},"m2","4786652606.101.1 ","UL Env.",2020,2.0699999999999998,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,139,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS144:$BB144,0))","v":false}]
["Metal Panels - Steel / AEP Span / All products / 24 gauge","Metal Panels - Steel","AEP Span","All products","24 gauge",null,null,null,"USA",null,1263.9000000000001,"92.9m2",{"$f":"(K145/92.9)","v":13.604951560818083},"m2","SCS-EPD-04462","SCS Global",2022,8030,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,6.0999999999999997E-4,null,null,null,null,140,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS145:$BB145,0))","v":false}]
["Metal Panels - Steel / ArcelorMittal / All products / 24 gauge","Metal Panels - Steel","ArcelorMittal","All products","24 gauge",null,null,null,"USA & CAN",null,1308,"92.9m2",{"$f":"(K146/92.9)","v":14.079655543595264},"m2","4787488168.101.1 ","UL Env.",2021,8030,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,6.0999999999999997E-4,null,null,null,null,141,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS146:$BB146,0))","v":false}]
[{"$f":"B147&\" / \"&C147&\" / \"&E147","v":"Metal Panels - Steel / Canadian Sheet Steel Building Institute / 24 gauge"},"Metal Panels - Steel","Canadian Sheet Steel Building Institute","Includes: Agway, Bailey, Behlen, Canam,DASS, DCM, Duchesne, EB, Exsteel, Ideal Roofing, Imperial, LKME, Manugypse, Metal Up, Scotia, Steel Tile Co, Steelway, Trebor, Vicwest, Vulcraft, Westform, Westman","24 gauge",null,null,"Includes all styles of panel and tile at 24 gauge","CAN",null,1390,"92.9m2",{"$f":"(K147/92.9)","v":14.962325080731969},"m2","4786662040.101.1 ","UL Env.",2021,8030,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,6.0999999999999997E-4,null,null,null,null,142,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS147:$BB147,0))","v":false}]
[{"$f":"B148&\" / \"&C148&\" / \"&E148","v":"Metal Panels - Steel / Metal Building Manufacturers Assn / 24 gauge"},"Metal Panels - Steel","Metal Building Manufacturers Assn","See all members","24 gauge",null,null,"Avg of roof and wall panels","USA",null,1221.7,"92.9m2",{"$f":"(K148/92.9)","v":13.150699677072121},"m2","4786774590.103.1 ","UL Env.",2021,8030,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,6.0999999999999997E-4,null,null,null,null,143,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS148:$BB148,0))","v":false}]
[{"$f":"B149&\" / \"&C149&\" / \"&E149","v":"Metal Panels - Steel / Metal Construction Assn. / 24 gauge"},"Metal Panels - Steel","Metal Construction Assn.","Includes: ATAS, DMI, Englert, Fabral,McElroy, Pac-Clad","24 gauge",null,null,null,"USA",null,1530,"100m2",{"$f":"(K149/100)","v":15.3},"m2","4789289084.103.1 ","UL Env.",2025,8030,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,6.0999999999999997E-4,null,null,null,null,144,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS149:$BB149,0))","v":false}]
[{"$f":"B150&\" / \"&C150&\" / \"&D150&\" / \"&E150","v":"Metal Panels - Steel / Petersen Aluminum Corp / PAC-CLAD / 24 gauge"},"Metal Panels - Steel","Petersen Aluminum Corp","PAC-CLAD","24 gauge",null,null,null,"USA",null,3492.7,"92.9m2",{"$f":"(K150/92.9)","v":37.596340150699675},"m2","4786652606.101.2","UL Env.",2020,4.67,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,145,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS150:$BB150,0))","v":false}]
["MgO board 1/2\" / North American MgO / MagTech Ultra / 1/2\"","MgO board 1/2\"","North American MgO","MagTech Ultra","1/2\"",null,null,null,"USA",null,7.4,"m2",{"$f":"(7.4)","v":7.4},"m2","SCS-EPD-04873","SCS Global",2023,1000,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,146,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS151:$BB151,0))","v":false}]
["Mineral wool batt / Owens Corning / Thermafiber UltraBatt / R 4.3/inch","Mineral wool batt","Owens Corning","Thermafiber UltraBatt","R 4.3/inch",null,null,null,"USA & CAN",null,4,"m2 RSI 1",{"$f":"(4)","v":4},"m2 RSI 1","4788956323.103.1 ","UL Env.",2024,64,"kg/m3",null,null,4.3,{"$f":"5.678*0.0254/V152","v":3.3539813953488373E-2},"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,147,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS152:$BB152,0))","v":false}]
["Mineral wool batt / Rockwool / Safe'n'Sound, ComfortBatt / R 3.8/inch","Mineral wool batt","Rockwool","Safe'n'Sound, ComfortBatt","R 3.8/inch",null,null,null,"USA & CAN",null,1.31,"m2 RSI 1",{"$f":"(1.31)","v":1.31},"m2 RSI 1","4789092768.101.1 ","UL Env.",2024,32,"kg/m3",null,null,3.8,{"$f":"5.678*0.0254/V153","v":3.7952947368421051E-2},"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,148,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS153:$BB153,0))","v":false}]
[{"$f":"B154&\" / \"&C154&\" / \"&E154","v":"Mineral wool board - heavy density / NAIMA / R 4.2/inch"},"Mineral wool board - heavy density","NAIMA","Includes: Rolan, Armstrong, Rockwool, Thermafiber, American Rock Wool, IIG, Delta, USG","R 4.2/inch",null,null,null,"USA & CAN",null,8.16,"m2 RSI 1",{"$f":"(8.16)","v":8.16},"m2 RSI 1","4788703029.101.2","UL Env.",2023,123.5,"kg/m3",null,null,4.2,{"$f":"5.678*0.0254/V154","v":3.4338380952380947E-2},"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,149,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS154:$BB154,0))","v":false}]
["Mineral wool board / Rockwool / Rockboard 60 / R 4.3/inch","Mineral wool board","Rockwool","Rockboard 60","R 4.3/inch",null,null,null,"USA & CAN",null,2.88,"m2 RSI 1",{"$f":"(2.88)","v":2.88},"m2 RSI 1","4789092768.101.2","UL Env.",2024,96,"kg/m3",null,null,4.3,{"$f":"5.678*0.0254/V155","v":3.3539813953488373E-2},"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,150,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS155:$BB155,0))","v":false}]
[{"$f":"B156&\" / \"&C156&\" / \"&E156","v":"Mineral wool board - light density / NAIMA / R 3.7/inch"},"Mineral wool board - light density","NAIMA","Includes: Rolan, Armstrong, Rockwool, Thermafiber, American Rock Wool, IIG, Delta, USG","R 3.7/inch",null,null,null,"USA & CAN",null,3.33,"m2 RSI 1",{"$f":"(3.33)","v":3.33},"m2 RSI 1","4788703029.101.1 ","UL Env.",2023,44.1,"kg/m3",null,null,3.7,{"$f":"5.678*0.0254/V156","v":3.8978702702702699E-2},"W/(mK)",null,null,null,null,null,null,null,null,null,null,null,null,null,151,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS156:$BB156,0))","v":false}]
[{"$f":"B157&\" / \"&C157&\" / \"&E157","v":"Mineral wool loose fill / NAIMA / R 3/inch"},"Mineral wool loose fill","NAIMA","Includes: Rolan, Armstrong, Rockwool, Thermafiber, American Rock Wool, IIG, Delta, USG","R 3/inch",null,null,null,"USA & CAN",null,1.56,"m2 RSI 1",{"$f":"(1.56)","v":1.56},"m2 RSI 1","4788703029.102.1 ","UL Env.",2023,23.1,"kg/m3",null,null,3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,152,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS157:$BB157,0))","v":false}]
["Mycelium board / Ecovative / Mycofoam / R 3.7/inch","Mycelium board","Ecovative","Mycofoam","R 3.7/inch",null,null,null,"USA",null,275.38,"m3",{"$f":"(K158*W158)","v":10.73982},"m2 RSI1","New York State Pollution Prevention Institute LCA, 2013",null,"",121,"kg/m3",4.7190000000000003,"kg/m2 at RSI1",{"$f":"1/W158*0.0254*5.678","v":3.6979794871794871},3.9E-2,"W/(mK)",1,0.5,{"$f":"(T158*Y158*Z158*3.67)*rng_biogenic_storage","v":7.793428500000001},null,null,null,null,null,null,null,null,null,null,153,null,null,null,"Independent LCA, 2013",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS158:$BB158,0))","v":false}]
[{"$f":"B159&\" / \"&C159&\" / \"&D159&\" / \"&E159","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 1/2\""},"OSB sheathing","American Wood Council & Canadian Wood Council",null,"1/2\"",null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,242.58,"m3",{"$f":"(K159*0.0127)","v":3.0807660000000001},"m2 at 0.0127 m (1/2\")","4788424634.101.1 ","UL Env.",2025,620,"kg/m3",{"$f":"R159*0.0127","v":7.8739999999999997},"kg/m2 at 1/2\"",null,null,null,0.95799999999999996,0.5,null,null,0.82499999999999996,{"$f":"T159*Y159*Z159","v":3.7716459999999996},null,null,1.2699999999999999E-2,null,null,null,null,154,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS159:$BB159,0))","v":false}]
[{"$f":"B160&\" / \"&C160&\" / \"&D160&\" / \"&E160","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 5/8\""},"OSB sheathing","American Wood Council & Canadian Wood Council",null,"5/8\"",null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,242.58,"m3",{"$f":"(K160*0.01588)","v":3.8521703999999999},"m2 at 0.0159 m (5/8\")","4788424634.101.1 ","UL Env.",2025,620,"kg/m3",{"$f":"R160*0.01588","v":9.8455999999999992},"kg/m2 at 5/8\"",null,null,null,0.95799999999999996,0.5,null,null,0.82499999999999996,{"$f":"T160*Y160*Z160","v":4.7160423999999992},null,null,1.5900000000000001E-2,null,null,null,null,155,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS160:$BB160,0))","v":false}]
[{"$f":"B161&\" / \"&C161&\" / \"&D161&\" / \"&E161","v":"OSB sheathing / Huber  / AdvanTech / 1/2\" Sheathing"},"OSB sheathing","Huber ","AdvanTech","1/2\" Sheathing",null,null,"No biogenic carbon credited","US","2023-02-26",420,"m3",5.3340106680213362,"m2 @ 1/2\"","4789103593.101.1","UL",2025,662,"kg/m3",8.407,"kg/m2 at 1/2\"",78.739999999999995,"m2 @ 1/2'' / m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,156,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS161:$BB161,0))","v":false}]
["(ARCHIVED 2023) OSB sheathing / Huber / AdvanTech / 1/2\" Sheathing","(ARCHIVED 2023) OSB sheathing","Huber","AdvanTech","1/2\" Sheathing",null,null,"Wood biogenic carbon storage set to zero","USA",null,6.6,"m2",{"$f":"(6.6)","v":6.6},"m2","4786451831.101.1 ","UL Env.",2019,8.3919999999999995,"kg/m2 at 1/2\"",null,null,null,null,null,0.92500000000000004,0.5,null,"m2 at product thickness",0.82499999999999996,{"$f":"R162*Y162*Z162","v":3.8813},null,null,1.2699999999999999E-2,null,null,null,null,"156_Archived",null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS162:$BB162,0))","v":false}]
[{"$f":"B163&\" / \"&C163&\" / \"&D163&\" / \"&E163","v":"OSB sheathing / Huber  / ZIP System / 7/16\" Sheathing, protective barrier and tape"},"OSB sheathing","Huber ","ZIP System","7/16\" Sheathing, protective barrier and tape",null,null,"No biogenic carbon credited","US","2023-02-26",380,"m²",4.2222222222222223,"m2 @  7/16\"","4789103593.102.1","UL",2025,660,"kg/m3",7.26,"kg/m2 at  7/16\"",90,"m2 @ 7/16'' / m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,157,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS163:$BB163,0))","v":false}]
["(ARCHIVED 2023) OSB sheathing / Huber / ZIP System / 7/16\" Sheathing, protective barrier and tape","(ARCHIVED 2023) OSB sheathing","Huber","ZIP System","7/16\" Sheathing, protective barrier and tape",null,null,"Wood biogenic carbon storage set to zero","USA",null,4,"m2",{"$f":"(4)","v":4},"m2","4786451831.103.1 ","UL Env.",2019,8.3919999999999995,"kg/m2 at 1/2\"",{"$f":"(7/16)/0.5*R164","v":7.343},"kg/m2 at 7/16\"",null,null,null,0.92500000000000004,0.5,null,"m2 at product thickness",0.82499999999999996,{"$f":"T164*Y164*Z164","v":3.3961375},null,null,null,null,null,null,null,"157_Archived",null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS164:$BB164,0))","v":false}]
[{"$f":"B165&\" / \"&C165&\" / \"&D165&\" / \"&E165","v":"OSB subflooring / Huber  / AdvanTech / 19/32\" Subflooring"},"OSB subflooring","Huber ","AdvanTech","19/32\" Subflooring",null,null,"No biogenic carbon credited","US","2023-02-26",470,"m3",7.0879203740009045,"m2 @ 19/32\"","4789103593.101.1","UL",2025,670,"kg/m3",10.119999999999999,"kg/m2 at 1/2\"",66.31,"m2 @ 19/32'' / m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,158,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS165:$BB165,0))","v":false}]
["(ARCHIVED 2023) OSB subflooring / Huber / AdvanTech / 19/32\" Subflooring","(ARCHIVED 2023) OSB subflooring","Huber","AdvanTech","19/32\" Subflooring",null,null,"Wood biogenic carbon storage set to zero","USA",null,6.6,"m2",{"$f":"(6.6)","v":6.6},"m2","4786451831.101.2","UL Env.",2019,8.3919999999999995,"kg/m2 at 1/2\"",{"$f":"(19/32)/0.5*R162","v":9.9654999999999987},"kg/m2 at 19/32\"",null,null,null,0.92500000000000004,0.5,null,"m2 at product thickness",0.82499999999999996,{"$f":"T166*Y166*Z166","v":4.6090437499999997},null,null,1.5081000000000001E-2,null,null,null,null,"158_Archived",null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS166:$BB166,0))","v":false}]
["Plywood / American Wood Council & Canadian Wood Council /  / 1/2\"","Plywood","American Wood Council & Canadian Wood Council",null,"1/2\"",null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,219.32,"m3",{"$f":"(K167*0.0127)","v":2.785364},"m2 at 1/2\"","4788424634.103.1 ","UL Env.",2025,484,"kg/m3",{"$f":"R167*0.0127","v":6.1467999999999998},"kg/m2 at 1/2\"",null,null,null,0.97099999999999997,0.5,null,null,0.82499999999999996,{"$f":"T167*Y167*Z167","v":2.9842713999999999},null,null,1.2699999999999999E-2,null,null,null,null,159,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS167:$BB167,0))","v":false}]
[{"$f":"B168&\" / \"&C168&\" / \"&D168&\" / \"&E168","v":"Plywood / American Wood Council & Canadian Wood Council /  / 5/8\""},"Plywood","American Wood Council & Canadian Wood Council",null,"5/8\"",null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,219.32,"m3",{"$f":"(K168*0.0159)","v":3.4871880000000002},"m2 at 5/8\"","4788424634.103.1 ","UL Env.",2025,484,"kg/m3",{"$f":"R168*0.0159","v":7.6956000000000007},"kg/m2 at 5/8\"",null,null,null,0.97099999999999997,0.5,null,null,0.82499999999999996,{"$f":"T168*Y168*Z168","v":3.7362138000000003},null,null,1.5900000000000001E-2,null,null,null,null,160,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS168:$BB168,0))","v":false}]
[{"$f":"B169&\" / \"&C169&\" / \"&D169&\" / \"&E169","v":"Plywood / American Wood Council & Canadian Wood Council /  / 3/4\""},"Plywood","American Wood Council & Canadian Wood Council",null,"3/4\"",null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,219.32,"m3",{"$f":"(K169*0.01905)","v":4.1780460000000001},"m2 at 3/4\"","4788424634.103.1 ","UL Env.",2025,484,"kg/m3",{"$f":"R169*0.01905","v":9.2202000000000002},"kg/m2 at 3/4\"",null,null,null,0.97099999999999997,0.5,null,null,0.82499999999999996,{"$f":"T169*Y169*Z169","v":4.4764071000000003},null,null,1.5900000000000001E-2,null,null,null,null,161,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS169:$BB169,0))","v":false}]
[{"$f":"B170&\" / \"&C170&\" / \"&D170&\" / \"&E170","v":"Polyiso - roof boards / Carlisle / GRF cellulosic facer / R 5.8/inch"},"Polyiso - roof boards","Carlisle","GRF cellulosic facer","R 5.8/inch",null,null,null,"US & CA",null,2.1800000000000002,"m2•RSI",2.1800000000000002,"m2•RSI","EPD 255","ASTM International",2026,28.92,"kg/m3",null,null,5.8,2.4865724137931033E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,162,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS170:$BB170,0))","v":false}]
["(ARCHIVED 2023) Polyiso - roof boards / Carlisle / InsulBase, SecurShield, StormBase / R 5.8/inch","(ARCHIVED 2023) Polyiso - roof boards","Carlisle","InsulBase, SecurShield, StormBase","R 5.8/inch",null,null,null,"USA",null,2.41,"m2 RSI 1",{"$f":"(2.41)","v":2.41},"m2 RSI 1","4789092768.101.1 ","UL Env.",2022,28.92,"kg/m3",null,null,5.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"162_Archived",null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS171:$BB171,0))","v":false}]
["Polyiso - roof boards / Hunter / Polysio Roof insulation boards / R 5.8/inch","Polyiso - roof boards","Hunter","Polysio Roof insulation boards","R 5.8/inch",null,null,null,"US",null,2.1800000000000002,"m2•RSI",2.1800000000000002,"m2•RSI","EPD 271","ASTM International",2026,28.92,"kg/m3",null,null,5.8,{"$f":"0.0254*5.678/V172","v":2.4865724137931033E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,163,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS172:$BB172,0))","v":false}]
["(ARCHIVED 2023) Polyiso - roof boards / Hunter / H-Shield products / R 5.8/inch","(ARCHIVED 2023) Polyiso - roof boards","Hunter","H-Shield products","R 5.8/inch",null,null,null,"USA",null,2.41,"m2 RSI 1",{"$f":"(2.41)","v":2.41},"m2 RSI 1","4788092227.101.1 ","UL Env.",2022,28.92,"kg/m3",null,null,5.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"163_Archived",null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS173:$BB173,0))","v":false}]
["Polyiso - roof boards / PIMA / Includes: Atlas, Firestone, GAF, Johns Manville, Rmax / R 5.8/inch","Polyiso - roof boards","PIMA","Includes: Atlas, Firestone, GAF, Johns Manville, Rmax","R 5.8/inch",null,null,null,"USA",null,2.8,"m2 RSI 1",{"$f":"(2.8)","v":2.8},"m2 RSI 1","EPD10043 ","NSF",2020,28.92,"kg/m3",null,null,5.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,164,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS174:$BB174,0))","v":false}]
["Polyiso - roof boards / Versico / VersiCore, SecurShield, DuraFaceR / R 5.8/inch","Polyiso - roof boards","Versico","VersiCore, SecurShield, DuraFaceR","R 5.8/inch",null,null,null,"USA",null,2.41,"m2 RSI 1",{"$f":"(2.41)","v":2.41},"m2 RSI 1","4787622255.104.1 ","UL Env.",2022,28.92,"kg/m3",null,null,5.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,165,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS175:$BB175,0))","v":false}]
["Polyiso - wall boards / Dow Chemical Company / Tuff-R, Super Tuff-R, Thermax / R 6.5/inch","Polyiso - wall boards","Dow Chemical Company","Tuff-R, Super Tuff-R, Thermax","R 6.5/inch",null,null,null,"USA",null,4.01,"m2 RSI 1",{"$f":"(4.01)","v":4.01},"m2 RSI 1","4786101271.101.1 ","UL Env.",2019,null,null,null,null,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,166,null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS176:$BB176,0))","v":false}]
["Polyiso - wall boards / Hunter / Polysio Wall insulation boards / R 6.5/inch","Polyiso - wall boards","Hunter","Polysio Wall insulation boards","R 6.5/inch",null,null,null,"US",null,4.2510000000000003,"m2•RSI",4.2510000000000003,"m2•RSI","EPD 253","ASTM International",2026,33.729999999999997,"kg/m3",null,null,6.5,{"$f":"0.0254*5.678/V177","v":2.2187876923076923E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,167,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS177:$BB177,0))","v":false}]
["(ARCHIVED 2023) Polyiso - wall boards / Hunter / Xci / R 6.5/inch","(ARCHIVED 2023) Polyiso - wall boards","Hunter","Xci","R 6.5/inch",null,null,null,"USA",null,2.27,"m2 RSI 1",{"$f":"(2.27)","v":2.27},"m2 RSI 1","4788092227.102.1 ","UL Env.",2022,33.729999999999997,"kg/m3",null,null,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"167_Archived",null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS178:$BB178,0))","v":false}]
["Polyiso - wall boards / PIMA / Includes: Atlas, Firestone, GAF, Johns Manville, Rmax / R 6.5/inch","Polyiso - wall boards","PIMA","Includes: Atlas, Firestone, GAF, Johns Manville, Rmax","R 6.5/inch",null,null,null,"USA",null,2.3199999999999998,"m2 RSI 1",{"$f":"(2.32)","v":2.3199999999999998},"m2 RSI 1","EPD10042 ","NSF",2020,34,"kg/m3",null,null,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,168,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS179:$BB179,0))","v":false}]
[{"$f":"B180&\" / \"&C180&\" / \"&D180&\" / \"&E180","v":"Polypropylene siding / Novik / NovikStone, NovikShake / Avg of 5 products"},"Polypropylene siding","Novik","NovikStone, NovikShake","Avg of 5 products",null,null,null,"CAN",null,27.04,"100 ft2",{"$f":"(K180/9.29)","v":2.9106566200215287},"m2","4332-7381","CSA",2022,2.4500000000000002,"kg/m2",9.2899999999999991,"m2/100ft2",null,null,null,null,null,null,null,null,null,null,null,9.1999999999999998E-2,null,null,null,null,169,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS180:$BB180,0))","v":false}]
[{"$f":"B181&\" / \"&C181&\" / \"&D181&\" / \"&E181","v":"Polypropylene siding / Vinyl Siding Institute  /  / 0.085\" Single 7\" wood Shake appearance"},"Polypropylene siding","Vinyl Siding Institute ",null,"0.085\" Single 7\" wood Shake appearance",null,null,null,"US & CA",null,9.81,"m2",9.81,"m²","EPD 327","ASTM International",2027,1025,"kg/m3",9.2899999999999991,"m2/100ft2",null,null,null,null,null,null,null,null,null,null,null,null,null,2.1589999999999999E-3,null,null,170,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS181:$BB181,0))","v":false}]
["(ARCHIVED 2023) Polypropylene siding / Vinyl Siding Institute /  / 0.085\" Single 7\" \"Cedar\" Shake","(ARCHIVED 2023) Polypropylene siding","Vinyl Siding Institute",null,"0.085\" Single 7\" \"Cedar\" Shake",null,null,null,"USA & CAN",null,63.42,"100 ft2",{"$f":"(K182/9.29)","v":6.8266953713670624},"m2","4787108620.103.1 ","UL Env.",2021,1030,"kg/m3",9.2899999999999991,"m2/100ft2",null,null,null,null,null,null,null,null,null,null,null,2.1589999999999999E-3,null,null,null,null,"170_Archived",null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS182:$BB182,0))","v":false}]
["Polypropylene ICF webbing /  /  / ","Polypropylene ICF webbing",null,null,null,null,null,"ICE database is 1.93, CDN database is 1.9","EU",null,1.93,"kg",{"$f":"(K183*T183)","v":5.1219979818365289},"m2 of ICF block","ICE V3.0, 2019",null,"",1030,"kg/m3",{"$f":"1.315/0.4955","v":2.6538849646821392},"kg/m2 at 1.315 kg webbing per 0.4955 m2 block",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,171,null,null,null,"ICE Database (UK)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS183:$BB183,0))","v":false}]
["PVC Roofing Membrane / CIFA / Includes: Canadian General-Tower, Duro-Last, FiberTite / 48 mils","PVC Roofing Membrane","CIFA","Includes: Canadian General-Tower, Duro-Last, FiberTite","48 mils",null,null,"Installed","USA & CAN",null,4.26,"m2",{"$f":"(4.26)","v":4.26},"m2","EPD‐009 ","ASTM",2019,1.4630000000000001,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,172,null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS184:$BB184,0))","v":false}]
["Rammed earth /  / Stabilized with 3% NHL / ","Rammed earth",null,"Stabilized with 3% NHL",null,null,null,"Includes hydraulic ramming on site","EU",null,47.5,"m3",{"$f":"(K185*T185)","v":1.2064999999999999},"m2 at 1\"","Fernandes et al LCA, 2020",null,"",1900,"kg/m3",2.5399999999999999E-2,"m/1\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,173,null,null,null,"Peer-reviewed LCA",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS185:$BB185,0))","v":false}]
["Rammed earth /  / Stabilized with 5% cement / ","Rammed earth",null,"Stabilized with 5% cement",null,null,null,null,"EU",null,6.0999999999999999E-2,"kg",{"$f":"(K186*T186)","v":2.9438599999999999},"m2 at 1\"","ICE V3.0, 2019",null,"",1900,"kg/m3",{"$f":"R186*0.0254","v":48.26},"kg/m2-1\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,174,null,null,null,"ICE Database (UK)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS186:$BB186,0))","v":false}]
["Rammed earth /  / Stabilized with 8% cement / ","Rammed earth",null,"Stabilized with 8% cement",null,null,null,null,"EU",null,8.4000000000000005E-2,"kg",{"$f":"(K187*T187)","v":4.0538400000000001},"m2 at 1\"","ICE V3.0, 2020",null,"",1900,"kg/m3",{"$f":"R187*0.0254","v":48.26},"kg/m2-1\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,175,null,null,null,"ICE Database (UK)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS187:$BB187,0))","v":false}]
["Rebar / Concrete Reinforcing Steel Institute /  / 10M","Rebar","Concrete Reinforcing Steel Institute",null,"10M",null,null,null,"USA & CAN",null,0.97899999999999998,"kg",{"$f":"(K188*T188)","v":0.76851500000000006},"m","EPD 070","ASTM",2022,7850,"kg/m3",0.78500000000000003,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,176,null,null,null,{"$f":"IF(LEN(Q188)=4,IF(Q188<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q188),\"\"),\"\")","v":"Expired 2022"},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS188:$BB188,0))","v":false}]
["Rebar / Concrete Reinforcing Steel Institute /  / 15M","Rebar","Concrete Reinforcing Steel Institute",null,"15M",null,null,null,"USA & CAN",null,0.97899999999999998,"kg",{"$f":"(K189*T189)","v":1.5370300000000001},"m","EPD 069","ASTM",2022,7850,"kg/m3",1.57,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,177,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS189:$BB189,0))","v":false}]
["Rubber flooring / ECOsurfaces / ECOsurfaces / ","Rubber flooring","ECOsurfaces","ECOsurfaces",null,null,null,null,"USA",null,5.9,"m2",{"$f":"(5.9)","v":5.9},"m2","SCS-EPD-03576","SCS Global",2020,7.476,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,5.7000000000000002E-3,null,null,null,null,178,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS190:$BB190,0))","v":false}]
["Rubber flooring / Resilient Floor Covering Institute / Includes tiles and rolls from American Biltrite, Armstrong, Burke, FLEXCO, Johnsonite, Mannington, Roppe, Tarkett / ","Rubber flooring","Resilient Floor Covering Institute","Includes tiles and rolls from American Biltrite, Armstrong, Burke, FLEXCO, Johnsonite, Mannington, Roppe, Tarkett",null,null,null,null,"USA & CAN",null,15.6,"m2",{"$f":"(15.6)","v":15.6},"m2","4788753451.104.1 ","UL Env.",2024,5.6,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,2E-3,null,null,null,null,179,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS191:$BB191,0))","v":false}]
["SBS Modified Bitumen Roofing / ARMA / Includes: CertainTeed, Firestone, GAF, Henry, IKO, Johns Mansville, Malarkey, Siplast, Soprema / ","SBS Modified Bitumen Roofing","ARMA","Includes: CertainTeed, Firestone, GAF, Henry, IKO, Johns Mansville, Malarkey, Siplast, Soprema",null,null,null,"Installed","USA & CAN",null,6.7,"m2",{"$f":"(6.7)","v":6.7},"m2","4787168709.104.1 ","UL Env.",2021,8.4,"kg/m2",null,null,null,null,null,0.04,null,null,null,null,null,null,null,null,null,null,null,null,180,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS192:$BB192,0))","v":false}]
["SIP panel - EPS foam core /  /  / 7/16\" OSB, Type II EPS","SIP panel - EPS foam core",null,null,"7/16\" OSB, Type II EPS",null,null,null,"USA & CAN",null,null,null,{"$f":"((M58*1.75)+M93)","v":4.0142007534983852},"m2 at 1\"",null,null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,181,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS193:$BB193,0))","v":false}]
["SIP panel - Straw core / Agriboard / Agriboard 7-7/8\" / R?/inch","SIP panel - Straw core","Agriboard","Agriboard 7-7/8\"","R?/inch",null,null,null,"USA",null,-4.3999999999999997E-2,"m2",null,null,"Beck LCA",null,"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,182,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS194:$BB194,0))","v":false}]
["Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch","Spray polyurethane foam - Closed Cell (HFC)","SPFA",null,"R 6.6/inch",null,null,"Includes: Accella, BASF, DAP, Demilec, Dow, Gaco Western, General Coatings, ICP, Icynene Lapolla, Johns Manville, NCFI, SES","USA & CAN",null,13.16,"m2 RSI 1",{"$f":"(K195)","v":13.16},"m2 RSI 1","EPD-087","ASTM",2023,31.2,"kg/m3",null,null,6.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,183,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS195:$BB195,0))","v":false}]
["Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch","Spray polyurethane foam - Closed Cell - HFO gas filled","SPFA",null,"R 6.6/inch",null,null,"Includes: Accella, BASF, DAP, Demilec, Dow, Gaco Western, General Coatings, ICP, Icynene Lapolla, Johns Manville, NCFI, SES","US & CA",null,3.47,"m2•RSI",3.47,"m2•RSI","EPD 070 ","ASTM",2027,31.2,"kg/m3",null,null,6.6,{"$f":"0.0254*5.678/V196","v":2.1851696969696969E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,184,null,null,null,{"$f":"IF(LEN(Q196)=4,IF(Q196<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q196),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS196:$BB196,0))","v":false}]
["(ARCHIVED 2023) Spray polyurethane foam - Closed Cell (HFO) / SPFA /  / R 6.6/inch","(ARCHIVED 2023) Spray polyurethane foam - Closed Cell (HFO)","SPFA",null,"R 6.6/inch",null,null,"Includes: Accella, BASF, DAP, Demilec, Dow, Gaco Western, General Coatings, ICP, Icynene Lapolla, Johns Manville, NCFI, SES","USA & CAN",null,4.16,"m2 RSI 1",4.16,"m2 RSI 1","EPD-085 ","ASTM",2023,31.2,"kg/m3",null,null,6.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"184_Archived",null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS197:$BB197,0))","v":false}]
["Spray polyurethane foam - High Density (HFC) / SPFA /  / R 6.3/inch","Spray polyurethane foam - High Density (HFC)","SPFA",null,"R 6.3/inch",null,null,"Includes: Accella, BASF, DAP, Demilec, Dow, Gaco Western, General Coatings, ICP, Icynene Lapolla, Johns Manville, NCFI, SES","USA & CAN",null,17.02,"m2 RSI 1",17.02,"m2 RSI 1","EPD-087","ASTM",2023,52,"kg/m3",null,null,6.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,185,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS198:$BB198,0))","v":false}]
["Spray polyurethane foam - High Density - HFO gas filled / SPFA /  / R 6.5/inch","Spray polyurethane foam - High Density - HFO gas filled","SPFA",null,"R 6.5/inch",null,null,"Includes: Accella, BASF, DAP, Demilec, Dow, Gaco Western, General Coatings, ICP, Icynene Lapolla, Johns Manville, NCFI, SES","US & CA",null,4.05,"m2•RSI",4.05,"m2•RSI","EPD 070","ASTM",2027,52,"kg/m3",null,null,6.5,{"$f":"0.0254*5.678/V199","v":2.2187876923076923E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,186,null,null,null,{"$f":"IF(LEN(Q199)=4,IF(Q199<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q199),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS199:$BB199,0))","v":false}]
["(ARCHIVED 2023) Spray polyurethane foam - High Density (HFO) / SPFA /  / R 6.5/inch","(ARCHIVED 2023) Spray polyurethane foam - High Density (HFO)","SPFA",null,"R 6.5/inch",null,null,"Includes: Accella, BASF, DAP, Demilec, Dow, Gaco Western, General Coatings, ICP, Icynene Lapolla, Johns Manville, NCFI, SES","USA & CAN",null,4.95,"m2 RSI 1",4.95,"m2 RSI 1","EPD-085 ","ASTM",2023,52,"kg/m3",null,null,6.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"186_Archived",null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS200:$BB200,0))","v":false}]
["Spray polyurethane foam - Open Cell (HFC) / SPFA /  / R 4.1/inch","Spray polyurethane foam - Open Cell (HFC)","SPFA",null,"R 4.1/inch",null,null,"Includes: Accella, BASF, DAP, Demilec, Dow, Gaco Western, General Coatings, ICP, Icynene Lapolla, Johns Manville, NCFI, SES","USA & CAN",null,1.66,"m2 RSI 1",1.66,"m2 RSI 1","EPD-087","ASTM",2023,9.6,"kg/m3",null,null,4.0999999999999996,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,187,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS201:$BB201,0))","v":false}]
["Spray polyurethane foam - Open Cell - HFO gas / SPFA /  / R 4.1/inch","Spray polyurethane foam - Open Cell - HFO gas","SPFA",null,"R 4.1/inch",null,null,"Includes: Accella, BASF, DAP, Demilec, Dow, Gaco Western, General Coatings, ICP, Icynene Lapolla, Johns Manville, NCFI, SES","US & CA",null,1.42,"m2•RSI",1.42,"m2•RSI","EPD 070","ASTM",2027,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,188,null,null,null,{"$f":"IF(LEN(Q202)=4,IF(Q202<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q202),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS202:$BB202,0))","v":false}]
["(ARCHIVED 2023) Spray polyurethane foam - Open Cell (HFO) / SPFA /  / R 4.1/inch","(ARCHIVED 2023) Spray polyurethane foam - Open Cell (HFO)","SPFA",null,"R 4.1/inch",null,null,"Includes: Accella, BASF, DAP, Demilec, Dow, Gaco Western, General Coatings, ICP, Icynene Lapolla, Johns Manville, NCFI, SES","USA & CAN",null,1.66,"m2 RSI 1",1.66,"m2 RSI 1","EPD-085 ","ASTM",2023,9.6,"kg/m3",null,null,4.0999999999999996,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"188_Archived",null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS203:$BB203,0))","v":false}]
[{"$f":"B204&\" / \"&E204&\" / \"&C204","v":"Steel beam / W150x22 (W6x15) / American Institute of Steel Construction"},"Steel beam","American Institute of Steel Construction","Hot-rolled strucutural steel","W150x22 (W6x15)",null,null,null,"USA",null,1.1599999999999999,"kg",{"$f":"(K204*T204)","v":26.099999999999998},"linear m","4786979051.102.1 ","UL Env.",2021,7800,"kg/m3",22.5,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,189,null,null,null,{"$f":"IF(LEN(Q204)=4,IF(Q204<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q204),\"\"),\"\")","v":"Expired 2021"},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS204:$BB204,0))","v":false}]
[{"$f":"B205&\" / \"&E205&\" / \"&C205","v":"Steel beam / W200x22 (W8x15) / American Institute of Steel Construction"},"Steel beam","American Institute of Steel Construction","Hot-rolled strucutural steel","W200x22 (W8x15)",null,null,null,"USA",null,1.1599999999999999,"kg",26.099999999999998,"linear m","4786979051.102.1 ","UL Env.",2021,7800,"kg/m3",22.5,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,190,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS205:$BB205,0))","v":false}]
["Steel beam / W200x27 (W8x18) / American Institute of Steel Construction","Steel beam","American Institute of Steel Construction","Hot-rolled strucutural steel","W200x27 (W8x18)",null,null,null,"USA",null,1.1599999999999999,"kg",30.855999999999998,"linear m","4786979051.102.1 ","UL Env.",2021,7800,"kg/m3",26.6,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,191,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS206:$BB206,0))","v":false}]
["Steel beam / W200x31 (W8x21) / American Institute of Steel Construction","Steel beam","American Institute of Steel Construction","Hot-rolled strucutural steel","W200x31 (W8x21)",null,null,null,"USA",null,1.1599999999999999,"kg",36.308,"linear m","4786979051.102.1 ","UL Env.",2021,7800,"kg/m3",31.3,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,192,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS207:$BB207,0))","v":false}]
["Steel beam / W250x25 (W10x17) / American Institute of Steel Construction","Steel beam","American Institute of Steel Construction","Hot-rolled strucutural steel","W250x25 (W10x17)",null,null,null,"USA",null,1.1599999999999999,"kg",29.347999999999999,"linear m","4786979051.102.1 ","UL Env.",2021,7800,"kg/m3",25.3,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,193,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS208:$BB208,0))","v":false}]
["Steel beam / W250x33 (W10x22) / American Institute of Steel Construction","Steel beam","American Institute of Steel Construction","Hot-rolled strucutural steel","W250x33 (W10x22)",null,null,null,"USA",null,1.1599999999999999,"kg",37.932000000000002,"linear m","4786979051.102.1 ","UL Env.",2021,7800,"kg/m3",32.700000000000003,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,194,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS209:$BB209,0))","v":false}]
["Steel beam / W250x39 (W10x26) / American Institute of Steel Construction","Steel beam","American Institute of Steel Construction","Hot-rolled strucutural steel","W250x39 (W10x26)",null,null,null,"USA",null,1.1599999999999999,"kg",44.66,"linear m","4786979051.102.1 ","UL Env.",2021,7800,"kg/m3",38.5,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,195,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS210:$BB210,0))","v":false}]
["Steel beam / W310x33 (W12x22) / American Institute of Steel Construction","Steel beam","American Institute of Steel Construction","Hot-rolled strucutural steel","W310x33 (W12x22)",null,null,null,"USA",null,1.1599999999999999,"kg",37.932000000000002,"linear m","4786979051.102.1 ","UL Env.",2021,7800,"kg/m3",32.700000000000003,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,196,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS211:$BB211,0))","v":false}]
["Steel beam / W310x39 (W12x26) / American Institute of Steel Construction","Steel beam","American Institute of Steel Construction","Hot-rolled strucutural steel","W310x39 (W12x26)",null,null,null,"USA",null,1.1599999999999999,"kg",44.66,"linear m","4786979051.102.1 ","UL Env.",2021,7800,"kg/m3",38.5,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,197,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS212:$BB212,0))","v":false}]
["Steel joist, open web / Steel Joist Institute /  / 12\" 12K3 joist","Steel joist, open web","Steel Joist Institute",null,"12\" 12K3 joist",null,null,null,"USA & CAN",null,1.38,"kg",11.703751836734694,"linear m","4786052959.101.1","UL Env.",2020,7800,"kg/m3",{"$f":"5.7/2.205*3.2808","v":8.4809795918367357},"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,198,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS213:$BB213,0))","v":false}]
["Steel post / Generic /  / 3.5 x 0.216\" (89 x 5.5 mm), Sched 40 STD","Steel post","Generic",null,"3.5 x 0.216\" (89 x 5.5 mm), Sched 40 STD",null,null,null,null,null,2.48,"kg",{"$f":"(T214*K214)","v":30.464320000000001},"m of pier length","11345278.101.2","UL Env.",2021,7800,"kg/m3",12.284000000000001,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,199,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS214:$BB214,0))","v":false}]
["Steel studs - Load bearing  / ClarkDietrich /  / 600-S-137-54, 16 gauge","Steel studs - Load bearing ","ClarkDietrich",null,"600-S-137-54, 16 gauge",null,null,null,"US","2023-02-26",2.38,"kg",6.1975199999999999,"m of \"2x6\" stud","4789752901.101.1","UL Environment",2026,7850,"kg/m3",2.6040000000000001,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS215:$BB215,0))","v":false}]
["(ARCHIVED 2023) Steel studs - Load bearing / ClarkDietrich /  / 600-S-137-54, 16 gauge","(ARCHIVED 2023) Steel studs - Load bearing","ClarkDietrich",null,"600-S-137-54, 16 gauge",null,null,null,"USA",null,2.39,"kg",6.2140000000000004,"m at 6\"","EPD10057","NSF",2020,7850,"kg/m3",2.6,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.6920000000000002,null,"200_Archived",null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS216:$BB216,0))","v":false}]
["Steel studs - Load bearing / MarinoWARE / Structural stud and track / 600-S-137-54, 16 gauge, \"2x6\"","Steel studs - Load bearing","MarinoWARE","Structural stud and track","600-S-137-54, 16 gauge, \"2x6\"",null,null,null,"US",null,2.48,"kg",6.4579200000000005,"m of \"2x6\" stud","4789995390.101.1","UL",2026,7800,"kg/m3",2.6040000000000001,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,201,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS217:$BB217,0))","v":false}]
["(ARCHIVED 2023) Steel studs - Load bearing / MarinoWARE / Structural stud and track / 600-S-137-54, 16 gauge","(ARCHIVED 2023) Steel studs - Load bearing","MarinoWARE","Structural stud and track","600-S-137-54, 16 gauge",null,null,null,"USA",null,2.41,"kg",6.2660000000000009,"m at 6\"","4786795523.101.1 ","UL Env.",2021,7800,"kg/m3",2.6,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.6920000000000002,null,"201_Archived",null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS218:$BB218,0))","v":false}]
["Steel studs - Load bearing / MBA Building Supplies /  / 600-S-137-54, 16 gauge","Steel studs - Load bearing","MBA Building Supplies",null,"600-S-137-54, 16 gauge",null,null,null,"USA",null,2.0099999999999998,"kg",5.226,"m at 6\"","SCS-EPD-04104","SCS Global",2021,7850,"kg/m3",2.6,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.6920000000000002,null,202,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS219:$BB219,0))","v":false}]
["Steel studs - Load bearing / Scafco /  / 600-S-137-54, 16 gauge","Steel studs - Load bearing","Scafco",null,"600-S-137-54, 16 gauge",null,null,null,"USA",null,3.29,"kg",8.5540000000000003,"m at 6\"","SCS-EPD05753","SCS Global",2024,7850,"kg/m3",2.6,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.6920000000000002,null,203,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS220:$BB220,0))","v":false}]
["Steel studs - Load bearing / Steel Recycling Institute /  / 600-S-137-54, 16 gauge","Steel studs - Load bearing","Steel Recycling Institute",null,"600-S-137-54, 16 gauge",null,null,null,"USA & CAN",null,2.2799999999999998,"kg",5.9279999999999999,"m at 6\"","SCS-EPD-03839","SCS Global",2021,7800,"kg/m3",2.6,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.6920000000000002,null,204,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS221:$BB221,0))","v":false}]
["Steel studs - Non-loadbearing / ClarkDietrich /  / 362-S-125-18, 20EQ gauge, \"2x4\"","Steel studs - Non-loadbearing","ClarkDietrich",null,"362-S-125-18, 20EQ gauge, \"2x4\"",null,null,null,"US","2023-02-26",2.38,"kg",1.4979284459999997,"m of \"2x6\" stud","4789752901.101.1","UL Environment",2026,7850,"kg/m3",0.62938169999999993,"kg/m",null,null,null,null,null,null,null,null,null,null,null,"72' = 21.95m","21.95m/5.946m2","9 studs/8x8 section",null,null,205,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS222:$BB222,0))","v":false}]
["(ARCHIVED 2023) Steel studs - Non-loadbearing / ClarkDietrich /  / 362-S-125-18, 20EQ gauge","(ARCHIVED 2023) Steel studs - Non-loadbearing","ClarkDietrich",null,"362-S-125-18, 20EQ gauge",null,null,null,"USA",null,2.39,"kg",1.5042222629999999,"m at 4\"","EPD10056 ","NSF",2020,7850,"kg/m3",{"$f":"0.423*1.4879","v":0.62938169999999993},"kg/m",null,null,null,null,null,null,null,null,null,null,null,"9 studs/8x8 section","72' = 21.95m","21.95m/5.946m2",3.6920000000000002,null,"205_Archived",null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS223:$BB223,0))","v":false}]
["Steel studs - Non-loadbearing / MarinoWARE / Viper Stud Viper 20 / 362-S-125-18, 20EQ gauge, \"2x4\"","Steel studs - Non-loadbearing","MarinoWARE","Viper Stud Viper 20","362-S-125-18, 20EQ gauge, \"2x4\"",null,null,null,"US",null,2.48,"kg",1.5608666159999998,"m of \"2x4\" stud","4789995390.101.1","UL",2026,7850,"kg/m3",0.62938169999999993,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,206,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS224:$BB224,0))","v":false}]
["(ARCHIVED 2023) Steel studs - Non-loadbearing / MarinoWARE / Viper Stud Viper 20 / 362-S-125-18, 20EQ gauge","(ARCHIVED 2023) Steel studs - Non-loadbearing","MarinoWARE","Viper Stud Viper 20","362-S-125-18, 20EQ gauge",null,null,null,null,null,2.41,"kg",1.5168098969999999,"m at 4\"","4786795523.101.0","UL Env.",2021,7850,"kg/m3",{"$f":"0.423*1.4879","v":0.62938169999999993},"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.6920000000000002,null,"206_Archived",null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS225:$BB225,0))","v":false}]
["Steel studs - Non-loadbearing / MBA Building Supplies /  / 362-S-125-18, 20EQ gauge, ProSTUD, ProTRAK","Steel studs - Non-loadbearing","MBA Building Supplies",null,"362-S-125-18, 20EQ gauge, ProSTUD, ProTRAK",null,null,null,"USA",null,2.0099999999999998,"kg",1.2650572169999996,"m at 4\"","SCS-EPD-04103 ","SCS Global",2021,7850,"kg/m3",{"$f":"0.423*1.4879","v":0.62938169999999993},"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.6920000000000002,null,207,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS226:$BB226,0))","v":false}]
["Steel studs - Non-loadbearing / Scafco /  / 362VS125-18, 20EQ gauge","Steel studs - Non-loadbearing","Scafco",null,"362VS125-18, 20EQ gauge",null,null,null,"USA",null,3.29,"kg",2.0706657929999999,"m at 4\"","SCS-EPD05752","SCS Global",2024,7850,"kg/m3",{"$f":"0.423*1.4879","v":0.62938169999999993},"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.6920000000000002,null,208,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS227:$BB227,0))","v":false}]
["Steel studs - Non-loadbearing / Steel Recycling Institute /  / 362-S-125-18, 20EQ gauge","Steel studs - Non-loadbearing","Steel Recycling Institute",null,"362-S-125-18, 20EQ gauge",null,null,null,"USA & CAN",null,2.2799999999999998,"kg",1.4349902759999997,"m at 4\"","SCS-EPD-03838","SCS Global",2021,7800,"kg/m3",{"$f":"0.423*1.4879","v":0.62938169999999993},"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.6920000000000002,null,209,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS228:$BB228,0))","v":false}]
["Straw Bale /  / Wheat & rye straw / R 3.3/inch","Straw Bale",null,"Wheat & rye straw","R 3.3/inch",null,null,null,"EU",null,7.79,"m3",{"$f":"(K229*W229)","v":0.34276000000000001},"m2 RSI 1","EPD-FASBA-2014-1-ECOINVENT","Construction EPD GmbH",2019,100,"kg/m3",{"$f":"R229/K229*M229","v":4.4000000000000004},"kg/m2-RSI1",{"$f":"0.0254*5.67826/W229","v":3.2779046363636364},4.3999999999999997E-2,"W/mK",0.99909999999999999,0.47,{"$f":"(T229*Y229*Z229*44/12)*rng_biogenic_storage","v":6.8182580399999999},"m2 RSI 1",null,null,null,null,null,null,null,null,null,210,null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS229:$BB229,0))","v":false}]
["Straw Panels / EcoCocon /  / R 2.9/inch","Straw Panels","EcoCocon",null,"R 2.9/inch",null,null,"Wood biogenic carbon storage set to zero","EU",null,8.8800000000000008,"m2",{"$f":"(K230*W230/0.4)","v":1.0965264550684932},"m2 RSI 1","VTT-CRM-158424-18","VTT Technical Research Centre",2023,63.2,"kg/m2",5,"kg/m2-RSI1",2.92,{"$f":"1/V230*0.0254*5.67826","v":4.9393083561643833E-2},"W/mK",0.99260000000000004,0.47,{"$f":"(40.62*Y230*Z230*44/12*W230/0.4)*rng_biogenic_storage","v":7.7220415837455176},"m2 RSI 1",null,null,null,{"$f":"T230*Y230*Z230*3.67","v":8.5606786999999986},null,null,null,null,null,211,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS230:$BB230,0))","v":false}]
["Acrylic Stucco Textured Finish / Sto / Stolit 1.0, Stolit 1.5, Stolit Freeform / ","Acrylic Stucco Textured Finish","Sto","Stolit 1.0, Stolit 1.5, Stolit Freeform",null,null,null,"Single application lifetime 10 years","USA",null,35,"m2",{"$f":"(K231)","v":35},"m2","01-001","Epsen",2024,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,212,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS231:$BB231,0))","v":false}]
["TPO Roofing Membrane / Carlisle /  / 60 mils","TPO Roofing Membrane","Carlisle",null,"60 mils",null,null,null,"USA",null,4.42,"m2",{"$f":"(4.42)","v":4.42},"m2","4787408569.102.1","UL Env.",2021,1.42,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,213,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS232:$BB232,0))","v":false}]
["Vacuum Insulated Panel / Porextherm / Vacupor / R 30/inch","Vacuum Insulated Panel","Porextherm","Vacupor","R 30/inch",null,null,null,"EU",null,42.2,"m2 at 25 mm",{"$f":"(K233/0.025*W233)","v":7.4272},"m2 RSI 1","EPD-POR-20140214-IBC1-EN ","IBU",2019,181,"kg/m3",null,null,30,4.4000000000000003E-3,"W/mK",null,null,null,null,null,null,null,null,null,null,null,null,null,214,null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS233:$BB233,0))","v":false}]
["Vinyl flooring / Altro / Altro Lavencia Click / ","Vinyl flooring","Altro","Altro Lavencia Click",null,null,null,null,"USA & CAN",null,14.2,"m2",{"$f":"(14.2)","v":14.2},"m2","SCS-EPD-05047","SCS Global",2024,9.7200000000000006,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,5.0000000000000001E-3,null,null,null,null,215,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS234:$BB234,0))","v":false}]
["Vinyl flooring / Altro / Altro Lavencia Plus / ","Vinyl flooring","Altro","Altro Lavencia Plus",null,null,null,null,"USA & CAN",null,9.6,"m2",{"$f":"(9.6)","v":9.6},"m2","SCS-EPD-05046","SCS Global",2023,5.64,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,3.0000000000000001E-3,null,null,null,null,216,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS235:$BB235,0))","v":false}]
["Vinyl flooring / Gerflor / Creation 70 CLIC / ","Vinyl flooring","Gerflor","Creation 70 CLIC",null,null,null,null,"USA",null,6.24,"m2",{"$f":"(6.24)","v":6.24},"m2","4786877674.101.1 ","UL Env.",2021,9.8949999999999996,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,6.0000000000000001E-3,null,null,null,null,217,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS236:$BB236,0))","v":false}]
["Vinyl flooring / Resilient Floor Covering Institute / Includes tile products from Armstrong, Congoleum, Tarkett / ","Vinyl flooring","Resilient Floor Covering Institute","Includes tile products from Armstrong, Congoleum, Tarkett",null,null,null,null,"USA & CAN",null,4.96,"m2",{"$f":"(4.96)","v":4.96},"m2","4788753451.105.1 ","UL Env.",2024,6.5,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,2.8E-3,null,null,null,null,218,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS237:$BB237,0))","v":false}]
["Vinyl Siding / Vinyl Siding Institute / Double 4.5\" products from: American Original, Associated Materials, CertainTeed, Novik, Ply Gem / 0.040\" Double 4.5\"","Vinyl Siding","Vinyl Siding Institute","Double 4.5\" products from: American Original, Associated Materials, CertainTeed, Novik, Ply Gem","0.040\" Double 4.5\"",null,null,null,"US & CA",null,4.71,"m2",4.71,"m²","EPD 325","ASTM",2027,1430,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,219,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS238:$BB238,0))","v":false}]
[{"$f":"B239&\" / \"&C239&\" / \"&E239","v":"(ARCHIVED 2023) Vinyl Siding / Vinyl Siding Institute / 0.040\" Double 4.5\""},"(ARCHIVED 2023) Vinyl Siding","Vinyl Siding Institute","Double 4.5\" products from: American Original, Associated Materials, CertainTeed, Novik, Ply Gem","0.040\" Double 4.5\"",null,null,null,"USA & CAN",null,49.98,"9.29m2",{"$f":"(K239/9.29)","v":5.3799784714747041},"m2","4787108620.102.1 ","UL Env.",2021,1430,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,1.016E-3,null,null,null,null,"219_Archived",null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS239:$BB239,0))","v":false}]
["Waterproofing membrane adhesive / GCP / Bituthene / ","Waterproofing membrane adhesive","GCP","Bituthene",null,null,null,null,null,null,2.4,"m2",{"$f":"(2.4)","v":2.4},"m2","EPD-073 ","ASTM",2022,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,220,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS240:$BB240,0))","v":false}]
[{"$f":"B241&\" / \"&C241&\" / \"&D241&\" / \"&E241&\" / \"&I241","v":"Welded wire mesh / Serfas /  / 6\" x 6\" x 6/6g / Norway"},"Welded wire mesh","Serfas",null,"6\" x 6\" x 6/6g",null,null,null,"Norway",null,0.8,"kg",{"$f":"(K241*T241)","v":1.64},"m2","NEPD-457-296-EN","Norwegian EPD Foundation",2021,null,null,2.0499999999999998,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,221,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS241:$BB241,0))","v":false}]
[{"$f":"B242&\" / \"&E242&\" / \"&C242&\" / \"&I242","v":"Window - double pane / Fiberglass frame /  / USA & CAN"},"Window - double pane",null,null,"Fiberglass frame",null,null,null,"USA & CAN",null,null,null,{"$f":"(114)","v":114},"m2","BfCA Study (Tally)","J. D. Racusin","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,222,null,null,null,"BfCA Study (Tally)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS242:$BB242,0))","v":false}]
[{"$f":"B243&\" / \"&C243&\" / \"&D243&\" / \"&E243&\" / \"&I243","v":"Window - double pane / Andersen / Fibrex / PVC & Wood composite / USA"},"Window - double pane","Andersen","Fibrex","PVC & Wood composite",null,null,"Wood biogenic carbon storage set to zero","USA",null,69.099999999999994,"m2",{"$f":"(K243)","v":69.099999999999994},"m2","4786100242.101.1 ","UL Env.",2020,null,null,{"$f":"2.47*0.88","v":2.1736},"kg reclaimed wood/m2",null,null,null,1,0.5,null,"m2",1.84,{"$f":"T243*Y243*Z243","v":1.0868},null,null,null,null,null,null,null,223,null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS243:$BB243,0))","v":false}]
[{"$f":"B244&\" / \"&E244&\" / \"&C244&\" / \"&I244","v":"Window - double pane / Vinyl frame /  / USA & CAN"},"Window - double pane",null,null,"Vinyl frame",null,null,null,"USA & CAN",null,null,null,{"$f":"(86)","v":86},"m2","BfCA Study (Tally)","J. D. Racusin","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,224,null,null,null,"BfCA Study (Tally)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS244:$BB244,0))","v":false}]
["Window - double pane / Wood frame /  / EU","Window - double pane",null,null,"Wood frame",null,null,"Wood biogenic carbon storage set to zero","EU",null,109,"1.82 m2",{"$f":"(K245/1.82)","v":59.890109890109891},"m2","SP-00812","EPD International AB",2023,null,null,{"$f":"18.4/1.82","v":10.109890109890109},"kg pine/m2",null,null,null,1,0.5,null,"m2",1.26,{"$f":"T245*Y245*Z245","v":5.0549450549450547},null,null,null,null,null,null,null,225,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS245:$BB245,0))","v":false}]
["Window - double pane / Wood frame /  / USA & CAN","Window - double pane",null,null,"Wood frame",null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,null,null,{"$f":"(72)","v":72},"m2","BfCA Study (Tally)","J. D. Racusin","",null,null,null,null,null,null,null,null,null,null,"m2",null,null,null,null,null,null,null,null,null,226,null,null,null,"BfCA Study (Tally)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS246:$BB246,0))","v":false}]
["Window - double pane / Wood frame, aluminum cladding /  / EU","Window - double pane",null,null,"Wood frame, aluminum cladding",null,null,"Wood biogenic carbon storage set to zero","EU",null,97.4,"1.82 m2",{"$f":"(K247/1.82)","v":53.516483516483518},"m2","ECO EPD Ref.No. 81","Norwegian EPD Foundation",2019,null,null,{"$f":"6/1.82","v":3.2967032967032965},"kg pine/m2",null,null,null,1,0.5,null,"m2",1.26,{"$f":"T247*Y247*Z247","v":1.6483516483516483},null,null,null,null,null,null,null,227,null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS247:$BB247,0))","v":false}]
["Window - double pane / Wood frame, aluminum cladding /  / USA & CAN","Window - double pane",null,null,"Wood frame, aluminum cladding",null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,null,null,{"$f":"(99)","v":99},"m2","BfCA Study (Tally)","J. D. Racusin","",null,null,null,null,null,null,null,null,null,null,"m2",null,null,null,null,null,null,null,null,null,228,null,null,null,"BfCA Study (Tally)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS248:$BB248,0))","v":false}]
["Window - triple pane / Fiberglass frame /  / USA & CAN","Window - triple pane",null,null,"Fiberglass frame",null,null,null,"USA & CAN",null,null,null,{"$f":"(127)","v":127},"m2","BfCA Study (Tally)","J. D. Racusin","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,229,null,null,null,"BfCA Study (Tally)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS249:$BB249,0))","v":false}]
["Window - triple pane / Vinyl frame /  / USA & CAN","Window - triple pane",null,null,"Vinyl frame",null,null,null,"USA & CAN",null,null,null,{"$f":"(99)","v":99},"m2","BfCA Study (Tally)","J. D. Racusin","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,230,null,null,null,"BfCA Study (Tally)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS250:$BB250,0))","v":false}]
["Window - triple pane / Wood frame /  / EU","Window - triple pane",null,null,"Wood frame",null,null,"Wood biogenic carbon storage set to zero","EU",null,115.19,"1.82 m2",{"$f":"(K251/1.82)","v":63.291208791208788},"m2","ECO EPD Ref.No. 79","Norwegian EPD Foundation",2019,null,null,{"$f":"16.42/1.82","v":9.0219780219780219},"kg pine/m2",null,null,null,1,0.5,null,"m2",1.26,{"$f":"T251*Y251*Z251","v":4.5109890109890109},null,null,null,null,null,null,null,231,null,null,null,{"$f":"IF(LEN(Q251)=4,IF(Q251<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q251),\"\"),\"\")","v":"Expired 2019"},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS251:$BB251,0))","v":false}]
["Window - triple pane / Wood frame /  / USA & CAN","Window - triple pane",null,null,"Wood frame",null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,null,null,{"$f":"(85)","v":85},"m2","BfCA Study (Tally)","J. D. Racusin","",null,null,null,null,null,null,null,null,null,null,"m2",null,null,null,null,null,null,null,null,null,232,null,null,null,"BfCA Study (Tally)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS252:$BB252,0))","v":false}]
["Window - triple pane / Wood frame, aluminum cladding /  / EU","Window - triple pane",null,null,"Wood frame, aluminum cladding",null,null,"Wood biogenic carbon storage set to zero","EU",null,134.62,"1.82 m2",{"$f":"(K253/1.82)","v":73.967032967032964},"m2","ECO EPD Ref.No. 79","Norwegian EPD Foundation",2019,null,null,{"$f":"16.42/1.82","v":9.0219780219780219},"kg pine/m2",null,null,null,1,0.5,null,"m2",1.26,{"$f":"T253*Y253*Z253","v":4.5109890109890109},null,null,null,null,null,null,null,233,null,null,null,{"$f":"IF(LEN(Q253)=4,IF(Q253<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q253),\"\"),\"\")","v":"Expired 2019"},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS253:$BB253,0))","v":false}]
["Window - triple pane / Wood frame, aluminum cladding /  / USA & CAN","Window - triple pane",null,null,"Wood frame, aluminum cladding",null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,null,null,{"$f":"(112)","v":112},"m2","BfCA Study (Tally)","J. D. Racusin","",null,null,null,null,null,null,null,null,null,null,"m2",null,null,null,null,null,null,null,null,null,234,null,null,null,"BfCA Study (Tally)",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS254:$BB254,0))","v":false}]
["Wood chip cement ICF / Isospan / Okopur / NEEDS REVIEW","Wood chip cement ICF","Isospan","Okopur","NEEDS REVIEW",null,null,"79.5 kg/m2 of wood-chip block,213.4 kg/m2 of filling concrete","EU",null,-52.1,"m2",{"$f":"(K255--AA255)","v":16.280125000000005},"m2","EPD-ISOSPAN-2017-1-ECOINVENT ","Bau EPD GmbH",2022,550,"kg/m3",75.349999999999994,"kg/m2 (17 kg/block * 5.382 blocks/m2)","R-27.5/block",null,null,0.55000000000000004,0.5,{"$f":"(44/12*AD255)*rng_biogenic_storage","v":68.380125000000007},"m2",1.84,{"$f":"T255*Y255*Z255","v":20.721250000000001},null,{"$f":"AD255*44/12","v":75.977916666666673},0.36499999999999999,1.25,0.25,null,null,235,null,null,null,{"$f":"IF(LEN(Q255)=4,IF(Q255<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q255),\"\"),\"\")","v":"Expired 2022"},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS255:$BB255,0))","v":false}]
["Wood chip cement ICF / Nexcem, Faswall /  / 12\" R22 block","Wood chip cement ICF","Nexcem, Faswall",null,"12\" R22 block",null,null,null,"USA & CAN","2021-03-19",{"$f":"410-317","v":93},"m3",{"$f":"(410*$T256)","v":76.12811805233197},"m2","LCA","Armtec Ltd","",550,"kg/m3",{"$f":"19/R256*AK256","v":0.18567833671300482},"m3/m2","R-22/block",8.3000000000000004E-2,"W/(mK)",0.7,0.52400000000000002,{"$f":"(317*T256)*rng_biogenic_storage","v":52.974029464220273},"m2",null,null,null,null,0.30499999999999999,0.61,0.30499999999999999,null,{"$f":"1/(AG256*AH256)","v":5.3748992206396133},236,null,null,null,"Indedpendent LCA",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS256:$BB256,0))","v":false}]
["Wood chip cement ICF / Nexcem, Faswall /  / 14\" R28 block","Wood chip cement ICF","Nexcem, Faswall",null,"14\" R28 block",null,null,null,"USA & CAN","2021-03-19",{"$f":"410-317","v":93},"m3",{"$f":"(410*T257)","v":84.141604163103764},"m2","LCA","Armtec Ltd","",550,"kg/m3",{"$f":"21/R257*AK257","v":0.20522342478805797},"m3/m2","R-28/block",8.3000000000000004E-2,"W/(mK)",0.7,0.52400000000000002,{"$f":"(317*T257)*rng_biogenic_storage","v":58.550243092032943},"m2",null,null,null,null,0.30499999999999999,0.61,0.36,null,{"$f":"1/(AG257*AH257)","v":5.3748992206396133},237,null,null,null,"Indedpendent LCA",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS257:$BB257,0))","v":false}]
["Wood fiber - loose fill / GUTEX / ThermoFiber / R 3.6/inch","Wood fiber - loose fill","GUTEX","ThermoFiber","R 3.6/inch",null,null,"35kg/m3",null,"2023-02-26",-1.14483,"kg",0.5917380000000001,"m2•RSI","EPD-GTX-20190018-IBA1-EN","IBU",2024,35,"kg/m3",{"$f":"R258*W258","v":1.4000000000000001},"kg/m2•RSI",{"$f":"0.0254*5.678/W258","v":3.6055299999999999},0.04,null,0.95,0.5,{"$f":"(AF258)*rng_biogenic_storage","v":2.1945000000000001},"m2-RSI1",null,{"$f":"T258*Y258*Z258","v":0.66500000000000004},null,{"$f":"AD258*44/12","v":2.4383333333333335},null,null,null,null,null,238,null,null,null,{"$f":"IF(LEN(Q258)=4,IF(Q258<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q258),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS258:$BB258,0))","v":false}]
["(ARCHIVED 2023) Wood fiber - loose fill / GUTEX / ThermoFiber / R 3.6/inch","(ARCHIVED 2023) Wood fiber - loose fill","GUTEX","ThermoFiber","R 3.6/inch",null,null,null,"EU",null,-43.2,"m3",{"$f":"((K259*W259)--AF259)","v":0.60319999999999974},"m2-RSI1","EPD-GTX-20140222-IBC2-EN ","IBU",2020,32,"kg/m3",{"$f":"R259*W259","v":1.248},"kg/m2-RSI1",null,3.9E-2,"W/(mK)",1,0.5,{"$f":"(AF259)*rng_biogenic_storage","v":2.0591999999999997},"m2-RSI1",null,{"$f":"T259*Y259*Z259","v":0.624},null,{"$f":"AD259*44/12","v":2.2879999999999998},null,null,null,null,null,"238_Archived",null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS259:$BB259,0))","v":false}]
["Wood fiber batt / GUTEX / ThermoFlex / R 4/inch","Wood fiber batt","GUTEX","ThermoFlex","R 4/inch",null,null,null,"EU",null,-67.5,"m3",{"$f":"((K260*W260)--AF260)","v":0.375},"m2-RSI1","EPD-GTX-20180071-IBA1-DE","IBU",2023,50,"kg/m3",1.7999999999999998,"kg/m2-RSI1",4,3.5999999999999997E-2,"W/(mK)",0.85,0.5,2.5244999999999997,"m2-RSI1",null,0.7649999999999999,null,{"$f":"AD260*44/12","v":2.8049999999999997},null,null,null,null,null,239,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS260:$BB260,0))","v":false}]
["Wood fiber batt / Pavatex / Pavaflex / R 3.8/inch","Wood fiber batt","Pavatex","Pavaflex","R 3.8/inch",null,null,null,"EU",null,1.63,"m3",{"$f":"(K261*W261)","v":6.1939999999999995E-2},"m2-RSI1","EPD-PAV-20150043-IBA2-EN ","IBU",2019,55,"kg/m3",2.09,"kg/m2-RSI1",3.8,3.7999999999999999E-2,"W/(mK)",0.82499999999999996,0.5,2.8450124999999997,"m2-RSI1",null,0.86212499999999992,null,{"$f":"AD261*44/12","v":3.1611249999999997},null,null,null,null,null,240,null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS261:$BB261,0))","v":false}]
["Wood fiber batt / Steico / SteicoFlex / R 3.8/inch","Wood fiber batt","Steico","SteicoFlex","R 3.8/inch",null,null,null,"EU",null,-70.16,"m3",{"$f":"((K262*W262)--AF262)","v":0.43756999999999957},"m2-RSI1","EPD-STE-20150327-IBD1-EN ","IBU",2021,50,"kg/m3",1.9,"kg/m2-RSI1",null,3.7999999999999999E-2,"W/(mK)",0.89100000000000001,0.5,2.7932849999999996,"m2-RSI1",null,0.84644999999999992,null,{"$f":"AD262*44/12","v":3.1036499999999996},null,null,null,null,null,241,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS262:$BB262,0))","v":false}]
[{"$f":"B263&\" / \"&C263&\" / \"&D263&\" / \"&E263","v":"(ARCHIVED 2023) Wood fiber board / AWC/CWC / Includes: Georgia Pacific, Louisville, BPC, Temple-Inland, Blue Ridge, Int'l Bildrite / R 2.7/inch"},"(ARCHIVED 2023) Wood fiber board","AWC/CWC","Includes: Georgia Pacific, Louisville, BPC, Temple-Inland, Blue Ridge, Int'l Bildrite","R 2.7/inch",null,null,null,"USA & CAN",null,295.05,"m3",{"$f":"(K263*W263)","v":15.99789983842105},"m2-RSI1","4787319688.101.1 ","UL Env.",2021,254,"kg/m3",13.772128652631576,"kg/m2-RSI1",2.66,{"$f":"1/V263*0.0254*5.67826","v":5.4220978947368409E-2},"W/(mK)",0.92200000000000004,0.5,20.951539319248422,"m2-RSI1",null,6.3489513088631568,null,{"$f":"AD263*44/12","v":23.279488132498244},null,null,null,null,null,242,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS263:$BB263,0))","v":false}]
["Wood fiber board / GUTEX / Multi-Therm / R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm","Wood fiber board","GUTEX","Multi-Therm","R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm",null,null,null,null,"2023-02-26",{"$f":"-198.4/167*R264","v":-166.32335329341319},"m3",{"$f":"((K264*W264)--AA264)","v":2.1250658682634729},"m2•RSI","EPD-GTX-20200178-IBC1-EN","IBU",2025,140,"kg/m3",5.6000000000000005,"kg/m2•RSI",{"$f":"0.0254*5.678/W264","v":3.6055299999999999},0.04,null,0.95,0.5,{"$f":"(AF264)*rng_biogenic_storage","v":8.7780000000000005},"m2-RSI1",null,2.66,null,{"$f":"$AD264*44/12","v":9.7533333333333339},null,null,null,null,null,243,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS264:$BB264,0))","v":false}]
["(ARCHIVED 2023) Wood fiber board / GUTEX / Multi-Therm / R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm","(ARCHIVED 2023) Wood fiber board","GUTEX","Multi-Therm","R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm",null,null,null,"EU",null,-132.69999999999999,"m3",{"$f":"((K265*W265)--AA265)","v":3.4238},"m2-RSI1","EPD-GTX-20140222-IBC2-EN ","IBU",2020,140,"kg/m3",5.6000000000000005,"kg/m2-RSI1",3.6,0.04,"W/(mK)",0.94499999999999995,0.5,8.7317999999999998,"m2-RSI1",null,{"$f":"T265*Y265*Z265","v":2.6459999999999999},null,{"$f":"$AD265*44/12","v":9.702},null,null,null,null,null,"243_Archived",null,null,null,"Expired 2020",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS265:$BB265,0))","v":false}]
["Wood fiber board / Pavatex / Pavatherm / R 3.4/inch","Wood fiber board","Pavatex","Pavatherm","R 3.4/inch",null,null,null,"EU",null,-219.34,"m3",{"$f":"((K266*W266)--AF266)","v":4.1720799999999993},"m2-RSI1","EPD­PAV­2014197­CBG1­DE ","IBU",2019,180,"kg/m3",7.92,"kg/m2-RSI1",3.35,4.3999999999999997E-2,"W/(mK)",0.95199999999999996,0.5,12.440735999999999,"m2-RSI1",null,3.7699199999999999,null,{"$f":"AD266*44/12","v":13.823039999999999},null,null,null,null,null,244,null,null,null,"Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS266:$BB266,0))","v":false}]
["Wood fiber board / Steico / Special Dry / R 3.6/inch, 40, 120, 140, 160, 180, 200 mm","Wood fiber board","Steico","Special Dry","R 3.6/inch, 40, 120, 140, 160, 180, 200 mm",null,null,null,"EU",null,-196.44,"m3",{"$f":"((K267*W267)--AF267)","v":1.8957333333333342},"m2-RSI1","EPD-STE-20150327-IBD1-EN ","IBU",2021,140,"kg/m3",5.6000000000000005,"kg/m2-RSI1",3.6,0.04,"W/(mK)",0.95,0.5,8.7780000000000005,"m2-RSI1",null,{"$f":"T267*Y267*Z267","v":2.66},null,{"$f":"AD267*44/12","v":9.7533333333333339},null,null,null,null,null,245,null,null,null,"Expired 2021",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS267:$BB267,0))","v":false}]
["Wood framing - Softwood / Roseburg /  / ","Wood framing - Softwood","Roseburg",null,null,null,null,"Wood biogenic carbon storage set to zero","USA",null,44.7,"m3",{"$f":"(K268)","v":44.7},"m3","4786969381.105.1 ","UL Env.",2023,456,"kg/m3",null,null,null,null,null,1,0.5,null,"m3",0.82499999999999996,{"$f":"R268*Y268*Z268","v":228},null,null,null,null,null,null,null,246,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS268:$BB268,0))","v":false}]
["Wood framing & siding - Redwood / American Wood Council & Canadian Wood Council /  / ","Wood framing & siding - Redwood","American Wood Council & Canadian Wood Council",null,null,null,null,"Wood biogenic carbon storage set to zero","USA",null,37.97,"m3",{"$f":"(K269*0.0254)","v":0.96443799999999991},"m2 at 1\"","4788424634.107.1 ","UL Env.",2025,{"$f":"R268","v":456},{"$f":"S268","v":"kg/m3"},null,null,null,null,null,1,0.5,null,{"$f":"AB268","v":"m3"},{"$f":"AC268","v":0.82499999999999996},{"$f":"R269*Y269*Z269","v":228},null,null,null,null,null,null,null,247,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS269:$BB269,0))","v":false}]
["Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / ","Wood framing & siding - SPF","American Wood Council & Canadian Wood Council",null,null,null,null,"Wood biogenic carbon storage set to zero","USA",null,63.12,"m3",{"$f":"(63.12)","v":63.12},"m3","4788424634.102.1","UL Env.",2025,460,"kg/m3",null,null,null,null,null,1,0.5,null,"m3",0.82499999999999996,{"$f":"R270*Y270*Z270","v":230},null,null,null,null,null,null,null,248,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS270:$BB270,0))","v":false}]
["Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360","Wood I joist","American Wood Council & Canadian Wood Council",null,"TJI 230/360",null,null,"Wood biogenic carbon storage set to zero","USA & CAN",null,1.97,"m at 11-7/8\"",{"$f":"(1.054)","v":1.054},"m at 11-7/8\"","4788424634.106.1 ","UL Env.",2025,4.34,"kg/m at 11-7/8\"",null,null,null,null,null,0.97499999999999998,0.5,null,"m",0.82499999999999996,{"$f":"R271*Y271*Z271","v":2.1157499999999998},"kgC/m",null,null,null,null,null,null,249,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS271:$BB271,0))","v":false}]
["Wood I joist / Roseburg / RFPI Joist / ","Wood I joist","Roseburg","RFPI Joist",null,null,null,"Wood biogenic carbon storage set to zero","USA",null,1.82,"m",{"$f":"(K272)","v":1.82},"m at unit size","4786969381.106.1 ","UL Env.",2023,3.9,"kg/m",null,null,null,null,null,0.9,0.5,null,"m at unit size",0.82499999999999996,{"$f":"R272*Y272*Z272","v":1.7549999999999999},null,null,null,null,null,null,null,250,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS272:$BB272,0))","v":false}]
[{"$f":"B273&\" / \"&C273&\" / \"&D273&\" / \"&E273","v":"Wood floor truss - prefabricated / Quebec Wood Export Bureau / Common (Warren, 45 deg) web pattern / Top chord bearing, variable depth"},"Wood floor truss - prefabricated","Quebec Wood Export Bureau","Common (Warren, 45 deg) web pattern","Top chord bearing, variable depth",null,null,"Wood biogenic carbon storage set to zero","USA",null,181.6,"m3",{"$f":"(K273*T273)","v":2.0611600000000001},"linear m of truss","EPD 1725-6769","CSA Group",2022,417,"kg/m3",1.1350000000000001E-2,"m3/linear m",null,null,null,0.95,0.5,null,"linear m of truss",0.82499999999999996,{"$f":"R273*Y273*Z273*T273","v":2.2481512499999998},null,null,null,null,null,null,null,251,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS273:$BB273,0))","v":false}]
["Wood roof truss - prefabricated / Quebec Wood Export Bureau / Common (Double Howe) Gabrel Roof / 2x6 Chords, 2x4 Webs, 4:12 Pitch, 40 ft span, 20\" overhang","Wood roof truss - prefabricated","Quebec Wood Export Bureau","Common (Double Howe) Gabrel Roof","2x6 Chords, 2x4 Webs, 4:12 Pitch, 40 ft span, 20\" overhang",null,null,"Wood biogenic carbon storage set to zero","USA",null,178,"m3",{"$f":"(K274*T274)","v":2.5276000000000001},"linear m of truss","EPD 3409-8229","CSA Group",2022,417,"kg/m3",1.4200000000000001E-2,"m3/linear m",null,null,null,0.95,0.5,null,"linear m of truss",null,null,null,null,null,null,null,null,null,252,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS274:$BB274,0))","v":false}]
[{"$f":"B275&\" / \"&C275&\" / \"&D275&\" / \"&E275","v":"Wood wool boards / Armstrong / Tectum / 2\" (50.8 mm)"},"Wood wool boards","Armstrong","Tectum","2\" (50.8 mm)",null,null,null,"USA",null,1.054,"m2",{"$f":"(1.054)","v":1.054},"m2","4787863341.101.1 ","UL Env.",2022,17.087,"kg/m2",null,null,null,null,null,0.5,0.5,{"$f":"(AC275*AD275)*rng_biogenic_storage","v":3.171774375},"m2 product",0.82499999999999996,{"$f":"R275*Y275*Z275","v":4.2717499999999999},null,null,null,null,null,null,null,253,null,null,null,"Expired 2022",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS275:$BB275,0))","v":false}]
["Wool batt / Havelock Wool /  / R 3.6/inch","Wool batt","Havelock Wool",null,"R 3.6/inch",null,null,null,"USA",null,2.99,"m2 RSI 1",{"$f":"(2.99)","v":2.99},"m2 RSI 1","HW-20200605-001","Sustainable Minds",2025,24,"kg/m3",0.93600000000000005,"kg/m2 at RSI1",3.64,null,null,0.97850000000000004,0.505,{"$f":"(AD276*3.67)*rng_biogenic_storage","v":1.5276949061400003},"m2 at RSI1",null,{"$f":"T276*Y276*Z276","v":0.46251738000000009},null,null,null,null,null,null,null,254,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS276:$BB276,0))","v":false}]
["Wool loose fill / Havelock Wool /  / R 4.4/inch","Wool loose fill","Havelock Wool",null,"R 4.4/inch",null,null,null,"USA",null,2.99,"m2 RSI 1",{"$f":"(2.99)","v":2.99},"m2 RSI 1","HW-20200605-002","Sustainable Minds",2026,18.100000000000001,"kg/m3",0.59730000000000005,"kg/m2 at RSI1",4.3600000000000003,null,null,0.97850000000000004,0.505,{"$f":"(AD277*3.67)*rng_biogenic_storage","v":0.97488479427075014},"m2 at RSI1",null,{"$f":"T277*Y277*Z277","v":0.29515131525000005},null,null,null,null,null,null,null,255,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS277:$BB277,0))","v":false}]
["(ARCHIVED 2023) XPS foam board / Dow Chemical Company / Styrofoam SM / R 5/inch","(ARCHIVED 2023) XPS foam board","Dow Chemical Company","Styrofoam SM","R 5/inch",null,null,null,"USA & CAN",null,{"$f":"95.3-33.3","v":62},"m2 RSI 1",{"$f":"(61.63)","v":61.63},"m2 RSI 1","4786548101.101.1 ","UL Env.",2019,null,null,null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,256,null,null,null,"A1-B1, Expired 2019",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS278:$BB278,0))","v":false}]
["(ARCHIVED 2023) XPS foam board / Owens Corning / Foamular 250 / R 5/inch","(ARCHIVED 2023) XPS foam board","Owens Corning","Foamular 250","R 5/inch",null,null,null,"USA & CAN",null,50.5,"m2 RSI 1",{"$f":"(50.5)","v":50.5},"m2 RSI 1","4788721182.101.1","UL Env.",2024,24.8,"kg/m3",null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,257,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS279:$BB279,0))","v":false}]
["XPS foam board / Owens Corning / Foamular NGX 250  / R 5/inch","XPS foam board","Owens Corning","Foamular NGX 250 ","R 5/inch",null,null,null,"USA & CAN",null,8.1199999999999992,"m2 RSI 1",{"$f":"(8.12)","v":8.1199999999999992},"m2 RSI 1","4789639125.101.1","UL Env.",2026,24.8,"kg/m3",null,null,5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,258,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS280:$BB280,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A2","v":"EPS FOAM ICF R-23, 2 Sheets of 2.75\" @ R4/in., 15M rebar (6\" CONCRETE CORE must be added separately)"},"from Composite Master Sheet",null,null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$B2)","v":24.801453057919655},{"$f":"'Composite Master Sheet'!$D2","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C2)*rng_biogenic_storage","v":0},{"$f":"'Composite Master Sheet'!$D2","v":"m2"},null,null,null,null,null,null,null,null,null,259,null,null,null,{"$f":"IF(LEN(Q281)=4,IF(Q281<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q281),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS281:$BB281,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A3","v":"SIP PANEL - R23 6.5\" - EPS 5.5\" @ R4/in. core, 2 sheets 1/2\" OSB"},"from Composite Master Sheet",null,null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$B3)","v":20.76878807608313},{"$f":"'Composite Master Sheet'!$D3","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C3)*rng_biogenic_storage","v":0},{"$f":"'Composite Master Sheet'!$D3","v":"m2"},null,null,null,null,null,null,null,null,null,260,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS282:$BB282,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A4","v":"SIP PANEL - R30 8.25\" - EPS 7.25\" @ R4/in. core, 2 sheets 1/2\" OSB"},"from Composite Master Sheet",null,null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$B4)","v":25.41655137301867},{"$f":"'Composite Master Sheet'!$D4","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C4)*rng_biogenic_storage","v":0},{"$f":"'Composite Master Sheet'!$D4","v":"m2"},null,null,null,null,null,null,null,null,null,261,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS283:$BB283,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A5","v":"SIP PANEL - R38 10.5\" - EPS 9.5\" @ R4/in. core, 2 sheets 1/2\" OSB"},"from Composite Master Sheet",null,null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$B5)","v":31.392247040507225},{"$f":"'Composite Master Sheet'!$D5","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C5)*rng_biogenic_storage","v":0},{"$f":"'Composite Master Sheet'!$D5","v":"m2"},null,null,null,null,null,null,null,null,null,262,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS284:$BB284,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A6","v":"SIP PANEL - R48 12-7/8\" - EPS 11.875\" @ R4/in. core, 2 sheets 1/2\" OSB"},"from Composite Master Sheet",null,null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$B6)","v":37.699925800634027},{"$f":"'Composite Master Sheet'!$D6","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C6)*rng_biogenic_storage","v":0},{"$f":"'Composite Master Sheet'!$D6","v":"m2"},null,null,null,null,null,null,null,null,null,263,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS285:$BB285,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A7","v":"WOOD CHIP CEMENT ICF 12\" R-22 with MINERAL WOOL INSERTS, (3 in. @ R4.2/in.), 15M REBAR"},"from Composite Master Sheet",null,null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$B7)","v":99.308101483469699},{"$f":"'Composite Master Sheet'!$D7","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C7)*rng_biogenic_storage","v":47.676626517798248},{"$f":"'Composite Master Sheet'!$D7","v":"m2"},null,null,null,null,null,null,null,null,null,264,null,null,null,"LCA in Composite",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS286:$BB286,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A8","v":"WOOD CHIP CEMENT ICF 14\" R-28 with MINERAL WOOL INSERTS (5 in. @ R4.2/in.), 15M REBAR"},"from Composite Master Sheet",null,null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$B8)","v":119.39344388166664},{"$f":"'Composite Master Sheet'!$D8","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C8)*rng_biogenic_storage","v":52.695218782829649},{"$f":"'Composite Master Sheet'!$D8","v":"m2"},null,null,null,null,null,null,null,null,null,265,null,null,null,"LCA in Composite",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS287:$BB287,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A9","v":"WOOD CHIP CEMENT ICF 12\" R-21 with CORK BOARD INSERTS (3 in. @ R4/in.), 15M REBAR"},"from Composite Master Sheet",null,null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$B9)","v":87.48957383288851},{"$f":"'Composite Master Sheet'!$D9","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C9)*rng_biogenic_storage","v":66.328937895043765},{"$f":"'Composite Master Sheet'!$D9","v":"m2"},null,null,null,null,null,null,null,null,null,266,null,null,null,"LCA in Composite",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS288:$BB288,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A10","v":"WOOD CHIP CEMENT ICF 14\" R-27 with CORK BOARD INSERTS (5 in. @ R4/in.), 15M REBAR"},"from Composite Master Sheet",null,null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$B10)","v":99.695897797364651},{"$f":"'Composite Master Sheet'!$D10","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C10)*rng_biogenic_storage","v":83.782404411572173},{"$f":"'Composite Master Sheet'!$D10","v":"m2"},null,null,null,null,null,null,null,null,null,267,null,null,null,"LCA in Composite",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS289:$BB289,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A11","v":"TREATED WOOD FOUNDATION - 2x8 framing @ 16\" OC, 3/4\" plywood sheathing"},"from Composite Master Sheet",null,null,null,null,null,"Wood biogenic carbon storage set to zero",null,null,null,null,{"$f":"('Composite Master Sheet'!$B11)","v":8.6898397835717578},{"$f":"'Composite Master Sheet'!$D11","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C11)*rng_biogenic_storage","v":0},{"$f":"'Composite Master Sheet'!$D11","v":"m2"},null,null,null,null,null,null,null,null,null,268,null,null,null,{"$f":"IF(LEN(Q290)=4,IF(Q290<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q290),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS290:$BB290,0))","v":false}]
[{"$f":"'Composite Master Sheet'!A12","v":"WOOD FRAME with STRAW BALE INFILL - 14\" R-46, Double 2x4 @ 30\" o/c"},"from Composite Master Sheet",null,null,null,null,null,"Wood biogenic carbon storage set to zero",null,null,null,null,{"$f":"('Composite Master Sheet'!$B12)","v":5.0165688977809086},{"$f":"'Composite Master Sheet'!$D12","v":"m2"},null,null,"",null,null,null,null,null,null,null,null,null,{"$f":"('Composite Master Sheet'!$C12)*rng_biogenic_storage","v":49.627504099527997},{"$f":"'Composite Master Sheet'!$D12","v":"m2"},null,null,null,null,null,null,null,null,null,269,null,null,null,"LCA in Composite",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS291:$BB291,0))","v":false}]
[{"$f":"B292&\" / \"&C292&\" / \"&D292&\" / \"&E292","v":"Concrete - 25 MPa, Quebec Baseline Average / ABQ / Can. Quebec Avg. / "},"Concrete - 25 MPa, Quebec Baseline Average","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Baseline with & without air","CA","2023-02-26",293.14999999999998,"m3",{"$f":"K292","v":293.14999999999998},"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,270,"0-25",1,null,{"$f":"IF(LEN(Q292)=4,IF(Q292<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q292),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS292:$BB292,0))","v":false},"Quebec","Québec"]
["Concrete - 25 MPa, 10% SL, GU / ABQ / Can. Quebec Avg. / ","Concrete - 25 MPa, 10% SL, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",280.57,"m3",280.57,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,271,"0-25",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS293:$BB293,0))","v":false},"Quebec","Québec"]
["Concrete - 25 MPa, 10% FA, GU / ABQ / Can. Quebec Avg. / ","Concrete - 25 MPa, 10% FA, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",276.22000000000003,"m3",276.22000000000003,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,272,"0-25",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS294:$BB294,0))","v":false},"Quebec","Québec"]
["Concrete - 25 MPa, 20% SL, GU / ABQ / Can. Quebec Avg. / ","Concrete - 25 MPa, 20% SL, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",258.8,"m3",258.8,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,273,"0-25",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS295:$BB295,0))","v":false},"Quebec","Québec"]
["Concrete - 25 MPa, 20% FA, GU / ABQ / Can. Quebec Avg. / ","Concrete - 25 MPa, 20% FA, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",250.12,"m3",250.12,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,274,"0-25",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS296:$BB296,0))","v":false},"Quebec","Québec"]
["Concrete - 25 MPa, 30% SL, GU / ABQ / Can. Quebec Avg. / ","Concrete - 25 MPa, 30% SL, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",237.5,"m3",237.5,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,275,"0-25",6,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS297:$BB297,0))","v":false},"Quebec","Québec"]
["Concrete - 25 MPa, 30% FA, GU / ABQ / Can. Quebec Avg. / ","Concrete - 25 MPa, 30% FA, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",224.48,"m3",224.48,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,276,"0-25",7,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS298:$BB298,0))","v":false},"Quebec","Québec"]
["Concrete - 30 MPa, Quebec Baseline Average / ABQ / Can. Quebec Avg. / ","Concrete - 30 MPa, Quebec Baseline Average","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Baseline with & without air","CA","2023-02-26",326.97000000000003,"m3",326.97000000000003,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,277,"26-30",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS299:$BB299,0))","v":false},"Quebec","Québec"]
["Concrete - 30 MPa, 10% SL, GU / ABQ / Can. Quebec Avg. / ","Concrete - 30 MPa, 10% SL, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",312.77999999999997,"m3",312.77999999999997,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,278,"26-30",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS300:$BB300,0))","v":false},"Quebec","Québec"]
["Concrete - 30 MPa, 10% FA, GU / ABQ / Can. Quebec Avg. / ","Concrete - 30 MPa, 10% FA, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",307.94,"m3",307.94,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,279,"26-30",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS301:$BB301,0))","v":false},"Quebec","Québec"]
["Concrete - 30 MPa, 20% SL, GU / ABQ / Can. Quebec Avg. / ","Concrete - 30 MPa, 20% SL, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",289.05,"m3",289.05,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,280,"26-30",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS302:$BB302,0))","v":false},"Quebec","Québec"]
["Concrete - 30 MPa, 20% FA, GU / ABQ / Can. Quebec Avg. / ","Concrete - 30 MPa, 20% FA, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",279.27999999999997,"m3",279.27999999999997,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,281,"26-30",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS303:$BB303,0))","v":false},"Quebec","Québec"]
["Concrete - 30 MPa, 30% SL, GU / ABQ / Can. Quebec Avg. / ","Concrete - 30 MPa, 30% SL, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",264.86,"m3",264.86,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,282,"26-30",6,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS304:$BB304,0))","v":false},"Quebec","Québec"]
["Concrete - 30 MPa, 30% FA, GU / ABQ / Can. Quebec Avg. / ","Concrete - 30 MPa, 30% FA, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",250.16,"m3",250.16,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,283,"26-30",7,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS305:$BB305,0))","v":false},"Quebec","Québec"]
["Concrete - 35 MPa, Quebec Baseline Average / ABQ / Can. Quebec Avg. / ","Concrete - 35 MPa, Quebec Baseline Average","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Baseline with & without air","CA","2023-02-26",369.32,"m3",369.32,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,284,"31-35",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS306:$BB306,0))","v":false},"Quebec","Québec"]
["Concrete - 35 MPa, 10% SL, GU / ABQ / Can. Quebec Avg. / ","Concrete - 35 MPa, 10% SL, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",353.75,"m3",353.75,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,285,"31-35",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS307:$BB307,0))","v":false},"Quebec","Québec"]
["Concrete - 35 MPa, 10% FA, GU / ABQ / Can. Quebec Avg. / ","Concrete - 35 MPa, 10% FA, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",348.16,"m3",348.16,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,286,"31-35",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS308:$BB308,0))","v":false},"Quebec","Québec"]
["Concrete - 35 MPa, 20% SL, GU / ABQ / Can. Quebec Avg. / ","Concrete - 35 MPa, 20% SL, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",326.39999999999998,"m3",326.39999999999998,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,287,"31-35",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS309:$BB309,0))","v":false},"Quebec","Québec"]
["Concrete - 35 MPa, 20% FA, GU / ABQ / Can. Quebec Avg. / ","Concrete - 35 MPa, 20% FA, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",315.14999999999998,"m3",315.14999999999998,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,288,"31-35",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS310:$BB310,0))","v":false},"Quebec","Québec"]
["Concrete - 35 MPa, 30% SL, GU / ABQ / Can. Quebec Avg. / ","Concrete - 35 MPa, 30% SL, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",298.49,"m3",298.49,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,289,"31-35",6,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS311:$BB311,0))","v":false},"Quebec","Québec"]
["Concrete - 35 MPa, 30% FA, GU / ABQ / Can. Quebec Avg. / ","Concrete - 35 MPa, 30% FA, GU","ABQ","Can. Quebec Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",281.66000000000003,"m3",281.66000000000003,"m3","EPD 352","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,290,"31-35",7,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS312:$BB312,0))","v":false},"Quebec","Québec"]
["Concrete - 25 MPa, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 25 MPa, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Mix without air","CA","2023-02-26",273.67,"m3",273.67,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,291,"0-25",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS313:$BB313,0))","v":false},"Ontario","Ontario"]
["Concrete - 25 MPa, 15% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 25 MPa, 15% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Mix without air","CA","2023-02-26",244.24,"m3",244.24,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,292,"0-25",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS314:$BB314,0))","v":false},"Ontario","Ontario"]
["Concrete - 25 MPa, 25% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 25 MPa, 25% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Mix without air","CA","2023-02-26",224.62,"m3",224.62,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,293,"0-25",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS315:$BB315,0))","v":false},"Ontario","Ontario"]
["Concrete - 25 MPa, 35% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 25 MPa, 35% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Mix without air","CA","2023-02-26",205.01,"m3",205.01,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,294,"0-25",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS316:$BB316,0))","v":false},"Ontario","Ontario"]
["Concrete - 25 MPa, 50% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 25 MPa, 50% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Mix without air","CA","2023-02-26",175.58,"m3",175.58,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,295,"0-25",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS317:$BB317,0))","v":false},"Ontario","Ontario"]
["Concrete - 30 MPa, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 30 MPa, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Mix without air","CA","2023-02-26",296.62,"m3",296.62,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,296,"26-30",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS318:$BB318,0))","v":false},"Ontario","Ontario"]
["Concrete - 30 MPa, 15% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 30 MPa, 15% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Mix without air","CA","2023-02-26",264.38,"m3",264.38,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,297,"26-30",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS319:$BB319,0))","v":false},"Ontario","Ontario"]
["Concrete - 30 MPa, 25% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 30 MPa, 25% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Mix without air","CA","2023-02-26",242.88,"m3",242.88,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,298,"26-30",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS320:$BB320,0))","v":false},"Ontario","Ontario"]
["Concrete - 30 MPa, 35% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 30 MPa, 35% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Mix without air","CA","2023-02-26",221.39,"m3",221.39,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,299,"26-30",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS321:$BB321,0))","v":false},"Ontario","Ontario"]
["Concrete - 30 MPa, 50% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 30 MPa, 50% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Mix without air","CA","2023-02-26",189.14,"m3",189.14,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"26-30",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS322:$BB322,0))","v":false},"Ontario","Ontario"]
["Concrete - 35 MPa, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 35 MPa, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",354.3,"m3",354.3,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,301,"31-35",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS323:$BB323,0))","v":false},"Ontario","Ontario"]
["Concrete - 35 MPa, 15% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 35 MPa, 15% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",314.98,"m3",314.98,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,302,"31-35",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS324:$BB324,0))","v":false},"Ontario","Ontario"]
["Concrete - 35 MPa, 25% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 35 MPa, 25% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",288.76,"m3",288.76,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,303,"31-35",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS325:$BB325,0))","v":false},"Ontario","Ontario"]
["Concrete - 35 MPa, 35% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 35 MPa, 35% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",262.54000000000002,"m3",262.54000000000002,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,304,"31-35",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS326:$BB326,0))","v":false},"Ontario","Ontario"]
["Concrete - 35 MPa, 50% SL, GU / RMCAO / Can. Ontario Avg. / ","Concrete - 35 MPa, 50% SL, GU","RMCAO","Can. Ontario Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",223.22,"m3",223.22,"m3","EPD 351","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,305,"31-35",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS327:$BB327,0))","v":false},"Ontario","Ontario"]
["Concrete - 25 MPa, GU / SRMCA / Can. Sask Avg. / ","Concrete - 25 MPa, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",345.28,"m3",345.28,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,306,"0-25",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS328:$BB328,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 25 MPa, 10% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 25 MPa, 10% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",318.05,"m3",318.05,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,307,"0-25",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS329:$BB329,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 25 MPa, 20% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 25 MPa, 20% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",290.83,"m3",290.83,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,308,"0-25",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS330:$BB330,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 25 MPa, 30% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 25 MPa, 30% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",263.61,"m3",263.61,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,309,"0-25",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS331:$BB331,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 25 MPa, 40% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 25 MPa, 40% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",236.39,"m3",236.39,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,310,"0-25",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS332:$BB332,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 30 MPa, GU / SRMCA / Can. Sask Avg. / ","Concrete - 30 MPa, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",376.92,"m3",376.92,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,311,"26-30",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS333:$BB333,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 30 MPa, 10% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 30 MPa, 10% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",346.99,"m3",346.99,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,312,"26-30",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS334:$BB334,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 30 MPa, 20% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 30 MPa, 20% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",316.58,"m3",316.58,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,313,"26-30",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS335:$BB335,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 30 MPa, 30% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 30 MPa, 30% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",286.64999999999998,"m3",286.64999999999998,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,314,"26-30",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS336:$BB336,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 30 MPa, 40% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 30 MPa, 40% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",256.24,"m3",256.24,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,315,"26-30",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS337:$BB337,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 35 MPa, GU / SRMCA / Can. Sask Avg. / ","Concrete - 35 MPa, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",442.03,"m3",442.03,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,316,"31-35",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS338:$BB338,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 35 MPa, 10% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 35 MPa, 10% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",406.22,"m3",406.22,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,317,"31-35",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS339:$BB339,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 35 MPa, 20% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 35 MPa, 20% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",369.44,"m3",369.44,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,318,"31-35",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS340:$BB340,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 35 MPa, 30% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 35 MPa, 30% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",333.63,"m3",333.63,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,319,"31-35",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS341:$BB341,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 35 MPa, 40% FA, GU / SRMCA / Can. Sask Avg. / ","Concrete - 35 MPa, 40% FA, GU","SRMCA","Can. Sask Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",296.83999999999997,"m3",296.83999999999997,"m3","EPD 350","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,320,"31-35",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS342:$BB342,0))","v":false},"Saskatchewan","Saskatchewan"]
["Concrete - 25 MPa, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 25 MPa, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",270.73,"m3",270.73,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,321,"0-25",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS343:$BB343,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 25 MPa, 10% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 25 MPa, 10% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",249.17,"m3",249.17,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,322,"0-25",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS344:$BB344,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 25 MPa, 20% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 25 MPa, 20% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",226.64,"m3",226.64,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,323,"0-25",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS345:$BB345,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 25 MPa, 30% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 25 MPa, 30% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",205.07,"m3",205.07,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,324,"0-25",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS346:$BB346,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 25 MPa, 40% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 25 MPa, 40% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",182.54,"m3",182.54,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,325,"0-25",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS347:$BB347,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 30 MPa, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 30 MPa, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",298.23,"m3",298.23,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,326,"26-30",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS348:$BB348,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 30 MPa, 10% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 30 MPa, 10% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",273.77,"m3",273.77,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,327,"26-30",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS349:$BB349,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 30 MPa, 20% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 30 MPa, 20% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",249.23,"m3",249.23,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,328,"26-30",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS350:$BB350,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 30 MPa, 30% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 30 MPa, 30% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",224.77,"m3",224.77,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,329,"26-30",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS351:$BB351,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 30 MPa, 40% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 30 MPa, 40% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",200.24,"m3",200.24,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,330,"26-30",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS352:$BB352,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 35 MPa, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 35 MPa, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",339.35,"m3",339.35,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,331,"31-35",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS353:$BB353,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 35 MPa, 10% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 35 MPa, 10% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",311.66000000000003,"m3",311.66000000000003,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,332,"31-35",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS354:$BB354,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 35 MPa, 20% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 35 MPa, 20% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",283,"m3",283,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,333,"31-35",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS355:$BB355,0))","v":false},"Manitoba","Manitoba"]
[{"$f":"B356&\" / \"&C356&\" / \"&D356&\" / \"&E356","v":"Concrete - 35 MPa, 30% FA, GU / MRMCA / Can. Manitoba Avg. / "},"Concrete - 35 MPa, 30% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",255.31,"m3",255.31,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,334,"31-35",4,null,{"$f":"IF(LEN(Q356)=4,IF(Q356<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q356),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS356:$BB356,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 35 MPa, 40% FA, GU / MRMCA / Can. Manitoba Avg. / ","Concrete - 35 MPa, 40% FA, GU","MRMCA","Can. Manitoba Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",226.66,"m3",226.66,"m3","EPD 349","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,335,"31-35",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS357:$BB357,0))","v":false},"Manitoba","Manitoba"]
["Concrete - 25 MPa, GU / BCRMCA / Can. BC Avg. / ","Concrete - 25 MPa, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",263.94,"m3",263.94,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,336,"0-25",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS358:$BB358,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 25 MPa, 15% SCM, GU / BCRMCA / Can. BC Avg. / ","Concrete - 25 MPa, 15% SCM, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",234.65,"m3",234.65,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,337,"0-25",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS359:$BB359,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 25 MPa, 25% SCM, GU / BCRMCA / Can. BC Avg. / ","Concrete - 25 MPa, 25% SCM, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",215.66,"m3",215.66,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,338,"0-25",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS360:$BB360,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 25 MPa, 40% SCM, GU / BCRMCA / Can. BC Avg. / ","Concrete - 25 MPa, 40% SCM, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",186.29,"m3",186.29,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,339,"0-25",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS361:$BB361,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 30 MPa, GU / BCRMCA / Can. BC Avg. / ","Concrete - 30 MPa, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",310.69,"m3",310.69,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,340,"26-30",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS362:$BB362,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 30 MPa, 15% SCM, GU / BCRMCA / Can. BC Avg. / ","Concrete - 30 MPa, 15% SCM, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",275.95999999999998,"m3",275.95999999999998,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,341,"26-30",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS363:$BB363,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 30 MPa, 25% SCM, GU / BCRMCA / Can. BC Avg. / ","Concrete - 30 MPa, 25% SCM, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",252.8,"m3",252.8,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,342,"26-30",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS364:$BB364,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 30 MPa, 40% SCM, GU / BCRMCA / Can. BC Avg. / ","Concrete - 30 MPa, 40% SCM, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",218.06,"m3",218.06,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,343,"26-30",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS365:$BB365,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 35 MPa, GU / BCRMCA / Can. BC Avg. / ","Concrete - 35 MPa, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",355.26,"m3",355.26,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,344,"31-35",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS366:$BB366,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 35 MPa, 15% SCM, GU / BCRMCA / Can. BC Avg. / ","Concrete - 35 MPa, 15% SCM, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",315.41000000000003,"m3",315.41000000000003,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,345,"31-35",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS367:$BB367,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 35 MPa, 25% SCM, GU / BCRMCA / Can. BC Avg. / ","Concrete - 35 MPa, 25% SCM, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",288.94,"m3",288.94,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,346,"31-35",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS368:$BB368,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 35 MPa, 40% SCM, GU / BCRMCA / Can. BC Avg. / ","Concrete - 35 MPa, 40% SCM, GU","BCRMCA","Can. BC Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",248.67,"m3",248.67,"m3","EPD 348","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,347,"31-35",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS369:$BB369,0))","v":false},"British Columbia","Colombie-Britannique"]
["Concrete - 25 MPa, GU / ACA / Can. Atlantic Avg. / ","Concrete - 25 MPa, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",387.2,"m3",387.2,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,348,"0-25",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS370:$BB370,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 25 MPa, 10% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 25 MPa, 10% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",357.51,"m3",357.51,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,349,"0-25",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS371:$BB371,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 25 MPa, 20% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 25 MPa, 20% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",327.82,"m3",327.82,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350,"0-25",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS372:$BB372,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 25 MPa, 30% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 25 MPa, 30% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",298.12,"m3",298.12,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,351,"0-25",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS373:$BB373,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 25 MPa, 40% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 25 MPa, 40% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",268.43,"m3",268.43,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,352,"0-25",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS374:$BB374,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 30 MPa, GU / ACA / Can. Atlantic Avg. / ","Concrete - 30 MPa, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",419.64,"m3",419.64,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,353,"26-30",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS375:$BB375,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 30 MPa, 10% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 30 MPa, 10% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",386.75,"m3",386.75,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,354,"26-30",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS376:$BB376,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 30 MPa, 20% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 30 MPa, 20% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",353.86,"m3",353.86,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,355,"26-30",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS377:$BB377,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 30 MPa, 30% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 30 MPa, 30% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",320.97000000000003,"m3",320.97000000000003,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,356,"26-30",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS378:$BB378,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 30 MPa, 40% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 30 MPa, 40% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",288.08,"m3",288.08,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,357,"26-30",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS379:$BB379,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 35 MPa, GU / ACA / Can. Atlantic Avg. / ","Concrete - 35 MPa, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",487.53,"m3",487.53,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,358,"31-35",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS380:$BB380,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 35 MPa, 10% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 35 MPa, 10% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",448.25,"m3",448.25,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,359,"31-35",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS381:$BB381,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 35 MPa, 20% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 35 MPa, 20% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",408.96,"m3",408.96,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,360,"31-35",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS382:$BB382,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 35 MPa, 30% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 35 MPa, 30% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",369.67,"m3",369.67,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,361,"31-35",4,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS383:$BB383,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 35 MPa, 40% FA, GU / ACA / Can. Atlantic Avg. / ","Concrete - 35 MPa, 40% FA, GU","ACA","Can. Atlantic Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",330.39,"m3",330.39,"m3","EPD 347","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,362,"31-35",5,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS384:$BB384,0))","v":false},"New Brunswick","Nouveau-Brunswick","Newfoundland and Labrador","Terre-Neuve-et-Labrador","Prince Edward Island","Île-du-Prince-Édouard","Nova Scotia","Nouvelle-Écosse"]
["Concrete - 25 MPa, GU / ARMCA / Can. Alberta Avg. / ","Concrete - 25 MPa, GU","ARMCA","Can. Alberta Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",341.8,"m3",341.8,"m3","EPD 346","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,363,"0-25",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS385:$BB385,0))","v":false},"Alberta","Alberta"]
["Concrete - 25 MPa, 10% FA, GU / ARMCA / Can. Alberta Avg. / ","Concrete - 25 MPa, 10% FA, GU","ARMCA","Can. Alberta Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",312.37,"m3",312.37,"m3","EPD 346","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,364,"0-25",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS386:$BB386,0))","v":false},"Alberta","Alberta"]
["Concrete - 25 MPa, 20% FA, GU / ARMCA / Can. Alberta Avg. / ","Concrete - 25 MPa, 20% FA, GU","ARMCA","Can. Alberta Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",282.5,"m3",282.5,"m3","EPD 346","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,365,"0-25",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS387:$BB387,0))","v":false},"Alberta","Alberta"]
["Concrete - 30 MPa, GU / ARMCA / Can. Alberta Avg. / ","Concrete - 30 MPa, GU","ARMCA","Can. Alberta Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",384.98,"m3",384.98,"m3","EPD 346","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,366,"26-30",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS388:$BB388,0))","v":false},"Alberta","Alberta"]
["Concrete - 30 MPa, 10% FA, GU / ARMCA / Can. Alberta Avg. / ","Concrete - 30 MPa, 10% FA, GU","ARMCA","Can. Alberta Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",351.67,"m3",351.67,"m3","EPD 346","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,367,"26-30",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS389:$BB389,0))","v":false},"Alberta","Alberta"]
["Concrete - 30 MPa, 20% FA, GU / ARMCA / Can. Alberta Avg. / ","Concrete - 30 MPa, 20% FA, GU","ARMCA","Can. Alberta Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",317.89999999999998,"m3",317.89999999999998,"m3","EPD 346","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,368,"26-30",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS390:$BB390,0))","v":false},"Alberta","Alberta"]
["Concrete - 35 MPa, GU / ARMCA / Can. Alberta Avg. / ","Concrete - 35 MPa, GU","ARMCA","Can. Alberta Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",435.13,"m3",435.13,"m3","EPD 346","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,369,"31-35",1,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS391:$BB391,0))","v":false},"Alberta","Alberta"]
["Concrete - 35 MPa, 10% FA, GU / ARMCA / Can. Alberta Avg. / ","Concrete - 35 MPa, 10% FA, GU","ARMCA","Can. Alberta Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",397.06,"m3",397.06,"m3","EPD 346","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,370,"31-35",2,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS392:$BB392,0))","v":false},"Alberta","Alberta"]
["Concrete - 35 MPa, 20% FA, GU / ARMCA / Can. Alberta Avg. / ","Concrete - 35 MPa, 20% FA, GU","ARMCA","Can. Alberta Avg.",null,null,null,"Avg of Mix with & without air","CA","2023-02-26",358.54,"m3",358.54,"m3","EPD 346","ASTM",2027,2305,"kg/m3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,371,"31-35",3,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS393:$BB393,0))","v":false},"Alberta","Alberta"]
["Vinyl flooring / Shaw - Patcraft / Luxury Vinyl Tile / 2 - 5 mm ","Vinyl flooring","Shaw - Patcraft","Luxury Vinyl Tile","2 - 5 mm ",null,null,null,"US & CA","2022-12-16",9.59,"m2",9.59,"m²","4790050503.103.1","UL Environment",2026,5.7600000000000004E-3,"g/mm2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,372,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS394:$BB394,0))","v":false}]
["Linoleum flooring / Gerflor  / DLW Linoleum Compact / 2.5 mm sheet style linoleum","Linoleum flooring","Gerflor ","DLW Linoleum Compact","2.5 mm sheet style linoleum",null,null,null,"US","2022-12-21",0.10099999999999998,"m²",4.6609400000000001,"m²","4788756650.102.1 ","UL Environment",2025,2.94,"kg/m2",null,null,null,null,null,null,null,{"$f":"AF395*rng_biogenic_storage","v":5.742},null,null,null,null,6.38,null,null,2.5300000000000001E-3,null,null,373,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS395:$BB395,0))","v":false}]
["Fiberglass loose fill / Johns Manville / Climate Pro, Attic Protector, JM Spider PLUS (Canada) / R 2.8/inch, Formaldehyde-free","Fiberglass loose fill","Johns Manville","Climate Pro, Attic Protector, JM Spider PLUS (Canada)","R 2.8/inch, Formaldehyde-free",null,null,null,"US & CA","2022-12-21",0.55100000000000005,"m2•RSI",0.55100000000000005,"m2•RSI","4789973160.110.1","UL Environment",2028,0.46,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,374,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS396:$BB396,0))","v":false}]
["Window - double pane / Andersen / E-series (Average Double-hung/Awning/Picture) / Wood frame, aluminum cladding","Window - double pane","Andersen","E-series (Average Double-hung/Awning/Picture)","Wood frame, aluminum cladding",null,null,"No biogenic carbon credited","US & CA","2023-02-26",73.8,"m²",73.8,"m²","SCS-EPD-07201","SCS Global Services",2026,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,375,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS397:$BB397,0))","v":false}]
["Drywall 1/2\" / National Gypsum / Gold Bond XP Gypsum Board  / 1/2\" (12.7 mm)","Drywall 1/2\"","National Gypsum","Gold Bond XP Gypsum Board ","1/2\" (12.7 mm)",null,null,null,"US & CA","2023-02-26",428,"92.9m2",4.6071044133476855,"m2 @ 1/2\"","EPD10792","NSF",2027,859,"kg/92.9m2",{"$f":"R398/92.9","v":9.2465016146393975},"kg/m2",null,null,null,0.05,0.5,{"$f":"(AF398)*rng_biogenic_storage","v":0.76283638320775027},null,null,{"$f":"Y398*Z398*T398","v":0.23116254036598494},null,{"$f":"AD398*44/12","v":0.84759598134194469},null,null,null,null,null,376,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS398:$BB398,0))","v":false}]
["Drywall 5/8\" Type X / National Gypsum / Gold Bond XP Fire-Shield Gypsum Board  / 5/8'' type X","Drywall 5/8\" Type X","National Gypsum","Gold Bond XP Fire-Shield Gypsum Board ","5/8'' type X",null,null,null,"US & CA","2023-02-26",481,"92.9m2",5.177610333692142,"m2 @ 5/8\"","EPD10792","NSF",2027,1195,"kg/92.9m2",12.86329386437029,"kg/m2",null,null,null,0.05,0.5,{"$f":"(AF399)*rng_biogenic_storage","v":1.0612217438105491},null,null,{"$f":"Y399*Z399*T399","v":0.32158234660925727},null,{"$f":"AD399*44/12","v":1.17913527090061},null,null,null,null,null,377,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS399:$BB399,0))","v":false}]
["Carpet / J+J Flooring / Standard Back / all Broadloom styles","Carpet","J+J Flooring","Standard Back","all Broadloom styles",null,null,null,"US & CA","2023-02-26",9.44,"m²",9.44,"m²","EPD10781","NSF",2024,2.16,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.065E-2,null,null,378,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS400:$BB400,0))","v":false}]
["Vinyl flooring / Mannington / Luxury Vinyl Tile / 2.5 mm Tile and Plank","Vinyl flooring","Mannington","Luxury Vinyl Tile","2.5 mm Tile and Plank",null,null,null,"US & CA","2023-02-26",6.51,"m²",6.51,"m²","EPD10668","NSF",2026,2.79,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.5000000000000001E-3,null,null,379,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS401:$BB401,0))","v":false}]
["Asphalt Shingles / GAF / Timberline Cool Series / ","Asphalt Shingles","GAF","Timberline Cool Series",null,null,null,null,"US & CA","2023-02-26",4.34,"m²",4.34,"m²","EPD10396","NSF",2025,10.119999999999999,"kg/m2","Excl. Fasteners",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,380,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS402:$BB402,0))","v":false}]
["Linoleum flooring / Mannington / Legato Flooring / liquid applied","Linoleum flooring","Mannington","Legato Flooring","liquid applied",null,null,null,"US & CA","2023-02-26",2.65,"m²",2.65,"m²","EPD10362","NSF",2025,0.9,"kg/dm3",1.98,"kg/m2",null,null,null,null,0.6,{"$f":"(AF403)*rng_biogenic_storage","v":3.9203999999999999},null,null,{"$f":"Z403*T403","v":1.1879999999999999},null,{"$f":"AD403*44/12","v":4.3559999999999999},null,null,2.2000000000000001E-3,null,null,381,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS403:$BB403,0))","v":false}]
["Ceramic tile / Fireclay Tile / Ceramic - recycled content / Standard and Second grade","Ceramic tile","Fireclay Tile","Ceramic - recycled content","Standard and Second grade",null,null,"recycled content","US & CA","2023-02-26",45.9,"m²",45.9,"m²","EPD10355","NSF",2025,17.579999999999998,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7.9399999999999991E-3,null,null,382,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS404:$BB404,0))","v":false}]
["Ceramic tile / American Wonder Porcelain / Procelain - recycled content / Standard and Second grade","Ceramic tile","American Wonder Porcelain","Procelain - recycled content","Standard and Second grade",null,null,null,"US & CA","2023-02-26",11.5,"m²",11.5,"m²","EPD10277","NSF",2024,20.105,"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8.8500000000000002E-3,null,null,383,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS405:$BB405,0))","v":false}]
["Fiber Cement siding / Equitone / Pictura and Natura Pro / 8 mm (5/16\")","Fiber Cement siding","Equitone","Pictura and Natura Pro","8 mm (5/16\")",null,null,null,"Global","2023-02-26",16.305,"m²",16.305,"m2 at 8 mm (5/16\")","EPD-ETE-20190179-CCC1-EN","IBU",2025,1850,"kg/m3",{"$f":"R406*0.008","v":14.8},"kg/m2 at 8mm",null,null,null,9.5000000000000001E-2,0.5,{"$f":"(AF406)*rng_biogenic_storage","v":2.3199000000000005},"m²",null,{"$f":"Y406*Z406*T406","v":0.70300000000000007},null,{"$f":"AD406*44/12","v":2.577666666666667},null,null,null,null,null,384,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS406:$BB406,0))","v":false}]
["Fiber Cement siding / Equitone / Tectiva / 8 mm (5/16\")","Fiber Cement siding","Equitone","Tectiva","8 mm (5/16\")",null,null,null,"Global","2023-02-26",8.06,"m²",8.06,"m2 at 8 mm (5/16\")","EPD-ETE-20190007-ICA1-EN","IBU",2024,null,null,14.22,"kg/m2 at 8mm",null,null,null,9.5000000000000001E-2,0.5,{"$f":"(AF407)*rng_biogenic_storage","v":2.2289849999999998},"m²",null,{"$f":"Y407*Z407*T407","v":0.67544999999999999},null,{"$f":"AD407*44/12","v":2.4766499999999998},null,null,null,null,null,385,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS407:$BB407,0))","v":false}]
["Fiber Cement siding / Equitone / Natura, Textura and Materia / 8 mm (5/16\")","Fiber Cement siding","Equitone","Natura, Textura and Materia","8 mm (5/16\")",null,null,null,"Global","2023-02-26",11.324,"m²",11.324,"m2 at 8 mm (5/16\")","EPD-ELH-20180136-CAC1-EN","IBU",2024,null,null,15.07,"kg/m2 at 8mm",null,null,null,0.05,0.5,{"$f":"(AF408)*rng_biogenic_storage","v":1.2432750000000001},"m²",null,{"$f":"Y408*Z408*T408","v":0.37675000000000003},null,{"$f":"AD408*44/12","v":1.3814166666666667},null,null,null,null,null,386,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS408:$BB408,0))","v":false}]
["Straw Panels / Ecocoon / Standard and Brace Panels / 40cm R16, panel only","Straw Panels","Ecocoon","Standard and Brace Panels","40cm R16, panel only",null,null,"Wooden frame with straw filling",null,"2023-02-26",14.3,"m²",14.3,"m²","EPD-2022-7601","N.a.",2027,110,"kg/m3",{"$f":"R409*0.4","v":44},"kg/m2 at 40cm",{"$f":"0.0254*5.678/W409","v":0.99462896551724145},0.14499999999999999,null,0.9,0.5,{"$f":"(AF409)*rng_biogenic_storage","v":65.34},"m²",null,{"$f":"Y409*Z409*T409","v":19.8},null,{"$f":"AD409*44/12","v":72.600000000000009},null,null,null,null,null,387,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS409:$BB409,0))","v":false}]
["Brick, Clay / SHAW / Slender - Thin Face Brick / 2 1/4\" x 1/2\" x 7-1/2\" (57 x 12.7 mm x 190) incl. 3/8\" mortar","Brick, Clay","SHAW","Slender - Thin Face Brick","2 1/4\" x 1/2\" x 7-1/2\" (57 x 12.7 mm x 190) incl. 3/8\" mortar",null,null,null,"US & CA","2023-02-26",721,"m3",8.1808319999999988,"m²","EPD 359","ASTM",2027,269,"kgCO2/m3 mortar",null,"83% brick, 17% mortar",null,null,null,null,null,null,null,null,null,null,null,0.56999999999999995,0.19,1.2699999999999999E-2,{"$f":"AI410*AH410*AG410","v":1.3754099999999997E-3},null,388,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS410:$BB410,0))","v":false}]
["Brick, Clay / SHAW / Avg Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar","Brick, Clay","SHAW","Avg Face Brick","3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar",null,null,null,"US & CA","2023-02-26",721,"m3",59.262719999999995,"m²","EPD 359","ASTM",2027,269,"kgCO2/m3 mortar",null,"83% brick, 17% mortar",null,null,null,null,null,null,null,null,null,null,null,7.0000000000000007E-2,0.19367500000000001,9.1999999999999998E-2,1.247267E-3,null,389,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS411:$BB411,0))","v":false}]
["Rebar / Nucor Corporation / Canadian sizes / 10M","Rebar","Nucor Corporation","Canadian sizes","10M",null,null,null,"North America","2022-03-17",0.86299999999999999,"kg",0.67745500000000003,"m","4789793365.101.1","UL Environment",2026,7800,"kg/m3",0.78500000000000003,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,390,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS412:$BB412,0))","v":false}]
["Rebar / Nucor Corporation / Canadian sizes / 15M","Rebar","Nucor Corporation","Canadian sizes","15M",null,null,null,"North America","2022-03-17",0.86299999999999999,"kg",1.3549100000000001,"m","4789793365.101.1","UL Environment",2026,7800,"kg/m3",1.57,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,391,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS413:$BB413,0))","v":false}]
["Rebar / Nucor Corporation / Canadian sizes / 20M","Rebar","Nucor Corporation","Canadian sizes","20M",null,null,null,"North America","2022-03-17",0.86299999999999999,"kg",2.032365,"m","4789793365.101.1","UL Environment",2026,7800,"kg/m3",2.355,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,392,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS414:$BB414,0))","v":false}]
["Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 10M","Rebar","ArcelorMittal Long Products Canada","Canadian sizes","10M",null,null,null,"Canada","2022-03-17",1.2855000000000001,"kg",1.0091175000000001,"m","4937-6316","CSA Groups",2024,7850,"kg/m3",0.78500000000000003,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,393,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS415:$BB415,0))","v":false}]
["Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 15M","Rebar","ArcelorMittal Long Products Canada","Canadian sizes","15M",null,null,null,"Canada","2022-03-17",1.2855000000000001,"kg",2.0182350000000002,"m","4937-6316","CSA Groups",2024,7850,"kg/m3",1.57,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,394,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS416:$BB416,0))","v":false}]
["Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 20M","Rebar","ArcelorMittal Long Products Canada","Canadian sizes","20M",null,null,null,"Canada","2022-03-17",1.2855000000000001,"kg",3.0273525000000001,"m","4937-6316","CSA Groups",2024,7850,"kg/m3",2.355,"kg/m",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,395,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS417:$BB417,0))","v":false}]
["Wood fiber board / North American Fiberboard Association / Includes: MSL, Blue Ridge Fiberboard Inc. / R 2.7/inch","Wood fiber board","North American Fiberboard Association","Includes: MSL, Blue Ridge Fiberboard Inc.","R 2.7/inch",null,null,null,"US & CA","2022-03-20",196.13,"m3",10.634360600947366,"m2•RSI","4789410886.101.1","UL Environment",2026,254,"kg/m3",13.772128652631576,"kg/m2•RSI",2.66,{"$f":"1/V418*0.0254*5.67826","v":5.4220978947368409E-2},null,0.92200000000000004,0.5,{"$f":"(AF418)*rng_biogenic_storage","v":20.951539319248422},"m2•RSI",null,{"$f":"Y418*Z418*T418","v":6.3489513088631568},null,{"$f":"AD418*44/12","v":23.279488132498244},null,null,null,null,null,397,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS418:$BB418,0))","v":false}]
[{"$f":"B419&\" / \"&C419&\" / \"&D419&\" / \"&E419","v":"(ARCHIVED 2023) XPS foam board / DuPont / Styrofoam (Blue) (Legacy) / R 5.6/inch"},"(ARCHIVED 2023) XPS foam board","DuPont","Styrofoam (Blue) (Legacy)","R 5.6/inch",null,null,"Includes B1 offgasing","US & CA",null,60.8,"m2•RSI",60.8,"m2•RSI","4789559274.101.1","UL Environment",2026,null,null,null,null,5.6,{"$f":"0.0254*5.678/V419","v":2.5753785714285715E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,398,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS419:$BB419,0))","v":false}]
["(ARCHIVED 2023) XPS foam board / DuPont / Styrofoam (Grey, Reduced GWP) / R 5.6/inch","(ARCHIVED 2023) XPS foam board","DuPont","Styrofoam (Grey, Reduced GWP)","R 5.6/inch",null,null,"Includes B1 offgasing","US & CA",null,36.5,"m2•RSI",36.5,"m2•RSI","4789559274.102.1","UL Environment",2026,null,null,null,null,5.6,2.5753785714285715E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,399,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS420:$BB420,0))","v":false}]
["XPS foam board / DuPont / Reduced GWP Grey Styrofoam™ (same as ST-100) / R 5.0/inch","XPS foam board","DuPont","Reduced GWP Grey Styrofoam™ (same as ST-100)","R 5.0/inch",null,null,"Includes B1 offgasing","US & CA",null,4.67,"m2•RSI",4.67,"m2•RSI","4790979004.101.1","UL Environment",2026,null,null,null,null,5,2.884424E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,400,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS421:$BB421,0))","v":false}]
["XPS foam board / Soprema / SOPRA-XPS / R 5.0/inch","XPS foam board","Soprema","SOPRA-XPS","R 5.0/inch",null,null,"Includes B1 offgasing","US & CA","2022-04-01",1.92588,"m2•RSI",1.92588,"m2•RSI","EPD-283","ASTM International",2026,32.799999999999997,"kg/m3",1.1020000000000001,"kg/m2 at RSI1",5,2.884424E-2,null,null,null,null,null,null,null,null,null,2.4384000000000001,0.60960000000000003,null,null,null,401,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS422:$BB422,0))","v":false}]
["Mineral wool batt / Rockwool / ComfortBatt R14 / R 4.0/inch, 3.5\"","Mineral wool batt","Rockwool","ComfortBatt R14","R 4.0/inch, 3.5\"",null,null,null,"CAN","2021-08-12",1.179,"m2•RSI",1.179,"m2•RSI","4789092768.101.1 ","UL Environment",2024,null,null,2.4700000000000002,"RSI (m2K/W)",4,3.6055299999999998E-2,null,null,null,null,null,null,null,null,null,null,8.8999999999999996E-2,null,null,null,402,null,null,null,{"$f":"IF(LEN(Q423)=4,IF(Q423<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q423),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS423:$BB423,0))","v":false}]
["Mineral wool batt / Rockwool / ComfortBatt R15 / R 4.3/inch, 3.5\"","Mineral wool batt","Rockwool","ComfortBatt R15","R 4.3/inch, 3.5\"",null,null,null,"US","2021-08-12",1.31,"m2•RSI",1.31,"m2•RSI","4789092768.101.1 ","UL Environment",2024,null,null,2.64,"RSI (m2K/W)",4.3,3.3539813953488373E-2,null,null,null,null,null,null,null,null,null,null,8.8999999999999996E-2,null,null,null,403,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS424:$BB424,0))","v":false}]
["Mineral wool batt / Rockwool / ComfortBatt R22 / R 4.0/inch, 5.5\"","Mineral wool batt","Rockwool","ComfortBatt R22","R 4.0/inch, 5.5\"",null,null,null,"CAN","2021-08-12",1.179,"m2•RSI",1.179,"m2•RSI","4789092768.101.1 ","UL Environment",2024,null,null,3.87,"RSI (m2K/W)",4,3.6055299999999998E-2,null,null,null,null,null,null,null,null,null,null,0.14000000000000001,null,null,null,404,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS425:$BB425,0))","v":false}]
["Mineral wool batt / Rockwool / ComfortBatt R24 / R 4.4/inch, 5.5\"","Mineral wool batt","Rockwool","ComfortBatt R24","R 4.4/inch, 5.5\"",null,null,null,"CAN","2021-08-12",1.7030000000000001,"m2•RSI",1.7030000000000001,"m2•RSI","4789092768.101.1 ","UL Environment",2024,null,null,4.2300000000000004,"RSI (m2K/W)",4.367,3.3025234714907259E-2,null,null,null,null,null,null,null,null,null,null,0.14000000000000001,null,null,null,405,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS426:$BB426,0))","v":false}]
["Mineral wool batt / Rockwool / ComfortBatt R24 SS / R 4.0/inch, 6\" Steel Studs","Mineral wool batt","Rockwool","ComfortBatt R24 SS","R 4.0/inch, 6\" Steel Studs",null,null,null,"CAN","2021-08-12",1.179,"m2•RSI",1.179,"m2•RSI","4789092768.101.1 ","UL Environment",2024,null,null,4.2300000000000004,"RSI (m2K/W)",4,3.6055299999999998E-2,null,null,null,null,null,null,null,null,null,null,0.152,null,null,null,406,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS427:$BB427,0))","v":false}]
["Mineral wool board  / Rockwool / Comfortboard 80 / R 4.2/inch","Mineral wool board ","Rockwool","Comfortboard 80","R 4.2/inch",null,null,null,"US & CA","2021-10-01",4.0609999999999999,"m2•RSI",4.0609999999999999,"m2•RSI","4789092768.101.1","UL Environment",2024,128,"kg/m3",null,null,4.2,3.4338380952380947E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,407,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS428:$BB428,0))","v":false}]
["Polyiso - wall boards / DuPont / Thermax / R 6.5/inch","Polyiso - wall boards","DuPont","Thermax","R 6.5/inch",null,null,null,"US & CA","2022-03-11",2.39,"m2•RSI",2.39,"m2•RSI","4789559274.103.1","UL Environment",2026,29.53,"kg/m3",null,null,6.5,2.2187876923076923E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,408,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS429:$BB429,0))","v":false}]
["Laminated veneer lumber / Roseburg Forest Products / RigidLam LVL / ","Laminated veneer lumber","Roseburg Forest Products","RigidLam LVL",null,null,null,"No biogenic carbon credited","US & CA","2022-04-27",274,"m3",274,"m3","4786969381.104.1","UL Environment",2023,539,"kg/m3",null,null,null,null,null,0.95599999999999996,0.5,null,"m3",null,null,null,null,null,null,null,null,null,409,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS430:$BB430,0))","v":false}]
["Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / ","Spray polyurethane foam - Closed Cell (HFO)","Huntsman Building Solutions","Heatlok HFO & Heatlok Soya HFO",null,null,null,null,"US & CA","2022-04-26",2.5026000000000002,"m2•RSI",2.5026000000000002,"m2•RSI","4789773836.101.1","UL Environment",2026,38.4,"kg/m3",null,null,6.5,{"$f":"0.0254*5.678/V431","v":2.2187876923076923E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,410,null,null,null,"A1-B1",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS431:$BB431,0))","v":false}]
["Polyiso - wall boards / PIMA / Includes: Atlas, Firestone, GAF, Johns Manville, Rmax, Carlisle, Iko, Soprema / R 6.5/inch","Polyiso - wall boards","PIMA","Includes: Atlas, Firestone, GAF, Johns Manville, Rmax, Carlisle, Iko, Soprema","R 6.5/inch",null,null,null,"US","2022-03-13",4.0959000000000003,"m2•RSI",4.0959000000000003,"m2•RSI","EPD10466","NSF",2025,49.09,"kg/m3",null,null,6.5,2.2187876923076923E-2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,411,null,null,null,{"$f":"IF(LEN(Q432)=4,IF(Q432<YEAR(NOW()),_xlfn.CONCAT(\"Expired \",Q432),\"\"),\"\")","v":""},null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS432:$BB432,0))","v":false}]
["Straw Bale / SNaB (UK) / Wheat & barley straw / R 2.8/inch","Straw Bale","SNaB (UK)","Wheat & barley straw","R 2.8/inch",null,null,null,"EU","2022-03-14",12.947115,"m3",0.67324998000000003,"m2•RSI","S-P-03854","EPD International AB",2026,100,"kg/m3",{"$f":"R433*W433","v":5.2},"kg/m2•RSI",{"$f":"0.0254*5.678/W433","v":2.7734846153846155},5.1999999999999998E-2,null,null,0.47660000000000002,{"$f":"(AF433)*rng_biogenic_storage","v":6.0371751959999997},"m2•RSI",null,128.99947,"From EPD",{"$f":"AD433*W433","v":6.7079724399999998},null,null,null,null,null,412,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS433:$BB433,0))","v":false}]
["Engineered Wood Siding & Trim / LP / SmartSide / 0.315\" (8 mm)","Engineered Wood Siding & Trim","LP","SmartSide","0.315\" (8 mm)",null,null,"SFI sourced raw logs (aspen)","US & CA",null,347.31,"m3",2.7784800000000001,"m2 at 8 mm (0.315\")","EPD192","ASTM International",2026,657,"kg/m3",null,null,null,null,null,0.8,0.48,null,"m2 at 8 mm (5/16\")",null,null,null,null,null,null,8.0000000000000002E-3,null,null,413,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS434:$BB434,0))","v":false}]
["Engineered Wood Siding & Trim / LP / SmartSide / 0.375\" (9.5 mm)","Engineered Wood Siding & Trim","LP","SmartSide","0.375\" (9.5 mm)",null,null,"SFI sourced raw logs (aspen)","US & CA",null,347.31,"m3",3.299445,"m2 at 9.5 mm (0.375\")","EPD192","ASTM International",2026,657,"kg/m3",null,null,null,null,null,0.81499999999999995,0.48,null,"m2 at 9.5 mm (3/8\")",null,null,null,null,null,null,9.4999999999999998E-3,null,null,414,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS435:$BB435,0))","v":false}]
["Engineered Wood Siding & Trim / LP / SmartSide / 0.530\" (13.5 mm)","Engineered Wood Siding & Trim","LP","SmartSide","0.530\" (13.5 mm)",null,null,"SFI sourced raw logs (aspen)","US & CA",null,347.31,"m3",4.6886849999999995,"m2 at 13.5 mm (0.530\")","EPD192","ASTM International",2026,657,"kg/m3",null,null,null,null,null,0.85499999999999998,0.48,null,"m2 at 13.5 mm (0.530\")",null,null,null,null,null,null,1.35E-2,null,null,415,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS436:$BB436,0))","v":false}]
["Window - double pane / Inline Fiberglass / 300 Series Tilt and Turn, 300 Series Fixed, 325 Series Awning/Casement, 325 Series Fixed, and 400 Series / Fiberglass frame","Window - double pane","Inline Fiberglass","300 Series Tilt and Turn, 300 Series Fixed, 325 Series Awning/Casement, 325 Series Fixed, and 400 Series","Fiberglass frame",null,null,"Assumed to be double-glazed","CAN","2022-03-19",75.7,"m²",75.7,"m2 of window","EPD 266","ASTM International",2026,60.5,"kg",{"$f":"R437/(AG437*AH437)","v":31.025641025641022},"kg/m2 window",null,null,null,null,null,null,null,null,null,null,null,1.3,1.5,null,null,null,416,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS437:$BB437,0))","v":false}]
["Fiber Cement siding / James Hardie / HardiePanel® / 8 mm","Fiber Cement siding","James Hardie","HardiePanel®","8 mm",null,null,null,"EU","2022-05-18",8.94,"m2",8.94,"m²","S-P-01432","International EPD® System",2023,1300,"kg/m3",11.2,"kg/m2 at 8mm",null,null,null,6.5000000000000002E-2,0.5,{"$f":"(AF438)*rng_biogenic_storage","v":1.1970000000000001},"m²",1.84,0.36399999999999999,null,1.33,null,null,8.0000000000000002E-3,null,null,417,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS438:$BB438,0))","v":false}]
["Gypsum panels - glass mat / CertainTeed / GlasRoc Sheathing gypsum board / 5/8\" ","Gypsum panels - glass mat","CertainTeed","GlasRoc Sheathing gypsum board","5/8\" ",null,null,null,"US",null,310,"92.9m2",3.3369214208826694,"m2 @ 5/8\"","4789532059.140.1","UL Environment",2026,1165,"kg/92.9m2",{"$f":"R439/92.9","v":12.540365984930032},"kg/m2",null,null,null,null,null,null,null,null,null,null,null,null,5.8749999999999997E-2,null,null,null,418,null,null,null,"",null,{"$f":"ISNUMBER(MATCH(IF(LEN('USER INPUT SHEET'!rng_province)>0,'USER INPUT SHEET'!rng_province,\"Canada\"),$AS439:$BB439,0))","v":false}]
["Fiber Cement siding / James Hardie / Hardie VL Plank / 11 mm","Fiber Cement siding","James Hardie","Hardie VL Plank","11 mm",null,null,null,"EU","2022-05-18",12,"m2",12,"m²","S-P-01432 Version 2.0","International EPD® System",2023,1300,"kg/m3",13.6,"kg/m2 at 11mm",null,null,null,6.5000000000000002E-2,0.5,"1.62","m²",null,0.442,null,1.62,null,null,1.0999999999999999E-2,null,null,419,null,null,null,null,null,false]
["Fiber Cement siding / James Hardie / HardiePlank / 8 mm","Fiber Cement siding","James Hardie","HardiePlank","8 mm",null,null,null,"EU","2022-05-18",7.34,"m2",7.34,"m²","S-P-01432 Version 2.0","International EPD® System",2023,1300,"kg/m3",11.2,"kg/m2 at 8mm",null,null,null,6.5000000000000002E-2,0.5,"1.33","m²",1.84,0.36399999999999999,null,1.33,null,null,8.0000000000000002E-3,null,null,420,null,null,null,null,null,false]

{"sheet":"Composite Master Sheet","index":31,"n_rows":244,"n_cols":35,"rows_kept":244,"cut":false,"hidden":true,"merged":[]}
["Composite Product","Composite Emissions co2","Composite Storage CO2/m2","Unit","Material1","Incoming Unit","M1 Emission","M1 Storage","Material2","Incoming Unit","M2 Emission","M2 Storage","Material3","Incoming Unit","M3 Emission","M3 Storage","Material4","Incoming Unit","M4 Emission","M4 Storage","Material5","Incoming Unit","M5 Emission","M5 Storage","Notes","Product ID of Material1","Product ID of Material2","Product ID of Material3","Product ID of Material4","Product ID of Material5"]
["EPS FOAM ICF R-23, 2 Sheets of 2.75\" @ R4/in., 15M rebar (6\" CONCRETE CORE must be added separately)",{"$f":"G2+K2+O2+S2+W2","v":24.801453057919655},0,"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z2,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},"m2 RSI 1",{"$f":"VLOOKUP($E2,'Master sheet'!$A:$AJ,13,FALSE)*2*2.75*4/5.678","v":14.607256076083127},{"$f":"VLOOKUP($E2,'Master sheet'!$A:$AJ,27,FALSE)*2*2.75*4/5.678","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA2,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Polypropylene ICF webbing /  /  / "},"m2",{"$f":"VLOOKUP($I2,'Master sheet'!$A:$AJ,13,FALSE)","v":5.1219979818365289},{"$f":"VLOOKUP(I2,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB2,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Rebar / Concrete Reinforcing Steel Institute /  / 15M"},"m",{"$f":"VLOOKUP(M2,'Master sheet'!$A:$AJ,13,FALSE)*3.3","v":5.0721990000000003},{"$f":"VLOOKUP(M2,'Master sheet'!$A:$AJ,27,FALSE)*3.3","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC2,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD2,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,"Fill volume of concrete: 0.15875 m3/m2 of wall area",94,171,177,"",""]
["SIP PANEL - R23 6.5\" - EPS 5.5\" @ R4/in. core, 2 sheets 1/2\" OSB",20.76878807608313,0,"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z3,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},"m2 RSI 1",{"$f":"VLOOKUP($E3,'Master sheet'!$A:$AJ,13,FALSE)*4/5.678*5.5","v":14.607256076083129},{"$f":"VLOOKUP($E3,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA3,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 1/2\""},"m2",{"$f":"VLOOKUP($I3,'Master sheet'!$A:$AJ,13,FALSE)*2","v":6.1615320000000002},{"$f":"VLOOKUP($I3,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB3,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC3,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD3,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,null,94,154,"","",""]
["SIP PANEL - R30 8.25\" - EPS 7.25\" @ R4/in. core, 2 sheets 1/2\" OSB",25.41655137301867,0,"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z4,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},"m2 RSI 1",{"$f":"VLOOKUP($E4,'Master sheet'!$A:$AJ,13,FALSE)*4/5.678*7.25","v":19.255019373018669},{"$f":"VLOOKUP($E4,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA4,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 1/2\""},"m2",{"$f":"VLOOKUP($I4,'Master sheet'!$A:$AJ,13,FALSE)*2","v":6.1615320000000002},{"$f":"VLOOKUP($I4,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB4,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC4,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD4,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,null,94,154,"","",""]
["SIP PANEL - R38 10.5\" - EPS 9.5\" @ R4/in. core, 2 sheets 1/2\" OSB",31.392247040507225,0,"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z5,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},"m2 RSI 1",{"$f":"VLOOKUP($E5,'Master sheet'!$A:$AJ,13,FALSE)*4/5.678*9.5","v":25.230715040507224},{"$f":"VLOOKUP($E5,'Master sheet'!$A:$AJ,27,FALSE)*4/5.678*9.5","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA5,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 1/2\""},"m2",{"$f":"VLOOKUP($I5,'Master sheet'!$A:$AJ,13,FALSE)*2","v":6.1615320000000002},{"$f":"VLOOKUP($I5,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB5,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC5,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD5,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,null,94,154,"","",""]
["SIP PANEL - R48 12-7/8\" - EPS 11.875\" @ R4/in. core, 2 sheets 1/2\" OSB",37.699925800634027,0,"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z6,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},"m2 RSI 1",{"$f":"VLOOKUP($E6,'Master sheet'!$A:$AJ,13,FALSE)*4/5.678*11.875","v":31.538393800634029},{"$f":"VLOOKUP($E6,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA6,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 1/2\""},"m2",{"$f":"VLOOKUP($I6,'Master sheet'!$A:$AJ,13,FALSE)*2","v":6.1615320000000002},{"$f":"VLOOKUP($I6,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB6,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC6,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD6,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,null,94,154,"","",""]
["WOOD CHIP CEMENT ICF 12\" R-22 with MINERAL WOOL INSERTS, (3 in. @ R4.2/in.), 15M REBAR",{"$f":"G7+K7+O7+S7+W7","v":99.308101483469699},52.974029464220273,"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z7,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Wood chip cement ICF / Nexcem, Faswall /  / 12\" R22 block"},"m2",{"$f":"VLOOKUP($E7,'Master sheet'!$A:$AJ,13,FALSE)","v":76.12811805233197},{"$f":"VLOOKUP($E7,'Master sheet'!$A:$AJ,27,FALSE)","v":52.974029464220273},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA7,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Mineral wool board - heavy density / NAIMA / R 4.2/inch"},"m2 RSI 1",{"$f":"VLOOKUP($I7,'Master sheet'!$A:$AJ,13,FALSE)*(3*4.2/5.678)","v":18.107784431137727},{"$f":"VLOOKUP(I7,'Master sheet'!$A:$AJ,27,FALSE)*(3*4.2/5.678)","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB7,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Rebar / Concrete Reinforcing Steel Institute /  / 15M"},"m",{"$f":"VLOOKUP(M7,'Master sheet'!$A:$AJ,13,FALSE)*3.3","v":5.0721990000000003},{"$f":"VLOOKUP(M7,'Master sheet'!$A:$AJ,27,FALSE)*3.3","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC7,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD7,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,"Fill volume of concrete: 0.105 m3/m2 of wall area",236,149,177,"",""]
["WOOD CHIP CEMENT ICF 14\" R-28 with MINERAL WOOL INSERTS (5 in. @ R4.2/in.), 15M REBAR",119.39344388166664,58.550243092032943,"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z8,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Wood chip cement ICF / Nexcem, Faswall /  / 14\" R28 block"},"m2",{"$f":"VLOOKUP($E8,'Master sheet'!$A:$AJ,13,FALSE)","v":84.141604163103764},{"$f":"VLOOKUP($E8,'Master sheet'!$A:$AJ,27,FALSE)","v":58.550243092032943},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA8,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Mineral wool board - heavy density / NAIMA / R 4.2/inch"},"m2 RSI 1",{"$f":"VLOOKUP($I8,'Master sheet'!$A:$AJ,13,FALSE)*(5*4.2/5.678)","v":30.179640718562876},{"$f":"VLOOKUP($I8,'Master sheet'!$A:$AJ,27,FALSE)*(5*4.2/5.678)","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB8,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Rebar / Concrete Reinforcing Steel Institute /  / 15M"},"m",{"$f":"VLOOKUP(M8,'Master sheet'!$A:$AJ,13,FALSE)*3.3","v":5.0721990000000003},{"$f":"VLOOKUP(M8,'Master sheet'!$A:$AJ,27,FALSE)*3.3","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC8,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD8,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,"Fill volume of concrete: 0.098 m3/m2 of wall area",237,149,177,"",""]
["WOOD CHIP CEMENT ICF 12\" R-21 with CORK BOARD INSERTS (3 in. @ R4/in.), 15M REBAR",{"$f":"G9+K9+O9+S9+W9","v":87.48957383288851},{"$f":"H9+L9+P9+T9+X9","v":73.698819883381958},"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z9,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Wood chip cement ICF / Nexcem, Faswall /  / 12\" R22 block"},"m2",{"$f":"VLOOKUP($E9,'Master sheet'!$A:$AJ,13,FALSE)","v":76.12811805233197},{"$f":"VLOOKUP($E9,'Master sheet'!$A:$AJ,27,FALSE)","v":52.974029464220273},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA9,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Cork board insulation / Amorim / Isolamentos / R4/inch"},"m2 RSI 1",{"$f":"VLOOKUP($I9,'Master sheet'!$A:$AJ,13,FALSE)*(3*4/5.678)","v":6.2892567805565376},{"$f":"VLOOKUP(I9,'Master sheet'!$A:$AJ,27,FALSE)*(3*4/5.678)","v":20.724790419161678},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB9,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Rebar / Concrete Reinforcing Steel Institute /  / 15M"},"m",{"$f":"VLOOKUP(M9,'Master sheet'!$A:$AJ,13,FALSE)*3.3","v":5.0721990000000003},{"$f":"VLOOKUP(M9,'Master sheet'!$A:$AJ,27,FALSE)*3.3","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC9,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD9,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,"Fill volume of concrete: 0.105 m3/m2 of wall area",236,80,177,"",""]
["WOOD CHIP CEMENT ICF 14\" R-27 with CORK BOARD INSERTS (5 in. @ R4/in.), 15M REBAR",{"$f":"G10+K10+O10+S10+W10","v":99.695897797364651},{"$f":"H10+L10+P10+T10+X10","v":93.091560457302407},"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z10,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Wood chip cement ICF / Nexcem, Faswall /  / 14\" R28 block"},"m2",{"$f":"VLOOKUP($E10,'Master sheet'!$A:$AJ,13,FALSE)","v":84.141604163103764},{"$f":"VLOOKUP($E10,'Master sheet'!$A:$AJ,27,FALSE)","v":58.550243092032943},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA10,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Cork board insulation / Amorim / Isolamentos / R4/inch"},"m2 RSI 1",{"$f":"VLOOKUP($I10,'Master sheet'!$A:$AJ,13,FALSE)*(5*4/5.678)","v":10.482094634260896},{"$f":"VLOOKUP($I10,'Master sheet'!$A:$AJ,27,FALSE)*(5*4/5.678)","v":34.541317365269464},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB10,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Rebar / Concrete Reinforcing Steel Institute /  / 15M"},"m",{"$f":"VLOOKUP(M10,'Master sheet'!$A:$AJ,13,FALSE)*3.3","v":5.0721990000000003},{"$f":"VLOOKUP(M10,'Master sheet'!$A:$AJ,27,FALSE)*3.3","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC10,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD10,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,"Fill volume of concrete: 0.098 m3/m2 of wall area",237,80,177,"",""]
["TREATED WOOD FOUNDATION - 2x8 framing @ 16\" OC, 3/4\" plywood sheathing",8.6898397835717578,0,"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z11,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},"m3",{"$f":"VLOOKUP($E11,'Master sheet'!$A:$AJ,13,FALSE)*7.25*0.0254*0.25","v":2.9058869999999999},{"$f":"VLOOKUP($E11,'Master sheet'!$A:$AJ,27,FALSE)*7.25*0.0254*0.25","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA11,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Plywood / American Wood Council & Canadian Wood Council /  / 3/4\""},"m2",{"$f":"VLOOKUP($I11,'Master sheet'!$A:$AJ,13,FALSE)","v":4.1780460000000001},{"$f":"VLOOKUP($I11,'Master sheet'!$A:$AJ,27,FALSE)","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB11,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"ACQ wood treatment /  /  / "},"m2",{"$f":"VLOOKUP(M11,'Master sheet'!$A:$AJ,13,FALSE)*2","v":1.6059067835717582},{"$f":"VLOOKUP(M11,'Master sheet'!$A:$AJ,27,FALSE)*2","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC11,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD11,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,null,248,161,1,"",""]
["WOOD FRAME with STRAW BALE INFILL - 14\" R-46, Double 2x4 @ 30\" o/c",{"$f":"G12+K12+O12+S12+W12","v":5.0165688977809086},{"$f":"H12+L12+P12+T12+X12","v":55.14167122169777},"m2",{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z12,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},"m3",{"$f":"VLOOKUP($E12,'Master sheet'!$A:$AJ,13,FALSE)*2*3.5*0.0254*0.2","v":2.2445472},{"$f":"VLOOKUP($E12,'Master sheet'!$A:$AJ,27,FALSE)*2*3.5*0.0254*0.2","v":0},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA12,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":"Straw Bale /  / Wheat & rye straw / R 3.3/inch"},"m2 RSI 1",{"$f":"VLOOKUP($I12,'Master sheet'!$A:$AJ,13,FALSE)*(14*3.28/5.678)","v":2.7720216977809082},{"$f":"VLOOKUP($I12,'Master sheet'!$A:$AJ,27,FALSE)*(14*3.28/5.678)","v":55.14167122169777},{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB12,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC12,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD12,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,null,248,210,"","",""]
[null,null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z13,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA13,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB13,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC13,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD13,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,null,"","","","",""]
[null,null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!Z14,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AA14,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AB14,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AC14,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,{"$f":"_xlfn.IFNA(INDEX('Master sheet'!$A$1:$A$441,MATCH('Composite Master Sheet'!AD14,'Master sheet'!$AL$1:$AL$441,0)),\"\")","v":""},null,null,null,null,"","","","",""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"","","","",""]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"B122&\" / \"&C122&\" / \"&E122","v":" /  / "}]
[{"$f":"B123&\" / \"&C123&\" / \"&E123","v":" /  / "}]
[]
[]
[]
[]
[{"$f":"B128&\" / \"&C128&\" / \"&E128","v":" /  / "}]
[{"$f":"B129&\" / \"&C129&\" / \"&E129","v":" /  / "}]
[]
[]
[]
[]
[{"$f":"B134&\" / \"&C134&\" / \"&E134","v":" /  / "}]
[]
[{"$f":"B136&\" / \"&C136&\" / \"&E136","v":" /  / "}]
[{"$f":"B137&\" / \"&C137&\" / \"&E137","v":" /  / "}]
[null,null,null,null,"7/16\"",null,null,null,null,null,null,null,{"$f":"K138*0.0111","v":0},"m2 at 0.0111 m (1/2\")",null,null,null,null,null,{"$f":"R138*0.0111","v":0},"kg/m2 at 7/16\"",null,null,{"$f":"P138*T138*U138","v":{"$error":"#VALUE!"}},null,null,null,null,null,null,null,null,null,null,1.2699999999999999E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"P139*T139*U139","v":0},null,null,null,null,null,null,null,null,null,null,1.2699999999999999E-2]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,"0.085\" Single 7\" \"Cedar\" Shake"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"B179&\" / \"&D179&\" / \"&E179","v":" /  / "}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Straw Bale Infill"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[{"$f":"B203&\" / \"&D203&\" / \"&E203","v":" /  / "}]
[{"$f":"B204&\" / \"&D204&\" / \"&E204","v":" /  / "}]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["R-22 BLOCK - 2 LAYERS 2.75\" EPS FOAM with 6.25\" CONCRETE CORE","from Composite Master Sheet"]
[null,"from Composite Master Sheet"]
[null,"from Composite Master Sheet"]
[null,"from Composite Master Sheet"]
[null,"from Composite Master Sheet"]

{"sheet":"Data","index":32,"n_rows":285,"n_cols":24,"rows_kept":285,"cut":false,"hidden":true,"merged":[]}
["SECTION","COMPONENT","MATERIAL",{"$f":"SUM($D$3:$D$544)","v":0},{"$f":"SUM($E$3:$E$544)","v":0},{"$f":"SUM($F$3:$F$544)","v":0},{"$f":"SUM(G3:G520)","v":0},"Items selected","RANK","NET CARBON","TAB","SECTION","MATERIAL",null,"Year","Materials","Operations","Total"]
[]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B3)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B3))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B3)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B3))),\"\")","v":""},{"$f":"IFERROR(E3-F3,\"\")","v":""},{"$f":"IF(ROWS($B$3:$B3)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B3))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B3)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B3))),\"\")","v":""},{"$f":"COUNTIF('Footings & Slabs'!$H$1:$H$518,1)","v":0},null,1,{"$f":"LARGE($D$3:$D$1020,I3)","v":{"$error":"#NUM!"}},{"$f":"INDEX(A$3:A$1020,MATCH($J3,$D$3:$D$1020,0))","v":{"$error":"#NUM!"}},{"$f":"INDEX(B$3:B$1020,MATCH($J3,$D$3:$D$1020,0))","v":{"$error":"#NUM!"}},{"$f":"INDEX(C$3:C$1020,MATCH($J3,$D$3:$D$1020,0))","v":{"$error":"#NUM!"}},null,0,{"$f":"'USER INPUT SHEET'!M21","v":0},0,{"$f":"P3+Q3","v":0},null,"Emissions","Emissions Bar","Scaled iIndicator","Lower Bound","Upper Bound"]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B4)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B4))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B4)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B4))),\"\")","v":""},{"$f":"IFERROR(E4-F4,\"\")","v":""},{"$f":"IF(ROWS($B$3:$B4)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B4))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B4)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B4))),\"\")","v":""},null,null,2,{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},null,1,{"$f":"$P$3","v":0},{"$f":"'USER INPUT SHEET'!M16","v":0},{"$f":"P4+Q4","v":0},null,{"$f":"ROUND('USER INPUT SHEET'!$N$21,0)","v":0},{"$f":"IF(T4>400,400-$V$4/2,IF(T4=0,0,T4-$V$4/2))","v":0},{"$f":"IF(T4=0,0,IF(T4>0,ROUND((X4-W4)*0.0125,1),-ROUND((X4-W4)*0.0125,1)))","v":0},-200,400]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B5)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B5))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B5)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B5))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B5)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B5))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B5)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B5))),\"\")","v":""},null,null,3,{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},null,2,{"$f":"$P$3","v":0},{"$f":"Q4+Q$4","v":0},0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B6)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B6))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B6)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B6))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B6)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B6))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B6)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B6))),\"\")","v":""},null,null,4,{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},null,3,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B7)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B7))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B7)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B7))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B7)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B7))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B7)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B7))),\"\")","v":""},null,null,5,{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},null,4,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B8)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B8))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B8)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B8))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B8)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B8))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B8)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B8))),\"\")","v":""},null,null,6,{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},null,5,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B9)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B9))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B9)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B9))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B9)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B9))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B9)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B9))),\"\")","v":""},null,null,7,{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},null,6,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B10)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B10))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B10)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B10))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B10)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B10))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B10)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B10))),\"\")","v":""},null,null,8,{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},null,7,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B11)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B11))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B11)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B11))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B11)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B11))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B11)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B11))),\"\")","v":""},null,null,9,{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},null,8,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B12)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B12))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B12)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B12))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B12)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B12))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B12)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B12))),\"\")","v":""},null,null,10,{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},{"$error":"#NUM!"},null,9,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B13)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B13))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B13)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B13))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B13)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B13))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B13)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B13))),\"\")","v":""},null,null,null,null,null,null,null,null,10,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B14)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B14))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B14)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B14))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B14)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B14))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B14)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B14))),\"\")","v":""},null,null,null,null,null,null,null,null,11,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B15)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B15))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B15)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B15))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B15)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B15))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B15)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B15))),\"\")","v":""},null,null,null,null,"Section","Embodied Carbon \n[kg CO2e]",null,null,12,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B16)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B16))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B16)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B16))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B16)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B16))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B16)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B16))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"'Footings & Slabs'!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,13,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B17)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B17))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B17)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B17))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B17)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B17))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B17)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B17))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"'Foundation Walls'!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,14,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B18)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B18))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B18)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B18))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B18)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B18))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B18)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B18))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"},{"$f":"'Structural Elements'!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,15,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B19)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B19))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B19)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B19))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B19)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B19))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B19)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B19))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"'Ext. Walls'!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,16,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B20)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B20))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B20)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B20))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B20)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B20))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B20)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B20))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"'Ext. Wall Systems'!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,17,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B21)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B21))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B21)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B21))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B21)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B21))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B21)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B21))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"'Party Walls'!M4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,18,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B22)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B22))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B22)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B22))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B22)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B22))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B22)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B22))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"Cladding!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,19,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B23)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B23))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B23)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B23))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B23)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B23))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B23)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B23))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"Windows!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,20,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B24)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B24))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B24)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B24))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B24)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B24))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B24)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B24))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"'Int. Walls'!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,21,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B25)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B25))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B25)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B25))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B25)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B25))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B25)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B25))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"Floors!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,22,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B26)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B26))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B26)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B26))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B26)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B26))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B26)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B26))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"Ceilings!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,23,0,0,0]
[{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"},{"$f":"IF(ROWS($B$3:$B27)<=$G$3,INDEX('Footings & Slabs'!$P:$P,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B27))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B27)<=$G$3,INDEX('Footings & Slabs'!C:C,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B27))),\"\")","v":""},"",{"$f":"IF(ROWS($B$3:$B27)<=$G$3,INDEX('Footings & Slabs'!K:K,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B27))),\"\")","v":""},{"$f":"IF(ROWS($B$3:$B27)<=$G$3,INDEX('Footings & Slabs'!L:L,_xlfn.AGGREGATE(15,3,('Footings & Slabs'!$H$1:$H$251=1)/('Footings & Slabs'!$H$1:$H$251=1)*ROW('Footings & Slabs'!$H$1:$H$251),ROWS($B$3:$B27))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"Roof!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,24,0,0,0]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B28)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B28))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B28)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B28))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B28)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B28))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B28)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B28))),\"\")","v":""},{"$f":"COUNTIF('Foundation Walls'!$H$1:$H$551,1)","v":0},null,null,null,{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"Garage!$M$4+SUMIF('User-Defined'!A1:A100,VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE), 'User-Defined'!K1:K100)","v":0},null,null,25,0,0,0]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B29)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B29))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B29)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B29))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B29)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B29))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B29)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B29))),\"\")","v":""},null,null,null,null,{"$f":"VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE)","v":"User-Defined"},{"$f":"'User-Defined'!N4","v":0},null,null,26,0,0,0]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B30)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B30))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B30)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B30))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B30)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B30))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B30)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B30))),\"\")","v":""},null,null,null,null,"TOTAL",{"$f":"SUM(Summary[Embodied Carbon \n'[kg CO2e']])","v":0},null,null,27,0,0,0]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B31)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B31))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B31)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B31))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B31)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B31))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B31)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B31))),\"\")","v":""},null,null,null,null,null,null,null,null,28,0,0,0]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B32)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B32))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B32)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B32))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B32)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B32))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B32)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B32))),\"\")","v":""},null,null,null,null,null,null,null,null,29,0,0,0]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B33)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B33))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B33)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B33))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B33)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B33))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B33)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B33))),\"\")","v":""},null,null,null,null,null,null,null,null,30,0,0,0]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B34)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B34))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B34)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B34))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B34)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B34))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B34)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B34))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B35)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B35))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B35)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B35))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B35)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B35))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B35)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B35))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B36)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B36))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B36)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B36))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B36)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B36))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B36)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B36))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B37)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B37))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B37)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B37))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B37)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B37))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B37)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B37))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B38)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B38))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B38)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B38))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B38)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B38))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B38)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B38))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B39)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B39))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B39)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B39))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B39)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B39))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B39)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B39))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B40)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B40))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B40)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B40))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B40)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B40))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B40)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B40))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B41)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B41))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B41)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B41))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B41)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B41))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B41)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B41))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B42)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B42))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B42)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B42))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B42)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B42))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B42)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B42))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B43)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B43))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B43)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B43))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B43)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B43))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B43)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B43))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B44)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B44))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B44)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B44))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B44)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B44))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B44)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B44))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B45)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B45))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B45)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B45))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B45)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B45))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B45)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B45))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B46)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B46))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B46)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B46))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B46)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B46))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B46)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B46))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B47)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B47))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B47)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B47))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B47)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B47))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B47)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B47))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B48)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B48))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B48)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B48))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B48)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B48))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B48)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B48))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B49)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B49))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B49)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B49))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B49)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B49))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B49)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B49))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B50)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B50))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B50)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B50))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B50)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B50))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B50)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B50))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"},{"$f":"IF(ROWS($B$28:$B51)<=$G$28,INDEX('Foundation Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B51))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B51)<=$G$28,INDEX('Foundation Walls'!C:C,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B51))),\"\")","v":""},"",{"$f":"IF(ROWS($B$28:$B51)<=$G$28,INDEX('Foundation Walls'!K:K,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B51))),\"\")","v":""},{"$f":"IF(ROWS($B$28:$B51)<=$G$28,INDEX('Foundation Walls'!L:L,_xlfn.AGGREGATE(15,3,('Foundation Walls'!$H$1:$H$260=1)/('Foundation Walls'!$H$1:$H$260=1)*ROW('Foundation Walls'!$H$1:$H$260),ROWS($B$28:$B51))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"},{"$f":"IF(ROWS($B$52:$B52)<=$G$52,INDEX('Structural Elements'!$P:$P,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B52))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B52)<=$G$52,INDEX('Structural Elements'!C:C,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B52))),\"\")","v":""},"",{"$f":"IF(ROWS($B$52:$B52)<=$G$52,INDEX('Structural Elements'!K:K,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B52))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B52)<=$G$52,INDEX('Structural Elements'!L:L,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B52))),\"\")","v":""},{"$f":"COUNTIF('Structural Elements'!$H$1:$H$196,1)","v":0}]
[{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"},{"$f":"IF(ROWS($B$52:$B53)<=$G$52,INDEX('Structural Elements'!$P:$P,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B53))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B53)<=$G$52,INDEX('Structural Elements'!C:C,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B53))),\"\")","v":""},"",{"$f":"IF(ROWS($B$52:$B53)<=$G$52,INDEX('Structural Elements'!K:K,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B53))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B53)<=$G$52,INDEX('Structural Elements'!L:L,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B53))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"},{"$f":"IF(ROWS($B$52:$B54)<=$G$52,INDEX('Structural Elements'!$P:$P,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B54))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B54)<=$G$52,INDEX('Structural Elements'!C:C,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B54))),\"\")","v":""},"",{"$f":"IF(ROWS($B$52:$B54)<=$G$52,INDEX('Structural Elements'!K:K,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B54))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B54)<=$G$52,INDEX('Structural Elements'!L:L,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B54))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"},{"$f":"IF(ROWS($B$52:$B55)<=$G$52,INDEX('Structural Elements'!$P:$P,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B55))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B55)<=$G$52,INDEX('Structural Elements'!C:C,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B55))),\"\")","v":""},"",{"$f":"IF(ROWS($B$52:$B55)<=$G$52,INDEX('Structural Elements'!K:K,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B55))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B55)<=$G$52,INDEX('Structural Elements'!L:L,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B55))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"},{"$f":"IF(ROWS($B$52:$B56)<=$G$52,INDEX('Structural Elements'!$P:$P,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B56))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B56)<=$G$52,INDEX('Structural Elements'!C:C,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B56))),\"\")","v":""},"",{"$f":"IF(ROWS($B$52:$B56)<=$G$52,INDEX('Structural Elements'!K:K,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B56))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B56)<=$G$52,INDEX('Structural Elements'!L:L,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B56))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"},{"$f":"IF(ROWS($B$52:$B57)<=$G$52,INDEX('Structural Elements'!$P:$P,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B57))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B57)<=$G$52,INDEX('Structural Elements'!C:C,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B57))),\"\")","v":""},"",{"$f":"IF(ROWS($B$52:$B57)<=$G$52,INDEX('Structural Elements'!K:K,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B57))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B57)<=$G$52,INDEX('Structural Elements'!L:L,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B57))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"},{"$f":"IF(ROWS($B$52:$B58)<=$G$52,INDEX('Structural Elements'!$P:$P,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B58))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B58)<=$G$52,INDEX('Structural Elements'!C:C,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B58))),\"\")","v":""},"",{"$f":"IF(ROWS($B$52:$B58)<=$G$52,INDEX('Structural Elements'!K:K,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B58))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B58)<=$G$52,INDEX('Structural Elements'!L:L,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B58))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"},{"$f":"IF(ROWS($B$52:$B59)<=$G$52,INDEX('Structural Elements'!$P:$P,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B59))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B59)<=$G$52,INDEX('Structural Elements'!C:C,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B59))),\"\")","v":""},"",{"$f":"IF(ROWS($B$52:$B59)<=$G$52,INDEX('Structural Elements'!K:K,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B59))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B59)<=$G$52,INDEX('Structural Elements'!L:L,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B59))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"},{"$f":"IF(ROWS($B$52:$B60)<=$G$52,INDEX('Structural Elements'!$P:$P,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B60))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B60)<=$G$52,INDEX('Structural Elements'!C:C,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B60))),\"\")","v":""},"",{"$f":"IF(ROWS($B$52:$B60)<=$G$52,INDEX('Structural Elements'!K:K,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B60))),\"\")","v":""},{"$f":"IF(ROWS($B$52:$B60)<=$G$52,INDEX('Structural Elements'!L:L,_xlfn.AGGREGATE(15,3,('Structural Elements'!$H$1:$H$196=1)/('Structural Elements'!$H$1:$H$196=1)*ROW('Structural Elements'!$H$1:$H$196),ROWS($B$52:$B60))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B61)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B61))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B61)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B61))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B61)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B61))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B61)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B61))),\"\")","v":""},{"$f":"COUNTIF('Ext. Walls'!$H$1:$H$521,1)","v":0}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B62)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B62))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B62)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B62))),\"\")","v":""},{"$f":"IFERROR(E62-F62,\"\")","v":""},{"$f":"IF(ROWS($B$61:$B62)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B62))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B62)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B62))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B63)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B63))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B63)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B63))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B63)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B63))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B63)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B63))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B64)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B64))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B64)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B64))),\"\")","v":""},{"$f":"IFERROR(E64-F64,\"\")","v":""},{"$f":"IF(ROWS($B$61:$B64)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B64))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B64)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B64))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B65)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B65))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B65)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B65))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B65)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B65))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B65)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B65))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B66)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B66))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B66)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B66))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B66)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B66))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B66)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B66))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B67)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B67))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B67)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B67))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B67)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B67))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B67)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B67))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B68)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B68))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B68)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B68))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B68)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B68))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B68)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B68))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B69)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B69))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B69)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B69))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B69)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B69))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B69)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B69))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B70)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B70))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B70)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B70))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B70)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B70))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B70)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B70))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B71)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B71))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B71)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B71))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B71)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B71))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B71)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B71))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B72)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B72))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B72)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B72))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B72)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B72))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B72)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B72))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B73)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B73))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B73)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B73))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B73)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B73))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B73)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B73))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B74)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B74))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B74)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B74))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B74)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B74))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B74)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B74))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B75)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B75))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B75)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B75))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B75)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B75))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B75)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B75))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B76)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B76))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B76)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B76))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B76)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B76))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B76)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B76))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B77)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B77))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B77)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B77))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B77)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B77))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B77)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B77))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B78)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B78))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B78)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B78))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B78)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B78))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B78)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B78))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B79)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B79))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B79)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B79))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B79)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B79))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B79)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B79))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"},{"$f":"IF(ROWS($B$61:$B80)<=$G$61,INDEX('Ext. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B80))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B80)<=$G$61,INDEX('Ext. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B80))),\"\")","v":""},"",{"$f":"IF(ROWS($B$61:$B80)<=$G$61,INDEX('Ext. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B80))),\"\")","v":""},{"$f":"IF(ROWS($B$61:$B80)<=$G$61,INDEX('Ext. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Walls'!$H$1:$H$221=1)/('Ext. Walls'!$H$1:$H$221=1)*ROW('Ext. Walls'!$H$1:$H$221),ROWS($B$61:$B80))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B81)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B81))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B81)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B81))),\"\")","v":""},{"$f":"IFERROR(E81-F81,\"\")","v":""},{"$f":"IF(ROWS($B$81:$B81)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B81))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B81)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B81))),\"\")","v":""},{"$f":"COUNTIF('Ext. Wall Systems'!$H$1:$H$537,1)","v":0}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B82)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B82))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B82)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B82))),\"\")","v":""},{"$f":"IFERROR(E82-F82,\"\")","v":""},{"$f":"IF(ROWS($B$81:$B82)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B82))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B82)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B82))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B83)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B83))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B83)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B83))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B83)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B83))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B83)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B83))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B84)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B84))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B84)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B84))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B84)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B84))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B84)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B84))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B85)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B85))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B85)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B85))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B85)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B85))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B85)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B85))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B86)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B86))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B86)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B86))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B86)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B86))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B86)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B86))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B87)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B87))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B87)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B87))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B87)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B87))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B87)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B87))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B88)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B88))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B88)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B88))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B88)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B88))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B88)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B88))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B89)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B89))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B89)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B89))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B89)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B89))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B89)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B89))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B90)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B90))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B90)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B90))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B90)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B90))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B90)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B90))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B91)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B91))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B91)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B91))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B91)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B91))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B91)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B91))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B92)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B92))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B92)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B92))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B92)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B92))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B92)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B92))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B93)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B93))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B93)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B93))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B93)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B93))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B93)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B93))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"},{"$f":"IF(ROWS($B$81:$B94)<=$G$81,INDEX('Ext. Wall Systems'!$P:$P,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B94))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B94)<=$G$81,INDEX('Ext. Wall Systems'!C:C,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B94))),\"\")","v":""},"",{"$f":"IF(ROWS($B$81:$B94)<=$G$81,INDEX('Ext. Wall Systems'!K:K,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B94))),\"\")","v":""},{"$f":"IF(ROWS($B$81:$B94)<=$G$81,INDEX('Ext. Wall Systems'!L:L,_xlfn.AGGREGATE(15,3,('Ext. Wall Systems'!$H$1:$H$230=1)/('Ext. Wall Systems'!$H$1:$H$230=1)*ROW('Ext. Wall Systems'!$H$1:$H$230),ROWS($B$81:$B94))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B95)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B95))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B95)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B95))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B95)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B95))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B95)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B95))),\"\")","v":""},{"$f":"COUNTIF('Party Walls'!$H$1:$H$553,1)","v":0}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B96)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B96))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B96)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B96))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B96)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B96))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B96)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B96))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B97)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B97))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B97)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B97))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B97)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B97))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B97)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B97))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B98)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B98))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B98)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B98))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B98)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B98))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B98)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B98))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B99)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B99))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B99)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B99))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B99)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B99))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B99)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B99))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B100)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B100))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B100)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B100))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B100)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B100))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B100)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B100))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B101)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B101))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B101)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B101))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B101)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B101))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B101)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B101))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B102)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B102))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B102)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B102))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B102)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B102))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B102)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B102))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B103)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B103))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B103)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B103))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B103)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B103))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B103)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B103))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B104)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B104))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B104)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B104))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B104)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B104))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B104)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B104))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B105)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B105))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B105)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B105))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B105)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B105))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B105)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B105))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B106)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B106))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B106)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B106))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B106)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B106))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B106)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B106))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B107)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B107))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B107)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B107))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B107)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B107))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B107)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B107))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B108)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B108))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B108)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B108))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B108)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B108))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B108)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B108))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B109)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B109))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B109)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B109))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B109)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B109))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B109)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B109))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B110)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B110))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B110)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B110))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B110)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B110))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B110)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B110))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B111)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B111))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B111)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B111))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B111)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B111))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B111)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B111))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B112)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B112))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B112)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B112))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B112)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B112))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B112)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B112))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B113)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B113))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B113)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B113))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B113)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B113))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B113)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B113))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"},{"$f":"IF(ROWS($B$95:$B114)<=$G$95,INDEX('Party Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B114))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B114)<=$G$95,INDEX('Party Walls'!C:C,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B114))),\"\")","v":""},"",{"$f":"IF(ROWS($B$95:$B114)<=$G$95,INDEX('Party Walls'!K:K,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B114))),\"\")","v":""},{"$f":"IF(ROWS($B$95:$B114)<=$G$95,INDEX('Party Walls'!L:L,_xlfn.AGGREGATE(15,3,('Party Walls'!$H$1:$H$259=1)/('Party Walls'!$H$1:$H$259=1)*ROW('Party Walls'!$H$1:$H$259),ROWS($B$95:$B114))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B115)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B115))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B115)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B115))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B115)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B115))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B115)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B115))),\"\")","v":""},{"$f":"COUNTIF(Cladding!$H$1:$H$514,1)","v":0}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B116)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B116))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B116)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B116))),\"\")","v":""},{"$f":"IFERROR(E116-F116,\"\")","v":""},{"$f":"IF(ROWS($B$115:$B116)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B116))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B116)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B116))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B117)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B117))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B117)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B117))),\"\")","v":""},{"$f":"IFERROR(E117-F117,\"\")","v":""},{"$f":"IF(ROWS($B$115:$B117)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B117))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B117)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B117))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B118)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B118))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B118)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B118))),\"\")","v":""},{"$f":"IFERROR(E118-F118,\"\")","v":""},{"$f":"IF(ROWS($B$115:$B118)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B118))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B118)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B118))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B119)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B119))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B119)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B119))),\"\")","v":""},{"$f":"IFERROR(E119-F119,\"\")","v":""},{"$f":"IF(ROWS($B$115:$B119)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B119))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B119)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B119))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B120)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B120))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B120)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B120))),\"\")","v":""},{"$f":"IFERROR(E120-F120,\"\")","v":""},{"$f":"IF(ROWS($B$115:$B120)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B120))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B120)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B120))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B121)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B121))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B121)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B121))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B121)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B121))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B121)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B121))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B122)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B122))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B122)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B122))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B122)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B122))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B122)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B122))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B123)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B123))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B123)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B123))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B123)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B123))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B123)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B123))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B124)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B124))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B124)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B124))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B124)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B124))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B124)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B124))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B125)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B125))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B125)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B125))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B125)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B125))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B125)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B125))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B126)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B126))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B126)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B126))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B126)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B126))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B126)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B126))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B127)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B127))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B127)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B127))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B127)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B127))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B127)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B127))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B128)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B128))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B128)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B128))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B128)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B128))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B128)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B128))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B129)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B129))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B129)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B129))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B129)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B129))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B129)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B129))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B130)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B130))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B130)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B130))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B130)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B130))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B130)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B130))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B131)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B131))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B131)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B131))),\"\")","v":""},{"$f":"IFERROR(E131-F131,\"\")","v":""},{"$f":"IF(ROWS($B$115:$B131)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B131))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B131)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B131))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B132)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B132))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B132)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B132))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B132)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B132))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B132)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B132))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B133)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B133))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B133)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B133))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B133)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B133))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B133)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B133))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B134)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B134))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B134)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B134))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B134)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B134))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B134)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B134))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B135)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B135))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B135)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B135))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B135)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B135))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B135)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B135))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"},{"$f":"IF(ROWS($B$115:$B136)<=$G$115,INDEX(Cladding!$P:$P,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B136))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B136)<=$G$115,INDEX(Cladding!C:C,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B136))),\"\")","v":""},"",{"$f":"IF(ROWS($B$115:$B136)<=$G$115,INDEX(Cladding!K:K,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B136))),\"\")","v":""},{"$f":"IF(ROWS($B$115:$B136)<=$G$115,INDEX(Cladding!L:L,_xlfn.AGGREGATE(15,3,(Cladding!$H$1:$H$215=1)/(Cladding!$H$1:$H$215=1)*ROW(Cladding!$H$1:$H$215),ROWS($B$115:$B136))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B137)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B137))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B137)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B137))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B137)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B137))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B137)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B137))),\"\")","v":""},{"$f":"COUNTIF(Windows!$H$1:$H$196,1)","v":0}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B138)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B138))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B138)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B138))),\"\")","v":""},{"$f":"IFERROR(E138-F138,\"\")","v":""},{"$f":"IF(ROWS($B$137:$B138)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B138))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B138)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B138))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B139)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B139))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B139)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B139))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B139)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B139))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B139)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B139))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B140)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B140))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B140)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B140))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B140)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B140))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B140)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B140))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B141)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B141))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B141)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B141))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B141)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B141))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B141)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B141))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B142)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B142))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B142)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B142))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B142)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B142))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B142)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B142))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B143)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B143))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B143)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B143))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B143)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B143))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B143)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B143))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B144)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B144))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B144)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B144))),\"\")","v":""},{"$f":"IFERROR(E144-F144,\"\")","v":""},{"$f":"IF(ROWS($B$137:$B144)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B144))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B144)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B144))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B145)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B145))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B145)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B145))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B145)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B145))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B145)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B145))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B146)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B146))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B146)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B146))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B146)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B146))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B146)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B146))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B147)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B147))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B147)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B147))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B147)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B147))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B147)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B147))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B148)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B148))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B148)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B148))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B148)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B148))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B148)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B148))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B149)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B149))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B149)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B149))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B149)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B149))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B149)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B149))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"},{"$f":"IF(ROWS($B$137:$B150)<=$G$137,INDEX(Windows!$P:$P,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B150))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B150)<=$G$137,INDEX(Windows!C:C,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B150))),\"\")","v":""},"",{"$f":"IF(ROWS($B$137:$B150)<=$G$137,INDEX(Windows!K:K,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B150))),\"\")","v":""},{"$f":"IF(ROWS($B$137:$B150)<=$G$137,INDEX(Windows!L:L,_xlfn.AGGREGATE(15,3,(Windows!$H$1:$H$196=1)/(Windows!$H$1:$H$196=1)*ROW(Windows!$H$1:$H$196),ROWS($B$137:$B150))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B151)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B151))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B151)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B151))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B151)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B151))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B151)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B151))),\"\")","v":""},{"$f":"COUNTIF('Int. Walls'!$H$1:$H$510,1)","v":0}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B152)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B152))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B152)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B152))),\"\")","v":""},{"$f":"IFERROR(E152-F152,\"\")","v":""},{"$f":"IF(ROWS($B$151:$B152)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B152))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B152)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B152))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B153)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B153))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B153)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B153))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B153)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B153))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B153)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B153))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B154)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B154))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B154)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B154))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B154)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B154))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B154)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B154))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B155)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B155))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B155)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B155))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B155)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B155))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B155)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B155))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B156)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B156))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B156)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B156))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B156)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B156))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B156)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B156))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B157)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B157))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B157)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B157))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B157)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B157))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B157)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B157))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B158)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B158))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B158)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B158))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B158)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B158))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B158)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B158))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B159)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B159))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B159)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B159))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B159)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B159))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B159)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B159))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B160)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B160))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B160)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B160))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B160)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B160))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B160)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B160))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B161)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B161))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B161)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B161))),\"\")","v":""},{"$f":"IFERROR(E161-F161,\"\")","v":""},{"$f":"IF(ROWS($B$151:$B161)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B161))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B161)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B161))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B162)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B162))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B162)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B162))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B162)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B162))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B162)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B162))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B163)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B163))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B163)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B163))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B163)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B163))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B163)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B163))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B164)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B164))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B164)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B164))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B164)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B164))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B164)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B164))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B165)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B165))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B165)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B165))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B165)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B165))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B165)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B165))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B166)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B166))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B166)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B166))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B166)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B166))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B166)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B166))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B167)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B167))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B167)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B167))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B167)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B167))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B167)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B167))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B168)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B168))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B168)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B168))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B168)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B168))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B168)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B168))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B169)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B169))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B169)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B169))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B169)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B169))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B169)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B169))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B170)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B170))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B170)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B170))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B170)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B170))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B170)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B170))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B171)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B171))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B171)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B171))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B171)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B171))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B171)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B171))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B172)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B172))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B172)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B172))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B172)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B172))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B172)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B172))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B173)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B173))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B173)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B173))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B173)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B173))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B173)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B173))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B174)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B174))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B174)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B174))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B174)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B174))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B174)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B174))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B175)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B175))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B175)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B175))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B175)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B175))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B175)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B175))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"},{"$f":"IF(ROWS($B$151:$B176)<=$G$151,INDEX('Int. Walls'!$P:$P,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B176))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B176)<=$G$151,INDEX('Int. Walls'!C:C,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B176))),\"\")","v":""},"",{"$f":"IF(ROWS($B$151:$B176)<=$G$151,INDEX('Int. Walls'!K:K,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B176))),\"\")","v":""},{"$f":"IF(ROWS($B$151:$B176)<=$G$151,INDEX('Int. Walls'!L:L,_xlfn.AGGREGATE(15,3,('Int. Walls'!$H$1:$H$245=1)/('Int. Walls'!$H$1:$H$245=1)*ROW('Int. Walls'!$H$1:$H$245),ROWS($B$151:$B176))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B177)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B177))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B177)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B177))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B177)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B177))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B177)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B177))),\"\")","v":""},{"$f":"COUNTIF(Floors!$H$1:$H$513,1)","v":0}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B178)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B178))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B178)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B178))),\"\")","v":""},{"$f":"IFERROR(E178-F178,\"\")","v":""},{"$f":"IF(ROWS($B$177:$B178)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B178))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B178)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B178))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B179)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B179))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B179)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B179))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B179)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B179))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B179)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B179))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B180)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B180))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B180)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B180))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B180)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B180))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B180)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B180))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B181)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B181))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B181)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B181))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B181)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B181))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B181)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B181))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B182)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B182))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B182)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B182))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B182)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B182))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B182)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B182))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B183)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B183))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B183)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B183))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B183)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B183))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B183)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B183))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B184)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B184))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B184)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B184))),\"\")","v":""},{"$f":"IFERROR(E184-F184,\"\")","v":""},{"$f":"IF(ROWS($B$177:$B184)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B184))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B184)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B184))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B185)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B185))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B185)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B185))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B185)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B185))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B185)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B185))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B186)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B186))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B186)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B186))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B186)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B186))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B186)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B186))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B187)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B187))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B187)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B187))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B187)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B187))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B187)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B187))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B188)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B188))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B188)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B188))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B188)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B188))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B188)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B188))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B189)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B189))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B189)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B189))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B189)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B189))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B189)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B189))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B190)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B190))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B190)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B190))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B190)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B190))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B190)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B190))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B191)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B191))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B191)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B191))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B191)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B191))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B191)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B191))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B192)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B192))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B192)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B192))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B192)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B192))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B192)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B192))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B193)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B193))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B193)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B193))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B193)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B193))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B193)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B193))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B194)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B194))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B194)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B194))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B194)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B194))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B194)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B194))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B195)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B195))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B195)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B195))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B195)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B195))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B195)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B195))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"},{"$f":"IF(ROWS($B$177:$B196)<=$G$177,INDEX(Floors!$P:$P,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B196))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B196)<=$G$177,INDEX(Floors!C:C,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B196))),\"\")","v":""},"",{"$f":"IF(ROWS($B$177:$B196)<=$G$177,INDEX(Floors!K:K,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B196))),\"\")","v":""},{"$f":"IF(ROWS($B$177:$B196)<=$G$177,INDEX(Floors!L:L,_xlfn.AGGREGATE(15,3,(Floors!$H$1:$H$218=1)/(Floors!$H$1:$H$218=1)*ROW(Floors!$H$1:$H$218),ROWS($B$177:$B196))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B197)<=$G197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B197))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B197)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B197))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B197)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B197))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B197)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B197))),\"\")","v":""},{"$f":"COUNTIF(Ceilings!$H$1:$H$502,1)","v":0}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B198)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B198))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B198)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B198))),\"\")","v":""},{"$f":"IFERROR(E198-F198,\"\")","v":""},{"$f":"IF(ROWS($B$197:$B198)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B198))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B198)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B198))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B199)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B199))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B199)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B199))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B199)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B199))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B199)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B199))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B200)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B200))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B200)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B200))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B200)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B200))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B200)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B200))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B201)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B201))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B201)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B201))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B201)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B201))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B201)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B201))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B202)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B202))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B202)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B202))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B202)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B202))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B202)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B202))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B203)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B203))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B203)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B203))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B203)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B203))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B203)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B203))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B204)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B204))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B204)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B204))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B204)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B204))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B204)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B204))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B205)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B205))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B205)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B205))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B205)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B205))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B205)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B205))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B206)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B206))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B206)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B206))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B206)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B206))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B206)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B206))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B207)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B207))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B207)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B207))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B207)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B207))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B207)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B207))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B208)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B208))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B208)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B208))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B208)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B208))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B208)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B208))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B209)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B209))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B209)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B209))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B209)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B209))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B209)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B209))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B210)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B210))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B210)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B210))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B210)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B210))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B210)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B210))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B211)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B211))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B211)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B211))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B211)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B211))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B211)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B211))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B212)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B212))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B212)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B212))),\"\")","v":""},"",{"$f":"IF(ROWS($B$197:$B212)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B212))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B212)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B212))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B213)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B213))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B213)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B213))),\"\")","v":""},{"$f":"IFERROR(E213-F213,\"\")","v":""},{"$f":"IF(ROWS($B$197:$B213)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B213))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B213)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B213))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B214)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B214))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B214)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B214))),\"\")","v":""},{"$f":"IFERROR(E214-F214,\"\")","v":""},{"$f":"IF(ROWS($B$197:$B214)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B214))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B214)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B214))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B215)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B215))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B215)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B215))),\"\")","v":""},{"$f":"IFERROR(E215-F215,\"\")","v":""},{"$f":"IF(ROWS($B$197:$B215)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B215))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B215)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B215))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"},{"$f":"IF(ROWS($B$197:$B216)<=$G$197,INDEX(Ceilings!$P:$P,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B216))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B216)<=$G$197,INDEX(Ceilings!C:C,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B216))),\"\")","v":""},{"$f":"IFERROR(E216-F216,\"\")","v":""},{"$f":"IF(ROWS($B$197:$B216)<=$G$197,INDEX(Ceilings!K:K,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B216))),\"\")","v":""},{"$f":"IF(ROWS($B$197:$B216)<=$G$197,INDEX(Ceilings!L:L,_xlfn.AGGREGATE(15,3,(Ceilings!$H$1:$H$196=1)/(Ceilings!$H$1:$H$196=1)*ROW(Ceilings!$H$1:$H$196),ROWS($B$197:$B216))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B217)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B217))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B217)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B217))),\"\")","v":""},{"$f":"IFERROR(E217-F217,\"\")","v":""},{"$f":"IF(ROWS($B$217:$B217)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B217))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B217)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B217))),\"\")","v":""},{"$f":"COUNTIF(Roof!$H$1:$H$514,1)","v":0}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B218)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B218))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B218)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B218))),\"\")","v":""},{"$f":"IFERROR(E218-F218,\"\")","v":""},{"$f":"IF(ROWS($B$217:$B218)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B218))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B218)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B218))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B219)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B219))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B219)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B219))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B219)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B219))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B219)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B219))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B220)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B220))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B220)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B220))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B220)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B220))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B220)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B220))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B221)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B221))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B221)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B221))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B221)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B221))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B221)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B221))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B222)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B222))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B222)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B222))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B222)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B222))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B222)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B222))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B223)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B223))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B223)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B223))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B223)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B223))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B223)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B223))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B224)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B224))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B224)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B224))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B224)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B224))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B224)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B224))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B225)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B225))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B225)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B225))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B225)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B225))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B225)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B225))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B226)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B226))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B226)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B226))),\"\")","v":""},{"$f":"IFERROR(E226-F226,\"\")","v":""},{"$f":"IF(ROWS($B$217:$B226)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B226))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B226)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B226))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B227)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B227))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B227)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B227))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B227)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B227))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B227)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B227))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B228)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B228))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B228)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B228))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B228)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B228))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B228)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B228))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B229)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B229))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B229)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B229))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B229)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B229))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B229)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B229))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B230)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B230))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B230)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B230))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B230)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B230))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B230)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B230))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B231)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B231))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B231)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B231))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B231)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B231))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B231)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B231))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B232)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B232))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B232)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B232))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B232)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B232))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B232)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B232))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B233)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B233))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B233)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B233))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B233)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B233))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B233)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B233))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B234)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B234))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B234)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B234))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B234)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B234))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B234)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B234))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B235)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B235))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B235)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B235))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B235)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B235))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B235)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B235))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B236)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B236))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B236)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B236))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B236)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B236))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B236)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B236))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B237)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B237))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B237)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B237))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B237)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B237))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B237)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B237))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B238)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B238))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B238)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B238))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B238)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B238))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B238)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B238))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B239)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B239))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B239)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B239))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B239)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B239))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B239)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B239))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B240)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B240))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B240)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B240))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B240)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B240))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B240)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B240))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"},{"$f":"IF(ROWS($B$217:$B241)<=$G$217,INDEX(Roof!$P:$P,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B241))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B241)<=$G$217,INDEX(Roof!C:C,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B241))),\"\")","v":""},"",{"$f":"IF(ROWS($B$217:$B241)<=$G$217,INDEX(Roof!K:K,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B241))),\"\")","v":""},{"$f":"IF(ROWS($B$217:$B241)<=$G$217,INDEX(Roof!L:L,_xlfn.AGGREGATE(15,3,(Roof!$H$1:$H$239=1)/(Roof!$H$1:$H$239=1)*ROW(Roof!$H$1:$H$239),ROWS($B$217:$B241))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B242)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B242))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B242)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B242))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B242)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B242))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B242)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B242))),\"\")","v":""},{"$f":"COUNTIF(Garage!$H$1:$H$669,1)","v":0}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B243)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B243))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B243)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B243))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B243)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B243))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B243)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B243))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B244)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B244))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B244)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B244))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B244)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B244))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B244)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B244))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B245)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B245))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B245)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B245))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B245)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B245))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B245)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B245))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B246)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B246))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B246)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B246))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B246)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B246))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B246)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B246))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B247)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B247))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B247)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B247))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B247)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B247))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B247)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B247))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B248)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B248))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B248)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B248))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B248)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B248))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B248)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B248))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B249)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B249))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B249)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B249))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B249)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B249))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B249)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B249))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B250)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B250))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B250)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B250))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B250)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B250))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B250)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B250))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B251)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B251))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B251)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B251))),\"\")","v":""},{"$f":"IFERROR(E251-F251,\"\")","v":""},{"$f":"IF(ROWS($B$242:$B251)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B251))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B251)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B251))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B252)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B252))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B252)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B252))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B252)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B252))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B252)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B252))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B253)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B253))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B253)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B253))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B253)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B253))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B253)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B253))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B254)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B254))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B254)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B254))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B254)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B254))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B254)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B254))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B255)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B255))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B255)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B255))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B255)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B255))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B255)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B255))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B256)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B256))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B256)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B256))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B256)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B256))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B256)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B256))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B257)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B257))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B257)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B257))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B257)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B257))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B257)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B257))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B258)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B258))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B258)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B258))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B258)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B258))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B258)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B258))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B259)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B259))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B259)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B259))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B259)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B259))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B259)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B259))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B260)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B260))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B260)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B260))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B260)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B260))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B260)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B260))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B261)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B261))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B261)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B261))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B261)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B261))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B261)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B261))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B262)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B262))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B262)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B262))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B262)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B262))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B262)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B262))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B263)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B263))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B263)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B263))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B263)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B263))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B263)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B263))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B264)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B264))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B264)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B264))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B264)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B264))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B264)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B264))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B265)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B265))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B265)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B265))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B265)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B265))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B265)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B265))),\"\")","v":""}]
[{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"},{"$f":"IF(ROWS($B$242:$B266)<=$G$242,INDEX(Garage!$P:$P,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B266))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B266)<=$G$242,INDEX(Garage!C:C,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B266))),\"\")","v":""},"",{"$f":"IF(ROWS($B$242:$B266)<=$G$242,INDEX(Garage!K:K,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B266))),\"\")","v":""},{"$f":"IF(ROWS($B$242:$B266)<=$G$242,INDEX(Garage!L:L,_xlfn.AGGREGATE(15,3,(Garage!$H$1:$H$669=1)/(Garage!$H$1:$H$669=1)*ROW(Garage!$H$1:$H$669),ROWS($B$242:$B266))),\"\")","v":""}]
[{"$f":"IF(LEN(B267)>0,B267,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B267)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B267))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B267)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B267))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B267)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B267))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B267)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B267))),\"\")","v":""},{"$f":"COUNTIF('User-Defined'!$I$1:$I$504,1)","v":0}]
[{"$f":"IF(LEN(B268)>0,B268,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B268)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B268))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B268)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B268))),\"\")","v":""},{"$f":"IFERROR(E268-F268,\"\")","v":""},{"$f":"IF(ROWS($B$267:$B268)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B268))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B268)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B268))),\"\")","v":""}]
[{"$f":"IF(LEN(B269)>0,B269,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B269)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B269))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B269)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B269))),\"\")","v":""},{"$f":"IFERROR(E269-F269,\"\")","v":""},{"$f":"IF(ROWS($B$267:$B269)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B269))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B269)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B269))),\"\")","v":""}]
[{"$f":"IF(LEN(B270)>0,B270,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B270)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B270))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B270)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B270))),\"\")","v":""},{"$f":"IFERROR(E270-F270,\"\")","v":""},{"$f":"IF(ROWS($B$267:$B270)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B270))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B270)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B270))),\"\")","v":""}]
[{"$f":"IF(LEN(B271)>0,B271,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B271)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B271))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B271)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B271))),\"\")","v":""},{"$f":"IFERROR(E271-F271,\"\")","v":""},{"$f":"IF(ROWS($B$267:$B271)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B271))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B271)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B271))),\"\")","v":""}]
[{"$f":"IF(LEN(B272)>0,B272,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B272)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B272))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B272)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B272))),\"\")","v":""},{"$f":"IFERROR(E272-F272,\"\")","v":""},{"$f":"IF(ROWS($B$267:$B272)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B272))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B272)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B272))),\"\")","v":""}]
[{"$f":"IF(LEN(B273)>0,B273,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B273)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B273))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B273)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B273))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B273)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B273))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B273)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B273))),\"\")","v":""}]
[{"$f":"IF(LEN(B274)>0,B274,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B274)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B274))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B274)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B274))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B274)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B274))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B274)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B274))),\"\")","v":""}]
[{"$f":"IF(LEN(B275)>0,B275,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B275)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B275))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B275)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B275))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B275)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B275))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B275)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B275))),\"\")","v":""}]
[{"$f":"IF(LEN(B276)>0,B276,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B276)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B276))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B276)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B276))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B276)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B276))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B276)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B276))),\"\")","v":""}]
[{"$f":"IF(LEN(B277)>0,B277,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B277)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B277))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B277)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B277))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B277)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B277))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B277)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B277))),\"\")","v":""}]
[{"$f":"IF(LEN(B278)>0,B278,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B278)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B278))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B278)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B278))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B278)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B278))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B278)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B278))),\"\")","v":""}]
[{"$f":"IF(LEN(B279)>0,B279,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B279)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B279))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B279)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B279))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B279)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B279))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B279)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B279))),\"\")","v":""}]
[{"$f":"IF(LEN(B280)>0,B280,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B280)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B280))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B280)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B280))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B280)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B280))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B280)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B280))),\"\")","v":""}]
[{"$f":"IF(LEN(B281)>0,B281,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B281)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B281))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B281)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B281))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B281)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B281))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B281)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B281))),\"\")","v":""}]
[{"$f":"IF(LEN(B282)>0,B282,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B282)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B282))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B282)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B282))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B282)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B282))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B282)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B282))),\"\")","v":""}]
[{"$f":"IF(LEN(B283)>0,B283,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B283)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B283))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B283)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B283))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B283)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B283))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B283)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B283))),\"\")","v":""}]
[{"$f":"IF(LEN(B284)>0,B284,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B284)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B284))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B284)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B284))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B284)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B284))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B284)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B284))),\"\")","v":""}]
[{"$f":"IF(LEN(B285)>0,B285,VLOOKUP(\"User-Defined\",Setting!$E$6:$H$31,4,FALSE))","v":"User-Defined"},{"$f":"IF(ROWS($B$267:$B285)<=$G$267,INDEX('User-Defined'!$Q:$Q,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B285))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B285)<=$G$267,INDEX('User-Defined'!D:D,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B285))),\"\")","v":""},"",{"$f":"IF(ROWS($B$267:$B285)<=$G$267,INDEX('User-Defined'!L:L,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B285))),\"\")","v":""},{"$f":"IF(ROWS($B$267:$B285)<=$G$267,INDEX('User-Defined'!M:M,_xlfn.AGGREGATE(15,3,('User-Defined'!$I$1:$I$205=1)/('User-Defined'!$I$1:$I$205=1)*ROW('User-Defined'!$I$1:$I$205),ROWS($B$267:$B285))),\"\")","v":""}]

{"sheet":"Windows Methodology","index":33,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[]
[null,"UEC of Windows - Study"]
[null,"Builders for Climate Action"]
[null,"Window Type","ICE value","Tally value (no bioC storage)","Tally value (with bio C storage)","Bio C storage","Wood using SFP GWP factor","Notes"]
[null,"glazing only 3-pane",null,{"$f":"46.23/1.11484","v":41.467833949266257},null,null,null,"glazing is ~78% of total in a wood frame unit"]
[null,"Cladding only",null,{"$f":"54.21/1.11484","v":48.625811775680816},null,null,null,"aluminum extrusion - representative of Marvin, may be larger than other thinner units"]
[null,"Wood frame only 3-pane",null,{"$f":"D15-D10-D9","v":21.581572243550646},null,null,{"$f":"C34","v":2.0880000000000001},"This seems prety close to ICE's numbers - any chance those are for frame only?"]
[null,"Wood Double Pane",13,{"$f":"80.79/1.11484","v":72.467798069678167},{"$f":"60.48/1.11484","v":54.249937210720816},{"$f":"D12-E12","v":18.217860858957351},{"$f":"D12-D11+G11","v":52.974225826127523},"ICE seems impossibly low. Biogenic C slightly lower than wood frame  - this makes sense, small amount of unrecovered emissions balanced off by wood carbon"]
[null,"Wood Triple Pane",18,{"$f":"94.69/1.11484","v":84.935954935237334},{"$f":"74.75/1.11484","v":67.049980266226541},{"$f":"D13-E13","v":17.885974669010793},{"$f":"D13-D11+G11","v":65.442382691686689},"Bio C calculated by difference, not declared - minor discrepencies in framing btw 2 and 3 pane?"]
[null,"Wood/Metal 2-pane",43,{"$f":"110.6/1.11484","v":99.207061102938525},{"$f":"99.88/1.11484","v":89.591331491514467},{"$f":"D14-E14","v":9.615729611424058},{"$f":"D14-D11+G11","v":79.713488859387866},"Marvin's approach is extrusion replacing outer wood frame, as opposed to rolled material over wood; hence less wood bio C"]
[null,"Wood/Metal 3-pane",57,{"$f":"124.5/1.11484","v":111.67521796849772},{"$f":"114.1/1.11484","v":102.34652506189228},{"$f":"D15-E15","v":9.3286929066054398},{"$f":"D15-D11+G11","v":92.18164572494706},"Marvin's approach is extrusion replacing outer wood frame, as opposed to rolled material over wood; hence less wood bio C"]
[null,"Vinyl 2-pane",82,{"$f":"95.77/1.11484","v":85.904703814000214},"n/a",null,null,"checks out against ICE, seems about where I'd expect comp to wood only"]
[null,"Vinyl 3-pane",109,{"$f":"110/1.11484","v":98.668867281403607},"n/a",null,null,"checks out against ICE, seems about where I'd expect comp to wood only"]
[null,"Fiberglass 2-pane","n/a",{"$f":"127.4/1.11484","v":114.27648810591654},"n/a",null,null,"Seems about where I'd expect compared to vinyl"]
[null,"Fiberglass 3-pane","n/a",{"$f":"141.6/1.11484","v":127.01374188224318},"n/a",null,null,"Seems about where I'd expect compared to vinyl"]
[]
[null,"Anderson Fibrex",null,69.099999999999994,"kg/m2"]
[null,"EUROPEAN FIBERGLASS - CLF FORUM"]
[]
[null,"All UEC values kgCO2e A1-A3 per sq m"]
[null,"All windows 3' w x 4' h = 1.11484 m2"]
[null,"Marvin Essential modeled for fiberglass and vinyl frames"]
[null,"Marvin Ultimate modeled for wood and wood with aluminum clad frames"]
[]
[null,"Reverse CO2e calc from our numbers:"]
[null,"SPF framing kg CO2e/m3",72,null,"from NA softwood LCA"]
[null,"3-pane wood weight",11.6,"kg","from Tally"]
[null,"ave softwood density",400,"kg/m3","from Engineering Toolbox"]
[null,"calculated approx volume",{"$f":"C31/C32","v":2.8999999999999998E-2},"m3"]
[null,"approximate UEC",{"$f":"C30*C33","v":2.0880000000000001},"kg CO2e","from NA softwood LCA"]
[null,"Tally UEC",{"$f":"D11","v":21.581572243550646},"kg CO2e","from GaBi LCI: DE: Wooden frame (EN15804 A1-A3) ts (2017)"]
[]
[null,"Window dimensions:"]
[null,"length",4.26,"m","from Tally"]
[null,"area:",7.54,"in2","gross area per frame (2 sides)"]
[null,null,4.7999999999999996E-3,"m2","metric conversion"]
[null,null,{"$f":"C38*(C40*2*0.75)","v":3.0671999999999998E-2},"m3","roughly equates to calculated volume above"]
[]
[]
[null,"© His Majesty the king in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Dropdown Lists","index":34,"n_rows":155,"n_cols":30,"rows_kept":155,"cut":false,"hidden":true,"merged":[]}
["Thickness","Spacing","Steel Joist Spacing","Roof insulation parallel to…","User-defined options: VOLUME – m3","User-defined options: SURFACE AREA – m2","User-defined options: Length - m","User-defined options: R-Value & Area - m2-RSI",null,"Y/N?","List of Assembly/Component Sheets"]
["in",16,24,"Roof surface",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(4,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate /  /  / Avg construction aggregate (gravel & sand)"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(1,'Master sheet'!$AL$1:$AL$441,0))","v":"ACQ wood treatment /  /  / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(176,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Concrete Reinforcing Steel Institute /  / 10M"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(3,'Master sheet'!$AL$1:$AL$441,0))","v":"Aerogel blanket / Aspen Aerogels /  / R9.6/inch, White/Grey blanket"},null,"Yes",{"$f":"VLOOKUP(\"Footings & Slabs\",Setting!$E$6:$H$31,4,FALSE)","v":"Footings & Slabs"}]
["mm",24,36,"Ceiling surface",{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(5,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Kangley Rock & Recycling /  / Avg construction aggregate (gravel & sand)"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(2,'Master sheet'!$AL$1:$AL$441,0))","v":"Adobe block /  / 8\" block wall / Avg of site made and factory made (Cyprus)"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(177,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Concrete Reinforcing Steel Institute /  / 15M"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(32,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - batt / CMS / R 3.6/inch / EcoCell"},null,"No",{"$f":"VLOOKUP(\"Foundation Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Foundation Walls"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(6,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Martin Marietta /  / Avg construction aggregate (gravel & sand)"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(9,'Master sheet'!$AL$1:$AL$441,0))","v":"Air barrier / Dupont / Tyvek Fluid Applied Weather Barrier System - All components / 25 Perms"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(120,'Master sheet'!$AL$1:$AL$441,0))","v":"Helical pier / Generic /  / 3\" Nominal Pipe, 3.5 x 3/16\" (89 x 5.5 mm), 10\" Helix, Sched 40 STD Galvanized steel"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(33,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - dense pack /  / R 3.7/inch / Includes AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},null,null,{"$f":"VLOOKUP(\"Structural Elements\",Setting!$E$6:$H$31,4,FALSE)","v":"Structural Elements"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(7,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Polaris Mtls Corp. /  / Avg construction aggregate (gravel & sand)"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(10,'Master sheet'!$AL$1:$AL$441,0))","v":"Air barrier / Dupont / Tyvek HomeWrap / 54 Perms"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(189,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel beam / W150x22 (W6x15) / American Institute of Steel Construction"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(34,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - loose fill /  / R 3.7/inch / Includes: AFT, Applegate, Can-Cell, Cell-Pak, Cleanfiber, Climatizer, Fiberlite, Igloo, ICC, Mason City, Nu-Wool, Soprema, Thermo-Kool"},null,null,{"$f":"VLOOKUP(\"Ext. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Walls"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(8,'Master sheet'!$AL$1:$AL$441,0))","v":"Aggregate / Vulcan Mtls Co. /  / Avg construction aggregate (gravel & sand)"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(11,'Master sheet'!$AL$1:$AL$441,0))","v":"Air barrier / GCP / Perm-a-Barrier VPL liquid applied permeable barrier / 15 Perms, 40 mils thickness"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(190,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel beam / W200x22 (W8x15) / American Institute of Steel Construction"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(35,'Master sheet'!$AL$1:$AL$441,0))","v":"Cellulose - spray applied / R 3.75/inch / International Cellulose Corp. / K-13, ThermoCon"},null,null,{"$f":"VLOOKUP(\"Ext. Wall Systems\",Setting!$E$6:$H$31,4,FALSE)","v":"Ext. Wall Systems"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(24,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / Brick Industry Association / US-Canada Industrywide Average / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(12,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Includes: Atlas, BP, CertainTeed, GAF, IKO, Malarkey, Owens Corning, Pabco /  / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(191,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel beam / W200x27 (W8x18) / American Institute of Steel Construction"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(80,'Master sheet'!$AL$1:$AL$441,0))","v":"Cork board insulation / Amorim / Isolamentos / R4/inch"},null,null,{"$f":"VLOOKUP(\"Party Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Party Walls"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(56,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete / Butler Concrete / Avg of 19 different 25 Mpa mixes / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(13,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / GAF / Timberline / Timberline"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(192,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel beam / W200x31 (W8x21) / American Institute of Steel Construction"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(93,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board / EPS Industry Alliance /  / R 4.6/inch, Type IX, 25 psi (Type 3, 140 kPa)"},null,null,{"$f":"VLOOKUP(\"Cladding\",Setting!$E$6:$H$31,4,FALSE)","v":"Cladding"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(57,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 0-25 MPa, Industry Average Benchmark / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(14,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Owens Corning / Duration / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(193,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel beam / W250x25 (W10x17) / American Institute of Steel Construction"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(94,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board / EPS Industry Alliance /  / R 4/inch, Type II, 15 psi (Type 2, 110 kPa)"},null,null,{"$f":"VLOOKUP(\"Windows\",Setting!$E$6:$H$31,4,FALSE)","v":"Windows"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(58,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 0-25 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(15,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Owens Corning / Oakridge / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(194,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel beam / W250x33 (W10x22) / American Institute of Steel Construction"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(95,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board with graphite / BASF / Neopor / R 4.7/inch, Type IX"},null,null,{"$f":"VLOOKUP(\"Int. Walls\",Setting!$E$6:$H$31,4,FALSE)","v":"Int. Walls"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(59,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 0-25 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(16,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / Owens Corning / Supreme / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(195,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel beam / W250x39 (W10x26) / American Institute of Steel Construction"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(96,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS foam board with graphite / BASF / Neopor / R 4.7/inch, Type II, 15 psi (Type 2, 110 kPa)"},null,null,{"$f":"VLOOKUP(\"Floors\",Setting!$E$6:$H$31,4,FALSE)","v":"Floors"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(60,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 0-25 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(17,'Master sheet'!$AL$1:$AL$441,0))","v":"Bamboo plywood / Smith & Fong / Plyboo / 1/2\" (12.7 mm)"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(196,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel beam / W310x33 (W12x22) / American Institute of Steel Construction"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(102,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / CertainTeed / Sustainable Insulation / R 3.6/inch"},null,null,{"$f":"VLOOKUP(\"Ceilings\",Setting!$E$6:$H$31,4,FALSE)","v":"Ceilings"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(61,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 0-25 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(18,'Master sheet'!$AL$1:$AL$441,0))","v":"BioBased Tile / Armstrong / BioBased Tile / Non-PVC with BioStride polyester binder, Striations BBT and Migrations BBT"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(197,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel beam / W310x39 (W12x26) / American Institute of Steel Construction"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(103,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Knauf / EcoBatt / R 3.6/inch"},null,null,{"$f":"VLOOKUP(\"Roof\",Setting!$E$6:$H$31,4,FALSE)","v":"Roof"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(62,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 0-25 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(19,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Calcium Silicate / Arriscraft / Contemporary Brick / 3-1/8\" x 3-1/2\" x any length, incl. mortar and ties"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(198,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel joist, open web / Steel Joist Institute /  / 12\" 12K3 joist"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(104,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass batt / Owens Corning / EcoTouch Pink batt and roll / R 3.6/inch"},null,null,{"$f":"VLOOKUP(\"Garage\",Setting!$E$6:$H$31,4,FALSE)","v":"Garage"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(63,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 26-30 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(20,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Cement / MidWest / Architectural Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(199,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel post / Generic /  / 3.5 x 0.216\" (89 x 5.5 mm), Sched 40 STD"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(105,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / CertainTeed / InsulSafe, Optima, TruComfort / R 2.6/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(64,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 26-30 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(21,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / Interstate / Avg Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(200,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing  / ClarkDietrich /  / 600-S-137-54, 16 gauge"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(106,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Knauf / Jet Stream ULTRA / R 2.2/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(65,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 26-30 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(22,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / Interstate / Avg Thin Face Brick / 3-9/16\" x 5/8\" x 11-5/8\" (90 x 16 mm x 295) incl. 3/8\" mortar"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(201,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / MarinoWARE / Structural stud and track / 600-S-137-54, 16 gauge, \"2x6\""},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(107,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Owens Corning / AttiCat, ProCat, ProPink / R 2.8/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(66,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 26-30 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(23,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay, Generic Modular / Brick Industry Association / US-Canada Industry Average / 3-5/8\" x 2-3/4\" x 7-5/8\" incl. 3/8\" mortar"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(202,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / MBA Building Supplies /  / 600-S-137-54, 16 gauge"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(108,'Master sheet'!$AL$1:$AL$441,0))","v":"Foam glass aggregate / Glasopor AS /  / R 1.7/inch, 10-60 mm"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(67,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 26-30 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(25,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet /  /  / Average from 150 samples in the EC3 database"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(203,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / Scafco /  / 600-S-137-54, 16 gauge"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(109,'Master sheet'!$AL$1:$AL$441,0))","v":"Foam glass aggregate / Hasopor /  / R 1.7/inch, 10-60 mm"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(68,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 26-30 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(26,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet /  / Achievable from EC3 / Achievable from 150 samples in the EC3 database"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(204,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Load bearing / Steel Recycling Institute /  / 600-S-137-54, 16 gauge"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(110,'Master sheet'!$AL$1:$AL$441,0))","v":"Foam glass aggregate / Misapor / Glavel / R 1.7/inch, 10-60 mm"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(69,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 31-35 MPa, Canadian Benchmark Average / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(27,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet /  / Conservative from EC3 / Conservative from 150 samples in the EC3 database"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(205,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / ClarkDietrich /  / 362-S-125-18, 20EQ gauge, \"2x4\""},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(111,'Master sheet'!$AL$1:$AL$441,0))","v":"Foam glass board / Pittsburgh Corning Europe / Foamglas T4 / R3.7/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(70,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 31-35 MPa, 0-14% FA/SL, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(28,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet / Interface / GLASBAC®RE, Nylon / Modular tile carpet (closed loop recycling)"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(206,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / MarinoWARE / Viper Stud Viper 20 / 362-S-125-18, 20EQ gauge, \"2x4\""},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(112,'Master sheet'!$AL$1:$AL$441,0))","v":"Foam glass board / Pittsburgh Corning Europe / Foamglas W+F, Foamglas T3 / R4/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(71,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 31-35 MPa, 15-29% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(29,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet / Interface / Cquest BioX / 1.5 mm Modular tile carpet"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(207,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / MBA Building Supplies /  / 362-S-125-18, 20EQ gauge, ProSTUD, ProTRAK"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(121,'Master sheet'!$AL$1:$AL$441,0))","v":"Hemp fiber batt / NaturFibre / Hemp Wool / R 3.7/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(72,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 31-35 MPa, 30-40% Fly Ash, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(30,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Shingles/shakes /  /  / 3/4\" coverage"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(208,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / Scafco /  / 362VS125-18, 20EQ gauge"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(122,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / IsoHemp / Europe / R 2.1/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(73,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 31-35 MPa, 25-34% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(31,'Master sheet'!$AL$1:$AL$441,0))","v":"Cedar Siding / Western Red Cedar Lumber Assn /  / 1 x 6 Boards"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(209,'Master sheet'!$AL$1:$AL$441,0))","v":"Steel studs - Non-loadbearing / Steel Recycling Institute /  / 362-S-125-18, 20EQ gauge"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(123,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / Europe / R 2.1/inch, Avg. of 9 mixes"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(74,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 31-35 MPa, 35-50% Slag, GU / CRMCA / Can. Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(36,'Master sheet'!$AL$1:$AL$441,0))","v":"Cement board 1/2\" / USG / Durock (132) / 1/2\" (12.7 mm)"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(249,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / American Wood Council & Canadian Wood Council /  / TJI 230/360"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(124,'Master sheet'!$AL$1:$AL$441,0))","v":"Hempcrete / Site mixed / USA / R 2.1/inch, Avg. mix using NHL & PHL"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(75,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 20 MPa, Standard mix / NRMCA / US Avg / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(37,'Master sheet'!$AL$1:$AL$441,0))","v":"Cement board 1/2\" / USG / Durock (133) / 1/2\" (12.7 mm)"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(250,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood I joist / Roseburg / RFPI Joist / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(147,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Owens Corning / Thermafiber UltraBatt / R 4.3/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(76,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 20 MPa, 20-30% Fly Ash / NRMCA / US Avg / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(38,'Master sheet'!$AL$1:$AL$441,0))","v":"Cement mortar, tile / Tile Council of North America /  / Industry average. Includes dry-set, modified dry-set and improved modified dry-set cement mortar"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(251,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood floor truss - prefabricated / Quebec Wood Export Bureau / Common (Warren, 45 deg) web pattern / Top chord bearing, variable depth"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(148,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / Safe'n'Sound, ComfortBatt / R 3.8/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(77,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 20 MPa, 30-40% FA/SL / NRMCA / US Avg / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(39,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Crossville / Porcelain / Standard grade"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(252,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood roof truss - prefabricated / Quebec Wood Export Bureau / Common (Double Howe) Gabrel Roof / 2x6 Chords, 2x4 Webs, 4:12 Pitch, 40 ft span, 20\" overhang"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(149,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board - heavy density / NAIMA / R 4.2/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(78,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 20 MPa, 40-50% FA/SL mix / NRMCA / US Avg / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(40,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / StonePeak / Porcelain / Porcelain, standard grade"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(390,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Nucor Corporation / Canadian sizes / 10M"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(150,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board / Rockwool / Rockboard 60 / R 4.3/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(79,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 20 MPa, >50% SCM mix / NRMCA / US Avg / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(41,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Tile Council of North America /  / Industry average. Includes porcelain, pressed, mosaic and quarry tile"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(391,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Nucor Corporation / Canadian sizes / 15M"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(151,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board - light density / NAIMA / R 3.7/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(113,'Master sheet'!$AL$1:$AL$441,0))","v":"Glued laminated timber / American Wood Council & Canadian Wood Council /  / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(42,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay plaster / Site mixed /  / 15 mm"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(392,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / Nucor Corporation / Canadian sizes / 20M"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(152,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool loose fill / NAIMA / R 3/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(114,'Master sheet'!$AL$1:$AL$441,0))","v":"Glued laminated timber / Structurlam / Glulam Plus / 3-1/2\" (90mm) thick"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(43,'Master sheet'!$AL$1:$AL$441,0))","v":"Clay roof tiles / HISPALYT /  / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(393,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 10M"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(162,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - roof boards / Carlisle / GRF cellulosic facer / R 5.8/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(126,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminated strand lumber (LSL) / American Wood Council & Canadian Wood Council /  / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(44,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Angelus Block Co. / 8\" Light weight blocks / 9 x 8 x 16 Precision"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(394,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 15M"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(163,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - roof boards / Hunter / Polysio Roof insulation boards / R 5.8/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(127,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminated veneer lumber (LVL) / American Wood Council & Canadian Wood Council /  / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(45,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Brampton Brick / 8\" Carbon Cure Lightweight blocks / Carbon Cure 15 MPa"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(395,'Master sheet'!$AL$1:$AL$441,0))","v":"Rebar / ArcelorMittal Long Products Canada / Canadian sizes / 20M"},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(164,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - roof boards / PIMA / Includes: Atlas, Firestone, GAF, Johns Manville, Rmax / R 5.8/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(128,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminated veneer lumber (LVL) / RedBuilt / RedLam / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(46,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Light weight / Canadian Concrete Masonry Producers Assn / 8\" Light weight blocks / 390 x 190 x 190 mm"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(165,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - roof boards / Versico / VersiCore, SecurShield, DuraFaceR / R 5.8/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(137,'Master sheet'!$AL$1:$AL$441,0))","v":"Masonry Mortar Mix / 1 part Masonry cement / 3 parts avg sand / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(47,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Angelus Block Co. / 8\" Normal weight blocks / 8 x 8 x 16 Precision"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(166,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / Dow Chemical Company / Tuff-R, Super Tuff-R, Thermax / R 6.5/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(246,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing - Softwood / Roseburg /  / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(48,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Canadian Concrete Masonry Producers Assn / 8\" Normal weight blocks / 390 x 190 x 190 mm"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(167,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / Hunter / Polysio Wall insulation boards / R 6.5/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(248,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood framing & siding - SPF / American Wood Council & Canadian Wood Council /  / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(49,'Master sheet'!$AL$1:$AL$441,0))","v":"CMU - Normal weight / Permacon / 8\" Normal weight blocks / NW STD 20CM GLPW"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(168,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / PIMA / Includes: Atlas, Firestone, GAF, Johns Manville, Rmax / R 6.5/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(270,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, Quebec Baseline Average / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(52,'Master sheet'!$AL$1:$AL$441,0))","v":"Earthen Floor / Site made /  / 3\" cob, 1\" clay plaster"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(183,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFC) / SPFA /  / R 6.6/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(271,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 10% SL, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(55,'Master sheet'!$AL$1:$AL$441,0))","v":"Compressed straw board / Stramit / 60 mm board / R 3.9/inch"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(184,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell - HFO gas filled / SPFA /  / R 6.6/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(272,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 10% FA, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(81,'Master sheet'!$AL$1:$AL$441,0))","v":"Cork flooring / Amorim / Revestimentos S.A. / Cork floating floor planks"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(185,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - High Density (HFC) / SPFA /  / R 6.3/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(273,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 20% SL, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(82,'Master sheet'!$AL$1:$AL$441,0))","v":"Cork flooring / European Resilient Flooring Manufacturers' Institute / Includes: Altro, Amorim, Amtico, Artigo, Aspecta, BeauFlor, Dickson, Mflor, Forbo, Gerflor, IVC, Nora, Polyflor, Tarkett, Kahrs, Windmoller / Cork floor tiles"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(186,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - High Density - HFO gas filled / SPFA /  / R 6.5/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(274,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 20% FA, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(83,'Master sheet'!$AL$1:$AL$441,0))","v":"Cross Laminated Timber / Nordic / X-Lam / 3-1/2\" (90mm) thick"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(187,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell (HFC) / SPFA /  / R 4.1/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(275,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 30% SL, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(84,'Master sheet'!$AL$1:$AL$441,0))","v":"Cross Laminated Timber / Structurlam / CrossLam / 3-1/2\" (90mm) thick"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(188,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Open Cell - HFO gas / SPFA /  / R 4.1/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(276,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 30% FA, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(85,'Master sheet'!$AL$1:$AL$441,0))","v":"Dowel Laminated Timber / StructureCraft / DowelLam / 3-1/2\" (90mm) thick"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(210,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale /  / Wheat & rye straw / R 3.3/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(277,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, Quebec Baseline Average / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(86,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / AirRenew / 1/2\" (12.7 mm)"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(211,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Panels / EcoCocon /  / R 2.9/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(278,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 10% SL, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(87,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / Easi-Lite / 1/2\" (12.7 mm)"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(214,'Master sheet'!$AL$1:$AL$441,0))","v":"Vacuum Insulated Panel / Porextherm / Vacupor / R 30/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(279,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 10% FA, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(88,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / CertainTeed / M2Tech moisture resistant / 1/2\" (12.7 mm)"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(238,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber - loose fill / GUTEX / ThermoFiber / R 3.6/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(280,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 20% SL, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(89,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / Pabco / QuietRock / QuietRock 1/2\""},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(239,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / GUTEX / ThermoFlex / R 4/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(281,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 20% FA, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(90,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 5/8\""},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(240,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Pavatex / Pavaflex / R 3.8/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(282,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 30% SL, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(91,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" / USG / EcoSmart Firecode / 5/8\""},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(241,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber batt / Steico / SteicoFlex / R 3.8/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(283,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 30% FA, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(92,'Master sheet'!$AL$1:$AL$441,0))","v":"EPDM Roofing Membrane / SPRI /  / "},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(242,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) Wood fiber board / AWC/CWC / Includes: Georgia Pacific, Louisville, BPC, Temple-Inland, Blue Ridge, Int'l Bildrite / R 2.7/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(284,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, Quebec Baseline Average / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(97,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement roofing / Cembrit / Corrugated sheets / 6.5 mm"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(243,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / GUTEX / Multi-Therm / R 3.6/inch, 40, 60, 80, 100, 120, 140, 160, 180, 200 mm"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(285,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 10% SL, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(98,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement roofing / Cembrit / Slates / 4 mm"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(244,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Pavatex / Pavatherm / R 3.4/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(286,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 10% FA, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(99,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement roofing / Mahaphant / Fibre-Cement / 5 mm"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(245,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / Steico / Special Dry / R 3.6/inch, 40, 120, 140, 160, 180, 200 mm"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(287,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 20% SL, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(100,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Cembrit / Patina / "},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(254,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool batt / Havelock Wool /  / R 3.6/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(288,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 20% FA, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(101,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Cembrit / Solid & Express / "},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(255,'Master sheet'!$AL$1:$AL$441,0))","v":"Wool loose fill / Havelock Wool /  / R 4.4/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(289,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 30% SL, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(115,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat /  / Includes American Gypsum, CertainTeed, Continental, Georgia-Pacific, National Gypsum, Pabco, USG, CGC / 1/2\""},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(258,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Owens Corning / Foamular NGX 250  / R 5/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(290,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 30% FA, GU / ABQ / Can. Quebec Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(116,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / USG / Securock ExoAir 430 / 1/2\""},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(374,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiberglass loose fill / Johns Manville / Climate Pro, Attic Protector, JM Spider PLUS (Canada) / R 2.8/inch, Formaldehyde-free"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(291,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(117,'Master sheet'!$AL$1:$AL$441,0))","v":"Hardwood flooring / Action Floor Systems /  / 25/32\" x 3-1/4\" FSC certified"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(397,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood fiber board / North American Fiberboard Association / Includes: MSL, Blue Ridge Fiberboard Inc. / R 2.7/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(292,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 15% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(118,'Master sheet'!$AL$1:$AL$441,0))","v":"Hardwood flooring / mafi / Natural Hardwood Planks / 3/4\", 3 ply laminated solid, oil pre-finished"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(399,'Master sheet'!$AL$1:$AL$441,0))","v":"(ARCHIVED 2023) XPS foam board / DuPont / Styrofoam (Grey, Reduced GWP) / R 5.6/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(293,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 25% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(119,'Master sheet'!$AL$1:$AL$441,0))","v":"Hardwood flooring / Typical Eastern Canadian, solid, pre-finished /  / 3-12\" x 3/4\" prefinished"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(400,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / DuPont / Reduced GWP Grey Styrofoam™ (same as ST-100) / R 5.0/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(294,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 35% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(125,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminate flooring / Novalis / LVT / "},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(401,'Master sheet'!$AL$1:$AL$441,0))","v":"XPS foam board / Soprema / SOPRA-XPS / R 5.0/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(295,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 50% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(131,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Armstrong / Sheet style / 2.5 mm sheet style linoleum"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(402,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R14 / R 4.0/inch, 3.5\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(296,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(132,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Forbo / Marmoleum / 2.5 mm sheet style linoleum"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(403,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R15 / R 4.3/inch, 3.5\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(297,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 15% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(133,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Forbo / Marmoleum Striato / 2.5 mm sheet style linoleum"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(404,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R22 / R 4.0/inch, 5.5\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(298,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 25% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(134,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Gerflor  / DLW Linoleum Acousticplus / 4.0 mm sheet style linoleum"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(405,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 / R 4.4/inch, 5.5\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(299,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 35% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(135,'Master sheet'!$AL$1:$AL$441,0))","v":"Liquid linoleum flooring / Duracryl Corques / Liquid Lino / 2.0 mm liquid applied"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(406,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool batt / Rockwool / ComfortBatt R24 SS / R 4.0/inch, 6\" Steel Studs"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(300,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 50% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(138,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Aluminum / Metal Construction Assn. / 22 gauge / Includes: ATAS, DMI, Englert, Fabral,McElroy, Pac-Clad"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(407,'Master sheet'!$AL$1:$AL$441,0))","v":"Mineral wool board  / Rockwool / Comfortboard 80 / R 4.2/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(301,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(139,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Aluminum / Petersen Aluminum Corp / Pac-Clad / 20EQ gauge"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(408,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / DuPont / Thermax / R 6.5/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(302,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 15% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(140,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / AEP Span / All products / 24 gauge"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(410,'Master sheet'!$AL$1:$AL$441,0))","v":"Spray polyurethane foam - Closed Cell (HFO) / Huntsman Building Solutions / Heatlok HFO & Heatlok Soya HFO / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(303,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 25% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(141,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / ArcelorMittal / All products / 24 gauge"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(411,'Master sheet'!$AL$1:$AL$441,0))","v":"Polyiso - wall boards / PIMA / Includes: Atlas, Firestone, GAF, Johns Manville, Rmax, Carlisle, Iko, Soprema / R 6.5/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(304,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 35% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(142,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Canadian Sheet Steel Building Institute / 24 gauge"},null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(412,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Bale / SNaB (UK) / Wheat & barley straw / R 2.8/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(305,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 50% SL, GU / RMCAO / Can. Ontario Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(143,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Metal Building Manufacturers Assn / 24 gauge"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(306,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(144,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Metal Construction Assn. / 24 gauge"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(307,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 10% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(145,'Master sheet'!$AL$1:$AL$441,0))","v":"Metal Panels - Steel / Petersen Aluminum Corp / PAC-CLAD / 24 gauge"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(308,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 20% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(146,'Master sheet'!$AL$1:$AL$441,0))","v":"MgO board 1/2\" / North American MgO / MagTech Ultra / 1/2\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(309,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 30% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(154,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 1/2\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(310,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 40% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(155,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / American Wood Council & Canadian Wood Council /  / 5/8\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(311,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(156,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / Huber  / AdvanTech / 1/2\" Sheathing"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(312,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 10% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(157,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB sheathing / Huber  / ZIP System / 7/16\" Sheathing, protective barrier and tape"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(313,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 20% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(158,'Master sheet'!$AL$1:$AL$441,0))","v":"OSB subflooring / Huber  / AdvanTech / 19/32\" Subflooring"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(314,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 30% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(159,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 1/2\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(315,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 40% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(160,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 5/8\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(316,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(161,'Master sheet'!$AL$1:$AL$441,0))","v":"Plywood / American Wood Council & Canadian Wood Council /  / 3/4\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(317,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 10% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(169,'Master sheet'!$AL$1:$AL$441,0))","v":"Polypropylene siding / Novik / NovikStone, NovikShake / Avg of 5 products"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(318,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 20% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(170,'Master sheet'!$AL$1:$AL$441,0))","v":"Polypropylene siding / Vinyl Siding Institute  /  / 0.085\" Single 7\" wood Shake appearance"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(319,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 30% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(171,'Master sheet'!$AL$1:$AL$441,0))","v":"Polypropylene ICF webbing /  /  / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(320,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 40% FA, GU / SRMCA / Can. Sask Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(172,'Master sheet'!$AL$1:$AL$441,0))","v":"PVC Roofing Membrane / CIFA / Includes: Canadian General-Tower, Duro-Last, FiberTite / 48 mils"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(321,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(178,'Master sheet'!$AL$1:$AL$441,0))","v":"Rubber flooring / ECOsurfaces / ECOsurfaces / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(322,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 10% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(179,'Master sheet'!$AL$1:$AL$441,0))","v":"Rubber flooring / Resilient Floor Covering Institute / Includes tiles and rolls from American Biltrite, Armstrong, Burke, FLEXCO, Johnsonite, Mannington, Roppe, Tarkett / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(323,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 20% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(180,'Master sheet'!$AL$1:$AL$441,0))","v":"SBS Modified Bitumen Roofing / ARMA / Includes: CertainTeed, Firestone, GAF, Henry, IKO, Johns Mansville, Malarkey, Siplast, Soprema / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(324,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 30% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(181,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP panel - EPS foam core /  /  / 7/16\" OSB, Type II EPS"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(325,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 40% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(182,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP panel - Straw core / Agriboard / Agriboard 7-7/8\" / R?/inch"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(326,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(212,'Master sheet'!$AL$1:$AL$441,0))","v":"Acrylic Stucco Textured Finish / Sto / Stolit 1.0, Stolit 1.5, Stolit Freeform / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(327,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 10% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(213,'Master sheet'!$AL$1:$AL$441,0))","v":"TPO Roofing Membrane / Carlisle /  / 60 mils"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(328,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 20% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(215,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Altro / Altro Lavencia Click / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(329,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 30% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(216,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Altro / Altro Lavencia Plus / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(330,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 40% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(217,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Gerflor / Creation 70 CLIC / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(331,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(218,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Resilient Floor Covering Institute / Includes tile products from Armstrong, Congoleum, Tarkett / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(332,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 10% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(219,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl Siding / Vinyl Siding Institute / Double 4.5\" products from: American Original, Associated Materials, CertainTeed, Novik, Ply Gem / 0.040\" Double 4.5\""}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(333,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 20% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(220,'Master sheet'!$AL$1:$AL$441,0))","v":"Waterproofing membrane adhesive / GCP / Bituthene / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(334,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 30% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(221,'Master sheet'!$AL$1:$AL$441,0))","v":"Welded wire mesh / Serfas /  / 6\" x 6\" x 6/6g / Norway"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(335,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 40% FA, GU / MRMCA / Can. Manitoba Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(222,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Fiberglass frame /  / USA & CAN"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(336,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(223,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Andersen / Fibrex / PVC & Wood composite / USA"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(337,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 15% SCM, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(224,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Vinyl frame /  / USA & CAN"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(338,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 25% SCM, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(225,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame /  / EU"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(339,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 40% SCM, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(226,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame /  / USA & CAN"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(340,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(227,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame, aluminum cladding /  / EU"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(341,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 15% SCM, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(228,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Wood frame, aluminum cladding /  / USA & CAN"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(342,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 25% SCM, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(229,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Fiberglass frame /  / USA & CAN"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(343,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 40% SCM, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(230,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Vinyl frame /  / USA & CAN"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(344,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(231,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Wood frame /  / EU"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(345,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 15% SCM, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(232,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Wood frame /  / USA & CAN"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(346,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 25% SCM, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(233,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Wood frame, aluminum cladding /  / EU"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(347,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 40% SCM, GU / BCRMCA / Can. BC Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(234,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - triple pane / Wood frame, aluminum cladding /  / USA & CAN"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(348,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(235,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood chip cement ICF / Isospan / Okopur / NEEDS REVIEW"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(349,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 10% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(236,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood chip cement ICF / Nexcem, Faswall /  / 12\" R22 block"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(350,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 20% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(237,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood chip cement ICF / Nexcem, Faswall /  / 14\" R28 block"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(351,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 30% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(253,'Master sheet'!$AL$1:$AL$441,0))","v":"Wood wool boards / Armstrong / Tectum / 2\" (50.8 mm)"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(352,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 40% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(259,'Master sheet'!$AL$1:$AL$441,0))","v":"EPS FOAM ICF R-23, 2 Sheets of 2.75\" @ R4/in., 15M rebar (6\" CONCRETE CORE must be added separately)"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(353,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(260,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R23 6.5\" - EPS 5.5\" @ R4/in. core, 2 sheets 1/2\" OSB"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(354,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 10% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(261,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R30 8.25\" - EPS 7.25\" @ R4/in. core, 2 sheets 1/2\" OSB"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(355,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 20% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(262,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R38 10.5\" - EPS 9.5\" @ R4/in. core, 2 sheets 1/2\" OSB"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(356,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 30% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(263,'Master sheet'!$AL$1:$AL$441,0))","v":"SIP PANEL - R48 12-7/8\" - EPS 11.875\" @ R4/in. core, 2 sheets 1/2\" OSB"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(357,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 40% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(264,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 12\" R-22 with MINERAL WOOL INSERTS, (3 in. @ R4.2/in.), 15M REBAR"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(358,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(265,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 14\" R-28 with MINERAL WOOL INSERTS (5 in. @ R4.2/in.), 15M REBAR"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(359,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 10% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(266,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 12\" R-21 with CORK BOARD INSERTS (3 in. @ R4/in.), 15M REBAR"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(360,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 20% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(267,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD CHIP CEMENT ICF 14\" R-27 with CORK BOARD INSERTS (5 in. @ R4/in.), 15M REBAR"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(361,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 30% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(268,'Master sheet'!$AL$1:$AL$441,0))","v":"TREATED WOOD FOUNDATION - 2x8 framing @ 16\" OC, 3/4\" plywood sheathing"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(362,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 40% FA, GU / ACA / Can. Atlantic Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(269,'Master sheet'!$AL$1:$AL$441,0))","v":"WOOD FRAME with STRAW BALE INFILL - 14\" R-46, Double 2x4 @ 30\" o/c"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(363,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, GU / ARMCA / Can. Alberta Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(372,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Shaw - Patcraft / Luxury Vinyl Tile / 2 - 5 mm "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(364,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 10% FA, GU / ARMCA / Can. Alberta Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(373,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Gerflor  / DLW Linoleum Compact / 2.5 mm sheet style linoleum"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(365,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 25 MPa, 20% FA, GU / ARMCA / Can. Alberta Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(375,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Andersen / E-series (Average Double-hung/Awning/Picture) / Wood frame, aluminum cladding"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(366,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, GU / ARMCA / Can. Alberta Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(376,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 1/2\" / National Gypsum / Gold Bond XP Gypsum Board  / 1/2\" (12.7 mm)"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(367,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 10% FA, GU / ARMCA / Can. Alberta Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(377,'Master sheet'!$AL$1:$AL$441,0))","v":"Drywall 5/8\" Type X / National Gypsum / Gold Bond XP Fire-Shield Gypsum Board  / 5/8'' type X"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(368,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 30 MPa, 20% FA, GU / ARMCA / Can. Alberta Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(378,'Master sheet'!$AL$1:$AL$441,0))","v":"Carpet / J+J Flooring / Standard Back / all Broadloom styles"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(369,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, GU / ARMCA / Can. Alberta Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(379,'Master sheet'!$AL$1:$AL$441,0))","v":"Vinyl flooring / Mannington / Luxury Vinyl Tile / 2.5 mm Tile and Plank"}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(370,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 10% FA, GU / ARMCA / Can. Alberta Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(380,'Master sheet'!$AL$1:$AL$441,0))","v":"Asphalt Shingles / GAF / Timberline Cool Series / "}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(371,'Master sheet'!$AL$1:$AL$441,0))","v":"Concrete - 35 MPa, 20% FA, GU / ARMCA / Can. Alberta Avg. / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(381,'Master sheet'!$AL$1:$AL$441,0))","v":"Linoleum flooring / Mannington / Legato Flooring / liquid applied"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"T141*Y141*Z141","v":0}]
[null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(409,'Master sheet'!$AL$1:$AL$441,0))","v":"Laminated veneer lumber / Roseburg Forest Products / RigidLam LVL / "},{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(382,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / Fireclay Tile / Ceramic - recycled content / Standard and Second grade"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(383,'Master sheet'!$AL$1:$AL$441,0))","v":"Ceramic tile / American Wonder Porcelain / Procelain - recycled content / Standard and Second grade"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(384,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Equitone / Pictura and Natura Pro / 8 mm (5/16\")"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(385,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Equitone / Tectiva / 8 mm (5/16\")"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(386,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / Equitone / Natura, Textura and Materia / 8 mm (5/16\")"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(387,'Master sheet'!$AL$1:$AL$441,0))","v":"Straw Panels / Ecocoon / Standard and Brace Panels / 40cm R16, panel only"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(388,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / SHAW / Slender - Thin Face Brick / 2 1/4\" x 1/2\" x 7-1/2\" (57 x 12.7 mm x 190) incl. 3/8\" mortar"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(389,'Master sheet'!$AL$1:$AL$441,0))","v":"Brick, Clay / SHAW / Avg Face Brick / 3-5/8\" x 2-3/4\" x 7-5/8\" (92 x 70 x 194 mm) incl. 3/8\" mortar"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(413,'Master sheet'!$AL$1:$AL$441,0))","v":"Engineered Wood Siding & Trim / LP / SmartSide / 0.315\" (8 mm)"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(414,'Master sheet'!$AL$1:$AL$441,0))","v":"Engineered Wood Siding & Trim / LP / SmartSide / 0.375\" (9.5 mm)"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(415,'Master sheet'!$AL$1:$AL$441,0))","v":"Engineered Wood Siding & Trim / LP / SmartSide / 0.530\" (13.5 mm)"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(416,'Master sheet'!$AL$1:$AL$441,0))","v":"Window - double pane / Inline Fiberglass / 300 Series Tilt and Turn, 300 Series Fixed, 325 Series Awning/Casement, 325 Series Fixed, and 400 Series / Fiberglass frame"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(417,'Master sheet'!$AL$1:$AL$441,0))","v":"Fiber Cement siding / James Hardie / HardiePanel® / 8 mm"}]
[null,null,null,null,null,{"$f":"INDEX('Master sheet'!$A$1:$A$441,MATCH(418,'Master sheet'!$AL$1:$AL$441,0))","v":"Gypsum panels - glass mat / CertainTeed / GlasRoc Sheathing gypsum board / 5/8\" "}]

{"sheet":"Setting","index":35,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":true,"merged":[[0,0,0,15],[3,4,4,4],[3,6,4,6],[3,5,4,5],[1,4,2,7],[3,7,4,7]]}
["This sheet acts as a setting page to set data such as dropdown items and other data used in the backend"]
[null,null,null,null,"Sheet Code & Names"]
[]
[null,null,null,null,"Sheet Code","English Sheet Names","French Sheet Names","Current Sheet Names"]
[]
["Language:","English",null,null,"License","License","License",{"$f":"IF(LOWER(rng_language)=\"english\",F6,G6)","v":"License"}]
[null,null,null,null,"USER INPUT SHEET","USER INPUT SHEET","FICHE D’ENTRÉE UTILISATEUR","USER INPUT SHEET"]
[null,null,null,null,"Footings & Slabs","Footings & Slabs","Semelles et dalles","Footings & Slabs"]
[null,null,null,null,"Foundation Walls","Foundation Walls","Murs de fondation","Foundation Walls"]
[null,null,null,null,"Structural Elements","Structural Elements","Éléments structuraux","Structural Elements"]
[null,null,null,null,"Ext. Walls","Ext. Walls","Murs ext.","Ext. Walls"]
[null,null,null,null,"Ext. Wall Systems","Ext. Wall Systems","Systèmes de murs ext.","Ext. Wall Systems"]
[null,null,null,null,"Party Walls","Party Walls","Murs mitoyens","Party Walls"]
[null,null,null,null,"Cladding","Cladding","Bardage","Cladding"]
[null,null,null,null,"Windows","Windows","Fenêtres","Windows"]
[null,null,null,null,"Int. Walls","Int. Walls","Murs int.","Int. Walls"]
[null,null,null,null,"Floors","Floors","Planchers","Floors"]
[null,null,null,null,"Ceilings","Ceilings","Plafonds","Ceilings"]
[null,null,null,null,"Roof","Roof","Toit","Roof"]
[null,null,null,null,"Garage","Garage","Garage","Garage"]
[null,null,null,null,"User-Defined","User-Defined","Défini par l’utilisateur","User-Defined"]
[null,null,null,null,"REVIEW","REVIEW","REVOIR","REVIEW"]
[null,null,null,null,"RESULTS","RESULTS","RÉSULTATS","RESULTS"]
[null,null,null,null,"SCENARIOS","SCENARIOS","SCÉNARIOS","SCENARIOS"]
[null,null,null,null,"Energy GHG","Energy GHG","GES Énergie","Energy GHG"]
[null,null,null,null,"Master sheet","Master sheet","Fiche principale","Master sheet"]
[null,null,null,null,"Composite Master Sheet","Composite Master Sheet","Fiche principale composite","Composite Master Sheet"]
[null,null,null,null,"Data","Data","Données","Data"]
[null,null,null,null,"Windows Methodology","Windows Methodology","Méthodes de fenestration","Windows Methodology"]
[null,null,null,null,"Dropdown Lists","Dropdown Lists","Listes déroulantes","Dropdown Lists"]
[null,null,null,null,"NOTE: Do NOT remove this cell. Insert the new sheets above this cell. And make sure no sheet code is blank."]
[]
[]
[]
[]
["© His Majesty the king in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
["© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]

{"sheet":"Formulas & Formats","index":36,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":true,"merged":[[0,0,0,1],[0,6,0,7]]}
["COLOURS",null,null,"FONTS",null,null,"FORMULAE"]
["a","Title Row\n(row ht 55)"]
["a","Header Row",null,"CO2E EMISSIONS","Calibri 18 Bold",null,"NET kgCO2e EMISSIONS","I6 = L6 - (M6 x N6)"]
["a","Worksheet Subtotal",null,"CO2 STORAGE","Calibri 18 Bold",null,"CO2e EMISSIONS","L6 = D6 x $H$6 x G6/100 x Column M (C13) from Master Sheet"]
["a","Section Heading\n(row ht 55)",null,"CO2 STORAGE FACTOR","Calibri 18",null,"CO2 STORAGE","M6 = D x $H$6 x G6/100 x Column AA (C27) from Master Sheet"]
["a","Material Group Heading",null,null,null,null,"CO2 STORAGE FACTOR","N6 = Column AC (C29) from Master Sheet"]
["a","User Input Cell",null,null,null,null,"CO2e EMISSIONS (w R-Value)","L37 = D37 x ($E$35/5.678) x G37/100 x Column M(C13) from Master sheet"]
["a","Selected Material\n(sheet total row ht 35)",null,null,null,null,"CO2 STORAGE (w R-Value)","M37 = D37 x ($E$35/5.678) x G37/100 x Column AA (C27) from Master sheet"]
[null,"Material Alternate Row Colour",null,null,null,null,null,"NOTE: The quantity for the cladding materials is:\nH30*2 + H29"]
[]
[null,null,null,null,null,null,null,"Steel Framing Factors"]
[]
[null,"Framing factors:","Wood dimensions in meters:",null,null,null,"Factor for","Load Bearing Walls"]
[null,"16\" = 25%","2x4",8.8900000000000007E-2,"m","16\" o.c.",3.794,"Equivalent m of linear stud per m2 (to account for horizontal members in a typical 10' wall)"]
[null,"24\" = 22%","2x6",0.13969999999999999,"m","24\" o.c.",2.9738000000000002,"Equivalent m of linear stud per m2 (to account for horizontal members in a typical 10' wall)"]
[null,null,"2x8",0.18415000000000001,"m"]
[null,null,"2x10",0.23494999999999999,"m",null,"Factor for","Non Load Bearing Walls"]
[null,null,"2x12",0.28575,"m","16\" o.c.",3.1273,"Equivalent m of linear stud per m2 (to account for horizontal members in a typical 10' wall)"]
[null,null,null,null,null,"24\" o.c.",2.3071000000000002,"Equivalent m of linear stud per m2 (to account for horizontal members in a typical 10' wall)"]
[null,"Spacing","Joists / m"]
[null,"16\"",{"$f":"1/(0.0254*16)","v":2.4606299212598426},null,null,null,"Factor for","Vertical Studs only"]
[null,"24\"",{"$f":"1/(0.0254*24)","v":1.6404199475065619},null,null,"16\" o.c.",{"$f":"1/(0.0254*16)","v":2.4606299212598426},"linear m of vertical studs per m2 of wall"]
[null,"36\"",{"$f":"1/(0.0254*36)","v":1.0936132983377078},null,null,"24\" o.c.",{"$f":"1/(0.0254*24)","v":1.6404199475065619},"linear m of vertical studs per m2 of wall"]
[]
[null,"TJI Size","Ratio of density/m of TJI"]
[null,"9-1/2\"",0.92600000000000005]
[null,"EPD avg",1]
[null,"11-7/8\"",1.0289999999999999]
[null,"14\"",1.1319999999999999]
[null,"16\"",1.2]
[]
[null,"SIP Panel","Factor"]
[null,"5-1/2\", R-22",{"$f":"5.5*4/5.678","v":3.8746037337090526}]
[null,"7-1/4\", \nR-29 Factor: 5.106",{"$f":"7.25*4/5.678","v":5.1074321944346606}]
[null,"9-1/2\", \nR-38 Factor: 10.326",{"$f":"9.5*4/5.678","v":6.6924973582247267}]
[null,"11-7/8\", \nR-48 Factor:13.043",{"$f":"11.875*4/5.678","v":8.3656216977809095}]
[]
[]
[null,"© His Majesty the king in Right of Canada, as represented by the Minister of Natural Resources, 2023"]
[null,"© Sa Majesté le Roi du chef du Canada, représentée par le ministre de Ressources naturelles, 2023"]